> ECS Schema Statistics
> The ECS schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by Schema Format String Syntax in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> ECS Schema Statistics

> Statistic | Description | Data Type
> General ECS Statistics
> ecs-subscribers | The combined total of the number of subscribers who have used the ECS service previously + other subscribers currently using the ECS service. | Int32
> ecs-subscribers-cur | The number of subscribers currently using the ECS service. | Int32
> gcdrs-generated | The total number of G-CDRs generated by ECS. | Int32
> edrs-generated | The total number of EDRs generated by ECS. | Int32
> udrs-generated | The total number of UDRs generated by ECS. | Int32
> IP Analyzer Specific Statistics
> ip-flows | The combined total of the number of IP flows previously analyzed + IP flows currently being analyzed. | Int64
> ip-flows-cur | The number of IP flows currently being analyzed. | Int64
> ip-uplk-bytes | The total number of IP bytes detected in uplink direction (from the MS). | Int64
> ip-dwnlk-bytes | The total number of IP bytes detected in downlink direction (to the MS). | Int64
> ip-uplk-pkts | The total number of IP packets detected in uplink direction. | Int64
> ip-dwnlk-pkts | The total number of IP packets detected in downlink direction. | Int64
> ip-uplk-pkts-frag | The total number of fragmented IP packets detected in uplink direction. | Int32
> ip-dwnlk-pkts-frag | The total number of fragmented IP packets detected in downlink direction. | Int32
> ip-uplk-bytes-frag | The total number of fragmented IP bytes detected in uplink direction. | Int32
> ip-dwnlk-bytes-frag | The total number of fragmented IP bytes detected in downlink direction. | Int32
> UDP Analyzer Specific Statistics
> udp-flows | The combined total of the number of UDP flows previously analyzed + UDP flows currently being analyzed. | Int32
> udp-flows-cur | The number of UDP flows currently being analyzed. | Int32
> udp-uplk-bytes | The total number of UDP bytes detected in uplink direction (from the MS). | Int64
> udp-dwnlk-bytes | The total number of UDP bytes detected in downlink direction (to the MS). | Int64
> udp-uplk-pkts | The total number of UDP packets detected in uplink direction. | Int32
> udp-dwnlk-pkts | The total number of UDP packets detected in downlink direction. | Int32
> udp-inv-pkts | The total number of invalid UDP packets detected. | Int32
> TCP Analyzer Specific Statistics
> tcp-flows | The combined total of the number of TCP flows previously analyzed + TCP flows currently being analyzed. | Int32
> tcp-flows-cur | The number of TCP flows currently being analyzed. | Int32
> tcp-uplk-bytes | The total number of TCP bytes detected in uplink direction (from the MS). | Int64
> tcp-dwnlk-bytes | The total number of TCP bytes detected in downlink direction (to the MS). | Int64
> tcp-uplk-pkts | The total number of TCP packets detected in uplink direction. | Int64
> tcp-dwnlk-pkts | The total number of TCP packets detected in downlink direction. | Int64
> tcp-uplk-bytes-retr | The total number of TCP bytes retransmitted in uplink direction. | Int32
> tcp-dwnlk-bytes-retr | The total number of TCP bytes retransmitted in downlink direction. | Int32
> tcp-uplk-pkts-retr | The total number of TCP packets retransmitted in uplink direction. | Int32
> tcp-dwnlk-pkts-retr | The total number of TCP packets retransmitted in downlink direction. | Int32
> tcp-uplk-pkts-ooo-analyzd | The total number of out-of-order TCP packets analyzed in uplink direction. | Int32
> tcp-dwnlk-pkts-ooo-analyzd | The total number of out-of-order TCP packets analyzed in downlink direction. | Int32
> tcp-uplk-pkts-ooo-fail | The total number of failed out-of-order TCP packets detected in uplink direction. | Int32
> tcp-dwnlk-pkts-ooo-fail | The total number of failed out-of-order TCP packets detected in downlink direction. | Int32
> tcp-uplk-pkts-ooo-retr | The total number of out-of-order TCP packets retransmitted in uplink direction. | Int32
> tcp-dwnlk-pkts-ooo-retr | The total number of out-of-order TCP packets retransmitted in downlink direction. | Int32
> ICMP Analyzer Specific Statistics
> icmp-flows | The combined total of the number of ICMP flows previously analyzed + ICMP flows currently being analyzed. | Int32
> icmp-flows-cur | The number of ICMP flows currently being analyzed. | Int32
> icmp-uplk-bytes | The total number of ICMP bytes detected in uplink direction (from the MS). | Int32
> icmp-dwnlk-bytes | The total number of ICMP bytes detected in downlink direction (to the MS). | Int32
> icmp-uplk-pkts | The total number of ICMP packets detected in uplink direction. | Int32
> icmp-dwnlk-pkts | The total number of ICMP packets detected in downlink direction. | Int32
> icmp-ech-req | The total number of ICMP ECHO requests detected. | Int32
> icmp-ech-rep | The total number of ICMP ECHO replies detected. | Int32
> icmp-dst-unrch | The total number of ICMP Destination Unreachable messages detected. | Int32
> icmp-redir | The total number of ICMP Redirect messages detected. | Int32
> icmp-tm-excd | The total number of ICMP Time Exceeded messages detected. | Int32
> icmp-trace-route | The total number of ICMP Trace Route messages detected. | Int32
> icmp-oth | The total number of ICMP Other Messages detected. | Int32
> icmp-inv-pkts | The total number of ICMP invalid packets detected. | Int32
> HTTP Analyzer Specific Statistics
> http-flows | The combined total of the number of HTTP flows previously analyzed + HTTP flows currently being analyzed. | Int32
> http-flows-cur | The number of HTTP flows currently being analyzed. | Int32
> http-uplk-bytes | The total number of HTTP bytes detected in uplink direction (from the MS). | Int64
> http-dwnlk-bytes | The total number of HTTP bytes detected in downlink direction (to the MS). | Int64
> http-uplk-pkts | The total number of HTTP packets detected in uplink direction. | Int64
> http-dwnlk-pkts | The total number of HTTP packets detected in downlink direction. | Int64
> http-uplk-bytes-retr | The total number of HTTP bytes retransmitted in uplink direction. | Int32
> http-dwnlk-bytes-retr | The total number of HTTP bytes retransmitted in downlink direction. | Int32
> http-uplk-pkts-retr | The total number of HTTP packets retransmitted in uplink direction. | Int32
> http-dwnlk-pkts-retr | The total number of HTTP packets retransmitted in downlink direction. | Int32
> http-req-succ | The total number of successful HTTP requests detected. | Int32
> http-req-fail | The total number of failed HTTP requests detected. | Int32
> http-get-req | The total number of HTTP GET requests detected. | Int32
> http-post-req | The total number of HTTP POST requests detected. | Int32
> http-connect-req | The total number of HTTP CONNECT requests detected. | Int32
> http-inv-pkts | The total number of invalid HTTP packets detected. | Int32
> HTTPS Analyzer Specific Statistics
> https-flows | The combined total of the number of HTTPS flows previously analyzed + HTTPS flows currently being analyzed. | Int32
> https-flows-cur | The number of HTTPS flows currently being analyzed. | Int32
> https-uplk-bytes | The total number of HTTPS bytes detected in uplink direction (from the MS). | Int64
> https-dwnlk-bytes | The total number of HTTPS bytes detected in downlink direction (to the MS). | Int64
> https-uplk-pkts | The total number of HTTPS packets detected in uplink direction. | Int64
> https-dwnlk-pkts | The total number of HTTPS packets detected in downlink direction. | Int64
> https-uplk-bytes-retr | The total number of HTTPS bytes retransmitted in uplink direction. | Int32
> https-dwnlk-bytes-retr | The total number of HTTPS bytes retransmitted in downlink direction. | Int32
> https-uplk-pkts-retr | The total number of HTTPS packets retransmitted in uplink direction. | Int32
> https-dwnlk-pkts-retr | The total number of HTTPS packets retransmitted in downlink direction. | Int32
> WTP Analyzer Specific Statistics
> wtp-trans | The total number of WTP transactions detected. | Int32
> wtp-cls-zero | The total number of WTP Class 0 transactions detected. | Int32
> wtp-cls-one | The total number of WTP Class 1 transactions detected. | Int32
> wtp-cls-two | The total number of WTP Class 2 transactions detected. | Int32
> wtp-uplk-bytes | The total number of WTP bytes detected in uplink direction (from the MS). | Int32
> wtp-dwnlk-bytes | The total number of WTP bytes detected in downlink direction (to the MS). | Int32
> wtp-uplk-pkts | The total number of WTP packets detected in uplink direction. | Int32
> wtp-dwnlk-pkts | The total number of WTP packets detected in downlink direction. | Int32
> wtp-uplk-bytes-retr | The total number of WTP bytes retransmitted in uplink direction. | Int32
> wtp-dwnlk-bytes-retr | The total number of WTP bytes retransmitted in downlink direction. | Int32
> wtp-uplk-pkts-retr | The total number of WTP packets retransmitted in uplink direction. | Int32
> wtp-dwnlk-pkts-retr | The total number of WTP packets retransmitted in downlink direction. | Int32
> wtp-invk-pkts | The total number of WTP INVOKE packets detected. | Int32
> wtp-invk-tcl-zero | The total number of WTP INVOKE TCL-0 packets detected. | Int32
> wtp-invk-tcl-one | The total number of WTP INVOKE TCL-1 packets detected. | Int32
> wtp-invk-tcl-two | The total number of WTP INVOKE TCL-2 packets detected. | Int32
> wtp-invk-tid-new | The total number of WTP INVOKE with TID-new flag packets detected. | Int32
> wtp-rslt-pkts | The total number of WTP RESULT packets detected. | Int32
> wtp-ack-to-resp | The total number of WTP ACK from Initiator to Responder detected. | Int32
> wtp-ack-to-init | The total number of WTP ACK from Responder to Initiator detected. | Int32
> wtp-abrt-to-resp | The total number of WTP ABORT from Initiator to Responder detected. | Int32
> wtp-abrt-to-init | The total number of WTP ABORT from Responder to Initiator detected. | Int32
> wtp-seg-invk | The total number of WTP Segmented INVOKE packets detected. | Int32
> wtp-seg-rslt | The total number of WTP Segmented RESULT packets detected. | Int32
> wtp-neg-ack | The total number of WTP Negative ACK packets detected. | Int32
> wtp-tid-vrf | The total number of WTP TID Verification packets detected. | Int32
> wtp-noninit-invk | The total number of WTP Non-initial INVOKE packets detected. | Int32
> wtp-unk-pdu | The total number of WTP unknown PDUs detected. | Int32
> WSP Analyzer Specific Statistics
> wsp-flows | The combined total of the number of WSP flows previously analyzed + WSP flows currently being analyzed. | Int32
> wsp-flows-cur | The number of WSP flows currently being analyzed. | Int32
> wsp-co-conn | The total number of WSP connection-oriented connections detected. | Int32
> wsp-cl-conn | The total number of WSP connection-less connections detected. | Int32
> wsp-uplk-bytes | The total number of WSP bytes detected in uplink direction. | Int32
> wsp-dwnlk-bytes | The total number of WSP bytes detected in downlink direction. | Int32
> wsp-uplk-pkts | The total number of WSP packets detected in uplink direction. | Int32
> wsp-dwnlk-pkts | The total number of WSP packets detected in downlink direction. | Int32
> wsp-uplk-bytes-retr | The total number of WSP bytes retransmitted in uplink direction. | Int32
> wsp-dwnlk-bytes-retr | The total number of WSP bytes retransmitted in downlink direction. | Int32
> wsp-uplk-pkts-retr | The total number of WSP packets retransmitted in uplink direction. | Int32
> wsp-dwnlk-pkts-retr | The total number of WSP packets retransmitted in downlink direction. | Int32
> wsp-co-req-succ | The total number of WSP Connection Oriented Requests succeeded. | Int32
> wsp-co-req-fail | The total number of WSP Connection Oriented Requests failed. | Int32
> wsp-cl-req-succ | The total number of WSP Connection-less Requests succeeded. | Int32
> wsp-cl-req-fail | The total number of WSP Connection-less Requests failed. | Int32
> wsp-conn-pdu | The total number of WSP CONNECT PDU detected. | Int32
> wsp-conn-rep | The total number of WSP CONNECT REPLY PDU detected. | Int32
> wsp-redir | The total number of WSP REDIRECT PDU detected. | Int32
> wsp-disc | The total number of WSP DISCONNECT PDU detected. | Int32
> wsp-susp | The total number of WSP SUSPEND PDU detected. | Int32
> wsp-resm | The total number of WSP RESUME PDU detected. | Int32
> wsp-opt | The total number of WSP OPTIONS PDU detected. | Int32
> wsp-head | The total number of WSP HEAD PDU detected. | Int32
> wsp-del | The total number of WSP DELETE PDU detected. | Int32
> wsp-trace | The total number of WSP TRACE PDU detected. | Int32
> wsp-reply | The total number of WSP REPLY PDU detected. | Int32
> wsp-put | The total number of WSP PUT PDU detected. | Int32
> wsp-get | The total number of WSP GET PDU detected. | Int32
> wsp-push | The total number of WSP PUSH PDU detected. | Int32
> wsp-conf-push | The total number of WSP CONFIRMED-PUSH PDU detected. | Int32
> wsp-post | The total number of WSP POST PDU detected. | Int32
> wsp-data-frag | The total number of WSP DATA-FRAGMENT PDU detected. | Int32
> wsp-rsrvd | The total number of WSP RESERVED PDU detected. | Int32
> wsp-inv-pkts | The total number of invalid WSP packets detected. | Int32
> MMS Analyzer Specific Statistics
> mms-send | The total number of MMS message send transactions detected. | Int32
> mms-send-succ | The total number of successful MMS message send transactions detected. | Int32
> mms-send-fail | The total number of failed MMS message send transactions detected. | Int32
> mms-retrv | The total number of MMS message retrieve transactions detected. | Int32
> mms-retrv-succ | The total number of MMS message retrieve transactions succeeded. | Int32
> mms-retrv-fail | The total number of MMS message retrieve transactions failed. | Int32
> mms-uplk-bytes | The total number of MMS bytes detected in uplink direction. | Int32
> mms-dwnlk-bytes | The total number of MMS bytes detected in downlink direction. | Int32
> mms-uplk-pkts | The total number of MMS packets detected in uplink direction. | Int32
> mms-dwnlk-pkts | The total number of MMS packets detected in downlink direction. | Int32
> mms-uplk-bytes-retr | The total number of MMS bytes retransmitted in uplink direction. | Int32
> mms-dwnlk-bytes-retr | The total number of MMS bytes retransmitted in downlink direction. | Int32
> mms-uplk-pkts-retr | The total number of MMS packets retransmitted in uplink direction. | Int32
> mms-dwnlk-pkts-retr | The total number of MMS packets retransmitted in downlink direction. | Int32
> mms-snd-req | The total number of MMS SEND Requests detected. | Int32
> mms-snd-conf | The total number of MMS SEND Confirms detected. | Int32
> mms-ntf-ind | The total number of MMS Notification Indication detected. | Int32
> mms-ntf-ind-imm | The total number of MMS Notification Indication Immediate detected. | Int32
> mms-ntf-ind-del | The total number of MMS Notification Indication Delayed detected. | Int32
> mms-ntf-rsp | The total number of MMS Notification Response detected. | Int32
> mms-retrv-conf | The total number of MMS Retrieve Confirm detected. | Int32
> mms-ack-ind | The total number of MMS ACK Indication detected. | Int32
> mms-delvry-ind | The total number of MMS Delivery Indication detected. | Int32
> mms-unk-pdu | The total number of MMS Unknown PDU Type detected. | Int32
> mms-inv-pkts | The total number of invalid MMS packets detected. | Int32
> SIP Analyzer Specific Statistics
> sip-flows | The combined total of the number of SIP flows previously analyzed + SIP flows currently being analyzed. | Int32
> sip-flows-cur | The number of SIP flows currently being analyzed. | Int32
> sip-calls | The total number of SIP calls detected. | Int32
> sip-uplk-bytes | The total number of SIP bytes detected in uplink direction. | Int64
> sip-dwnlk-bytes | The total number of SIP bytes detected in downlink direction. | Int64
> sip-uplk-pkts | The total number of SIP packets detected in uplink direction. | Int32
> sip-dwnlk-pkts | The total number of SIP packets detected in downlink direction. | Int32
> sip-uplk-bytes-retr | The total number of SIP bytes retransmitted in uplink direction. | Int64
> sip-dwnlk-bytes-retr | The total number of SIP bytes retransmitted in downlink direction. | Int64
> sip-uplk-pkts-retr | The total number of SIP packets retransmitted in uplink direction. | Int32
> sip-dwnlk-pkts-retr | The total number of SIP packets retransmitted in downlink direction. | Int32
> sip-invite | The total number of SIP INVITE commands detected. | Int32
> sip-bye | The total number of SIP BYE commands detected. | Int32
> sip-ack | The total number of SIP ACK commands detected. | Int32
> sip-cancel | The total number of SIP CANCEL commands detected. | Int32
> sip-register | The total number of SIP REGISTER commands detected. | Int32
> sip-inv-pkts | The total number of invalid SIP packets detected. | Int32
> RTSP Analyzer Specific Statistics
> rtsp-flows | The combined total of the number of RTSP flows previously analyzed + RTSP flows currently being analyzed. | Int32
> rtsp-flows-cur | The number of RTSP flows currently being analyzed. | Int32
> rtsp-sess | The total number of RTSP sessions detected. | Int32
> rtsp-uplk-bytes | The total number of RTSP bytes detected in uplink direction. | Int64
> rtsp-dwnlk-bytes | The total number of RTSP bytes detected in downlink direction. | Int64
> rtsp-uplk-pkts | The total number of RTSP packets detected in uplink direction. | Int32
> rtsp-dwnlk-pkts | The total number of RTSP packets detected in downlink direction. | Int32
> rtsp-uplk-bytes-retr | The total number of RTSP bytes retransmitted in uplink direction. | Int64
> rtsp-dwnlk-bytes-retr | The total number of RTSP bytes retransmitted in downlink direction. | Int64
> rtsp-uplk-pkts-retr | The total number of RTSP packets retransmitted in uplink direction. | Int32
> rtsp-dwnlk-pkts-retr | The total number of RTSP packets retransmitted in downlink direction. | Int32
> rtsp-play | The total number of RTSP PLAY commands detected. | Int32
> rtsp-setup | The total number of RTSP SETUP commands detected. | Int32
> rtsp-pause | The total number of RTSP PAUSE commands detected. | Int32
> rtsp-record | The total number of RTSP RECORD commands detected. | Int32
> rtsp-option | The total number of RTSP OPTION commands detected. | Int32
> rtsp-redir | The total number of RTSP REDIRECT commands detected. | Int32
> rtsp-desc | The total number of RTSP DESCRIBE commands detected. | Int32
> rtsp-announ | The total number of RTSP ANNOUNCE commands detected. | Int32
> rtsp-trdwn | The total number of RTSP TEARDOWN commands detected. | Int32
> rtsp-get-param | The total number of RTSP GET PARAMETER commands detected. | Int32
> rtsp-set-param | The total number of RTSP SET PARAMETER commands detected. | Int32
> rtsp-inv-pkts | The total number of invalid RTSP packets detected. | Int32
> RTP Analyzer Specific Statistics
> rtp-flows | The combined total of the number of RTP flows previously analyzed + RTP flows currently being analyzed. | Int32
> rtp-flows-cur | The number of RTP flows currently being analyzed. | Int32
> rtp-uplk-bytes | The total number of RTP bytes detected in uplink direction. | Int64
> rtp-dwnlk-bytes | The total number of RTP bytes detected in downlink direction. | Int64
> rtp-uplk-pkts | The total number of RTP packtes detected in uplink direction. | Int64
> rtp-dwnlk-pkts | The total number of RTP packtes detected in downlink direction. | Int64
> FTP Analyzer Specific Statistics
> ftp-flows | The combined total of the number of FTP flows previously analyzed + FTP flows currently being analyzed. | Int32
> ftp-flows-cur | The number of FTP flows currently being analyzed. | Int32
> ftp-uplk-bytes | The total number of FTP bytes detected in uplink direction. | Int64
> ftp-dwnlk-bytes | The total number of FTP bytes detected in downlink direction. | Int64
> ftp-uplk-pkts | The total number of FTP packets detected in uplink direction. | Int64
> ftp-dwnlk-pkts | The total number of FTP packets detected in downlink direction. | Int64
> ftp-retr | The total number of FTP RETR commands detected. | Int32
> ftp-stor | The total number of FTP STOR commands detected. | Int32
> ftp-inv-pkts | The total number of invalid FTP packets detected. | Int32
> SMTP Analyzer Specific Statistics
> smtp-flows | The combined total of the number of SMTP flows previously analyzed + SMTP flows currently being analyzed. | Int32
> smtp-flows-cur | The number of SMTP flows currently being analyzed. | Int32
> smtp-uplk-bytes | The total number of SMTP bytes detected in uplink direction. | Int64
> smtp-dwnlk-bytes | The total number of SMTP bytes detected in downlink direction. | Int64
> smtp-uplk-pkts | The total number of SMTP packets detected in uplink direction. | Int64
> smtp-dwnlk-pkts | The total number of SMTP packets detected in downlink direction. | Int64
> smtp-uplk-bytes-retr | The total number of SMTP bytes retransmitted in uplink direction. | Int32
> smtp-dwnlk-bytes-retr | The total number of SMTP bytes retransmitted in downlink direction. | Int32
> smtp-uplk-pkts-retr | The total number of SMTP packets retransmitted in uplink direction. | Int32
> smtp-dwnlk-pkts-retr | The total number of SMTP packets retransmitted in downlink direction. | Int32
> smtp-unk-cmd | The total number of SMTP Unknown commands detected. | Int32
> smtp-unk-resp | The total number of SMTP Unknown responses detected. | Int32
> smtp-req-succ | The total number of SMTP requests succeeded. | Int32
> smtp-req-fail | The total number of failed SMTP requests. | Int32
> smtp-helo | The total number of SMTP HELO commands detected. | Int32
> smtp-ehlo | The total number of SMTP EHLO commands detected. | Int32
> smtp-mail-frm | The total number of SMTP MAIL FROM commands detected. | Int32
> smtp-rcpt-to | The total number of SMTP RCPT TO commands detected. | Int32
> smtp-data | The total number of SMTP DATA commands detected. | Int32
> smtp-bdat | The total number of SMTP BDAT commands detected. | Int32
> smtp-vrfy | The total number of SMTP VERIFY commands detected. | Int32
> smtp-expn | The total number of SMTP EXPN commands detected. | Int32
> smtp-noop | The total number of SMTP NOOP commands detected. | Int32
> smtp-rset | The total number of SMTP RSET commands detected. | Int32
> smtp-quit | The total number of SMTP QUIT commands detected. | Int32
> smtp-inv-pkts | The total number of invalid SMTP packets detected. | Int32
> POP3 Analyzer Specific Statistics
> pop3-flows | The combined total of the number of POP3 flows previously analyzed + POP3 flows currently being analyzed. | Int32
> pop3-flows-cur | The number of POP3 flows currently being analyzed. | Int32
> pop3-uplk-bytes | The total number of POP3 bytes detected in uplink direction. | Int64
> pop3-dwnlk-bytes | The total number of POP3 bytes detected in downlink direction. | Int64
> pop3-uplk-pkts | The total number of POP3 packets detected in uplink direction. | Int64
> pop3-dwnlk-pkts | The total number of POP3 packets detected in downlink direction. | Int64
> pop3-uplk-bytes-retr | The total number of POP3 bytes retransmitted in uplink direction. | Int32
> pop3-dwnlk-bytes-retr | The total number of POP3 bytes retransmitted in downlink direction. | Int32
> pop3-uplk-pkts-retr | The total number of POP3 packets retransmitted in uplink direction. | Int32
> pop3-dwnlk-pkts-retr | The total number of POP3 packets retransmitted in downlink direction. | Int32
> pop3-retr | The total number of POP3 RETR commands detected. | Int32
> pop3-retr-succ | The total number of POP3 RETR commands successful. | Int32
> pop3-list | The total number of POP3 LIST commands detected. | Int32
> pop3-list-succ | The total number of POP3 LIST commands successful. | Int32
> pop3-inv-pkts | The total number of invalid POP3 packets detected. | Int32
> IMAP Statistics
> imap-uplk-bytes | The total number of IMAP bytes detected in uplink direction. | Int64
> imap-dwnlk-bytes | The total number of IMAP bytes detected in downlink direction. | Int64
> imap-uplk-pkts | The total number of IMAP packets detected in uplink direction. | Int32
> imap-dwnlk-pkts | The total number of IMAP packets detected in downlink direction. | Int32
> imap-uplk-bytes-retr | The total number of IMAP retry bytes detected in uplink direction. | Int64
> imap-dwnlk-bytes-retr | The total number of IMAP retry bytes detected in downlink direction. | Int64
> imap-uplk-pkts-retr | The total number of IMAP retry packets detected in uplink direction. | Int32
> imap-dwnlk-pkts-retr | The total number of IMAP retry packets detected in downlink direction. | Int32
> imap-req-succ | The total number of successful IMAP requests detected. | Int32
> imap-req-fail | The total number of failed IMAP requests detected. | Int32
> imap-reply-untag | The total number of untagged IMAP replies detected. | Int32
> imap-reply-commcont | The total number of IMAP Command Cont replies detected. | Int32
> imap-unk-command | The total number of unknown IMAP commands detected. | Int32
> imap-unk-reply | The total number of unknown IMAP replies detected. | Int32
> acf-req-created | Total number of ACF requests created. | Int64
> acf-wr-req-succ | Total number of successful ACF WRITE requests. | Int64
> acf-wr-req-failed | Total number of ACF WRITE requests failed. | Int64
> acf-rd-rsp-succ | Total number of successful ACF READ responses. | Int64
> acf-rd-rsp-failed | Total number of failed READ responses. | Int64
> acf-http-permit | Total number of HTTP URLs permitted from ACF. | Int64
> acf-http-deny | Total number of HTTP URLs denied from ACF. | Int64
> acf-http-redirect | Total number of HTTP URLs redirected from ACF. | Int64
> acf-wap-permit | Total number of WAP URLs permitted from ACF. | Int64
> acf-wap-deny | Total number of WAP URLs denied from ACF. | Int64
> acf-wap-redirect | Total number of WAP URLs redirected from ACF. | Int64
> P2P Specific Statistics
> p2p-flows | This proprietary counter indicates the total number of P2P flows detected. Triggers: Increments when a flow is marked as P2P. Availability: Per Active Charging Service. Type: Counter | Int32
> p2p-flows-cur | This proprietary counter indicates the number of currently active P2P flows. Triggers: Increments when a flow is marked as P2P. This is decremented when the flow state is cleaned up. Availability: Per Active Charging Service. Type: Counter | Int32
> p2p-subscribers | The total number of subscribers who had P2P flows. Triggers: Increments when Availability: Per Active Charging Service. Type: Counter | Int32
> p2p-subscribers-cur | The current active subscribers who have P2P flows. Triggers: Increments when Availability: Per Active Charging Service. Type: Counter | Int32
> p2p-skype-voice-duration | This proprietary counter indicates the total skype voice duration for a P2P subscriber at a given instance in time. | Int32
> p2p-msn-voice-duration | This proprietary counter indicates the total msn voice duration for a P2P subscriber at a given instance in time. | Int32
> p2p-oscar-voice-duration | This proprietary counter indicates the total oscar voice duration for a P2P subscriber at a given instance in time. | Int32
> p2p-gtalk-voice-duration | This proprietary counter indicates the total gtalk voice duration for a P2P subscriber at a given instance in time. | Int32
> p2p-yahoo-voice-duration | This proprietary counter indicates the total yahoo voice duration for a P2P subscriber at a given instance in time. | Int32
> p2p-skype-uplnk-bytes | This proprietary counter indicates the number of bytes of Skype traffic detected in uplink direction. Triggers: Increments when a packet of Skype traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-dwlnk-bytes | This proprietary counter indicates the number of bytes of Skype traffic detected in downlink direction. Triggers: Increments when a packet of Skype traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-uplnk-pkts | This proprietary counter indicates the number of packets of Skype traffic detected in uplink direction. Triggers: Increments when a packet of Skype traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-dwlnk-pkts | This proprietary counter indicates the number of packets of Skype traffic detected in downlink direction. Triggers: Increments when a packet of Skype traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of Skype voice traffic detected in uplink direction. Triggers: Increments when a packet of Skype voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of Skype voice traffic detected in downlink direction. Triggers: Increments when a packet of Skype voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-voice-uplnk-pkts | This proprietary counter indicates the number of packets of Skype voice traffic detected in uplink direction. Triggers: Increments when a packet of Skype voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of Skype voice traffic detected in downlink direction. Triggers: Increments when a packet of Skype voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-non-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of Skype non-voice traffic detected in uplink direction. Triggers: Increments when a packet of Skype non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-non-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of Skype non-voice traffic detected in downlink direction. Triggers: Increments when a packet of Skype non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-non-voice-uplnk-pkts | This proprietary counter indicates the number of packets of Skype non-voice traffic detected in uplink direction. Triggers: Increments when a packet of Skype non-voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skype-non-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of Skype non-voice traffic detected in downlink direction. Triggers: Increments when a packet of Skype non-voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-bittorrent-uplnk-bytes | This proprietary counter indicates the number of bytes of BitTorrent traffic detected in uplink direction. Triggers: Increments when a packet of BitTorrent traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-bittorrent-dwlnk-bytes | This proprietary counter indicates the number of bytes of BitTorrent traffic detected in downlink direction. Triggers: Increments when a packet of BitTorrent traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-bittorrent-uplnk-pkts | This proprietary counter indicates the number of packets of BitTorrent traffic detected in uplink direction. Triggers: Increments when a packet of BitTorrent traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-bittorrent-dwlnk-pkts | This proprietary counter indicates the number of packets of BitTorrent traffic detected in downlink direction. Triggers: Increments when a packet of BitTorrent traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-edonkey-uplnk-bytes | This proprietary counter indicates the number of bytes of eDonkey traffic detected in uplink direction. Triggers: Increments when a packet of eDonkey traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-edonkey-dwlnk-bytes | This proprietary counter indicates the number of bytes of eDonkey traffic detected in downlink direction. Triggers: Increments when a packet of eDonkey traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-edonkey-uplnk-pkts | This proprietary counter indicates the number of packets of eDonkey traffic detected in uplink direction. Triggers: Increments when a packet of eDonkey traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-edonkey-dwlnk-pkts | This proprietary counter indicates the number of packets of eDonkey traffic detected in downlink direction. Triggers: Increments when a packet of eDonkey traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-uplnk-bytes | This proprietary counter indicates the number of bytes of MSN traffic detected in uplink direction. Triggers: Increments when a packet of MSN traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-dwlnk-bytes | This proprietary counter indicates the number of bytes of MSN traffic detected in downlink direction. Triggers: Increments when a packet of MSN traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-uplnk-pkts | This proprietary counter indicates the number of packets of MSN traffic detected in uplink direction. Triggers: Increments when a packet of MSN traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-dwlnk-pkts | This proprietary counter indicates the number of packets of MSN traffic detected in downlink direction. Triggers: Increments when a packet of MSN traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of MSN voice traffic detected in uplink direction. Triggers: Increments when a packet of MSN voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of MSN voice traffic detected in downlink direction. Triggers: Increments when a packet of MSN voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-voice-uplnk-pkts | This proprietary counter indicates the number of packets of MSN voice traffic detected in uplink direction. Triggers: Increments when a packet of MSN voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of MSN voice traffic detected in downlink direction. Triggers: Increments when a packet of MSN voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-non-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of MSN non-voice traffic detected in uplink direction. Triggers: Increments when a packet of MSN non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-non-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of MSN non-voice traffic detected in downlink direction. Triggers: Increments when a packet of MSN non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-non-voice-uplnk-pkts | This proprietary counter indicates the number of packets of MSN non-voice traffic detected in uplink direction. Triggers: Increments when a packet of MSN non-voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-msn-non-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of MSN non-voice traffic detected in downlink direction. Triggers: Increments when a packet of MSN non-voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-uplnk-bytes | This proprietary counter indicates the number of bytes of Yahoo traffic detected in uplink direction. Triggers: Increments when a packet of Yahoo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-dwlnk-bytes | This proprietary counter indicates the number of bytes of Yahoo traffic detected in downlink direction. Triggers: Increments when a packet of Yahoo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-uplnk-pkts | This proprietary counter indicates the number of packets of Yahoo traffic detected in uplink direction. Triggers: Increments when a packet of Yahoo traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-dwlnk-pkts | This proprietary counter indicates the number of packets of Yahoo traffic detected in downlink direction. Triggers: Increments when a packet of Yahoo traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of Yahoo voice traffic detected in uplink direction. Triggers: Increments when a packet of Yahoo voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of Yahoo voice traffic detected in downlink direction. Triggers: Increments when a packet of Yahoo voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-voice-uplnk-pkts | This proprietary counter indicates the number of packets of Yahoo voice traffic detected in uplink direction. Triggers: Increments when a packet of Yahoo voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of Yahoo voice traffic detected in downlink direction. Triggers: Increments when a packet of Yahoo voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-non-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of Yahoo non-voice traffic detected in uplink direction. Triggers: Increments when a packet of Yahoo non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-non-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of Yahoo non-voice traffic detected in downlink direction. Triggers: Increments when a packet of Yahoo non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-non-voice-uplnk-pkts | This proprietary counter indicates the number of packets of Yahoo non-voice traffic detected in uplink direction. Triggers: Increments when a packet of Yahoo non-voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-yahoo-non-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of Yahoo non-voice traffic detected in downlink direction. Triggers: Increments when a packet of Yahoo non-voice traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-orb-uplnk-bytes | This proprietary counter indicates the number of bytes of ORB traffic detected in uplink direction. Triggers: Increments when a packet of ORB traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-orb-dwlnk-bytes | This proprietary counter indicates the number of bytes of ORB traffic detected in downlink direction. Triggers: Increments when a packet of ORB traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-orb-uplnk-pkts | This proprietary counter indicates the number of packets of ORB traffic detected in uplink direction. Triggers: Increments when a packet of ORB traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-orb-dwlnk-pkts | This proprietary counter indicates the number of packets of ORB traffic detected in downlink direction. Triggers: Increments when a packet of ORB traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winny-uplnk-bytes | This proprietary counter indicates the number of bytes of Winny traffic detected in uplink direction. Triggers: Increments when a packet of Winny traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winny-dwlnk-bytes | This proprietary counter indicates the number of bytes of Winny traffic detected in downlink direction. Triggers: Increments when a packet of Winny traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winny-uplnk-pkts | This proprietary counter indicates the number of packets of Winny traffic detected in uplink direction. Triggers: Increments when a packet of Winny traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winny-dwlnk-pkts | This proprietary counter indicates the number of packets of Winny traffic detected in downlink direction. Triggers: Increments when a packet of Winny traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-slingbox-uplnk-bytes | This proprietary counter indicates the number of bytes of Slingbox traffic detected in uplink direction. Triggers: Increments when a packet of Slingbox traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-slingbox-dwlnk-bytes | This proprietary counter indicates the number of bytes of Slingbox traffic detected in downlink direction. Triggers: Increments when a packet of Slingbox traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-slingbox-uplnk-pkts | This proprietary counter indicates the number of packets of Slingbox traffic detected in uplink direction. Triggers: Increments when a packet of Slingbox traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-slingbox-dwlnk-pkts | This proprietary counter indicates the number of packets of Slingbox traffic detected in downlink direction. Triggers: Increments when a packet of Slingbox traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fasttrack-uplnk-bytes | This proprietary counter indicates the number of bytes of FastTrack traffic detected in uplink direction. Triggers: Increments when a packet of FastTrack traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fasttrack-dwlnk-bytes | This proprietary counter indicates the number of bytes of FastTrack traffic detected in downlink direction. Triggers: Increments when a packet of FastTrack traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fasttrack-uplnk-pkts | This proprietary counter indicates the number of packets of FastTrack traffic detected in uplink direction. Triggers: Increments when a packet of FastTrack traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fasttrack-dwlnk-pkts | This proprietary counter indicates the number of packets of FastTrack traffic detected in downlink direction. Triggers: Increments when a packet of FastTrack traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gnutella-uplnk-bytes | This proprietary counter indicates the number of bytes of Gnutella traffic detected in uplink direction. Triggers: Increments when a packet of Gnutella traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gnutella-dwlnk-bytes | This proprietary counter indicates the number of bytes of Gnutella traffic detected in downlink direction. Triggers: Increments when a packet of Gnutella traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gnutella-uplnk-pkts | This proprietary counter indicates the number of packets of Gnutella traffic detected in uplink direction. Triggers: Increments when a packet of Gnutella traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gnutella-dwlnk-pkts | This proprietary counter indicates the number of packets of Gnutella traffic detected in downlink direction. Triggers: Increments when a packet of Gnutella traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-jabber-uplnk-bytes | This proprietary counter indicates the number of bytes of Jabber traffic detected in uplink direction. Triggers: Increments when a packet of Jabber traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-jabber-dwlnk-bytes | This proprietary counter indicates the number of bytes of Jabber traffic detected in downlink direction. Triggers: Increments when a packet of Jabber traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-jabber-uplnk-pkts | This proprietary counter indicates the number of packets of Jabber traffic detected in uplink direction. Triggers: Increments when a packet of Jabber traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-jabber-dwlnk-pkts | This proprietary counter indicates the number of packets of Jabber traffic detected in downlink direction. Triggers: Increments when a packet of Jabber traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-manolito-uplnk-bytes | This proprietary counter indicates the number of bytes of manolito traffic detected in uplink direction. Triggers: Increments when a packet of manolito traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-manolito-dwlnk-bytes | This proprietary counter indicates the number of bytes of manolito traffic detected in downlink direction. Triggers: Increments when a packet of manolito traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-manolito-uplnk-pkts | This proprietary counter indicates the number of packets of manolito traffic detected in uplink direction. Triggers: Increments when a packet of manolito traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-manolito-dwlnk-pkts | This proprietary counter indicates the number of packets of manolito traffic detected in downlink direction. Triggers: Increments when a packet of manolito traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pando-uplnk-bytes | This proprietary counter indicates the number of bytes of pando traffic detected in uplink direction. Triggers: Increments when a packet of pando traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pando-dwlnk-bytes | This proprietary counter indicates the number of bytes of pando traffic detected in downlink direction. Triggers: Increments when a packet of pando traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pando-uplnk-pkts | This proprietary counter indicates the number of packets of pando traffic detected in uplink direction. Triggers: Increments when a packet of pando traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pando-dwlnk-pkts | This proprietary counter indicates the number of packets of pando traffic detected in downlink direction. Triggers: Increments when a packet of pando traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-filetopia-uplnk-bytes | This proprietary counter indicates the number of bytes of filetopia traffic detected in uplink direction. Triggers: Increments when a packet of filetopia traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-filetopia-dwlnk-bytes | This proprietary counter indicates the number of bytes of filetopia traffic detected in downlink direction. Triggers: Increments when a packet of filetopia traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-filetopia-uplnk-pkts | This proprietary counter indicates the number of packets of filetopia traffic detected in uplink direction. Triggers: Increments when a packet of filetopia traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-filetopia-dwlnk-pkts | This proprietary counter indicates the number of packets of filetopia traffic detected in downlink direction. Triggers: Increments when a packet of filetopia traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-soulseek-uplnk-bytes | This proprietary counter indicates the number of bytes of soulseek traffic detected in uplink direction. Triggers: Increments when a packet of soulseek traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-soulseek-dwlnk-bytes | This proprietary counter indicates the number of bytes of soulseek traffic detected in downlink direction. Triggers: Increments when a packet of soulseek traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-soulseek-uplnk-pkts | This proprietary counter indicates the number of packets of soulseek traffic detected in uplink direction. Triggers: Increments when a packet of soulseek traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-soulseek-dwlnk-pkts | This proprietary counter indicates the number of packets of soulseek traffic detected in downlink direction. Triggers: Increments when a packet of soulseek traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ppstream-uplnk-bytes | This proprietary counter indicates the number of bytes of ppstream traffic detected in uplink direction. Triggers: Increments when a packet of ppstream traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ppstream-dwlnk-bytes | This proprietary counter indicates the number of bytes of ppstream traffic detected in downlink direction. Triggers: Increments when a packet of ppstream traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ppstream-uplnk-pkts | This proprietary counter indicates the number of packets of ppstream traffic detected in uplink direction. Triggers: Increments when a packet of ppstream traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ppstream-dwlnk-pkts | This proprietary counter indicates the number of packets of ppstream traffic detected in downlink direction. Triggers: Increments when a packet of ppstream traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qq-uplnk-bytes | This proprietary counter indicates the number of bytes of qq traffic detected in uplink direction. Triggers: Increments when a packet of qq traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qq-dwlnk-bytes | This proprietary counter indicates the number of bytes of qq traffic detected in downlink direction. Triggers: Increments when a packet of qq traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qq-uplnk-pkts | This proprietary counter indicates the number of packets of qq traffic detected in uplink direction. Triggers: Increments when a packet of qq traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qq-dwlnk-pkts | This proprietary counter indicates the number of packets of qq traffic detected in downlink direction. Triggers: Increments when a packet of qq traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qqlive-uplnk-bytes | This proprietary counter indicates the number of bytes of qqlive traffic detected in uplink direction. Triggers: Increments when a packet of qqlive traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qqlive-dwlnk-bytes | This proprietary counter indicates the number of bytes of qqlive traffic detected in downlink direction. Triggers: Increments when a packet of qqlive traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qqlive-uplnk-pkts | This proprietary counter indicates the number of packets of qqlive traffic detected in uplink direction. Triggers: Increments when a packet of qqlive traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-qqlive-dwlnk-pkts | This proprietary counter indicates the number of packets of qqlive traffic detected in downlink direction. Triggers: Increments when a packet of qqlive traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-mute-uplnk-bytes | This proprietary counter indicates the number of bytes of Mute traffic detected in uplink direction. Triggers: Increments when a packet of mute traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-mute-dwlnk-bytes | This proprietary counter indicates the number of bytes of Mute traffic detected in downlink direction. Triggers: Increments when a packet of mute traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-mute-uplnk-pkts | This proprietary counter indicates the number of packets of Mute traffic detected in uplink direction. Triggers: Increments when a packet of mute traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-mute-dwlnk-pkts | This proprietary counter indicates the number of packets of Mute traffic detected in downlink direction. Triggers: Increments when a packet of mute traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gadugadu-uplnk-bytes | This proprietary counter indicates the number of bytes of gadugadu traffic detected in uplink direction. Triggers: Increments when a packet of gadugadu traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gadugadu-dwlnk-bytes | This proprietary counter indicates the number of bytes of gadugadu traffic detected in downlink direction. Triggers: Increments when a packet of gadugadu traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gadugadu-uplnk-pkts | This proprietary counter indicates the number of packets of gadugadu traffic detected in uplink direction. Triggers: Increments when a packet of gadugadu traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gadugadu-dwlnk-pkts | This proprietary counter indicates the number of packets of gadugadu traffic detected in downlink direction. Triggers: Increments when a packet of gadugadu traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-feidian-uplnk-bytes | This proprietary counter indicates the number of bytes of feidian traffic detected in uplink direction. Triggers: Increments when a packet of feidian traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-feidian-dwlnk-bytes | This proprietary counter indicates the number of bytes of feidian traffic detected in downlink direction. Triggers: Increments when a packet of feidian traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-feidian-uplnk-pkts | This proprietary counter indicates the number of packets of feidian traffic detected in uplink direction. Triggers: Increments when a packet of feidian traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-feidian-dwlnk-pkts | This proprietary counter indicates the number of packets of feidian traffic detected in downlink direction. Triggers: Increments when a packet of feidian traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-applejuice-uplnk-bytes | This proprietary counter indicates the number of bytes of applejuice traffic detected in uplink direction. Triggers: Increments when a packet of applejuice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-applejuice-dwlnk-bytes | This proprietary counter indicates the number of bytes of applejuice traffic detected in downlink direction. Triggers: Increments when a packet of applejuice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-applejuice-uplnk-pkts | This proprietary counter indicates the number of packets of applejuice traffic detected in uplink direction. Triggers: Increments when a packet of applejuice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-applejuice-dwlnk-pkts | This proprietary counter indicates the number of packets of applejuice traffic detected in downlink direction. Triggers: Increments when a packet of applejuice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-zattoo-uplnk-bytes | This proprietary counter indicates the number of bytes of zattoo traffic detected in uplink direction. Triggers: Increments when a packet of zattoo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-zattoo-dwlnk-bytes | This proprietary counter indicates the number of bytes of zattoo traffic detected in downlink direction. Triggers: Increments when a packet of zattoo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-zattoo-uplnk-pkts | This proprietary counter indicates the number of packets of zattoo traffic detected in uplink direction. Triggers: Increments when a packet of zattoo traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-zattoo-dwlnk-pkts | This proprietary counter indicates the number of packets of zattoo traffic detected in downlink direction. Triggers: Increments when a packet of feidian traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skinny-uplnk-bytes | This proprietary counter indicates the number of bytes of skinny traffic detected in uplink direction. Triggers: Increments when a packet of skinny traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skinny-dwlnk-bytes | This proprietary counter indicates the number of bytes of skinny traffic detected in downlink direction. Triggers: Increments when a packet of skinny traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skinny-uplnk-pkts | This proprietary counter indicates the number of packets of skinny traffic detected in uplink direction. Triggers: Increments when a packet of skinny traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-skinny-dwlnk-pkts | This proprietary counter indicates the number of packets of skinny traffic detected in downlink direction. Triggers: Increments when a packet of skinny traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-sopcast-uplnk-bytes | This proprietary counter indicates the number of bytes of sopcast traffic detected in uplink direction. Triggers: Increments when a packet of sopcast traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-sopcast-dwlnk-bytes | This proprietary counter indicates the number of bytes of sopcast traffic detected in downlink direction. Triggers: Increments when a packet of sopcast traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-sopcast-uplnk-pkts | This proprietary counter indicates the number of packets of sopcast traffic detected in uplink direction. Triggers: Increments when a packet of sopcast traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-sopcast-dwlnk-pkts | This proprietary counter indicates the number of packets of sopcast traffic detected in downlink direction. Triggers: Increments when a packet of sopcast traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ares-uplnk-bytes | This proprietary counter indicates the number of bytes of ares traffic detected in uplink direction. Triggers: Increments when a packet of ares traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ares-dwlnk-bytes | This proprietary counter indicates the number of bytes of ares traffic detected in downlink direction. Triggers: Increments when a packet of ares traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ares-uplnk-pkts | This proprietary counter indicates the number of packets of ares traffic detected in uplink direction. Triggers: Increments when a packet of ares traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ares-dwlnk-pkts | This proprietary counter indicates the number of packets of ares traffic detected in downlink direction. Triggers: Increments when a packet of ares traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-directconnect-uplnk-bytes | This proprietary counter indicates the number of bytes of directconnect traffic detected in uplink direction. Triggers: Increments when a packet of directconnect traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-directconnect-dwlnk-bytes | This proprietary counter indicates the number of bytes of directconnect traffic detected in downlink direction. Triggers: Increments when a packet of directconnect traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-directconnect-uplnk-pkts | This proprietary counter indicates the number of packets of directconnect traffic detected in uplink direction. Triggers: Increments when a packet of directconnect traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-directconnect-dwlnk-pkts | This proprietary counter indicates the number of packets of directconnect traffic detected in downlink direction. Triggers: Increments when a packet of directconnect traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-imesh-uplnk-bytes | This proprietary counter indicates the number of bytes of imesh traffic detected in uplink direction. Triggers: Increments when a packet of imesh traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-imesh-dwlnk-bytes | This proprietary counter indicates the number of bytes of imesh traffic detected in downlink direction. Triggers: Increments when a packet of imesh traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-imesh-uplnk-pkts | This proprietary counter indicates the number of packets of imesh traffic detected in uplink direction. Triggers: Increments when a packet of imesh traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-imesh-dwlnk-pkts | This proprietary counter indicates the number of packets of imesh traffic detected in downlink direction. Triggers: Increments when a packet of imesh traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pplive-uplnk-bytes | This proprietary counter indicates the number of bytes of pplive traffic detected in uplink direction. Triggers: Increments when a packet of pplive traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pplive-dwlnk-bytes | This proprietary counter indicates the number of bytes of pplive traffic detected in downlink direction. Triggers: Increments when a packet of pplive traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pplive-uplnk-pkts | This proprietary counter indicates the number of packets of pplive traffic detected in uplink direction. Triggers: Increments when a packet of pplive traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-pplive-dwlnk-pkts | This proprietary counter indicates the number of packets of pplive traffic detected in downlink direction. Triggers: Increments when a packet of pplive traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-uplnk-bytes | This proprietary counter indicates the number of bytes of oscar traffic detected in uplink direction. Triggers: Increments when a packet of oscar traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-dwlnk-bytes | This proprietary counter indicates the number of bytes of oscar traffic detected in downlink direction. Triggers: Increments when a packet of oscar traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-uplnk-pkts | This proprietary counter indicates the number of packets of oscar traffic detected in uplink direction. Triggers: Increments when a packet of oscar traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-dwlnk-pkts | This proprietary counter indicates the number of packets of oscar traffic detected in downlink direction. Triggers: Increments when a packet of oscar traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of oscar voice traffic detected in uplink direction. Triggers: Increments when a packet of oscar voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of oscar voice traffic detected in downlink direction. Triggers: Increments when a packet of oscar voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-voice-uplnk-pkts | This proprietary counter indicates the number of packets of oscar voice traffic detected in uplink direction. Triggers: Increments when a packet of oscar voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of oscar voice traffic detected in downlink direction. Triggers: Increments when a packet of oscar voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-non-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of oscar non-voice traffic detected in uplink direction. Triggers: Increments when a packet of oscar non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-non-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of oscar non-voice traffic detected in downlink direction. Triggers: Increments when a packet of oscar non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-non-voice-uplnk-pkts | This proprietary counter indicates the number of packets of oscar non-voice traffic detected in uplink direction. Triggers: Increments when a packet of oscar non-voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oscar-non-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of oscar non-voice traffic detected in downlink direction. Triggers: Increments when a packet of oscar non-voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-popo-uplnk-bytes | This proprietary counter indicates the number of bytes of popo traffic detected in uplink direction. Triggers: Increments when a packet of popo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-popo-dwlnk-bytes | This proprietary counter indicates the number of bytes of popo traffic detected in downlink direction. Triggers: Increments when a packet of popo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-popo-uplnk-pkts | This proprietary counter indicates the number of packets of popo traffic detected in uplink direction. Triggers: Increments when a packet of popo traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-popo-dwlnk-pkts | This proprietary counter indicates the number of packets of popo traffic detected in downlink direction. Triggers: Increments when a packet of popo traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-irc-uplnk-bytes | This proprietary counter indicates the number of bytes of IRC traffic detected in uplink direction. Triggers: Increments when a packet of IRC traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-irc-dwlnk-bytes | This proprietary counter indicates the number of bytes of IRC traffic detected in downlink direction. Triggers: Increments when a packet of IRC traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-irc-uplnk-pkts | This proprietary counter indicates the number of packets of IRC traffic detected in uplink direction. Triggers: Increments when a packet of IRC traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-irc-dwlnk-pkts | This proprietary counter indicates the number of packets of IRC traffic detected in downlink direction. Triggers: Increments when a packet of IRC traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-steam-uplnk-bytes | This proprietary counter indicates the number of bytes of steam traffic detected in uplink direction. Triggers: Increments when a packet of steam traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-steam-dwlnk-bytes | This proprietary counter indicates the number of bytes of steam traffic detected in downlink direction. Triggers: Increments when a packet of steam traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-steam-uplnk-pkts | This proprietary counter indicates the number of packets of steam traffic detected in uplink direction. Triggers: Increments when a packet of steam traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-steam-dwlnk-pkts | This proprietary counter indicates the number of packets of steam traffic detected in downlink direction. Triggers: Increments when a packet of steam traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ddlink-uplnk-bytes | This proprietary counter indicates the number of bytes of ddlink traffic detected in uplink direction. Triggers: Increments when a packet of ddlink traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ddlink-dwlnk-bytes | This proprietary counter indicates the number of bytes of ddlink traffic detected in downlink direction. Triggers: Increments when a packet of ddlink traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ddlink-uplnk-pkts | This proprietary counter indicates the number of packets of ddlink traffic detected in uplink direction. Triggers: Increments when a packet of ddlink traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-ddlink-dwlnk-pkts | This proprietary counter indicates the number of packets of ddlink traffic detected in downlink direction. Triggers: Increments when a packet of ddlink traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-halflife2-uplnk-bytes | This proprietary counter indicates the number of bytes of halflife2 traffic detected in uplink direction. Triggers: Increments when a packet of halflife2 traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-halflife2-dwlnk-bytes | This proprietary counter indicates the number of bytes of halflife2 traffic detected in downlink direction. Triggers: Increments when a packet of halflife2 traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-halflife2-uplnk-pkts | This proprietary counter indicates the number of packets of halflife2 traffic detected in uplink direction. Triggers: Increments when a packet of halflife2 traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-halflife2-dwlnk-pkts | This proprietary counter indicates the number of packets of halflife2 traffic detected in downlink direction. Triggers: Increments when a packet of halflife2 traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-hamachivpn-uplnk-bytes | This proprietary counter indicates the number of bytes of hamachivpn traffic detected in uplink direction. Triggers: Increments when a packet of hamachivpn traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-hamachivpn-dwlnk-bytes | This proprietary counter indicates the number of bytes of hamachivpn traffic detected in downlink direction. Triggers: Increments when a packet of hamachivpn traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-hamachivpn-uplnk-pkts | This proprietary counter indicates the number of packets of hamachivpn traffic detected in uplink direction. Triggers: Increments when a packet of hamachivpn traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-hamachivpn-dwlnk-pkts | This proprietary counter indicates the number of packets of hamachivpn traffic detected in downlink direction. Triggers: Increments when a packet of hamachivpn traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvants-uplnk-bytes | This proprietary counter indicates the number of bytes of tvants traffic detected in uplink direction. Triggers: Increments when a packet of tvants traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvants-dwlnk-bytes | This proprietary counter indicates the number of bytes of tvants traffic detected in downlink direction. Triggers: Increments when a packet of tvants traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvants-uplnk-pkts | This proprietary counter indicates the number of packets of tvants traffic detected in uplink direction. Triggers: Increments when a packet of tvants traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvants-dwlnk-pkts | This proprietary counter indicates the number of packets of tvants traffic detected in downlink direction. Triggers: Increments when a packet of tvants traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvuplayer-uplnk-bytes | This proprietary counter indicates the number of bytes of tvuplayer traffic detected in uplink direction. Triggers: Increments when a packet of tvuplayer traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvuplayer-dwlnk-bytes | This proprietary counter indicates the number of bytes of tvuplayer traffic detected in downlink direction. Triggers: Increments when a packet of tvuplayer traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvuplayer-uplnk-pkts | This proprietary counter indicates the number of packets of tvuplayer traffic detected in uplink direction. Triggers: Increments when a packet of tvuplayer traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-tvuplayer-dwlnk-pkts | This proprietary counter indicates the number of packets of tvuplayer traffic detected in downlink direction. Triggers: Increments when a packet of tvuplayer traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-uusee-uplnk-bytes | This proprietary counter indicates the number of bytes of uusee traffic detected in uplink direction. Triggers: Increments when a packet of uusee traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-uusee-dwlnk-bytes | This proprietary counter indicates the number of bytes of uusee traffic detected in downlink direction. Triggers: Increments when a packet of uusee traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-uusee-uplnk-pkts | This proprietary counter indicates the number of packets of uusee traffic detected in uplink direction. Triggers: Increments when a packet of uusee traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-uusee-dwlnk-pkts | This proprietary counter indicates the number of packets of uusee traffic detected in downlink direction. Triggers: Increments when a packet of uusee traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vpnx-uplnk-bytes | This proprietary counter indicates the number of bytes of vpnx traffic detected in uplink direction. Triggers: Increments when a packet of vpnx traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vpnx-dwlnk-bytes | This proprietary counter indicates the number of bytes of vpnx traffic detected in downlink direction. Triggers: Increments when a packet of vpnx traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vpnx-uplnk-pkts | This proprietary counter indicates the number of packets of vpnx traffic detected in uplink direction. Triggers: Increments when a packet of vpnx traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vpnx-dwlnk-pkts | This proprietary counter indicates the number of packets of vpnx traffic detected in downlink direction. Triggers: Increments when a packet of vpnx traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vtun-uplnk-bytes | This proprietary counter indicates the number of bytes of vtun traffic detected in uplink direction. Triggers: Increments when a packet of vtun traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vtun-dwlnk-bytes | This proprietary counter indicates the number of bytes of vtun traffic detected in downlink direction. Triggers: Increments when a packet of vtun traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vtun-uplnk-pkts | This proprietary counter indicates the number of packets of vtun traffic detected in uplink direction. Triggers: Increments when a packet of vtun traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-vtun-dwlnk-pkts | This proprietary counter indicates the number of packets of vtun traffic detected in downlink direction. Triggers: Increments when a packet of vtun traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winmx-uplnk-bytes | This proprietary counter indicates the number of bytes of winmx traffic detected in uplink direction. Triggers: Increments when a packet of winmx traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winmx-dwlnk-bytes | This proprietary counter indicates the number of bytes of winmx traffic detected in downlink direction. Triggers: Increments when a packet of winmx traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winmx-uplnk-pkts | This proprietary counter indicates the number of packets of winmx traffic detected in uplink direction. Triggers: Increments when a packet of winmx traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-winmx-dwlnk-pkts | This proprietary counter indicates the number of packets of winmx traffic detected in downlink direction. Triggers: Increments when a packet of winmx traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-wofwarcraft-uplnk-bytes | This proprietary counter indicates the number of bytes of wofwarcraft traffic detected in uplink direction. Triggers: Increments when a packet of wofwarcraft traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-wofwarcraft-dwlnk-bytes | This proprietary counter indicates the number of bytes of wofwarcraft traffic detected in downlink direction. Triggers: Increments when a packet of wofwarcraft traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-wofwarcraft-uplnk-pkts | This proprietary counter indicates the number of packets of wofwarcraft traffic detected in uplink direction. Triggers: Increments when a packet of wofwarcraft traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-wofwarcraft-dwlnk-pkts | This proprietary counter indicates the number of packets of wofwarcraft traffic detected in downlink direction. Triggers: Increments when a packet of wofwarcraft traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-xbox-uplnk-bytes | This proprietary counter indicates the number of bytes of xbox traffic detected in uplink direction. Triggers: Increments when a packet of xbox traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-xbox-dwlnk-bytes | This proprietary counter indicates the number of bytes of xbox traffic detected in downlink direction. Triggers: Increments when a packet of xbox traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-xbox-uplnk-pkts | This proprietary counter indicates the number of packets of xbox traffic detected in uplink direction. Triggers: Increments when a packet of xbox traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-xbox-dwlnk-pkts | This proprietary counter indicates the number of packets of xbox traffic detected in downlink direction. Triggers: Increments when a packet of xbox traffic is detected by P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fring-uplnk-bytes | This proprietary counter indicates the number of bytes of fring traffic detected in uplink direction. Triggers: Increments when a packet of fring traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fring-dwlnk-bytes | This proprietary counter indicates the number of bytes of fring traffic detected in downlink direction. Triggers: Increments when a packet of fring traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fring-uplnk-pkts | This proprietary counter indicates the number of packets of fring traffic detected in uplink direction. Triggers: Increments when a packet of fring traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-fring-dwlnk-pkts | This proprietary counter indicates the number of packets of fring traffic detected in downlink direction. Triggers: Increments when a packet of fring traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-iskoot-uplnk-bytes | This proprietary counter indicates the number of bytes of iskoot traffic detected in uplink direction. Triggers: Increments when a packet of iskoot traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-iskoot-dwlnk-bytes | This proprietary counter indicates the number of bytes of iskoot traffic detected in downlink direction. Triggers: Increments when a packet of iskoot traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-iskoot-uplnk-pkts | This proprietary counter indicates the number of packets of iskoot traffic detected in uplink direction. Triggers: Increments when a packet of iskoot traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-iskoot-dwlnk-pkts | This proprietary counter indicates the number of packets of iskoot traffic detected in downlink direction. Triggers: Increments when a packet of iskoot traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oovoo-uplnk-bytes | This proprietary counter indicates the number of bytes of oovoo traffic detected in uplink direction. Triggers: Increments when a packet of oovoo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oovoo-dwlnk-bytes | This proprietary counter indicates the number of bytes of oovoo traffic detected in downlink direction. Triggers: Increments when a packet of oovoo traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oovoo-uplnk-pkts | This proprietary counter indicates the number of packets of oovoo traffic detected in uplink direction. Triggers: Increments when a packet of oovoo traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-oovoo-dwlnk-pkts | This proprietary counter indicates the number of packets of oovoo traffic detected in downlink direction. Triggers: Increments when a packet of oovoo traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-uplnk-bytes | This proprietary counter indicates the number of bytes of gtalk traffic detected in uplink direction. Triggers: Increments when a packet of gtalk traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-dwlnk-bytes | This proprietary counter indicates the number of bytes of gtalk traffic detected in downlink direction. Triggers: Increments when a packet of gtalk traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-uplnk-pkts | This proprietary counter indicates the number of packets of gtalk traffic detected in uplink direction. Triggers: Increments when a packet of gtalk traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-dwlnk-pkts | This proprietary counter indicates the number of packets of gtalk traffic detected in downlink direction. Triggers: Increments when a packet of gtalk traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of gtalk voice traffic detected in uplink direction. Triggers: Increments when a packet of gtalk voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of gtalk voice traffic detected in downlink direction. Triggers: Increments when a packet of gtalk voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-voice-uplnk-pkts | This proprietary counter indicates the number of packets of gtalk voice traffic detected in uplink direction. Triggers: Increments when a packet of gtalk voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of gtalk voice traffic detected in downlink direction. Triggers: Increments when a packet of gtalk voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-non-voice-uplnk-bytes | This proprietary counter indicates the number of bytes of gtalk non-voice traffic detected in uplink direction. Triggers: Increments when a packet of gtalk non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-non-voice-dwlnk-bytes | This proprietary counter indicates the number of bytes of gtalk non-voice traffic detected in downlink direction. Triggers: Increments when a packet of gtalk non-voice traffic is detected by the P2P analyzer; payload length is added to this counter. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-non-voice-uplnk-pkts | This proprietary counter indicates the number of packets of gtalk non-voice traffic detected in uplink direction. Triggers: Increments when a packet of gtalk non-voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-gtalk-non-voice-dwlnk-pkts | This proprietary counter indicates the number of packets of gtalk non-voice traffic detected in downlink direction. Triggers: Increments when a packet of gtalk non-voice traffic is detected by the P2P analyzer. Availability: Per Active Charging Service. Type: Counter | Int64
> p2p-freenet-uplnk-bytes | This proprietary counter indicates the total number of bytes of freenet traffic received from an MS. | Int64
> p2p-freenet-dwlnk-bytes | This proprietary counter indicates the total number of bytes of freenet traffic sent to MS. | Int64
> p2p-freenet-uplnk-pkts | This proprietary counter indicates the total number of packets of freenet traffic received from an MS. | Int64
> p2p-freenet-dwlnk-pkts | This proprietary counter indicates the total number of packets of freenet traffic sent to MS. | Int64
> p2p-aimini-uplnk-bytes | This proprietary counter indicates the total number of bytes of aimini traffic received from an MS. | Int64
> p2p-aimini-dwlnk-bytes | This proprietary counter indicates the total number of bytes of aimini traffic sent to MS. | Int64
> p2p-aimini-uplnk-pkts | This proprietary counter indicates the total number of packets of aimini traffic received from an MS. | Int64
> p2p-aimini-dwlnk-pkts | This proprietary counter indicates the total number of packets of aimini traffic sent to MS. | Int64
> p2p-battlefld-uplnk-bytes | This proprietary counter indicates the total number of bytes of battlefld traffic received from an MS. | Int64
> p2p-battlefld-dwlnk-bytes | This proprietary counter indicates the total number of bytes of battlefld traffic sent to MS. | Int64
> p2p-battlefld-uplnk-pkts | This proprietary counter indicates the total number of packets of battlefld traffic received from an MS. | Int64
> p2p-battlefld-dwlnk-pkts | This proprietary counter indicates the total number of packets of battlefld traffic sent to MS. | Int64
> p2p-openft-uplnk-bytes | This proprietary counter indicates the total number of bytes of openft traffic received from an MS. | Int64
> p2p-openft-dwlnk-bytes | This proprietary counter indicates the total number of bytes of openft traffic sent to MS. | Int64
> p2p-openft-uplnk-pkts | This proprietary counter indicates the total number of packets of openft traffic received from an MS. | Int64
> p2p-openft-dwlnk-pkts | This proprietary counter indicates the total number of packets of openft traffic sent to MS. | Int64
> p2p-qqgame-uplnk-bytes | This proprietary counter indicates the total number of bytes of qqgame traffic received from an MS. | Int64
> p2p-qqgame-dwlnk-bytes | This proprietary counter indicates the total number of bytes of qqgame traffic sent to MS. | Int64
> p2p-qqgame-uplnk-pkts | This proprietary counter indicates the total number of packets of qqgame traffic received from an MS. | Int64
> p2p-qqgame-dwlnk-pkts | This proprietary counter indicates the total number of packets of qqgame traffic sent to MS. | Int64
> p2p-quake-uplnk-bytes | This proprietary counter indicates the total number of bytes of quake traffic received from an MS. | Int64
> p2p-quake-dwlnk-bytes | This proprietary counter indicates the total number of bytes of quake traffic sent to MS. | Int64
> p2p-quake-uplnk-pkts | This proprietary counter indicates the total number of packets of quake traffic received from an MS. | Int64
> p2p-quake-dwlnk-pkts | This proprietary counter indicates the total number of packets of quake traffic sent to MS. | Int64
> p2p-secondlife-uplnk-bytes | This proprietary counter indicates the total number of bytes of secondlife traffic received from an MS. | Int64
> p2p-secondlife-dwlnk-bytes | This proprietary counter indicates the total number of bytes of secondlife traffic sent to MS. | Int64
> p2p-secondlife-uplnk-pkts | This proprietary counter indicates the total number of packets of secondlife traffic received from an MS. | Int64
> p2p-secondlife-dwlnk-pkts | This proprietary counter indicates the total number of packets of secondlife traffic sent to MS. | Int64
> p2p-actsync-uplnk-bytes | This proprietary counter indicates the total number of bytes of actsync traffic received from an MS. | Int64
> p2p-actsync-dwlnk-bytes | This proprietary counter indicates the total number of bytes of actsync traffic sent to MS. | Int64
> p2p-actsync-uplnk-pkts | This proprietary counter indicates the total number of packets of actsync traffic received from an MS. | Int64
> p2p-actsync-dwlnk-pkts | This proprietary counter indicates the total number of packets of actsync traffic sent to MS. | Int64
> p2p-nimbuzz-uplnk-bytes | This proprietary counter indicates the total number of bytes of nimbuzz traffic received from an MS. | Int64
> p2p-nimbuzz-dwlnk-bytes | This proprietary counter indicates the total number of bytes of nimbuzz traffic sent to MS. | Int64
> p2p-nimbuzz-uplnk-pkts | This proprietary counter indicates the total number of packets of nimbuzz traffic received from an MS. | Int64
> p2p-nimbuzz-dwlnk-pkts | This proprietary counter indicates the total number of packets of nimbuzz traffic sent to MS. | Int64
> p2p-iax-uplnk-bytes | This proprietary counter indicates the total number of bytes of iax traffic received from an MS. | Int64
> p2p-iax-dwlnk-bytes | This proprietary counter indicates the total number of bytes of iax traffic sent to MS. | Int64
> p2p-iax-uplnk-pkts | This proprietary counter indicates the total number of packets of iax traffic received from an MS. | Int64
> p2p-iax-dwlnk-pkts | This proprietary counter indicates the total number of packets of iax traffic sent to MS. | Int64
> p2p-paltalk-uplnk-bytes | This proprietary counter indicates the total number of bytes of paltalk traffic received from an MS. | Int64
> p2p-paltalk-dwlnk-bytes | This proprietary counter indicates the total number of bytes of paltalk traffic sent to MS. | Int64
> p2p-paltalk-uplnk-pkts | This proprietary counter indicates the total number of packets of paltalk traffic received from an MS. | Int64
> p2p-paltalk-dwlnk-pkts | This proprietary counter indicates the total number of packets of paltalk traffic sent to MS. | Int64
> p2p-warcft3-uplnk-bytes | This proprietary counter indicates the total number of bytes of warcft3 traffic received from an MS. | Int64
> p2p-warcft3-dwlnk-bytes | This proprietary counter indicates the total number of bytes of warcft3 traffic sent to MS. | Int64
> p2p-warcft3-uplnk-pkts | This proprietary counter indicates the total number of packets of warcft3 traffic received from an MS. | Int64
> p2p-warcft3-dwlnk-pkts | This proprietary counter indicates the total number of packets of warcft3 traffic sent to MS. | Int64
> p2p-rdp-uplnk-bytes | This proprietary counter indicates the total number of bytes of rdp traffic received from an MS. | Int64
> p2p-rdp-dwlnk-bytes | This proprietary counter indicates the total number of bytes of rdp traffic sent to MS. | Int64
> p2p-rdp-uplnk-pkts | This proprietary counter indicates the total number of packets of rdp traffic received from an MS. | Int64
> p2p-rdp-dwlnk-pkts | This proprietary counter indicates the total number of packets of rdp traffic sent to MS. | Int64
> p2p-iptv-uplnk-bytes | This proprietary counter indicates the total number of bytes of iptv traffic received from an MS. | Int64
> p2p-iptv-dwlnk-bytes | This proprietary counter indicates the total number of bytes of iptv traffic sent to MS. | Int64
> p2p-iptv-uplnk-pkts | This proprietary counter indicates the total number of packets of iptv traffic received from an MS. | Int64
> p2p-iptv-dwlnk-pkts | This proprietary counter indicates the total number of packets of iptv traffic sent to MS. | Int64
> p2p-pandora-uplnk-bytes | This proprietary counter indicates the total number of bytes of pandora traffic received from an MS. | Int64
> p2p-pandora-dwlnk-bytes | This proprietary counter indicates the total number of bytes of pandora traffic sent to MS. | Int64
> p2p-pandora-uplnk-pkts | This proprietary counter indicates the total number of packets of pandora traffic received from an MS. | Int64
> p2p-pandora-dwlnk-pkts | This proprietary counter indicates the total number of packets of pandora traffic sent to MS. | Int64
> DNS Stats
> dns-flows | The combined total of the number of DNS flows previously analyzed + DNS flows currently being analyzed. | Int32
> dns-flows-cur | The number of DNS flows currently being analyzed. | Int32
> dns-uplk-bytes | The total number of DNS bytes detected in uplink direction. | Int64
> dns-dwnlk-bytes | The total number of DNS bytes detected in downlink direction. | Int64
> dns-uplk-pkts | The total number of DNS packets detected in uplink direction. | Int64
> dns-dwnlk-pkts | The total number of DNS packets detected in downlink direction. | Int64
> dns-unk-opcode | The total number of DNS packets with an unknown operational code. | Int32
> dns-inv-pkts | The total number of invalid DNS packets detected. | Int32
> dns-over-tcp-uplk-bytes | The total number of DNS uplink bytes that were detected over TCP. | Int64
> dns-over-tcp-dwnlk-bytes | The total number of DNS downlink bytes that were detected over TCP. | Int64
> dns-over-tcp-uplk-pkts | The total number of DNS uplink packets that were detected over TCP. | Int64
> dns-over-tcp-dwnlk-pkts | The total number of DNS downlink packets that were detected over TCP. | Int64
> dns-req-a-query | The total number of DNS requests received for queries. | Int64
> dns-req-cname-query | The total number of DNS requests received for cname queries. | Int64
> dns-req-ns-query | The total number of DNS requests received for ns queries. | Int64
> dns-req-ptr-query | The total number of DNS requests received for ptr queries. | Int64
> dns-req-aaaa-query | The total number of DNS requests received for AAAA queries. | Int64
> dns-req-unknown-query | The total number of DNS requests received for unknown queries. | Int64
> dns-rsp-a-query | The total number of DNS responses received for queries. | Int64
> dns-rsp-cname-query | The total number of DNS responses received for cname queries. | Int64
> dns-rsp-ns-query | The total number of DNS responses received for ns queries. | Int64
> dns-rsp-ptr-query | The total number of DNS responses received for ptr queries. | Int64
> dns-rsp-aaaa-query | The total number of DNS responses received for AAAA queries. | Int64
> dns-rsp-unknown-query | The total number of DNS responses received for unknown queries. | Int64
> Historical ECS Statistics
> ecs-ttlsuccess | The total number of successful ECS sessions. | Int32
> ecs-ttlfail | The total number of failed ECS sessions. | Int32
> ecs-curactive | The number of currently active ECS sessions. | Int32
> ecs-15peak-curactive | The peak number of active ECS sessions in 15 one-minute intervals over the last 15 minutes. ecs-15peak-curactive is computed from ecs-curactive gathered every minute over the last 15 minutes. | Int32
> ecs-ruleshit | The total number of rules hit. | Int32
> ecs-ppruleshit | The total number of post-processing rules hit. | Int32
> ecs-ttldlinkbytes | The total number of downlink bytes detected for ECS sessions. | Int64
> ecs-ttlulinkbytes | The total number of uplink bytes detected for ECS sessions. | Int64
> ecs-ttldlinkpackets | The total number of downlink packets detected for ECS sessions. | Int64
> ecs-ttlulinkpackets | The total number of uplink packets detected for ECS sessions. | Int64
> ecs-ttlflowconn | The total number of flows established by ECS sessions. | Int32
> ecs-ttlflowdisc | The total number of flows disconnected for ECS sessions. | Int32
> ecs-curflow | The number of currently active ECS flows. | Int32
> ecs-15peak-curflow | The peak number of active ECS flows in 15 one-minute intervals over the last 15 minutes. ecs-15peak-curflow is computed from ecs-curflow gathered every minute over the last 15 minutes. | Int32
> ecs-15min-usage-flowall | The total number of active ECS flows detected in the last 15 minutes. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883