> show apn
> This chapter includes the show apn command output tables.
> show apn all
> show apn all Command Output Descriptions

> Field | Description
> access point name (APN) | Indicates the name of the access point name (APN) for which counters are displayed.
> authentication context | Name of the system context used for authentication for this APN.
> pdp type | Indicates the type of PDP context. Possible types are:
> • | IPv4
> • | IPv6
> • | PPP
> Selection Mode | Indicates the APN selection mode applicable for this APN. Possible selection modes are:
> • | Chosen by SGSN
> • | Sent by MS
> • | Subscribed
> ip source violation | Indicates whether check for IPv4 source validation violations enabled or not. Possible status are:
> • | Checked
> • | Ignored
> drop limit | Indicates the IP source-violation drop limit configured for the subscriber. The drop-limit is the number of invalid packets that can be received from a subscriber prior to their session being deleted. Refer to the ip source-violation command in the APN configuration mode.
> ip source violation no accounting | The IP source validation violations that were detected but not included in the statistics.
> accounting mode | Indicates the accounting mode configured for this APN. Possible modes are:
> • | gtpp - GTPP CDR accounting
> • | none - No accounting
> • | radius-diameter - RADIUS or Diameter accounting
> No early PDUs | Specifies whether “no-early-pdu” option configured in this APN or not. If “no-early-PDUs” is enabled, the chassis shall not send uplink/downlink data from/to a MS till it receives the Acct-Rsp Start for the same from the AAA device. On receiving the Acct-Rsp, pending PDUs are sent out.
> no-interims | Specifies whether “no-interims” option configured in this APN or not. If “no-interims” is enabled, the chassis shall not send any interim message to the AAA device.
> Bearer Control Mode | Specifies whether Bearer Control Mode is enabled in this APN or not.
> max-primary-pdp-contexts | Specifies the maximum primary PDP contexts allowed in this APN.
> total-pdp-contexts | Specifies the total primary and secondary PDP contexts allowed in this APN.
> primary contexts | Specifies the total primary contexts allowed in this APN.
> total contexts | Specifies the total primary and secondary contexts allowed in this APN.
> max secondary contexts per-subscriber | Specifies the maximum secondary contexts allowed in this APN for a subscriber.
> IMS Authorization | Specifies whether IMS authorization support is enabled in this APN or not.
> Credit Control | Specifies whether Diameter pre-paid credit control support is enabled in this APN or not.
> mbms bearer absolute timeout | Indicates the absolute time out duration in seconds for Multimedia Broadcast-Multicast Service (MBMS) bearer context.
> mbms bearer idle timeout | Indicates the idle time out duration in seconds for Multimedia Broadcast-Multicast Service (MBMS) bearer context.
> mbms ue absolute timeout | Indicates the absolute time out duration in seconds for Multimedia Broadcast-Multicast Service (MBMS) UE context.
> local ip | Specifies the local IP address of the interface assigned to this APN.
> nexthop gateway addr | Specifies the IP address of the next hop gateway configured in this APN.
> primary dns | Indicates the IP address of primary Domain Name Server (DNS).
> secondary dns | Indicates the IP address of secondary Domain Name Server (DNS).
> primary nbns | Indicates the IP address of primary NetBIOS Name Server (NBNS).
> secondary nbns | Indicates the IP address of secondary NetBIOS Name Server (NBNS).
> ppp keep alive period | Indicates the duration in seconds to transmit LCP keep-alive packet.
> ppp mtu | Indicates the maximum size of transmission units in bytes configured for this APN.
> absolute timeout | Indicates the absolute timeout duration in seconds for session configured in this APN.
> idle timeout | Indicates the idle timeout duration in seconds for session configured in this APN.
> idle-timeout-activity ignore-downlink | Indicates whether idle timeout activity configured in this APN to consider downlink traffic as activity for idle-timeout or not.
> long duration timeout | Indicates the timeout duration in seconds for long duration timeout support configured in this APN.
> long dur inactivity time | Indicates the inactivity duration in seconds for long duration timeout support configured in this APN.
> long duration action | Indicates the action configured in this APN for long duration timeout support. Possible actions are:
> • | Detection
> • | Disconnection
> ip header compression | Indicates the IP header compression method configured in this APN for RObust Header Compression (ROHC) support. Supported method is Van Jacobsen (VJ).
> ip hide service address | Indicates whether APN is configured to hide service IP address from the subscriber (for security reasons) or not.
> ip output access-group | The IPv4 access control list (ACL) configured in this APN for outward traffic.
> ip input access-group | The IPv4 access control list (ACL) configured in this APN for inward traffic.
> ipv6 output access-group | The IPv6 access control list (ACL) configured in this APN for outward traffic.
> ipv6 input access-group | The IPv6 access control list (ACL) configured in this APN for inward traffic.
> policy-group in | The traffic policy group configured in this APN for inward traffic.
> policy-group out | The traffic policy group configured in this APN for outward traffic.
> permit ip multicast | Indicates whether APN is configured to discard or permit the IP multicast.
> ppp authentication | Indicates the type of PPP authentication configured for this APN.
> allow noauthentication | Indicates the whether PPP session is allowed without authentication in this APN or not.
> imsi authentication | Indicates the whether PPP session authentication in this APN is configured for IMSI authentication or not.
> msisdn authentication | Indicates the whether PPP session authentication in this APN is configured for MSISDN authentication or not.
> ip destination context | Indicates the name of the configured destination context for this APN.
> Rule Base | Indicates the name of the configured rulebase for this APN.
> Content-Filtering Policy-Id | Indicates the whether inline content filtering policy is configured for this APN or not.
> mediation accounting | Indicates the whether mediation device is configured for accounting in this APN or not.
> mediation-device context | Indicates the name of the system context to use for mediation device for accounting in this APN.
> mediation no early PDUs | Specifies whether “no-early-pdu” option configured for this subscriber or not. If “no-early-PDUs” is enabled, the chassis shall not send uplink/downlink data from/to a MS till it receives the Acct-Rsp Start for the same from the mediation device. On receiving the Acct-Rsp, pending PDUs are sent out.
> mediation no-interims | Specifies whether “no-interims” option configured for this subscriber or not. If “no-interims” is enabled, the chassis shall not send any interim message to the mediation device.
> mediation delay-GTP-response | Specifies whether “delay-GTP-response” option configured for this subscriber or not. When enabled, this option delays the Create PDP Context response until an Accounting Start response is received from the mediation device.
> outbound username | Name of the user for outbound traffic.
> ip address pools | Indicates the IP address pool used for this APN.
> access-link ip-frag | Indicates the IP packet fragmentation setting for access link.
> ignore DF-bit data-tunnel | Indicates whether “ignore df-bit” is set for data tunnel or not.
> ip allocation type | Specifies the type of IP allocation method used for IP address allocation. Possible types are:
> • | DHCP-Proxy
> • | DHCP-Relay
> • | Local
> • | Dynamic
> • | Static
> allow user specified ip addr | Indicates whether user specified IP address is allowed or not for IP allocation.
> prefer dhcp options | Indicates whether support for DHCP supplied parameters, like DNS/NBNS addresses, in subscriber session is configured for this APN. This support can be enabled with ip address alloc-method dhcp-proxy prefer-dhcp-options command in APN Configuration mode.
> 3gpp qos to dscp mapping | This group indicates the 3GPP QoS to DSCP mapping information.
> conversational | Indicates the DSCP configured for conversational type of traffic.
> streaming | Indicates the DSCP configured for streaming type of traffic.
> interactive (TP 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1.
> interactive (TP 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2.
> interactive (TP 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3.
> background | Indicates the DSCP configured for background type of traffic.
> 3GPP Qos to DSCP Mapping based on Alloc. Prio | This group indicates the 3GPP QoS to DSCP mapping information based on allocation priority.
> interactive (TP 1, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 1.
> interactive (TP 1, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 2.
> interactive (TP 1, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 3.
> interactive (TP 2, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 1.
> interactive (TP 2, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 2.
> interactive (TP 2, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 3.
> interactive (TP 3, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 1.
> interactive (TP 3, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 2.
> interactive (TP 3, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 3.
> Copy user-datagram IP TOS | Indicates whether copying of IP TOS octet value from user IPv4 datagrams to IP header of tunnel encapsulation is enabled or not.
> APN defined Charging Characteristics | This group displays the APN defined charging characteristics for various types of subscribers.
> Home Subscribers | This sub-group displays the APN defined charging characteristics for home subscribers.
> Behavior Bits | Indicates the behavior bits configured for home subscribers in APN defined charging characteristics.
> Profile Value | Indicates the profile value configured for home subscribers in APN defined charging characteristics.
> Visiting Subscribers | This sub-group displays the APN defined charging characteristics for visiting subscribers.
> Behavior Bits | Indicates the behavior bits configured for visiting subscribers in APN defined charging characteristics.
> Profile Value | Indicates the profile value configured for visiting subscribers in APN defined charging characteristics.
> Roaming Subscribers | This sub-group displays the APN defined charging characteristics for roaming subscribers.
> Behavior Bits | Indicates the behavior bits configured for roaming subscribers in APN defined charging characteristics.
> Profile Value | Indicates the profile value configured for roaming subscribers in APN defined charging characteristics.
> All (Home/Visiting/Roaming) Subscribers | This sub-group displays the APN defined charging characteristics for all subscribers (including home, visiting, and roaming).
> Behavior Bits | Indicates the behavior bits configured for all subscribers (including home, visiting, and roaming) in APN defined charging characteristics.
> Profile Value | Indicates the profile value configured for all subscribers (including home, visiting, and roaming) in APN defined charging characteristics.
> Subscribers to use APN defined charging characteristics | Indicates the number of subscriber to use APN defined charging characteristics.
> Subscribers to use RADIUS returned charging characteristics | Indicates whether subscribers in this APN are configured to use charging characteristics returned from RADIUS server.
> dhcp service name | Specifies the name of the DHCP service configured for IP address allocation.
> dhcp context name | Specifies the name of the DHCP context where DHCP service is configured for IP address allocation.
> dhcp lease expiry policy | Specifies the DHCP address lease expiry policy. Possible actions are:
> • | autoconnect
> • | disconnect
> mobile-ip | Specifies the whether Mobile IP is configured in this APN or not.
> mobile-ip home-agent | Specifies the IP address of home agent (HA) to use for Mobile IP session in this APN.
> mobile-ip alternate-home-agent(s) | Specifies the IP address of alternate home agent (HA) to use for Mobile IP session in this APN.
> mobile-ip reverse-tunnel | Specifies the whether Mobile IP reverse tunnel is enabled for Mobile IP session in this APN or not.
> mobile-ip mn-aaa-removal-indication | Specifies the whether “mn-aaa-removal-indication” parameter is configured for Mobile IP session in this APN or not.
> mobile-ip mn-ha-spi | Specifies the security parameter index (SPI) configured between MN and HA for Mobile IP session in this APN.
> mobile-ip mn-ha-hash-algorithm | Specifies the hash algorithm configured for Mobile IP session in this APN. Possible hash algorithms are:
> • | hmac-md5
> • | md5
> • | rfc2002-md5
> proxy-mip | Specifies the whether Proxy-Mobile IP is configured in this APN or not.
> proxy-mip null-username static home address | Specifies the whether handling of RRQ to enable the acceptance without NAI extension in this APN is enabled or not.
> Tunnel peer load-balancing | Specifies the tunnel peer selection method in this APN for load balancing between tunnel-peers. Possible selection methods are:
> • | balanced
> • | prioritized
> • | random
> L3-to-L2 tunnel address-policy no-alloc-validate | Specifies whether this APN is configured, to not to allocate or validate subscriber addresses locally for such sessions, it passes the address between remote tunnel terminator to the Mobile Node, or not.
> tunnel address-policy alloc-validate | Specifies whether this APN is configured, to allocate addresses for cases in which IP addresses are dynamically assigned, or not.
> NPU QoS Traffic Priority | Indicates the configured NPU QoS priority queue for packets facilitated by the APN. Possible priorities are:
> • | best-effort
> • | bronze
> • | derive-from-packet-dscp
> • | gold
> • | silver.
> APN QoS Attributes | Specifies the QoS attribute configure in this APN.
> Newcall Policy | Indicates the policy for action on new calls coming on this APN. Possible actions are:
> • | Accept
> • | Reject
> SDU Error Ratio | Indicates the QoS attribute reliability class based on Service Data Unit (SDU) Error Ratio attributes configured in this APN.
> Residual BER | Indicates the QoS attribute reliability class based on Residual Bit Error Ratio (BER) attributes configured in this APN.
> Class: Conversational | Specifies the statistics for use traffic of conversational QoS class along with traffic policing/shaping status.
> Downlink Negotiate Limit | Specifies whether traffic data QoS negotiation limit in downlink direction is enabled or not for this class of QoS in this APN.
> Uplink Negotiate Limit | Specifies whether traffic data QoS negotiation limit in uplink direction is enabled or not for this class of QoS in this APN.
> Peak Data Rate (in bps) | The peak data rate in bit per seconds for this class of QoS in this APN.
> Committed Data Rate(in bps) | The committed data rate in bit per seconds for this class of QoS in this APN.
> Downlink Rate Limit | Specifies whether traffic data rate limit in downlink direction is enabled or not for this class of QoS in this APN.
> Uplink Rate Limit | Specifies whether traffic data rate limit in uplink direction is enabled or not for this class of QoS in this APN.
> Burst Size | This group indicates the static/dynamic burst size in bytes for peak and guaranteed rate limiting for this class of QoS in this APN.
> Auto Readjust | Indicates whether auto readjustment of burst size is enabled or not. Possible states are:
> • | Enabled
> • | Disabled
> Auto Readjust Duration | Indicates the configured auto readjust duration in a seconds. If auto readjust is enabled and no readjust duration is specified the default value is 1 second.
> Peak Burst Size(bytes) | Indicates the peak burst size in bytes calculated dynamically by auto readjust duration and rate limit value.
> Guaranteed Burst Size(bytes) | Indicates the guaranteed burst size in bytes calculated dynamically by auto readjust duration (seconds) and rate limit value (bytes). This counter is applicable only when auto readjustment is enabled.
> Exceed Action | Specifies the action on downlink/uplink data rate when exceeds the allowed rate limit for this class of QoS. Possible actions are:
> • | drop: drop the packets.
> • | lower-ip-precedence: transmit the packet after lowering the ip-precedence.
> • | transmit: transmit the packet.
> Violate Action | Specifies the action on downlink/uplink data rate violation of allowed rate limit for this class of QoS. Possible actions are:
> • | drop: drop the packets.
> • | lower-ip-precedence: transmit the packet after lowering the ip-precedence.
> • | shape: enables the traffic shaping and provides the buffering of user packets when subscriber traffic violates the allowed peak/committed data rate.
> • | shape-transmit-when-buffer-full: enables the traffic shaping and allows the packet to be transmitted when buffer memory is full.
> • | transmit: transmit the packet.
> Class: Streaming | Specifies the statistics for use traffic of streaming QoS class along with traffic policing/shaping status.
> Class: Interactive | Specifies the statistics for use traffic of interactive QoS class along with traffic policing/shaping status. It showed for the traffic handling priority 1 through 3.
> Traffic Handling Priority | Specifies the traffic handling priority for interactive QoS class along with traffic policing/shaping status. Possible values are priority 1 through 3.
> Class: Background | Specifies the statistics for use traffic of background QoS class along with traffic policing/shaping status.
> ppp accept peer ipv6 ifid | Indicates the IPv6 interface id of peer to accept PPP session.
> ipv6 init router advt interval | Indicates the initial IPv6 router advertisement interval in seconds for this APN.
> ipv6 init router number of advts | Indicates the total number of initial IPv6 router advertisement for this APN.
> ipv6 address prefix | Indicates the IPv6 address prefix configured for sessions facilitated by this APN.
> ipv6 address prefix pool | Indicates the IPv6 address prefix pool name configured for sessions facilitated by this APN.
> ipv6 interface id | Indicates the IPv6 interface id configured for sessions facilitated by this APN.
> ipv6 dns primary server | Indicates the IPv6 address of primary DNS server configured for sessions facilitated by this APN.
> ipv6 dns secondary server | Indicates the IPv6 address of secondary DNS server configured for sessions facilitated by this APN.
> ipv6 egress address filtering | Indicates whether egress address filtering configured in this APN or not to filter out packets not meant for the mobile interface ID.
> ipv6 dns proxy | Indicates whether IPv6 DNS proxy server configured for sessions facilitated by this APN or not.
> ipv6 minimum link MTU | Indicates the size of packet in bytes configured for access-link MTU for fragment.
> Radius Group | Indicates the AAA server group associated with this APN.
> Radius Returned Framed IP Address | This group specifies the action and policy to handle the framed IP address returned from RADIUS server.
> Policy | Specifies the policy to handle the framed IP address returned from RADIUS server. Possible actions are:
> • | accept-call-when-ms-ip-not-supplied
> • | reject-call-when-ms-ip-not-supplied
> Access-flow traffic-validation | Specifies whether traffic validation for access flow is enabled for this APN or not.
> Virtual APN Configuration | Indicates whether virtual APN is configured with APN or not.
> IPv6 Configuration | This group displays the configuration related to IPv6 parameters.
> IPv6 initial number of router advertisements | Indicates the total number of initial IPv6 router advertisement for this APN.
> IPv6 initial router advertisements interval | Indicates the initial IPv6 router advertisement interval in seconds for this APN.
> IPv6 Prefix Pool | Indicates the IPv6 address prefix pool name configured for sessions facilitated by this APN.
> IPv6 Egress address filtering | Indicates whether egress address filtering configured in this APN or not to filter out packets not meant for the mobile interface ID.
> IPv6 Primary DNS server address | Indicates the IPv6 address of primary DNS server configured for sessions facilitated by this APN.
> IPv6 Secondary DNS server address | Indicates the IPv6 address of secondary DNS server configured for sessions facilitated by this APN.
> GTPP Group | Indicates the GTPP server group associated with this APN.
> GTPP Accounting Context | Specifies the GTPP accounting context name associated with this APN.
> Firewall Policy | Indicates whether stateful firewall policy is applicable with this APN or not.
> Mobile IPv6 Tunnel MTU | Indicates the configured maximum transmission unit of packet in bytes for Mobile IPv6 tunnel traffic.
> Mobile IPv6 Tunnel MTU Exceed Action | Indicates the action to take on packets which exceeds the maximum transmission unit of packet in bytes for Mobile IPv6 tunnel traffic. Possible actions are:
> • | Normal processing
> • | Ignore defragment bit
> • | Fragment and forward the packet and notify the sender
> Mobile IPv6 Home Agent | Specifies the IPv6 address of home agent (HA) to use for Mobile IP session in this APN.
> Mobile IPv6 Home Link Prefix | Specifies the home link prefix for to use for Mobile IP session in this APN.
> Mobile IPv6 Home Address | Specifies the home IPv6 address of subscriber to use for Mobile IP session in this APN.

> ‌
> show apn counter ip-allocation all
> show apn coutner ip-allocation all Command Output Descriptions

> Field | Description
> APN | Indicates the name of the access point name (APN) for which counters are displayed.
> UE PROVID. | Indicates the total number of active sessions using UE provided IP allocation method through this APN.
> LOCAL POOL | Indicates the total number of active sessions using Local Pool method for IP allocation through this APN.
> AAA | Indicates the total number of active sessions using AAA provided IP allocation method through this APN.
> DHCP | This group indicates the total number of active sessions using DHCP method for IP allocation through this APN. Possible groups are: CLIENT: Indicates the number of active sessions using DHCP client method for IP allocation through this APN. RELAY: Indicates the number of active sessions using DHCP relay method for IP allocation through this APN.
> PASSTHRU | Indicates the total number of active sessions using PASSTHRU IP allocation method through this APN.

> ‌
> show apn statistics name
> show apn statistics name Command Output Descriptions

> Field | Description
> Gi interface statistics ('uplink'=to PDN, 'downlink'=from PDN):
> uplink bytes | The current total number of bytes sent on the Gi interface for the APN.
> downlink bytes | The current total number of bytes received on the Gi interface for the APN.
> uplink pkts | The current total number of IP packets sent from the Gi interface for the APN.
> downlink pkts | The current total number of IP packets received from the Gi interface for the APN.
> uplink pkts dropped | The current total number of IP packets for the APN that were dropped prior to sending over the Gi interface.
> downlink pkts dropped | The current total number of IP packets received from the Gi interface for the APN and dropped.
> ipv4 bad hdr | The current total number IP packets received and dropped due to bad headers.
> ipv4 ttl exceeded | The current total number of IP packets dropped because they were received with TTL values of 0.
> ipv4 fragments sent | The current total number of number of times IP packets were fragmented before being sent over the Gi interface.
> ipv4 could not fragment | The current total number of IP packets which failed in fragmentation.
> ipv4 input acl drop | The current total number IP packets that were received and then dropped due to ACL filtering. Important: This counter may increment even if no ACL is configured.
> ipv4 output acl drop | The current total number of IP packets that were dropped prior to sending due to ACL filtering.
> ipv4 input css down drop | The current total number of IP packets the CSS received and then dropped.
> ipv4 source violations | The current total number of IP packets received for which source violations were detected and then dropped.
> ipv4 source violations no accounting | The IP packets received for source violations that were detected but not included in the statistics.
> ipv4 source violation ignored | The IPv4 source validation violations that were detected and then ignored.
> ipv4 early pdu rcvd | The current total number of early IP packet data units (PDUs) received.
> QoS Statistics
> Class: Conversational | Specifies the statistics for use traffic of conversational QoS class along with traffic policing/shaping status.
> Downlink Negotiate Limit | Specifies whether traffic data QoS negotiation limit in downlink direction is enabled or not for this class of QoS in this APN.
> Uplink Negotiate Limit | Specifies whether traffic data QoS negotiation limit in uplink direction is enabled or not for this class of QoS in this APN.
> Peak Data Rate(in bps) | The peak data rate in bit per seconds for this class of QoS in this APN.
> Committed Data Rate(in bps) | The committed data rate in bit per seconds for this class of QoS in this APN.
> Downlink Rate Limit | Specifies whether traffic data rate limit in downlink direction is enabled or not for this class of QoS in this APN.
> Uplink Rate Limit | Specifies whether traffic data rate limit in uplink direction is enabled or not for this class of QoS in this APN.
> Burst Size | This group indicates the static/dynamic burst size in bytes for peak and guaranteed rate limiting for this class of QoS in this APN.
> Auto Readjust | Indicates whether auto readjustment of burst size is enabled or not. Possible states are:
> • | Enabled
> • | Disabled
> Auto Readjust Duration | Indicates the configured auto readjust duration in a seconds. If auto readjust is enabled and no readjust duration is specified the default value is 1 second.
> Peak Burst Size(bytes) | Indicates the peak burst size in bytes calculated dynamically by auto readjust duration and rate limit value.
> Guaranteed Burst Size(bytes) | Indicates the guaranteed burst size in bytes calculated dynamically by auto readjust duration (seconds) and rate limit value (bytes). This counter is applicable only when auto readjustment is enabled.
> Exceed Action | Specifies the action on downlink/uplink data rate when exceeds the allowed rate limit for this class of QoS. Possible actions are:
> • | drop: drop the packets.
> • | lower-ip-precedence: transmit the packet after lowering the ip-precedence.
> • | transmit: transmit the packet.
> Violate Action | Specifies the action on downlink/uplink data rate violation of allowed rate limit for this class of QoS. Possible actions are:
> • | drop: drop the packets.
> • | lower-ip-precedence: transmit the packet after lowering the ip-precedence.
> • | shape: enables the traffic shaping and provides the buffering of user packets when subscriber traffic violates the allowed peak/committed data rate.
> • | shape-transmit-when-buffer-full: enables the traffic shaping and allows the packet to be transmitted when buffer memory is full.
> • | transmit: transmit the packet.
> Class: Streaming | Specifies the statistics for use traffic of streaming QoS class along with traffic policing/shaping status.
> Class: Interactive | Specifies the statistics for use traffic of interactive QoS class along with traffic policing/shaping status. It showed for the traffic handling priority 1 through 3.
> Traffic Handling Priority | Specifies the traffic handling priority for interactive QoS class along with traffic policing/shaping status. Possible values are priority 1 through 3.
> Class: Background | Specifies the statistics for use traffic of background QoS class along with traffic policing/shaping status.
> IP address allocation statistics:
> ip type static | The current total number of PDP contexts facilitated by the APN that used static IP address.
> ip type local pool | The current total number of PDP contexts facilitated by the APN that were dynamically assigned IP addresses from pools configured locally on the system.
> ip type radius | The current total number of PDP contexts facilitated by the APN that were dynamically assigned IP addresses from a RADIUS server.
> ip type dhcp proxy | The current total number of PDP contexts facilitated by the APN that were dynamically assigned IP addresses by the system using the DHCP client mode.
> ip type dhcp relay | The current total number of PDP contexts facilitated by the APN that were dynamically assigned IP addresses by the system using the DHCP relay mode.
> ip type no allocation | The current total number of PDP contexts facilitated by the APN that were not dynamically allocated IP addresses. This counters is relevant for a multicast sessions (MBMS) where IP allocation is not applicable.
> Session statistics
> current contexts (selected APN(s)) | The current total number of PDP contexts facilitated by the APN.
> current contexts (system wide) | The current total number of PDP contexts facilitated by the entire system.
> cumulative contexts (selected APN(s)) | The cumulative number of PDP contexts facilitated by the APN.
> cumulative contexts (system wide) | The cumulative number of PDP contexts facilitated by the entire system.
> Current APN context load | The current percent utilization of the APN as function of the APN’s configured maximum number of supported PDP contexts and the current total number of PDP contexts facilitated by the APN.
> Cumulative APN context load | The cumulative percent utilization of the APN as function of the APN’s configured maximum number of supported PDP contexts and the cumulative number of PDP contexts facilitated by the APN.
> AAA Counters
> Authentication Counters
> Access-Request Sent | The total number of access requests that were sent.
> Access-Request Timeouts | The total number of access request timeouts.
> Accounting Counters
> Accounting-Request Sent | The total number of accounting requests that were sent.
> Accounting-Response Received | The total number of accounting responses that were received.
> Accounting-Request Timeouts | The total number of accounting request timeouts.
> RADIUS Acct-Req purged | The total number of RADIUS accounting requests purged.
> GTPP Acct-req purged | The total number of GTTP accounting requests purged.
> GTPP sec Acct-req purged | The total number of secondary G-CDR accounting requests being processed and purged by this AAAMgr instance for which the GTPP protocol is being used to deliver the accounting message to the Charging Gateway Function (CGF) . It counts total secondary G-CDR accounting requests purged by this AAAMgr instance
> GTPP Chrg-req purged | The total number of GTTP charging requests purged.
> GTPP sec Chrg-req purged | The total number of secondary eG-CDR charging requests being processed and purged by this AAAMgr instance for which the GTPP protocol is being used to deliver the charging message to the Charging Gateway Function (CGF) . It counts total secondary eG-CDR charging requests purged by this AAAMgr instance

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883