> Supported Registration Reply Codes
> Each of the three sections that follow describe the registration reply codes supported by thesystem for the PDSN and FA services.
> PDSN Service Reply Codes
> The following registration reply codes are supported by the system’s PDSN service inaccordance with the 3GPP2 A.S0001-A v2: 3GPP2 Access Network InterfacesInteroperability Specification (also known as 3G-IOS v4.1.1).
> Supported PDSN Service Registration Reply Codes

> Reply Code(Hex / Base 10) | Description | Notes
> 00H / 0 | Registration Accepted | Sent when he subscriber session is successfully set up.
> 80H / 128 | Registration Denied - reason unspecified | Sent when internal errors are encountered when processing the Request packet.
> 81H / 129 | Registration Denied - administratively prohibited | Sent when a newcall policy is set to reject.
> 82H / 130 | Registration Denied - insufficient resources | Sent when no memory or session managers are available to process the session.
> 83H / 131 | Registration Denied - mobile node failed authentication | Sent when the mobile node failed authentication. When multiple errors occur on authentication this message takes precedence and is listed first.
> 85H / 133 | Registration Denied - identification mismatch | Sent when the PCF's timestamp does not match the PDSN. The PDSN sends a corrected timestamp to be used as the ID by the PCF in subsequent requests.
> 86H / 134 | Registration Denied - poorly formed request | Sent when an unsupported Service option is received or the packet is malformed in any way.
> 88H / 136 | Registration Denied - unknown PDSN address | Sent when PDSN redirect policy is invoked.
> 89H / 137 | Registration Denied - requested reverse tunnel unavailable | Sent when reverse tunneling is requested by the mobile node but it is not enabled on the system.
> 8AH / 138 | Registration Denied - reverse tunnel is mandatory and ‘T’ bit not set | Sent when reverse tunneling is enabled on the system but is not supported by the mobile node.
> 8DH / 139 | Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE | Sent when the Airlink records from the PCF contain a Vendor ID value other than 0x159F or the Accounting VSE contains an Application Sub Type other than RADIUS or the Request contains a Critical Vendor Specific Extension Type that is not recognized by the PDSN.

> ‌
> FA Service Reply Codes
> The following registration reply codes are supported by the system’s FA service inaccordance with the following Request For Comments (RFCs):

> • | RFC-2002, IPv4 Mobility, May 1995

> • | RFC-2344, Reverse Tunneling for Mobile IP, May 1998

> • | RFC-2794, Mobile IP Network Access Identifier Extension for IPv4, March 2000

> • | RFC-3012, Mobile IPv4 Challenge/Response Extensions, November 2000

> Supported PDSN Service Registration Reply Codes

> Reply Code(Hex / Base 10) | Description | Notes
> 40H / 64 | Registration Denied - reason unspecified | Sent when internal errors are encountered when processing the Request packet.
> 41H / 65 | Registration Denied - administratively prohibited | Sent when a newcall policy is set to reject calls or the subscriber us not permitted to use Mobile IP FA services.
> 42H / 66 | Registration Denied - insufficient resources | Sent when no memory or session managers are available to process the session.
> 43H / 67 | Registration Denied - mobile node failed authentication | Sent when the mobile node failed authentication.
> 44H / 68 | Registration Denied - home agent failed authentication | Sent when an HA attempted to communicate with the FA service using an incorrect security parameter index (SPI).
> 45H / 69 | Registration Denied - requested lifetime too long | Sent when the mobile node requests a registration lifetime longer than the maximum supported by the FA.
> 46H / 70 | Registration Denied - poorly formed request | Sent when the registration request is poorly formed (i.e. missing an Authentication extension).
> 47H / 71 | Registration Denied - poorly formed reply | Sent when the registration reply is poorly formed (i.e. missing an Authentication extension).
> 48H / 72 | Registration Denied - requested encapsulation unavailable | Sent when requested encapsulation type is unavailable (GRE or minimal IP encapsulation).
> 4AH / 74 | Registration Denied - reverse tunneling unavailable | Sent when reverse tunneling is requested by the mobile node but it is not enabled on the system.
> 4BH / 75 | Registration Denied - reverse tunneling mandatory | Sent when reverse tunneling is enabled on the system but is not supported by the mobile node.
> 4CH / 76 | Registration Denied - reverse tunneling mobile node too distant | Sent when IP TTL is not set to 255 in Reg Request with T bit set
> 4DH / 77 | Registration Denied - invalid care-of address | Sent when D bit is set in the Registration Request.
> 4EH / 78 | Registration Denied - registration timeout | Sent when FA reg-timeout is exceeded.
> 4FH / 79 | Registration Denied - reverse tunneling delivery style unavailable | Sent if the Encapsulating Delivery Style Extension sent by the mobile is not supported by the FA service.
> 50H / 80 | Registration Denied - home network unreachable (ICMP error received) | Sent when the FA service can not contact the home network due to an Internet Control Message Protocol (ICMP) error.
> 51H / 81 | Registration Denied - home agent host unreachable (ICMP error received) | Sent when the FA service can not contact the HA host due to an Internet Control Message Protocol (ICMP) error.
> 52H / 82 | Registration Denied - home agent port unreachable (ICMP error received) | Sent when the FA service can not contact the HA port due to an Internet Control Message Protocol (ICMP) error.
> 58H / 88 | Registration Denied - home agent unreachable (other ICMP error received) | Sent when the FA service can not contact the HA due to an Internet Control Message Protocol (ICMP) error.
> 60H / 96 | Registration Denied - missing home address | Sent when the FA service could not determine the IP address of the mobile node.
> 61H / 97 | Registration Denied - missing NAI | Sent when the FA service could not determine the subscriber’s network access identifier.
> 62H / 98 | Registration Denied - missing home agent | Sent when the FA service could not determine the IP address of the mobile node’s home agent.
> 68H / 104 | Registration Denied - unknown challenge | Sent if the FA cannot validate the Mobile IP mobile-to-foreign agent advertisement challenge extension provided in the Registration Request.
> 69H / 105 | Registration Denied - missing challenge | Sent if the mobile node’s Registration Request does not include a mobile-to-foreign agent advertisement challenge extension.
> 6AH / 106 | Registration Denied - stale challenge | Sent when the mobile node has sent a Registration Request with a challenge value that was already used before.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883