> SGSN Schema Statistics
> The SGSN schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. The limit depends upon the counter data type.

> • | Gauge: A gauge statistic indicates a single value representative of a single instance. This type is often used to track particular events in time.

> Important: The format string syntax is described by “Schema Format String Syntax” in the Bulk Statistics Overview chapter.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615. All counter statistics are cumulative and reset only by one of the following methods: roll-over (as described above), after a system restart, or after a clear command is performed. All statistics are considered standards-based unless otherwise noted.
> The following variables are supported:
> SGSN Service Schema Statistics

> Statistic | Description | Data Type
> vpnname | Indicates the name of VPN context in which SGSN service is configured. This is a stat key variable. | String
> vpnid | Indicates the identifier of VPN context in which SGSN service is configured. This is a stat key variable. | Int32
> servname | Indicates the name of SGSN service for which these statistics are collected. This is a stat key variable. | String
> mcc | Indicates the mobile country code (MCC) of SGSN service for which these statistics are collected. This is a stat key variable. | Int32
> mnc | Indicates the mobile network code (MNC) of SGSN service for which these statistics are collected. This is a stat key variable. | Int32
> lac | Indicates the location area code (LAC) of SGSN service for which these statistics are collected. This is a stat key variable. | Int32
> rac | Indicates the routing area code (RAC) of SGSN service for which these statistics are collected. This is a stat key variable. | Int32
> 3G-attached | Description: Total number of subscribers, including home and visiting, attached for 3G service. Triggers: 1. Increments when a subscriber attaches to the SGSN. 2. Decrements when a subscriber detaches from the SGSN. Availability: per SGSN service, per RA Type: Gauge | Int32
> 2G-attached | Description: Total number of subscribers, including home and visiting, attached for 2G service. Triggers: 1. Increments when a subscriber attaches to the SGSN. 2. Decrements when a subscriber detaches from the SGSN. Availability: per GPRS service; per RA Type: Gauge | Int32
> 3G-home-subscribers | Indicates the total number of home subscribers attached for 3G service; where ‘home’ means the MCC and MNC of the IMSI are equal to the SGSN PLMN ID. Type: Gauge. | Int32
> 2G-home-subscribers | Indicates the total number of home subscribers attached for 2G service; where ‘home’ means the MCC and MNC of the IMSI are equal to the SGSN PLMN ID. Type: Gauge. | Int32
> 3G-visiting-national | Description: This proprietary gauge indicates the total number of attached subscribers (active and standby) whose MCC (from IMSI) matches with SGSN service’s MCC, but MNC is different from the SGSN service’s MNC for 3G service. Triggers: 1. Increments when a national subscriber attaches to the SGSN. 2. Decrements when a national subscriber detaches from the SGSN. Availability: per SGSN service, per RA Type: Gauge | Int32
> 2G-visiting-national | Description: This proprietary gauge indicates the total number of attached subscribers (active and standby) whose MCC (from IMSI) matches with GPRS service’s MCC, but MNC is different from the GPRS service’s MNC for 2G service. Triggers: 1. Increments when a national subscriber attaches to the SGSN. 2. Decrements when a national subscriber detaches from the SGSN. Availability: per GPRS service; per RA Type: Gauge | Int32
> 3G-visiting-foreign | Description: This proprietary gauge indicates the total number of attached subscribers (active and standby) whose MCC/MNC (from IMSI) does not match with the PLMN of the 3G SGSN service. Triggers: 1. Increments when a foreign subscriber attaches to the SGSN. 2. Decrements when a foreign subscriber detaches from the SGSN. Availability: per SGSN service, per RA Type: Gauge | Int32
> 2G-visiting-foreign | Description: This proprietary gauge indicates the total number of attached subscribers (active and standby) whose MCC/MNC (from IMSI) does not match with the PLMN of the 2G SGSN service. Triggers: 1. Increments when a subscriber establishes an Iu and completes the security procedure in it. 2. Decrements when a connected subscriber releases the Iu. Availability: per GPRS service; per RA Type: Gauge | Int32
> 3G-network-sharing-supp-ue | Description: This proprietary gauge indicates the total number of 3G Network Sharing Supporting User Equipment currently in the system. This statistics is specific to releases 8.1 and higher. Triggers: Increments when a network sharing supporting UE connects with the 3G SGSN. Availability: per SGSN service, per RA Type: Gauge | Int32
> 3G-network-sharing-non-supp-ue | Description: This proprietary gauge indicates the total number of 3G Network Sharing Non-supporting User Equipment currently in the system. This statistics is specific to releases 8.1 and higher. Triggers: Increments when a network sharing non-supporting UE connects with the 3G SGSN. Availability: per SGSN service, per RA Type: Gauge | Int32
> pmm-connected | Description: Total number of subscribers in packet mobility management-connected (PMM-CONNECTED) state. Triggers: 1. Increments when a subscriber attaches to the SGSN. 2. Decrements when a subscriber detaches from the SGSN. Availability: per SGSN service, per RA Type: Gauge | Int32
> pmm-idle | Total number of subscribers in packet mobility management-idle (PMM-IDLE) mode. Type: Gauge | Int32
> gprs-standby | Total number of GPRS subscribers in standby mode. Type: Gauge | Int32
> gprs-ready | Total number of GPRS subscribers in ready mode. Type: Gauge | Int32
> 3G-attached-with-pdp | Description: Total number of 3G visiting and home subscribers in attached state with at least one active PDP context. Triggers: This gauge changes after successful activation of the first PDP context for a subscriber. Availability: per SGSN service, per RA Type: Gauge | Int32
> 2G-attached-with-pdp | Description: Total number of 2G visiting and home subscribers in attached state with at least one active PDP context per GPRS service. Triggers: This gauge changes after successful activation of the first PDP context for a subscriber. Availability: per GPRS service Type: Gauge | Int32
> 3G-attached-no-pdp | This statistic has been obsoleted. | Int32
> 2G-attached-no-pdp | This statistic has been obsoleted. | Int32
> 3G-detached | Total number of subscribers in detached state with PDP context for 3G service. Type: Gauge | Int32
> 3G-total-attach-req-all | Total number of all types of 3G attach request messages on the SGSN service, including SGSN-only and combined attaches. Type: Counter | Int32
> 3G-total-attach-req | Total number of IMSI and P-TMSI 3G attach request messages for GPRS and IMSI (PS and CS). Type: Counter | Int32
> 3G-total-comb-attach-req | Total number of combined 3G attach request messages. Type: Counter | Int32
> 2G-total-attach-req-all | Total number of all types of 2G attach request messages on the GPRS service, including GPRS-only and combined attaches. Type: Counter | Int32
> 2G-total-attach-req | Total number of GPRS-only IMSI and P-TMSI attach request messages for GPRS and IMSI (PS and CS). Type: Counter | Int32
> 2G-total-comb-attach-req | Total number of combined 2G attach request messages. Type: Counter. | Int32
> 3G-IMSI-Attch | Total number of International Mobile Subscriber Identifier (IMSI) attach request messages for CS attach in 3G service. | Int32
> 3G-IMSI-Attch-Combined | Total number of IMSI and P-TMSI attach request messages for GPRS and IMSI (PS and CS) attach in 3G service. | Int32
> 2G-IMSI-Attch | Total number of IMSI attach request messages for CS in 2G service. | Int32
> 2G-IMSI-Attch-Combined | Total number of IMSI and P-TMSI attach request messages for GPRS and IMSI (PS and CS) attach in 2G service. | Int32
> 3G-ptmsi-Attch | Total number of Packet-Temporary Mobile Subscriber Identifier (P-TMSI) attach request messages for CS attach in 3G service. | Int32
> 3G-ptmsi-Attch-Combined | Total number of P-TMSI attach request messages for combined GPRS and IMSI (PS and CS) in 3G service. | Int32
> 3G-local-ptmsi-Attch | Total number of local P-TMSI attach request messages for CS attach in 3G service. Type: Counter | Int32
> 3G-local-ptmsi-Attch-comb | Total number of local P-TMSI attach request messages for combined PS and CS attach in 3G service. Type: Counter. | Int32
> 3G-remote-ptmsi-Attch | Total number of remote P-TMSI attach request messages for CS in 3G service. Type: Counter. | Int32
> 3G-remote-ptmsi-Attch-comb | Total number of remote P-TMSI attach request messages for combined PS and CS attach in 3G service. Type: Counter. | Int32
> 2G-ptmsi-Attch | Total number of P-TMSI attach request messages for CS attach in 2G service. | Int32
> 2G-ptmsi-Attch-Combined | Total number of P-TMSI attach request messages for combined GPRS and IMSI (PS and CS) in 2G service. | Int32
> 2G-local-ptmsi-Attch | Total number of remote P-TMSI attach request messages for CS in 2G service. | Int32
> 2G-local-ptmsi-Attch-comb | Total number of local P-TMSI attach request messages for combined GPRS and IMSI (PS and CS) in 2G service. | Int32
> 2G-remote-ptmsi-Attch | Total number of remote P-TMSI attach request messages for CS in 2G service. | Int32
> 2G-remote-ptmsi-Attch-comb | Total number of remote P-TMSI attach request messages for combined GPRS and IMSI (PS and CS) in 2G service. | Int32
> 3G-ret-imsi-attach | Total number of IMSI attach request messages retransmitted for 3G service. | Int32
> 3G-ret-imsi-attach-comb | Total number of IMSI attach request messages retransmitted for combined GPRS and IMSI (PS and CS) in 3G service. | Int32
> 2G-ret-imsi-attach | Total number of IMSI attach request messages retransmitted for 2G service. | Int32
> 2G-ret-imsi-attach-comb | Total number of IMSI attach request messages retransmitted for combined GPRS and IMSI (PS and CS) in 2G service. | Int32
> 3G-ret-local-ptmsi-attach | Total number of local-P-TMSI attach request messages retransmitted for 3G service. | Int32
> 3G-ret-local-ptmsi-attach-comb | Total number of local P-TMSI attach request messages retransmitted for combined GPRS and IMSI (PS and CS) in 3G service. | Int32
> 2G-ret-local-ptmsi-attach | Total number of local-P-TMSI attach request messages retransmitted for 2G service. | Int32
> 2G-ret-local-ptmsi-attach-comb | Total number of local P-TMSI attach request messages retransmitted for combined GPRS and IMSI (PS and CS) in 2G service. | Int32
> 3G-ret-remote-ptmsi-attach | Total number of remote P-TMSI attach request messages retransmitted for 3G service. | Int32
> 3G-ret-remote-ptmsi-attach-comb | Total number of remote P-TMSI attach request messages retransmitted for combined GPRS and IMSI (PS and CS) in 3G service. | Int32
> 2G-ret-remote-ptmsi-attach | Total number of remote P-TMSI attach request messages retransmitted for 2G service. | Int32
> 2G-ret-remote-ptmsi-attach-comb | Total number of remote P-TMSI attach request messages retransmitted for combined GPRS and IMSI (PS and CS) in 2G service. | Int32
> 3G-attach-accept | Description: Total number of Attach Request messages accepted for 3G service. Triggers: On sending a successful attach-accept with attach-result “GPRS-only Attached”. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-comb-attach-accept | Description: Total number of Attach Accept messages sent with attach result “Combined GPRS/IMSI Attached” in 3G service. Triggers: On sending a successful attach-accept with attach-result “Combined attached”. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-ret-attach-accept | Total number of attach request accept messages retransmitted for 3G service. | Int32
> 3G-ret-attach-accept-comb | Total number of combined (GPRS and IMSI) attach request accept messages retransmitted for 3G service. | Int32
> 2G-attch-accept | Description: Total number of Attach Request messages accepted for 2G service. Triggers: On sending a successful attach-accept with attach-result “GPRS-only Attached”. Availability: per GPRS service Type: Counter | Int32
> 2G-comb-attch-accept | Description: Total number of Attach Accepts sends with attach-result “Combined GPRS/IMSI Attached” in 2G service. Triggers: On sending a successful attach-accept with attach-result “Combined attached”. Availability: per GPRS service Type: Counter | Int32
> 2G-ret-attch-accept | Total number of attach request accepted messages retransmitted for 2G service. | Int32
> 2G-ret-attch-accept-comb | Total number of combined (GPRS and IMSI) attach request accept messages retransmitted for 2G service. | Int32
> 3G-attach-complete | Total number of attach procedures completed for 3G service. | Int32
> 2G-attach-complete | Total number of attach procedures completed for 2G service. | Int32
> 3G-attach-reject-all | Total number of attach request messages rejected for for 3G service. | Int32
> 3G-attach-reject | Description: Total number of attach rejects sent with individual causes against attach request of type “GPRS Attach” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-attach-reject-comb | Description: Sum of all Attach-Reject counters with individual causes sent against Attach Requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-reject-all | Total number of attach request messages rejected for for 2G service. | Int32
> 2G-attach-reject | Description: Total number of Attach Rejects sent with individual causes against Attach Requests of type “GPRS Attach” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 2G-attach-reject-comb | Description: Sum of all Attach-Reject counters with individual causes sent against Attach requests of type "Combined GPRS/IMSI Attach" in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-imsi-unknown-at-hlr | Description: Total number of Attach Rejects sent with cause "imsi unknown at hlr" against Attach requests of type "GPRS Attach" in 3G service. Triggers:
> • | On HLR sending a bad response to an SAI-Req or a GLU-Req.
> • | On getting zero auth vectors for HLR for a SAI-Req.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-imsi-unknown-at-hlr | Description: Total number of Attach Rejects sent with cause "imsi unknown at hlr" against Attach requests of type "GPRS Attach" in 2G service. Triggers:
> • | On HLR sending a bad response to an SAI-Req or a GLU-Req.
> • | On HLR getting zero auth vectors for a SAI-Req.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-illegal-ms | Total number of attach requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-attach-rej-illegal-ms | Total number of attach requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-attach-rej-illegal-me | Total number of attach requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-attach-rej-illegal-me | Total number of attach requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-gprs-service-not-allowed | Description: Total number of attach rejects sent with cause "GPRS Services not allowed" against Attach requests of type "GPRS Attach" in 3G service. Triggers: 1. On getting a cl (subs-with) while a RAU/attach is in progress. 2. On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req. 3. For rejecting attaches due to subscriber control inactivity. 4. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-gprs-service-not-allowed | Description: Total number of attach rejects sent with cause "GPRS Services not allowed" against Attach requests of type "GPRS Attach" in 3G service. Triggers: 1. On getting a cl (subs-with) while a RAU/attach is in progress. 2. On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req. 3. For rejecting attaches due to subscriber control inactivity. 4. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service. Type: Counter | Int32
> 3G-gprs-and-non-gprs-service-not-allowed | Description: Total number of attach rejects sent with cause "GPRS and non-GPRS Services not allowed" against Attach requests of type "GPRS Attach" in 3G service. Triggers:
> • | On getting "IMSI unknown" from HLR for SAI-Req/GLU-Req.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-gprs-and-non-gprs-service-not-allowed | Description: Total number of attach rejects sent with cause "GPRS and non-GPRS Services not allowed" against Attach requests of type "GPRS Attach" in 2G service. Triggers:
> • | On getting "IMSI unknown" from HLR for SAI-Req/GLU-Req.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-msid-not-derived-by-nwt | Description: Total number of Attach Rejects sent with cause "msid not derived by nwt" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | On getting periodic RAU with old RAI as a non-local RAI.
> • | When PTMSI-IE is missing in RAU.
> • | When old RAI has invalid location area values (0x0000 or 0xfffe) for PTMSI-attaches/RAUs.
> • | When getting a RAU with old RAI in 2G and PTMSI is unknown.
> • | When getting PTMSI-SIG-MISMATCH SGSN Context Request sent with IMSI Validated.
> • | When getting a RAU Request while an attach with the same peer-SGSN-PTMSI is in progress.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-msid-not-derived-by-nwt | Description: Total number of Attach Rejects sent with cause "msid not derived by nwt" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When SGSN-Context-Resp arrives with any cause other than “accepted".
> • | When GMM-Identity-Req with MS fails.
> • | When GTP-Identity-Req with MS fails.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-implicitly-detach | Description: Total number of attach requests rejected with cause "implicitly detached" against Attach requests of type "GPRS Attach" in 3G service. Triggers:
> • | RAU at 3G when subscriber was detached from 2G.
> • | When we get a different IMSI in SGSN Context Response for an SGSN Context Request sent with IMSI validated.
> • | When we get RAU while awaiting a Detach Accept.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-implicitly-detach | Description: Total number of attach requests rejected with cause "implicitly detached" against Attach requests of type "GPRS Attach" in 2G service. Triggers:
> • | When we get an RAU from an unknown MS.
> • | On T3350 expiry for the attach-accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-plmn-not-allowed | Description: Total number of Attach Rejects sent with cause "plmn not allowed" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-plmn-not-allowed | Description: Total number of Attach Rejects sent with cause "plmn not allowed" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-la-not-allowed | Total number of GPRS attach rejected for 3G service due to specific location area not allowed. | Int32
> 2G-attach-rej-la-not-allowed | Total number of GPRS attach rejected for 2G service due to specific location area not allowed. | Int32
> 3G-roaming-not-allowed-in-this-location-area | Description: Total number of attach rejects sent with cause “Roaming not allowed in this Location Area” against attach requests of type “GPRS Attach” in 3G service. Triggers: 1. When rejecting as a shared SGSN as operator not accepting the given IMSI. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-roaming-not-allowed-in-this-location-area | Description: Total number of attach rejects sent with cause “Roaming not allowed in this Location Area” against attach requests of type “GPRS Attach” in 2G service. Triggers: When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-gprs-service-not-allowed-in-this-plmn | Description: Total number of attach rejects sent with cause “GPRS services not allowed in this PLMN” against attach requests of type “GPRS Attach” in 3G service. Triggers: 1. On getting "Roaming Not allowed" from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-gprs-service-not-allowed-in-this-plmn | Description: Total number of attach rejects sent with cause “GPRS services not allowed in this PLMN” against attach requests of type “GPRS Attach” in 2G service. Triggers: 1. On getting "Roaming not allowed" from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-no-suitable-cells-in-location-area | Description: Total number of attach rejects sent with cause "No suitable cell in location area" against Attach requests of type "GPRS Attach" in 3G service. Triggers: 1. On getting "UMTS Access Control” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-no-suitable-cells-in-location-area | Description: Total number of attach rejects sent with cause "No suitable cell in location area" against Attach requests of type "GPRS Attach" in 2G service. Triggers: 1. On getting "UMTS Access Control” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-msc-not-reachable | Total number of GPRS attach rejected for 3G service as MSC not reachable. | Int32
> 2G-attach-rej-msc-not-reachable | Total number of GPRS attach rejected for 2G service as MSC not reachable. | Int32
> 3G-attach-rej-network-failure | Description: Total number of attach rejects sent with cause "Network Failure" against Attach requests of type "GPRS Attach" in 3G service. Triggers: 1. RNC is overloaded. 2. Not enough credits at session manager. 3. On getting cause “data missing from HLR” in SAI-Req/GLU-Req. 4. Too many IU’s for the same IMSI. 5. On congestion, if configured for attach-throttling. 6. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-network-failure | Description: Total number of attach rejects sent with cause "Network Failure" against Attach requests of type "GPRS Attach" in 3G service. Triggers: 1. RNC is overloaded. 2. Not enough credits at session manager. 3. On getting cause “data missing from HLR” in SAI-Req/GLU-Req. 4. Too many IU’s for the same IMSI. 5. On congestion, if configured for attach-throttling. 6. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-mac-failure | Total number of GPRS attach rejected for 3G service due to message authenticate code (MAC) failure. | Int32
> 2G-attach-rej-mac-failure | Total number of GPRS attach rejected for 2G service due to MAC failure. | Int32
> 3G-attach-rej-sync-failure | Description: Total number of Attach Rejects sent with cause "sync failure" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-sync-failure | Description: Total number of Attach Rejects sent with cause "sync failure" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-congestion | Description: Total number of attach rejects sent with cause “Congestion” against attach request of type “GPRS Attach” in a 3G service. Triggers:
> • | On congestion, if configured for attach-throttling.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-congestion | Description: Total number of GPRS attach rejected for 2G service due to network congestion. Triggers:
> • | On congestion, if configured for attach-throttling.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-gsm-auth-unacceptable | Description: Total number of Attach Rejects sent with cause "gsm auth unacceptable" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-gsm-auth-unacceptable | Description: Total number of Attach Rejects sent with cause "gsm auth unacceptable" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-no-pdp-ctx-activated | Description: Total number of Attach Rejects sent with cause "no pdp ctx activated" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-no-pdp-ctx-activated | Description: Total number of Attach Rejects sent with cause "no pdp ctx activated" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-retry-from-new-cell | Description: Total number of Attach Rejects sent with cause "retry from new cell" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-retry-from-new-cell | Description: Total number of Attach Rejects sent with cause "retry from new cell" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-sem-wrong-msg | Description: Total number of Attach Rejects sent with cause "sem wrong msg" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-sem-wrong-msg | Description: Total number of Attach Rejects sent with cause "sem wrong msg" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-invalid-mand-info | Description: Total number of Attach Rejects sent with cause "invalid mand info" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-invalid-mand-info | Description: Total number of Attach Rejects sent with cause "invalid mand info" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-msg-type-not-exist | Description: Total number of Attach Rejects sent with cause "msg type not exist" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-msg-type-not-exist | Description: Total number of Attach Rejects sent with cause "msg type not exist" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-msg-type-not-comp-prot-state | Description: Total number of Attach Rejects sent with cause "msg type not comp prot state" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-msg-type-not-comp-prot-state | Description: Total number of Attach Rejects sent with cause "msg type not comp prot state" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-ie-non-existent | Description: Total number of Attach Rejects sent with cause "ie non existent" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-ie-non-existent | Description: Total number of Attach Rejects sent with cause "ie non existent" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-conditional-ie-err | Description: Total number of Attach Rejects sent with cause "conditional ie err" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-conditional-ie-err | Description: Total number of Attach Rejects sent with cause "conditional ie err" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-msg-not-comp-prot-state | Description: Total number of Attach Rejects sent with cause "msg not comp prot state" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an Attach Request before getting Relocation-complete during SRNS.
> • | When getting periodic RAU in a direct transfer message.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-msg-not-comp-prot-state | Description: Total number of Attach Rejects sent with cause "msg not comp prot state" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-protocol-error | Description: Total number of Attach Rejects sent with cause "protocol error" against Attach Requests of type "GPRS Attach" in 3G service. Triggers:
> • | When getting an appropriate decode error.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-protocol-error | Description: Total number of Attach Rejects sent with cause "protocol error" against Attach Requests of type "GPRS Attach" in 2G service. Triggers:
> • | When the PLMN-id in BSSGP message does not match the configured PLMN at GPRS-service.
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-rej-unknown-cause | Description: Total number of Attach Rejects sent with cause "unknown cause" against Attach Requests of type "GPRS Attach" in 3G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-rej-unknown-cause | Description: Total number of Attach Rejects sent with cause "unknown cause" against Attach Requests of type "GPRS Attach" in 2G service. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-attach-rej-imsi-unknown-at-hlr | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service due to IMSI not known at HLR. | Int32
> 2G-comb-attach-rej-imsi-unknown-at-hlr | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service due to IMSI not known at HLR. | Int32
> 3G-comb-attach-rej-illegal-ms | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-comb-attach-rej-illegal-ms | Total number of combined (GPRS and IMSI) attach requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-comb-attach-rej-illegal-me | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-comb-attach-rej-illegal-me | Total number of combined (GPRS and IMSI) attach requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-comb-gprs-service-not-allowed | Description: Total number of attach rejects sent with cause "GPRS services not allowed" against attach requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: 1. On getting a cl (subs-with) while a RAU/attach is in progress. 2. On getting “Subscriber Unknown” failure from hlr for glu/sai-req. 3. For rejecting attaches due to subscriber-control-inactivity. 4. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-gprs-service-not-allowed | Description: Total number of attach rejects sent with cause "GPRS services not allowed" against attach requests of type "Combined GPRS/IMSI Attach" in 2G service. Triggers: 1. On getting a cl (subs-with) while a RAU/attach is in progress. 2. On getting “Subscriber Unknown” failure from hlr for glu/sai-req. 3. For rejecting attaches due to subscriber-control-inactivity. 4. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-gprs-and-non-gprs-svc-not-allow | Description: Total number of attach rejects sent with cause "GPRS and non-GPRS services not allowed" against attach requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: 1. On getting “Imsi unknown” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-gprs-and-non-gprs-svc-not-allow | Description: Total number of attach rejects sent with cause "GPRS and non-GPRS services not allowed" against attach requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: 1. On getting “Imsi unknown” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-attach-rej-msid-not-derived-by-nwt | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service as network failed to derive MSID from request message. | Int32
> 2G-comb-attach-rej-msid-not-derived-by-nwt | Total number of combined (GPRS and IMSI) attach requests rejected for 2G service as network failed to derive MSID from request message. | Int32
> 3G-comb-attach-rej-implicitly-detach | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service as subscriber implicitly detached from network. | Int32
> 2G-comb-attach-rej-implicitly-detach | Total number of combined (GPRS and IMSI) attach requests rejected for 3G service as subscriber implicitly detached from network. | Int32
> 3G-comb-attach-rej-plmn-not-allowed | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to specific PLMN not allowed. | Int32
> 2G-comb-attach-rej-plmn-not-allowed | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to specific PLMN not allowed. | Int32
> 3G-comb-attach-rej-la-not-allowed | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to specific location area not allowed. | Int32
> 2G-comb-attach-rej-la-not-allowed | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to specific location area not allowed. | Int32
> 3G-comb-roam-not-allow-in-loc-area | Description: Total number of attach rejects sent with cause “Roaming not allowed in LA” against attached request of type “Combined GPRS/IMSI Attach” in 3G service. Triggers: 1. When rejecting as a shared SGSN due to no operator accepting the given IMSI. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-roam-not-allow-in-loc-area | Description: Total number of attach rejects sent with cause “Roaming not allowed in LA” against attached request of type “Combined GPRS/IMSI Attach” in 2G service. Triggers: When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-gprs-svc-not-allow-in-plmn | Description: Total number of attach rejects sent with cause "GPRS Service Not Allowed in PLMN" against attach requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-gprs-svc-not-allow-in-plmn | Description: Total number of attach rejects sent with cause "GPRS Service Not Allowed in PLMN" against attach requests of type "Combined GPRS/IMSI Attach" in 2G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-no-suitable-cells-in-loc-area | Description: Total number of attach rejects sent with cause “No suitable cells in LA” against Attach requests of type “Combined GPRS/IMSI Attach” in 3G service. Triggers: 1. On getting “UMTS access control” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-no-suitable-cells-in-loc-area | Description: Total number of attach rejects sent with cause “No suitable cells in LA” against Attach requests of type “Combined GPRS/IMSI Attach” in 2G service. Triggers: 1. On getting “UMTS access control” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-attach-rej-msc-not-reachable | Total number of combined (GPRS and IMSI) attach rejected for 3G service as MSC not reachable. | Int32
> 2G-comb-attach-rej-msc-not-reachable | Total number of combined (GPRS and IMSI) attach rejected for 2G service as MSC not reachable. | Int32
> 3G-comb-attach-rej-network-failure | Description: Total number of attach rejects sent with cause "Network Failure" against Attach requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: 1. On getting cause “data missing from HLR” in SAI-Req/GLU-Req. 2. On XID failure for RAU. 3. Inability to send an SGSN-CTX-Req out for an RAU. 4. Inability to send a Check-IMEI Request out. 5. On congestion, if configured for attach-throttling. 6. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-attach-rej-network-failure | Description: Total number of attach rejects sent with cause "Network Failure" against Attach requests of type "Combined GPRS/IMSI Attach" in 2G service. Triggers: 1. On getting cause “data missing from HLR” in SAI-Req/GLU-Req. 2. On XID failure for RAU. 3. Inability to send an SGSN-CTX-Req out for an RAU. 4. Inability to send a Check-IMEI Request out. 5. On congestion, if configured for attach-throttling. 6. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-attach-rej-mac-failure | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to message authenticate code (MAC) failure. | Int32
> 2G-comb-attach-rej-mac-failure | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to MAC failure. | Int32
> 3G-comb-attach-rej-sync-failure | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to context synchronization failure. | Int32
> 2G-comb-attach-rej-sync-failure | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to context synchronization failure. | Int32
> 3G-comb-attach-rej-congestion | Description: Total number of attach rejects sent with cause "Congestion" against Attach requests of type "Combined GPRS/IMSI Attach" in 3G service. Triggers: 1) On congestion, if configured for attach-throttling. 2) When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-attach-rej-congestion | Description: Total number of attach rejects sent with cause "Congestion" against Attach requests of type "Combined GPRS/IMSI Attach" in 2G service. Triggers: 1) On congestion, if configured for attach-throttling. 2) When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-attach-rej-gsm-auth-unacceptable | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to unacceptable authentication from GSM network. | Int32
> 2G-comb-attach-rej-gsm-auth-unacceptable | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to unacceptable authentication from GSM network. | Int32
> 3G-comb-attach-rej-no-pdp-ctx-activated | Total number of combined (GPRS and IMSI) attach rejected for 3G service as PDP context is not activated. | Int32
> 2G-comb-attach-rej-no-pdp-ctx-activated | Total number of combined (GPRS and IMSI) attach rejected for 2G service as PDP context is not activated. | Int32
> 3G-comb-attach-rej-retry-from-new-cell | Total number of combined (GPRS and IMSI) attach rejected for 3G service as subscriber retried the attach from new cell. | Int32
> 2G-comb-attach-rej-retry-from-new-cell | Total number of combined (GPRS and IMSI) attach rejected for 3G service as subscriber retried the attach from new cell. | Int32
> 3G-comb-attach-rej-sem-wrong-msg | Total number of combined (GPRS and IMSI) attach rejected for 3G service as attach request message is semantically wrong. | Int32
> 2G-comb-attach-rej-sem-wrong-msg | Total number of combined (GPRS and IMSI) attach rejected for 2G service as attach request message is semantically wrong. | Int32
> 3G-comb-attach-rej-invalid-mand-info | Total number of combined (GPRS and IMSI) attach rejected for 3G service as mandatory information in message is invalid. | Int32
> 2G-comb-attach-rej-invalid-mand-info | Total number of combined (GPRS and IMSI) attach rejected for 2G service as mandatory information in message is invalid. | Int32
> 3G-comb-attach-rej-msg-type-not-exist | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to non-existent type of message. | Int32
> 2G-comb-attach-rej-msg-type-not-exist | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to non-existent type of message. | Int32
> 3G-comb-attach-rej-msg-type-not-comp-pstate | Total number of combined (GPRS and IMSI) attach rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-comb-attach-rej-msg-type-not-comp-pstate | Total number of combined (GPRS and IMSI) attach rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-comb-attach-rej-ie-non-existent | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to error in conditional information element. | Int32
> 2G-comb-attach-rej-ie-non-existent | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to error in conditional information element. | Int32
> 3G-comb-attach-rej-conditional-ie-err | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to error in conditional information element. | Int32
> 2G-comb-attach-rej-conditional-ie-err | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to error in conditional information element. | Int32
> 3G-comb-attach-rej-msg-not-comp-prot-state | Total number of combined (GPRS and IMSI) attach rejected for 3G service as message is not compatible with protocol state. | Int32
> 2G-comb-attach-rej-msg-not-comp-prot-state | Total number of combined (GPRS and IMSI) attach rejected for 2G service as message is not compatible with protocol state. | Int32
> 3G-comb-attach-rej-protocol-error | Total number of combined (GPRS and IMSI) attach rejected for 3G service due to protocol error in message. | Int32
> 2G-comb-attach-rej-protocol-error | Total number of combined (GPRS and IMSI) attach rejected for 2G service due to protocol error in message. | Int32
> 3G-comb-attach-rej-unknown-cause | Total number of combined (GPRS and IMSI) attach rejected for 3G service where cause is unknown or not specified here. | Int32
> 2G-comb-attach-rej-unknown-cause | Total number of combined (GPRS and IMSI) attach rejected for 2G service where cause is unknown or not specified here. | Int32
> 3G-total-attach-fail | Description: Total number of attach requests of type “GPRS Attach” that were dropped from processing in 3G service. Triggers: 1. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. 2. Iu released while the attach procedure was in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-total-attach-fail-comb | Description: Total number of attach requests of type “Combined GPRS/IMSI Attach” that were dropped from processing in 3G service. Triggers: 1. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. 2. Iu released while the attach procedure was in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-total-attach-fail-all | Description: Sum of 3G-total-attach-fail + 3G-total-attach-fail-comb. Triggers: n/a Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-total-attach-fail | Description: Total number of attach requests of type “GPRS Attach” that were dropped from processing in 2G service. Triggers: Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service, per RA Type: Counter | Int32
> 2G-total-attach-fail-comb | Description: Total number of attach requests of type “Combined GPRS/IMSI Attach” that were dropped from processing in 2G service. Triggers: Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service, per RA Type: Counter | Int32
> 2G-total-attach-fail-all | Description: Sum of the stats for 2G-total-attach-fail + 2G-total-attach-fail-comb. This is new in release 9.0. Triggers: n/a Availability: per GPRS service, per RA Type: Counter | Int32
> 3G-attach-fail-iu_release | Total number of attach procedures failed for 3G service due to Iu interface release. | Int32
> 3G-attach-fail-ongoing-proc | Description: This proprietary counter indicates the total number of attach procedures failed for 3G service due to a new attach received. Triggers: Increments when we abort an ongoing attach due to another new attach in 3G. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-attach-fail-ongoing-proc | Description: This proprietary counter indicates the total number of Attach procedures failed for 2G service due to a new attach received. Triggers:
> • | Suspend during Attach procedure
> • | Radio-status lost during Attach procedure
> • | BVC-block during Attach procedure
> • | T3350 expiry during Attach procedure
> • | T3360 expiry during Attach procedure
> • | XID timer expiry during Attach procedure
> Availability: per GPRS service Type: Counter | Int32
> 3G-attach-fail-iu_release-comb | Total number of combined (GPRS and IMSI) attach procedures failed due to Iu released for 3G service. | Int32
> 3G-attach-fail-ongoing-proc-comb | Total number of combined (GPRS and IMSI) attach procedures failed due to on going attach procedures for 3G service. | Int32
> 2G-attach-fail-ongoing-proc-comb | Total number of combined (GPRS and IMSI) attach procedures failed due to on going attach procedures for 2G service. | Int32
> 3G-intra-rau | Total number of intra SGSN routing area updates received for 3G service. | Int32
> 2G-intra-rau | Total number of intra SGSN routing area updates received for 2G service. | Int32
> 3G-periodic-rau | Total number of periodic routing area updates received for 3G service. | Int32
> 2G-periodic-rau | Total number of periodic routing area updates received for 2G service. | Int32
> 3G-intra-comb-rau | Total number of intra SGSN combined (GPRS and IMSI) routing area updates received for 3G service. | Int32
> 2G-intra-comb-rau | Total number of intra SGSN combined (GPRS and IMSI) routing area updates received for 2G service. | Int32
> 3G-inter-sgsn-rau | Total packet switched inter-SGSN-RA update request messages for 3G service. | Int32
> 2G-inter-sgsn-rau | Total packet switched inter-SGSN-RA update request messages for 2G service. | Int32
> 3G-inter-sgsn-comb-rau | Total combined (GPRS and IMSI) inter-SGSN-RA update request messages for 3G service. | Int32
> 2G-inter-sgsn-comb-rau | Total combined (GPRS and IMSI) inter-SGSN-RA update request messages for 2G service. | Int32
> 3G-ret-intra-rau | Total routing area update request messages retransmitted for intra-SGSN RA updates for 3G. | Int32
> 2G-ret-intra-rau | Total routing area update request messages retransmitted for intra-SGSN RA updates for 2G. | Int32
> 3G-ret-periodic-rau | Total periodic intra-RA update messages retransmitted for 3G. | Int32
> 2G-ret-periodic-rau | Total periodic intra-RA update messages retransmitted for 2G. | Int32
> 3G-ret-inter-sgsn-rau | Total packet switched inter-SGSN-RA update request messages retransmitted for 3G service. | Int32
> 2G-ret-inter-sgsn-rau | Total packet switched inter-SGSN-RA update request messages retransmitted for 2G service. | Int32
> 3G-rau-accept-intra | Description: Sum of all RAU-Accepts sent against Intra-SGSN-RAU requests with update type “ RA Updating” in 3G service. Triggers: On sending a successful RAU-Accept with update-result “RA Updating”. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-comb-upd-rau-accept-intra | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU request with update type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: On sending a successful rau-accept with update-result "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach". Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-rau-accept-inter | Description: Sum of all RAU-Accepts sent against Inter-SGSN-RAU requests with update type “ RA Updating” in 3G service. Triggers: On sending a successful RAU-Accept with update-result “RA Updating”. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-comb-upd-rau-accept-inter | Description: Sum of all RAU-reject counters with individual causes against Inter-SGSN-RAU requests with update type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-rau-accept-intra | Description: Sum of all RAU-Accepts sent against Intra-SGSN-RAU requests with update type “ RA Updated” in 2G service. Triggers: On sending a successful RAU-Accept with update-result “RA Updated”. Availability: per GPRS service Type: Counter | Int32
> 2G-comb-upd-rau-accept-intra | Description: Sum of all RAU-reject counters with individual causes against Inra-SGSN-RAU requests with update type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: On sending a successful RAU-accept with update-result "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach". Availability: per GPRS service Type: Counter | Int32
> 2G-rau-accept-inter | Description: Sum of all RAU-Accepts sent against Inter-SGSN-RAU requests with update type “ RA Updated” in 2G service. Triggers: On sending a successful RAU-Accept with update-result “RA Updated”. Availability: per GPRS service Type: Counter | Int32
> 2G-comb-upd-rau-accept-inter | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU request with update type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 3G-rau-accept-periodic | Description: Sum of all RAU-Accepts sent against Intra-SGSN-RAU requests of type “Periodic Updating” with update type “RA updating” in 3G service. Triggers: On sending a successful RAU-Accept with update-result “Periodic Updating”. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-rau-accept-periodic | Description: Sum of all RAU-Accepts sent against Intra-SGSN-RAU requests of type “Periodic Updating” with update type “RA updated” in 2G service. Triggers: On sending a successful RAU-Accept with update-result “Periodic Updated”. Availability: per GPRS service Type: Counter | Int32
> 3G-ret-rau-accept-intra | Total number of intra-SGSN routing area update accept messages retransmitted for 3G service. | Int32
> 2G-ret-rau-accept-intra | Total number of intra-SGSN routing area update accept messages retransmitted for 2G service. | Int32
> 3G-ret-rau-accept-inter | Total number of inter-SGSN routing area update accept messages retransmitted for 3G service. | Int32
> 2G-ret-rau-accept-inter | Total number of inter-SGSN routing area update accept messages retransmitted for 2G service. | Int32
> 3G-ret-rau-accept-periodic | Total number of periodic routing area update accept messages retransmitted for 3G service. | Int32
> 2G-ret-rau-accept-periodic | Total number of periodic routing area update accept messages retransmitted for 2G service. | Int32
> 3G-rau-complete | Total number of routing area update complete messages for 3G service. | Int32
> 2G-rau-complete | Total number of routing area update complete messages for 2G service. | Int32
> 3G-rau-reject | Total number of routing area update reject messages for 3G service. | Int32
> 3G-intra-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU requests of type “RA Updating” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-periodic-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU requests of type “ Periodic RA Updating” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-inter-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Inter-SGSN-RAU requests of type “RA Updating” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-comb-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-comb-inter-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Inter-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-rau-reject | Total number of routing area update messages rejected for 2G service. | Int32
> 2G-intra-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU requests of type “RAU Updating” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 2G-periodic-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU requests of type “ Periodic RA Updating” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 2G-inter-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Inter-SGSN-RAU requests of type “RAU Updating” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 2G-comb-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Intra-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 2G-comb-inter-rau-reject | Description: Sum of all RAU-reject counters with individual causes against Inter-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per GPRS service Type: Counter | Int32
> 3G-rau-rej-imsi-unknown-hlr | This statistic has been deleted. | Int32
> 2G-rau-rej-imsi-unknown-hlr | This statistic has been deleted. | Int32
> 3G-rau-rej-illegal-ms | This statistic has been deleted. | Int32
> 2G-rau-rej-illegal-ms | This statistic has been deleted. | Int32
> 3G-rau-rej-illegal-me | This statistic has been deleted. | Int32
> 2G-rau-rej-illegal-me | This statistic has been deleted. | Int32
> 3G-rau-rej-gprs-svc-not-allow | This statistic has been deleted. | Int32
> 2G-rau-rej-gprs-svc-not-allow | This statistic has been deleted. | Int32
> 3G-rau-rej-gprs-and-nongprs-svc-not-allow | This statistic has been deleted. | Int32
> 2G-rau-rej-gprs-and-nongprs-svc-not-allow | This statistic has been deleted. | Int32
> 3G-rau-rej-msid-not-derived-by-nw | This statistic has been deleted. | Int32
> 2G-rau-rej-msid-not-derived-by-nw | This statistic has been deleted. | Int32
> 3G-rau-rej-implicitly-detach | This statistic has been deleted. | Int32
> 2G-rau-rej-implicitly-detach | This statistic has been deleted. | Int32
> 3G-rau-rej-plmn-not-allowed | This statistic has been deleted. | Int32
> 2G-rau-rej-plmn-not-allowed | This statistic has been deleted. | Int32
> 3G-rau-rej-location-area-not-allowed | This statistic has been deleted. | Int32
> 2G-rau-rej-location-area-not-allowed | This statistic has been deleted. | Int32
> 3G-rau-rej-roam-not-allowed-in-larea | This statistic has been deleted. | Int32
> 2G-rau-rej-roam-not-allowed-in-larea | This statistic has been deleted. | Int32
> 3G-rau-rej-gprs-svc-not-allowed-in-plmn | This statistic has been deleted. | Int32
> 2G-rau-rej-gprs-svc-not-allowed-in-plmn | This statistic has been deleted. | Int32
> 3G-rau-rej-no-cells-in-location-area | This statistic has been deleted. | Int32
> 2G-rau-rej-no-cells-in-location-area | This statistic has been deleted. | Int32
> 3G-rau-rej-msc-not-reachable | This statistic has been deleted. | Int32
> 2G-rau-rej-msc-not-reachable | This statistic has been deleted. | Int32
> 3G-rau-rej-network-failure | This statistic has been deleted. | Int32
> 2G-rau-rej-network-failure | This statistic has been deleted. | Int32
> 3G-rau-rej-mac-failure | This statistic has been deleted. | Int32
> 2G-rau-rej-mac-failure | This statistic has been deleted. | Int32
> 3G-rau-rej-syn-failure | This statistic has been deleted. | Int32
> 2G-rau-rej-syn-failure | This statistic has been deleted. | Int32
> 3G-rau-rej-congestion | This statistic has been deleted. | Int32
> 2G-rau-rej-congestion | This statistic has been deleted. | Int32
> 3G-rau-rej-gsm-auth-unacceptable | This statistic has been deleted. | Int32
> 2G-rau-rej-gsm-auth-unacceptable | This statistic has been deleted. | Int32
> 3G-rau-rej-no-pdp-ctx-actv | This statistic has been deleted. | Int32
> 2G-rau-rej-no-pdp-ctx-actv | This statistic has been deleted. | Int32
> 3G-rau-rej-retry-from-new-cell | This statistic has been deleted. | Int32
> 2G-rau-rej-retry-from-new-cell | This statistic has been deleted. | Int32
> 3G-rau-rej-sem-wrong-msg | This statistic has been deleted. | Int32
> 2G-rau-rej-sem-wrong-msg | This statistic has been deleted. | Int32
> 3G-rau-rej-inval-mand-info | This statistic has been deleted. | Int32
> 2G-rau-rej-inval-mand-info | This statistic has been deleted. | Int32
> 3G-rau-rej-msg-type-non-exist | This statistic has been deleted. | Int32
> 2G-rau-rej-msg-type-non-exist | This statistic has been deleted. | Int32
> 3G-rau-rej-mtype-not-compat-prot-state | This statistic has been deleted. | Int32
> 2G-rau-rej-mtype-not-compat-prot-state | This statistic has been deleted. | Int32
> 3G-rau-rej-ie-non-existent | This statistic has been deleted. | Int32
> 2G-rau-rej-ie-non-existent | This statistic has been deleted. | Int32
> 3G-rau-rej-cond-ie-error | This statistic has been deleted. | Int32
> 2G-rau-rej-cond-ie-error | This statistic has been deleted. | Int32
> 3G-rau-rej-msg-not-compat-prot-state | This statistic has been deleted. | Int32
> 2G-rau-rej-msg-not-compat-prot-state | This statistic has been deleted. | Int32
> 3G-rau-rej-prot-error | This statistic has been deleted. | Int32
> 2G-rau-rej-prot-error | This statistic has been deleted. | Int32
> 3G-rau-rej-unknown-error | This statistic has been deleted. | Int32
> 2G-rau-rej-unknown-error | This statistic has been deleted. | Int32
> 3G-intra-rau-rej-imsi-unknown-hlr | Total number of intra-SGSN routing area update requests rejected for 3G service due to unknown IMSI in HLR. | Int32
> 2G-intra-rau-rej-imsi-unknown-hlr | Total number of intra-SGSN routing area update requests rejected for 2G service due to unknown IMSI in HLR. | Int32
> 3G-intra-rau-rej-illegal-ms | Total number of intra-SGSN routing area update requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-intra-rau-rej-illegal-ms | Total number of intra-SGSN routing area update requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-intra-rau-rej-illegal-me | Total number of intra-SGSN routing area update requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-intra-rau-rej-illegal-me | Total number of intra-SGSN routing area update requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-intra-rau-rej-gprs-svc-not-allw | Total number of intra-SGSN routing area update requests rejected for 3G service due to GPRS service not allowed for subscriber. | Int32
> 2G-intra-rau-rej-gprs-svc-not-allw | Total number of intra-SGSN routing area update requests rejected for 2G service due to GPRS service not allowed for subscriber. | Int32
> 3G-intra-rau-rej-nongprs-svc-not-allow | Total number of intra-SGSN routing area update requests rejected for 3G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 2G-intra-rau-rej-nongprs-svc-not-allow | Total number of intra-SGSN routing area update requests rejected for 2G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 3G-intra-rau-rej-msid-not-derived-by-nw | Total number of intra-SGSN routing area update requests rejected for 3G service due to network failed to derive MSID from attach message. | Int32
> 2G-intra-rau-rej-msid-not-derived-by-nw | Total number of intra-SGSN routing area update requests rejected for 2G service due to network failed to derive MSID from attach message. | Int32
> 3G-intra-rau-rej-implicitly-detach | Total number of intra-SGSN routing area update requests rejected for 3G service due to implicitly detach. | Int32
> 2G-intra-rau-rej-implicitly-detach | Total number of intra-SGSN routing area update requests rejected for 2G service due to implicitly detach. | Int32
> 3G-intra-rau-rej-plmn-not-allowed | Total number of intra-SGSN routing area update requests rejected for 3G service due to specific PLMN not allowed. | Int32
> 2G-intra-rau-rej-plmn-not-allowed | The total intra-SGSN routing area update message rejected in intra-2G roaming due to specific PLMN not allowed. | Int32
> 3G-intra-rau-rej-loc-area-not-allow | Total number of intra-SGSN routing area update requests rejected for 3G service due to specific location area not allowed. | Int32
> 2G-intra-rau-rej-loc-area-not-allow | Total number of intra-SGSN routing area update requests rejected for 2G service due to specific location area not allowed. | Int32
> 3G-intra-rau-rej-roam-not-allow-larea | Total number of intra-SGSN routing area update requests rejected for 3G service due to roaming not allowed in specific location area. | Int32
> 2G-intra-rau-rej-roam-not-allow-larea | Total number of intra-SGSN routing area update requests rejected for 2G service due to roaming not allowed in specific location area. | Int32
> 3G-intra-rau-rej-gprs-svc-not-allow-plmn | Description: Total number of RAU rejects sent with cause “GPRS service not allowed in this PLMN” against Intra-SGSN-RAU requests of type “RA Updating” in 3G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-rau-rej-gprs-svc-not-allow-plmn | Description: Total number of RAU rejects sent with cause “GPRS service not allowed in this PLMN” against Intra-SGSN-RAU requests of type “RA Updating” in 2G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-rau-rej-no-cells-in-loc-area | Total number of intra-SGSN routing area update requests rejected for 3G service due to non availability of suitable cell in specific location area. | Int32
> 2G-intra-rau-rej-no-cells-in-loc-area | Total number of intra-SGSN routing area update requests rejected for 2G service due to non availability of suitable cell in specific location area. | Int32
> 3G-intra-rau-rej-msc-not-reachable | Total number of intra-SGSN routing area update requests rejected for 3G service as MSC not reachable. | Int32
> 2G-intra-rau-rej-msc-not-reachable | Total number of intra-SGSN routing area update requests rejected for 2G service as MSC not reachable. | Int32
> 3G-intra-rau-rej-network-failure | Total number of intra-SGSN routing area update requests rejected for 3G service due to network failure. | Int32
> 2G-intra-rau-rej-network-failure | Total number of intra-SGSN routing area update requests rejected for 2G service due to network failure. | Int32
> 3G-intra-rau-rej-mac-failure | Total number of intra-SGSN routing area update requests rejected for 3G service due to message authenticate code (MAC) failure. | Int32
> 2G-intra-rau-rej-mac-failure | Total number of intra-SGSN routing area update requests rejected for 2G service due to MAC failure. | Int32
> 3G-intra-rau-rej-syn-failure | Total number of intra-SGSN routing area update requests rejected for 3G service due to context synchronization failure. | Int32
> 2G-intra-rau-rej-syn-failure | Total number of intra-SGSN routing area update requests rejected for 2G service due to context synchronization failure. | Int32
> 3G-intra-rau-rej-congestion | Total number of intra-SGSN routing area update requests rejected for 3G service due to network congestion. | Int32
> 2G-intra-rau-rej-congestion | Total number of intra-SGSN routing area update requests rejected for 2G service due to network congestion. | Int32
> 3G-intra-rau-rej-gsm-auth-unacceptable | Total number of intra-SGSN routing area update requests rejected for 3G service due to unacceptable authentication from GSM network. | Int32
> 2G-intra-rau-rej-gsm-auth-unacceptable | Total number of intra-SGSN routing area update requests rejected for 2G service due to unacceptable authentication from GSM network. | Int32
> 3G-intra-rau-rej-no-pdp-ctx-actv | Total number of intra-SGSN routing area update requests rejected for 3G service as PDP context is not activated. | Int32
> 2G-intra-rau-rej-no-pdp-ctx-actv | Total number of intra-SGSN routing area update requests rejected for 2G service as PDP context is not activated. | Int32
> 3G-intra-rau-rej-retry-from-new-cell | Total number of intra-SGSN routing area update requests rejected for 3G service as subscriber retried for update from new cell. | Int32
> 2G-intra-rau-rej-retry-from-new-cell | Total number of intra-SGSN routing area update requests rejected for 2G service as subscriber retried for update from new cell. | Int32
> 3G-intra-rau-rej-inval-mand-info | Total number of intra-SGSN routing area update requests rejected for 3G service as mandatory information in message is invalid. | Int32
> 2G-intra-rau-rej-inval-mand-info | Total number of intra-SGSN routing area update requests rejected for 2G service as mandatory information in message is invalid. | Int32
> 3G-intra-rau-rej-msg-type-non-exist | Total number of intra-SGSN routing area update requests rejected for 3G service due to non-existent type of message. | Int32
> 2G-intra-rau-rej-msg-type-non-exist | Total number of intra-SGSN routing area update requests rejected for 2G service due to non-existent type of message. | Int32
> 3G-intra-rau-rej-mtype-incompat-pstate | Total number of intra-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-intra-rau-rej-mtype-incompat-pstate | Total number of intra-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-intra-rau-rej-ie-non-existent | Total number of intra-SGSN routing area update requests rejected for 3G service due to non-existence of information element. | Int32
> 2G-intra-rau-rej-ie-non-existent | Total number of intra-SGSN routing area update requests rejected for 2G service due to non-existence of information element. | Int32
> 3G-intra-rau-rej-cond-ie-error | Total number of intra-SGSN routing area update requests rejected for 3G service due to error in conditional information element. | Int32
> 2G-intra-rau-rej-cond-ie-error | Total number of intra-SGSN routing area update requests rejected for 2G service due to error in conditional information element. | Int32
> 3G-intra-rau-rej-msg-incompat-prot-state | Total number of intra-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-intra-rau-rej-msg-incompat-prot-state | Total number of intra-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-intra-rau-rej-prot-error | Total number of intra-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 2G-intra-rau-rej-prot-error | Total number of intra-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 3G-intra-rau-rej-unknown-error | Total number of intra-SGSN routing area update requests rejected for 3G service where cause is unknown or not specified here. | Int32
> 2G-intra-rau-rej-unknown-error | Total number of intra-SGSN routing area update requests rejected for 2G service where cause is unknown or not specified here. | Int32
> 3G-intra-prau-rej-imsi-unknown-hlr | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to unknown IMSI in HLR. | Int32
> 2G-intra-prau-rej-imsi-unknown-hlr | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to unknown IMSI in HLR. | Int32
> 3G-intra-prau-rej-illegal-ms | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-intra-prau-rej-illegal-ms | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-intra-prau-rej-illegal-me | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-intra-prau-rej-illegal-me | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-intra-prau-rej-gprs-svc-not-allow | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to GPRS service not allowed for subscriber. | Int32
> 2G-intra-prau-rej-gprs-svc-not-allow | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to GPRS service not allowed for subscriber. | Int32
> 3G-intra-prau-rej-nongprs-svc-not-allow | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 2G-intra-prau-rej-nongprs-svc-not-allow | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 3G-intra-prau-rej-msid-not-derived-by-nw | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to network failed to derive MSID from attach message. | Int32
> 2G-intra-prau-rej-msid-not-derived-by-nw | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to network failed to derive MSID from attach message. | Int32
> 3G-intra-prau-rej-implicitly-detach | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to implicitly detach. | Int32
> 2G-intra-prau-rej-implicitly-detach | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to implicitly detach. | Int32
> 3G-intra-prau-rej-plmn-not-allowed | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to specific PLMN not allowed. | Int32
> 2G-intra-prau-rej-plmn-not-allowed | The total periodic intra-SGSN routing area update message rejected in intra-2G roaming due to specific PLMN not allowed. | Int32
> 3G-intra-prau-rej-loc-area-not-allowed | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to specific location area not allowed. | Int32
> 2G-intra-prau-rej-loc-area-not-allowed | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to specific location area not allowed. | Int32
> 3G-intra-prau-rej-roam-not-allowed-larea | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to roaming not allowed in specific location area. | Int32
> 2G-intra-prau-rej-roam-not-allowed-larea | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to roaming not allowed in specific location area. | Int32
> 3G-intra-prau-rej-gprs-svc-not-allowed-plmn | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to GPRS service not allowed in specific PLMN. | Int32
> 2G-intra-prau-rej-gprs-svc-not-allowed-plmn | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to GPRS service not allowed in specific PLMN. | Int32
> 3G-intra-prau-rej-no-cells-in-loc-area | Description: Total number of intra-SGSN RAU requests, of type “periodic updating”, for 3G service that were rejected with reject messages sent with a cause of "No Suitable Cells In Location Area". Triggers: Increments: - upon receiving a "UMTS access control" message from a Siemens HLR for a sai-req (service area identify request). - when an operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-prau-rej-no-cells-in-loc-area | Description: Total number of intra-SGSN RAU requests, of type “periodic updating”, for 2G service that were rejected where “rau-reject” messages were sent with a cause of "No Suitable Cells In Location Area". Triggers: Increments: - upon receiving a "UMTS access control" message from a Siemens HLR for a sai-req (service area identify request). - when an operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-prau-rej-msc-not-reachable | Description: Total number of intra-SGSN RAU requests, of type “periodic updating”, for 3G service that were rejected where “rau-reject” messages were sent with a cause of "MSC temporarily not reachable". Triggers: Increments: when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-prau-rej-msc-not-reachable | Description: Total number of intra-SGSN RAU requests, of type “periodic updating”, for 2G service that were rejected where “rau-reject” messages were sent with a cause of "MSC temporarily not reachable". Triggers: Increments: when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-prau-rej-network-failure | Description: Total number of intra-SGSN RAU requests, of type “period updating”, for 3G service that were rejected where the “rau-reject” message was sent with a cause "Network Failure" Triggers: Increments : - if RNC is overloaded. - if not enough credits at session manager. - upon receiving sai-request with cause of "data missing from hlr" . - if there are too many IU's for the same subscriber. - upon receiving RAU with a peer-sgsn P-TMSI when another attach is ongoing with the same P-TMSI. - when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-prau-rej-network-failure | Description: Total number of intra-SGSN RAU requests, of type “period updating”, for 2G service that were rejected where the “rau-reject” message was sent with a cause "Network Failure" Triggers: Increments : - upon receiving a sai-req with cause "data missing from hlr". - on XID failure for RAU. - if unable to send a “check-imei” request out. - when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-prau-rej-mac-failure | Description: Total number of intra-SGSN RAU requests, of type “period updating”, for 3G service that were rejected where the “rau-reject” message was sent with a cause "MAC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-prau-rej-mac-failure | Description: Total number of intra-SGSN RAU requests, of type “period updating”, for 2G service that were rejected where the “rau-reject” message was sent with a cause "MAC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-prau-rej-syn-failure | Description: Total number of intra-SGSN RAU requests, of type “period updating”, for 3G service that were rejected where the “rau-reject” message was sent with a cause "SYNC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-prau-rej-syn-failure | Description: Total number of intra-SGSN RAU requests, of type “period updating”, for 2G service that were rejected where the “rau-reject” message was sent with a cause "SYNC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-prau-rej-congestion | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to network congestion. | Int32
> 2G-intra-prau-rej-congestion | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to network congestion. | Int32
> 3G-intra-prau-rej-gsm-auth-unacceptable | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to unacceptable authentication from GSM network. | Int32
> 2G-intra-prau-rej-gsm-auth-unacceptable | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to unacceptable authentication from GSM network. | Int32
> 3G-intra-prau-rej-no-pdp-ctx-actv | Total number of periodic intra-SGSN routing area update requests rejected for 3G service as PDP context is not activated. | Int32
> 2G-intra-prau-rej-no-pdp-ctx-actv | Total number of periodic intra-SGSN routing area update requests rejected for 2G service as PDP context is not activated. | Int32
> 3G-intra-prau-rej-retry-from-new-cell | Total number of periodic intra-SGSN routing area update requests rejected for 3G service as subscriber retried for update from new cell. | Int32
> 2G-intra-prau-rej-retry-from-new-cell | Total number of periodic intra-SGSN routing area update requests rejected for 2G service as subscriber retried for update from new cell. | Int32
> 3G-intra-prau-rej-sem-wrong-msg | Total number of periodic intra-SGSN routing area update requests rejected for 3G service as attach request message is semantically wrong. | Int32
> 2G-intra-prau-rej-sem-wrong-msg | Total number of periodic intra-SGSN routing area update requests rejected for 2G service as attach request message is semantically wrong. | Int32
> 3G-intra-prau-rej-inval-mand-info | Total number of periodic intra-SGSN routing area update requests rejected for 3G service as mandatory information in message is invalid. | Int32
> 2G-intra-prau-rej-inval-mand-info | Total number of periodic intra-SGSN routing area update requests rejected for 2G service as mandatory information in message is invalid. | Int32
> 3G-intra-prau-rej-msg-type-non-exist | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to non-existent type of message. | Int32
> 2G-intra-prau-rej-msg-type-non-exist | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to non-existent type of message. | Int32
> 3G-intra-prau-rej-mtype-incompat-pstate | Total number of periodic intra-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-intra-prau-rej-mtype-incompat-pstate | Total number of periodic intra-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-intra-prau-rej-ie-non-existent | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to non-existence of information element. | Int32
> 2G-intra-prau-rej-ie-non-existent | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to non-existence of information element. | Int32
> 3G-intra-prau-rej-cond-ie-error | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to error in conditional information element. | Int32
> 2G-intra-prau-rej-cond-ie-error | Total number of periodic intra-SGSN routing area update requests rejected for 2G service due to error in conditional information element. | Int32
> 3G-intra-prau-rej-msg-incompat-pstate | Total number of periodic intra-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-intra-prau-rej-msg-incompat-pstate | Total number of periodic intra-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-intra-prau-rej-prot-error | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 2G-intra-prau-rej-prot-error | Total number of periodic intra-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 3G-intra-prau-rej-unknown-error | Total number of periodic intra-SGSN routing area update requests rejected for 3G service where cause is unknown or not specified here. | Int32
> 2G-intra-prau-rej-unknown-error | Total number of periodic intra-SGSN routing area update requests rejected for 2G service where cause is unknown or not specified here. | Int32
> 3G-comb-rau-rej-imsi-unknown-hlr | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to unknown IMSI in HLR. | Int32
> 2G-comb-rau-rej-imsi-unknown-hlr | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to unknown IMSI in HLR. | Int32
> 3G-comb-rau-rej-illegal-ms | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-comb-rau-rej-illegal-ms | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-comb-rau-rej-illegal-me | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-comb-rau-rej-illegal-me | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-comb-rau-rej-gprs-svc-not-allow | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to GPRS service not allowed for subscriber. | Int32
> 2G-comb-rau-rej-gprs-svc-not-allow | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to GPRS service not allowed for subscriber. | Int32
> 3G-comb-rau-rej-nongprs-svc-not-allow | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 2G-comb-rau-rej-nongprs-svc-not-allow | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 3G-comb-rau-rej-msid-not-derived-by-nw | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to network failed to derive MSID from attach message. | Int32
> 2G-comb-rau-rej-msid-not-derived-by-nw | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to network failed to derive MSID from attach message. | Int32
> 3G-comb-rau-rej-implicitly-detach | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to implicitly detach. | Int32
> 2G-comb-rau-rej-implicitly-detach | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to implicitly detach. | Int32
> 3G-comb-rau-rej-plmn-not-allowed | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to specific PLMN not allowed. | Int32
> 2G-comb-rau-rej-plmn-not-allowed | The total intra-SGSN routing area update message rejected in intra-2G roaming due to specific PLMN not allowed. | Int32
> 3G-comb-rau-rej-loc-area-not-allowed | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to specific location area not allowed. | Int32
> 2G-comb-rau-rej-loc-area-not-allowed | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to specific location area not allowed. | Int32
> 3G-comb-rau-rej-roam-not-allowed-larea | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to roaming not allowed in specific location area. | Int32
> 2G-comb-rau-rej-roam-not-allowed-larea | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to roaming not allowed in specific location area. | Int32
> 3G-comb-rau-rej-gprs-svc-not-allowed-plmn | Description: Total number of RAU rejects sent with cause “GPRS service not allowed in this PLMN” against Intra-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-rau-rej-gprs-svc-not-allowed-plmn | Description: Total number of RAU reject messages sent with cause “GPRS service not allowed in this PLMN” against Intra-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-rau-rej-no-cells-in-loc-area | Description: Total number of intra-SGSN RAU requests for 3G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "No Suitable Cells In Location Area". Triggers: Increments: - upon receiving “UMTS access control” for the SAI-Request from the Siemens HLR. - when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-rau-rej-no-cells-in-loc-area | Description: Total number of intra-SGSN RAU requests for 2G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "No Suitable Cells In Location Area". Triggers: Increments: - upon receiving “UMTS access control” for the SAI-Request from the Siemens HLR. - when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-rau-rej-msc-not-reachable | Description: Total number of intra-SGSN RAU requests for 3G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "MSC temporarily not reachable". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-rau-rej-msc-not-reachable | Description: Total number of intra-SGSN RAU requests for 2G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "MSC temporarily not reachable". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-rau-rej-network-failure | Description: Total number of intra-SGSN RAU requests for 3G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "MSC temporarily not reachable". Triggers: Increments: - if the RNC is overloaded. - if there is not enough credits at session manager. - upon receiving cause "data missing from hlr" in the SAI-request. - if there are too many IU's for the same subscriber. - upon receiving an RAU with a peer-sgsn P-TMSI when another attach is ongoing with the same P-TMSI. - when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-rau-rej-network-failure | Description: Total number of intra-SGSN RAU requests for 2G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "MSC temporarily not reachable". Triggers: Increments - if the RNC is overloaded. - if there is not enough credits at session manager. - upon receiving cause "data missing from hlr" in the SAI-request. - if there are too many IU's for the same subscriber. - upon receiving an RAU with a peer-sgsn P-TMSI when another attach is ongoing with the same P-TMSI. - when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-rau-rej-mac-failure | Description: Total number of intra-SGSN RAU requests for 3G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "MAC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-rau-rej-mac-failure | Description: Total number of intra-SGSN RAU requests for 2G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "MAC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-rau-rej-syn-failure | Description: Total number of intra-SGSN RAU requests for 3G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "SYNC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-rau-rej-syn-failure | Description: Total number of intra-SGSN RAU requests for 2G service, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", sent with cause "SYNC Failure". Triggers: Increments when the operator policy is configured with this value as the reject cause for RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-rau-rej-congestion | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to network congestion. | Int32
> 2G-comb-rau-rej-congestion | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to network congestion. | Int32
> 3G-comb-rau-rej-gsm-auth-unacceptable | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to unacceptable authentication from GSM network. | Int32
> 2G-comb-rau-rej-gsm-auth-unacceptable | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to unacceptable authentication from GSM network. | Int32
> 3G-comb-rau-rej-no-pdp-ctx-actv | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service as PDP context is not activated. | Int32
> 2G-comb-rau-rej-no-pdp-ctx-actv | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service as PDP context is not activated. | Int32
> 3G-comb-rau-rej-retry-from-new-cell | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service as subscriber retried for update from new cell. | Int32
> 2G-comb-rau-rej-retry-from-new-cell | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service as subscriber retried for update from new cell. | Int32
> 3G-comb-rau-rej-sem-wrong-msg | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service as attach request message is semantically wrong. | Int32
> 2G-comb-rau-rej-sem-wrong-msg | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service as attach request message is semantically wrong. | Int32
> 3G-comb-rau-rej-inval-mand-info | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service as mandatory information in message is invalid. | Int32
> 2G-comb-rau-rej-inval-mand-info | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service as mandatory information in message is invalid. | Int32
> 3G-comb-rau-rej-msg-type-non-exist | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to non-existence of information element. | Int32
> 2G-comb-rau-rej-msg-type-non-exist | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to non-existence of information element. | Int32
> 3G-comb-rau-rej-mtype-incompat-pstate | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-comb-rau-rej-mtype-incompat-pstate | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-comb-rau-rej-ie-non-existent | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to non-existent type of message. | Int32
> 2G-comb-rau-rej-ie-non-existent | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to non-existent type of message. | Int32
> 3G-comb-rau-rej-cond-ie-error | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to error in conditional information element. | Int32
> 2G-comb-rau-rej-cond-ie-error | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service due to error in conditional information element. | Int32
> 3G-comb-rau-rej-msg-incompat-pstate | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-comb-rau-rej-msg-incompat-pstate | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-comb-rau-rej-prot-error | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 2G-comb-rau-rej-prot-error | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 3G-comb-rau-rej-unknown-error | Total number of combined (GPRS and IMSI) routing area update requests rejected for 3G service where cause is unknown or not specified here. | Int32
> 2G-comb-rau-rej-unknown-error | Total number of combined (GPRS and IMSI) routing area update requests rejected for 2G service where cause is unknown or not specified here. | Int32
> 3G-inter-rau-rej-imsi-unknown-hlr | Total number of inter-SGSN routing area update requests rejected for 3G service due to unknown IMSI in HLR. | Int32
> 2G-inter-rau-rej-imsi-unknown-hlr | Total number of inter-SGSN routing area update requests rejected for 2G service due to unknown IMSI in HLR. | Int32
> 3G-inter-rau-rej-illegal-ms | Total number of inter-SGSN routing area update requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-inter-rau-rej-illegal-ms | Total number of inter-SGSN routing area update requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-inter-rau-rej-illegal-me | Total number of inter-SGSN routing area update requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-inter-rau-rej-illegal-me | Total number of inter-SGSN routing area update requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-inter-rau-rej-gprs-svc-not-allow | Total number of inter-SGSN routing area update requests rejected for 3G service due to GPRS service not allowed for subscriber. | Int32
> 2G-inter-rau-rej-gprs-svc-not-allow | Total number of inter-SGSN routing area update requests rejected for 2G service due to GPRS service not allowed for subscriber. | Int32
> 3G-inter-rau-rej-nongprs-svc-not-allow | Total number of inter-SGSN routing area update requests rejected for 3G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 2G-inter-rau-rej-nongprs-svc-not-allow | Total number of inter-SGSN routing area update requests rejected for 2G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 3G-inter-rau-rej-msid-not-derived-by-nw | Description: Total number of inter-SGSN routing area update request rejects sent with cause “MSID not derived by network” against Inter-SGSN-RAU requests of type “RA Updating” in 3G service. Triggers: 1. When PTMSI IE is missing in RAU. 2. When old RAI has invalid location area values (0x0000 or 0xFFFE) for P-TMSI-attaches/RAU. 3. When getting a RAU with old RAI in 2G, and P-TMSI is unknown. 4. When getting P-TMSI-SIG-MISMATCH for an SGSN Context Request sent with IMSI Validated. 5. When getting a RAU Request while an attach with the same peer-SGSN-P-TMSI is in progress. 6. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-inter-rau-rej-msid-not-derived-by-nw | Description: Total number of inter-SGSN routing area update request rejects sent with cause “MSID not derived by network” against Inter-SGSN-RAU requests of type “RA Updating” in 2G service. Triggers: 1. When SGSN-Context-resp arrives with any cause other than “accepted”. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-inter-rau-rej-implicitly-detach | Total number of inter-SGSN routing area update requests rejected for 3G service due to implicitly detach. | Int32
> 2G-inter-rau-rej-implicitly-detach | Total number of inter-SGSN routing area update requests rejected for 2G service due to implicitly detach. | Int32
> 3G-inter-rau-rej-plmn-not-allowed | Total number of inter-SGSN routing area update requests rejected for 3G service due to specific PLMN not allowed. | Int32
> 2G-inter-rau-rej-plmn-not-allowed | The total inter-SGSN routing area update message rejected in intra-2G roaming due to specific PLMN not allowed. | Int32
> 3G-inter-rau-rej-loc-area-not-allowed | Total number of inter-SGSN routing area update requests rejected for 3G service due to specific location area not allowed. | Int32
> 2G-inter-rau-rej-loc-area-not-allowed | Total number of inter-SGSN routing area update requests rejected for 2G service due to specific location area not allowed. | Int32
> 3G-inter-rau-rej-roam-not-allowed-larea | Total number of inter-SGSN routing area update requests rejected for 3G service due to roaming not allowed in specific location area. | Int32
> 2G-inter-rau-rej-roam-not-allowed-larea | Total number of inter-SGSN routing area update requests rejected for 2G service due to roaming not allowed in specific location area. | Int32
> 3G-inter-rau-rej-gprs-svc-not-allowed-plmn | Description: Total number of RAU rejects sent with cause “GPRS service not allowed in this PLMN” against Intter-SGSN-RAU requests of type “RA Updating” in 3G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-inter-rau-rej-gprs-svc-not-allowed-plmn | Description: Total number of RAU rejects sent with cause “GPRS service not allowed in this PLMN” against Intter-SGSN-RAU requests of type “RA Updating” in 2G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-inter-rau-rej-no-cells-in-location-area | Total number of inter-SGSN routing area update requests rejected for 3G service due to non availability of suitable cell in specific location area. | Int32
> 2G-inter-rau-rej-no-cells-in-location-area | Total number of inter-SGSN routing area update requests rejected for 2G service due to non availability of suitable cell in specific location area. | Int32
> 3G-inter-rau-rej-msc-not-reachable | Total number of inter-SGSN routing area update requests rejected for 3G service as MSC not reachable. | Int32
> 2G-inter-rau-rej-msc-not-reachable | Total number of inter-SGSN routing area update requests rejected for 2G service as MSC not reachable. | Int32
> 3G-inter-rau-rej-network-failure | Total number of inter-SGSN routing area update requests rejected for 3G service due to network failure. | Int32
> 2G-inter-rau-rej-network-failure | Total number of inter-SGSN routing area update requests rejected for 2G service due to network failure. | Int32
> 3G-inter-rau-rej-mac-failure | Total number of inter-SGSN routing area update requests rejected for 3G service due to message authenticate code (MAC) failure. | Int32
> 2G-inter-rau-rej-mac-failure | Total number of inter-SGSN routing area update requests rejected for 2G service due to MAC failure. | Int32
> 3G-inter-rau-rej-syn-failure | Total number of inter-SGSN routing area update requests rejected for 3G service due to context synchronization failure. | Int32
> 2G-inter-rau-rej-syn-failure | Total number of inter-SGSN routing area update requests rejected for 2G service due to context synchronization failure. | Int32
> 3G-inter-rau-rej-congestion | Total number of inter-SGSN routing area update requests rejected for 3G service due to network congestion. | Int32
> 2G-inter-rau-rej-congestion | Total number of inter-SGSN routing area update requests rejected for 2G service due to network congestion. | Int32
> 3G-inter-rau-rej-gsm-auth-unacceptable | Total number of inter-SGSN routing area update requests rejected for 3G service due to unacceptable authentication from GSM network. | Int32
> 2G-inter-rau-rej-gsm-auth-unacceptable | Total number of inter-SGSN routing area update requests rejected for 2G service due to unacceptable authentication from GSM network. | Int32
> 3G-inter-rau-rej-no-pdp-ctx-actv | Total number of inter-SGSN routing area update requests rejected for 3G service as PDP context is not activated. | Int32
> 2G-inter-rau-rej-no-pdp-ctx-actv | Total number of inter-SGSN routing area update requests rejected for 2G service as PDP context is not activated. | Int32
> 3G-inter-rau-rej-retry-from-new-cell | Total number of inter-SGSN routing area update requests rejected for 3G service as subscriber retried for update from new cell. | Int32
> 2G-inter-rau-rej-retry-from-new-cell | Total number of inter-SGSN routing area update requests rejected for 2G service as subscriber retried for update from new cell. | Int32
> 3G-inter-rau-rej-sem-wrong-msg | Total number of inter-SGSN routing area update requests rejected for 3G service as attach request message is semantically wrong. | Int32
> 2G-inter-rau-rej-sem-wrong-msg | Total number of inter-SGSN routing area update requests rejected for 2G service as attach request message is semantically wrong. | Int32
> 3G-inter-rau-rej-inval-mand-info | Total number of inter-SGSN routing area update requests rejected for 3G service as mandatory information in message is invalid. | Int32
> 2G-inter-rau-rej-inval-mand-info | Total number of inter-SGSN routing area update requests rejected for 2G service as mandatory information in message is invalid. | Int32
> 3G-inter-rau-rej-msg-type-non-exist | Total number of inter-SGSN routing area update requests rejected for 3G service due to non-existent type of message. | Int32
> 2G-inter-rau-rej-msg-type-non-exist | Total number of inter-SGSN routing area update requests rejected for 2G service due to non-existent type of message. | Int32
> 3G-inter-rau-rej-mtype-incompat-pstate | Total number of inter-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-inter-rau-rej-mtype-incompat-pstate | Total number of inter-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-inter-rau-rej-ie-non-existent | Total number of inter-SGSN routing area update requests rejected for 3G service due to non-existence of information element. | Int32
> 2G-inter-rau-rej-ie-non-existent | Total number of inter-SGSN routing area update requests rejected for 2G service due to non-existence of information element. | Int32
> 3G-inter-rau-rej-cond-ie-error | Total number of inter-SGSN routing area update requests rejected for 3G service due to error in conditional information element. | Int32
> 2G-inter-rau-rej-cond-ie-error | Total number of inter-SGSN routing area update requests rejected for 2G service due to error in conditional information element. | Int32
> 3G-inter-rau-rej-msg-not-compat-pstate | Total number of inter-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-inter-rau-rej-msg-not-compat-pstate | Total number of inter-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-inter-rau-rej-prot-error | Total number of inter-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 2G-inter-rau-rej-prot-error | Total number of inter-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 3G-inter-rau-rej-unknown-error | Total number of inter-SGSN routing area update requests rejected for 3G service where cause is unknown or not specified here. | Int32
> 2G-inter-rau-rej-unknown-error | Total number of inter-SGSN routing area update requests rejected for 2G service where cause is unknown or not specified here. | Int32
> 3G-comb-irau-rej-imsi-unknown-hlr | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to unknown IMSI in HLR. | Int32
> 2G-comb-irau-rej-imsi-unknown-hlr | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to unknown IMSI in HLR. | Int32
> 3G-comb-irau-rej-illegal-ms | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to illegal mobile subscriber. | Int32
> 2G-comb-irau-rej-illegal-ms | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to illegal mobile subscriber. | Int32
> 3G-comb-irau-rej-illegal-me | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to illegal mobile equipment. | Int32
> 2G-comb-irau-rej-illegal-me | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to illegal mobile equipment. | Int32
> 3G-comb-irau-rej-gprs-svc-not-allow | Description: Total number of inter-SGSN routing area update request rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: 1. On getting "Roaming not allowed" from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-irau-rej-gprs-svc-not-allow | Description: Total number of inter-SGSN routing area update request rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: 1. On getting "Roaming not allowed" from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-irau-rej-nongprs-svc-not-allow | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 2G-comb-irau-rej-nongprs-svc-not-allow | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to GPRS and non-GPRS service not allowed for subscriber. | Int32
> 3G-comb-irau-rej-msid-not-derived-by-nw | Description: Total number of inter-SGSN routing area update request rejects sent with cause “MSID not derived by network” against Inter-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 3G service. Triggers: 1. When PTMSI IE is missing in RAU. 2. When old RAI has invalid location area values (0x0000 or 0xFFFE) for P-TMSI-attaches/RAU. 3. When getting a RAU with old RAI in 2G, and P-TMSI is unknown. 4. When getting P-TMSI-SIG-MISMATCH for an SGSN Context Request sent with IMSI Validated. 5. When getting a RAU Request while an attach with the same peer-SGSN-P-TMSI is in progress. 6. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-irau-rej-msid-not-derived-by-nw | Description: Total number of inter-SGSN routing area update request rejects sent with cause “MSID not derived by network” against Inter-SGSN-RAU requests of type “Combined RA/LA update” or “Combined RA/LA update with IMSI Attach” in 2G service. Triggers: 1. When SGSN-Context-resp arrives with any cause other than “accepted”. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-irau-rej-implicitly-detach | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to implicitly detach. | Int32
> 2G-comb-irau-rej-implicitly-detach | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to implicitly detach. | Int32
> 3G-comb-irau-rej-plmn-not-allowed | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to specific PLMN not allowed. | Int32
> 2G-comb-irau-rej-plmn-not-allowed | The total inter-SGSN routing area update message rejected in intra-2G roaming due to specific PLMN not allowed. | Int32
> 3G-comb-irau-rej-loc-area-not-allowed | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to specific location area not allowed. | Int32
> 2G-comb-irau-rej-loc-area-not-allowed | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to specific location area not allowed. | Int32
> 3G-comb-irau-rej-roam-not-allowed-larea | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to roaming not allowed in specific location area. | Int32
> 2G-comb-irau-rej-roam-not-allowed-larea | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to roaming not allowed in specific location area. | Int32
> 3G-comb-irau-rej-gprs-svc-not-allowed-plmn | Description: Total number of RAU rejects sent with cause "GPRS service not allowed in PLMN" against Inter-SGSN-RAU requests of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach" in 3G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-comb-irau-rej-gprs-svc-not-allowed-plmn | Description: Total number of RAU rejects sent with cause "GPRS service not allowed in PLMN" against Inter-SGSN-RAU requests of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach" in 2G service. Triggers: 1. On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req. 2. When operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per GPRS service Type: Counter | Int32
> 3G-comb-irau-rej-no-cells-in-location-area | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to non availability of suitable cell in specific location area. | Int32
> 2G-comb-irau-rej-no-cells-in-location-area | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to non availability of suitable cell in specific location area. | Int32
> 3G-comb-irau-rej-msc-not-reachable | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as MSC not reachable. | Int32
> 2G-comb-irau-rej-msc-not-reachable | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as MSC not reachable. | Int32
> 3G-comb-irau-rej-network-failure | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to network failure. | Int32
> 2G-comb-irau-rej-network-failure | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to network failure. | Int32
> 3G-comb-irau-rej-mac-failure | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to message authenticate code (MAC) failure. | Int32
> 2G-comb-irau-rej-mac-failure | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to MAC failure. | Int32
> 3G-comb-irau-rej-syn-failure | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to context synchronization failure. | Int32
> 2G-comb-irau-rej-syn-failure | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to context synchronization failure. | Int32
> 3G-comb-irau-rej-congestion | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to network congestion. | Int32
> 2G-comb-irau-rej-congestion | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to network congestion. | Int32
> 3G-comb-irau-rej-gsm-auth-unacceptable | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to unacceptable authentication from GSM network. | Int32
> 2G-comb-irau-rej-gsm-auth-unacceptable | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to unacceptable authentication from GSM network. | Int32
> 3G-comb-irau-rej-no-pdp-ctx-actv | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as PDP context is not activated. | Int32
> 2G-comb-irau-rej-no-pdp-ctx-actv | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as PDP context is not activated. | Int32
> 3G-comb-irau-rej-retry-from-new-cell | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as subscriber retried for update from new cell. | Int32
> 2G-comb-irau-rej-retry-from-new-cell | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as subscriber retried for update from new cell. | Int32
> 3G-comb-irau-rej-sem-wrong-msg | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as attach request message is semantically wrong. | Int32
> 2G-comb-irau-rej-sem-wrong-msg | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as attach request message is semantically wrong. | Int32
> 3G-comb-irau-rej-inval-mand-info | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as mandatory information in message is invalid. | Int32
> 2G-comb-irau-rej-inval-mand-info | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as mandatory information in message is invalid. | Int32
> 3G-comb-irau-rej-msg-type-non-exist | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to non-existent type of message. | Int32
> 2G-comb-irau-rej-msg-type-non-exist | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to non-existent type of message. | Int32
> 3G-comb-irau-rej-mtype-incompat-pstate | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-comb-irau-rej-mtype-incompat-pstate | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-comb-irau-rej-ie-non-existent | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to non-existence of information element. | Int32
> 2G-comb-irau-rej-ie-non-existent | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to non-existence of information element. | Int32
> 3G-comb-irau-rej-cond-ie-error | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to error in conditional information element. | Int32
> 2G-comb-irau-rej-cond-ie-error | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service due to error in conditional information element. | Int32
> 3G-comb-irau-rej-msg-not-compat-pstate | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service as message type is not compatible with protocol state. | Int32
> 2G-comb-irau-rej-msg-not-compat-pstate | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service as message type is not compatible with protocol state. | Int32
> 3G-comb-irau-rej-prot-error | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 2G-comb-irau-rej-prot-error | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service due to protocol error in message. | Int32
> 3G-comb-irau-rej-unknown-error | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 3G service where cause is unknown or not specified here. | Int32
> 2G-comb-irau-rej-unknown-error | Total number of combined (GPRS and IMSI) inter-SGSN routing area update requests rejected for 2G service where cause is unknown or not specified here. | Int32
> 3G-total-rau-failure | Total number of routing area updates failed for 3G service. | Int32
> 2G-total-rau-failure | Total number of routing area updates failed for 2G service. | Int32
> 3G-total-intra-rau-failure | Description: This proprietary counter indicates the total number of Intra-SGSN-RAU requests of type “RA Updating” that were dropped from processing in 3G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-total-intra-rau-failure | Description: This proprietary counter indicates the total number of Intra-SGSN-RAU requests of type “RA Updating” that were dropped from processing in 2G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service Type: Counter | Int32
> 3G-total-periodic-rau-failure | Description: This proprietary counter indicates the total number of Intra-SGSN-RAU requests of type “Periodic Updating” that were dropped from processing in 3G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. 3. Iu released while attach procedure in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-total-periodic-rau-failure | Description: This proprietary counter indicates the total number of Intra-SGSN RAU requests, of type “Periodic Updating”, that were dropped from processing in 2G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service Type: Counter | Int32
> 3G-total-intra-rau-failure-comb | Description: This proprietary counter indicates the total number of Inter-SGSN RAU requests, of type “Combined RA/LA Update or “Combined RA/LA Update with IMSI Attach”, that were failed in 3G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. 3. Iu released while attach procedure in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-total-intra-rau-failure-comb | Description: This proprietary counter indicates the total number of Inter-SGSN-RAU requests of type “Combined RA/LA Update or “Combined RA/LA Update with IMSI Attach” that were failed in 3G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service Type: Counter | Int32
> 3G-total-inter-rau-failure | Description: This proprietary counter indicates the total number of Inter-SGSN-RAU requests of type “RA Updating” that were failed in 3G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. 3. Iu released while attach procedure in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-total-inter-rau-failure | Description: This proprietary counter indicates the total number of Inter-SGSN-RAU requests of type “RA Updating” that were failed in 2G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service Type: Counter | Int32
> 3G-total-comb-inter-rau-failure | Description: This proprietary counter indicates the total number of Inter-SGSN-RAU requests of type “Combined RA/LA Update or “Combined RA/LA Ipdate with IMSI Attach” that were failed in 3G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. 3. Iu released while attach procedure was in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-total-comb-inter-rau-failure | Description: This proprietary counter indicates the total number of Inter-SGSN-RAU requests of type “Combined RA/LA Update or “Combined RA/LA Ipdate with IMSI Attach” that were failed in 2G service. “Dropped” indicates that the requests were silently discarded and no reject was sent for such requests. Triggers: 1. Another RAU, differing from this RAU, was received and pre-empted existing RAU procedure. 2. Another Attach, differing from this attach, was received and pre-empted existing Attach procedure. Availability: per GPRS service Type: Counter | Int32
> 3G-intra-ra-upd-rau-fail-iu_release | Total number of intra-SGSN routing area updates failed for 3G service due to Iu released. | Int32
> 3G-intra-ra-upd-rau-fail-ongoing-proc | Total number of intra-SGSN routing area updates failed for 3G service due ongoing procedures. | Int32
> 2G-intra-ra-upd-rau-fail-ongoing-proc | Total number of intra-SGSN routing area updates failed for 2G service due ongoing procedures. | Int32
> 3G-intra-perio-rau-fail-iu_release | Total number of intra-SGSN periodic routing area updates failed for 3G service due Iu released. | Int32
> 3G-intra-perio-rau-fail-ongoing-proc | Total number of intra-SGSN periodic routing area updates failed for 3G service due ongoing procedures. | Int32
> 2G-intra-perio-rau-fail-ongoing-proc | Total number of intra-SGSN periodic routing area updates failed for 2G service due ongoing procedures. | Int32
> 3G-inter-rau-fail-iu_release | Total number of inter-SGSN periodic routing area updates failed for 3G service due Iu released. | Int32
> 3G-inter-rau-fail-ongoing-proc | Total number of inter-SGSN periodic routing area updates failed for 3G service due ongoing procedures. | Int32
> 2G-inter-rau-fail-ongoing-proc | Total number of inter-SGSN periodic routing area updates failed for 2G service due ongoing procedures. | Int32
> 3G-intra-comb-rau-fail-iu_release | Description:Total number of combined RAUs dropped from processing as the Iu (in which the RAU came) was released. This counter is new in release 9.0. Triggers: Increments when the Iu releases during an ongoing RAU. Availability:per SGSN service, per RA Type: Counter | Int32
> 3G-intra-comb-rau-fail-ongoing-proc | Description:Total number of combined RAUs dropped from processing as another RAU/Attach/Detach was received. This counter is new in release 9.0. Triggers: Increments when another Attach/RAU/Detach is received. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-intra-comb-rau-fail-ongoing-proc | Description:Total number of combined RAUs dropped from processing as another RAU/Attach/Detach was received. This counter is new in release 9.0. Triggers: Increments when another Attach/RAU/Detach is received. Availability: per GPRS service Type: Counter | Int32
> 3G-inter-comb-rau-fail-iu_release | Description:Total number of combined inter-SGSN RAUs dropped from processing as the Iu (in which the RAU came) was released. This counter is new in release 9.0. Triggers: Increments when the Iu releases during an ongoing RAU. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-inter-comb-rau-fail-ongoing-proc | Description:Total number of combined inter-SGSN RAUs dropped from processing as another RAU/Attach/Detach was received. This counter is new in release 9.0. Triggers: Increments when another Attach/RAU/Detach is received. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-inter-comb-rau-fail-ongoing-proc | Description:Total number of combined inter-SGSN RAUs dropped from processing as another RAU/Attach/Detach was received. This counter is new in release 9.0. Triggers: Increments when another Attach/RAU/Detach is received. Availability: per GPRS service Type: Counter | Int32
> intra-sgsn-inter-system-gsm-to-wcdma-success | Description: Total number of Attach and RAU Requests received at 3G from 2G mobile stations (MS) attached in the same SGSN. Triggers: Increments when a Mobile Station (MS) performs an intra-SGSN inter-RAT Attach/RAU from 2G to 3G. Availability: Across all SGSN services Type: Counter | Int32
> intra-sgsn-inter-system-gsm-to-wcdma-rej | Description: Total number of Attach/RAU Rejects sent against Attach/RAU Requests received at 3G from 2G mobile stations (MS) attached in the same SGSN. Triggers: Increments when an Attach/RAU procedure is rejected on an intra-SGSN inter-RAT Attach/RAU Request from 2G to 3G. Availability: Across all SGSN services Type: Counter | Int32
> intra-sgsn-inter-system-gsm-to-wcdma-fail | Description: Total number of failed Attach/RAU Procedures initiated at 3G from 2G mobile stations (MS) attached in the same SGSN. Triggers: Increments when an Attach/RAU procedure is dropped without an Attach/RAU Reject on an intra-SGSN inter-RAT from 2G to 3G. Availability: Across all SGSN services Type: Counter | Int32
> intra-sgsn-inter-system-wcdma-to-gsm-success | Description: Total number of RAU and Attach Requests received at 2G from 3G mobile stations (MS) attached in the same SGSN. Triggers: Increments when a Mobile Station (MS) performs an intra-SGSN inter-RAT Attach/RAU from 3G to 2G. Availability: Across all GPRS services Type: Counter | Int32
> intra-sgsn-inter-system-wcdma-to-gsm-rej | Description: Total number of Attach/RAU Rejects sent against Attach/RAU Requests received at 2G from 3G mobile stations (MS) attached in the same SGSN. Triggers: Increments when an Attach/RAU procedure is rejected on an intra-SGSN inter-RAT Attach/RAU Request from 3G to 2G. Availability: Across all GPRS services Type: Counter | Int32
> intra-sgsn-inter-system-wcdma-to-gsm-fail | Description: Total number of failed Attach/RAU Procedures initiated at 2G from 3G mobile stations (MS) attached in the same SGSN. Triggers: Increments when an Attach/RAU procedure is dropped without an Attach/RAU Reject on an intra-SGSN inter-RAT from 3G to 2G. Availability: Across all GPRS services Type: Counter | Int32
> inter-system-2G-to-3G-rau-requests | Description: Total number of RAU-requests of type "RA Updating" received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon reception of a RAU-request at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-rau-accepts | Description: Total number of RAU-accepts with update-result - "RA updated" issued against RAU-requests from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such a RAU-accept message at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-rau-rejects | Description: Total number of RAU-rejects issued against RAU-requests of the type "RA Updating" which were received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such a RAU-reject message by the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-comb-rau-requests | Description: Total number of RAU-requests, of type "Combined RA/LA update" or "Combined RA/LA update, with IMSI Attach" received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon reception of such a RAU-request message at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-comb-rau-accepts | Description: Total number of RAU-accepts, with update-result - "Combined RA/LA updated", issued against RAU-requests from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such RAU-accept message at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-comb-rau-rejects | Description: Total number of RAU-rejects ,issued against RAU-requests of the type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such a RAU-reject message at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-attach-requests | Description: Total number of attach-request messages, of the type "GPRS Attach", received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon reception of such an attach-request message at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-attach-accepts | Description: Total number of attach-accepts of type "GPRS only attached" issued against attach-requests from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such an attach-accept message at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-attach-rejects | Description: Total number of attach-reject messages, issued against attach-requests of type "GPRS Attach", received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such an attach-reject message from the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-comb-attach-requests | Description: Total number of attach-request messages, of type "Combined GPRS/IMSI Attach", received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon reception of such attach-request messages at the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-comb-attach-accepts | Description: Total number of attach-accept messages, of the type "Combined GPRS/IMSI attached", issued against attach-requests from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such an attach-accept message by the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-2G-to-3G-comb-attach-rejects | Description: Total number of attach-reject messages, issued against attach-requests of type "Combined GPRS/IMSI Attach", received from subscribers who attached previously to the same SGSN under 2G. Triggers: Increments upon issue of such an attach-reject message by the 3G SGSN. Availability: per SGSN service, per RA Type: Counter | Int32
> inter-system-3G-to-2G-rau-requests | Description: Total number of RAU-request messages, of type "RA Updating", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon reception of such a RAU-request message at the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-rau-accepts | Description: Total number of RAU-accept messages, with update-result - "RA updated", issued against RAU-requests from subscribers who previously attached to the same SGSN under 3G. Triggers: Increments upon issue of such a RAU-accept message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-rau-rejects | Description: Total number of RAU-reject messages, issued against RAU-requests of type "Ra Updating", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon issue of such a RAU-reject message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-comb-rau-requests | Description: Total number of RAU-request messages, of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon reception of such a RAU-request message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-comb-rau-accepts | Description: Total number of RAU-accept messages, with update-result - "Combined RA/LA updated", issued against RAU-requests from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon issue of such a RAU-accept message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-comb-rau-rejects | Description: Total number of RAU-reject messages, issued against RAU-requests of type "Combined RA/LA update" or "Combined RA/LA update with IMSI Attach", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon issue of such a RAU-reject message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-attach-requests | Description: Total number of “attach request” messages, of type "GPRS Attach", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon reception of such an ‘”attach request” message at the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-attach-accepts | Description: Total number of “attach-accept” messages, of type "GPRS only attached", issued against “attach-requests” from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon issue of such an “attach-accept” message at the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-attach-rejects | Description: Total number of “attach-reject” messages, issued against “attach-requests” of type "GPRS Attach", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon issue of such an “attach-reject” message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-comb-attach-requests | Description: Total number of “attach-request” messages, of type "Combined GPRS/IMSI Attach", received from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon reception of such an “attach-request” message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-comb-attach-accepts | Description: Total number of “attach-accept” messages, of type "Combined GPRS/IMSI attached", issued against “attach-requests” from subscribers who attached previously to the same SGSN under 3G. Triggers: Increments upon reception of such an “attach-request” message by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> inter-system-3G-to-2G-comb-attach-rejects | Description: Total number of Attach rejects issued against attach-requests of type "Combined GPRS/IMSI Attach" received from subscribers who are previously attached in the same sgsn under 3g. Triggers: Increments upon issue of such an “attach-reject” by the 2G SGSN. Availability: across all GPRS services Type: Counter | Int32
> ps-inter-rat-rau-total | Description: Total number of GPRS only Inter RAT RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ps-inter-rat-rau-3g | Description: Total number of GPRS only Inter RAT RAU Requests received in a 3G service from a 2G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ps-inter-rat-rau-2g | Description: Total number of GPRS only Inter RAT RAU Requests received in a 2G service from a 3G service. Availability: per RA, per GPRS service Type: Counter | Int32
> comb-inter-rat-rau-total | Description: Total number of Combined Inter RAT RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> comb-inter-rat-rau-3g | Description: Total number of Combined Inter RAT RAU Requests received in a 3G service from a 2G service. Availability: per RA, per SGSN service Type: Counter | Int32
> comb-inter-rat-rau-2g | Description: Total number of Combined Inter RAT RAU Requests received in a 2G service from a 3G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-ps-inter-rat-rau-total | Description: Total number of retransmitted GPRS only Inter RAT RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-ps-inter-rat-rau-3g | Description: Total number of retransmitted GPRS only Inter RAT RAU Requests received in a 3G service from a 2G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-ps-inter-rat-rau-2g | Description: Total number of retransmitted GPRS only Inter RAT RAU Requests received in a 2G service from a 3G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-comb-inter-rat-rau-total | Description: Total number of retransmitted Combined Inter RAT RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-comb-inter-rat-rau-3g | Description: Total number of retransmitted Combined Inter RAT RAU Requests received in a 3G service from a 2G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-comb-inter-rat-rau-2g | Description: Total number of retransmitted Combined Inter RAT RAU Requests received in a 2G service from a 3G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ps-inter-service-rau-total | Description: Total number of GPRS only Inter Service RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ps-inter-service-rau-3g | Description: Total number of GPRS only Inter Service RAU Requests from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ps-inter-service-rau-2g | Description: Total number of GPRS only Inter Service RAU Requests from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> comb-inter-service-rau-total | Description: Total number of Combined Inter Service RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> comb-inter-service-rau-3g | Description: Total number of Combined Inter Service RAU Requests from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> comb-inter-service-rau-2g | Description: Total number of Combined Inter Service RAU Requests from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-ps-inter-service-rau-total | Description: Total number of retransmitted GPRS only Inter Service RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-ps-inter-service-rau-3g | Description: Total number of retransmitted GPRS only Inter Service RAU Requests from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-ps-inter-service-rau-2g | Description: Total number of retransmitted GPRS only Inter Service RAU Requests from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-comb-inter-service-rau-total | Description: Total number of retransmitted Combined Inter Service RAU Requests received in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-comb-inter-service-rau-3g | Description: Total number of retransmitted Combined Inter Service RAU Requests from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-comb-inter-service-rau-2g | Description: Total number of retransmitted Combined Inter Service RAU Requests from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ps-inter-rat-rau-acc-total | Description: Total number of GPRS only Inter RAT RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ps-inter-rat-rau-acc-3g | Description: Total number of GPRS only Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 2G service to a 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ps-inter-rat-rau-acc-2g | Description: Total number of GPRS only Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 3G service to a 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> comb-inter-rat-rau-acc-total | Description: Total number of Combined Inter RAT RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> comb-inter-rat-rau-acc-3g | Description: Total number of Combined Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 2G service to a 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> comb-inter-rat-rau-acc-2g | Description: Total number of Combined Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 3G service to a 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-ps-inter-rat-rau-acc-total | Description: Total number of retransmitted GPRS only Inter RAT RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-ps-inter-rat-rau-acc-3g | Description: Total number of retransmitted GPRS only Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 2G service to a 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-ps-inter-rat-rau-acc-2g | Description: Total number of retransmitted GPRS only Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 3G service to a 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-comb-inter-rat-rau-acc-total | Description: Total number of retransmitted Combined Inter RAT RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-comb-inter-rat-rau-acc-3g | Description: Total number of retransmitted Combined Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 3G service to a 2G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-comb-inter-rat-rau-acc-2g | Description: Total number of retransmitted Combined Inter RAT RAU Accepts sent against RAU Requests from subscribers moving from a 2G service to a 3G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ps-inter-service-rau-acc-total | Description: Total number of GPRS only Inter Service RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ps-inter-service-rau-acc-3g | Description: Total number of GPRS only Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ps-inter-service-rau-acc-2g | Description: Total number of GPRS only Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> comb-inter-service-rau-acc-total | Description: Total number of Combined Inter Service RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> comb-inter-service-rau-acc-3g | Description: Total number of Combined Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> comb-inter-service-rau-acc-2g | Description: Total number of Combined Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-ps-inter-service-rau-acc-total | Description: Total number of retransmitted GPRS only Inter Service RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-ps-inter-service-rau-acc-3g | Description: Total number of retransmitted GPRS only Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-ps-inter-service-rau-acc-2g | Description: Total number of retransmitted GPRS only Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ret-comb-inter-service-rau-acc-total | Description: Total number of retransmitted Combined Inter Service RAU Accepts sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ret-comb-inter-service-rau-acc-3g | Description: Total number of retransmitted Combined Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ret-comb-inter-service-rau-acc-2g | Description: Total number of retransmitted Combined Inter Service RAU Accepts sent against RAU Requests from subscribers moving from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ps-inter-rat-rau-rej-total | Description: Total number of GPRS only Inter RAT RAU Rejects sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ps-inter-rat-rau-rej-3g | Description: Total number of GPRS only Inter RAT RAU Rejects sent against RAU Requests for subscribers moving from 2G service to a 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ps-inter-rat-rau-rej-2g | Description: Total number of GPRS only Inter RAT RAU Rejects sent against RAU Requests for subscribers moving from 3G service to a 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> comb-inter-rat-rau-rej-total | Description: Total number of Combined Inter RAT RAU Rejects sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> comb-inter-rat-rau-rej-3g | Description: Total number of Combined Inter RAT RAU Rejects sent against RAU Requests for subscribers moving from 2G service to a 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> comb-inter-rat-rau-rej-2g | Description: Total number of Combined Inter RAT RAU Rejects sent against RAU Requests for subscribers moving from 3G service to a 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> ps-inter-service-rau-rej-total | Description: Total number of GPRS only Inter Service RAU Rejects sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> ps-inter-service-rau-rej-3g | Description: Total number of GPRS only Inter Service RAU Rejects sent against RAU Requests for subscribers moving from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> ps-inter-service-rau-rej-2g | Description: Total number of GPRS only Inter Service RAU Rejects sent against RAU Requests for subscribers moving from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> comb-inter-service-rau-rej-total | Description: Total number of Combined Inter Service RAU Rejects sent in both 2G and 3G services. Availability: per RA, per GPRS/SGSN service Type: Counter | Int32
> comb-inter-service-rau-rej-3g | Description: Total number of Combined Inter Service RAU Rejects sent against RAU Requests for subscribers moving from one 3G service to another 3G service. Availability: per RA, per SGSN service Type: Counter | Int32
> comb-inter-service-rau-rej-2g | Description: Total number of Combined Inter Service RAU Rejects sent against RAU Requests for subscribers moving from one 2G service to another 2G service. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-imsi-unknown-hlr | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “IMSI unknown at HLR”. Triggers:
> • | On HLR sending a bad response to a SAI-Req or GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-imsi-unknown-hlr | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “IMSI unknown at HLR”. Triggers:
> • | On HLR sending a bad response to a SAI-Req or GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-illegal-ms | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Illegal M”. Triggers:
> • | On HLR sending a bad response to a SAI-Req or GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-illegal-ms | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Illegal MS”.
> • | Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs.
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-illegal-me | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Illegal ME”. Triggers:
> • | Unable to retrieve IMEI/IMEISV from MS
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-illegal-me | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Illegal ME”. Triggers:
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-gprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-gprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-nongprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-nongprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-msid-not-derived-by-nw | Description: Total number of GPRS only Inter Service RAU Request Rejects sent with cause “MSID not derived by network” against Inter-Service-RAU Requests in 3G service. Triggers:
> • | On getting periodic RAU with old RAI as a non-local RAI
> • | When PTMSI-IE is missing in RAU
> • | When old RAI has invalid location area values (0x0000 or 0xfffe) for PTMSI-attaches/RAUs
> • | When getting a RAU with old RAI in 2G and PTMSI is unknown
> • | When getting PTMSI-SIG-MISMATCH for a SGSN Context Request sent with IMSI Validated
> • | When getting a RAU Request while an attach with the same peer-SGSN-PTMSI is in progress
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-msid-not-derived-by-nw | Description: Total number of GPRS only Inter Service RAU Request Rejects sent with cause “MSID not derived by network” against Inter-Service-RAU Requests in 2G service. Triggers:
> • | When SGSN-Context-Resp arrives with any cause other than “accepted”
> • | When GMM-Identity-Req with MS fails
> • | When GTP-Identity-Req with MS fails
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-implicitly-detach | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Implicitly detached”. Triggers:
> • | RAU at 3G when subscriber was detached from 2G
> • | When we get a different IMSI in SGSN Context Response for an SGSN Context Request sent with IMSI validated
> • | When we get RAU while awaiting a Detach Accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-implicitly-detach | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Implicitly detached”. Triggers:
> • | When we get an RAU from an unknown MS
> • | On T3350 expiry for the attach-accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-plmn-not-allowed | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-plmn-not-allowed | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-loc-area-not-allowed | Description: Total number of GPRS only Inter Service RAU rejects in 3G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-loc-area-not-allowed | Description: Total number of GPRS only Inter Service RAU rejects in 2G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-roam-not-allowed-larea | Description: Total number of GPRS only Inter Service RAU rejects in 3G service with cause “Roaming area not allowed in the given location area”. Triggers:
> • | When rejecting as a shared SGSN due to no operator accepting the given IMSI
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-roam-not-allowed-larea | Description: Total number of GPRS only Inter Service RAU rejects in 2G service with cause “Roaming area not allowed in the given location area”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-gprs-svc-not-allowed-plmn | Description: Total number of GPRS only RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Intter-Service-RAU Requests in 3G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-gprs-svc-not-allowed-plmn | Description: Total number of GPRS only RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Intter-Service-RAU Requests in 2G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-no-cells-in-location-area | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-no-cells-in-location-area | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-msc-not-reachable | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-msc-not-reachable | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-network-failure | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Network Failure”. Triggers:
> • | RNC is overloaded
> • | Not enough credits at session manager
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | Too many IUs for the same IMSI
> • | On getting a RAU with a peer SGSN PTMSI when another Attach is ongoing with the same PTMSI
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-network-failure | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Network Failure”. Triggers:
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | On XID failure for RAU
> • | Inability to send an SGSN-Ctx-Req out for an RAU.
> • | Inability to send a Check-IMEI Request out
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-mac-failure | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-mac-failure | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-syn-failure | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-syn-failure | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-congestion | Description: Total number of GPRS Only Inter Service RAU Rejects in 3G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-congestion | Description: Total number of GPRS Only Inter Service RAU Rejects in 2G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-gsm-auth-unacceptable | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-gsm-auth-unacceptable | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-no-pdp-ctx-actv | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-no-pdp-ctx-actv | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-retry-from-new-cell | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-retry-from-new-cell | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-sem-wrong-msg | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-sem-wrong-msg | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-inval-mand-info | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-inval-mand-info | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-msg-type-non-exist | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-msg-type-non-exist | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-mtype-incompat-pstate | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-mtype-incompat-pstate | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-ie-non-existent | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-ie-non-existent | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-cond-ie-error | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-cond-ie-error | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-msg-not-compat-pstate | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “message not compatible with protocol state”. Triggers:
> • | When getting an Attach Request before getting Relocation-complete during SRNS
> • | When getting periodic RAU in a direct transfer message
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-msg-not-compat-pstate | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “message not compatible with protocol state”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-prot-error | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “protocol error”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-prot-error | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “protocol error”. Triggers:
> • | When the PLMN ID in BSSGP message does not match the configured PLMN at GPRS service
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-ps-rej-unknown-error | Description: Total number of GPRS only Inter Service RAU Rejects in 3G service with cause “unknown error”. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-ps-rej-unknown-error | Description: Total number of GPRS only Inter Service RAU Rejects in 2G service with cause “unknown error”. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-imsi-unknown-hlr | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “IMSI unknown at HLR”. Triggers:
> • | On HLR sending a bad response to a SAI-Req/GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-imsi-unknown-hlr | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “IMSI unknown at HLR”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-illegal-ms | Description: Total number of Combined Inter Service RAU rejects in 3G service with cause “Illegal MS”. Triggers:
> • | Unable to retrieve IMEI/IMEISV from MS
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-illegal-ms | Description: Total number of Combined Inter Service RAU rejects in 2G service with cause “Illegal MS”. Triggers:
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-illegal-me | Description: Total number of Combined Inter Service RAU rejects in 3G service with cause “Illegal ME”. Triggers:
> • | Unable to retrieve IMEI/IMEISV from MS
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-illegal-me | Description: Total number of Combined Inter Service RAU rejects in 2G service with cause “Illegal ME”. Triggers:
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-gprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-gprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-nongprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-nongprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-msid-not-derived-by-nw | Description: Total number of Combined Inter Service RAU Request Rejects sent with cause “MSID not derived by network” against Inter-Service-RAU Requests in 3G service. Triggers:
> • | On getting periodic RAU with old RAI as a non-local RAI
> • | When PTMSI-IE is missing in RAU
> • | When old RAI has invalid location area values (0x0000 or 0xfffe) for PTMSI-attaches/RAUs
> • | When getting a RAU with old RAI in 2G and PTMSI is unknown
> • | When getting PTMSI-SIG-MISMATCH for a SGSN Context Request sent with IMSI Validated
> • | When getting a RAU Request while an attach with the same peer-SGSN-PTMSI is in progress
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-msid-not-derived-by-nw | Description: Total number of Combined Inter Service RAU Request Rejects sent with cause “MSID not derived by network” against Inter-Service-RAU Requests in 2G service. Triggers:
> • | When SGSN-Context-Resp arrives with any cause other than “accepted”
> • | When GMM-Identity-Req with MS fails
> • | When GTP-Identity-Req with MS fails
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-implicitly-detach | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Implicitly detached”. Triggers:
> • | RAU at 3G when subscriber was detached from 2G
> • | When we get a different IMSI in SGSN Context Response for an SGSN Context Request sent with IMSI validated
> • | When we get RAU while awaiting a Detach Accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-implicitly-detach | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Implicitly detached”. Triggers:
> • | When we get an RAU from an unknown MS
> • | On T3350 expiry for the attach-accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-plmn-not-allowed | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-plmn-not-allowed | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-loc-area-not-allowed | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-loc-area-not-allowed | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-roam-not-allowed-larea | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Roaming area not allowed in the given location area”. Triggers:
> • | When rejecting as a shared SGSN due to no operator accepting the given IMSI
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-roam-not-allowed-larea | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Roaming area not allowed in the given location area”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-gprs-svc-not-allowed-plmn | Description: Total number of Combined RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Intter-Service-RAU Requests in 3G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-gprs-svc-not-allowed-plmn | Description: Total number of Combined RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Intter-Service-RAU Requests in 2G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-no-cells-in-location-area | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-no-cells-in-location-area | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-msc-not-reachable | Description: Total number of Combined Inter Service RAU rejects in 3G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-msc-not-reachable | Description: Total number of Combined Inter Service RAU rejects in 2G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-network-failure | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Network Failure”. Triggers:
> • | RNC is overloaded
> • | Not enough credits at session manager
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | Too many IUs for the same IMSI
> • | On getting a RAU with a peer SGSN PTMSI when another Attach is ongoing with the same PTMSI
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-network-failure | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Network Failure”. Triggers:
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | On XID failure for RAU
> • | Inability to send an SGSN-Ctx-Req out for an RAU
> • | Inability to send a Check-IMEI Request out
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-mac-failure | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-mac-failure | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-syn-failure | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-syn-failure | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-congestion | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-congestion | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-gsm-auth-unacceptable | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-gsm-auth-unacceptable | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-no-pdp-ctx-actv | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-no-pdp-ctx-actv | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-retry-from-new-cell | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-retry-from-new-cell | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-sem-wrong-msg | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-sem-wrong-msg | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-inval-mand-info | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-inval-mand-info | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-msg-type-non-exist | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-msg-type-non-exist | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-mtype-incompat-pstate | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-mtype-incompat-pstate | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-ie-non-existent | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-ie-non-existent | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-cond-ie-error | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-cond-ie-error | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-msg-not-compat-pstate | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “message not compatible with protocol state”. Triggers:
> • | When getting an Attach Request before getting Relocation-complete during SRNS
> • | When getting periodic RAU in a direct transfer message
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-msg-not-compat-pstate | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “message not compatible with protocol state”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-prot-error | Description: Total number of Combined Inter Service RAU rejects in 3G service with cause “protocol error”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-prot-error | Description: Total number of Combined Inter Service RAU rejects in 2G service with cause “protocol error”. Triggers:
> • | When the PLMN ID in BSSGP message does not match the configured PLMN at GPRS service
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-isrv-comb-rej-unknown-error | Description: Total number of Combined Inter Service RAU Rejects in 3G service with cause “unknown error”. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-isrv-comb-rej-unknown-error | Description: Total number of Combined Inter Service RAU Rejects in 2G service with cause “unknown error”. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-imsi-unknown-hlr | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “IMSI unknown at HLR”. Triggers:
> • | On HLR sending a bad response to SAI-Req/GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-imsi-unknown-hlr | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “IMSI unknown at HLR”. Triggers:
> • | On HLR sending a bad response to SAI-Req/GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-illegal-ms | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Illegal MS”. Triggers:
> • | On HLR sending a bad response to SAI-Req/GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-illegal-ms | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Illegal MS”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-illegal-me | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Illegal ME”. Triggers:
> • | Unable to retrieve IMEI/IMEISV from MS
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-illegal-me | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Illegal ME”. Triggers:
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-gprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-gprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-nongprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-nongprs-svc-not-allow | Description: Total number of GPRS only Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-msid-not-derived-by-nw | Description: Total number of GPRS only inter-service routing area update request rejects sent with cause “MSID not derived by network” against Inter-Service-RAU requests in 3G service. Triggers:
> • | On getting periodic RAU with old RAI as a non-local RAI
> • | When PTMSI-IE is missing in RAU
> • | When old RAI has invalid location area values (0x0000 or 0xfffe) for PTMSI-attaches/RAUs
> • | When getting a RAU with old RAI in 2G and PTMSI is unknown
> • | When getting PTMSI-SIG-MISMATCH for a SGSN Context Request sent with IMSI Validated
> • | When getting a RAU Request while an attach with the same peer-SGSN-PTMSI is in progress
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-msid-not-derived-by-nw | Description: Total number of GPRS only inter-service routing area update request rejects sent with cause “MSID not derived by network” against Inter-Service-RAU requests in 3G service. Triggers:
> • | When SGSN-Context-Resp arrives with any cause other than “accepted”
> • | When GMM-Identity-Req with MS fails
> • | When GTP-Identity-Req with MS fails
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-implicitly-detach | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Implicitly detached”. Triggers:
> • | RAU at 3G when subscriber was detached from 2G
> • | When we get a different IMSI in SGSN Context Response for an SGSN Context Request sent with IMSI validated
> • | When we get RAU while awaiting a Detach Accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-implicitly-detach | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Implicitly detached”. Triggers:
> • | When we get an RAU from an unknown MS
> • | On T3350 expiry for the Attach-accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-plmn-not-allowed | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-plmn-not-allowed | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-loc-area-not-allowed | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-loc-area-not-allowed | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-roam-not-allowed-larea | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Roaming area not allowed in the given location area”. Triggers:
> • | When rejecting as a shared SGSN due to no operator accepting the given IMSI
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-roam-not-allowed-larea | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Roaming area not allowed in the given location area”. Triggers:
> • | When rejecting as a shared SGSN due to no operator accepting the given IMSI
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-gprs-svc-not-allowed-plmn | Description: Total number of GPRS only RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Inter-Service-RAU Requests in 3G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-gprs-svc-not-allowed-plmn | Description: Total number of GPRS only RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Inter-Service-RAU Requests in 2G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-no-cells-in-location-area | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-no-cells-in-location-area | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-msc-not-reachable | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-msc-not-reachable | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-network-failure | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Network Failure”. Triggers:
> • | RNC is overloaded
> • | Not enough credits at session manager
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | Too many IUs for the same IMSI
> • | On getting a RAU with a peer SGSN PTMSI when another Attach is ongoing with the same PTMSI
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-network-failure | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Network Failure”. Triggers:
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | On XID failure for RAU
> • | Inability to send an SGSN-Ctx-Req out for an RAU.
> • | Inability to send a Check-IMEI Request out
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-mac-failure | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-mac-failure | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-syn-failure | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-syn-failure | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-congestion | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-congestion | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-gsm-auth-unacceptable | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-gsm-auth-unacceptable | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-no-pdp-ctx-actv | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-no-pdp-ctx-actv | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-retry-from-new-cell | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-retry-from-new-cell | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-sem-wrong-msg | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-sem-wrong-msg | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-inval-mand-info | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-inval-mand-info | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-msg-type-non-exist | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-msg-type-non-exist | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-mtype-incompat-pstate | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-mtype-incompat-pstate | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-ie-non-existent | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-ie-non-existent | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-cond-ie-error | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-cond-ie-error | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-msg-not-compat-pstate | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “message not compatible with protocol state”. Triggers:
> • | When getting an Attach Request before getting Relocation-complete during SRNS
> • | When getting periodic RAU in a direct transfer message
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-msg-not-compat-pstate | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “message not compatible with protocol state”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-prot-error | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “protocol error”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-prot-error | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “protocol error”. Triggers:
> • | When the PLMN ID in BSSGP message does not match the configured PLMN at GPRS service
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-ps-rej-unknown-error | Description: Total number of GPRS only Inter RAT RAU Rejects in 3G service with cause “unknown error”. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-ps-rej-unknown-error | Description: Total number of GPRS only Inter RAT RAU Rejects in 2G service with cause “unknown error”. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-imsi-unknown-hlr | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “IMSI unknown at HLR”. Triggers:
> • | On HLR sending a bad response to a SAI-Req/GLU-Req
> • | On getting zero auth vectors for HLR for a SAI-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-imsi-unknown-hlr | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “IMSI unknown at HLR”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-illegal-ms | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Illegal MS”. Triggers:
> • | Unable to retrieve IMEI/IMEISV from MS
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-illegal-ms | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Illegal MS”. Triggers:
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-illegal-me | Description: Total number of Combined Inter RAT RAU rejects in 3G service with cause “Illegal ME”. Triggers:
> • | Unable to retrieve IMEI/IMEISV from MS
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-illegal-me | Description: Total number of Combined Inter RAT RAU rejects in 3G service with cause “Illegal ME”. Triggers:
> • | On IMEI verification failure with EIR
> • | On getting unknown equipment failure from EIR/HLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-gprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-gprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS services not allowed in this PLMN” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting a cl (subs-with) while an attach/RAU is in progress
> • | On getting “Subscriber Unknown” failure from HLR for SAI-Req/GLU-Req
> • | For rejecting attaches due to subscriber control inactivity
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-nongprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 3G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-nongprs-svc-not-allow | Description: Total number of Combined Inter Service RAU Rejects sent with cause “GPRS and non-GPRS service not allowed for subscriber” against Inter-service-RAU Requests in 2G service. Triggers:
> • | On getting “IMSI unknown” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-msid-not-derived-by-nw | Description: Total number of Combined Inter Service RAU Request Rejects sent with cause “MSID not derived by network” against Inter-Service-RAU Requests in 3G service. Triggers:
> • | On getting periodic RAU with old RAI as a non-local RAI
> • | When PTMSI-IE is missing in RAU
> • | When old RAI has invalid location area values (0x0000 or 0xfffe) for PTMSI-attaches/RAUs
> • | When getting a RAU with old RAI in 2G and PTMSI is unknown
> • | When getting PTMSI-SIG-MISMATCH for a SGSN Context Request sent with IMSI Validated
> • | When getting a RAU Request while an attach with the same peer-SGSN-PTMSI is in progress
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-msid-not-derived-by-nw | Description: Total number of Combined Inter Service RAU Request Rejects sent with cause “MSID not derived by network” against Inter-Service-RAU Requests in 2G service. Triggers:
> • | When SGSN-Context-Resp arrives with any cause other than “accepted”
> • | When GMM-Identity-Req with MS fails
> • | When GTP-Identity-Req with MS fails
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-implicitly-detach | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Implicitly detached”. Triggers:
> • | RAU at 3G when subscriber was detached from 2G
> • | When we get a different IMSI in SGSN Context Response for an SGSN Context Request sent with IMSI validated
> • | When we get RAU while awaiting a Detach Accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-implicitly-detach | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Implicitly detached”. Triggers:
> • | When we get an RAU from an unknown MS
> • | On T3350 expiry for the attach-accept
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-plmn-not-allowed | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-plmn-not-allowed | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “PLMN not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-loc-area-not-allowed | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-loc-area-not-allowed | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Location area not allowed”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-roam-not-allowed-larea | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Roaming area not allowed in the given location area”. Triggers:
> • | When rejecting as a shared SGSN due to no operator accepting the given IMSI
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-roam-not-allowed-larea | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Roaming area not allowed in the given location area”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-gprs-svc-not-allowed-plmn | Description: Total number of Combined RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Inter-Service-RAU Requests in 3G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-gprs-svc-not-allowed-plmn | Description: Total number of Combined RAU Rejects sent with cause “GPRS service not allowed in this PLMN” against Inter-Service-RAU Requests in 2G service. Triggers:
> • | On getting “Roaming not allowed” from HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-no-cells-in-location-area | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-no-cells-in-location-area | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “No cells in location area”. Triggers:
> • | On getting “UMTS access control” from Siemens HLR for SAI-Req/GLU-Req
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-msc-not-reachable | Description: Total number of Combined Inter RAT RAU rejects in 3G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-msc-not-reachable | Description: Total number of Combined Inter RAT RAU rejects in 2G service with cause “MSC not reachable”. Triggers:
> • | On sending an attach/RAU Accept with cause “GPRS only attached” or “RA updated” for a combined CS/PS request either because:
> • | the request is timed out
> • | inability to send to VLR
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-network-failure | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Network Failure”. Triggers:
> • | RNC is overloaded
> • | Not enough credits at session manager
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | Too many IUs for the same IMSI
> • | On getting a RAU with a peer SGSN PTMSI when another Attach is ongoing with the same PTMSI
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-network-failure | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Network Failure”. Triggers:
> • | On getting cause “data missing from HLR” in SAI-Req/GLU-Req
> • | On XID failure for RAU
> • | Inability to send an SGSN-Ctx-Req out for an RAU
> • | Inability to send a Check-IMEI Request out
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-mac-failure | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-mac-failure | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Message Authenticate Code (MAC) Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-syn-failure | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-syn-failure | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Context Synchronization Failure”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-congestion | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-congestion | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Network Congestion”. Triggers:
> • | On congestion, if configured for attach-throttling
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-gsm-auth-unacceptable | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-gsm-auth-unacceptable | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “GSM Authentication unacceptable”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-no-pdp-ctx-actv | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-no-pdp-ctx-actv | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “PDP context not activated”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-retry-from-new-cell | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-retry-from-new-cell | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Subscriber retried from a new cell”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-sem-wrong-msg | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-sem-wrong-msg | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Semantically wrong message”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-inval-mand-info | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-inval-mand-info | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Invalid Mandatory Info”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-msg-type-non-exist | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-msg-type-non-exist | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Message type does not exist”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-mtype-incompat-pstate | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-mtype-incompat-pstate | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Message type not compatible with protocol state”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-ie-non-existent | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-ie-non-existent | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “Information element not existent”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-cond-ie-error | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-cond-ie-error | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “error in conditional informational element”. Triggers:
> • | On decode failure of messages
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-msg-not-compat-pstate | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “message not compatible with protocol state”. Triggers:
> • | When getting an Attach Request before getting Relocation-complete during SRNS
> • | When getting periodic RAU in a direct transfer message
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-msg-not-compat-pstate | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “message not compatible with protocol state”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-prot-error | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “protocol error”. Triggers: Increments when operator policy is configured with this value as the reject cause for attaches/RAUs. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-prot-error | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “protocol error”. Triggers:
> • | When the PLMN ID in BSSGP message does not match the configured PLMN at GPRS service
> • | When operator policy is configured with this value as the reject cause for attaches/RAUs
> Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-irat-comb-rej-unknown-error | Description: Total number of Combined Inter RAT RAU Rejects in 3G service with cause “unknown error”. Availability: per RA, per SGSN service Type: Counter | Int32
> 2G-irat-comb-rej-unknown-error | Description: Total number of Combined Inter RAT RAU Rejects in 2G service with cause “unknown error”. Availability: per RA, per GPRS service Type: Counter | Int32
> 3G-ms-init-detach | Description: Total number of MS initiated Detach Requests of type 'GPRS Detach' received for 3G service. Triggers: Increments when the MS initiates a Detach Request. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-ms-init-detach | Description: Total number of MS initiated Detach Requests of type 'GPRS Detach' received for 2G service. Triggers: Increments when the MS initiates a Detach Request. Availability: per GPRS service Type: Counter | Int32
> 3G-ms-init-imsi-detach | Description: Total number of MS initiated Detach Requests of type 'Imsi Detach' received for 3G service. Triggers: Increments when the MS initiates a Detach Request. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-ms-init-imsi-detach | Description: Total number of MS initiated Detach Requests of type 'Imsi Detach' received for 2G service. Triggers: Increments when the MS initiates a Detach Request. Availability: per GPRS service Type: Counter | Int32
> 3G-ms-init-comb-detach | Description: Total number of MS initiated GPRS and IMSI (PS and CS) Detach Requests of type 'Combined Gprs/Imsi Detach' received for 3G service. Triggers: Increments when the MS initiates a Detach Request. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-ms-init-comb-detach | Description: Total number of MS initiated GPRS and IMSI (PS and CS) Detach Requests of type 'Combined Gprs/Imsi Detach' received for 2G service. Triggers: Increments when the MS initiates a Detach Request. Availability: per GPRS service Type: Counter | Int32
> 3G-nw-init-detach | Description: Total number of network initiated Detach Request procedures sent for 3G service. Triggers: 1. When a subscriber cleared by Administrator/operator. 2. When “Cancel Location” received from HLR. 3. When stand-alone DSD is received with “All GPRS Subscription withdrawn”. 4. When subscriber-control-inactivity timer expires and action is to detach immediately. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-nw-init-detach | Description: Total number of network initiated Detach Request procedures received for 2G service. Triggers: 1. When a subscriber cleared by Administrator/operator. 2. When “Cancel Location” received from HLR. 3. When stand-alone DSD is received with “All GPRS Subscription withdrawn”. 4. When subscriber-control-inactivity timer expires and action is to detach immediately. Availability: per GPRS service, per RA Type: Counter | Int32
> 3G-ms-init-detach-accept | Description: Total number of 3G service MS-initiated Detach Accept messages received by the SGSN and sent by the mobile station (MS) in response to network-initiated Detach Request messages. Triggers: Increments when a Detach Accept is received from an MS. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-ms-init-detach-accept | Description: Total number of 2G service MS-initiated Detach Accept messages received by the SGSN and sent by the mobile station (MS) in response to network-initiated Detach Request messages. Triggers: Increments when a Detach Accept is received from an MS. Availability: per GPRS service Type: Counter | Int32
> 3G-nw-init-detach-accept | Description: Total number of Network initiated Detach Accept messages in response to requests of type 'Gprs Detach' in 3G service. Triggers: Increments when the network accepts a detach initiated by the MS. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-nw-init-imsi-detach-accept | Description: Total number of Network initiated IMSI (CS) Detach Accept messages in response to requests of type 'Imsi Detach' in 3G service. Triggers: Increments when the network accepts a detach initiated by the MS. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-nw-init-comb-detach-accept | Description: Total number of Network initiated combined (GPRS and IMSI) Detach Accept messages in response to requests of type 'Combined Gprs/Imsi Detach' in 3G service. Triggers: Increments when the network accepts a detach initiated by the MS. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-nw-init-detach-accept | Description: Total number of Network initiated Detach Accept messages in response to requests of type 'Gprs Detach' in 2G service. Triggers: Increments when the network accepts a detach initiated by the MS. Availability: per GPRS service Type: Counter | Int32
> 2G-nw-init-imsi-detach-accept | Description: Total number of Network initiated IMSI (CS) Detach Accept messages in response to requests of type 'Imsi Detach' in 2G service. Triggers: Increments when the network accepts a detach initiated by the MS. Availability: per GPRS service Type: Counter | Int32
> 2G-nw-init-comb-detach-accept | Description: Total number of Network initiated combined (GPRS and IMSI) Detach Accept messages in response to requests of type 'Combined Gprs/Imsi Detach' in 2G service. Triggers: Increments when the network accepts a detach initiated by the MS. Availability: per GPRS service Type: Counter | Int32
> 3G-signalling-service-request | Description: Total number of Service Request messages received for type "Signalling" in 3G service. Triggers: Increments when the MS initiates a Serving Request message. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-signalling-service-request | This statistics has been obsoleted. | Int32
> 3G-data-service-request | Description: Total number of Service Request messages received for type "Data" in 3G service. Triggers: Increments when the MS initiates a Serving Request message. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-data-service-request | This statistics has been obsoleted. | Int32
> 3G-service-response | Description: Total number of Service Accept messages sent by the network in 3G service. Triggers: Increments when the SGSN receives and accepts a Serving Request message in connected state. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-response | This statistics has been obsoleted. | Int32
> 3G-service-reject | Description: Total number of Service Reject messages sent by the network in 3G service. Triggers: A derived counter. See individual counters for trigger points. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-reject | This statistics has been obsoleted. | Int32
> 3G-service-rej-netwk-fail | Description: Total number of Service Request messages rejected for 3G service due to network failure. Triggers:
> • | When we initiate SAI towards HLR but we get no SAI response
> • | Too many Iu’s to the same MM context
> • | RNC overload
> Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-netwk-fail | This statistics has been obsoleted. | Int32
> 3G-service-rej-imsi-unknown-at-hlr | Description: Total number of Service Request messages rejected for 3G service due to unknown IMSI in HLR. Triggers: Increments when we initiate SAI towards HLR but we get an 'imsi not known' from HLR. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-imsi-unknown-at-hlr | This statistics has been obsoleted. | Int32
> 3G-service-rej-msid-not-derived-by-nwtk | Description: Total number of Service Request messages rejected for 3G service as MSID can not derived by network from message. Triggers: Increments when we get an unknown PTMSI service request from an MS. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-msid-not-derived-by-nwtk | This statistics has been obsoleted. | Int32
> 3G-service-rej-implicity-detach | Description: Total number of Service Request messages rejected for 3G service due to implicitly detach. Triggers: Increments when we get a service request from an MS that is already detached. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-implicity-detach | This statistics has been obsoleted. | Int32
> 3G-service-rej-illegal-ms | Description: Total number of Service Request messages rejected for 3G service due to illegal mobile subscriber. Triggers: Increments when authentication fails on a service request. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-illegal-ms | This statistics has been obsoleted. | Int32
> 3G-service-rej-msg-not-compat-prot-state | Description: Total number of Service Request messages rejected for 3G service as message is not compatible with protocol state. Triggers: Increments when we get a service request for ongoing authentication or attach. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-msg-not-compat-prot-state | This statistics has been obsoleted. | Int32
> 3G-service-rej-no-pdp-ctx-actv | Description: Total number of Service Request messages rejected for 3G service as no PDP context is activated. Triggers: Increments when we get a service request of type ‘data’ and we have no PDP contexts activated. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-no-pdp-ctx-actv | This statistics has been obsoleted. | Int32
> 3G-service-rej-sem-wrong-msg | Description: Total number of Service Request messages rejected for 3G service as request message is semantically wrong. Triggers: Increments when a decode failure happens on a service request. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-service-rej-unknown-cause | Description: Total number of 3G Service Request messages rejected for unknown causes. Any number other than zero (0) indicates a software problem. This counter is new in release 9.0. Triggers: Increments when a 3G Service Request is rejected. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-service-rej-sem-wrong-msg | This statistic has been obsoleted in release 9.0. Description: Total number of Service Request messages rejected for 2G service as request message is semantically wrong. Triggers: Increments when a decode failure happens on a service request. Availability: per GPRS service, per RA Type: Counter | Int32
> 3G-paging-request | Description: Total number of 3G service Paging Request messages originated by SGSN and sent to the Radio Network Controller (RNC) to contact mobile stations (MS). Triggers: 1. Subscriber is in standby state and SGSN has some downlink signalling activity to do for network initiated detach procedure or downlink SM-messages (like modify-PDP-Request) to be sent. 2. Downlink data is to be sent to a standby subscriber Availability: per SGSN service Type: Counter | Int32
> 2G-paging-request | Description: Total number of 2G service Paging Request messages originated by SGSN and sent to the Radio Network Controller (RNC) to contact mobile stations (MS). Triggers: 1. Subscriber is in standby state and SGSN has some downlink signalling activity to do for network initiated detach procedure or downlink SM-messages (like modify-PDP-Request) to be sent. 2. Downlink data is to be sent to a standby subscriber. Availability: per GPRS service Type: Counter | Int32
> 3G-ret-paging-request | Total paging request messages retransmitted in packet switching (PS) domain for 3G service. | Int32
> 2G-ret-paging-request | Total paging request messages retransmitted in packet switching (PS) domain for 2G service. | Int32
> 3G-paging-success | Description: Total number of successful paging responses in 3G service. Triggers: Any successful Iu passing security started after Paging is started. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-paging-success | Description: Total number of successful paging responses in 2G service. Triggers: Any LLC uplink frame received after a Page-Request is sent to MS. Availability: per GPRS service Type: Counter | Int32
> 3G-cs-page-request | Total paging request messages in circuit switching (CS) domain for 3G service. | Int32
> 2G-cs-page-request | Total paging request messages in circuit switching (CS) domain for 2G service. | Int32
> 3G-cs-page-response | Total paging request response messages sent in circuit switching (CS) domain for 3G service. | Int32
> 2G-cs-page-response | Total paging request response messages sent in circuit switching (CS) domain for 2G service. | Int32
> 3G-gmm-status-sent | Total GPRS mobility management procedure status messages sent for 3G service. | Int32
> 2G-gmm-status-sent | Total GPRS mobility management procedure status messages sent for 2G service. | Int32
> 3G-gmm-status-rcvd | Total GPRS mobility management procedure status messages received for 3G service. | Int32
> 2G-gmm-status-rcvd | Total GPRS mobility management procedure status messages received for 2G service. | Int32
> 3G-gmm-info-sent | Total messages sent with GPRS mobility management information for 3G service. | Int32
> 2G-gmm-info-sent | Total messages sent with GPRS mobility management information for 2G service. | Int32
> 3G-auth-cipher-request | Description: Total authentication and ciphering request messages for 3G service. Triggers: Whenever authentication procedure is initiated. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-auth-cipher-request | Description: Total authentication and ciphering request messages for 2G service. Triggers: Whenever authentication procedure is initiated. Availability: per GPRS service Type: Counter | Int32
> 3G-ret-auth-cipher-request | Total authentication and ciphering request messages retransmitted for 3G service. | Int32
> 2G-ret-auth-cipher-request | Total authentication and ciphering request messages retransmitted for 2G service. | Int32
> 3G-auth-cipher-response | Description: Total authentication and ciphering request response messages for 3G service. Triggers: Whenever the MS sends a authentication and cipher response message. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-auth-cipher-response | Description: Total authentication and ciphering request response messages for 2G service. Triggers: Whenever the MS sends a authentication and cipher response message. Availability: per GPRS service Type: Counter | Int32
> 3G-auth-cipher-rsp-sres-mismatch | Total authentication and ciphering request response messages having Signed RESponse (SRES) mismatch for 3G service. | Int32
> 2G-auth-cipher-rsp-sres-mismatch | Total authentication and ciphering request response messages having Signed RESponse (SRES) mismatch for 2G service. | Int32
> 3G-auth-cipher-reject | Total authentication and ciphering request reject messages for 3G service. | Int32
> 2G-auth-cipher-reject | Total authentication and ciphering request reject messages for 2G service. | Int32
> 3G-auth-cipher-rej-xres-mismatch | Total authentication and ciphering requests rejected for 3G service due to mismatch in expected authentication response (XRES) from subscriber. | Int32
> 2G-auth-cipher-rej-xres-mismatch | Total authentication and ciphering requests rejected for 2G service due to mismatch in expected authentication response (XRES) from subscriber | Int32
> 3G-auth-cipher-rej-sync-not-have-auts | Total authentication and ciphering requests rejected for 3G service where synchronization is missing Authentication Token for Re-synchronization (AUTS). | Int32
> 2G-auth-cipher-rej-sync-not-have-auts | Total authentication and ciphering requests rejected for 2G service where synchronization is missing Authentication Token for Re-synchronization (AUTS). | Int32
> 3G-auth-cipher-rej-many-sync-fail | Total authentication and ciphering requests rejected for 3G service due to synchronization failure beyond allowed number of time. | Int32
> 2G-auth-cipher-rej-many-sync-fail | Total authentication and ciphering requests rejected for 3G service due to synchronization failure beyond allowed number of time. | Int32
> 3G-auth-cipher-rej-many-mac-fail | Total authentication and ciphering requests rejected for 3G service due to message authentication code failure beyond allowed number of time. | Int32
> 2G-auth-cipher-rej-many-mac-fail | Total authentication and ciphering requests rejected for 2G service due to message authentication code failure beyond allowed number of time. | Int32
> 3G-auth-cipher-mac-fail | Description: Total authentication and ciphering failed due to message authentication code (MAC) failure in 3G service. Triggers: When a authorization and cipher failure message is received with this cause. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-auth-cipher-mac-fail | Description: Total authentication and ciphering failed due to message authentication code (MAC) failure for 2G service. Triggers: When a authorization and cipher failure message is received with this cause. Availability: per GPRS service Type: Counter | Int32
> 3G-auth-cipher-syn-fail | Description: Total number of authentication and cipher procedure failures messages received with cause “SYNC failure” in 3G service. Triggers: When a authorization and cipher failure message is received with this cause. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-auth-cipher-syn-fail | Description: Total number of authentication and cipher procedure failures messages received with cause “SYNC failure” in 2G service. Triggers: When a authorization and cipher failure message is received with this cause. Availability: per GPRS service Type: Counter | Int32
> 3G-auth-unacceptable | Description: Total number of authentication and cipher procedure fail messages received with cause “authentication unacceptable” in 3G service. Triggers: When a authorization and cipher failure message is received with this cause. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-auth-unacceptable | Indicates the number of authentication and cipher procedure fail messages received with cause “authentication unacceptable” in 2G service. Triggers: When a authorization and cipher failure message is received with this cause. Availability: per GPRS service Type: Counter | Int32
> 3G-ptmsi-realloc | Total Packet-Temporary Mobile Subscriber Identity reallocation procedure for 3G service. | Int32
> 2G-ptmsi-realloc | Total Packet-Temporary Mobile Subscriber Identity reallocation procedure for 2G service. | Int32
> 3G-ret-ptmsi-realloc | Total Packet-Temporary Mobile Subscriber Identity reallocation messages retransmitted for 3G service. | Int32
> 2G-ret-ptmsi-realloc | Total Packet-Temporary Mobile Subscriber Identity reallocation procedure messages retransmitted for 2G service. | Int32
> 3G-ptmsi-realloc-complete | Description: Total number of PTMSI-Reallocation Complete messages received at 3G. Triggers: Increments when we receive a PTMSI Realloc Complete from MS in 3G. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-ptmsi-realloc-complete | Description: Total number of PTMSI-Reallocation Complete messages received at 2G. Triggers: Increments when we receive a PTMSI Realloc Complete from MS in 2G. Availability: per GPRS service Type: Counter | Int32
> 3G-imsi-identity-request | Description: Total number of identity request messages sent with identity type as “IMSI” in 3G service. Triggers: When the SGSN initiates a Identity request to know the IMSI of the subscriber. This is done when: - Unknown local P-TMSI attach is received. - GTP-Identity with peer SGSN failed on a peer SGSN P-TMSI attach. - Authenticate response X-RES mismatch and the IMSI was not ascertained from the MS itself. - On a MAC failure and the IMSI was not ascertained from the MS itself. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-imsi-identity-request | Description: Total number of identity request messages sent with identity type as “IMSI” in 2G service. Triggers: When the SGSN initiates an identity request to know the IMSI of the subscriber due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per GPRS service Type: Counter | Int32
> 3G-imei-identity-request | Description: Total number of identity request messages sent with identity type as “IMEI” for 3G service. Triggers: When the SGSN initiates an identity request to know the IMEI of the UE due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per SGSN service Type: Counter | Int32
> 2G-imei-identity-request | Description: Total number of identity request messages sent with identity type as “IMEI” for 2G service. Triggers: When the SGSN initiates an identity request to know the IMEI of the subscriber due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per GPRS service Type: Counter | Int32
> 3G-imeisv-identity-request | Description: Total number of identity request messages sent with identity type as “IMEI-SV” for 3G service. Triggers: When the SGSN initiates an identity request to know the IMEI-SV of the UE due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-imeisv-identity-request | Description: Total number of identity request messages sent with identity type as “IMEI-SV” for 2G service. Triggers: When the SGSN initiates an identity request to know the IMEI-SV of the subscriber due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per GPRS service Type: Counter | Int32
> 3G-tmsi-identity-request | Description: Total number of identity request messages sent with identity type as “T-IMSI” for 3G service. Triggers: When the SGSN initiates an identity request to know the temporary IMSI of the subscriber due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-tmsi-identity-request | Description: Total number of identity request messages sent with identity type as “IMSI” for 2G service. Triggers: When the SGSN initiates an identity request to know the IMSI of the subscriber due to unknown local-PTMSI attach is received or GTP identity with Peer SGSN failed on a Peer SGSN PTMSI attach. Availability: per GPRS service Type: Counter | Int32
> 3G-ret-imsi-identity-request | Total number of IMSI identity request messages retransmitted for 3G service. | Int32
> 2G-ret-imsi-identity-request | Total number of IMSI identity request messages retransmitted for 2G service. | Int32
> 3G-ret-imei-identity-request | Total number of IMEI identity request messages retransmitted for 3G service. | Int32
> 2G-ret-imei-identity-request | Total number of IMEI identity request messages retransmitted for 2G service. | Int32
> 3G-ret-imeisv-identity-request | Total number of IMEI-SV identity request messages retransmitted for 3G service. | Int32
> 2G-ret-imeisv-identity-request | Total number of IMEI-SV identity request messages retransmitted for 2G service. | Int32
> 3G-ret-tmsi-identity-request | Total number of temporary IMS identity request messages retransmitted for 3G service. | Int32
> 2G-ret-tmsi-identity-request | Total number of temporary IMSI identity request messages retransmitted for 2G service. | Int32
> 3G-imsi-identity-response | Description: Total number of identity response messages received with MS identity of type “IMSI” for 3G service. Triggers: When the SGSN receives an Identity response initiated to an identity request initiated of identity type IMSI. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-imsi-identity-response | Description: Total number of identity response messages received with MS identity of type “IMSI” for 2G service. Triggers: When the SGSN receives an Identity response initiated to an identity request initiated of identity type IMSI. Availability: per GPRS service Type: Counter | Int32
> 3G-imei-identity-response | Description: Total number of identity response messages received with MS identity of type “IMEI” for 3G service. Triggers: When the SGSN receives an Identity response initiated to an identity request initiated of identity type IMEI. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-imei-identity-response | Description: Total number of identity response messages received with MS identity of type “IMEI” for 2G service. Triggers: When the SGSN receives an Identity response initiated to an identity request initiated of identity type IMEI. Availability: per GPRS service Type: Counter | Int32
> 3G-imeisv-identity-response | Description: Total number of identity response messages received with MS identity of type “IMEI-SV” for 3G service. Triggers: When the SGSN receives an Identity response initiated to an identity request initiated of identity type IMEI-SV. Availability: per SGSN service, per RA Type: Counter | Int32
> 2G-imeisv-identity-response | Description: Total number of identity response messages received with MS identity of type “IMEI-SV” for 2G service. Triggers: When the SGSN receives an Identity response initiated to an identity request initiated of identity type IMEI-SV. Availability: per GPRS service Type: Counter | Int32
> 3G-unknown-identity-response | Total number of unknown identity response sent for 3G service. | Int32
> 2G-unknown-identity-response | Total number of unknown identity response sent for 2G service. | Int32
> 3G-tmsi-identity-response | Total number of temporary IMSI identity response messages sent for 3G service. | Int32
> 2G-tmsi-identity-response | Total number of temporary IMSI identity response messages sent for 2G service. | Int32
> new-connection-rejected-overload | Description: This proprietary counter indicates the total number of new connection (Inter-SGSN RAU and/or Attach) requests that were rejected due to an overload situation. Triggers: 1. A congestion control mechanism is configured so that any new connection request received, that goes beyond the set threshold, will be rejected. 2. A network overload control feature is enabled and configured to accept new connections only at a defined rate. Incoming requests are buffered in a queue. When the queue is full additional requests can be rejected. Availability: per SGSN Service Type: Counter | Int32
> 3G-T3350-expiry | Total number of times the T3350 timer timed-out for 3G service. | Int32
> 2G-T3350-expiry | Total number of times the T3350 timer timed-out for 2G service. | Int32
> 3G-T3360-expiry | Total number of times the T3360 timer timed-out for 3G service. | Int32
> 2G-T3360-expiry | Total number of times the T3360 timer timed-out for 2G service. | Int32
> 3G-T3370-expiry | Total number of times the T3370 timer timed-out for 3G service. | Int32
> 2G-T3370-expiry | Total number of times the T3370 timer timed-out for 2G service. | Int32
> 3G-T3322-expiry | Total number of times the T3322 timer timed-out for 3G service. | Int32
> 2G-T3322-expiry | Total number of times the T3322 timer timed-out for 2G service. | Int32
> 3G-T3313-expiry | Total number of times the T3313 timer timed-out for 3G service. | Int32
> 2G-T3313-expiry | Total number of times the T3313 timer timed-out for 2G service. | Int32
> 2G-ready-timer-expiry | Total number of times the 2G service ready timer timed-out. | Int32
> Rnc-overload-attach-dropped | Total number of attach requests dropped due to overload at RNC. | Int32
> Rnc-overload-service-req-dropped | Total number of service requests dropped due to overload at RNC. | Int32
> Rnc-overload-skip-ptmsi-realloc | Total number of P-TMSI reallocation procedure skipped due to overload at RNC. | Int32
> Rnc-overload-skip-auth | Total number of authentication procedure skipped due to overload at RNC. | Int32
> Initial-UE-Rcvd | Total number of initial user equipment (UE) messages received. | Int32
> Direct-Trans-Rcvd | Total number of common identifier messages sent. | Int32
> Direct-Trans-Sent | Total number of direct transfer messages sent. | Int32
> common-id-sent | Total number of direct transfer messages received. | Int32
> sec-mode-command | Total number of security mode commands received. | Int32
> sec-mode-complete | Total number of security mode completed. | Int32
> sec-mode-reject | Total number of security mode commands rejected. | Int32
> Iu-release-request | Total number of Iu interface release request received. | Int32
> Iu-release-command | Total number of Iu interface release commands received. | Int32
> Iu-release-complete | Total number of Iu interface release completed. | Int32
> Reset-received | Total number of reset requests received. | Int32
> Retransmitted-reset-received | Total number of retransmitted reset requests received. | Int32
> Reset-Ack-sent | Total number of reset request acknowledgement sent. | Int32
> Reset-sent | Total number of reset requests sent. | Int32
> Retransmitted-reset-sent | Total number of reset requests retransmitted. | Int32
> Reset-Ack-received | Total number of reset request acknowledgement received. | Int32
> Resource-reset-received | Total number of resource reset requests received. | Int32
> Resource-reset-ack-sent | Total number of resource reset request acknowledgement sent. | Int32
> Resource-reset-sent | Total number of resource reset request sent. | Int32
> Resource-reset-ack-received | Total number of resource reset request acknowledgement received. | Int32
> Overload-control-rcvd | Total number of resource overload control message received. | Int32
> Pc-congested-rcvd | Total number of point code (PC) congested message received. | Int32
> Error-indication-rcvd | Total number of error indication message received. | Int32
> Error-indication-sent | Total number of error indication message sent. | Int32
> Relocation-required | Total number of message received for Serving Radio Network Subsystem (SRNS) relocation required. | Int32
> Relocation-command | Total number of message received with SRNS relocation command. | Int32
> Relocation-request | Total number of SRNS relocation requests received. | Int32
> Relocation-request-ack | Total number of SRNS relocation requests Ack sent. | Int32
> Relocation-failure | Total number of SRNS relocation failure messages received. | Int32
> Relocation-prep-failure | Total number of SRNS relocation preparation failure messages received. | Int32
> Relocation-cancel | Total number of SRNS relocation cancel messages received. | Int32
> Relocation-cancel-ack | Total number of SRNS relocation cancel acknowledge messages sent. | Int32
> Relocation-detect | Total number of SRNS relocation detected. | Int32
> Relocation-complete | Total number of SRNS relocation completed. | Int32
> Forward-srns-context | Total number of SRNS contexts forwarded. | Int32
> GMM-received-nas-pdu | Total protocol data units received by GPRS mobility management (GMM) service through NAS interface. | Int32
> GMM-sent-nas-pdu | Total protocol data units sent by GMM service through NAS interface. | Int32
> SM-received-nas-pdu | Total protocol data units received by Service Management (SM) service through NAS interface. | Int32
> SM-sent-nas-pdu | Total protocol data units sent by SM service through NAS interface. | Int32
> SMS-received-nas-pdu | Total protocol data units received by short message service (SMS) through NAS interface. | Int32
> SMS-sent-nas-pdu | Total protocol data units sent by short message service (SMS) through NAS interface. | Int32
> SMS-unexpected-nas-pdu | Total unexpected type of protocol data units received by short message service (SMS) through NAS interface. | Int32
> Unidentified-nas-pdu | Total number of unknown type PDUs received through NAS interface. | Int32
> exist-conn-proc-rej-overload | Total number of existing procedures rejected due to overload. |
> 3G-ptmsi-signature-mismatch-attach | Total number of NAS PDU dropped due to mismatch in P-TMSI signatures in attach procedures for 3G service. | Int32
> 2G-ptmsi-signature-mismatch-attach | Total number of NAS PDU dropped due to mismatch in P-TMSI signatures in attach procedures for 2G service. | Int32
> 3G-ptmsi-signature-mismatch-detach | Total number of NAS PDU dropped due to mismatch in P-TMSI signatures in detach procedures for 3G service. | Int32
> 2G-ptmsi-signature-mismatch-detach | Total number of NAS PDU dropped due to mismatch in P-TMSI signatures in detach procedures for 2G service. | Int32
> 3G-ptmsi-signature-mismatch-rau | Total number of NAS PDU dropped due to mismatch in P-TMSI signatures in routing area update procedures for 3G service. | Int32
> 2G-ptmsi-signature-mismatch-rau | Total number of NAS PDU dropped due to mismatch in P-TMSI signatures in routing area update procedures for 2G service. | Int32
> 3G-total-actv-req | Total number of request messages received for 3G context activation including primary and secondary type. | Int32
> 2G-total-actv-req | Total number of request messages received for 2G context activation including primary and secondary type. | Int32
> 3G-total-actv-accept | Description: Total number of request messages accepted for 3G context activation including primary and secondary type. Triggers: Increments when the SGSN sends Activate Accept or Activate Secondary Accept to the MS upon successful PDP Activation. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-total-actv-accept | Description: Total number of request messages accepted for 2G context activation including primary and/or secondary type. Triggers: Increments when the SGSN sends Activate Accept or Activate Secondary Accept to the MS upon successful PDP Activation. Availability: per GPRS service Type: Counter | Int32
> 3G-total-num-actv-pdp | Description: Total number of active PDP context (primary and secondary type) for 3G service in SGSN. Triggers: 1. Increments when the context is completely active in the SGSN. 2. Decrements when the context is deleted from the SGSN. Availability: per SGSN service, per RAI Type: Gauge | Int32
> 2G-total-num-actv-pdp | Description: Total number of active PDP context (primary and secondary type) for 2G service in SGSN. Triggers: 1. Increments when the context is completely active in the SGSN. 2. Decrements when the context is deleted from the SGSN. Availability: per GPRS service Type: Gauge | Int32
> 3G-total-actv-pdp-with-dir-tunnel | Total number of active PDP context (primary and secondary type) for 3G service with direct tunnel enabled. This statistic value is of Gauge. | Int32
> 3G-primary-actv-req | Total number of request messages received for 3G primary PDP context activation. | Int32
> 2G-primary-actv-req | Total number of request messages received for 2G primary PDP context activation. | Int32
> 3G-primary-actv-req-nrpca | Total number of request messages received for 3G primary PDP context activation from network side. | Int32
> 3G-primary-req-act-pdp | Total number of requests to activate primary PDP context for 3G service. | Int32
> 3G-primary-req-act-pdp-retrans | Total number of requests retransmitted to activate primary PDP context for 3G service. | Int32
> 3G-primary-actv-accept | Total number of requests accepted to activate primary PDP context for 3G service. | Int32
> 2G-primary-actv-accept | Total number of requests accepted to activate primary PDP context for 2G service. | Int32
> 3G-total-actv-reject | Description: Total number of requests rejected to activate PDP context (primary and secondary) for 3G service. Triggers: Increments when the SGSN sends Activate Reject or Activate Secondary Reject to the MS. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-total-actv-reject | Description: Total number of requests rejected to activate PDP context (primary and secondary) for 2G service. Triggers: Increments when the SGSN sends Activate Reject or Activate Secondary Reject to the MS. Availability: per GPRS service Type: Counter | Int32
> 3G-primary-actv-reject | Total number of requests rejected to activate primary PDP context for 3G service. | Int32
> 2G-primary-actv-reject | Total number of requests rejected to activate primary PDP context for 2G service. | Int32
> 3G-secondary-actv-req | Total number of requests to activate secondary PDP context for 3G service. | Int32
> 2G-secondary-actv-req | Total number of requests to activate secondary PDP context for 2G service. | Int32
> 3G-secondary-actv-acc | Total number of requests to activate secondary PDP context for 3G service accepted. | Int32
> 2G-secondary-actv-acc | Total number of requests to activate secondary PDP context for 2G service accepted. | Int32
> 3G-secondary-actv-rej | Total number of requests to activate secondary PDP context for 3G service rejected. | Int32
> 2G-secondary-actv-rej | Total number of requests to activate secondary PDP context for 2G service rejected. | Int32
> 3G-actv-rej-odb | Total number of requests to activate PDP context for 3G service rejected due to operator determined barring. | Int32
> 2G-actv-rej-odb | Total number of requests to activate PDP context for 2G service rejected due to operator determined barring. | Int32
> 3G-actv-rej-insufficient-resources | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to:
> • | Resource allocation failures (memory, GTP-C Teid, GTP-U Teid, etc.) in SGSN
> • | Incorrect information sent by GGSN in CPC response (PDP Type modified by GGSN, missing PDP IP address, etc.
> • | SNDCP activation failure
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-insufficient-resources | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to:
> • | Resource allocation failures (memory, GTP-C Teid, GTP-U Teid, etc.) in SGSN
> • | Incorrect information sent by GGSN in CPC response (PDP Type modified by GGSN, missing PDP IP address, etc.)
> • | SNDCP activation failure
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS Service, RAI Type: Counter | Int32
> 3G-actv-rej-network-failure | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to network failure. Triggers: Increments when the SGSN sends Activate Reject due to SGSN operator policy restrictions and the cause code was configured as Network failure. Activations can be rejected due to SGSN operator policy in which the reject cause is configurable. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-network-failure | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to network failure. Triggers: Increments when the SGSN sends Activate Reject due to SGSN operator policy restrictions and the cause code was configured as Network failure. Activations can be rejected due to SGSN operator policy in which the reject cause is configurable. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-missing-or-unknown-apn | Description: Total number of requests to activate PDP context for 3G service rejected due to APN related errors such as:
> • | APN not present in Activate Request but multiple subscription records exist
> • | DNS query fails for APN to GGSN resolution
> • | Missing/Unknown APN received from GGSN
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-missing-or-unknown-apn | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to APN related errors such as:
> • | APN not present in Activate Request but multiple subscription records exist
> • | DNS query fails for APN to GGSN resolution
> • | Missing/Unknown APN received from GGSN
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-unknown-pdp-addr-type | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to PDP Address related errors such as:
> • | PDP Address requested in Activate Request but PDP Address Type not requested
> • | APN requested in Activate Request without PDP Address Type
> • | Unknown PDP Address or Type error received in Create PDP Context Response from GGSN
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-unknown-pdp-addr-type | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to PDP Address related errors such as:
> • | PDP Address requested in Activate Request but PDP Address Type not requested
> • | APN requested in Activate Request without PDP Address Type
> • | Unknown PDP Address or Type error received in Create Pdp Context Response from GGSN
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-usr-auth-failed | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to user authentication failure on GGSN. Triggers: Increments when the SGSN receives Create PDP Context Response with authentication failure cause. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-usr-auth-failed | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to user authentication failure on GGSN. Triggers: Increments when the SGSN receives Create PDP Context Response with authentication failure cause. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-by-ggsn | Description: Total number of requests sent to MS to activate PDP context for 3G service due to receiving Create PDP Context Response from GGSN with a cause of:
> • | "Insufficient resources"
> • | "All Dynamic PDP address occupied"
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-by-ggsn | Description: Total number of requests sent to MS to activate PDP context for 2G service due to receiving Create PDP Context Response from GGSN with a cause of:
> • | "Insufficient resources"
> • | "All Dynamic PDP address occupied"
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 3G-actv-rej-unspecified-error | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to:
> • | Receiving Create PDP Context Response from GGSN with a cause of "system failure"
> • | GGSN fails to respond to CPC Request
> • | SGSN triggers PDP deletion before receiving CPC response from GGSN
> • | HLR triggers PDP deletion before receiving CPC response (DSD received from HLR for the PDP)
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-unspecified-error | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to:
> • | Receiving Create PDP Context Response from GGSN with a cause of "system failure"
> • | GGSN fails to respond to CPC Request
> • | SGSN triggers PDP deletion before receiving CPC response from GGSN
> • | HLR triggers PDP deletion before receiving CPC response (DSD received from HLR for the PDP)
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-service-not-supported | Description: Total number of requests to activate PDP context for 3G service rejected as requested service is not supported. Triggers: Increments when the SGSN sends Activate Reject due to SGSN operator policy restrictions and the cause code was configured as Service Not Supported. Activations can be rejected due to SGSN operator policy in which the reject cause is configurable. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-service-not-supported | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected as requested service is not supported. Triggers: Increments when the SGSN sends Activate Reject due to SGSN operator policy restrictions and the cause code was configured as Service Not Supported. Activations can be rejected due to SGSN operator policy in which the reject cause is configurable. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-service-not-subscribed | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected as subscriber is not subscribed to requested service due to:
> • | APN Selection failures such as:
> • | Requested APN/PDP-Type/PDP-Addr not matching the subscription.
> • | Wild card APN requested but multiple subscription records exist for the subscriber.
> • | APN Access denied, No subscription error was received in Create PDP Context Response from GGSN.
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-service-not-subscribed | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected as subscriber is not subscribed to requested service due to:
> • | APN selection failures such as:
> • | Requested APN/PDP-Type/PDP-Addr not matching the subscription.
> • | Wild card APN requested but multiple subscription records exist for the subscriber.
> • | APN Access denied and No subscription error was received in Create PDP Context Response from GGSN.
> Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service Type: Counter | Int32
> 3G-actv-rej-svc-opt-tmp-out-of-order | Total number of requests to activate PDP context for 3G service rejected as requested service option is temporarily out of order. | Int32
> 2G-actv-rej-svc-opt-tmp-out-of-order | Total number of requests to activate PDP context for 2G service rejected as requested service option is temporarily out of order. | Int32
> 3G-actv-rej-apn-restriction-incompatible | Total number of requests to activate PDP context for 3G service rejected due to restriction of APN or incompatibility of APN for service. | Int32
> 2G-actv-rej-apn-restriction-incompatible | Total number of requests to activate PDP context for 2G service rejected due to restriction of APN or incompatibility of APN for service. | Int32
> 3G-actv-rej-semantically-incorrect | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to semantically incorrect IE message in Activate PDP Request. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-semantically-incorrect | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to semantically incorrect IE message in Activate PDP Request. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 3G-actv-rej-invalid-mandatory-info | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to invalid mandatory IE in Activate PDP Request. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-invalid-mandatory-info | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to invalid mandatory IE in Activate PDP Request. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 3G-actv-rej-msg-type-non-existent | Total number of requests to activate PDP context for 3G service rejected due to non-existent type of message. | Int32
> 2G-actv-rej-msg-type-non-existent | Total number of requests to activate PDP context for 3G service rejected due to non-existent type of message. | Int32
> 3G-actv-rej-ie-non-existent | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected upon receiving Create PDP Context Response from GGSN with a cause of "Mandatory IE missing". Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-ie-non-existent | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected upon receiving Create PDP Context Response from GGSN with a cause of "Mandatory IE missing". Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 3G-actv-rej-conditional-ie-err | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected due to conditional IE (Information Element) error in Activate PDP Request. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-conditional-ie-err | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected due to conditional IE (Information Element) error in Activate PDP Request. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 3G-actv-rej-msg-not-compatible-with-prot-state | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected as message type is not compatible with protocol state. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-msg-not-compatible-with-prot-state | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected as message type is not compatible with protocol state. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 3G-actv-rej-recovery-on-timer-expiry | Total number of requests to activate PDP context for 3G service rejected as timer expired for recovery. | Int32
> 2G-actv-rej-recovery-on-timer-expiry | Total number of requests to activate PDP context for 2G service rejected as timer expired for recovery. | Int32
> 3G-actv-rej-prot-err-unspecified | Description: Total number of requests sent to MS to activate PDP context for 3G service rejected upon receiving Create PDP Context Response from GGSN with a cause of "unspecified protocol error”. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-actv-rej-prot-err-unspecified | Description: Total number of requests sent to MS to activate PDP context for 2G service rejected upon receiving Create PDP Context Response from GGSN with a cause of "unspecified protocol error”. Triggers: Increments when the SGSN sends Activate Reject for the above conditions. Availability: per GPRS service, per RAI Type: Counter | Int32
> 2G-actv-rej-llc-sndcp-fail | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-qos-not-acc | This bulkstat is not used and has been obsoleted. | Int32
> 3G-actv-rej-semantic-error-tft-operation | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-semantic-error-tft-operation | This bulkstat is not used and has been obsoleted. | Int32
> 3G-actv-rej-syntax-err-in-tft-operation | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-syntax-err-in-tft-operation | This bulkstat is not used and has been obsoleted. | Int32
> 3G-actv-rej-unknown-pdp-context | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-unknown-pdp-context | This bulkstat is not used and has been obsoleted. | Int32
> 3G-actv-rej-semantic-err-in-pkt-filter | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-semantic-err-in-pkt-filter | This bulkstat is not used and has been obsoleted. | Int32
> 3G-actv-rej-syntax-err-in-pkt-filter | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-syntax-err-in-pkt-filter | This bulkstat is not used and has been obsoleted. | Int32
> 3G-actv-rej-pdp-notft-actv | This bulkstat is not used and has been obsoleted. | Int32
> 2G-actv-rej-pdp-notft-actv | This bulkstat is not used and has been obsoleted. | Int32
> 3G-sec-actv-rej-odb | Total number of requests to activate secondary PDP context for 3G service rejected due to operator determined barring. | Int32
> 2G-sec-actv-rej-odb | Total number of requests to activate secondary PDP context for 2G service rejected due to operator determined barring. | Int32
> 3G-sec-actv-rej-insufficient-resources | Total number of requests to activate secondary PDP context for 3G service rejected due to insufficient resources. | Int32
> 2G-sec-actv-rej-insufficient-resources | Total number of requests to activate secondary PDP context for 2G service rejected due to insufficient resources. | Int32
> 3G-sec-actv-rej-by-ggsn | Total number of requests to activate secondary PDP context for 3G service rejected as request rejected by the GGSN. | Int32
> 2G-sec-actv-rej-by-ggsn | Total number of requests to activate secondary PDP context for 2G service rejected as request rejected by the GGSN. | Int32
> 3G-sec-actv-rej-unspecified-error | Total number of requests to activate secondary PDP context for 3G service rejected due to error which is not specified in this table or unknown. | Int32
> 2G-sec-actv-rej-unspecified-error | Total number of requests to activate secondary PDP context for 2G service rejected due to error which is not specified in this table or unknown. | Int32
> 3G-sec-actv-rej-service-not-supported | Description: Total number of requests sent to MS to activate secondary PDP context for 3G service rejected as requested service is not supported. Triggers: Increments when the SGSN sends Activate Secondary Reject due to SGSN operator policy restrictions and the cause code was configured as Service Not Supported. Activations can be rejected due to SGSN operator policy in which the reject cause is configurable. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-sec-actv-rej-service-not-supported | Description: Total number of requests sent to MS to activate secondary PDP context for 2G service rejected as requested service is not supported. Triggers: Increments when the SGSN sends Activate Secondary Reject due to SGSN operator policy restrictions and the cause code was configured as Service Not Supported. Activations can be rejected due to SGSN operator policy in which the reject cause is configurable. Availability: per GPRS service Type: Counter | Int32
> 3G-sec-actv-rej-service-not-subscribed | Description: Total number of requests sent to MS to activate secondary PDP context for 3G service rejected as subscriber is not subscribed to requested service due to:
> • | APN Selection related errors such as:
> • | Activate PDP Request without PDP Address/Type and APN, and multiple subscription records present.
> • | Activate PDP Request with PDP Type (and address) and no matching subscription records for the PDP Type.
> • | Activate PDP Request with dynamic addressing but matching subscription records have static address.
> • | Create PDP Context Response from GGSN is received with error code “Access denied, no subscription”.
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-sec-actv-rej-service-not-subscribed | Description: Total number of requests sent to MS to activate secondary PDP context for 2G service rejected as subscriber is not subscribed to requested service due to:
> • | APN Selection related errors such as:
> • | Activate PDP Request without PDP Address/Type and APN, and multiple subscription records present.
> • | Activate PDP Request with PDP Type (and address) and no matching subscription records for the PDP Type.
> • | Activate PDP Request with dynamic addressing but matching subscription records have static address.
> • | Create PDP Context Response from GGSN is received with error code “Access denied, no subscription”.
> Triggers: Increments when the SGSN sends Activate Reject for all the above conditions. Availability: per GPRS service Type: Counter | Int32
> 3G-sec-actv-rej-svc-opt-tmp-out-of-order | Total number of requests to activate secondary PDP context for 3G service rejected as requested service option is temporarily out of order. | Int32
> 2G-sec-actv-rej-svc-opt-tmp-out-of-order | Total number of requests to activate secondary PDP context for 3G service rejected as requested service option is temporarily out of order. | Int32
> 3G-sec-actv-rej-semantically-incorrect | Total number of requests to activate secondary PDP context for 2G service rejected due to semantically incorrect message. | Int32
> 2G-sec-actv-rej-semantically-incorrect | Total number of requests to activate secondary PDP context for 3G service rejected as mandatory information in message is invalid. | Int32
> 3G-sec-actv-rej-invalid-mandatory-info | Total number of requests to activate secondary PDP context for 3G service rejected as mandatory information in message is invalid. | Int32
> 2G-sec-actv-rej-invalid-mandatory-info | Total number of requests to activate secondary PDP context for 2G service rejected as mandatory information in message is invalid. | Int32
> 3G-sec-actv-rej-msg-type-non-existent | Total number of requests to activate secondary PDP context for 3G service rejected due to non-existent type of message. | Int32
> 2G-sec-actv-rej-msg-type-non-existent | Total number of requests to activate secondary PDP context for 3G service rejected due to non-existent type of message. | Int32
> 3G-sec-actv-rej-ie-non-existent | Total number of requests to activate secondary PDP context for 3G service rejected due to non-existence of information element. | Int32
> 2G-sec-actv-rej-ie-non-existent | Total number of requests to activate secondary PDP context for 2G service rejected due to non-existence of information element. | Int32
> 3G-sec-actv-rej-conditional-ie-err | Total number of requests to activate secondary PDP context for 3G service rejected due to error in conditional information element. | Int32
> 2G-sec-actv-rej-conditional-ie-err | Total number of requests to activate secondary PDP context for 2G service rejected due to error in conditional information element. | Int32
> 3G-sec-actv-rej-msg-not-compat-prot-state | Total number of requests to activate secondary PDP context for 3G service rejected as message type is not compatible with protocol state. | Int32
> 2G-sec-actv-rej-msg-not-compat-prot-state | Total number of requests to activate secondary PDP context for 2G service rejected as message type is not compatible with protocol state. | Int32
> 3G-sec-actv-rej-recovery-on-timer-expiry | Total number of requests to activate secondary PDP context for 3G service rejected as timer expired for recovery. | Int32
> 2G-sec-actv-rej-recovery-on-timer-expiry | Total number of requests to activate secondary PDP context for 2G service rejected as timer expired for recovery. | Int32
> 3G-sec-actv-rej-prot-err-unspecified | Total number of requests to activate secondary PDP context for 3G service rejected due to unspecified protocol error. | Int32
> 2G-sec-actv-rej-prot-err-unspecified | Total number of requests to activate secondary PDP context for 2G service rejected due to unspecified protocol error. | Int32
> 2G-sec-actv-rej-llc-sndcp-fail | This bulkstat is not used and has been obsoleted. | Int32
> 2G-sec-actv-rej-qos-not-acc | This bulkstat is not used and has been obsoleted. | Int32
> 3G-sec-actv-rej-semantic-error-tft-operation | Total number of requests to activate secondary PDP context for 3G service rejected due to semantic error in traffic flow template (TFT) operation. | Int32
> 2G-sec-actv-rej-semantic-error-tft-operation | Total number of requests to activate secondary PDP context for 3G service rejected due to semantic error in traffic flow template (TFT) operation. | Int32
> 3G-sec-actv-rej-syntax-err-in-tft-operation | Total number of requests to activate secondary PDP context for 3G service rejected due to syntax error in traffic flow template (TFT) operation. | Int32
> 2G-sec-actv-rej-syntax-err-in-tft-operation | Total number of requests to activate secondary PDP context for 2G service rejected due to syntax error in traffic flow template (TFT) operation. | Int32
> 3G-sec-actv-rej-unknown-pdp-context | Total number of requests to activate secondary PDP context for 3G service rejected due to unknown type of PDP context. | Int32
> 2G-sec-actv-rej-unknown-pdp-context | Total number of requests to activate secondary PDP context for 2G service rejected due to unknown type of PDP context. | Int32
> 3G-sec-actv-rej-semantic-err-in-pkt-filter | Total number of requests to activate secondary PDP context for 3G service rejected due to semantic error in packet filter. | Int32
> 2G-sec-actv-rej-semantic-err-in-pkt-filter | Total number of requests to activate secondary PDP context for 3G service rejected due to semantic error in packet filter. | Int32
> 3G-sec-actv-rej-syntax-err-in-pkt-filter | Total number of requests to activate secondary PDP context for 3G service rejected due to syntax error in packet filter. | Int32
> 2G-sec-actv-rej-syntax-err-in-pkt-filter | Total number of requests to activate secondary PDP context for 2G service rejected due to syntax error in packet filter. | Int32
> 3G-sec-actv-rej-pdp-notft-actv | Total number of requests to activate secondary PDP context for 3G service rejected due to TFT was not active. | Int32
> 2G-sec-actv-rej-pdp-notft-actv | Total number of requests to activate secondary PDP context for 3G service rejected due to TFT was not active. | Int32
> 3G-total-actv-fail | Description: Total number of PDP context activation (primary and secondary) failed for 3G service due to:
> • | GMM procedure collision
> • | Duplicate Activate Requests in non-active states (activation or deactivation in progress)
> • | Detach before activation is over
> • | Handoff to Peer before activation is over
> • | GTP Tunnel deletion in case of Second PDP Activations
> • | IU release before the completion of activation procedure
> Triggers: Increments when the SGSN drops PDP Activate Request for all the above conditions. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-total-actv-fail | Description: Total number of PDP context activation (primary and secondary) failed for 2G service due to:
> • | GMM procedure collision
> • | Duplicate Activate Requests in non-active states (activation or deactivation in progress)
> • | Detach before activation is over
> • | Handoff to Peer before activation is over
> • | GTP Tunnel deletion in case of Second PDP Activations
> Triggers: Increments when the SGSN drops PDP Activate Request for all the above conditions. Availability: per GPRS service Type: Counter | Int32
> 3G-primary-actv-fail | Total number of primary PDP context activations that failed in the 3G service. | Int32
> 2G-primary-actv-fail | Description: New counter in release 9.0: Total number of Primary PDP Activation Requests dropped due to:
> 1. | GMM procedure collision.
> 2. | Duplicate Activate Requests in non-active states (activation or deactivation in progress).
> 3. | Detach before activation completes.
> 4. | Handoff to peer before activation completes.
> Triggers: Increments when the SGSN drops the Primary PDP Activate Request for indicated condition. Availability: per GPRS service, per RA Type: Counter | Int32
> 3G-secondary-actv-fail | Total number of secondary PDP context activations that failed in the 3G service. | Int32
> 2G-secondary-actv-fail | Description: New counter in release 9.0: Total number of Secondary PDP Activation Requests dropped due to:
> 1. | GMM procedure collision.
> 2. | Duplicate Activate Requests in non-active states (activation or deactivation in progress).
> 3. | Detach before activation completes.
> 4. | Handoff to peer before activation completes.
> 5. | GTP tunnel deletion.
> Triggers: Increments when the SGSN drops the Secondary PDP Activate Request for indicated condition. Availability: per GPRS service, per RA Type: Counter | Int32
> 3G-actv-fail-iu-release-before-activate | Description: Total number of PDP Activation Requests dropped due to IU release before the completion of activation procedure. Triggers: Increments when the SGSN drops PDP Activate Request due to IU release before the completion of activation procedure. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-actv-fail-gaurd-timer-expiry | Description: Total number of PDP Activation Requests dropped due to SM Guard Timer Expiry. Triggers: Increments when the SGSN drops PDP Activate Request due to SM Guard Timer Expiry. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-actv-fail-duplicate-activation | Description: Total number of PDP Activation Requests dropped due to an ongoing PDP Activation. Triggers: Increments when the SGSN drops PDP Activate Request due to PDP Activation in progress. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-actv-fail-other-ongoing-procedure | Description: Total number of PDP Activation Requests dropped due to other ongoing procedures such as:
> • | Activate Request during network initiated detach
> • | Page timer expiry while trying to send Activate Accept/Reject
> Triggers: Increments when the SGSN drops PDP Activate Request due to other ongoing procedures. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-actv-fail-tunnel-deactivation | Description: Total number of PDP Activation Requests that fail due to tunnel deactivation. Availability: per SGSN service, per RA Type: Counter | Int32
> 3G-actv-fail-handoff-before-activate-over | Description: Total number of PDP Activation Request dropped due to Handoff request from Peer SGSN for the subscriber. Triggers: Increments when the SGSN drops PDP Activate Request due to Handoff request from Peer SGSN for the subscriber. Availability: per SGSN Service and per RA Type: Counter | Int32
> 3G-actv-fail-detach-before-activate-over | Description: Total number of PDP Activation Requests dropped due to detach request while activation was in progress. Triggers: Increments when the SGSN drops PDP Activate Request due to detach request while activation was in progress. SGSN for the subscriber. Availability: per SGSN Service and per RA Type: Counter | Int32
> 3G-actv-fail-phase-2-offload | Description: This proprietary counter indicates the total number of PDP Activation failures due to Phase 2 offloading in 3G service. This statistics is specific to releases 8.1 and higher. Triggers: Increments when PDP Activation fails due to Phase 2 offloading. Availability: per SGSN service, per RA, per RNC Type: Counter | Int32
> 3G-actv-fail-invalid-message-content | Description: Total number of PDP Activation Requests dropped due to invalid information in activate request such as invalid Ti flag value. Triggers: Increments when the SGSN drops PDP Activate Request due to above condition. Availability: per SGSN Service and per RA Type: Counter | Int32
> 2G-actv-fail-gaurd-timer-expiry | Description: Total number of PDP Activation Requests dropped due to SM Guard Timer Expiry. Triggers: Increments when the SGSN drops PDP Activate Request due to SM Guard Timer Expiry. Availability: per GPRS service Type: Counter | Int32
> 2G-actv-fail-duplicate-activation | Description: Total number of PDP Activation Requests dropped due to an ongoing PDP Activation. Triggers: Increments when the SGSN drops PDP Activate Request due to PDP Activation in progress. Availability: per GPRS service Type: Counter | Int32
> 2G-actv-fail-other-ongoing-procedure | Description: Total number of PDP Activation Requests dropped due to other ongoing procedures such as: (1) Activate Request during network initiated detach. (2) Page timer expiry while trying to send Activate Accept/Reject. Triggers: Increments when the SGSN drops PDP Activate Request due to other ongoing procedures Availability: per GPRS service Type: Counter | Int32
> 2G-actv-fail-tunnel-deactivation | Description: Total number of PDP Activation Requests that fail due to tunnel deactivation. Availability: per GPRS Service and per NSEI Type: Counter | Int32
> 2G-actv-fail-handoff-before-activate-over | Description: Total number of PDP Activation Requests dropped due to Handoff request from Peer SGSN for the subscriber. Triggers: Increments when the SGSN drops PDP Activate Request due to Handoff request from Peer SGSN for the subscriber. Availability: per GPRS service Type: Counter | Int32
> 2G-actv-fail-detach-before-activate-over | Description: Total number of PDP Activation Requests dropped due to detach request while activation was in progress. Triggers: Increments when the SGSN drops PDP Activate Request due to detach request while activation was in progress. SGSN for the subscriber. Availability: per GPRS service Type: Counter | Int32
> 2G-actv-fail-phase-2-offload | Description: This proprietary counter indicates the total number of PDP Activation failures due to Phase 2 offloading in 2G service. This statistics is specific to releases 8.1 and higher. Triggers: Increments when PDP Activation fails due to Phase 2 offloading. Availability: per GPRS service, per RA Type: Counter | Int32
> 2G-actv-fail-invalid-msg-content | Description: Total number of PDP Activation Requests dropped due to invalid information in activate request such as invalid Ti flag value Triggers: Increments when the SGSN drops PDP Activate Request due to above condition Availability: per GPRS service Type: Counter | Int32
> 3G-dupl-ti-pdpactive | Total number of duplicate context activation requests for 3G service with duplicate transaction identifiers (TIs). | Int32
> 2G-dupl-ti-pdpactive | Total number of duplicate context activation requests for 2G service with duplicate transaction identifiers (TIs). | Int32
> 3G-dupl-nsapi-pdpactv | Total number of duplicate context activation requests for 3G service with duplicate Network Service Access Point Identifier (NSAPI). | Int32
> 2G-dupl-nsapi-pdpactv | Total number of duplicate context activation requests for 2G service with duplicate Network Service Access Point Identifier (NSAPI). | Int32
> 3G-dupl-pdpaddr-apn-pdpactv | Total number of duplicate context activation requests for 3G service with duplicate PDP address or APN name. | Int32
> 2G-dupl-pdpaddr-apn-pdpactv | Total number of duplicate context activation requests for 2G service with duplicate PDP address or APN name. | Int32
> 3G-dupl-ti-n-pdpactive | Total number of duplicate context activation requests for 3G service which are not in PDP active state with duplicate transaction identifiers (TIs). | Int32
> 2G-dupl-ti-n-pdpactive | Total number of duplicate context activation requests for 2G service which are not in PDP active state with duplicate transaction identifiers (TIs). | Int32
> 3G-dupl-nsapi-n-pdpactv | Total number of duplicate context activation requests for 3G service which are not in PDP active state with duplicate Network Service Access Point Identifier (NSAPI). | Int32
> 2G-dupl-nsapi-n-pdpactv | Total number of duplicate context activation requests for 2G service which are not in PDP active state with duplicate Network Service Access Point Identifier (NSAPI). | Int32
> 3G-dupl-pdpaddr-apn-n-pdpactv | Total number of duplicate context activation requests for 3G service which are not in PDP active state with duplicate PDP address and access point name. | Int32
> 2G-dupl-pdpaddr-apn-n-pdpactv | Total number of duplicate context activation requests for 2G service which are not in PDP active state with duplicate PDP address and access point name. | Int32
> 3G-ms-modify-req | Total number of MS initiated PDP context modification requests received for 3G service. | Int32
> 2G-ms-modify-req | Total number of MS initiated PDP context modification requests received for 2G service. | Int32
> 3G-ms-modify-accept | Total number of MS initiated PDP context modification requests accepted for 3G service. | Int32
> 2G-ms-modify-accept | Total number of MS initiated PDP context modification requests accepted for 2G service. | Int32
> 3G-ms-modify-rej | Total number of MS initiated PDP context modification requests rejected for 3G service. | Int32
> 2G-ms-modify-rej | Total number of MS initiated PDP context modification requests rejected for 2G service. | Int32
> 3G-nw-modify-req | Total number of network initiated PDP context modification requests received for 3G service. | Int32
> 2G-nw-modify-req | Total number of network initiated PDP context modification requests received for 2G service. | Int32
> 3G-nw-ret-modify-req | Total number of retransmitted network initiated PDP context modification requests received for 3G service. | Int32
> 2G-nw-ret-modify-req | Total number of retransmitted network initiated PDP context modification requests received for 2G service. | Int32
> 3G-nw-modify-accept | Total number of network initiated PDP context modification requests accepted for 3G service. | Int32
> 2G-nw-modify-accept | Total number of network initiated PDP context modification requests accepted for 2G service. | Int32
> 3G-nw-modify-rej | Total number of network initiated PDP context modification requests rejected for 3G service. | Int32
> 2G-nw-modify-rej | Total number of network initiated PDP context modification requests rejected for 2G service. | Int32
> 3G-ms-modify-rej-insufficient-resources | Total number of MS initiated modify PDP context requests for 3G service rejected due to insufficient resources. | Int32
> 2G-ms-modify-rej-insufficient-resources | Total number of MS initiated modify PDP context requests for 2G service rejected due to insufficient resources. | Int32
> 3G-ms-modify-rej-service-opt-not-supported | Total number of MS initiated modify PDP context requests for 3G service rejected as requested service option is not supported. | Int32
> 2G-ms-modify-rej-service-opt-not-supported | Total number of MS initiated modify PDP context requests for 2G service rejected as requested service option is not supported. | Int32
> 3G-ms-modify-rej-semantic-err-tft-operation | Total number of MS initiated modify PDP context requests for 3G service rejected due to semantic error in subscriber traffic flow template processing. | Int32
> 2G-ms-modify-rej-semantic-err-tft-operation | Total number of MS initiated modify PDP context requests for 2G service rejected due to semantic error in subscriber traffic flow template processing. | Int32
> 3G-ms-modify-rej-syntax-err-tft-operation | Total number of MS initiated modify PDP context requests for 3G service rejected due to syntax error in subscriber traffic flow template operation. | Int32
> 2G-ms-modify-rej-syntax-err-tft-operation | Total number of MS initiated modify PDP context requests for 2G service rejected due to syntax error in subscriber traffic flow template operation. | Int32
> 3G-ms-modify-rej-semnatic-err-pkt-filter | Total number of MS initiated modify PDP context requests for 3G service rejected due to semantic error in packet filter. | Int32
> 2G-ms-modify-rej-semnatic-err-pkt-filter | Total number of MS initiated modify PDP context requests for 2G service rejected due to semantic error in packet filter. | Int32
> 3G-ms-modify-rej-syntax-err-pkt-filter | Total number of MS initiated modify PDP context requests for 3G service rejected due to syntax error in packet filter. | Int32
> 2G-ms-modify-rej-syntax-err-pkt-filter | Total number of MS initiated modify PDP context requests for 2G service rejected due to syntax error in packet filter. | Int32
> 3G-ms-modify-rej-semnatic-incorrect-message | Total number of MS initiated modify PDP context requests for 3G service rejected due to semantically incorrect message. | Int32
> 2G-ms-modify-rej-semnatic-incorrect-message | Total number of MS initiated modify PDP context requests for 2G service rejected due to semantically incorrect message. | Int32
> 3G-ms-modify-rej-invalid-mand-info | Total number of MS initiated modify PDP context requests for 3G service rejected as mandatory information in message is invalid. | Int32
> 2G-ms-modify-rej-invalid-mand-info | Total number of MS initiated modify PDP context requests for 2G service rejected as mandatory information in message is invalid. | Int32
> 3G-ms-modify-rej-msg-non-existent | Total number of MS initiated requests to modify PDP context for 3G service rejected due to non-existent type of message. | Int32
> 2G-ms-modify-rej-msg-non-existent | Total number of MS initiated requests to modify PDP context for 2G service rejected due to non-existent type of message. | Int32
> 3G-ms-modify-rej-ie-non-existent | Total number of MS initiated modify PDP context requests for 3G service rejected due to non-existence of information element. | Int32
> 2G-ms-modify-rej-ie-non-existent | Total number of MS initiated modify PDP context requests for 2G service rejected due to non-existence of information element. | Int32
> 3G-ms-modify-rej-conditional-ie-err | Total number of MS initiated modify PDP context requests for 3G service rejected due to error in conditional information element. | Int32
> 2G-ms-modify-rej-conditional-ie-err | Total number of MS initiated modify PDP context requests for 2G service rejected due to error in conditional information element. | Int32
> 3G-ms-modify-rej-msg-not-compatible-prot-state | Total number of MS initiated modify PDP context requests for 3G service rejected as message is not compatible with protocol state. | Int32
> 2G-ms-modify-rej-msg-not-compatible-prot-state | Total number of MS initiated modify PDP context requests for 2G service rejected as message is not compatible with protocol state. | Int32
> 3G-ms-modify-rej-rcvry-on-tmr-expiry | Total number of MS initiated modify PDP context requests for 3G service rejected as timer expired for recovery. | Int32
> 2G-ms-modify-rej-rcvry-on-tmr-expiry | Total number of MS initiated modify PDP context requests for 2G service rejected as timer expired for recovery. | Int32
> 3G-ms-modify-rej-prot-err-unspec | Total number of MS initiated modify PDP context requests for 3G service rejected due to unspecified protocol error. | Int32
> 2G-ms-modify-rej-prot-err-unspec | Total number of MS initiated modify PDP context requests for 2G service rejected due to unspecified protocol error. | Int32
> 3G-modify-rej-insufficient-resources | Total number of requests to modify PDP context for 3G service rejected due to insufficient resources. | Int32
> 2G-modify-rej-insufficient-resources | Total number of requests to modify PDP context for 2G service rejected due to insufficient resources. | Int32
> 3G-modify-rej-service-opt-not-supported | Total number of requests to modify PDP context for 3G service rejected as requested service option is not supported. | Int32
> 2G-modify-rej-service-opt-not-supported | Total number of requests to modify PDP context for 2G service rejected as requested service option is not supported. | Int32
> 3G-modify-rej-semantic-err-tft-operation | Total number of requests to modify PDP context for 3G service rejected due to semantic error in subscriber traffic flow template processing. | Int32
> 2G-modify-rej-semantic-err-tft-operation | Total number of requests to modify PDP context for 2G service rejected due to semantic error in subscriber traffic flow template processing. | Int32
> 3G-modify-rej-syntax-err-tft-operation | Total number of requests to modify PDP context for 3G service rejected due to syntax error in subscriber traffic flow template operation. | Int32
> 2G-modify-rej-syntax-err-tft-operation | Total number of requests to modify PDP context for 2G service rejected due to syntax error in subscriber traffic flow template operation. | Int32
> 3G-modify-rej-semnatic-err-pkt-filter | Total number of requests to modify PDP context for 3G service rejected due to semantic error in packet filter. | Int32
> 2G-modify-rej-semnatic-err-pkt-filter | Total number of requests to modify PDP context for 2G service rejected due to semantic error in packet filter. | Int32
> 3G-modify-rej-syntax-err-pkt-filter | Total number of requests to modify PDP context for 3G service rejected due to syntax error in packet filter. | Int32
> 2G-modify-rej-syntax-err-pkt-filter | Total number of requests to modify PDP context for 2G service rejected due to syntax error in packet filter. | Int32
> 3G-modify-rej-semnatic-incorrect-message | Total number of requests to modify PDP context for 3G service rejected due to semantically incorrect message. | Int32
> 2G-modify-rej-semnatic-incorrect-message | Total number of requests to modify PDP context for 2G service rejected due to semantically incorrect message. | Int32
> 3G-modify-rej-invalid-mand-info | Total number of requests to modify PDP context for 3G service rejected as mandatory information in message is invalid. | Int32
> 2G-modify-rej-invalid-mand-info | Total number of requests to modify PDP context for 2G service rejected as mandatory information in message is invalid. | Int32
> 3G-modify-rej-msg-non-existent | Total number of MS initiated requests to modify PDP context for 3G service rejected due to non-existent type of message. | Int32
> 2G-modify-rej-msg-non-existent | Total number of MS initiated requests to modify PDP context for 2G service rejected due to non-existent type of message. | Int32
> 3G-modify-rej-ie-non-existent | Total number of requests to modify PDP context for 3G service rejected due to non-existence of information element. | Int32
> 2G-modify-rej-ie-non-existent | Total number of requests to modify PDP context for 2G service rejected due to non-existence of information element. | Int32
> 3G-modify-rej-conditional-ie-err | Total number of requests to modify PDP context for 3G service rejected due to error in conditional information element. | Int32
> 2G-modify-rej-conditional-ie-err | Total number of requests to modify PDP context for 2G service rejected due to error in conditional information element. | Int32
> 3G-modify-rej-msg-not-compatible-prot-state | Total number of requests to modify PDP context for 3G service rejected as message is not compatible with protocol state. | Int32
> 2G-modify-rej-msg-not-compatible-prot-state | Total number of requests to modify PDP context for 2G service rejected as message is not compatible with protocol state. | Int32
> 3G-modify-rej-rcvry-on-tmr-expiry | Total number of requests to modify PDP context for 3G service rejected as timer expired for recovery. | Int32
> 2G-modify-rej-rcvry-on-tmr-expiry | Total number of requests to modify PDP context for 2G service rejected as timer expired for recovery. | Int32
> 3G-modify-rej-prot-err-unspec | Total number of requests to modify PDP context for 3G service rejected due to unspecified protocol error. | Int32
> 2G-modify-rej-prot-err-unspec | Total number of requests to modify PDP context for 2G service rejected due to unspecified protocol error. | Int32
> 3G-ms-deactv-req | Total number of MS initiated PDP context deactivation requests received for 3G service. | Int32
> 2G-ms-deactv-req | Total number of MS initiated PDP context deactivation requests received for 2G service. | Int32
> 3G-ms-deactv-accept | Description: Total number of MS initiated PDP context deactivation requests sent to MS accepted for 3G service. Triggers: Increments when the SGSN sends Deactivate Accept in response to MS initiated PDP deactivation. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-ms-deactv-accept | Description: Total number of MS initiated PDP context deactivation requests sent to MS accepted for 2G service. Triggers: Increments when the SGSN sends Deactivate Accept in response to MS initiated PDP deactivation. Availability: per GPRS service Type: Counter | Int32
> 3G-ms-deactv-reject | Total number of MS initiated PDP context deactivation requests rejected for 3G service. | Int32
> 2G-ms-deactv-reject | Total number of MS initiated PDP context deactivation requests rejected for 2G service. | Int32
> 3G-ms-deactv-rej-rx-odb | Total number of MS initiated PDP context deactivation requests rejected for 3G service due to operator determined barring. | Int32
> 2G-ms-deactv-rej-rx-odb | Total number of MS initiated PDP context deactivation requests rejected for 2G service due to operator determined barring. | Int32
> 3G-ms-deactv-rej-rx-mbms-cap-insuff-res | Total number of MS initiated PDP context deactivation requests rejected for 3G service due to insufficient resources for Multimedia Broadcast/Multicast Service (MBMS) capability. | Int32
> 2G-ms-deactv-rej-rx-mbms-cap-insuff-res | Total number of MS initiated PDP context deactivation requests rejected for 2G service due to insufficient resources for Multimedia Broadcast/Multicast Service (MBMS) capability. | Int32
> 3G-ms-deactv-rej-rx-llc-sndcp-fail-gb | Total number of MS initiated PDP context deactivation requests rejected for 3G service due to failure at the logical link control with sub network dependent convergence protocol at Gb interface. | Int32
> 2G-ms-deactv-rej-rx-llc-sndcp-fail-gb | Total number of MS initiated PDP context deactivation requests rejected for 2G service due to failure at the logical link control with sub network dependent convergence protocol at Gb interface. | Int32
> 3G-ms-deactv-rej-rx-insuff-res | Total number of MS initiated PDP context deactivation requests rejected due to insufficient resources in download direction for 3G service. | Int32
> 2G-ms-deactv-rej-rx-insuff-res | Total number of MS initiated PDP context deactivation requests rejected due to insufficient resources in download direction for 2G service. | Int32
> 3G-ms-deactv-rej-rx-miss-unkwn-apn | Total number of MS initiated PDP context deactivation requests rejected due to missing or unknown APN for 3G service. | Int32
> 2G-ms-deactv-rej-rx-miss-unkwn-apn | Total number of MS initiated PDP context deactivation requests rejected due to missing or unknown APN for 2G service. | Int32
> 3G-ms-deactv-rej-rx-unkwn-pdp-addr | Total number of MS initiated PDP context deactivation requests rejected due to unknown PDP context name or address for 3G service. | Int32
> 2G-ms-deactv-rej-rx-unkwn-pdp-addr | Total number of MS initiated PDP context deactivation requests rejected due to unknown PDP context name or address for 2G service. | Int32
> 3G-ms-deactv-rej-rx-usr-auth-fail | Total number of MS initiated PDP context deactivation requests rejected as user authentication failed for 3G service. | Int32
> 2G-ms-deactv-rej-rx-usr-auth-fail | Total number of MS initiated PDP context deactivation requests rejected as user authentication failed for 2G service. | Int32
> 3G-ms-deactv-rej-rx-actv-rej-ggsn | Total number of MS initiated PDP context deactivation requests rejected as request rejected by corresponding GGSN for 3G service. | Int32
> 2G-ms-deactv-rej-rx-actv-rej-ggsn | Total number of MS initiated PDP context deactivation requests rejected as request rejected by corresponding GGSN for 2G service. | Int32
> 3G-ms-deactv-rej-rx-actv-rej-unspec | Total number of MS initiated PDP context deactivation requests rejected due to unknown or unspecified reasons for 3G service. | Int32
> 2G-ms-deactv-rej-rx-actv-rej-unspec | Total number of MS initiated PDP context deactivation requests rejected due to unknown or unspecified reasons for 2G service. | Int32
> 3G-ms-deactv-rej-rx-service-opt-no-support | Total number of MS initiated PDP context deactivation requests rejected as requested service option is not supported for 3G service. | Int32
> 2G-ms-deactv-rej-rx-service-opt-no-support | Total number of MS initiated PDP context deactivation requests rejected as requested service option is not supported for 2G service. | Int32
> 3G-ms-deactv-rej-rx-service-opt-no-subs | Total number of MS initiated PDP context deactivation requests rejected as subscriber is not subscribed requested service option for 3G service. | Int32
> 2G-ms-deactv-rej-rx-service-opt-no-subs | Total number of MS initiated PDP context deactivation requests rejected as subscriber is not subscribed requested service option for 2G service. | Int32
> 3G-ms-deactv-rej-rx-svc-opt-temp-out-order | Total number of MS initiated PDP context deactivation requests rejected as requested service option is temporarily out of order for 3G service. | Int32
> 2G-ms-deactv-rej-rx-svc-opt-temp-out-order | Total number of MS initiated PDP context deactivation requests rejected as requested service option is temporarily out of order for 2G service. | Int32
> 3G-ms-deactv-rej-rx-nsapi-already-used | Total number of MS initiated PDP context deactivation requests rejected as requested NSAPI is already in use for 3G service. | Int32
> 2G-ms-deactv-rej-rx-nsapi-already-used | Total number of MS initiated PDP context deactivation requests rejected as requested NSAPI is already in use for 2G service. | Int32
> 3G-ms-deactv-rej-rx-reg-deactv | Total number of MS initiated PDP context deactivation requests rejected due to registration of deactivate message for 3G service. | Int32
> 2G-ms-deactv-rej-rx-reg-deactv | Total number of MS initiated PDP context deactivation requests rejected due to registration of deactivate message for 2G service. | Int32
> 3G-ms-deactv-rej-rx-qos-not-acc | Total number of MS initiated PDP context deactivation requests rejected as requested QoS is not accepted for 3G service. | Int32
> 2G-ms-deactv-rej-rx-qos-not-acc | Total number of MS initiated PDP context deactivation requests rejected as requested QoS is not accepted for 2G service. | Int32
> 3G-ms-deactv-rej-rx-nwt-fail | Total number of MS initiated PDP context deactivation requests rejected due to network failure for 3G service. | Int32
> 2G-ms-deactv-rej-rx-nwt-fail | Total number of MS initiated PDP context deactivation requests rejected due to network failure for 2G service. | Int32
> 3G-ms-deactv-rej-rx-reactivation-req | Total number of MS initiated PDP context deactivation requests rejected due re-activation request arrived before completion of deactivation procedure for 3G service. | Int32
> 2G-ms-deactv-rej-rx-reactivation-req | Total number of MS initiated PDP context deactivation requests rejected due re-activation request arrived before completion of deactivation procedure for 2G service. | Int32
> 3G-ms-deactv-rej-rx-no-feature-support | Total number of MS initiated PDP context deactivation requests for 3G service rejected as requested feature is not supported. | Int32
> 2G-ms-deactv-rej-rx-no-feature-support | Total number of MS initiated PDP context deactivation requests for 2G service rejected as requested feature is not supported. | Int32
> 3G-ms-deactv-rej-rx-sem-err-tft-op | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to semantic error in subscriber TFT option. | Int32
> 2G-ms-deactv-rej-rx-sem-err-tft-op | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to semantic error in subscriber TFT option. | Int32
> 3G-ms-deactv-rej-rx-syn-err-tft-op | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to syntax error in subscriber TFT option. | Int32
> 2G-ms-deactv-rej-rx-syn-err-tft-op | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to syntax error in subscriber TFT option. | Int32
> 3G-ms-deactv-rej-rx-unknown-ctx | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to unknown context in request. | Int32
> 2G-ms-deactv-rej-rx-unknown-ctx | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to unknown context in request. | Int32
> 3G-ms-deactv-rej-rx-ctx-no-tft-already-actv | Total number of MS initiated PDP context deactivation requests for 3G service rejected as no TFT is active in this context. | Int32
> 2G-ms-deactv-rej-rx-ctx-no-tft-already-actv | Total number of MS initiated PDP context deactivation requests for 2G service rejected as no TFT is active in this context. | Int32
> 3G-ms-deactv-rej-rx-mcast-grp-mem-tout | Total number of MS initiated PDP context deactivation requests for 3G service rejected as multicast group memory is timed-out. | Int32
> 2G-ms-deactv-rej-rx-mcast-grp-mem-tout | Total number of MS initiated PDP context deactivation requests for 2G service rejected as multicast group memory is timed-out. | Int32
> 3G-ms-deactv-rej-rx-sem-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to semantic error in packet filter. | Int32
> 2G-ms-deactv-rej-rx-sem-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to semantic error in packet filter. | Int32
> 3G-ms-deactv-rej-rx-syn-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to syntax error in packet filter. | Int32
> 2G-ms-deactv-rej-rx-syn-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to syntax error in packet filter. | Int32
> 3G-ms-deactv-rej-rx-invalid-trans-id | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to invalid transaction id. | Int32
> 2G-ms-deactv-rej-rx-invalid-trans-id | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to invalid transaction id. | Int32
> 3G-ms-deactv-rej-rx-sem-incorrect-msg | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to semantically incorrect message. | Int32
> 2G-ms-deactv-rej-rx-sem-incorrect-msg | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to semantically incorrect message. | Int32
> 3G-ms-deactv-rej-rx-inval-mand-info | Total number of MS initiated PDP context deactivation requests for 3G service rejected as mandatory information in message is invalid. | Int32
> 2G-ms-deactv-rej-rx-inval-mand-info | Total number of MS initiated PDP context deactivation requests for 2G service rejected as mandatory information in message is invalid. | Int32
> 3G-ms-deactv-rej-rx-msg-non-existent | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to non-existent type of message. | Int32
> 2G-ms-deactv-rej-rx-msg-non-existent | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to non-existent type of message. | Int32
> 3G-ms-deactv-rej-rx-ie-non-existent | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to non-existence of information element. | Int32
> 2G-ms-deactv-rej-rx-ie-non-existent | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to non-existence of information element. | Int32
> 3G-ms-deactv-rej-rx-cond-ie-err | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to error in conditional information element. | Int32
> 2G-ms-deactv-rej-rx-cond-ie-err | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to error in conditional information element. | Int32
> 3G-ms-deactv-rej-rx-prot-err-unspec | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to unspecified protocol error. | Int32
> 2G-ms-deactv-rej-rx-prot-err-unspec | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to unspecified protocol error. | Int32
> 3G-ms-deactv-rej-rx-apn-rest-incomap-actv-pdp | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to incompatible APN for PDP context activation. | Int32
> 2G-ms-deactv-rej-rx-apn-rest-incomap-actv-pdp | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to incompatible APN for PDP context activation. | Int32
> 3G-ms-deactv-rej-rx-msg-not-compat-prot-state | Total number of MS initiated PDP context deactivation requests for 3G service rejected as message is not compatible with protocol state. | Int32
> 2G-ms-deactv-rej-rx-msg-not-compat-prot-state | Total number of MS initiated PDP context deactivation requests for 2G service rejected as message is not compatible with protocol state. | Int32
> 3G-ms-deactv-rej-rx-rcvry-on-tmr-expiry | Total number of MS initiated PDP context deactivation requests for 3G service rejected as timer expired for recovery. | Int32
> 2G-ms-deactv-rej-rx-rcvry-on-tmr-expiry | Total number of MS initiated PDP context deactivation requests for 2G service rejected as timer expired for recovery. | Int32
> 3G-sgsn-init-deact-req | Total number of SGSN initiated PDP context deactivation requests received for 3G service. | Int32
> 2G-sgsn-init-deact-req | Total number of SGSN initiated PDP context deactivation requests received for 2G service. | Int32
> 3G-sgsn-init-deact-acc | Description: Total number of SGSN initiated PDP context deactivation requests received from MS accepted for 3G service. Triggers: Increments when the SGSN receives Deactivate Accept corresponding to SGSN initiated Deactivation Request sent to MS. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-sgsn-init-deact-acc | Description: Total number of SGSN initiated PDP context deactivation requests received from MS accepted for 2G service. Triggers: Increments when the SGSN receives Deactivate Accept corresponding to SGSN initiated Deactivation Request sent to MS. Availability: per GPRS service Type: Counter | Int32
> 3G-sgsn-init-deact-rej | Total number of SGSN initiated PDP context deactivation requests rejected for 3G service. | Int32
> 2G-sgsn-init-deact-rej | Total number of SGSN initiated PDP context deactivation requests rejected for 2G service. | Int32
> 3G-ggsn-init-deact-req | Total number of GGSN initiated PDP context deactivation requests received for 3G service. | Int32
> 2G-ggsn-init-deact-req | Total number of GGSN initiated PDP context deactivation requests received for 2G service. | Int32
> 3G-ggsn-init-deact-acc | Description: Total number of GGSN initiated PDP context deactivation requests received from MS accepted for 3G service. Triggers: Increments when the SGSN receives Deactivate Accept corresponding to GGSN initiated Deactivation Request sent to MS. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-ggsn-init-deact-acc | Description: Total number of GGSN initiated PDP context deactivation requests received from MS accepted for 2G service. Triggers: Increments when the SGSN receives Deactivate Accept corresponding to GGSN initiated Deactivation Request sent to MS. Availability: per GPRS service Type: Counter | Int32
> 3G-ggsn-init-deact-rej | Total number of GGSN initiated PDP context deactivation requests rejected for 3G service. | Int32
> 2G-ggsn-init-deact-rej | Total number of GGSN initiated PDP context deactivation requests rejected for 2G service. | Int32
> 3G-hlr-init-deact-req | Total number of HLR initiated PDP context deactivation requests received for 3G service. | Int32
> 2G-hlr-init-deact-req | Total number of HLR initiated PDP context deactivation requests received for 2G service. | Int32
> 3G-hlr-init-deact-acc | Description: Total number of HLR initiated PDP context deactivation requests received from MS accepted for 3G service. Triggers: Increments when the SGSN receives Deactivate Accept corresponding to HLR initiated Deactivation Request sent to MS. Availability: per SGSN service, per RAI Type: Counter | Int32
> 2G-hlr-init-deact-acc | Description: Total number of HLR initiated PDP context deactivation requests received from MS accepted for 2G service. Triggers: Increments when the SGSN receives Deactivate Accept corresponding to HLR initiated Deactivation Request sent to MS. Availability: per GPRS service Type: Counter | Int32
> 3G-hlr-init-deact-rej | Total number of HLR initiated PDP context deactivation requests rejected for 3G service. | Int32
> 2G-hlr-init-deact-rej | Total number of HLR initiated PDP context deactivation requests rejected for 2G service. | Int32
> 3G-nw-deactv-rej-tx-odb | Total number of MS initiated PDP context deactivation requests rejected for 3G service due to operator determined barring. | Int32
> 2G-nw-deactv-rej-tx-odb | Total number of MS initiated PDP context deactivation requests rejected for 2G service due to operator determined barring. | Int32
> 3G-nw-deactv-rej-tx-mbms-cap-insuff-res | Total number of MS initiated PDP context deactivation requests rejected for 3G service due to insufficient resources for Multimedia Broadcast/Multicast Service (MBMS) capability. | Int32
> 2G-nw-deactv-rej-tx-mbms-cap-insuff-res | Total number of MS initiated PDP context deactivation requests rejected for 2G service due to insufficient resources for Multimedia Broadcast/Multicast Service (MBMS) capability. | Int32
> 3G-nw-deactv-rej-tx-llc-sndcp-fail-gb | Total number of MS initiated PDP context deactivation requests rejected for 3G service due to failure at the logical link control with sub network dependent convergence protocol at Gb interface. | Int32
> 2G-nw-deactv-rej-tx-llc-sndcp-fail-gb | Total number of MS initiated PDP context deactivation requests rejected for 2G service due to failure at the logical link control with sub network dependent convergence protocol at Gb interface. | Int32
> 3G-nw-deactv-rej-tx-insuff-res | Total number of MS initiated PDP context deactivation requests rejected due to insufficient resources in download direction for 3G service. | Int32
> 2G-nw-deactv-rej-tx-insuff-res | Total number of MS initiated PDP context deactivation requests rejected due to insufficient resources in download direction for 2G service. | Int32
> 3G-nw-deactv-rej-tx-miss-unkwn-apn | Total number of MS initiated PDP context deactivation requests rejected due to missing or unknown APN for 3G service. | Int32
> 2G-nw-deactv-rej-tx-miss-unkwn-apn | Total number of MS initiated PDP context deactivation requests rejected due to missing or unknown APN for 2G service. | Int32
> 3G-nw-deactv-rej-tx-unkwn-pdp-addr | Total number of MS initiated PDP context deactivation requests rejected due to unknown PDP context name or address for 3G service. | Int32
> 2G-nw-deactv-rej-tx-unkwn-pdp-addr | Total number of MS initiated PDP context deactivation requests rejected due to unknown PDP context name or address for 2G service. | Int32
> 3G-nw-deactv-rej-tx-usr-auth-fail | Total number of MS initiated PDP context deactivation requests rejected as user authentication failed for 3G service. | Int32
> 2G-nw-deactv-rej-tx-usr-auth-fail | Total number of MS initiated PDP context deactivation requests rejected as user authentication failed for 2G service. | Int32
> 3G-nw-deactv-rej-tx-actv-rej-ggsn | Total number of MS initiated PDP context deactivation requests rejected as request rejected by corresponding GGSN for 3G service. | Int32
> 2G-nw-deactv-rej-tx-actv-rej-ggsn | Total number of MS initiated PDP context deactivation requests rejected as request rejected by corresponding GGSN for 2G service. | Int32
> 3G-nw-deactv-rej-tx-actv-rej-unspec | Total number of MS initiated PDP context deactivation requests rejected due to unknown or unspecified reasons for 3G service. | Int32
> 2G-nw-deactv-rej-tx-actv-rej-unspec | Total number of MS initiated PDP context deactivation requests rejected due to unknown or unspecified reasons for 2G service. | Int32
> 3G-nw-deactv-rej-tx-service-opt-no-support | Total number of MS initiated PDP context deactivation requests rejected as requested service option is not supported for 3G service. | Int32
> 2G-nw-deactv-rej-tx-service-opt-no-support | Total number of MS initiated PDP context deactivation requests rejected as requested service option is not supported for 2G service. | Int32
> 3G-nw-deactv-rej-tx-service-opt-no-subs | Total number of MS initiated PDP context deactivation requests rejected as subscriber is not subscribed requested service option for 3G service. | Int32
> 2G-nw-deactv-rej-tx-service-opt-no-subs | Total number of MS initiated PDP context deactivation requests rejected as subscriber is not subscribed requested service option for 2G service. | Int32
> 3G-nw-deactv-rej-tx-svc-opt-temp-out-order | Total number of MS initiated PDP context deactivation requests rejected as requested service option is temporarily out of order for 3G service. | Int32
> 2G-nw-deactv-rej-tx-svc-opt-temp-out-order | Total number of MS initiated PDP context deactivation requests rejected as requested service option is temporarily out of order for 2G service. | Int32
> 3G-nw-deactv-rej-tx-nsapi-already-used | Total number of MS initiated PDP context deactivation requests rejected as requested NSAPI is already in use for 3G service. | Int32
> 2G-nw-deactv-rej-tx-nsapi-already-used | Total number of MS initiated PDP context deactivation requests rejected as requested NSAPI is already in use for 2G service. | Int32
> 3G-nw-deactv-rej-tx-reg-deactv | Total number of MS initiated PDP context deactivation requests rejected due to registration of deactivate message for 3G service. | Int32
> 2G-nw-deactv-rej-tx-reg-deactv | Total number of MS initiated PDP context deactivation requests rejected due to registration of deactivate message for 2G service. | Int32
> 3G-nw-deactv-rej-tx-qos-not-acc | Total number of MS initiated PDP context deactivation requests rejected as requested QoS is not accepted for 3G service. | Int32
> 2G-nw-deactv-rej-tx-qos-not-acc | Total number of MS initiated PDP context deactivation requests rejected as requested QoS is not accepted for 2G service. | Int32
> 3G-nw-deactv-rej-tx-nwt-fail | Total number of MS initiated PDP context deactivation requests rejected due to network failure for 3G service. | Int32
> 2G-nw-deactv-rej-tx-nwt-fail | Total number of MS initiated PDP context deactivation requests rejected due to network failure for 2G service. | Int32
> 3G-nw-deactv-rej-tx-reactivation-req | Total number of MS initiated PDP context deactivation requests rejected due re-activation request arrived before completion of deactivation procedure for 3G service. | Int32
> 2G-nw-deactv-rej-tx-reactivation-req | Total number of MS initiated PDP context deactivation requests rejected due re-activation request arrived before completion of deactivation procedure for 2G service. | Int32
> 3G-nw-deactv-rej-tx-no-feature-support | Total number of MS initiated PDP context deactivation requests for 3G service rejected as requested feature is not supported. | Int32
> 2G-nw-deactv-rej-tx-no-feature-support | Total number of MS initiated PDP context deactivation requests for 2G service rejected as requested feature is not supported. | Int32
> 3G-nw-deactv-rej-tx-sem-err-tft-op | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to semantic error in subscriber TFT option. | Int32
> 2G-nw-deactv-rej-tx-sem-err-tft-op | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to semantic error in subscriber TFT option. | Int32
> 3G-nw-deactv-rej-tx-syn-err-tft-op | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to syntax error in subscriber TFT option. | Int32
> 2G-nw-deactv-rej-tx-syn-err-tft-op | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to syntax error in subscriber TFT option. | Int32
> 3G-nw-deactv-rej-tx-unknown-ctx | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to unknown context in request. | Int32
> 2G-nw-deactv-rej-tx-unknown-ctx | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to unknown context in request. | Int32
> 3G-nw-deactv-rej-tx-ctx-no-tft-already-actv | Total number of MS initiated PDP context deactivation requests for 3G service rejected as no TFT is active in this context. | Int32
> 2G-nw-deactv-rej-tx-ctx-no-tft-already-actv | Total number of MS initiated PDP context deactivation requests for 2G service rejected as no TFT is active in this context. | Int32
> 3G-nw-deactv-rej-tx-mcast-grp-mem-tout | Total number of MS initiated PDP context deactivation requests for 3G service rejected as multicast group memory is timed-out. | Int32
> 2G-nw-deactv-rej-tx-mcast-grp-mem-tout | Total number of MS initiated PDP context deactivation requests for 2G service rejected as multicast group memory is timed-out. | Int32
> 3G-nw-deactv-rej-tx-sem-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to semantic error in packet filter. | Int32
> 2G-nw-deactv-rej-tx-sem-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to semantic error in packet filter. | Int32
> 3G-nw-deactv-rej-tx-syn-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to syntax error in packet filter. | Int32
> 2G-nw-deactv-rej-tx-syn-err-pkt-filter | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to syntax error in packet filter. | Int32
> 3G-nw-deactv-rej-tx-invalid-trans-id | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to invalid transaction id. | Int32
> 2G-nw-deactv-rej-tx-invalid-trans-id | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to invalid transaction id. | Int32
> 3G-nw-deactv-rej-tx-sem-incorrect-msg | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to semantically incorrect message. | Int32
> 2G-nw-deactv-rej-tx-sem-incorrect-msg | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to semantically incorrect message. | Int32
> 3G-nw-deactv-rej-tx-inval-mand-info | Total number of MS initiated PDP context deactivation requests for 3G service rejected as mandatory information in message is invalid. | Int32
> 2G-nw-deactv-rej-tx-inval-mand-info | Total number of MS initiated PDP context deactivation requests for 2G service rejected as mandatory information in message is invalid. | Int32
> 3G-nw-deactv-rej-tx-msg-non-existent | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to non-existent type of message. | Int32
> 2G-nw-deactv-rej-tx-msg-non-existent | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to non-existent type of message. | Int32
> 3G-nw-deactv-rej-tx-ie-non-existent | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to non-existence of information element. | Int32
> 2G-nw-deactv-rej-tx-ie-non-existent | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to non-existence of information element. | Int32
> 3G-nw-deactv-rej-tx-cond-ie-err | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to error in conditional information element. | Int32
> 2G-nw-deactv-rej-tx-cond-ie-err | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to error in conditional information element. | Int32
> 3G-nw-deactv-rej-tx-prot-err-unspec | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to unspecified protocol error. | Int32
> 2G-nw-deactv-rej-tx-prot-err-unspec | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to unspecified protocol error. | Int32
> 3G-nw-deactv-rej-tx-apn-rest-incomap-actv-pdp | Total number of MS initiated PDP context deactivation requests for 3G service rejected due to incompatible APN for PDP context activation. | Int32
> 2G-nw-deactv-rej-tx-apn-rest-incomap-actv-pdp | Total number of MS initiated PDP context deactivation requests for 2G service rejected due to incompatible APN for PDP context activation. | Int32
> 3G-nw-deactv-rej-tx-msg-not-compat-prot-state | Total number of MS initiated PDP context deactivation requests for 3G service rejected as message is not compatible with protocol state. | Int32
> 2G-nw-deactv-rej-tx-msg-not-compat-prot-state | Total number of MS initiated PDP context deactivation requests for 2G service rejected as message is not compatible with protocol state. | Int32
> 3G-nw-deactv-rej-tx-rcvry-on-tmr-expiry | Total number of MS initiated PDP context deactivation requests for 3G service rejected as timer expired for recovery. | Int32
> 2G-nw-deactv-rej-tx-rcvry-on-tmr-expiry | Total number of MS initiated PDP context deactivation requests for 2G service rejected as timer expired for recovery. | Int32
> 3G-total-sm-status-req-rx | Total number of session management (SM) status request messages received for 3G service. | Int32
> 2G-total-sm-status-req-rx | Total number of session management (SM) status request messages received for 2G service. | Int32
> 3G-total-sm-status-req-tx | Total number of session management (SM) status request messages sent for 3G service. | Int32
> 2G-total-sm-status-req-tx | Total number of session management (SM) status request messages sent for 2G service. | Int32
> RNC-rab-modify-req | Total number of Radio Network Controller (RNC) initiated radio access bearer (RAB) modify requests received at the SGSN. | Int32
> RNC-rab-rel-req | Total number of RNC initiated RAB release requests received at the SGSN. | Int32
> RNC-rab-modify-num | Total number of RNC initiated RAB modified messages received. | Int32
> RNC-rab-rel-num | Total number of RNC initiated RAB release requests handled at SGSN. | Int32
> rab-assign-req | Total number of SGSN initiated RAB assignment requests sent to all RNCs. | Int32
> rab-assign-rsp | Total number of SGSN initiated RAB assignment response received from all RNCs. | Int32
> rab-assign-rej | This statistic has been obsoleted. | Int32
> rab-setup-reattempt | Total number of radio access bearer (RAB) setup reattempted. | Int32
> rab-set/mod-req | Total number of SGSN initiated RAB setup or modify requests sent to all RNCs. | Int32
> rab-set/mod-acc | Total number of SGSN initiated RAB setup or modify accept messages received from all RNCs. | Int32
> rab-set/mod-tmr-expired | Total events when RAB setup/modify timer expired. | Int32
> rab-set/mod-fail | Total events when RAB setup/modify procedure failed | Int32
> rab-rel-req | Total number of SGSN initiated RAB release request messages sent to all RNCs. | Int32
> rab-rel-accept | Total number of SGSN initiated RAB release accept messages received from all RNCs. | Int32
> rab-rel-tmr-expired | Total events when RAB release timer expired. | Int32
> rab-rel-fail | Total radio access bearer release requests failed | Int32
> rab-queued | Total radio access bearer requests queued for transmission. | Int32
> rab-rel-pre-empt | Total number of RAB released due to pre-empted event. | Int32
> rab-rel-utran | Total number of RAB released due to initiation from UTRAN. | Int32
> rab-rel-ue-radio-lost | Total number of RAB released due to UE radio connection lost. | Int32
> total-rab-rej | Total RAB setup/modify/release requests rejected. | Int32
> rab-rej-rab-preempt | Description: Total number of RAB requests rejected due to pre-empted event. Triggers: Increments when RNC initiated RAB release procedure sends RAB Release request with this cause. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-overall-tmr-exp | Description: Total number of RAB requests for relocation rejected due to expiry of timer TRELOCoverall. This specifies the maximum time for the protection of overall Relocation procedure in the source RNC. Triggers: Increments when the source RNC initiates the Iu Release Request procedure towards the SGSN with a cause value “TRELOCoverall expiry”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-prep-tmr-exp | Description: Total number of RAB requests for relocation rejected due to expiry of timer TRELOCprep. This specifies the maximum time for expiry of Relocation Preparation procedure in the source RNC. Triggers: Increments when the source RNC cancels the Relocation Preparation procedure by initiating the Relocation Cancel procedure with a cause value “TRELOCprep expiry”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-complete-tmr-exp | Description: Indicates the maximum time for waiting the relocation completion in the CN. Triggers: Increments when the SGSN initiate release of Iu connections towards the source and the target RNC initiates the Iu Release procedure with a cause value “TRELOCcomplete expiry”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-queuing-tmr-exp | Description: Indicates the maximum time in the RNC for queuing the request of RAB establishment or modification. Triggers: Increments when the RNC sends the RAB assignment response to report unsuccessful establishment/modification of RAB with the failed RAB ID list with the cause “Tqueuing Expiry”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-triggered | Description: Total number of RAB requests for relocation triggered. The action fails due to relocation of MS to another RNC. Triggers: Increments when the Relocation required message is sent with the cause “Relocation Triggered” to the SGSN. If the relocation becomes necessary during the RAB Assignment procedure, the RNC may interrupt the ongoing RAB Assignment procedure and initiate the Relocation Preparation procedure and send the RAB assignment response as failure cause “relocation required”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-unable-to-est-reloc | Description: Total number of RAB requests rejected because RAB failed to establish during relocation as it cannot be supported in the target RNC or the RAB did not exist in the source RNC. Triggers: Increments when the target RNC sends the RELOCATION REQUEST ACKNOWLEDGE message with a value in Cause IE “Unable to Establish During Relocation”, for the RABs rejected and received in RELOCATION REQUEST from SGSN, only if the Relocation Type IE is set to “UE involved in relocation of SRNS” in the request. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-unknown-target-rnc | Description: Total number of RAB requests rejected due to unknown target RNC in request. Triggers: Increments when the SGSN rejects the relocation of SRNS by sending a RELOCATION PREPARATION FAILURE message to the source RNC with Cause IE set to “Unknown target RNC”, if the target RNC is unknown to SGSN. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-cancel | Description: Total number of RAB requests rejected as relocation was cancelled due to interaction with other procedures. Triggers: Increments when SGSN issues the IU release command to RNC with the cause “Relocation Cancelled”, if the Relocation Preparation procedure is unsuccessfully terminated. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-success | Description: Total number of RAB requests rejected due to completion of successful relocation. Triggers: Increments when SGSN issues the IU release command to RNC with the cause “Successful Relocation”, if completion of successful relocation of SRNS happened. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-cypher-algo-no-support | Description: Total number of RAB requests rejected as the UTRAN or the UE is unable to support the requested ciphering and/or integrity protection algorithms. Triggers: If the target RNC cannot support any of the integrity protection (ciphering respectively) alternatives provided in the Integrity Protection Information IE or Encryption Information IE, in RELOCATION REQUEST from SGSN, it returns a RELOCATION FAILURE message with the cause “Requested Ciphering and/or Integrity Protection algorithms not supported”. RNC also sends the SECURITY MODE REJECT with the same cause for the same reason when receiving the SECURITY MODE COMMAND from SGSN. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-conflict-cypher-info | Description: Total number of RAB requests rejected due to conflict with the requested security mode configuration and the already existing security mode configuration. Triggers: If the target RNC receives a source RNC to target RNC Transparent Container IE containing Chosen Integrity Protection (Encryption respectively) Algorithm IE without Integrity Protection (Ciphering respectively) Key IE, it returns a RELOCATION FAILURE message with the cause “Conflict with already existing Integrity protection and/or Ciphering information”. RNC also sends the SECURITY MODE REJECT with the same cause for the same reason when receiving the SECURITY MODE COMMAND from SGSN. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-failure-radio-if-proc | Description: Total number of RAB requests rejected due to failure in radio interface procedure. Triggers: If the radio interface Security Mode Control procedure fails, a SECURITY MODE REJECT message will be sent to the SGSN with cause value “Failure in the Radio Interface Procedure” from RNC. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-rel-utran-reason | Description: Total number of RAB requests rejected as RAB release is initiated due to UTRAN generated reason. Triggers: Increments when RNC initiated RAB release procedure sends RAB Release request with this cause. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-utran-inactivity | Description: Total number of RAB requests rejected as RAB released due to user inactivity at UTRAN on one or more non real time RABs in order to optimize radio resource. Triggers: Increments when the source RNC initiates the Iu Release Request procedure towards the SGSN with a cause value “User Inactivity” for a particular MS. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-time-crit-relocation | Description: Total number of RAB requests rejected as relocation is requested for time critical reason. This cause value is reserved to represent all critical cases where the connection is likely to be dropped if relocation is not performed. Triggers: Increments when the source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Time Critical Relocation”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-traffic-class-unavail | Description: Total number of RAB request rejected as requested traffic class unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Traffic Class not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-invalid-rab-param-val | Description: Total number of RAB requests rejected due to invalid RAB parameter value. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Invalid RAB Parameters Value”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-max-bit-rate-unavail | Description: Total number of RAB requests rejected as requested maximum bit rate is unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Maximum Bit Rate not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-max-bit-rate-dl-unavail | Description: Total number of RAB requests rejected as requested maximum bit rate for downlink is unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Maximum Bit Rate for DL not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-max-bit-rate-ul-unavail | Description: Total number of RAB requests rejected as requested maximum bit rate for uplink is unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Maximum Bit Rate for DL not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-gbr-unavail | Description: Total number of RAB requests rejected as requested guaranteed bit rate is unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID with the cause “Requested Guaranteed Bit Rate not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-gbr-dl-unavail | Description: Total number of RAB requests rejected as requested guaranteed bit rate for downlink is unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Guaranteed Bit Rate for DL not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-gbr-ul-unavail | Description: Total number of RAB requests rejected as requested guaranteed bit rate for uplink is unavailable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Guaranteed Bit Rate for UL not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-trans-delay-not-achievable | Description: Total number of RAB requests rejected as requested transfer delay is not achievable. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Requested Transfer Delay not Achievable”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-inval-rab-param-combo | Description: Total number of RAB requests rejected due to invalid RAB parameter combination. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Invalid RAB Parameters Combination”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-violation-for-sdu-param | Description: Total number of RAB requests rejected due to occurrence of condition violation for Service Data Unit (SDU) parameters. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Condition Violation for SDU Parameters”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-violation-traffic-hanlde-prio | Description: Total number of RAB requests rejected due to occurrence of condition violation for traffic handling priority. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Condition Violation for Traffic Handling Priority”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-violation-for-gbr | Description: Total number of RAB request rejected due to occurrence of condition violation for guaranteed bit rate. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Condition Violation for Guaranteed Bit Rate”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-usr-plane-ver-unsupported | Description: Total number of RAB requests rejected as requested user plane version is not supported. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “User Plane Versions not Supported”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-iu-up-failure | Description: Total number of RAB requests rejected due to Iu UP activation failure. Triggers: Increments when RNC sends the RAB assignment response to report unsuccessful establishment/modification of a RAB with the failed RAB ID list with the cause “Iu UP Failure”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-alloc-expiry | Description: Total number of RAB requests rejected as Relocation Resource Allocation procedure failed due to expiry of the TRELOCalloc timer. Triggers: Increments when SGSN is unable to complete the relocation of SRNS before the TRELOCalloc expiry. The SGSN then issues a RELOCATION PREPARATION FAILURE message to the source RNC with the cause “TRELOCalloc expiry”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-failure-target-system | Description: Total number of RAB request rejected due to relocation failure in target CN/RNC or target system. Triggers: Increments when SGSN cannot complete the relocation of SRNS due to failure in the Target CN/RNC or Target System. The SGSN then issues a RELOCATION PREPARATION FAILURE message to the source RNC with the cause “Relocation Failure in Target CN/RNC or Target System”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-invalid-rdb-id | Description: Total number of RAB requests rejected due to invalid RAB ID in the RNC. Triggers: If the RAB ID of a RAB requested to be released is unknown in the RNC, RNC will report as a RAB failed to release with the cause value “Invalid RAB ID” in RAB Assignment Response to SGSN. If RAB ID of RAB requested to be transferred is unknown in RNC, the SRNS CONTEXT RESPONSE message will contain the cause with the RAB ID. The RAB ID IE for each RAB for which UTRAN is not able to transfer a data volume report due to unknown RAB ID is included in the DATA VOLUME REPORT message together with a Cause IE “Invalid RAB ID”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-no-remaining-rab | Description: Total number of RAB requests rejected as no RAB is available. Triggers: Increments when SGSN issues the IU release command to RNC with the cause “No remaining RAB”, if there is no RAB associated with the IU. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-interaction-with-other-proc | Description: Total number of RAB requests rejected as relocation was cancelled due to interaction with other procedure. Triggers: If source RNC triggers the RELOCATION CANCEL to SGSN with cause “Interaction with other procedure” when relocation preparation is triggered and it receives another message via the same signalling IU. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-integrity-check-fail | Description: Total number of RAB requests rejected due to repeated failure in integrity checking. Triggers: Increments when RNC issues the IU release request to SGSN with the cause “Repeated Integrity Checking Failure”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-type-not-supported | Description: Total number of RAB requests rejected as the RNC is not supporting the requested location request type either because it does not support the requested event or it does not support the requested report area. Triggers: If the RNC cannot deliver the location information as requested by the SGSN, due to non-support of the requested event, then it will send location report message indicating the UE location to be “Undetermined” with cause “Requested Request Type not supported”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-superseeded | Description: Total number of RAB requests rejected due to a second request on the same RAB. Triggers: In case of a request to modify or release a RAB that contains the RAB ID of a RAB being queued, the RAB will be taken out of the queue and treated according to the second request. The first request will be responded to as RAB failed to setup or modify the cause value “Request superseded” by RNC to SGSN in RAB Assignment Response. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-rel-due-to-ue-sig-con-rel | Description: Total number of RAB requests rejected as RAB released due to UE generated signaling connection release. Triggers: Increments when RNC issues the IU release request to SGSN with the cause “Release due to UE generated signalling connection release”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-res-optimization-reloc | Description: Total number of RAB requests rejected as resource optimization for relocation occurred. Triggers: Increments when the source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Resource Optimization Relocation”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-req-info-unavail | Description: Total number of RAB requests rejected as requested information is unavailable. Triggers: Increments when the source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Resource Optimization Relocation”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-due-to-radio-reason | Description: Total number of RAB requests rejected due to radio related errors/causes. Triggers: Increments when the source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Relocation desirable for radio reasons”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-unsupported-target-system | Description: Total number of RAB requests rejected as relocation is not supported in target system. Triggers: Increments when SGSN is unable to complete the relocation of SRNS due to failure in the Target CN/RNC or Target System. The SGSN then issues a RELOCATION PREPARATION FAILURE message to the source RNC with the cause “Relocation not supported in Target RNC or Target system”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-directed-retry | Description: Total number of RAB requests rejected as retries directed by system. Triggers: Directed retry is the process of assigning a User Equipment to a radio resource that does not belong to the serving RNC, for example, in situations of congestion. It is triggered by the RAB Assignment procedure and employs relocation procedures. The RNC may indicate an impending directed retry attempt to GSM by sending a RAB ASSIGNMENT RESPONSE message with a RAB ID included in the list of RABs failed to setup and a cause value of “Directed Retry”. The RNC invokes relocation by sending a RELOCATION REQUIRED message to the active SGSN node with the cause “Directed Retry”. The source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Time Critical Relocation”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-radio-con-with-ue-lost | Description: Total number of RAB requests rejected as radio connection with UE is lost. Triggers: Increments when RNC initiated RAB release procedure sends RAB Release request with this cause. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-rnc-unable-to-estab-all-rfcs | Description: Total number of RAB requests rejected as RNC is unable to establish all RAB subflow combinations indicated within the RAB Parameters IE. Triggers: Increments when the RNC cannot initialise the requested user plane mode for any of the user plane mode versions in the UP Mode Versions IE according to the rules for initialization of the respective user plane mode versions. The RAB Assignment Response (failure) with the cause value “RNC unable to establish all RFCs” will be received from RNC. It will be received for the same reason in RELOCATION REQUEST ACKNOWLEDGE message from RNC. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-deciphering-keys-unavail | Description: Total number of RAB requests rejected as RNC is unable to provide the requested deciphering keys. Triggers: Increments when the RNC is unable to provide the requested deciphering keys. The RNC will then send a LOCATION RELATED DATA FAILURE message including the Cause IE to the SGSN with the cause “Deciphering Keys Not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-dedicated-assistance-data-unavail | Description: Total number of RAB requests rejected as RNC is unable to successfully deliver the requested dedicated assistance data to the UE. Triggers: Increments when the RNC is unable to successfully deliver the requested dedicated assistance data to the UE. The RNC will then send a LOCATION RELATED DATA FAILURE message including the Cause IE to the SGSN with the cause “Dedicated Assistance data Not Available”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reloc-target-not-allowed | Description: Total number of RAB requests rejected as relocation to the indicated target cell is not allowed for the UE. Triggers: Increments when SGSN is unable to complete the relocation of SRNS if the Relocation is not allowed in Target Cell. The SGSN then issues a RELOCATION PREPARATION FAILURE message to the source RNC with the cause “Relocation Target not allowed”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-location-reporting-congestion | Description: Total number of RAB requests rejected due to an inability to support location reporting caused by overload. Triggers: Increments when the RNC cannot deliver the location information as requested by the SGSN due to non-availability of requested information. It will then send location report message indicating the UE location to be “Undetermined” with cause “Location Reporting Congestion”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-reduce-load-in-serving-cell | Description: Total number of RAB requests rejected as the load reduction on serving cell needs to be reduced. Triggers: Increments when the source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Reduce Load in Serving Cell”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-no-radio-res-avail-in-target-cell | Description: Total number of RAB requests rejected as radio resource is unavailable in target cell. Triggers: Increments when SGSN is unable to complete the relocation of SRNS if the Resource is not available in Target Cell. The SGSN then issues a RELOCATION PREPARATION FAILURE message to the source RNC with the cause “No Radio Resources Available in Target Cell”. Target RNC will send RELOCATION FAILURE message to SGSN with the cause “Radio Resources Available in Target Cell”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-geran-iu-mode-failure | Description: Total number of RAB requests rejected due to failure in Iu mode in GERAN. The RAB establishment/modification/relocation failed because the GERAN BSC cannot provide an appropriate RAB due to limited capabilities within GERAN. Triggers: Increments when the RAB establishment/modification/relocation fails because the GERAN BSC cannot provide an appropriate RAB due to limited capabilities within GERAN. The RNC will then send RAB assignment response with the cause “GERAN Iu-mode failure”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-access-restrict-shared-nwtk | Description: Total number of RAB requests rejected as access is restricted in the cell due to shared network. Triggers: Increments when the source RNC initiates the Iu Release Request procedure towards the SGSN with a cause value “Access Restricted Due to Shared Networks”. The source RNC initiates relocation preparation procedure by sending a RELOCATION REQUIRED message with the cause “Access Restricted Due to Shared Networks”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-incoming-reloc-nwt-support-puesbine | Description: Total number of RAB requests rejected as the incoming relocation request is not accepted by the target RNC because of the Provision of UE Specific Behavior Information to Network Entities (PUESBINE) feature. Triggers: Increments when the target RNC cannot support the relocation due to PUESBINE feature. It sends a RELOCATION FAILURE message with the cause “Incoming Relocation Not Supported Due To PUESBINE Feature” To SGSN. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-traffic-target-more-source-cell | Description: Total number of RAB requests rejected as the traffic load in the target cell is higher than that in the source cell. Triggers: Increments when SGSN is unable to complete the relocation of SRNS if the Resource is not available in Target Cell. The SGSN will then issue a RELOCATION PREPARATION FAILURE message to the source RNC with the cause “Traffic Load In The Target Cell Higher Than In The Source Cell”. Target RNC sends RELOCATION FAILURE message to SGSN with the cause “Traffic Load In The Target Cell Higher Than In The Source Cell” to SGSN when load at the target cell is higher than that in the source cell. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-mbms-no-multicat-svc-for-ue | Description: Total number of RAB requests rejected for Multimedia Broadcast/Multicast Service (MBMS) feature as multicast service is not supported by user equipment. Triggers: Increments when SGSN is unable to process the UPLINK INFORMATION EXCHANGE REQUEST for reason that MS does not have the multicat service. The SGSN then sends the UPLINK INFORMATION EXCHANGE FAILURE message to the RNC about the reason for unsuccessful operation with a cause value “MBMS - No Multicast Service For This UE”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-mbms-unknown-ue-id | Description: Total number of RAB requests rejected for MBMS feature because the user equipment identification is unknown to the CN. Triggers: Increments when SGSN is unable to process the UPLINK INFORMATION EXCHANGE REQUEST for reason that UE is unknown to SGSN. The SGSN then sends the UPLINK INFORMATION EXCHANGE FAILURE message to the RNC about the reason for unsuccessful operation with a cause value “MBMS - Unknown UE ID”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-mbms-sess-start-no-data-bearer | Description: Total number of RAB requests rejected for MBMS feature as the session starts without any necessary data bearer. Triggers: Increments when the RNC decides to wait to establish the MBMS RAB. It then sends the MBMS SESSION START RESPONSE message with the cause value “Successful MBMS Session Start - No Data Bearer Necessary” to SGSN for MBMS SESSION START REQUEST. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-mbms-superseed-nnsf | Description: Total number of RAB requests rejected for MBMS feature as request superseded due to NAS Node Selection Function (NNSF). Triggers: Increments when NNSF is active and the RNC is received from several CN nodes for a certain MBMS Bearer Service. The MBMS SESSION START message is also sent by the SGSN, and the RNC informs the SGSN with MBMS SESSION START FAILURE message and cause value “MBMS - Superseded Due To NNSF”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-mbms-ue-linking-already-done | Description: Total number of RAB requests rejected for MBMS feature as user equipment is already linked to the given Multicast service. Triggers: Increments when the RNC sends the MBMS UE LINKING RESPONSE message for unsuccessful linking(s) with cause value “MBMS - UE Linking Already Done”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-mbms-ue-delinking-failure | Description: Total number of RAB requests rejected for MBMS feature as user equipment delinking failed because the UE had not been linked to the given Multicast service. Triggers: Increments when the RNC sends the MBMS UE LINKING RESPONSE message for unsuccessful de-linking(s) with cause value “MBMS - UE De-Linking Failure - No Existing UE Linking”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-tmgi-unknown | Description: Total number of RAB requests rejected as the indicated Temporary Mobile Group Identifier (TMGI) is unknown. Triggers: Increments when the MBMS REGISTRATION FAILURE message sent from SGSN informs the RNC about the reason for unsuccessful MBMS registration operation with cause value “TMGI Unknown”. Availability: per SGSN service, per RAI Type: Counter | Int32
> rab-rej-ms-unspecified-failure | Description: Total number of RAB requests rejected due to unspecified failure at MS. Triggers: Availability: per SGSN service, per RAI Type: Counter | Int32
> SRNS-ctxt-req-sent | Total number of Serving Radio Network Subsystem (SRNS) context request sent. | Int32
> SRNS-ctxt-rsp-rcvd | Total number of SRNS context request received. | Int32
> SRNS-ctxt-req-tmr-expired | Total number of events when SRNS context request timer expired. | Int32
> SRNS-ctxt-total-pdp-acc | Total number of PDP context request by SRNS accepted. | Int32
> SRNS-ctxt-total-pdp-rej | Total number of PDP context request by SRNS rejected. | Int32
> SRNS-data-fwd-cmd-sent | Total number of data forward command sent by SRNS. | Int32
> srns-ctx-deny-rab-preempt | Total number of PDP context request by SRNS denied due to RAB preempted procedure. | Int32
> srns-ctx-deny-reloc-overall-tmr-exp | Total number of PDP context request by SRNS denied due to overall timer expired for relocation. | Int32
> srns-ctx-deny-reloc-prep-tmr-exp | Total number of PDP context request by SRNS denied due to relocation preparation timer expired. | Int32
> srns-ctx-deny-reloc-complete-tmr-exp | Total number of PDP context request by SRNS denied due to relocation complete timer expired. | Int32
> srns-ctx-deny-queuing-tmr-exp | Total number of PDP context request by SRNS denied due to relocation queuing timer expired. | Int32
> srns-ctx-deny-reloc-triggered | Total number of PDP context request by SRNS denied due to relocation triggered. | Int32
> srns-ctx-deny-unable-to-est-reloc | Total number of PDP context request by SRNS denied due to unable to establish relocation. | Int32
> srns-ctx-deny-unknown-target-rnc | Total number of PDP context request by SRNS denied due to unknown target RNC. | Int32
> srns-ctx-deny-reloc-cancel | Total number of PDP context request by SRNS denied due to relocation cancelled. | Int32
> srns-ctx-deny-reloc-success | Total number of PDP context request by SRNS denied due to successful relocation. | Int32
> srns-ctx-deny-cypher-algo-no-support | Total number of PDP context request by SRNS denied as requested ciphering algorithm not supported. | Int32
> srns-ctx-deny-conflict-cypher-info | Total number of PDP context request by SRNS denied due to conflict with existing ciphering information. | Int32
> srns-ctx-deny-failure-radio-if-proc | Total number of PDP context request by SRNS denied due to failure in radio interface procedure. | Int32
> srns-ctx-deny-rel-utran-reason | Total number of PDP context request by SRNS denied as release occurred due to UTRAN generated reason. | Int32
> srns-ctx-deny-utran-inactivity | Total number of PDP context request by SRNS denied due to inactivity at UTRAN. | Int32
> srns-ctx-deny-time-crit-relocation | Total number of PDP context request by SRNS denied due to time critical relocation. | Int32
> srns-ctx-deny-req-traffic-class-unavail | Total number of PDP context request by SRNS denied as requested traffic class unavailable. | Int32
> srns-ctx-deny-invalid-rab-param-val | Total number of PDP context request by SRNS denied due invalid RAB parameter value. | Int32
> srns-ctx-deny-req-max-bit-rate-unavail | Total number of PDP context request by SRNS denied as requested maximum bit rate unavailable. | Int32
> srns-ctx-deny-req-max-bit-rate-dl-unavail | Total number of PDP context request by SRNS denied as requested maximum bit rate for downlink unavailable. | Int32
> srns-ctx-deny-req-max-bit-rate-ul-unavail | Total number of PDP context request by SRNS denied as requested maximum bit rate for uplink unavailable. | Int32
> srns-ctx-deny-req-gbr-unavail | Total number of PDP context request by SRNS denied as requested guaranteed bit rate unavailable. | Int32
> srns-ctx-deny-req-gbr-dl-unavail | Total number of PDP context request by SRNS denied as requested guaranteed bit rate for downlink unavailable. | Int32
> srns-ctx-deny-req-gbr-ul-unavail | Total number of PDP context request by SRNS denied as requested guaranteed bit rate for uplink unavailable. | Int32
> srns-ctx-deny-req-trans-delay-not-achieve | Total number of PDP context request by SRNS denied as requested transfer delay is not achievable. | Int32
> srns-ctx-deny-inval-rab-param-combo | Total number of PDP context request by SRNS denied as invalid RAB parameter combination. | Int32
> srns-ctx-deny-violation-for-sdu-param | Total number of PDP context request by SRNS denied as violation for service data unit (SDU) parameters occurred. | Int32
> srns-ctx-deny-violation-traffic-hanlde-prio | Total number of PDP context request by SRNS denied as violation for traffic handling priority occurred. | Int32
> srns-ctx-deny-violation-for-gbr | Total number of PDP context request by SRNS denied as violation for guaranteed bit rate occurred. | Int32
> srns-ctx-deny-usr-plane-ver-unsupported | Total number of PDP context request by SRNS denied as user plane version not supported. | Int32
> srns-ctx-deny-ip-up-failure | Total number of PDP context request by SRNS denied as Iu activation failure occurred. | Int32
> srns-ctx-deny-reloc-alloc-expiry | Total number of PDP context request by SRNS denied as allocation timer expired for RAB relocation. | Int32
> srns-ctx-deny-reloc-failure-target-system | Total number of PDP context request by SRNS denied due to relocation failure in target system. | Int32
> srns-ctx-deny-invalid-rdb-id | Total number of PDP context request by SRNS denied due to invalid RAB id in message. | Int32
> srns-ctx-deny-no-remaining-rab | Total number of PDP context request by SRNS denied as no RAB available. | Int32
> srns-ctx-deny-interaction-with-other-proc | Total number of PDP context request by SRNS denied due to interaction with other procedure occurred. | Int32
> srns-ctx-deny-integrity-check-fail | Total number of PDP context request by SRNS denied as repeated integrity check failed. | Int32
> srns-ctx-deny-req-type-not-supported | Total number of PDP context request by SRNS denied as request type not supported. | Int32
> srns-ctx-deny-req-superseeded | Total number of PDP context request by SRNS denied as request superseded by new request. | Int32
> srns-ctx-deny-rel-due-to-ue-sig-con-rel | Total number of PDP context request by SRNS denied as RAB released due to UE generated signaling connection release. | Int32
> srns-ctx-deny-res-optimization-reloc | Total number of PDP context request by SRNS denied as resource optimization for relocation occurred. | Int32
> srns-ctx-deny-req-info-unavail | Total number of PDP context request by SRNS denied as requested information unavailable. | Int32
> srns-ctx-deny-reloc-due-to-radio-reason | Total number of PDP context request by SRNS denied due to radio related errors/causes. | Int32
> srns-ctx-deny-reloc-unsupport-target-sys | Total number of PDP context request by SRNS denied as relocation not supported in target system. | Int32
> srns-ctx-deny-directed-retry | Total number of PDP context request by SRNS denied as retries directed by system. | Int32
> srns-ctx-deny-radio-con-with-ue-lost | Total number of PDP context request by SRNS denied as radio connection with UE lost. | Int32
> srns-ctx-deny-rnc-unable-to-estab-all-rfcs | Total number of PDP context request by SRNS denied as RNCs unable to establish all radio frequency communications. | Int32
> srns-ctx-deny-deciphering-keys-unavail | Total number of PDP context request by SRNS denied as deciphering keys not available for procedure. | Int32
> srns-ctx-deny-dedicated-assist-data-unavail | Total number of PDP context request by SRNS denied as dedicated assistance data not available for procedure. | Int32
> srns-ctx-deny-reloc-target-not-allowed | Total number of PDP context request by SRNS denied as relocation is not allowed on target system. | Int32
> srns-ctx-deny-location-reporting-congestion | Total number of PDP context request by SRNS denied as congestion reported in specific location. | Int32
> srns-ctx-deny-reduce-load-in-serving-cell | Total number of PDP context request by SRNS denied as load reduction occurred in serving cell. | Int32
> srns-ctx-deny-no-radio-res-avail-target-cell | Total number of PDP context request by SRNS denied as no radio resource available in target cell. | Int32
> srns-ctx-deny-geran-iu-mode-failure | Total number of PDP context request by SRNS denied due to failure in Iu mode in GERAN. | Int32
> srns-ctx-deny-access-restrict-shared-nwtk | Total number of PDP context request by SRNS denied as access restricted in shared network. | Int32
> srns-ctx-deny-in-reloc-nwt-support-puesbine | Total number of PDP context request by SRNS denied as incoming relocation request is not supported in network due to Provision of UE Specific Behavior Information to Network Entities (PUESBINE) feature. | Int32
> srns-ctx-deny-traffic-target-more-src-cell | Total number of PDP context request by SRNS denied as traffic in target cell is higher than the source cell. | Int32
> srns-ctx-deny-mbms-no-multicat-svc-for-ue | Total number of SRNS context request for Multimedia Broadcast/Multicast Service (MBMS) feature denied as multicast service is not supported by user equipment. | Int32
> srns-ctx-deny-mbms-unknown-ue-id | Total number of SRNS context request for MBMS feature denied due to user equipment identification is unknown. | Int32
> srns-ctx-deny-mbms-sess-start-no-data-bearer | Total number of SRNS context request for MBMS feature denied as session start without any necessary data bearer. | Int32
> srns-ctx-deny-mbms-superseed-nnsf | Total number of SRNS context request for MBMS feature denied as request superseded due to NAS node selection function (NNSF). | Int32
> srns-ctx-deny-mbms-ue-linking-already-done | Total number of SRNS context request for MBMS feature denied as user equipment is already linked. | Int32
> srns-ctx-deny-mbms-ue-delinking-failure | Total number of SRNS context request for MBMS feature denied as user equipment delinking failed due to any reason. | Int32
> srns-ctx-deny-tmgi-unknown | Total number of SRNS context request denied as temporary mobile group identifier is unknown. | Int32
> srns-ctx-deny-ms-unspecified-failure | Total number of SRNS context request denied due to unspecified failure at MS. | Int32
> srns-ctx-deny-no-response-from-rnc | Total number of SRNS context request denied due to no response from RNC. | Int32
> map-open-req-tx | Total number of mobile application part (MAP) open requests sent. | Int32
> map-open-req-rx | Total number of mobile application part (MAP) open requests received. | Int32
> map-open-rsp-tx | Total number of MAP open response sent. | Int32
> map-open-rsp-rx | Total number of MAP open response received. | Int32
> map-close-tx | Total number of MAP close response sent. | Int32
> map-close-rx | Total number of MAP close response received. | Int32
> map-abort-tx | Total number of MAP abort request sent. | Int32
> map-abort-rx | Total number of MAP abort request received. | Int32
> map-auth-req-tx | Description: Total number of Send Authentication Request messages transmitted to HLR. Triggers: Counter increments when a MAP Send Authentication Request is initiated from SGSN. Availability: per SGSN service Type: Counter | Int32
> map-auth-succes | Total number of MAP authentication successful. | Int32
> map-auth-fail | Description: Total number of User Error / Provider Error received in response to SAI request. Triggers: Counter increments when User Error / Provider Error is received from HLR. Availability: per SGSN service Type: Counter | Int32
> map-auth-timeouts-rcvd | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when there is no response from the HLR for map-auth-fail-rep-req-tx message initiated from SGSN. Availability: per SGSN service Type: Counter | Int32
> map-imei-req-tx | Description: Total number of MAP Check IMEI requests initiated towards EIR. Triggers: Counter increments when MAP CHECK IMEI Request is sent. Availability: per SGSN service Type: Counter | Int32
> map-imei-succes | Description: Total number of successful responses for MAP Check IMEI requests. Triggers: Counter increments when MAP CHECK IMEI Request is sent. Availability: per SGSN service Type: Counter | Int32
> map-imei-fail | Description: Total number of failure responses for MAP Check IMEI requests received from EIR. Triggers: Counter increments when MAP Return Error / Provider Error is received in response. Availability: per SGSN service Type: Counter | Int32
> map-imei-timeout | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when there is no response from HLR. Availability: per SGSN service Type: Counter | Int32
> map-gprs-update-loc-req-tx | Description: Total number of UGL (GPRS Update Location) request initiated towards HLR. Triggers: Counter increments when UGL request is sent to HLR. Availability: per SGSN service Type: Counter | Int32
> map-gprs-update-loc-rsp-tx | Description: Total number of successful response messages sent in response to UGL request. Triggers: Counter increments when successful response is received from the HLR. Availability: per SGSN service Type: Counter | Int32
> map-gprs-update-loc-err-tx | Description: Total number of Failure response (User Error/Provider Error) messages received in response to UGL request. Triggers: Counter increments when MAP Return Error / Provider Error is received to UGL request. Availability: per SGSN service Type: Counter | Int32
> map-gprs-update-loc- timeouts-rx | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments if there is no response from HLR. Availability: per SGSN service Type: Counter | Int32
> map-cancel-loc-req-rx | Description: Total number of Cancel Location Request received from HLR. Triggers: Counter increments when MAP Cancel Location Request is received. Availability: per SGSN service Type: Counter | Int32
> map-cancel-loc-rsp-tx | Description: Total number of successful Cancel Location Response messages sent to HLR. Triggers: Counter increments when successful response is sent to HLR. Availability: per SGSN service Type: Counter | Int32
> map-cancel-loc-err-tx | Description: Total number of Error response messages sent to HLR. Triggers: Counter increments when MAP Return Error is sent to HLR. Availability: per SGSN service Type: Counter | Int32
> map-del-subs-req-rx | Description: Total number of Delete Subscription Data Request received from HLR. Triggers: Counter increments when MAP Delete Subscription Data (DSD) message is received. Availability: per SGSN service Type: Counter | Int32
> map-del-subs-rsp-tx | Description: Total number of successful responses for Delete Subscription Data request sent to HLR. Triggers: Counter increments when MAP Delete Subscription Data (DSD) message is received. Availability: per SGSN service Type: Counter | Int32
> map-del-subs-ret-tx | Description: Total number of Error responses sent for Delete Subscription Data (DSD) request received. Triggers: Counter increments when failure response is sent to HLR. Availability: per SGSN service Type: Counter | Int32
> map-insert-subs-rcvd | Total number of insert subscriber data requests received by MAP. | Int32
> map-standalone-isd-rcvd | Total number of standalone insert subscriber data requests received by MAP. | Int32
> map-isd-rsp-tx | Total number of insert subscriber data requests sent by MAP. | Int32
> map-isd-err-tx | Total number of insert subscriber data failure response sent by MAP. | Int32
> map-auth-fail-rept-req-tx | Description: Total number of Authentication Failure Report Request messages transmitted by MAP. Triggers: Counter increments when a message is initiated to inform HLR that certain vectors had problem in authenticating with the MS. Availability: per SGSN service Type: Counter | Int32
> map-auth-fail-rept-rsp-rx | Description: Total number of Authentication Failure Report Request messages received by MAP. Triggers: Counter increments when successful response is received in response to map-auth-fail-rep-req-tx. Availability: per SGSN service Type: Counter | Int32
> map-auth-fail-rept-err-rx | Description: Total number of User Error and Provider Error received for the Authentication Failure Report Request sent to HLR. Triggers: Counter increments when MAP Return Error/Provider Error is received in response to map-auth-fail-rep-req-tx message. There will be no effect on the call due to this. Availability: per SGSN service Type: Counter | Int32
> map-auth-fail-rept-timeouts-rcvd | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when MAP Return Error / Provider Error is received in response to map-auth-fail-rep-req-tx. There will be no effect on the call due to this. Availability: per SGSN service Type: Counter | Int32
> map-purge-req-tx | Description: Total number of MAP Purge Request messages initiated towards HLR. Triggers: Counter increments when MAP Purge Request is transmitted. Availability: per SGSN service Type: Counter | Int32
> map-purge-success | Description: Total number of successful MAP Purge Request messages sent to HLR. Triggers: Counter increments when successful response is received from HLR. Availability: per SGSN service Type: Counter | Int32
> map-purge-fail | Description: Total number of Failure response received from HLR. Triggers: Counter increments when MAP Return Error / Provider Error is received in response. Availability: per SGSN service Type: Counter | Int32
> map-purge-timeouts-rcvd | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when there is no response from HLR. Availability: per SGSN service Type: Counter | Int32
> map-hlr-reset-rcvd | Total number of HLR reset indicator received by MAP. | Int32
> map-mo-fwd-req-sent | Total number of mobile originated forward request messages sent to MAP. | Int32
> map-mo-fwd-rsp-rcvd | Total number of mobile originated forward response messages received from MAP. | Int32
> map-mo-fwd-rsp-failed | Total number of mobile originated forward response messages failed at MAP. | Int32
> map-mo-fwd-rsp-time-out | Total number of mobile originated forward response messages timed-out at MAP. | Int32
> map-mt-fwd-req-sent | Total number of mobile terminated forward request messages sent to MAP. | Int32
> map-mt-fwd-rsp-rcvd | Total number of mobile terminated forward request messages received from MAP. | Int32
> map-mt-fwd-rsp-failed | Total number of mobile terminated forward response messages failed at MAP. | Int32
> map-ready-for-sm-req | Total number of MAP ready for session management request received. | Int32
> map-ready-for-sm-rsp | Total number of MAP ready for session management request response received. | Int32
> map-ready-for-sm-rsp-failed | Total number of MAP ready for session management requests failed. | Int32
> map-ready-for-sm-rsp-time-out | Total number of MAP ready for session management requests timed-out. | Int32
> tcap-total-active-trans | Description: Total number of active transaction capabilities application part (TCAP) Dialogs in the system. Triggers: Counter increments when a new TCAP Dialog is created. Availability: per SGSN service Type: Gauge | Int32
> tcap-total-active-invoks | Total number of active transactions invoked by TCAP. Type: Gauge | Int32
> tcap-total-msg-drops | Total number of TCAP message drops. | Int32
> tcap-total-msg-rcvd | Total number of TCAP message received. | Int32
> tcap-total-msg-sent | Total number of TCAP message sent. | Int32
> tcap-uni-dir-msg-rcvd | Total number of TCAP unidirectional messages received. | Int32
> tcap-uni-dir-msg-sent | Total number of TCAP unidirectional messages sent. | Int32
> tcap-begin-msg-rcvd | Total number of messages received for TCAP begin state. | Int32
> tcap-begin-msg-sent | Total number of messages sent for TCAP begin state. | Int32
> tcap-continue-msg-rcvd | Total number of messages received for TCAP continue state. | Int32
> tcap-continue-msg-sent | Total number of messages sent for TCAP continue state. | Int32
> tcap-end-msg-rcvd | Total number of messages received for TCAP end state. | Int32
> tcap-end-msg-sent | Total number of messages sent for TCAP end state. | Int32
> tcap-total-abort-rcvd | Total number of messages received for TCAP abort state. | Int32
> tcap-total-abort-sent | Total number of messages sent for TCAP abort state. | Int32
> tcap-total-comp-rx | Total number of TCAP components received. | Int32
> tcap-total-comp-tx | Total number of TCAP components sent. | Int32
> tcap-total-comp-invoke-rx | Total number of invoke messages for TCAP component received. | Int32
> tcap-total-comp-invoke-tx | Total number of invoke messages for TCAP component sent. | Int32
> tcap-comp-retresult-rx | Total number of return result messages for TCAP component received. | Int32
> tcap-comp-retresult-tx | Total number of return result messages for TCAP component sent. | Int32
> tcap-comp-reterr-rx | Total number of return error messages for TCAP component received. | Int32
> tcap-comp-reterr-tx | Total number of return error messages for TCAP component sent. | Int32
> tcap-comp-retrej-rx | Total number of return reject messages for TCAP component received. | Int32
> tcap-comp-retrej-tx | Total number of return reject messages for TCAP component sent. | Int32
> tcap-tran-unrec-msgtype-rx | Total number of protocol errors in transaction portion (P-ABORT) with unrecognized message type for TCAP received. | Int32
> tcap-tran-unrec-msgtype-tx | Total number of protocol errors in transaction portion with unrecognized message type for TCAP sent. | Int32
> tcap-tran-incorrect-rx | Total number of protocol errors in transaction portion with incorrect information for TCAP received. | Int32
> tcap-tran-incorrect-tx | Total number of protocol errors in transaction portion with incorrect information for TCAP sent. | Int32
> tcap-tran-badformed-rx | Total number of protocol errors in transaction portion with badly formatted transaction portion for TCAP received. | Int32
> tcap-tran-badformed-tx | Total number of protocol errors in transaction portion with badly formatted transaction portion for TCAP sent. | Int32
> tcap-tran-unrecognised-rx | Total number of protocol errors in transaction portion with unrecognized transaction portion for TCAP received. | Int32
> tcap-tran-unrecognised-tx | Total number of protocol errors in transaction portion with unrecognized transaction portion for TCAP sent. | Int32
> tcap-tran-resource-limit-rx | Total number of protocol errors in transaction portion with resource limit message for TCAP received. | Int32
> tcap-tran-resource-limit-tx | Total number of protocol errors in transaction portion with resource limit message for TCAP sent. | Int32
> tcap-comp-unrecognised-rx | Total number of errors in component portion with unrecognized information for TCAP received. | Int32
> tcap-comp-unrecognised-tx | Total number of errors in component portion with unrecognized information for TCAP sent. | Int32
> tcap-comp-incorrect-rx | Total number of errors in component portion with incorrect information for TCAP received. | Int32
> tcap-comp-incorrect-tx | Total number of errors in component portion with incorrect information for TCAP sent. | Int32
> tcap-comp-badformed-rx | Total number of errors in component portion with badly formed information for TCAP received. | Int32
> tcap-comp-badformed-tx | Total number of errors in component portion with badly formed information for TCAP sent. | Int32
> tcap-comp-unrec-linkid-rx | Total number of errors in component portion with unrecognized link id for TCAP received. | Int32
> tcap-comp-unrec-linkid-tx | Total number of errors in component portion with unrecognized link id for TCAP sent. | Int32
> tcap-comp-unrec-invid-res-rx | Total number of errors in component portion with unrecognized invoke id (return result) for TCAP received. | Int32
> tcap-comp-unrec-invid-res-tx | Total number of errors in component portion with unrecognized invoke id (return result) for TCAP sent. | Int32
> tcap-comp-unexp-res-rx | Total number of errors in component portion with unexpected return result for TCAP received. | Int32
> tcap-comp-unexp-res-tx | Total number of errors in component portion with unexpected return result for TCAP sent. | Int32
> tcap-comp-unrec-invid-err-rx | Total number of errors in component portion with unrecognized invoke id (return error) for TCAP received. | Int32
> tcap-comp-unrec-invid-err-tx | Total number of errors in component portion with unrecognized invoke id (return error) for TCAP sent. | Int32
> tcap-comp-unexp-err-rx | Total number of errors in component portion with unexpected return error for TCAP received. | Int32
> tcap-comp-unexp-err-tx | Total number of errors in component portion with unexpected return error for TCAP sent. | Int32
> tcap-user-duplicate-invid-rx | Total number of user generated errors of duplicate invoke id for TCAP received. | Int32
> tcap-user-duplicate-invid-tx | Total number of user generated errors of duplicate invoke id for TCAP sent. | Int32
> tcap-user-unrec-opcode-rx | Total number of user generated errors of unrecognized operation code for TCAP received. | Int32
> tcap-user-unrec-opcode-tx | Total number of user generated errors of unrecognized operation code for TCAP sent. | Int32
> tcap-user-incorr-params-rx | Total number of user generated errors of incorrect invoke parameter for TCAP received. | Int32
> tcap-user-incorr-params-tx | Total number of user generated errors of incorrect invoke parameter for TCAP sent. | Int32
> tcap-user-resourcelimit-rx | Total number of user generated errors of resource limit invoke error for TCAP received. | Int32
> tcap-user-resourcelimit-tx | Total number of user generated errors of resource limit invoke error for TCAP sent. | Int32
> tcap-user-initiate-release-rx | Total number of user generated errors of release initiated invoke error for TCAP received. | Int32
> tcap-user-initiate-release-tx | Total number of user generated errors of release initiated invoke error for TCAP sent. | Int32
> tcap-user-unexp-linked-resp-rx | Total number of user generated errors of unexpected linked response error for TCAP received. | Int32
> tcap-user-unexp-linked-resp-tx | Total number of user generated errors of unexpected linked response error for TCAP sent. | Int32
> tcap-user-unexp-linked-oper-rx | Total number of user generated errors of unexpected linked operation error for TCAP received. | Int32
> tcap-user-unexp-linked-oper-tx | Total number of user generated errors of unexpected linked operation error for TCAP sent. | Int32
> tcap-user-res-incorr-params-rx | Total number of user generated errors of result code with incorrect parameter for TCAP received. | Int32
> tcap-user-res-incorr-params-tx | Total number of user generated errors of result code with incorrect parameter for TCAP sent. | Int32
> tcap-user-res-unrec-errcode-rx | Total number of user generated errors of result code with unrecognized error code for TCAP received. | Int32
> tcap-user-res-unrec-errcode-tx | Total number of user generated errors of result code with unrecognized error code for TCAP sent. | Int32
> tcap-user-res-unexp-errcode-rx | Total number of user generated errors of result code with unexpected error code for TCAP received. | Int32
> tcap-user-res-unexp-errcode-tx | Total number of user generated errors of result code with unexpected error code for TCAP sent. | Int32
> tcap-user-err-incorr-params-rx | Total number of user generated errors of error code with incorrect parameter for TCAP received. | Int32
> tcap-user-err-incorr-params-tx | Total number of user generated errors of error code with incorrect parameter for TCAP sent. | Int32
> mo-sms-in-progress | Total number of mobile originated SMS that are waiting in the SGSN to be delivered. Type: Gauge. | Int32
> mt-sms-in-progress | Total number of mobile terminated (MT) SMS in progress. Type: Gauge. | Int32
> mt-sms-in-queue | Description: New gauge in release 9.0: Total number of mobile terminated SMS in the queue. Triggers: If there is already an MT-SMS transaction in progress, then the gauge increments when any new messages are received and queued. Availability: per MAP service Type: Gauge | Int32
> sms-memory-available-in-progress | Total number of procedures for retrieval of available SMS memory in progress. Type: Gauge. | Int32
> mo-sms-attempted | Total number of mobile originated SMSs attempted. | Int32
> mo-sms-successful | Total number of mobile originated SMSs successful. | Int32
> mt-sms-attempted | Total number of mobile terminated SMSs attempted. | Int32
> mt-sms-successful | Total number of mobile terminated SMSs successful. | Int32
> sms-memory-available-attempted | Total number of procedures for retrieval of available SMS memory attempted. | Int32
> sms-memory-available-successful | Total number of procedures for retrieval of available SMS memory successful. | Int32
> conn-prot-data-tx | Total number of protocol data units sent during connection setup. | Int32
> conn-prot-data-rx | Total number of protocol data units received during connection setup. | Int32
> conn-prot-ack-tx | Total number of Ack messages sent during connection setup. | Int32
> conn-prot-ack-rx | Total number of Ack messages received during connection setup. | Int32
> conn-prot-error-tx | Total number of protocol errors during connection setup in Tx message. | Int32
> conn-prot-error-rx | Total number of protocol errors during connection setup n Rx message. | Int32
> conn-prot-error-nwt-fail-tx | Total number of protocol errors during connection setup due to network failure in Tx message. | Int32
> conn-prot-error-nwt-fail-rx | Total number of protocol errors during connection setup due to network failure in Rx message. | Int32
> conn-prot-error-congestion-tx | Total number of protocol errors during connection setup due to congestion in Tx message. | Int32
> conn-prot-error-congestion-rx | Total number of protocol errors during connection setup due to congestion in Rx message. | Int32
> conn-prot-error-invalid-tid-tx | Total number of protocol errors during connection setup due to invalid transaction id (TID) in Tx message. | Int32
> conn-prot-error-invalid-tid-rx | Total number of protocol errors during connection setup due to invalid transaction id (TID) in Rx message. | Int32
> conn-prot-error-invalid-semantic-tx | Total number of protocol errors during connection setup due to invalid semantics in Tx message. | Int32
> conn-prot-error-invalid-semantic-rx | Total number of protocol errors during connection setup due to invalid semantics in Rx message. | Int32
> conn-prot-error-invalid-mand-info-tx | Total number of protocol errors during connection setup as mandatory information in Tx message is invalid. | Int32
> conn-prot-error-invalid-mand-info-rx | Total number of protocol errors during connection setup as mandatory information in Rx message is invalid. | Int32
> conn-prot-error-invalid-msg-type-tx | Total number of protocol errors during connection setup due to invalid Tx message type. | Int32
> conn-prot-error-invalid-msg-type-rx | Total number of protocol errors during connection setup due to invalid Tx message type. | Int32
> conn-prot-error-invalid-prot-state-tx | Total number of protocol errors during connection setup as protocol state in Tx message is invalid. | Int32
> conn-prot-error-invalid-prot-state-rx | Total number of protocol errors during connection setup as protocol state in Rx message is invalid. | Int32
> conn-prot-error-invalid-ie-tx | Total number of protocol errors during connection setup as information element in Tx message is invalid. | Int32
> conn-prot-error-invalid-ie-rx | Total number of protocol errors during connection setup as information element in Rx message is invalid. | Int32
> conn-prot-error-protocol-error-tx | Total number of protocol errors during connection setup as protocol error in Tx message. | Int32
> conn-prot-error-protocol-error-rx | Total number of protocol errors during connection setup as protocol error in Rx message. | Int32
> conn-prot-error-undefined-cause-tx | Total number of protocol errors during connection setup due to unspecified error in Tx message. | Int32
> conn-prot-error-undefined-cause-rx | Total number of protocol errors during connection setup due to unspecified error in Rx message. | Int32
> conn-prot-data-dropped | Total number of data packets dropped during connection setup. | Int32
> conn-prot-ack-dropped | Total number of Ack message dropped during connection setup. | Int32
> conn-prot-error-dropped | Total number of data packets dropped during connection setup due to error in connection. | Int32
> conn-prot-inval-tid-rcvd | Total number of message dropped during connection setup due to invalid transaction id (TID) received. | Int32
> relay-prot-data-tx | Total number of protocol data units sent during message relay. | Int32
> relay-prot-data-rx | Total number of protocol data units received during message relay. | Int32
> relay-prot-ack-tx | Total number of Ack messages sent during message relay. | Int32
> relay-prot-ack-rx | Total number of Ack messages received during message relay. | Int32
> relay-prot-err-tx | Total number of protocol errors during message relay in Tx message. | Int32
> relay-prot-err-rx | Total number of protocol errors during message relay n Rx message. | Int32
> relay-prot-err-unassigned-num | Total number of protocol errors during message relay due to unassigned protocol number. | Int32
> relay-prot-err-opr-determ-barring | Total number of protocol errors during message relay due to operator determined barring. | Int32
> relay-prot-err-call-barred | Total number of protocol errors during message relay due to call barring. | Int32
> relay-prot-err-reserved | Total number of protocol errors during message relay due to reserved resources. | Int32
> relay-prot-err-sm-transfer-rej | Total number of protocol errors during message relay due to session manager transfer rejection. | Int32
> relay-prot-err-dest-out-of-order | Total number of protocol errors during message relay due to out of order on destination. | Int32
> relay-prot-err-unidentified-subs | Total number of protocol errors during message relay due to unidentified subscriber. | Int32
> relay-prot-err-facility-rej | Total number of protocol errors during message relay due facility rejection. | Int32
> relay-prot-err-unknown-subs | Total number of protocol errors during message relay due to unknown subscriber. | Int32
> relay-prot-err-netwk-out-of-order | Total number of protocol errors during message relay as network in out-of-order. | Int32
> relay-prot-err-temp-fail | Total number of protocol errors during message relay due to temporary failure in network. | Int32
> relay-prot-err-congestion | Total number of protocol errors during message relay due to congestion in network. | Int32
> relay-prot-err-not-subscribed | Total number of protocol errors during message relay as this service is not subscribed by subscriber. | Int32
> relay-prot-err-not-implemented | Total number of protocol errors during message relay as this service is not yet implemented. | Int32
> relay-prot-err-interworking-err | Total number of protocol errors during message relay due to interworking error between two network or technology. | Int32
> relay-prot-err-res-unavail | Total number of protocol errors during message relay as resources are not available. | Int32
> relay-prot-err-mem-capacity-exceed | Total number of protocol errors during message relay as capacity exceeded. | Int32
> relay-prot-err-inval-ref-num-tx | Total number of protocol errors during message relay as invalid reference in Tx message. | Int32
> relay-prot-err-inval-ref-num-rx | Total number of protocol errors during message relay as invalid reference in Rx message. | Int32
> relay-prot-err-inval-semantic-tx | Total number of protocol errors during message relay due to invalid semantics in Tx message. | Int32
> relay-prot-err-inval-semantic-rx | Total number of protocol errors during message relay due to invalid semantics in Rx message. | Int32
> relay-prot-err-inval-mand-info-tx | Total number of protocol errors during message relay as mandatory information in Tx message is invalid. | Int32
> relay-prot-err-inval-mand-info-rx | Total number of protocol errors during message relay as mandatory information in Rx message is invalid. | Int32
> relay-prot-err-inval-msg-type-tx | Total number of protocol errors during message relay due to invalid Tx message type. | Int32
> relay-prot-err-inval-msg-type-rx | Total number of protocol errors during message relay due to invalid Tx message type. | Int32
> relay-prot-err-inval-prot-state-tx | Total number of protocol errors during message relay as protocol state in Tx message is invalid. | Int32
> relay-prot-err-inval-prot-state-rx | Total number of protocol errors during message relay as protocol state in Rx message is invalid. | Int32
> relay-prot-err-inval-ie-tx | Total number of protocol errors during message relay as information element in Tx message is invalid. | Int32
> relay-prot-err-inval-ie-rx | Total number of protocol errors during message relay as the information element in Rx message is invalid. | Int32
> relay-prot-err-protocol-error-rx | Description: New counter in release 9.0: Total number of RP ERROR messages sent with the cause Protocol Error in the message header. Triggers: Counter increments when receiving an RP ERROR, with cause Protocol Error, from the MS/SMSC. Availability: per MAP service Type: Counter | Int32
> relay-prot-err-protocol-error-tx | Total number of protocol errors during message relay when there are protocol errors in the transmitted message. | Int32
> relay-prot-err-unidentified-error-tx | Total number of protocol errors during message relay due to unspecified error in Tx message. | Int32
> relay-prot-err-unidentified-error-rx | Total number of protocol errors during message relay due to unspecified error in Rx message. | Int32
> relay-prot-smma-rx | Description: Counter new in release 9.0: Total number RP SMMA messages received. Triggers: Counter increments when the SGSN receives an RP SMMA message from the MS/UE. Availability: per MAP service Type: Counter | Int32
> relay-prot-data-dropped | Total number of data packets dropped during message relay. | Int32
> relay-prot-ack-dropped | Total number of Ack message dropped during message relay. | Int32
> relay-prot-error-dropped | Total number of data packets dropped during message relay due to error in connection. | Int32
> relay-prot-decode-failure | Total number of message dropped during message relay due to invalid transaction id (TID) received. | Int32
> concat-mo-sms | Total number of concatenated mobile originated SMSs. | Int32
> conn-prot-timer-expiry | Total number of events when timer expired during connection setup. | Int32
> tr1n-timer-expiry | Total number of events when TR1N timer expired during mobile terminated SMS is in wait state for RP-ACK. | Int32
> tr2n-timer-expiry | Total number of events when TR2N timer expired during mobile terminated SMS is in wait state to send RP-ACK. | Int32
> conn-prot-data-retrans | Total number of protocol data units retransmitted during connection setup. | Int32
> relay-prot-msg-encode-fail | Total number of message encoding failed during message relay. | Int32
> conn-prot-data-tx-fail | Total number of protocol data units Tx messages failed during connection setup. | Int32
> conn-prot-data-inval-tid | Total number of protocol data units with invalid transaction id (ID) during connection setup. | Int32
> conn-prot-max-retrans-reached | Total number of events when retransmission limit exhausted during connection setup. | Int32
> mt-fail-no-db-rec | Total number of mobile terminated messages failed as not database record available. | Int32
> mt-fail-conn-prot-data-no-ack-rcvd | Total number of mobile terminated messages failed as no acknowledgement received during connection setup. | Int32
> mt-fail-fwd-busy-subs | Total mobile terminated messages failed due to busy subscriber. | Int32
> mt-fail-fwd-detached-subs | Total mobile terminated messages failed due to detached subscriber. | Int32
> mt-fail-mt-queue-full | Total mobile terminated messages failed as messaged queue was full. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883