> show asngw-service
> This chapter includes the show asngw-service command output tables.
> show asngw-service all
> show asngw-service all Command Output Descriptions

> Field | Description
> Service name | The ASN GW service name.
> Context | The context in which the service is configured.
> Bind | The bind status.
> Max Subscribers | The maximum number of subscribers.
> IP address | IP address of ASN GW server where this service is located.
> UDP Port | The UDP port number.
> Service Status | Status of this service.
> Authentication | The authentication mode. Possible modes are:
> • | None
> • | User (Single EAP)
> • | Device (Single EAP)
> • | Device-User (Double EAP)
> • | Device-User (Single EAP)
> Policy msid-dhcp-chaddr-mismatch | Indicates the status of the policy to handle the calls with mismatched DHCP Client Hardware (MAC) Address (CHADDR) and MSID of the ASN-GW session.
> Policy ms-unexpected-network-reentry | Indicates the status of the policy to handle the unexpected network re-entry of an MS.
> Policy asngw-initiated-reauth | Indicates the status of the policy to handle the ASN GW initiated reauthorization trigger.
> Policy non-anchor-mode | Indicates the status of the policy to handle the ASN GW to accept the session in non-anchor mode.
> Newcall Policy | Specify that the new call policy enabled or disabled to handle new calls. Possible values are:
> • | NONE
> • | REJECT
> Policy Overload | Specify that the session overload policy enabled or disabled to handle new calls. Possible values are:
> • | DROP
> • | REJECT
> Mobile IP FA context | The name of the context where MIP FA service is configured.
> Maximum number of retransmissions | The maximum number of retransmissions.
> Retransmission timeout | The retransmission timeout duration.
> Setup timeout | The session setup timeout duration.
> Active-relay timeout | Indicates the timeout duration for active relay of R4 or R6 messages.
> Handover anchor data-path termination timeout | Indicates the timeout duration in seconds to keep the data path registration with previous anchored BS after completion of handover.
> Handover anchor data-path pre-registration termination timeout | Indicates the timeout duration in seconds to keep the data path pre-registration termination information with anchored BS after completion of handover.
> Handover non-anchor data-path termination timeout | Indicates the timeout duration in seconds to keep the data path registration with non-anchored BS after completion of handover.
> Handover non-anchor data-path pre-registration termination timeout | Indicates the timeout duration in seconds to keep the data path pre-registration termination information with non-anchored BS after completion of handover.
> Handover max number of data-path pre-registrations | Indicates the maximum number of data paths created during pre-registration for a handover.
> Idle-mode entry timeout | Indicates the timeout duration in seconds for a session to enter the idle mode from active mode.
> Idle-mode exit timeout | Indicates the timeout duration in seconds for a session to reenter the active mode from idle mode.
> Idle-mode timeout | Indicates the total timeout duration in seconds.
> Policy transaction-id-validation | Indicates the status of the policy to validate the transaction id.
> Policy zero-function-type | Indicates the status of the policy to allow the zero function type of call.
> Transaction Id. Seed | Indicates the transaction identifier seed.
> Peer ASNGW addresses | Indicates the IP addresses of trusted ASN GW peers for handover.
> BS Monitor Config | Indicates the status of BS monitoring support. Possible values are:
> • | Enabled
> • | Disabled
> Interval | Indicates the configured amount of time in seconds between two ICMP ping message to an ASN BS.
> Timeout | Indicates the number of seconds to wait for response from the ASN BS before re-sending the ICMP ping message.
> Number of retries | Indicates the number of retries to sent ICMP ping messages to an ASN BS before the ASN BS is declared as dead/unreachable.
> MTU size | Indicates the maximum transmission unit size configured in bytes.
> Total BSs | Indicates the total number of BSs monitored.
> Active BSs | Indicates number of active BSs.
> Alive BSs | Indicates number of active and alive BSs.
> ICMP Monitored BSs | Indicates the number of BSs which are monitored through ICMP ping messages.
> Inactive BSs | Indicates number of inactive BSs.
> No Calls BSs | Indicates the total number of BSs which have no active calls or in idle mode.
> Going Down BSs | Indicates the total number of BSs which are going down or terminating sessions.
> BS | Indicates the IP address of BSs.
> Status | Indicates the status of listed BSs.
> Maximum Number of Secondary IP Hosts | Indicates the maximum number of secondary hosts connected behind a primary WiMAX CPE under multiple IP host support.
> Ran Peer Map Name | The name of the RAN Peer Map this service is using to reconcile base station MAC address received in R6 protocol messages to the actual IPv4 address of the base station.

> ‌
> show asngw-service session all
> show asngw-service session all Command Output Descriptions

> Field | Description
> vv | Displays service and session state information. This column provides a code consisting of two characters. From left-to-right, the first character represents the Call Type that the subscriber is using. The possible call types are:
> • | A: Anchor
> • | N: Non-Anchor
> From left-to-right, the second character represents the DP Status. The possible data path status are:
> • | A: Active
> • | I: Idle
> CALLID | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> NAI | The subscriber’s Network Access Identifier.
> Home Address | The IP address assigned to the subscriber’s mobile node for the duration of the session.
> Total Non-Anchor ASNGW Sessions | The total number of ASN GW sessions in non-anchor mode.
> Total Anchor ASNGW Sessions | The total number of ASN GW sessions in anchor mode.
> Total Active ASNGW Sessions | The total number of active ASN GW sessions including anchor and non-anchor mode.
> Total Idle ASNGW Sessions | The total number of idle ASN GW sessions including anchor and non-anchor mode.
> Total ASNGW Sessions | The total number of ASN GW sessions on chassis including all modes.

> ‌
> show asngw-service session counters
> show asngw-service session counters Command Output Descriptions

> Field | Description
> Username | The subscriber’s user name.
> Callid | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> Session Type | Indicates the type of session. Possible type of sessions are:
> • | Anchor
> • | Non-Anchor
> Initial Network Entry Events
> MS Pre-Attach | Displays the MS pre-attach event statistics.
> Attempted | Indicates the total number of attempts made for an event.
> Success | Indicates the total number of successful attempts made for an event.
> Failures | Indicates the total number of failed attempts made for an event.
> Authentications | Displays the authentication event statistics.
> EAP | Indicates the total number of authentication/re-authentication attempts failed due to EAP.
> Misc. Reason | Indicates the total number of authentication/re-authentication attempts failed due to miscellaneous reasons.
> MS Attach | Displays the MS attach event statistics.
> DP Registrations | Displays the data path registration event statistics.
> Re-Authentications | Displays the re-authentication event statistics.
> Handover Events
> Intra ASN-GW Handovers | Displays the intra-ASN GW (inter BS) handover event statistics.
> Inter ASN-GW Handovers | Displays the inter-ASN GW handover event statistics.
> DP De-Registrations | Displays the data path de-registration event statistics.
> Idle Mode entry events | Displays the idle mode entry event statistics.
> Idle Mode exit events | Displays the idle mode exit event statistics.
> Paging initiation events | Displays the paging initiation event statistics.
> Total R6/R4 Control Messages | Displays the statistics of total R4 and R6 control messages.
> Sent | Total number of R4/R6 control messages sent.
> Retransmissions Sent | Total number of R4/R6 control messages retransmitted.
> Received | The total number of R4/R6 control messages received.
> Accepted | The total number of R4/R6 control messages received and accepted.
> Relayed | The total number of R4/R6 control messages received and relayed.
> Denied | The total number of R4/R6 control messages received and denied.
> Discarded | The total number of R4/R6 control messages received and discarded.
> Badly Formed | The total number of badly formed R4/R6 control messages messages.
> Decode Error | The total number of decode errors found in the R4/R6 control messages.
> Unspecified Error | The total number of unspecified errors found in the R4/R6 control messages.
> Missing Mandatory TLV | The total number of R4/R6 control messages received with missing mandatory TLVs.
> TLV Value Invalid | The total number of R4/R6 control messages received with invalid TLV value.
> Unknown TLV | The total number of R4/R6 control messages received with unknown TLV value.
> Duplicate TLV Found | The total number of R4/R6 control messages received with duplicate TLV value.
> No Session Found | The total number of R4/R6 control messages received without session information.
> Transaction Id. Error | The total number of R4/R6 control messages received with error in transaction id.
> Key Change Success | The total number of R4/R6 control messages received with successful Key Change request.
> Key Change Failure | The total number of R4/R6 control messages with failed Key Change request.
> MS Initiated Re-Auth | The total number of R4/R6 control messages received with for MS initiated re-authentication.
> BS Initiated Re-Auth | The total number of R4/R6 control messages received with for BS initiated re-authentication.
> Total R4/R6 Data messages: | Displays the statistics of total R4 and R6 data messages.
> GRE Receive:
> Packets Received | The total number of packets received by the system through GRE tunnel.
> Bytes Received | The total number of bytes received by the system through GRE tunnel.
> Protocol Type Error | The total number of encapsulated packets received through GRE tunnel with protocol type errors.
> GRE Key Absent | Total number of GRE tunneled key absent errors received through GRE tunnel.
> GRE Checksum Error | Total number of checksum errors that occurred in GRE tunnels received by this system.
> Invalid Packet Length | Total number of encapsulated packets received with invalid packet lengths through GRE tunnel.
> No Session found | Total number of errors that occurred due to no session being present in received tunnels.
> Unspecified Error | Total number of data messages received with errors which are not specified in this table.
> GRE Send:
> Packets Sent | The total number of packets sent by the system through GRE tunnel.
> Bytes Sent | The total number of bytes sent by the system through GRE tunnel.
> Send Error | The total number of errors that occurred while sending replies through GRE tunnel.
> Unspecified Error | Total number of data messages sent with errors which are not specified in this table through GRE tunnel.
> Total Non-Anchor ASNGW Sessions | The total number of ASN GW sessions in non-anchor mode.
> Total Anchor ASNGW Sessions | The total number of ASN GW sessions in anchor mode.
> Total ASNGW Sessions | The total number of ASN GW sessions including anchor and non-anchor mode.

> ‌
> show asngw-service session counters verbose
> show asngw-service session counters verbose Command Output Descriptions

> Field | Description
> Username | The subscriber’s user name.
> Callid | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> Session Type | Indicates the type of session. Possible type of sessions are:
> • | Anchor
> • | Non-Anchor
> Message Groups
> R6 MS Pre-Attachment Request messages | Groups the statistics of the MS pre-attachment request messages on R6 interface.
> R6 MS Pre-Attachment Response messages | Groups the statistics of the MS pre-attachment response messages on R6 interface.
> R6 MS Pre-Attachment Ack messages | Groups the statistics of the MS pre-attachment ACK messages on R6 interface.
> R6 Network Exit MS State Change Request messages | Groups the statistics of the MS state change request messages on network exit R6 interface.
> R4 Network Exit MS State Change Request messages | Groups the statistics of the MS state change request messages on network exit R4 interface.
> R6 Network Exit MS State Change Response messages | Groups the statistics of the MS state change response messages on network exit R6 interface.
> R4 Network Exit MS State Change Response messages | Groups the statistics of the MS state change response messages on network exit R4 interface.
> R6 Context Request messages | Groups the statistics of the context request messages on R6 interface.
> R4 Context Request messages | Groups the statistics of the context request messages on R4 interface.
> R6 Context Report messages | Groups the statistics of the context report messages on R6 interface.
> R4 Context Report messages | Groups the statistics of the context report messages on R4 interface.
> R6 Context Ack messages | Groups the statistics of the context ACK messages on R6 interface.
> R4 Context Ack messages | Groups the statistics of the context ACK messages on R4 interface.
> R6 Authentication Relay EAP Transfer messages | Groups the statistics of the EAP authentication relay transfer messages on R6 interface.
> R4 Authentication Relay EAP Transfer messages | Groups the statistics of the EAP authentication relay transfer messages on R4 interface.
> R6 Authentication Relay EAP Start messages | Groups the statistics of the EAP authentication relay start messages on R6 interface.
> R4 Authentication Relay EAP Start messages | Groups the statistics of the EAP authentication relay start messages on R4 interface.
> R6 MS Attachment Request messages | Groups the statistics of the MS attachment request messages on R6 interface.
> R6 MS Attachment Response messages | Groups the statistics of the MS attachment response messages on R6 interface.
> R6 MS Attachment Ack messages | Groups the statistics of the MS attachment ACK messages on R6 interface.
> R6 Data-Path Pre-Registration Request messages | Groups the statistics of the data path pre-registration request messages on R6 interface.
> R4 Data-Path Pre-Registration Request messages | Groups the statistics of the data path pre-registration request messages on R4 interface.
> R6 Data-Path Pre-Registration Response messages | Groups the statistics of the data path pre-registration response messages on R6 interface.
> R4 Data-Path Pre-Registration Response messages | Groups the statistics of the data path pre-registration response messages on R4 interface.
> R6 Data-Path Pre-Registration Ack messages | Groups the statistics of the data path pre-registration ACK messages on R6 interface.
> R4 Data-Path Pre-Registration Ack messages | Groups the statistics of the data path pre-registration ACK messages on R4 interface.
> R6 Data-Path Registration Request messages | Groups the statistics of the data path registration request messages on R6 interface.
> R4 Data-Path Registration Request messages | Groups the statistics of the data path registration request messages on R4 interface.
> R6 Data-Path Registration Response messages | Groups the statistics of the data path registration response messages on R6 interface.
> R4 Data-Path Registration Response messages | Groups the statistics of the data path registration response messages on R4 interface.
> R6 Data-Path Registration Ack messages | Groups the statistics of the data path registration ACK messages on R6 interface.
> R4 Data-Path Registration Ack messages | Groups the statistics of the data path registration ACK messages on R4 interface.
> R6 Data-Path De-Registration Request messages | Groups the statistics of the data path de-registration request messages on R6 interface.
> R4 Data-Path De-Registration Request messages | Groups the statistics of the data path de-registration request messages on R4 interface.
> R6 Data-Path De-Registration Response messages | Groups the statistics of the data path de-registration response messages on R6 interface.
> R4 Data-Path De-Registration Response messages | Groups the statistics of the data path de-registration response messages on R4 interface.
> R6 Data-Path De-Registration Ack messages | Groups the statistics of the data path de-registration ACK messages on R6 interface.
> R4 Data-Path De-Registration Ack messages | Groups the statistics of the data path de-registration ACK messages on R4 interface.
> R6 Key Change Directive messages | Groups the statistics of the key change directive messages on R6 interface.
> R4 Key Change Directive messages | Groups the statistics of the key change directive messages on R4 interface.
> R6 Key Change Ack messages | Groups the statistics of the key change ACK messages on R6 interface.
> R4 Key Change Ack messages | Groups the statistics of the key change ACK messages on R4 interface.
> R6 Key Change Confirm messages | Groups the statistics of the key change confirm messages on R6 interface.
> R4 Key Change Confirm messages | Groups the statistics of the key change confirm messages on R4 interface.
> R6 Cmac Key Count Update Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count update messages on R6 interface.
> R4 Cmac Key Count Update Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count update messages on R4 interface.
> R6 Cmac Key Count Ack Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count ACK messages on R6 interface.
> R4 Cmac Key Count Ack Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count ACK messages on R46 interface.
> R6 Handoff Request Msg | Groups the statistics of the hand-off request messages on R6 interface.
> R4 Handoff Request Msg | Groups the statistics of the hand-off request messages on R4 interface.
> R6 Handoff Response Msg | Groups the statistics of the hand-off response messages on R6 interface.
> R4 Handoff Response Msg | Groups the statistics of the hand-off response messages on R4 interface.
> R6 Handoff Ack Msg | Groups the statistics of the hand-off ACK messages on R6 interface.
> R4 Handoff Ack Msg | Groups the statistics of the hand-off ACK messages on R4 interface.
> R6 Handoff Confirm Msg | Groups the statistics of the hand-off confirm messages on R6 interface.
> R4 Handoff Confirm Msg | Groups the statistics of the hand-off confirm messages on R4 interface.
> R6 Handoff Complete Msg | Groups the statistics of the hand-off complete messages on R6 interface.
> R4 Handoff Complete Msg | Groups the statistics of the hand-off complete messages on R4 interface.
> R4 IM Entry State Change Req Msg | Groups the statistics of the idle mode entry state change request messages on R4 interface.
> R4 IM Entry State Change Rsp Msg | Groups the statistics of the idle mode entry state change response messages on R4 interface.
> R4 IM Entry State Change Ack Msg | Groups the statistics of the idle mode entry state change ACK messages on R4 interface.
> R4 Anchor PC Indication Msg | Groups the statistics of anchor paging controller (PC) indication messages on R4 interface.
> R4 Anchor PC Ack Msg | Groups the statistics of anchor paging controller (PC) ACK messages on R4 interface.
> R4 IM Exit State Change Req Msg | Groups the statistics of the idle mode exit state change request messages on R4 interface.
> R4 IM Exit State Change Rsp Msg | Groups the statistics of the idle mode exit state change response messages on R4 interface.
> R4 Initiate Paging Req Msg | Groups the statistics of the initiated paging request messages on R4 interface.
> R4 Initiate Paging Rsp Msg | Groups the statistics of the initiated paging response messages on R4 interface.
> R4 Delete MS Entry Req Msg | Groups the statistics of the request messages to delete the MS entry request on R4 interface.
> R4 Delete MS Entry Rsp Msg | Groups the statistics of the messages sent in response of delete message for the MS entry request on R4 interface.
> R6 Unknown messages | Groups the statistics of the unknown type of request messages on R6 interface.
> R4 Unknown messages | Groups the statistics of the unknown type of request messages on R4 interface.
> Message Statistics
> Total Sent | The total number of this type of message sent on specific interface.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Retransmissions Sent | The total number of this type of message re-transmitted on specific interface.
> Total Received | The total number of this type of message received on specific interface.
> Total Accepted | The total number of this type of message accepted on specific interface.
> Total Relayed | The total number of this type of message relayed on specific interface.
> Total Denied | The total number of this type of message denied on specific interface.
> Total Discarded | The total number of this type of message discarded on specific interface.
> Badly Formed | The total number of badly formed this type of message on specific interface.
> Decode Error | The total number of this type of message on specific interface with decode error.
> Unspecified Error | The total number of this type of message on specific interface with unspecified error.
> Missing Mandatory TLV | The total number of this type of message on specific interface with missing mandatory TLVs.
> TLV Value Invalid | The total number of this type of message on specific interface with invalid TLV value.
> Unknown TLV | The total number of this type of message on specific interface with unknown TLVs.
> Duplicate TLV Found | The total number of this type of message on specific interface with duplicate TLVs.
> No session Found | The total number of this type of message on specific interface without any session information.
> Transaction Id. Error | The total number of this type of message on specific interface. with transaction id error.
> Key Change Success | The total number of successful Key Change Confirmation messages.
> Key Change Failure | The total number of Key Change Confirmation messages failed.
> Out Of Order Packet | The total number of authentication relay EAP transfer/start messages on R6 interface with out-of-order packets.
> MS Initiated Re-Auth | The total number of authentication relay EAP start messages on specific interface with MS initiated reauthorization.
> BS Initiated Re-Auth | The total number of authentication relay EAP start messages on specific interface with BS initiated reauthorization.
> ASNGW Initiated Re-Auth | Total number of the re-authentications initiated from the ASN GW.
> Data messages
> GRE R6 Receive | The total number of data message received with through GRE tunnel on R6 interface.
> GRE R4 Receive | The total number of data message received through GRE tunnel on R4 interface.
> Packets Received | The total number of data packets received/sent through GRE tunnel on R4/R6 interface.
> Bytes Received | The total number of data bytes received/sent through GRE tunnel on R4/R6 interface.
> Protocol Type Error | The total number of data message received/sent with protocol type error through GRE tunnel on R4/R6 interface.
> GRE Key Absent | The total number of data message received/sent without GRE key through GRE tunnel on R4/R6 interface.
> GRE Checksum Error | The total number of data message received/sent with checksum error through GRE tunnel on R4/R6 interface.
> Invalid Packet Length | The total number of data message received/sent with invalid packet length through GRE tunnel on R4/R6 interface.
> No Session found | The total number of data message received/sent without any session information through GRE tunnel on R4/R6 interface.
> Unspecified Error | The total number of data message received/sent with unknown error through GRE tunnel on R4/R6 interface.
> GRE R6 Send | The total number of data message sent through GRE tunnel on R6 interface.
> GRE R4 Send | The total number of data message sent through GRE tunnel on R4 interface.
> Packets Sent | The total number of data packets sent through GRE tunnel on R4/R6 interface.
> Send Error | The total number of data message sent with error through GRE tunnel on R4/R6 interface.
> Bytes Sent | The total number of data bytes sent through GRE tunnel on R4/R6 interface.

> ‌
> show asngw-service session full
> show asngw-service session full Command Output Descriptions

> Field | Description
> Username | The subscriber’s user name.
> Callid | The subscriber’s call identification number.
> Pseudoname | The subscriber’s pseudo name. It provides the pseudo user name for a WIMAX session if TTLS authentication is used for the call.
> MSID | The subscriber’s Mobile Station Identification number.
> Home Address | The IP address assigned to the subscriber’s mobile node for the duration of the session.
> ASNGW Service Address | IP address of system where ASN GW service is running.
> Session Type | Indicates the type of session. Possible type of sessions are:
> • | Anchor
> • | Non-Anchor
> DP Status | Indicates the status of data path. Possible data path status are:
> • | Active
> • | Idle
> Authenticator Address | IP address of the authenticator ASN GW.
> Anchor Address | IP address of the anchor ASN GW where subscriber is attached.
> Data Path Status | Identifies if the call can carry data over the R6/R4 interface. Idle: the ASN GW is attached to PCLR and is not capable of sending traffic to BS over R6/R4. Active: the IP-GRE tunnels between the ASN GW and the BS are setup and ready to transfer data from the IP network side.
> PCLR Address | IP address of PC-LR currently attached to this ASN GW.
> CMAC Key Count | Total number of Cipher-based Message Authentication Code (CMAC) key count.
> EAP MSK Lifetime | Total lifetime configured for EAP Master Session Key in seconds.
> Remaining MSK Lifetime | Remaining lifetime available for EAP Master Session Key in seconds.
> Number of Re-authentication | Total number of re-authentications happened for a WiMAX subscriber.
> Authentication Mode | The authentication mode. Possible modes are:
> • | None
> • | User (Single EAP)
> • | Device (Single EAP)
> • | Device-User (Double EAP)
> • | Device-User (Single EAP)
> EAP-Methods | Specifies the EAP authentication method. Possible methods are:
> • | EAP-Pre-shared Key (EAP-PSK)
> • | EAP-Transport Layer Security (EAP-TLS)
> • | EAP-Tunneled Transport Layer Security (EAP-TTLS)
> • | EAP-Authentication and Key Agreement (EAP-AKA)
> DHCP ChAddr of MS | Client Hardware (MAC) Address (CHADDR) of MS.
> Service Flow Information
> SFID | The service flow identifier.
> Direction | Direction of the service flow.
> SDFID | The service data flow identifier.
> PDFID | The packet data flow identifier.
> Profile ID | The profile id applicable for service flow.
> Peer (*) Address | Specifies the IP address of the trusted peer for handover.
> Peer Type | Specifies the type of peer for handover. Possible types are:
> • | BS
> • | ASN GW
> BSID | Specifies the ASN base station Id.
> GRE Key | The Generic Routing Encapsulation (GRE) key.
> Tunnel Endpoint | Indicates the IP address of GRE tunnel endpoint.
> Total Service flows(unidirectional) | Total number of service flows in both direction.
> Total Non-Anchor ASNGW Sessions | The total number of ASN GW sessions in non-anchor mode.
> Total Anchor ASNGW Sessions | The total number of ASN GW sessions in anchor mode.
> Total Active ASNGW Sessions | The total number of active ASN GW sessions.
> Total Idle ASNGW Sessions | The total number of ASN GW sessions in idle mode.
> Total ASNGW Sessions | The total number of ASN GW sessions including anchor and non-anchor mode.

> ‌
> show asngw-service session counters function-type data-path
> show asngw-service session counters function-type data-path Command Output Descriptions

> Field | Description
> Username | The subscriber’s user name.
> CALLID | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> Data-Path Registration Request Messages:
> Total Sent | The total number of Data-Path Registration Request messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Data-Path Registration Request messages received.
> Total Denied | The total number of Data-Path Registration Request messages denied.
> Total Discarded | The total number of Data-Path Registration Request messages discarded.
> Badly Formed | The total number of badly formed Data-Path Registration Request messages.
> Decode Error | The total number of decode errors in the Data-Path Registration Request messages sent.
> Unspecified Error | The total number of unspecified errors in the Data-Path Registration Request messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Data-Path Registration Request messages sent.
> TLV Value Invalid | The total number of Data-Path Registration Request messages sent with invalid TLV value.
> Unknown TLV | The total number of Data-Path Registration Request messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Data-Path Registration Request messages sent with duplicate TLV.
> No Session Found | The total number of Data-Path Registration Request messages sent without session information.
> Data-Path Registration Response Messages:
> Total Sent | The total number of Data-Path Registration Response messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Data-Path Registration Response messages received.
> Total Denied | The total number of Data-Path Registration Response messages denied.
> Total Discarded | The total number of Data-Path Registration Response messages discarded.
> Badly Formed | The total number of badly formed Data-Path Registration Response messages.
> Decode Error | The total number of decode errors in the Data-Path Registration Response messages sent.
> Unspecified Error | The total number of unspecified errors in the Data-Path Registration Response messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Data-Path Registration Response messages sent.
> TLV Value Invalid | The total number of Data-Path Registration Response messages sent with invalid TLV value.
> Unknown TLV | The total number of Data-Path Registration Response messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Data-Path Registration Response messages sent with duplicate TLV.
> No Session Found | The total number of Data-Path Registration Response messages sent without session information.
> Data-Path Registration Ack Messages:
> Total Sent | The total number of Data-Path Registration Request Ack messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Data-Path Registration Request Ack messages received.
> Total Denied | The total number of Data-Path Registration Request Ack messages denied.
> Total Discarded | The total number of Data-Path Registration Request Ack messages discarded.
> Badly Formed | The total number of badly formed Data-Path Registration Request Ack messages.
> Decode Error | The total number of decode errors in the Data-Path Registration Request Ack messages sent.
> Unspecified Error | The total number of unspecified errors in the Data-Path Registration Request Ack messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Data-Path Registration Request Ack messages sent.
> TLV Value Invalid | The total number of Data-Path Registration Request Ack messages sent with invalid TLV value.
> Unknown TLV | The total number of Data-Path Registration Request Ack messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Data-Path Registration Request Ack messages sent with duplicate TLV.
> No Session Found | The total number of Data-Path Registration Request Ack messages sent without session found.
> Data-Path De-Registration Request Messages:
> Total Sent | The total number of Data-Path De-Registration Request messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Data-Path De-Registration Request messages received.
> Total Denied | The total number of Data-Path De-Registration Request messages denied.
> Total Discarded | The total number of Data-Path De-Registration Request messages discarded.
> Badly Formed | The total number of badly formed Data-Path De-Registration Request messages.
> Decode Error | The total number of decode errors in the Data-Path De-Registration Request messages sent.
> Unspecified Error | The total number of unspecified errors in the Data-Path De-Registration Request messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Data-Path De-Registration Request messages sent.
> TLV Value Invalid | The total number of Data-Path De-Registration Request messages sent with invalid TLV value.
> Unknown TLV | The total number of Data-Path De-Registration Request messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Data-Path De-Registration Request messages sent with duplicate TLV.
> No Session Found | The total number of Data-Path De-Registration Request messages sent without session information.
> Data-Path De-Registration Response Messages:
> Total Sent | The total number of Data-Path De-Registration Response messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Data-Path De-Registration Response messages received.
> Total Denied | The total number of Data-Path De-Registration Response messages denied.
> Total Discarded | The total number of Data-Path De-Registration Response messages discarded.
> Badly Formed | The total number of badly formed Data-Path De-Registration Response messages.
> Decode Error | The total number of decode errors in the Data-Path De-Registration Response messages sent.
> Unspecified Error | The total number of unspecified errors in the Data-Path De-Registration Response messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Data-Path De-Registration Response messages sent.
> TLV Value Invalid | The total number of Data-Path De-Registration Response messages sent with invalid TLV value.
> Unknown TLV | The total number of Data-Path De-Registration Response messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Data-Path De-Registration Response messages sent with duplicate TLV.
> No Session Found | The total number of Data-Path De-Registration Response messages sent without session information.
> Total ASNGW Sessions | The total number of ASNGW messages.

> ‌
> show asngw-service session peer-address
> show asngw-service session peer-address Command Output Descriptions

> Field | Description
> vv | Displays service and session state information. This column provides a code consisting of two characters. From left-to-right, the first character represents the Call Type that the subscriber is using. The possible call types are:
> • | A: Anchor
> • | N: Non-Anchor
> From left-to-right, the second character represents the DP Status. The possible data path status are:
> • | A: Active
> • | I: Idle
> CALLID | The subscriber’s call identification number.
> MSID | The subscriber’s Mobile Station Identification number.
> NAI | The subscriber’s Network Access Identifier.
> Home Address | The IP address assigned to the subscriber’s mobile node for the duration of the session.
> Total Non-Anchor ASNGW Sessions | The total number of ASN GW sessions in non-anchor mode.
> Total Anchor ASNGW Sessions | The total number of ASN GW sessions in anchor mode.
> Total Active ASNGW Sessions | The total number of active ASN GW sessions including anchor and non-anchor mode.
> Total Idle ASNGW Sessions | The total number of idle ASN GW sessions including anchor and non-anchor mode.
> Total ASNGW Sessions | The total number of ASN GW sessions on chassis including all modes.

> ‌
> show asngw-service session summary
> show asngw-service session summary Command Output Descriptions

> Field | Description
> Total Non-Anchor ASNGW Sessions | The total number of ASN GW sessions in non-anchor mode.
> Total Anchor ASNGW Sessions | The total number of ASN GW sessions in anchor mode.
> Total Active ASNGW Sessions | The total number of active ASN GW sessions including anchor and non-anchor mode.
> Total Idle ASNGW Sessions | The total number of idle ASN GW sessions including anchor and non-anchor mode.
> Total ASNGW Sessions | The total number of ASN GW sessions on chassis including all modes.

> ‌
> show asngw-service statistics
> show asngw-service statistics Command Output Descriptions

> Field | Description
> Initial Network Entry Events
> MS Pre-Attach | Displays the MS pre-attach event statistics.
> Attempted | Indicates the total number of attempts made for an event.
> Success | Indicates the total number of successful attempts made for an event.
> Failures | Indicates the total number of failed attempts made for an event.
> Authentications | Displays the authentication event statistics.
> EAP | Indicates the total number of authentication/re-authentication attempts failed due to EAP.
> Misc. Reason | Indicates the total number of authentication/re-authentication attempts failed due to miscellaneous reasons.
> MS Attach | Displays the MS attach event statistics.
> Re-Authentications | Displays the re-authentication event statistics.
> Handover Events
> Intra ASN-GW Handovers | Displays the intra-ASN GW (inter BS) handover event statistics.
> Inter ASN-GW Handovers | Displays the inter-ASN GW handover event statistics.
> DP Pre-registration | Displays the data path pre-registration event statistics.
> DP Registration | Displays the data path registration event statistics.
> DP De-Registration | Displays the data path de-registration event statistics.
> Idle Mode entry events | Displays the idle mode entry event statistics.
> Idle Mode exit events | Displays the idle mode exit event statistics.
> Paging initiation events | Displays the paging initiation event statistics.
> Total Disconnects | Displays the reason statistics for the disconnection of session.
> MSK Lifetime Expiry | Indicates the total number of disconnects due to Master Session Key lifetime expiry.
> Auth Failures | Indicates the total number of disconnects due to authentication failure.
> Admin Drops | Indicates the total number of disconnects due to administrator intervention.
> De-registrations | Indicates the total number of disconnects due to de-registration request initiation.
> Other Reasons | Indicates the total number of disconnects due to unspecified reasons.
> Total R6/R4 Control Messages | Displays the statistics of total R4 and R6 control messages.
> Sent | Total number of R4/R6 control messages sent.
> Retransmissions Sent | Total number of R4/R6 control messages retransmitted.
> Received | Total number of R4/R6 control messages received.
> Accepted | Total number of R4/R6 control messages received and accepted.
> Relayed | Total number of R4/R6 control messages received and relayed.
> Denied | Total number of R4/R6 control messages received and denied.
> Discarded | Total number of R4/R6 control messages received and discarded.
> Badly Formed | Total number of badly formed R4/R6 control messages.
> Decode Error | Total number of decode errors found in the R4/R6 control messages.
> Unspecified Error | Total number of unspecified errors found in the R4/R6 control messages.
> Missing Mandatory TLV | Total number of R4/R6 control messages received with missing mandatory TLVs.
> TLV Value Invalid | Total number of R4/R6 control messages received with invalid TLV value.
> Unknown TLV | Total number of R4/R6 control messages received with unknown TLV value.
> Duplicate TLV Found | Total number of R4/R6 control messages received with duplicate TLV value.
> No Session Found | Total number of R4/R6 control messages received without session information.
> Transaction Id. Error | Total number of R4/R6 control messages received with error in transaction id.
> Key Change Success | Total number of R4/R6 control messages received with successful Key Change request.
> Key Change Failures | Total number of R4/R6 control messages with failed Key Change request.
> MS Initiated Re-Auth | Total number of R4/R6 control messages received with for MS initiated re-authentication.
> BS Initiated Re-Auth | Total number of R4/R6 control messages received with for BS initiated re-authentication.
> ASNGW Initiated Re-Auth | Total number of the re-authentications initiated from the ASN GW.
> Total R4/R6 Data messages: | Displays the statistics of total R4 and R6 data messages.
> GRE Receive:
> Total Packets Received | Total number of packets received by the system through GRE tunnel.
> Total Bytes Received | Total number of bytes received by the system through GRE tunnel.
> Protocol Type Error | Total number of encapsulated packets received through GRE tunnel with protocol type errors.
> GRE Key Absent | Total number of GRE tunneled key absent errors received through GRE tunnel.
> GRE Checksum Error | Total number of checksum errors that occurred in GRE tunnels received by this system.
> Invalid Packet Length | Total number of encapsulated packets received with invalid packet lengths through GRE tunnel.
> No Session found | Total number of errors that occurred due to no session being present in received tunnels.
> Unspecified Error | Total number of data messages received with errors which are not specified in this table.
> GRE Send:
> Total Packets Sent | Total number of packets sent by the system through GRE tunnel.
> Total Bytes Sent | Total number of bytes sent by the system through GRE tunnel.
> Send Error | Total number of errors that occurred while sending replies through GRE tunnel.
> Unspecified Error | Total number of data messages sent with errors which are not specified in this table through GRE tunnel.
> Total Sessions Connected | Historical count of the total number of ASNGW sessions setup on a per-service and a per-chassis basis.

> ‌
> show asngw-service statistics function-type ms-state-change
> show asngw-service statistics function-type ms-state-change Command Output Descriptions

> Field | Description
> Network Entry MS State Change Request Messages:
> Total Sent | The total number of Network Entry MS State Change Request messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Network Entry MS State Change Request messages received.
> Total Denied | The total number of Network Entry MS State Change Request messages denied.
> Total Discarded | The total number of Network Entry MS State Change Request messages discarded.
> Badly Formed | The total number of badly formed Network Entry MS State Change Request messages.
> Decode Error | The total number of decode errors in the Network Entry MS State Change Request messages sent.
> Unspecified Error | The total number of unspecified errors in the Network Entry MS State Change Request messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Network Entry MS State Change Request messages sent.
> TLV Value Invalid | The total number of Network Entry MS State Change Request messages sent with invalid TLV value.
> Unknown TLV | The total number of Network Entry MS State Change Request messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Network Entry MS State Change Request messages sent with duplicate TLV.
> No Session Found | The total number of Network Entry MS State Change Request messages sent without session information.
> Network Entry MS State Change Response Messages:
> Sent | The total number of Network Entry MS State Change Response messages sent.
> Total Received | The total number of Network Entry MS State Change Response messages received.
> Total Denied | The total number of Network Entry MS State Change Response messages denied.
> Total Discarded | The total number of Network Entry MS State Change Response messages discarded.
> Badly Formed | The total number of badly formed Network Entry MS State Change Response messages.
> Decode Error | The total number of decode errors in the Network Entry MS State Change Response messages sent.
> Unspecified Error | The total number of unspecified errors in the Network Entry MS State Change Response messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Network Entry MS State Change Response messages sent.
> TLV Value Invalid | The total number of Network Entry MS State Change Response messages sent with invalid TLV value.
> Unknown TLV | The total number of Network Entry MS State Change Response messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Network Entry MS State Change Response messages sent with duplicate TLV.
> No Session Found | The total number of Network Entry MS State Change Response messages sent without session information.
> Network Entry MS State Change Directive Messages:
> Total Sent | The total number of Network Entry MS State Change Directive messages sent.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Total Received | The total number of Network Entry MS State Change Directive messages received.
> Total Denied | The total number of Network Entry MS State Change Directive messages denied.
> Total Discarded | The total number of Network Entry MS State Change Directive messages discarded.
> Badly Formed | The total number of badly formed Network Entry MS State Change Directive messages.
> Decode Error | The total number of decode errors in the Network Entry MS State Change Directive messages sent.
> Unspecified Error | The total number of unspecified errors in the Network Entry MS State Change Directive messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Network Entry MS State Change Directive messages sent.
> TLV Value Invalid | The total number of Network Entry MS State Change Directive messages sent with invalid TLV value.
> Unknown TLV | The total number of Network Entry MS State Change Directive messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Network Entry MS State Change Directive messages sent with duplicate TLV.
> No Session Found | The total number of Network Entry MS State Change Directive Request messages sent without session information.
> Network Entry MS State Change Ack Messages:
> Total Sent | The total number of Network Entry MS State Change Ack messages sent.
> Total Received | The total number of Network Entry MS State Change Ack messages received.
> Total Denied | The total number of Network Entry MS State Change Ack messages denied.
> Total Discarded | The total number of Network Entry MS State Change Ack messages discarded.
> Badly Formed | The total number of badly formed Network Entry MS State Change Ack messages.
> Decode Error | The total number of decode errors in the Network Entry MS State Change Ack messages sent.
> Unspecified Error | The total number of unspecified errors in the Network Entry MS State Change Ack messages sent.
> Missing Mandatory TLV | The total number of missing mandatory TLVs in the Network Entry MS State Change Ack messages sent.
> TLV Value Invalid | The total number of Network Entry MS State Change Ack messages sent with invalid TLV value.
> Unknown TLV | The total number of Network Entry MS State Change Ack messages sent with unknown TLV.
> Duplicate TLV Found | The total number of Network Entry MS State Change Ack messages sent with duplicate TLV.
> No Session Found | The total number of Network Entry MS State Change Ack messages sent without session information.

> ‌
> show asngw-service statistics verbose
> show asngw-service statistics verbose Command Output Descriptions

> Field | Description
> Message Groups
> R6 MS Pre-Attachment Request messages | Groups the statistics of the MS pre-attachment request messages on R6 interface.
> R6 MS Pre-Attachment Response messages | Groups the statistics of the MS pre-attachment response messages on R6 interface.
> R6 MS Pre-Attachment Ack messages | Groups the statistics of the MS pre-attachment ACK messages on R6 interface.
> R6 Network Exit MS State Change Request messages | Groups the statistics of the MS state change request messages on network exit R6 interface.
> R4 Network Exit MS State Change Request messages | Groups the statistics of the MS state change request messages on network exit R4 interface.
> R6 Network Exit MS State Change Response messages | Groups the statistics of the MS state change response messages on network exit R6 interface.
> R4 Network Exit MS State Change Response messages | Groups the statistics of the MS state change response messages on network exit R4 interface.
> R6 Context Request messages | Groups the statistics of the context request messages on R6 interface.
> R4 Context Request messages | Groups the statistics of the context request messages on R4 interface.
> R6 Context Report messages | Groups the statistics of the context report messages on R6 interface.
> R4 Context Report messages | Groups the statistics of the context report messages on R4 interface.
> R6 Context Ack messages | Groups the statistics of the context ACK messages on R6 interface.
> R4 Context Ack messages | Groups the statistics of the context ACK messages on R4 interface.
> R6 Authentication Relay EAP Transfer messages | Groups the statistics of the EAP authentication relay transfer messages on R6 interface.
> R4 Authentication Relay EAP Transfer messages | Groups the statistics of the EAP authentication relay transfer messages on R4 interface.
> R6 Authentication Relay EAP Start messages | Groups the statistics of the EAP authentication relay start messages on R6 interface.
> R4 Authentication Relay EAP Start messages | Groups the statistics of the EAP authentication relay start messages on R4 interface.
> R6 MS Attachment Request messages | Groups the statistics of the MS attachment request messages on R6 interface.
> R6 MS Attachment Response messages | Groups the statistics of the MS attachment response messages on R6 interface.
> R6 MS Attachment Ack messages | Groups the statistics of the MS attachment ACK messages on R6 interface.
> R6 Data-Path Pre-Registration Request messages | Groups the statistics of the data path pre-registration request messages on R6 interface.
> R4 Data-Path Pre-Registration Request messages | Groups the statistics of the data path pre-registration request messages on R4 interface.
> R6 Data-Path Pre-Registration Response messages | Groups the statistics of the data path pre-registration response messages on R6 interface.
> R4 Data-Path Pre-Registration Response messages | Groups the statistics of the data path pre-registration response messages on R4 interface.
> R6 Data-Path Pre-Registration Ack messages | Groups the statistics of the data path pre-registration ACK messages on R6 interface.
> R4 Data-Path Pre-Registration Ack messages | Groups the statistics of the data path pre-registration ACK messages on R4 interface.
> R6 Data-Path Registration Request messages | Groups the statistics of the data path registration request messages on R6 interface.
> R4 Data-Path Registration Request messages | Groups the statistics of the data path registration request messages on R4 interface.
> R6 Data-Path Registration Response messages | Groups the statistics of the data path registration response messages on R6 interface.
> R4 Data-Path Registration Response messages | Groups the statistics of the data path registration response messages on R4 interface.
> R6 Data-Path Registration Ack messages | Groups the statistics of the data path registration ACK messages on R6 interface.
> R4 Data-Path Registration Ack messages | Groups the statistics of the data path registration ACK messages on R4 interface.
> R6 Data-Path De-Registration Request messages | Groups the statistics of the data path de-registration request messages on R6 interface.
> R4 Data-Path De-Registration Request messages | Groups the statistics of the data path de-registration request messages on R4 interface.
> R6 Data-Path De-Registration Response messages | Groups the statistics of the data path de-registration response messages on R6 interface.
> R4 Data-Path De-Registration Response messages | Groups the statistics of the data path de-registration response messages on R4 interface.
> R6 Data-Path De-Registration Ack messages | Groups the statistics of the data path de-registration ACK messages on R6 interface.
> R4 Data-Path De-Registration Ack messages | Groups the statistics of the data path de-registration ACK messages on R4 interface.
> R6 Key Change Directive messages | Groups the statistics of the key change directive messages on R6 interface.
> R4 Key Change Directive messages | Groups the statistics of the key change directive messages on R4 interface.
> R6 Key Change Ack messages | Groups the statistics of the key change ACK messages on R6 interface.
> R4 Key Change Ack messages | Groups the statistics of the key change ACK messages on R4 interface.
> R6 Key Change Confirm messages | Groups the statistics of the key change confirm messages on R6 interface.
> R4 Key Change Confirm messages | Groups the statistics of the key change confirm messages on R4 interface.
> R6 Cmac Key Count Update Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count update messages on R6 interface.
> R4 Cmac Key Count Update Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count update messages on R4 interface.
> R6 Cmac Key Count Ack Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count ACK messages on R6 interface.
> R4 Cmac Key Count Ack Msg | Groups the statistics of the Cipher-based Message Authentication Code (CMAC) key count ACK messages on R46 interface.
> R6 Handoff Request Msg | Groups the statistics of the hand-off request messages on R6 interface.
> R4 Handoff Request Msg | Groups the statistics of the hand-off request messages on R4 interface.
> R6 Handoff Response Msg | Groups the statistics of the hand-off response messages on R6 interface.
> R4 Handoff Response Msg | Groups the statistics of the hand-off response messages on R4 interface.
> R6 Handoff Ack Msg | Groups the statistics of the hand-off ACK messages on R6 interface.
> R4 Handoff Ack Msg | Groups the statistics of the hand-off ACK messages on R4 interface.
> R6 Handoff Confirm Msg | Groups the statistics of the hand-off confirm messages on R6 interface.
> R4 Handoff Confirm Msg | Groups the statistics of the hand-off confirm messages on R4 interface.
> R6 Handoff Complete Msg | Groups the statistics of the hand-off complete messages on R6 interface.
> R4 Handoff Complete Msg | Groups the statistics of the hand-off complete messages on R4 interface.
> R4 IM Entry State Change Req Msg | Groups the statistics of the idle mode entry state change request messages on R4 interface.
> R4 IM Entry State Change Rsp Msg | Groups the statistics of the idle mode entry state change response messages on R4 interface.
> R4 IM Entry State Change Ack Msg | Groups the statistics of the idle mode entry state change ACK messages on R4 interface.
> R4 Anchor PC Indication Msg | Groups the statistics of anchor paging controller (PC) indication messages on R4 interface.
> R4 Anchor PC Ack Msg | Groups the statistics of anchor paging controller (PC) ACK messages on R4 interface.
> R4 IM Exit State Change Req Msg | Groups the statistics of the idle mode exit state change request messages on R4 interface.
> R4 IM Exit State Change Rsp Msg | Groups the statistics of the idle mode exit state change response messages on R4 interface.
> R4 Initiate Paging Req Msg | Groups the statistics of the initiated paging request messages on R4 interface.
> R4 Initiate Paging Rsp Msg | Groups the statistics of the initiated paging response messages on R4 interface.
> R4 Delete MS Entry Req Msg | Groups the statistics of the request messages to delete the MS entry request on R4 interface.
> R4 Delete MS Entry Rsp Msg | Groups the statistics of the messages sent in response of delete message for the MS entry request on R4 interface.
> R6 Unknown messages | Groups the statistics of the unknown type of request messages on R6 interface.
> R4 Unknown messages | Groups the statistics of the unknown type of request messages on R4 interface.
> Message Statistics
> Total Sent | The total number of this type of message sent on specific interface.
> Total Send Failures | The total number of failures occurred during transaction id generation and message not sent for specific interface. This counter is used to count the error while sending the R6/R4 packets.
> Retransmissions Sent | The total number of this type of message re-transmitted on specific interface.
> Total Received | The total number of this type of message received on specific interface.
> Total Accepted | The total number of this type of message accepted on specific interface.
> Total Relayed | The total number of this type of message relayed on specific interface.
> Total Denied | The total number of this type of message denied on specific interface.
> Total Discarded | The total number of this type of message discarded on specific interface.
> Badly Formed | The total number of badly formed this type of message on specific interface.
> Decode Error | The total number of this type of message on specific interface with decode error.
> Unspecified Error | The total number of this type of message on specific interface with unspecified error.
> Missing Mandatory TLV | The total number of this type of message on specific interface with missing mandatory TLVs.
> TLV Value Invalid | The total number of this type of message unspecific interface with invalid TLV value.
> Unknown TLV | The total number of this type of message on specific interface with unknown TLVs.
> Duplicate TLV Found | The total number of this type of message on specific interface with duplicate TLVs.
> No session Found | The total number of this type of message on specific interface without any session information.
> Transaction Id. Error | The total number of this type of message on specific interface. with transaction id error.
> Key Change Success | The total number of successful Key Change Confirmation messages.
> Key Change Failure | The total number of Key Change Confirmation messages failed.
> Out Of Order Packet | The total number of authentication relay EAP transfer/start messages on R6 interface with out-of-order packets.
> MS Initiated Re-Auth | The total number of authentication relay EAP start messages on specific interface with MS initiated reauthorization.
> BS Initiated Re-Auth | The total number of authentication relay EAP start messages on specific interface with BS initiated reauthorization.
> Data messages
> GRE R6 Receive | The total number of data message received with through GRE tunnel on R6 interface.
> GRE R4 Receive | The total number of data message received through GRE tunnel on R4 interface.
> Packets Received | The total number of data packets received/sent through GRE tunnel on R4/R6 interface.
> Bytes Received | The total number of data bytes received/sent through GRE tunnel on R4/R6 interface.
> Protocol Type Error | The total number of data message received/sent with protocol type error through GRE tunnel on R4/R6 interface.
> GRE Key Absent | The total number of data message received/sent without GRE key through GRE tunnel on R4/R6 interface.
> GRE Checksum Error | The total number of data message received/sent with checksum error through GRE tunnel on R4/R6 interface.
> Invalid Packet Length | The total number of data message received/sent with invalid packet length through GRE tunnel on R4/R6 interface.
> No Session found | The total number of data message received/sent without any session information through GRE tunnel on R4/R6 interface.
> Unspecified Error | The total number of data message received/sent with unknown error through GRE tunnel on R4/R6 interface.
> GRE R6 Send | The total number of data message sent through GRE tunnel on R6 interface.
> GRE R4 Send | The total number of data message sent through GRE tunnel on R4 interface.
> Packets Sent | The total number of data packets sent through GRE tunnel on R4/R6 interface.
> Send Error | The total number of data message sent with error through GRE tunnel on R4/R6 interface.
> Bytes Sent | The total number of data bytes sent through GRE tunnel on R4/R6 interface.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883