> show sgsn-operator-policy
> This chapter describes the output of the show sgsn-operator-policy command.
> show sgsn-operator-policy full { all | name }
> This command displays the configuration for a specifically named SGSN operator policy or for all of them.
> show sgsn-operator-policy full all Command Output Descriptions

> Field | Description
> GPRS Attach All | Indicates whether GRPS attaches are to be allowed.
> GPRS Attach All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS Attach All | Indicates whether UMTS attaches are to be allowed.
> UMTS Attach All Failure Code | Indicates configured failure code to be sent in reject message.
> GPRS RAU Intra All | Indicates whether RAU Intra are to be allowed.
> GPRS RAU Intra All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS RAU Intra All | Indicates whether RAU Intra are to be allowed.
> UMTS RAU Intra All Failure Code | Indicates configured failure code to be sent in reject message.
> GPRS RAU Inter All | Indicates whether RAU Inter are to be allowed.
> GPRS RAU Inter All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS RAU Inter All | Indicates whether RAU Inter are to be allowed.
> UMTS RAU Inter All Failure Code | Indicates configured failure code to be sent in reject message.
> Failure Code For Peer Sgsn Address Resolution Failure | Indicates configured failure code to be sent in reject message.
> GPRS SMS MO All | Indicates whether
> GPRS SMS MO All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS SMS MO All Failure Code | Indicates configured failure code to be sent in reject message.
> GPRS SMS MT All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS SMS MT All Failure Code | Indicates configured failure code to be sent in reject message.
> GPRS PDP Context Activation All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS PDP Context Activation All Failure Code | Indicates configured failure code to be sent in reject message.
> GPRS Nw Init Primary PDP Ctxt Activation All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS Nw Init Primary PDP Ctxt Activation All Failure Code | Indicates configured failure code to be sent in reject message.
> UMTS Nw Init Secondary PDP Ctxt Activation All Failure Code | Indicates configured failure code to be sent in reject message.
> SRNS Intra All Failure Code | Indicates configured failure code to be sent in reject message.
> SRNS Inter All Failure Code | Indicates configured failure code to be sent in reject message.
> Authentication All-Events | Indicates if feature has been enabled or disabled.
> Authentication Attach | Indicates if feature has been enabled or disabled.
> Authentication Attach (Gprs only) | Indicates if feature has been enabled or disabled.
> Authentication Attach (Combined) | Indicates if feature has been enabled or disabled.
> Authentication Activate | Indicates if feature has been enabled or disabled.
> Authentication Service Request | Indicates if feature has been enabled or disabled.
> Authentication Service Request (Signaling) | Indicates if feature has been enabled or disabled.
> Authentication Service Request (Data) | Indicates if feature has been enabled or disabled.
> Authentication Service Request (Page Response) | Indicates if feature has been enabled or disabled.
> Authentication RAU | Indicates if feature has been enabled or disabled.
> Authentication RAU (Periodic) | Indicates if feature has been enabled or disabled.
> Authentication RAU (Ra update) | Indicates if feature has been enabled or disabled.
> Authentication RAU (Ra update with Local Ptmsi) | Indicates if feature has been enabled or disabled.
> Authentication RAU (Ra update with Foreign Ptmsi) | Indicates if feature has been enabled or disabled.
> Authentication RAU (Combined Update) | Indicates if feature has been enabled or disabled.
> Authentication RAU (Imsi Combined Update) | Indicates if feature has been enabled or disabled.
> Authentication Detach | Indicates if feature has been enabled or disabled.
> Usage of Auth Vectors From Old Sgsn | Indicates if feature has been enabled or disabled.
> PTMSI-Realloc Service Request (Page Response) | Indicates if feature has been enabled or disabled.
> PTMSI-Realloc Service Request (Page Response) Freq | Indicates frequency, if configured.
> Inactivity detection for establishing pdp contexts | Indicates if feature has been enabled or disabled.
> Inactivity detection for establishing pdp contexts - Timer | Indicates timeout value in milliseconds.
> Inactivity detection for establishing pdp contexts - Action | Indicates action to be taken.
> Monitor Re-attaches after Inactivity Detach | Indicates if feature has been enabled or disabled.
> Charging Characteristics Prefer Local | Indicates if feature has been enabled or disabled.
> Charging Characteristics Profile-Index | Indicates CC profile index.
> Charging Characteristics Behavior No Records | Indicates configured CC behavior.
> UMTS Gmm-Information | Indicates if feature has been enabled or disabled.
> GPRS Gmm-Information | Indicates if feature has been enabled or disabled.
> User Equipment Identity Retrieval | Indicates if feature has been enabled or disabled.
> Reuse of authentication triplets | Indicates if feature has been enabled or disabled.
> Re-Authentication | Indicates if feature has been enabled or disabled.
> GTPU Fast Path | Indicates if feature has been enabled or disabled.
> Sending Radio Access Technology (RAT) IE | Indicates if feature has been enabled or disabled.
> Sending User Location Information (ULI) IE | Indicates if feature has been enabled or disabled.
> Sending IMEISV IE | Indicates if feature has been enabled or disabled.
> Sending MS Time Zone IE | Indicates if feature has been enabled or disabled.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883