> show pdg-service
> This chapter describes the output of the show pdg-service command.
> show pdg-service all
> show pdg-service all Command Output Description

> Field | Description
> Service name | The name of the PDG service.
> Context name | The name of the context in which the PDG service resides.
> Bind | Displays the bind status for the PDG service for binding the service to a crypto template.
> Max sessions | The maximum number of sessions supported by the PDG service.
> IP address | The IPv4 address of the PDG service.
> UDP Port | The UDP port number associated with the IP address.
> Service State | The current state of the PDG service.
> Crypto-template | The name of the crypto template bound to the FNG service.
> SSL-template | The name of the SSL template bound to the FNG service. This is a customer-specific field.
> SGTP Service | The name of the SGTP service bound to the PDG service.
> SGTP Service context | The name of the context in which the SGTP service was created.
> Session Setup Timeout (sec) | The maximum time allowed to set up a session in seconds.
> Certificate Selection | The selection method for selecting the certificate to be included in the first IKE-AUTH message. Can be APN-based or crypto template-based.
> PLMN Id | The PLMN identifiers for the PDG/TTG.
> Duplicate Session Detection Type | The duplicate session detection type.
> IP Source Violation - Drop Limit | The drop-limit value, which is the maximum number of allowed IP source violations within the detection period before dropping a call.
> IP Source Violation - Period | The detection period in seconds for IP source violations.
> IP Source Violation - Clear On Valid Packet | Displays whether the option to reset the drop-limit counters upon receipt of a properly addressed packet is enabled or disabled.
> 3gpp qos to dscp Downlink mapping | This group indicates the 3GPP QoS to DSCP downlink mapping information.
> conversational | Indicates the DSCP configured for conversational type of traffic.
> streaming | Indicates the DSCP configured for streaming type of traffic.
> interactive (TP 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1.
> interactive (TP 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2.
> interactive (TP 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3.
> background | Indicates the DSCP configured for background type of traffic.
> 3GPP qos to dscp Downlink mapping based on Alloc. Prio | This group indicates the 3GPP QoS to DSCP downlink mapping information based on allocation priority.
> interactive (TP 1, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 1.
> interactive (TP 1, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 2.
> interactive (TP 1, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 3.
> interactive (TP 2, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 1.
> interactive (TP 2, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 2.
> interactive (TP 2, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 3.
> interactive (TP 3, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic withtraffic priority 3 and allocation priority 1.
> interactive (TP 3, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 2.
> interactive (TP 2, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 2.
> 3gpp qos to dscp Uplink mapping (TTG only) | This group indicates the 3GPP QoS to DSCP uplink mapping information.
> conversational | Indicates the DSCP configured for conversational type of traffic.
> streaming | Indicates the DSCP configured for streaming type of traffic.
> interactive (TP 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1.
> interactive (TP 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2.
> interactive (TP 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3.
> background | Indicates the DSCP configured for background type of traffic.
> 3GPP qos to dscp Uplink mapping based on Alloc. Prio | This group indicates the 3GPP QoS to DSCP downlink mapping information based on allocation priority.
> interactive (TP 1, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 1.
> interactive (TP 1, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 2.
> interactive (TP 1, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 1 and allocation priority 3.
> interactive (TP 2, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 1.
> interactive (TP 2, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 2.
> interactive (TP 2, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 2 and allocation priority 3.
> interactive (TP 3, Alloc.P 1) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 1.
> interactive (TP 3, Alloc.P 2) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 2.
> interactive (TP 3, Alloc.P 3) | Indicates the DSCP configured for interactive type of traffic with traffic priority 3 and allocation priority 3.

> ‌
> show pdg-service statistics
> show pdg-service statistics Command Output Description

> Field | Description
> Session Stats
> Current sessions total | Total number of sessions in progress including transient sessions.
> Direct-IP-IPv4 current | Total number of currently active Direct IP IPv4 sessions.
> TTG-IPv4 current | Total number of currently active TTG IPv4 sessions.
> Active current | Total number of currently active sessions.
> Dormant current | Total number of currently dormant sessions.
> Active IPv4 current | Total number of currently active IPv4 sessions.
> Active IPv6 current | Total number of currently active IPv6 sessions.
> Dormant IPv4 current | Total number of currently dormant IPv4 sessions.
> Dormant IPv6 current | Total number of currently dormant IPv6 sessions.
> Total Direct-IP IPv4 | Total number of Direct IP IPv4 sessions.
> Total TTG IPv4 | Total number of TTG IPv4 sessions.
> Direct-IP IPv4 attempts | Total number of Direct IP IPv4 attempts.
> Direct-IP IPv4 successes | Total number of Direct IP IPv4 successes.
> Direct-IP IPv4 failures | Total number of Direct IP IPv4 failures.
> Total setup attempts | Total number of session setup attempts.
> Total setup success | Total number of successful session attempts.
> Total Attempts Failed | Total number of failed session attempts.
> Total disconnected | Total number of sessions released locally and remotely.
> Disconnect locally | Total number of sessions released locally.
> Disconnect remotely | Total number of sessions released remotely.
> Disconnect remotely before connect | Total number of sessions released remotely before connecting.
> Reauthentication Stats
> Total reauth attempts | Total number of reauthentication attempts.
> Total reauth success | Total number of reauthentication successes.
> Total reauth failure | Total number of reauthentication failures.
> Session Disconnect reason
> Remote disc. ipsec | Number of sessions disconnected because of IPSec.
> Admin disconnect | Number of sessions disconnected by the administrator.
> Idle timeout | Number of sessions disconnected because the idle timer has timed out.
> Absolute timeout | Number of sessions disconnected because the Absolute timer has timed out.
> Long duration timeout | Number of sessions disconnected because the long duration timer has timed out.
> Session setup timeout | Number of sessions disconnected because the Session Manager’s session setup timer has timed out.
> No resource | Number of sessions disconnected because the system has run out of resources (flows, memory resources, etc.).
> Auth failure | Number of sessions disconnected because of an authentication failure.
> Flow add failure | Number of sessions disconnected because a flow could not be added on the NPU.
> Invalid dest-context | Number of sessions disconnected because the destination context received from the AAA server is invalid.
> Source address violation | Number of sessions disconnected because the source IP address is invalid.
> GTP | Number of GTP sessions disconnected.
> Duplicate Request | Number of sessions disconnected because of duplicate requests.
> Addr assign failure | Number of sessions disconnected because no remote IP address has been assigned.
> Miscellaneous reasons | Number sessions disconnected because of miscellaneous reasons.
> Data Stats
> Total Bytes Sent | Total number of bytes sent.
> Total Packets Sent | Total number of packets sent.
> Total Bytes Rcvd | Total number of bytes received.
> Total Packets Rcvd | Total number of packets received.
> EAP Server Statistics
> Total Received | Total number of EAP messages received from the EAP server in pass-through mode.
> Success Received | Total Number of EAP success messages received from the EAP server in pass-through mode.
> Challenge Received | Total number of EAP challenge messages received from the EAP server in pass-through mode.
> Failures Received | Total number of EAP failure messages received from the EAP server in pass-through mode.
> Total Sent | Total number of EAP messages transmitted to the EAP server in pass-through mode.
> Initial Requests | Total number of initial EAP messages transmitted to the EAP server in pass-through mode.
> Requests Forwarded | Total number of EAP requests forwarded to the EAP server in pass-through mode.
> EAP Mobile Stats
> Total Received | Total number of EAP messages received from the UEs in pass-through mode.
> Discarded | Total number of EAP messages received from the UEs in pass-though mode.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883