Management Attribute/Packet Table

Attribute | MGMT Access-Request | MGMT Access-Reject | MGMT Access-Accept | MGMT Acct-Request-Start | MGMT Acct-Request-Interim | MGMT Acct-Request-Stop
3GPP2-ESN | 1 | 0 | 0 | 0 | 0 | 0
Acct-Authentic | 0 | 0 | 0 | 1 | 1 | 1
Acct-Interim-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
Acct-Session-Id | 0 | 0 | 0 | 1 | 1 | 1
Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
EAP-Message | 0+ | 1 | 0+ | 0 | 0 | 0
Error-Cause | 0 | 0-1 | 0 | 0 | 0 | 0
Framed-IPv6-Prefix | 0 | 0 | 0 | 0 | 0+ | 0+
Idle-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
NAS-Port | 1 | 0 | 0 | 1 | 1 | 1
NAS-Port-Type | 1 | 0 | 0 | 1 | 1 | 1
Reply-Message | 0 | 0-1 | 0-1 | 0 | 0 | 0
Service-Type | 1 | 0 | 0-1 | 1 | 1 | 1
Session-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Admin-Expiry | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN1-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN1-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN1-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN1-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Acs-Credit-Control-Group | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Admin-Expiry | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Fast-Reauth-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Pseudonym-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
State | 1 | 0 | 0-1 | 0 | 0 | 0
User-Name | 1 | 0 | 0-1 | 1 | 1 | 1
User-Password | 1 | 0 | 0 | 0 | 0 | 0
WiMAX-Home-HNP-PMIP6 | 0 | 0 | 0 | 0 | 0+ | 0+

PSDN or FA Attribute/Packet Table

Attribute | PDSN or FA Access-Request | PDSN or FA Access-Reject | PDSN or FA Access-Accept | PDSN or FA Acct-Request-Start | PDSN or FA Acct-Request-Interim | PDSN or FA Acct-Request-Stop
3GPP2-Active-Time | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Airlink-Record-Type | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Airlink-Sequence-Number | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Air-QOS | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Allowed-Persistent-TFTs | 0 | 0-1 | 0-1 | 0 | 0 | 0
3GPP2-Always-On | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
3GPP2-Bad-PPP-Frame-Count | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-BCMCS-Flow-ID | 0-1 | 0 | 0 | 1 | 1 | 1
3GPP2-BCMCS-Flow-Transmit-Time | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-BCMCS-Mcast-IP-Addr | 0 | 0 | 0-1 | 1 | 0 | 1
3GPP2-BCMCS-Mcast-Port | 0 | 0 | 0-1 | 1 | 0 | 1
3GPP2-BCMCS-Reason-Code | 1 | 0 | 0 | 0 | 0 | 0
3GPP2-Beginning-Session | 0 | 0 | 0 | 1 | 0 | 0
3GPP2-BSID | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-Comp-Tunnel-Indicator | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Correlation-Id | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-DCCH-Frame-Size | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-ESN | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-FA-Address | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Flow-Status | 0 | 0 | 0 | 0 | 0 | 0-1
3GPP2-Forward-Fundamental-Rate | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Forward-Fundamental-RC | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Forward-Mux-Option | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Forward-Traffic-Type | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Fundamental-Frame-Size | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Fwd-Dcch-Mux-Option | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Fwd-Dcch-Rc | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Fwd-Pdch-Rc | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-IKE-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-IKE-Secret-Request | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-Inter-User-Priority | 0 | 0-1 | 0-1 | 0 | 0 | 0
3GPP2-IP-QOS | 0 | 0 | 0-1 | 1 | 1 | 1
3GPP2-IP-Technology | 0-1 | 0 | 0-1 | 1 | 1 | 1
3GPP2-KeyID | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-Last-Activity | 0 | 0 | 0 | 0 | 0-1 | 1
3GPP2-Max-Auth-Aggr-Bw-BET | 0 | 0-1 | 0-1 | 0 | 0 | 0
3GPP2-Max-Per-Fl-Pri-ForTheUser | 0 | 0-1 | 0-1 | 0 | 0 | 0
3GPP2-MEID | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-MIP6-Home-Address | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP6-Home-Agent | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP6-Home-Link-Prefix | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP-HA-Address | 1 | 0 | 0+ | 1 | 1 | 1
3GPP2-MIP-Rev-Tunnel-Required | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP-Sig-Octet-Count-In | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-MIP-Sig-Octet-Count-Out | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-MN-AAA-Removal-Indication | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MN-HA-SPI | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-Mobile-Term-Orig-Ind | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Number-Active-Transitions | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Num-Bytes-Received-Total | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Num-SDB-Input | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Num-SDB-Output | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Release-Indicator-Prepaid | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
3GPP2-Rev-Dcch-Mux-Option | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Rev-Dcch-Rc | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Reverse-Fundamental-Rate | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Reverse-Fundamental-RC | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Reverse-Mux-Option | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Reverse-Traffic-Type | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Rev-Pdch-Rc | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-RP-Session-ID | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-Rsvp-Signal-In-Count | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-Rsvp-Signal-In-Packets | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-Rsvp-Signal-Out-Count | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-Rsvp-Signal-Out-Packets | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-SDB-Output-Octets | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Security-Level | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-Service-Option | 0-1 | 0-1 | 0-1 | 1 | 1 | 1
3GPP2-Serving-PCF | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-Session-Continue | 0 | 0 | 0 | 0 | 1 | 1
3GPP2-Session-Term-Capability | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-User-Zone | 1 | 0 | 0 | 1 | 1 | 1
3GPP-Charging-Id | 1 | 0 | 0 | 0 | 0 | 0
3GPP-Chrg-Char | 0 | 0-1 | 0-1 | 0 | 0 | 0
Acct-Authentic | 0 | 0 | 0 | 1 | 1 | 1
Acct-Input-Packets | 0-1 | 0 | 0 | 0 | 1 | 1
Acct-Interim-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
Acct-Output-Packets | 0-1 | 0 | 0 | 0 | 1 | 1
Acct-Session-Id | 0 | 0 | 0 | 1 | 1 | 1
Called-Station-ID | 1 | 0-1 | 0-1 | 1 | 1 | 1
Calling-Station-Id | 1 | 0 | 1 | 1 | 1 | 1
Class | 0-1 | 0-1 | 0-1 | 0-1 | 0-1 | 0-1
Connect-Info | 1 | 0 | 0-1 | 1 | 1 | 1
CS-Prepaid-Quota | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
CS-Prepaid-Time-Quota | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
CS-Prepaid-Volume-Quota | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
CS-Service-Name | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
CUI | 0-1 | 0-1 | 0-1 | 0-1 | 0-1 | 0-1
EAP-Message | 0+ | 1 | 0+ | 0 | 0 | 0
Error-Cause | 0 | 0-1 | 0 | 0 | 0 | 0
Framed-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-Interface-Id | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-IP-Address | 0-1 | 0-1 | 0-1 | 1 | 1 | 1
Framed-IP-Netmask | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-IPv6-Pool | 0 | 0 | 0-1 | 0 | 0 | 0
Framed-IPv6-Prefix | 0+ | 0 | 0+ | 0+ | 0+ | 0+
Framed-MTU | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-Pool | 0 | 0-1 | 0+ | 0 | 0 | 0
Framed-Protocol | 1 | 0 | 0-1 | 1 | 1 | 1
Idle-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
MS-CHAP-Domain | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
MS-CHAP-Error | 0 | 0-1 | 0 | 0 | 0 | 0
MS-Primary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
MS-Secondary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
NAS-Port | 1 | 0 | 0 | 1 | 1 | 1
NAS-Port-Type | 1 | 0 | 0 | 1 | 1 | 1
Primary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
Reply-Message | 0 | 0-1 | 0-1 | 0 | 0 | 0
Secondary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
Service-Type | 1 | 0 | 0-1 | 1 | 1 | 1
Session-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Assigned-VLAN-ID | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN1-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN1-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN1-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN1-FMC-Location | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-HA-Send-DNS-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Header-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-In-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Out-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Pool-Name | 0 | 0-1 | 0+ | 0 | 0 | 0
SN1-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-DNS-Proxy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Egress-Filtering | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Min-Link-MTU | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-num-rtr-advt | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Primary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-rtr-advt-interval | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Secondary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN1-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN1-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Min-Compress-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-AAA-Assign-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-ANCID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN1-MIP-Match-AAA-Assign-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-Send-Ancid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-Send-Correlation-Info | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-Send-Imsi | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-Send-Term-Verification | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-NAI-Construction-Domain | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PDIF-MIP-Release-TIA | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PDIF-MIP-Required | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PDIF-MIP-Simple-IP-Fallback | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PDSN-Handoff-Req-IP-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Accept-Peer-v6Ifid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Always-On-Vse | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Data-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-PPP-Data-Compression-Mode | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-PPP-Keepalive | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-NW-Layer-IPv4 | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-NW-Layer-IPv6 | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Outbound-Password | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Outbound-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Progress-Code | 0 | 0 | 0 | 0 | 0 | 0-1
SN1-PPP-Reneg-Disc | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Compressed-Count | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Final-Duration-Alg | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Inbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Outbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Total-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Watermark | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Primary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Proxy-MIP | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Re-CHAP-Interval | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-ROHC-Direction | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-ROHC-Flow-Marking-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-ROHC-Mode | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-ROHC-Profile-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Secondary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Secondary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Service-Address | 0-1 | 0 | 0 | 0 | 0 | 0
SN1-Simultaneous-SIP-MIP | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-Acc-Flow-Traffic-Valid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Subscriber-Dormant-Activity | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-IP-Hdr-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-VJ-Slotid-Cmp-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Unclassify-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Voice-Push-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
SN-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Acs-Credit-Control-Group | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Assigned-VLAN-ID | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Bandwidth-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CBB-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Direction | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Fast-Reauth-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN-Firewall-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-FMC-Location | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-HA-Send-DNS-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Header-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-In-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Out-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Pool-Name | 0 | 0-1 | 0+ | 0 | 0 | 0
SN-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-DNS-Proxy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Egress-Filtering | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Min-Link-MTU | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-num-rtr-advt | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Primary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-rtr-advt-interval | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Secondary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Min-Compress-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-AAA-Assign-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-ANCID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN-MIP-Match-AAA-Assign-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-Send-Ancid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-Send-Correlation-Info | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-Send-Imsi | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-Send-Term-Verification | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Mode | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-NAI-Construction-Domain | 0 | 0 | 0-1 | 0 | 0 | 0
SN-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDG-TTG-Required | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDIF-MIP-Release-TIA | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDIF-MIP-Required | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDIF-MIP-Simple-IP-Fallback | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDSN-Handoff-Req-IP-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Accept-Peer-v6Ifid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Always-On-Vse | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Data-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-PPP-Data-Compression-Mode | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-PPP-Keepalive | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-NW-Layer-IPv4 | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-NW-Layer-IPv6 | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Outbound-Password | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Outbound-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Progress-Code | 0 | 0 | 0 | 0 | 0 | 0-1
SN-PPP-Reneg-Disc | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Compressed-Count | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Final-Duration-Alg | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Inbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Outbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Total-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Watermark | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Primary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Proxy-MIP | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Pseudonym-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QOS-HLR-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Re-CHAP-Interval | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-ROHC-Flow-Marking-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-ROHC-Profile-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Sec-IP-Pool-Name | 0 | 0 | 0+ | 0 | 0 | 0
SN-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Secondary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Secondary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Service-Address | 0-1 | 0 | 0 | 0 | 0 | 0
SN-Simultaneous-SIP-MIP | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-Acc-Flow-Traffic-Valid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Subscriber-Dormant-Activity | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-IP-Hdr-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-VJ-Slotid-Cmp-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-TrafficSelector-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Unclassify-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Voice-Push-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
SN-WiMAX-Auth-Only | 0 | 0 | 0-1 | 0 | 0 | 0
State | 1 | 0-1 | 0-1 | 0 | 0 | 0
Termination-Action | 0 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Assignment-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Medium-Type | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Private-Group-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Type | 0 | 0 | 0-1 | 1 | 1 | 1
User-Name | 1 | 0 | 0-1 | 1 | 1 | 1
User-Password | 0-1 | 0 | 0 | 0 | 0 | 0

HA Attribute/Packet Table

Attribute | HA Access-Request | HA Access-Reject | HA Access-Accept | HA Acct- Request-Start | HA Acct- Request-Interim | HA Acct- Request-Stop
3GPP2-Beginning-Session | 0 | 0 | 0 | 0-1 | 0 | 0
3GPP2-BSID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Comp-Tunnel-Indicator | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Correlation-Id | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-DNS-Update-Required | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-ESN | 1 | 0 | 0 | 0 | 0 | 0
3GPP2-FA-Address | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-IP-QOS | 0 | 0 | 0-1 | 1 | 1 | 1
3GPP2-IP-Technology | 0-1 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MEID | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP6-Authenticator | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-CoA | 0-1 | 0 | 0 | 0-1 | 0-1 | 0
3GPP2-MIP6-HA | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-HoA | 0-1 | 0 | 0 | 0-1 | 0-1 | 0
3GPP2-MIP6-HoA-Not-Authorized | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP6-MAC-Mobility-Data | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-Mesg-ID | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-Session-Key | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MN-HA-Shared-Key | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MN-HA-SPI | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-Mobile-Term-Orig-Ind | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Service-Option | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-Serving-PCF | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Session-Continue | 0 | 0 | 0 | 0 | 0 | 0-1
Acct-Authentic | 0 | 0 | 0 | 1 | 1 | 1
Acct-Input-Packets | 0-1 | 0 | 0 | 0 | 1 | 1
Acct-Interim-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
Acct-Multi-Session-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Acct-Output-Packets | 0-1 | 0 | 0 | 0 | 1 | 1
Acct-Session-Id | 0 | 0 | 0 | 1 | 1 | 1
Calling-Station-Id | 1 | 0 | 1 | 1 | 1 | 1
Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
CUI | 0-1 | 0 | 0-1 | 0 | 0 | 0
Error-Cause | 0 | 0-1 | 0 | 0 | 0 | 0
Framed-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
Framed-IP-Netmask | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-IPv6-Pool | 0 | 0 | 0-1 | 0 | 0 | 0
Framed-MTU | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-Pool | 0 | 0 | 0+ | 0 | 0 | 0
Idle-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
MS-Primary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
MS-Secondary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
NAS-Port | 1 | 0 | 0 | 1 | 1 | 1
NAS-Port-Type | 1 | 0 | 0 | 1 | 1 | 1
Primary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
Reply-Message | 0 | 0-1 | 0-1 | 0 | 0 | 0
Secondary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
Service-Type | 1 | 0 | 0-1 | 1 | 1 | 1
Session-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Assigned-VLAN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN1-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN1-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN1-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN1-FMC-Location | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Gratuitous-ARP-Aggressive | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ignore-Unknown-HA-Addr-Err | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IMS-AM-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IMS-AM-Domain-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Pool-Name | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN1-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN1-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-ANCID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-MIP-Dual-Anchor | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN1-MIP-Reg-Lifetime-Realm | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MN-HA-Timestamp-Tolerance | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Nw-Reachability-Server-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PDSN-Correlation-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-PDSN-NAS-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-PDSN-NAS-IP-Address | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Compressed-Count | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Final-Duration-Alg | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Inbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Outbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Total-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Watermark | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Primary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Re-CHAP-Interval | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Secondary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Secondary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Service-Address | 0-1 | 0 | 0 | 0 | 0 | 0
SN1-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Unclassify-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Voice-Push-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
SN-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Acs-Credit-Control-Group | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Assigned-VLAN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Bandwidth-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CBB-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN-Firewall-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-FMC-Location | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Gratuitous-ARP-Aggressive | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ignore-Unknown-HA-Addr-Error | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IMS-AM-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IMS-AM-Domain-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Pool-Name | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-ANCID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-MIP-Dual-Anchor | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN-MIP-Reg-Lifetime-Realm | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MN-HA-Timestamp-Tolerance | 0 | 0 | 0-1 | 0 | 0 | 0
SN-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Nw-Reachability-Server-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDSN-Correlation-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-PDSN-NAS-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-PDSN-NAS-IP-Address | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Compressed-Count | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Final-Duration-Alg | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Inbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Outbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Total-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Watermark | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Primary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Re-CHAP-Interval | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Secondary-DNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Secondary-NBNS-Server | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Service-Address | 0-1 | 0 | 0 | 0 | 0 | 0
SN-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-TrafficSelector-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Unclassify-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Voice-Push-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
SN-WiMAX-Auth-Only | 0 | 0 | 0-1 | 0 | 0 | 0
State | 1 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Assignment-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Medium-Type | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Private-Group-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Type | 0 | 0 | 0-1 | 1 | 1 | 1
User-Name | 1 | 0 | 0-1 | 1 | 1 | 1

GGSN Attribute/Packet Table

Attribute | GGSN Access-Request | GGSN Access-Reject | GGSN Access-Accept | GGSN Acct- Request-Start | GGSN Acct- Request-Interim | GGSN Acct- Request-Stop
3GPP2-BSID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-CAMEL-Charging-Info | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-CG-Address | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-Charging-Id | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-Chrg-Char | 0-1 | 0-1 | 0-1 | 0-1 | 0-1 | 0-1
3GPP-GGSN-Address | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-GGSN-Mcc-Mnc | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-IMEISV | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-IMSI | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-IMSI-Mcc-Mnc | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-MS-TimeZone | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-Negotiated-DSCP | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-Negotiated-QoS-Profile | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-NSAPI | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-PDP-Type | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-RAT-Type | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-Selection-Mode | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-Session-Stop-Ind | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP-SGSN-Address | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-SGSN-Mcc-Mnc | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP-User-Location-Info | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
Acct-Authentic | 0 | 0 | 0 | 1 | 1 | 1
Acct-Input-Packets | 0-1 | 0 | 0 | 0 | 0 | 0-1
Acct-Interim-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
Acct-Multi-Session-Id | 0-1 | 0 | 0 | 1 | 1 | 1
Acct-Output-Packets | 0-1 | 0 | 0 | 0 | 0 | 0-1
Acct-Session-Id | 0-1 | 0 | 0 | 1 | 1 | 1
Called-Station-ID | 1 | 0 | 0 | 1 | 1 | 1
Calling-Station-Id | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
Class | 0 | 0 | 0+ | 0-1 | 0-1 | 0-1
CUI | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
EAP-Message | 0+ | 1 | 0+ | 0 | 0 | 0
Error-Cause | 0 | 0-1 | 0 | 0 | 0 | 0
Framed-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-Interface-Id | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-IP-Address | 0-1 | 0 | 1 | 0-1 | 0-1 | 0-1
Framed-IP-Netmask | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Framed-IPv6-Prefix | 0+ | 0 | 0+ | 0+ | 0+ | 0+
Framed-MTU | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-Protocol | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Idle-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
MS-Primary-NBNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
MS-Secondary-NBNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
NAS-Port-Type | 0-1 | 0 | 0 | 0-1 | 0 | 0-1
Primary-DNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
Reply-Message | 0 | 0-1 | 0-1 | 0 | 0 | 0
Secondary-DNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
Service-Type | 0-1 | 0 | 0-1 | 0-1 | 0 | 0-1
Session-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Assigned-VLAN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Disconnect-Reason | 0 | 0 | 0 | 0 | 0-1 | 0-1
SN1-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN1-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN1-Ecs-Data-Volume | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN1-GTP-Version | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Home-Behavior | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Home-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Home-Sub-Use-GGSN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-In-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Out-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-DNS-Proxy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Egress-Filtering | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Min-Link-MTU | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-num-rtr-advt | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Primary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-rtr-advt-interval | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Secondary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN1-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN1-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Mediation-Acct-Rsp-Action | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Mediation-Enabled | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Mediation-No-Interims | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Mediation-VPN-Name | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Min-Compress-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN1-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Accept-Peer-v6Ifid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Always-On-Vse | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Data-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-PPP-Data-Compression-Mode | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-PPP-Keepalive | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-NW-Layer-IPv4 | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-NW-Layer-IPv6 | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Outbound-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PPP-Reneg-Disc | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Primary-DNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-NBNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Rad-APN-Name | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Radius-Returned-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Re-CHAP-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Roaming-Behavior | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Roaming-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Roaming-Sub-Use-GGSN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-ROHC-Flow-Marking-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-ROHC-Profile-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Secondary-DNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Secondary-NBNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-Acc-Flow-Traffic-Valid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Dormant-Activity | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-IP-Hdr-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-VJ-Slotid-Cmp-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Transparent-Data | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-Gn | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Virtual-APN-Name | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Visiting-Behavior | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Visiting-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Visiting-Sub-Use-GGSN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
SN-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Acs-Credit-Control-Group | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Assigned-VLAN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Bandwidth-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CBB-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Disconnect-Reason | 0 | 0 | 0 | 0 | 0-1 | 0-1
SN-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN-DNS-Proxy-Use-Subscr-Addr | 0 | 0 | 1 | 0 | 0 | 0
SN-Ecs-Data-Volume | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Fast-Reauth-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN-Firewall-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-GTP-Version | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Home-Behavior | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Home-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Home-Sub-Use-GGSN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-In-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Out-Plcy-Grp | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-DNS-Proxy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Egress-Filtering | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Min-Link-MTU | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-num-rtr-advt | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Primary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-rtr-advt-interval | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Secondary-DNS | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Mediation-Acct-Rsp-Action | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Mediation-Enabled | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Mediation-No-Interims | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Mediation-VPN-Name | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Min-Compress-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Accept-Peer-v6Ifid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Always-On-Vse | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Data-Compression | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-PPP-Data-Compression-Mode | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-PPP-Keepalive | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-NW-Layer-IPv4 | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-NW-Layer-IPv6 | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Outbound-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PPP-Reneg-Disc | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Primary-DNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-NBNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Pseudonym-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Rad-APN-Name | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Radius-Returned-Username | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Re-CHAP-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Roaming-Behavior | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Roaming-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Roaming-Sub-Use-GGSN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-ROHC-Flow-Marking-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-ROHC-Profile-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Secondary-DNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Secondary-NBNS-Server | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-Acc-Flow-Traffic-Valid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Dormant-Activity | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-IP-Hdr-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-VJ-Slotid-Cmp-Neg-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Transparent-Data | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-Gn | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Virtual-APN-Name | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Visiting-Behavior | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Visiting-Profile | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Visiting-Sub-Use-GGSN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
State | 1 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Assignment-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Medium-Type | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Private-Group-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Type | 0 | 0 | 0-1 | 1 | 1 | 1
User-Name | 1 | 0 | 0-1 | 0-1 | 0 | 0-1
User-Password | 0-1 | 0 | 0 | 0 | 0 | 0
WiMAX-BS-ID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
WiMAX-Home-HNP-PMIP6 | 0+ | 0 | 0+ | 0+ | 0+ | 0+
WiMAX-Home-IPv4-HoA-PMIP6 | 0-1 | 0 | 1 | 0-1 | 0-1 | 0-1
WiMAX-Prepaid-Indicator | 0 | 0 | 0 | 0-1 | 0-1 | 0-1

WIMAX Attribute/Packet Table

Attribute | WIMAX Access- Request | WIMAX Access- Reject | WIMAX Access- Accept | WIMAX Acct- Request-Start | WIMAX Acct- Request-Interim | WIMAX Acct- Request-Stop
3GPP2-Active-Time | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-Beginning-Session | 0 | 0 | 0 | 1 | 0 | 0
3GPP2-BSID | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
3GPP2-IP-QOS | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-IP-Technology | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-MIP-Sig-Octet-Count-In | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-MIP-Sig-Octet-Count-Out | 0 | 0 | 0 | 0 | 0-1 | 0-1
3GPP2-MN-HA-Shared-Key | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MN-HA-SPI | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-Session-Continue | 0 | 0 | 0 | 0 | 0 | 1
AAA-Session-ID | 0-1 | 0-1 | 1 | 0 | 0 | 0
Acct-Authentic | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Acct-Input-Packets | 0 | 0 | 0 | 0 | 0-1 | 0-1
Acct-Interim-Interval | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Acct-Multi-Session-Id | 0 | 0 | 0 | 1 | 1 | 1
Acct-Output-Packets | 0 | 0 | 0 | 0 | 0-1 | 0-1
Acct-Session-Id | 0 | 0 | 0 | 1 | 1 | 1
Calling-Station-Id | 1 | 0 | 0 | 1 | 1 | 1
Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Connect-Info | 1 | 0 | 0-1 | 1 | 1 | 1
CUI | 0-1 | 0 | 0-1 | 0-1 | 0-1 | 0-1
DHCPMSG-Server-IP | 0 | 0 | 0-1 | 0 | 0 | 0
DHCP-RK | 0 | 0 | 0-1 | 0 | 0 | 0
DHCP-RK-Key-ID | 0 | 0 | 0-1 | 0 | 0 | 0
DHCP-RK-Lifetime | 0 | 0 | 0-1 | 0 | 0 | 0
EAP-Message | 1+ | 1+ | 1+ | 0 | 0 | 0
Error-Cause | 0 | 0-1 | 0 | 0 | 0 | 0
Framed-Interface-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Framed-IP-Address | 0 | 0 | 0-1 | 1 | 1 | 1
Framed-IP-Netmask | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Framed-IPv6-Prefix | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Framed-MTU | 0-1 | 0 | 0 | 0 | 0 | 0
HA-IP-MIP4 | 0 | 0 | 0 | 1 | 1 | 1
HA-IP-MIP6 | 0 | 0 | 0 | 1 | 1 | 1
Hotline-Indicator | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Hotline-Profile-ID | 0 | 0 | 0-1 | 0 | 0 | 0
Hotline-Session-Timer | 0 | 0 | 0-1 | 0 | 0 | 0
HTTP-Redirection-Rule | 0 | 0 | 0+ | 0 | 0 | 0
IP-Redirection-Rule | 0 | 0 | 0+ | 0 | 0 | 0
MSK | 0 | 0 | 0-1 | 0 | 0 | 0
NAS-Port-Type | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
PMIP6-RK-KEY | 0 | 0 | 0-1 | 0 | 0 | 0
PMIP6-RK-SPI | 0 | 0 | 0-1 | 0 | 0 | 0
PMIP6-Service-Info | 0-1 | 0 | 0-1 | 0 | 0 | 0
Primary-DNS-Server | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Reply-Message | 0 | 0-1 | 0-1 | 0 | 0 | 0
Secondary-DNS-Server | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Service-Type | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Session-Timeout | 0 | 0-1 | 0-1 | 0 | 0 | 0
SN1-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN1-Prepaid-Compressed-Count | 0 | 0 | 0 | 0 | 0-1 | 0-1
SN1-Primary-DNS-Server | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Proxy-MIP | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Secondary-DNS-Server | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Subscriber-Accounting | 0 | 0 | 0 | 1 | 1 | 1
SN1-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-VPN-Name | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN-Prepaid-Compressed-Count | 0 | 0 | 0 | 0 | 0-1 | 0-1
SN-Primary-DNS-Server | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Proxy-MIP | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Secondary-DNS-Server | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Subscriber-Accounting | 0 | 0 | 0 | 1 | 1 | 1
SN-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-VPN-Name | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-WiMAX-Auth-Only | 0 | 0 | 0-1 | 0 | 0 | 0
State | 0-1 | 0-1 | 0-1 | 0 | 0 | 0
User-Name | 1 | 0 | 0-1 | 1 | 1 | 1
WiMAX-Active-Time | 0 | 0 | 0 | 0 | 0-1 | 0-1
WiMAX-Beginning-Of-Session | 0 | 0 | 0 | 1 | 0 | 0
WiMAX-BS-ID | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
WiMAX-Control-Octets-In | 0 | 0 | 0 | 0 | 0-1 | 0-1
WiMAX-Control-Octets-Out | 0 | 0 | 0 | 0 | 0-1 | 0-1
WiMAX-Control-Packets-In | 0 | 0 | 0 | 0 | 0-1 | 0-1
WiMAX-Control-Packets-Out | 0 | 0 | 0 | 0 | 0-1 | 0-1
WiMAX-Count-Type | 0 | 0 | 0 | 0 | 0-1 | 0-1
WiMAX-Device-Auth-Indicator | 0-1 | 0 | 0 | 0 | 0 | 0
WiMAX-Home-HNP-PMIP6 | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
WiMAX-Home-IPv4-HoA-PMIP6 | 0 | 0 | 0-1 | 1 | 1 | 1
WiMAX-Idle-Mode-Transition | 0 | 0 | 0 | 0 | 0-1 | 0
WiMAX-IP-Technology | 0 | 0 | 0 | 1 | 1 | 1
WiMAX-NAP-ID | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
WiMAX-NSP-ID | 0-1 | 0 | 0 | 0-1 | 0-1 | 0-1
WiMAX-Packet-Flow-Descriptor | 0 | 0 | 0+ | 0 | 0 | 0
WiMAX-Packet-Flow-Descriptor-V2 | 0 | 0 | 0+ | 0 | 0 | 0
WiMAX-PDF-ID | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
WiMAX-Prepaid-Indicator | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
WiMAX-QoS-Descriptor | 0 | 0 | 0+ | 0 | 0 | 0
WiMAX-SDF-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
WiMAX-Session-Continue | 0 | 0 | 0 | 0 | 0 | 1

CSCF Attribute/Packet Table

Attribute | CSCF Access- Request | CSCF Access- Reject | CSCF Access- Accept | CSCF Acct- Request-Start | CSCF Acct- Request-Interim | CSCF Acct- Request-Stop
Called-Station-ID | 0 | 0 | 0 | 1 | 1 | 1
Digest-AKA-Auts | 0-1 | 0 | 0 | 0 | 0 | 0
Digest-Algorithm | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Auth-Param | 0+ | 0 | 0+ | 0 | 0 | 0
Digest-CNonce | 0-1 | 0 | 0 | 0 | 0 | 0
Digest-Domain | 0 | 0 | 0+ | 0 | 0 | 0
Digest-Entity-Body-Hash | 0-1 | 0 | 0 | 0 | 0 | 0
Digest-HA1 | 0 | 0 | 0-1 | 0 | 0 | 0
Digest-Method | 0-1 | 0 | 0 | 0 | 0 | 0
Digest-Nextnonce | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Nonce | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Nonce-Count | 0-1 | 0 | 0 | 0 | 0 | 0
Digest-Opaque | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Qop | 0-1 | 0 | 0+ | 0 | 0 | 0
Digest-Realm | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Response | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Response-Auth | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Stale | 0 | 0 | 0-1 | 0 | 0 | 0
Digest-URI | 0-1 | 0 | 0-1 | 0 | 0 | 0
Digest-Username | 0-1 | 0 | 0 | 0 | 0 | 0
Framed-Interface-Id | 0-1 | 0 | 0-1 | 0 | 0 | 0
Framed-IP-Address | 0-1 | 0 | 0-1 | 0 | 0 | 0
Framed-IPv6-Prefix | 0-1 | 0 | 0-1 | 0 | 0 | 0
NAS-Port-Type | 1 | 0 | 0 | 1 | 1 | 1
SIP-AOR | 0-1 | 0 | 0 | 0 | 0 | 0
SN-Cause-Code | 0 | 0 | 0 | 0 | 0 | 0-1
SN-CF-Call-International | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Call-Local | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Call-LongDistance | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Call-Premium | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Call-RoamingInternatnl | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Call-Transfer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Call-Waiting | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-CId-Display | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-CId-Display-Blocked | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Follow-Me | 0 | 0 | 0+ | 0 | 0 | 0
SN-CF-Forward-Busy-Line | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Forward-No-Answer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Forward-Not-Regd | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CF-Forward-Unconditional | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Content-Disposition | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Content-Length | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Content-Type | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-CR-International-Cid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-CR-LongDistance-Cid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Cscf-Subscriber-Ip-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Event | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-GGSN-Address | 0 | 0 | 0 | 0-1 | 0-1 | 0
SN-IMS-Charging-Identifier | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-ISC-Template-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Is-Unregistered-Subscriber | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Node-Functionality | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Originating-IOI | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Role-Of-Node | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-SDP-Session-Description | 0 | 0 | 0 | 0-1 | 0-1 | 0
SN-Session-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-SIP-Method | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-SIP-Request-Time-Stamp | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-SIP-Response-Time-Stamp | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Terminating-IOI | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
State | 0-1 | 0 | 0-1 | 0 | 0 | 0
User-Name | 1 | 0 | 0 | 1 | 1 | 1
WiMAX-Home-HNP-PMIP6 | 0-1 | 0 | 0-1 | 0 | 0 | 0
WiMAX-Home-IPv4-HoA-PMIP6 | 0-1 | 0 | 0-1 | 0 | 0 | 0

MIPv6HA Attribute/Packet Table

Attribute | MIPv6HA Access -Request | MIPv6HA Access -Reject | MIPv6HA Access -Accept | MIPv6HA Acct -Request-Start | MIPv6HA Acct -Request-Interim | MIPv6HA Acct -Request-Stop
3GPP2-Comp-Tunnel-Indicator | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Correlation-Id | 1 | 0 | 0 | 1 | 1 | 1
3GPP2-DNS-Update-Required | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-ESN | 1 | 0 | 0 | 0 | 0 | 0
3GPP2-IP-QOS | 0 | 0 | 0-1 | 1 | 1 | 1
3GPP2-IP-Technology | 0-1 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MEID | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP6-Authenticator | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-CoA | 0-1 | 0 | 0 | 0-1 | 0-1 | 0
3GPP2-MIP6-HA | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-HoA | 0-1 | 0 | 0 | 0-1 | 0-1 | 0
3GPP2-MIP6-HoA-Not-Authorized | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MIP6-MAC-Mobility-Data | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-Mesg-ID | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-MIP6-Session-Key | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MN-HA-Shared-Key | 0 | 0 | 0-1 | 0 | 0 | 0
3GPP2-MN-HA-SPI | 0-1 | 0 | 0 | 0 | 0 | 0
3GPP2-Mobile-Term-Orig-Ind | 0 | 0 | 0 | 1 | 1 | 1
3GPP2-Serving-PCF | 0 | 0 | 0 | 1 | 1 | 1
AAA-Session-ID | 0-1 | 0 | 1 | 0 | 0 | 0
Acct-Authentic | 0 | 0 | 0 | 1 | 1 | 1
Acct-Input-Packets | 0-1 | 0 | 0 | 0 | 1 | 1
Acct-Interim-Interval | 0 | 0 | 0-1 | 0 | 0 | 0
Acct-Multi-Session-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Acct-Output-Packets | 0-1 | 0 | 0 | 0 | 1 | 1
Acct-Session-Id | 0 | 0 | 0 | 1 | 1 | 1
BU-CoA-Ipv6 | 0-1 | 0 | 0 | 0 | 0 | 0
Calling-Station-Id | 1 | 0 | 1 | 1 | 1 | 1
Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
CUI | 0-1 | 0 | 0-1 | 0 | 0 | 0
Error-Cause | 0 | 0-1 | 0 | 0 | 0 | 0
Framed-Interface-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
Framed-IPv6-Pool | 0 | 0 | 0-1 | 0 | 0 | 0
Framed-IPv6-Prefix | 0 | 0 | 0 | 0+ | 0+ | 0+
Framed-MTU | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
Framed-Pool | 0 | 0 | 0+ | 0 | 0 | 0
HA-IP-MIP4 | 1 | 0 | 0 | 1 | 1 | 1
HA-IP-MIP6 | 1 | 0 | 0 | 1 | 1 | 1
HA-RK-KEY | 0 | 0 | 0-1 | 0 | 0 | 0
HA-RK-Lifetime | 0 | 0 | 0-1 | 0 | 0 | 0
HA-RK-SPI | 0-1 | 0 | 0-1 | 0 | 0 | 0
hLMA-IPv6-PMIP6 | 0-1 | 0 | 0 | 0 | 0 | 0
Idle-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
MN-HA-MIP4-KEY | 0 | 0 | 1 | 0 | 0 | 0
MN-HA-MIP4-SPI | 1 | 0 | 1 | 0 | 0 | 0
MN-HA-MIP6-KEY | 0 | 0 | 0-1 | 0 | 0 | 0
MN-HA-MIP6-SPI | 0 | 0 | 0-1 | 0 | 0 | 0
NAS-Port | 1 | 0 | 0 | 1 | 1 | 1
NAS-Port-Type | 1 | 0 | 0 | 1 | 1 | 1
PMIP6-RK-KEY | 0 | 0 | 0-1 | 0 | 0 | 0
PMIP6-RK-SPI | 0-1 | 0 | 0 | 0 | 0 | 0
Reply-Message | 0 | 0-1 | 0-1 | 0 | 0 | 0
RRQ-HA-IP | 0-1 | 0 | 0 | 0 | 0 | 0
RRQ-MN-HA-KEY | 0 | 0 | 0-1 | 0 | 0 | 0
Service-Type | 1 | 0 | 0-1 | 1 | 1 | 1
Session-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Assigned-VLAN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN1-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN1-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN1-FMC-Location | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Gratuitous-ARP-Aggressive | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Ignore-Unknown-HA-Addr-Err | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IMS-AM-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IMS-AM-Domain-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Pool-Name | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN1-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN1-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN1-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Mediation-Enabled | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Mediation-VPN-Name | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-MIP-ANCID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-MIP-Dual-Anchor | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN1-MIP-Reg-Lifetime-Realm | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-MN-HA-Timestamp-Tolerance | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Nw-Reachability-Server-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-PDSN-Correlation-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-PDSN-NAS-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-PDSN-NAS-IP-Address | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN1-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Compressed-Count | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Final-Duration-Alg | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Inbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Outbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Total-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Prepaid-Watermark | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN1-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Re-CHAP-Interval | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN1-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Unclassify-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-Voice-Push-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN1-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN1-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
SN-Access-link-IP-Frag | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Acs-Credit-Control-Group | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Admin-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Assigned-VLAN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Bandwidth-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CBB-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-CFPolicy-ID | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Data-Tunnel-Ignore-DF-Bit | 0 | 0 | 0-1 | 0 | 0 | 0
SN-DHCP-Lease-Expiry-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Disconnect-Reason | 0 | 0 | 0 | 0 | 0 | 1
SN-DNS-Proxy-Intercept-List | 0 | 0 | 1 | 0 | 0 | 0
SN-Enable-QoS-Renegotiation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Context | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Down-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-Addr | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ext-Inline-Srvr-Up-VLAN | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Firewall-Enabled | 0 | 0 | 0 | 1 | 1 | 1
SN-Firewall-Policy | 0 | 0 | 1 | 0 | 0 | 0
SN-FMC-Location | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Gratuitous-ARP-Aggressive | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Ignore-Unknown-HA-Addr-Error | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IMS-AM-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IMS-AM-Domain-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Inactivity-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Filter-In | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Filter-Out | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Hide-Service-Address | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Pool-Name | 0 | 0 | 0+ | 0 | 0 | 0
SN-IP-Source-Validation | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IP-Source-Violate-No-Acct | 0 | 0 | 0-1 | 0 | 0 | 0
SN-IPv6-Sec-Pool | 0 | 0 | 0+ | 0 | 0 | 0
SN-IPv6-Sec-Prefix | 0 | 0 | 0+ | 0 | 0 | 0
SN-L3-to-L2-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Local-IP-Address | 0-1 | 0 | 0-1 | 1 | 1 | 1
SN-Long-Duration-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Notification | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Long-Duration-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Mediation-Enabled | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Mediation-VPN-Name | 0 | 0 | 0-1 | 1 | 1 | 1
SN-MIP-ANCID | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-MIP-Dual-Anchor | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MIP-HA-Assignment-Table | 0 | 0 | 1 | 0 | 0 | 0
SN-MIP-Reg-Lifetime-Realm | 0 | 0 | 0-1 | 0 | 0 | 0
SN-MN-HA-Timestamp-Tolerance | 0 | 0 | 0-1 | 0 | 0 | 0
SN-NPU-Qos-Priority | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Nw-Reachability-Server-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Connect-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disc-Inact-Time | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Overload-Disconnect | 0 | 0 | 0-1 | 0 | 0 | 0
SN-PDSN-Correlation-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-PDSN-NAS-Id | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-PDSN-NAS-IP-Address | 0 | 0 | 0 | 0-1 | 0-1 | 0-1
SN-Permit-User-Mcast-PDUs | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Compressed-Count | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Final-Duration-Alg | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Inbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Outbound-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Timeout | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Total-Octets | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Prepaid-Watermark | 0-1 | 0 | 0-1 | 0 | 0 | 0
SN-Primary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Background-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Conversation-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive1-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive2-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Interactive3-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Renegotiation-Timeout | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Streaming-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Dnlk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-QoS-Tp-Uplk | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Re-CHAP-Interval | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Rulebase | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Secondary-DCCA-Peer | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Accounting | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-Acct-Interim | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Mode | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Rsp-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Start | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Acct-Stop | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Class | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-Subscriber-IP-TOS-Copy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Nexthop-Address | 0 | 0 | 0-1 | 1 | 1 | 1
SN-Subscriber-No-Interims | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subscriber-Permission | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Subs-IMSA-Service-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Dnlk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Burst-Size | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Committed-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Exceed-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Peak-Data-Rate | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tp-Uplk-Violate-Action | 0 | 0 | 0-1 | 0 | 0 | 0
SN-TrafficSelector-Class | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tun-Addr-Policy | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Crypto-Map | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-ISAKMP-Secret | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Tunnel-Load-Balancing | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Unclassify-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-Voice-Push-List-Name | 0 | 0 | 0-1 | 0 | 0 | 0
SN-VPN-ID | 0 | 0 | 0-1 | 0-1 | 0-1 | 0-1
SN-VPN-Name | 0 | 0 | 1 | 0-1 | 0-1 | 0-1
State | 1 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Assignment-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Client-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Medium-Type | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Preference | 0 | 0 | 0-1 | 0 | 0 | 0
Tunnel-Private-Group-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Auth-ID | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Server-Endpoint | 0 | 0 | 0-1 | 1 | 1 | 1
Tunnel-Type | 0 | 0 | 0-1 | 1 | 1 | 1
User-Name | 1 | 0 | 0-1 | 1 | 1 | 1
WiMAX-Count-Type | 0-1 | 0 | 0-1 | 0 | 0 | 0
WiMAX-Home-HNP-PMIP6 | 0 | 0 | 0 | 0+ | 0+ | 0+
WiMAX-Home-IPv4-HoA-PMIP6 | 0 | 0 | 0 | 0 | 1 | 0
WiMAX-IP-Technology | 0-1 | 0 | 0-1 | 0 | 0 | 0
WiMAX-Prepaid-Indicator | 0 | 0 | 0 | 0-1 | 0-1 | 0-1

Dictionary Quick Reference

Attribute | standard | 3gpp | 3gpp2 | 3gpp2-835 | starent | starent-835 | starent-vsa1 | starent-vsa1-835
3GPP2-835-Release-Indicator | No | No | No | Yes | No | Yes | No | Yes
3GPP2-Acct-Session-Time | No | No | No | Yes | No | Yes | No | Yes
3GPP2-Active-Time | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Active-Time-Corrected | No | No | No | No | No | No | No | No
3GPP2-Airlink-Record-Type | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Airlink-Sequence-Number | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Air-QOS | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Allowed-Diffserv | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Allowed-Persistent-TFTs | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Alternate-Billing-ID | No | No | No | Yes | No | Yes | No | Yes
3GPP2-Always-On | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Auth-Flow-Profile-Id | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Bad-PPP-Frame-Count | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Auth-Parameters | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-BSN-Session-Info | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Capability | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Common-Session-Info | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Flow-ID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Flow-Transmit-Time | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Mcast-IP-Addr | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Mcast-Port | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-Reason-Code | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BCMCS-RN-Session-Info | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Beginning-Session | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-BSID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Carrier-ID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Comp-Tunnel-Indicator | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Container | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Correlation-Id | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Correlation-Id-Long | No | No | No | No | No | No | No | No
3GPP2-Correlation-Id-Old | No | No | No | No | No | No | No | No
3GPP2-DCCH-Frame-Size | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Diff-Service-Class-Option | No | No | No | No | No | No | No | No
3GPP2-Disconnect-Reason | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-DNS-Server-IP-Address | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-DNS-Update-Required | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-ESN | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-FA-Address | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Flow-Id | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Flow-Status | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Forward-Fundamental-Rate | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Forward-Fundamental-RC | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Forward-Mux-Option | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Forward-Traffic-Type | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Fundamental-Frame-Size | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Fwd-Dcch-Mux-Option | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Fwd-Dcch-Rc | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Fwd-Pdch-Rc | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-GMT-Timezone-Offset | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Granted-QoS | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-IKE-Secret | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-IKE-Secret-Request | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-IKE-Secret-Unencrypted | No | No | No | No | No | No | No | No
3GPP2-IMSI | No | No | No | No | No | No | No | No
3GPP2-Interconnect-IP | No | No | No | Yes | No | Yes | No | Yes
3GPP2-Interconnect-QOS | No | No | No | Yes | No | Yes | No | Yes
3GPP2-Inter-User-Priority | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-IP-QOS | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-IP-Technology | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-KeyID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Last-Activity | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Max-Auth-Aggr-Bw-BET | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Max-Per-Fl-Pri-ForTheUser | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MEID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-Authenticator | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-CoA | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-HA | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-HoA | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-HoA-Not-Authorized | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-Home-Address | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-Home-Agent | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-Home-Link-Prefix | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-MAC-Mobility-Data | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-Mesg-ID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP6-Session-Key | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP-HA-Address | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP-Lifetime | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP-Rev-Tunnel-Required | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP-Sig-Octet-Count-In | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MIP-Sig-Octet-Count-Out | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MN-AAA-Removal-Indication | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MN-HA-Shared-Key | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-MN-HA-Shared-Key-No-Enc | No | No | No | No | No | No | No | No
3GPP2-MN-HA-SPI | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Mobile-Term-Orig-Ind | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Number-Active-Transitions | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Num-Bytes-Received-Total | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Num-SDB-Input | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Num-SDB-Output | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Pre-Paid-Accounting-Quota | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Pre-Paid-Acct-Capability | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Pre-Paid-TariffSwitch | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-QoS-Service-Opt-Profile | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Release-Indicator | No | No | Yes | No | Yes | No | Yes | No
3GPP2-Release-Indicator-custom9 | No | No | No | No | No | No | No | No
3GPP2-Release-Indicator-Old | No | No | No | No | No | No | No | No
3GPP2-Release-Indicator-Prepaid | No | No | No | No | Yes | No | Yes | No
3GPP2-Remote-Addr-Table-Idx-Old | No | No | No | Yes | No | Yes | No | Yes
3GPP2-Remote-Addr-Table-Index | No | No | Yes | No | Yes | No | Yes | No
3GPP2-Remote-IPv4-Address | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Remote-IPv4-Addr-Octets | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rev-Dcch-Mux-Option | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rev-Dcch-Rc | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Reverse-Fundamental-Rate | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Reverse-Fundamental-RC | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Reverse-Mux-Option | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Reverse-Traffic-Type | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rev-Pdch-Rc | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-RP-Session-ID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rsvp-Signal-In-Count | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rsvp-Signal-In-Packets | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rsvp-Signal-Out-Count | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Rsvp-Signal-Out-Packets | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-SDB-Input-Octets | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-SDB-Output-Octets | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Security-Level | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Service-Option | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Service-Option-Profile | No | No | No | No | No | No | No | No
3GPP2-Service-Reference-ID | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Serving-PCF | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Session-Continue | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Session-Term-Capability | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-S-Key | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-S-Lifetime | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-S-Request | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-Subnet | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP2-S-Unencrypted | No | No | No | No | No | No | No | No
3GPP2-User-Zone | No | No | Yes | Yes | Yes | Yes | Yes | Yes
3GPP-CAMEL-Charging-Info | No | Yes | No | No | Yes | No | Yes | No
3GPP-CG-Address | No | Yes | No | No | Yes | No | Yes | No
3GPP-Charging-Id | No | Yes | No | No | Yes | No | Yes | No
3GPP-Chrg-Char | No | Yes | No | No | Yes | No | Yes | No
3GPP-GGSN-Address | No | Yes | No | No | Yes | No | Yes | No
3GPP-GGSN-Mcc-Mnc | No | Yes | No | No | Yes | No | Yes | No
3GPP-IMEISV | No | Yes | No | No | Yes | No | Yes | No
3GPP-IMSI | No | Yes | No | No | Yes | No | Yes | No
3GPP-IMSI-Mcc-Mnc | No | Yes | No | No | Yes | No | Yes | No
3GPP-MS-TimeZone | No | Yes | No | No | Yes | No | Yes | No
3GPP-Negotiated-DSCP | No | Yes | No | No | Yes | No | Yes | No
3GPP-Negotiated-QoS-Profile | No | Yes | No | No | Yes | No | Yes | No
3GPP-NSAPI | No | Yes | No | No | Yes | No | Yes | No
3GPP-Packet-Filter | No | Yes | No | No | Yes | No | Yes | No
3GPP-PDP-Type | No | Yes | No | No | Yes | No | Yes | No
3GPP-RAT-Type | No | Yes | No | No | Yes | No | Yes | No
3GPP-Selection-Mode | No | Yes | No | No | Yes | No | Yes | No
3GPP-Session-Stop-Ind | No | Yes | No | No | Yes | No | Yes | No
3GPP-SGSN-Address | No | Yes | No | No | Yes | No | Yes | No
3GPP-SGSN-Mcc-Mnc | No | Yes | No | No | Yes | No | Yes | No
3GPP-Teardown-Indicator | No | Yes | No | No | Yes | No | Yes | No
3GPP-User-Location-Info | No | Yes | No | No | Yes | No | Yes | No
AAA-Session-ID | No | No | No | No | Yes | No | Yes | No
Access-IN-Subs | No | No | No | No | No | No | No | No
Acct-Authentic | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Delay-Time | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Input-Gigawords | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Input-Octets | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Input-Packets | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Interim-Interval | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Link-Count | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Multi-Session-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Output-Gigawords | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Output-Octets | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Output-Packets | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Session-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Session-Id-Long | No | No | No | No | No | No | No | No
Acct-Session-Time | Yes | Yes | Yes | No | Yes | Yes | Yes | Yes
Acct-Status-Type | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Termination-Cause | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Tunnel-Connection | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Acct-Tunnel-Packets-Lost | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
ARAP-Challenge-Response | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
ARAP-Features | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
ARAP-Password | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
ARAP-Security | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
ARAP-Security-Data | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
ARAP-Zone-Access | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
BU-CoA-Ipv6 | No | No | No | No | Yes | No | Yes | No
Callback-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Callback-Number | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Called-Station-ID | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Calling-Station-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Calling-Subscriber-Type | No | No | No | No | No | No | No | No
CHAP-Challenge | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
CHAP-Password | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Charging-Id | No | No | No | No | No | No | No | No
Charging-Rules-Name | No | No | No | No | No | No | No | No
Charging-Server | No | No | No | No | No | No | No | No
Charging-Type | No | No | No | No | No | No | No | No
Class | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Configuration-Token | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Connect-Info | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
CS-AVPair | No | No | No | No | Yes | Yes | Yes | Yes
CS-Prepaid-Quota | No | No | No | No | Yes | Yes | Yes | Yes
CS-Prepaid-Time-Quota | No | No | No | No | Yes | Yes | Yes | Yes
CS-Prepaid-Volume-Quota | No | No | No | No | Yes | Yes | Yes | Yes
CS-Service-Name | No | No | No | No | Yes | Yes | Yes | Yes
CUI | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Custom-Correlation-Id | No | No | No | No | No | No | No | No
Custom-Prepaid-Ind | No | No | No | No | No | No | No | No
Custom-Primary-OCS | No | No | No | No | No | No | No | No
Custom-Requested-APN | No | No | No | No | No | No | No | No
Custom-Secondary-OCS | No | No | No | No | No | No | No | No
Custom-Session-Access-Method | No | No | No | No | No | No | No | No
Custom-Session-Charging-Type | No | No | No | No | No | No | No | No
DHCPMSG-Server-IP | No | No | No | No | Yes | No | Yes | No
DHCP-RK | No | No | No | No | Yes | No | Yes | No
DHCP-RK-Key-ID | No | No | No | No | Yes | No | Yes | No
DHCP-RK-Lifetime | No | No | No | No | Yes | No | Yes | No
Digest-AKA-Auts | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Algorithm | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Auth-Param | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-CNonce | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Domain | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Entity-Body-Hash | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-HA1 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Method | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Nextnonce | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Nonce | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Nonce-Count | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Opaque | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Qop | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Realm | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Response | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Response-Auth | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Stale | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-URI | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Digest-Username | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
DNS | No | No | No | No | Yes | No | Yes | No
Draft5-Digest-Response | No | No | No | No | No | No | No | No
DSCP_IP_Address | No | No | No | No | No | No | No | No
EAP-Message | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Ecs-List-of-Service-Data | No | No | No | No | No | No | No | No
Error-Cause | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Event-Timestamp | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
FA-RK-KEY | No | No | No | No | Yes | No | Yes | No
FA-RK-SPI | No | No | No | No | Yes | No | Yes | No
Filter-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-AppleTalk-Link | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-AppleTalk-Network | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-AppleTalk-Zone | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-Compression | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-Interface-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-IP-Address | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-IP-Netmask | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-IPv6-Pool | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-IPv6-Prefix | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-IPv6-Route | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-IPX-Network | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-MTU | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-Pool | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-Protocol | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-Route | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Framed-Routing | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
GGSN-GTP-IP-Address | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
GGSN-IP-Address | No | No | No | No | No | No | No | No
GMT-Time-Zone-Offset | No | No | No | No | Yes | No | Yes | No
HA-IP-MIP4 | No | No | No | No | Yes | No | Yes | No
HA-IP-MIP6 | No | No | No | No | Yes | No | Yes | No
HA-RK-KEY | No | No | No | No | Yes | No | Yes | No
HA-RK-Lifetime | No | No | No | No | Yes | No | Yes | No
HA-RK-SPI | No | No | No | No | Yes | No | Yes | No
hLMA-IPv6-PMIP6 | No | No | No | No | Yes | No | Yes | No
Hotline-Indicator | No | No | No | No | Yes | No | Yes | No
Hotline-Profile-ID | No | No | No | No | Yes | No | Yes | No
Hotline-Session-Timer | No | No | No | No | Yes | No | Yes | No
HTTP-Redirection-Rule | No | No | No | No | Yes | No | Yes | No
Idle-Timeout | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
IMSI | No | No | No | No | No | No | No | No
IMSI-MCC-MNC | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
IN-Packet-Period | No | No | No | No | No | No | No | No
Intelligent-Network-Service-Key | No | No | No | No | No | No | No | No
IN-Time-Period | No | No | No | No | No | No | No | No
IP-Redirection-Rule | No | No | No | No | Yes | No | Yes | No
KTF_VSA1 | No | No | No | No | No | No | No | No
KTF_VSA2 | No | No | No | No | No | No | No | No
Login-IP-Host | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-IPv6-Host | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-LAT-Group | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-LAT-Node | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-LAT-Port | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-LAT-Service | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-Service | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Login-TCP-Port | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Message-Authenticator | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MN-HA-MIP4-KEY | No | No | No | No | Yes | No | Yes | No
MN-HA-MIP4-SPI | No | No | No | No | Yes | No | Yes | No
MN-HA-MIP6-KEY | No | No | No | No | Yes | No | Yes | No
MN-HA-MIP6-SPI | No | No | No | No | Yes | No | Yes | No
MS-CHAP-Challenge | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MS-CHAP-Domain | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MS-CHAP-Error | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MS-CHAP-Response | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MSISDN | No | No | No | No | No | No | No | No
MSK | No | No | No | No | Yes | No | Yes | No
MS-MPPE-Recv-Key | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MS-MPPE-Send-Key | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MS-Primary-DNS-Server | No | No | No | No | No | No | Yes | No
MS-Primary-NBNS-Server | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
MS-Secondary-DNS-Server | No | No | No | No | No | No | Yes | No
MS-Secondary-NBNS-Server | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-Filter-Rule | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-Identifier | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-IP-Address | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-IPv6-Address | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-Port | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-Port-Id | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NAS-Port-Type | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
NEtype | No | No | No | No | No | No | No | No
Password-Retry | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
PMA-Capability-Indicator | No | No | No | No | No | No | No | No
PMA-Indicator | No | No | No | No | No | No | No | No
PMIP6-RK-KEY | No | No | No | No | Yes | No | Yes | No
PMIP6-RK-SPI | No | No | No | No | Yes | No | Yes | No
PMIP6-Service-Info | No | No | No | No | Yes | No | Yes | No
PMIP-Authenticated-Nwk-Id | No | No | No | No | Yes | No | Yes | No
Port-Limit | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Prepaid-Ind | No | No | No | No | No | No | No | No
Preservation-Indicator | No | No | No | No | No | No | No | No
Price-Plan | No | No | No | No | No | No | No | No
Primary-DNS-Server | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Prohibit-Payload-Compression | No | No | No | No | Yes | Yes | No | No
Prohibit-Payload-Compression1 | No | No | No | No | No | No | Yes | Yes
Prompt | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Proxy-State | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Reply-Message | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
RRQ-HA-IP | No | No | No | No | Yes | No | Yes | No
RRQ-MN-HA-KEY | No | No | No | No | Yes | No | Yes | No
Secondary-DNS-Server | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Selection-Mode | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Served-MDN | No | No | No | No | No | No | No | No
Service-Type | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Session-Timeout | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
SGSN-IP-Address | No | No | No | No | No | No | No | No
SIP-AOR | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
SN1-Access-link-IP-Frag | No | No | No | No | No | No | Yes | Yes
SN1-Acct-Input-Giga-Dropped | No | No | No | No | No | No | Yes | Yes
SN1-Acct-Input-Octets-Dropped | No | No | No | No | No | No | Yes | Yes
SN1-Acct-Input-Packets-Dropped | No | No | No | No | No | No | Yes | Yes
SN1-Acct-Output-Giga-Dropped | No | No | No | No | No | No | Yes | Yes
SN1-Acct-Output-Octets-Dropped | No | No | No | No | No | No | Yes | Yes
SN1-Acct-Output-Packets-Dropped | No | No | No | No | No | No | Yes | Yes
SN1-Admin-Expiry | No | No | No | No | No | No | Yes | Yes
SN1-Admin-Permission | No | No | No | No | No | No | Yes | Yes
SN1-Assigned-VLAN-ID | No | No | No | No | No | No | Yes | Yes
SN1-Call-Id | No | No | No | No | No | No | Yes | Yes
SN1-Cause-For-Rec-Closing | No | No | No | No | No | No | Yes | Yes
SN1-CFPolicy-ID | No | No | No | No | No | No | Yes | Yes
SN1-Change-Condition | No | No | No | No | No | No | Yes | Yes
SN1-Charging-VPN-Name | No | No | No | No | No | No | Yes | Yes
SN1-Chrg-Char-Selection-Mode | No | No | No | No | No | No | Yes | Yes
SN1-Data-Tunnel-Ignore-DF-Bit | No | No | No | No | No | No | Yes | Yes
SN1-DHCP-Lease-Expiry-Policy | No | No | No | No | No | No | Yes | Yes
SN1-Disconnect-Reason | No | No | No | No | No | No | Yes | Yes
SN1-DNS-Proxy-Intercept-List | No | No | No | No | No | No | Yes | Yes
SN1-DNS-Proxy-Use-Subscr-Addr | No | No | No | No | No | No | Yes | Yes
SN1-Dynamic-Addr-Alloc-Ind-Flag | No | No | No | No | No | No | Yes | Yes
SN1-Ecs-Data-Volume | No | No | No | No | No | No | Yes | Yes
SN1-Enable-QoS-Renegotiation | No | No | No | No | No | No | Yes | Yes
SN1-Ext-Inline-Srvr-Context | No | No | No | No | No | No | Yes | Yes
SN1-Ext-Inline-Srvr-Down-Addr | No | No | No | No | No | No | Yes | Yes
SN1-Ext-Inline-Srvr-Down-VLAN | No | No | No | No | No | No | Yes | Yes
SN1-Ext-Inline-Srvr-Preference | No | No | No | No | No | No | Yes | Yes
SN1-Ext-Inline-Srvr-Up-Addr | No | No | No | No | No | No | Yes | Yes
SN1-Ext-Inline-Srvr-Up-VLAN | No | No | No | No | No | No | Yes | Yes
SN1-Firewall-Enabled | No | No | No | No | No | No | Yes | Yes
SN1-FMC-Location | No | No | No | No | No | No | Yes | Yes
SN1-GGSN-MIP-Required | No | No | No | No | No | No | Yes | Yes
SN1-Gratuitous-ARP-Aggressive | No | No | No | No | No | No | Yes | Yes
SN1-GTP-Version | No | No | No | No | No | No | Yes | Yes
SN1-HA-Send-DNS-Address | No | No | No | No | No | No | Yes | Yes
SN1-Home-Behavior | No | No | No | No | No | No | Yes | Yes
SN1-Home-Profile | No | No | No | No | No | No | Yes | Yes
SN1-Home-Sub-Use-GGSN | No | No | No | No | No | No | Yes | Yes
SN1-Ignore-Unknown-HA-Addr-Err | No | No | No | No | No | No | Yes | Yes
SN1-IMS-AM-Address | No | No | No | No | No | No | Yes | Yes
SN1-IMS-AM-Domain-Name | No | No | No | No | No | No | Yes | Yes
SN1-IMSI | No | No | No | No | No | No | Yes | Yes
SN1-Inactivity-Time | No | No | No | No | No | No | Yes | Yes
SN1-Internal-SM-Index | No | No | No | No | No | No | Yes | Yes
SN1-IP-Alloc-Method | No | No | No | No | No | No | Yes | Yes
SN1-IP-Filter-In | No | No | No | No | No | No | Yes | Yes
SN1-IP-Filter-Out | No | No | No | No | No | No | Yes | Yes
SN1-IP-Header-Compression | No | No | No | No | No | No | Yes | Yes
SN1-IP-Hide-Service-Address | No | No | No | No | No | No | Yes | Yes
SN1-IP-In-ACL | No | No | No | No | No | No | Yes | Yes
SN1-IP-In-Plcy-Grp | No | No | No | No | No | No | Yes | Yes
SN1-IP-Out-ACL | No | No | No | No | No | No | Yes | Yes
SN1-IP-Out-Plcy-Grp | No | No | No | No | No | No | Yes | Yes
SN1-IP-Pool-Name | No | No | No | No | No | No | Yes | Yes
SN1-IP-Source-Validation | No | No | No | No | No | No | Yes | Yes
SN1-IP-Source-Violate-No-Acct | No | No | No | No | No | No | Yes | Yes
SN1-IP-Src-Valid-Drop-Limit | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-DNS-Proxy | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-Egress-Filtering | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-Min-Link-MTU | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-num-rtr-advt | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-Primary-DNS | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-rtr-advt-interval | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-Secondary-DNS | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-Sec-Pool | No | No | No | No | No | No | Yes | Yes
SN1-IPv6-Sec-Prefix | No | No | No | No | No | No | Yes | Yes
SN1-L3-to-L2-Tun-Addr-Policy | No | No | No | No | No | No | Yes | Yes
SN1-Local-IP-Address | No | No | No | No | No | No | Yes | Yes
SN1-Long-Duration-Action | No | No | No | No | No | No | Yes | Yes
SN1-Long-Duration-Notification | No | No | No | No | No | No | Yes | Yes
SN1-Long-Duration-Timeout | No | No | No | No | No | No | Yes | Yes
SN1-Mediation-Acct-Rsp-Action | No | No | No | No | No | No | Yes | Yes
SN1-Mediation-Enabled | No | No | No | No | No | No | Yes | Yes
SN1-Mediation-No-Interims | No | No | No | No | No | No | Yes | Yes
SN1-Mediation-VPN-Name | No | No | No | No | No | No | Yes | Yes
SN1-Min-Compress-Size | No | No | No | No | No | No | Yes | Yes
SN1-MIP-AAA-Assign-Addr | No | No | No | No | No | No | Yes | Yes
SN1-MIP-ANCID | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Dual-Anchor | No | No | No | No | No | No | Yes | Yes
SN1-MIP-HA-Assignment-Table | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Match-AAA-Assign-Addr | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Reg-Lifetime-Realm | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Send-Ancid | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Send-Correlation-Info | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Send-Imsi | No | No | No | No | No | No | Yes | Yes
SN1-MIP-Send-Term-Verification | No | No | No | No | No | No | Yes | Yes
SN1-MN-HA-Hash-Algorithm | No | No | No | No | No | No | Yes | Yes
SN1-MN-HA-Timestamp-Tolerance | No | No | No | No | No | No | Yes | Yes
SN1-MS-ISDN | No | No | No | No | No | No | Yes | Yes
SN1-NAI-Construction-Domain | No | No | No | No | No | No | Yes | Yes
SN1-NAT-Bind-Record | No | No | No | No | No | No | Yes | Yes
SN1-NAT-Info-Record | No | No | No | No | No | No | Yes | Yes
SN1-NAT-IP-Address | No | No | No | No | No | No | Yes | Yes
SN1-NAT-IP-Address-Old | No | No | No | No | No | No | Yes | Yes
SN1-NPU-Qos-Priority | No | No | No | No | No | No | Yes | Yes
SN1-Ntk-Initiated-Ctx-Ind-Flag | No | No | No | No | No | No | Yes | Yes
SN1-Ntk-Session-Disconnect-Flag | No | No | No | No | No | No | Yes | Yes
SN1-Nw-Reachability-Server-Name | No | No | No | No | No | No | Yes | Yes
SN1-Overload-Disc-Connect-Time | No | No | No | No | No | No | Yes | Yes
SN1-Overload-Disc-Inact-Time | No | No | No | No | No | No | Yes | Yes
SN1-Overload-Disconnect | No | No | No | No | No | No | Yes | Yes
SN1-PDIF-MIP-Release-TIA | No | No | No | No | No | No | Yes | Yes
SN1-PDIF-MIP-Required | No | No | No | No | No | No | Yes | Yes
SN1-PDIF-MIP-Simple-IP-Fallback | No | No | No | No | No | No | Yes | Yes
SN1-PDSN-Correlation-Id | No | No | No | No | No | No | Yes | Yes
SN1-PDSN-Handoff-Req-IP-Addr | No | No | No | No | No | No | Yes | Yes
SN1-PDSN-NAS-Id | No | No | No | No | No | No | Yes | Yes
SN1-PDSN-NAS-IP-Address | No | No | No | No | No | No | Yes | Yes
SN1-Permit-User-Mcast-PDUs | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Accept-Peer-v6Ifid | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Always-On-Vse | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Data-Compression | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Data-Compression-Mode | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Keepalive | No | No | No | No | No | No | Yes | Yes
SN1-PPP-NW-Layer-IPv4 | No | No | No | No | No | No | Yes | Yes
SN1-PPP-NW-Layer-IPv6 | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Outbound-Password | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Outbound-Username | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Progress-Code | No | No | No | No | No | No | Yes | Yes
SN1-PPP-Reneg-Disc | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Compressed-Count | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Final-Duration-Alg | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Inbound-Octets | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Outbound-Octets | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Preference | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Profile | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Timeout | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Total-Octets | No | No | No | No | No | No | Yes | Yes
SN1-Prepaid-Watermark | No | No | No | No | No | No | Yes | Yes
SN1-Primary-DCCA-Peer | No | No | No | No | No | No | Yes | Yes
SN1-Primary-DNS-Server | No | No | No | No | No | No | Yes | Yes
SN1-Primary-NBNS-Server | No | No | No | No | No | No | Yes | Yes
SN1-Proxy-MIP | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Background-Class | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Class-Background-PHB | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Class-Converstional-PHB | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Class-Interactive-1-PHB | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Class-Interactive-2-PHB | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Class-Interactive-3-PHB | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Class-Streaming-PHB | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Conversation-Class | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Interactive1-Class | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Interactive2-Class | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Interactive3-Class | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Negotiated | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Renegotiation-Timeout | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Streaming-Class | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Tp-Dnlk | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Tp-Uplk | No | No | No | No | No | No | Yes | Yes
SN1-QoS-Traffic-Policy | No | No | No | No | No | No | Yes | Yes
SN1-Rad-APN-Name | No | No | No | No | No | No | Yes | Yes
SN1-Radius-Returned-Username | No | No | No | No | No | No | Yes | Yes
SN1-Re-CHAP-Interval | No | No | No | No | No | No | Yes | Yes
SN1-Roaming-Behavior | No | No | No | No | No | No | Yes | Yes
SN1-Roaming-Profile | No | No | No | No | No | No | Yes | Yes
SN1-Roaming-Sub-Use-GGSN | No | No | No | No | No | No | Yes | Yes
SN1-ROHC-Direction | No | No | No | No | No | No | Yes | Yes
SN1-ROHC-Flow-Marking-Mode | No | No | No | No | No | No | Yes | Yes
SN1-ROHC-Mode | No | No | No | No | No | No | Yes | Yes
SN1-ROHC-Profile-Name | No | No | No | No | No | No | Yes | Yes
SN1-Routing-Area-Id | No | No | No | No | No | No | Yes | Yes
SN1-Rulebase | No | No | No | No | No | No | Yes | Yes
SN1-Secondary-DCCA-Peer | No | No | No | No | No | No | Yes | Yes
SN1-Secondary-DNS-Server | No | No | No | No | No | No | Yes | Yes
SN1-Secondary-NBNS-Server | No | No | No | No | No | No | Yes | Yes
SN1-Service-Address | No | No | No | No | No | No | Yes | Yes
SN1-Service-Type | No | No | No | No | No | No | Yes | Yes
SN1-Simultaneous-SIP-MIP | No | No | No | No | No | No | Yes | Yes
SN1-Subs-Acc-Flow-Traffic-Valid | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Accounting | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Acct-Interim | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Acct-Mode | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Acct-Rsp-Action | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Acct-Start | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Acct-Stop | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Class | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Dormant-Activity | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-IP-Hdr-Neg-Mode | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-IP-TOS-Copy | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Nexthop-Address | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-No-Interims | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Permission | No | No | No | No | No | No | Yes | Yes
SN1-Subscriber-Template-Name | No | No | No | No | No | No | Yes | Yes
SN1-Subs-IMSA-Service-Name | No | No | No | No | No | No | Yes | Yes
SN1-Subs-VJ-Slotid-Cmp-Neg-Mode | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Dnlk-Burst-Size | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Dnlk-Committed-Data-Rate | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Dnlk-Exceed-Action | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Dnlk-Peak-Data-Rate | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Dnlk-Violate-Action | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Uplk-Burst-Size | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Uplk-Committed-Data-Rate | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Uplk-Exceed-Action | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Uplk-Peak-Data-Rate | No | No | No | No | No | No | Yes | Yes
SN1-Tp-Uplk-Violate-Action | No | No | No | No | No | No | Yes | Yes
SN1-Traffic-Group | No | No | No | No | No | No | Yes | Yes
SN1-Transparent-Data | No | No | No | No | No | No | Yes | Yes
SN1-Tun-Addr-Policy | No | No | No | No | No | No | Yes | Yes
SN1-Tunnel-Gn | No | No | No | No | No | No | Yes | Yes
SN1-Tunnel-ISAKMP-Crypto-Map | No | No | No | No | No | No | Yes | Yes
SN1-Tunnel-ISAKMP-Secret | No | No | No | No | No | No | Yes | Yes
SN1-Tunnel-Load-Balancing | No | No | No | No | No | No | Yes | Yes
SN1-Tunnel-Password | No | No | No | No | No | No | Yes | Yes
SN1-Unclassify-List-Name | No | No | No | No | No | No | Yes | Yes
SN1-Virtual-APN-Name | No | No | No | No | No | No | Yes | Yes
SN1-Visiting-Behavior | No | No | No | No | No | No | Yes | Yes
SN1-Visiting-Profile | No | No | No | No | No | No | Yes | Yes
SN1-Visiting-Sub-Use-GGSN | No | No | No | No | No | No | Yes | Yes
SN1-Voice-Push-List-Name | No | No | No | No | No | No | Yes | Yes
SN1-VPN-ID | No | No | No | No | No | No | Yes | Yes
SN1-VPN-Name | No | No | No | No | No | No | Yes | Yes
SNA1-PPP-Unfr-data-In-Gig | No | No | No | No | No | No | Yes | Yes
SNA1-PPP-Unfr-data-In-Oct | No | No | No | No | No | No | Yes | Yes
SNA1-PPP-Unfr-data-Out-Gig | No | No | No | No | No | No | Yes | Yes
SNA1-PPP-Unfr-data-Out-Oct | No | No | No | No | No | No | Yes | Yes
SN-Access-link-IP-Frag | No | No | No | No | Yes | Yes | No | No
SN-Acct-Input-Giga-Dropped | No | No | No | No | Yes | Yes | No | No
SN-Acct-Input-Octets-Dropped | No | No | No | No | Yes | Yes | No | No
SN-Acct-Input-Packets-Dropped | No | No | No | No | Yes | Yes | No | No
SN-Acct-Output-Giga-Dropped | No | No | No | No | Yes | Yes | No | No
SN-Acct-Output-Octets-Dropped | No | No | No | No | Yes | Yes | No | No
SN-Acct-Output-Packets-Dropped | No | No | No | No | Yes | Yes | No | No
SN-Acs-Credit-Control-Group | No | No | No | No | Yes | Yes | No | No
SN-Admin-Expiry | No | No | No | No | Yes | Yes | No | No
SN-Admin-Permission | No | No | No | No | Yes | Yes | No | No
SNA-Input-Gigawords | No | No | No | No | No | No | No | No
SNA-Input-Octets | No | No | No | No | No | No | No | No
SN-ANID | No | No | No | No | No | No | No | No
SNA-Output-Gigawords | No | No | No | No | No | No | No | No
SNA-Output-Octets | No | No | No | No | No | No | No | No
SNA-PPP-Bad-Addr | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Bad-Ctrl | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Bad-FCS | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Ctrl-Input-Octets | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Ctrl-Input-Packets | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Ctrl-Output-Octets | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Ctrl-Output-Packets | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Discards-Input | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Discards-Output | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Echo-Req-Input | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Echo-Req-Output | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Echo-Rsp-Input | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Echo-Rsp-Output | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Errors-Input | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Errors-Output | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Framed-Input-Octets | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Framed-Output-Octets | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Packet-Too-Long | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Unfr-data-In-Gig | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Unfr-data-In-Oct | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Unfr-data-Out-Gig | No | No | No | No | Yes | Yes | No | No
SNA-PPP-Unfr-data-Out-Oct | No | No | No | No | Yes | Yes | No | No
SNA-RPRAK-Rcvd-Acc-Ack | No | No | No | No | Yes | Yes | No | No
SNA-RPRAK-Rcvd-Mis-ID | No | No | No | No | Yes | Yes | No | No
SNA-RPRAK-Rcvd-Msg-Auth-Fail | No | No | No | No | Yes | Yes | No | No
SNA-RPRAK-Rcvd-Total | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Acc-Dereg | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Acc-Reg | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Bad-Req | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Denied | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Mis-ID | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Send-Err | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Reply-Sent-Total | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Upd-Re-Sent | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Upd-Send-Err | No | No | No | No | Yes | Yes | No | No
SNA-RP-Reg-Upd-Sent | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-Acc-Dereg | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-Acc-Reg | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-Badly-Formed | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-Mis-ID | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-Msg-Auth-Fail | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-T-Bit-Not-Set | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-Total | No | No | No | No | Yes | Yes | No | No
SNA-RPRRQ-Rcvd-VID-Unsupported | No | No | No | No | Yes | Yes | No | No
SN-Assigned-VLAN-ID | No | No | No | No | Yes | Yes | No | No
SN-Authorised-Qos | No | No | No | No | Yes | Yes | No | No
SN-Bandwidth-Policy | No | No | No | No | Yes | Yes | No | No
SN-Call-Id | No | No | No | No | Yes | Yes | No | No
SN-Cause-Code | No | No | No | No | Yes | Yes | No | No
SN-Cause-For-Rec-Closing | No | No | No | No | Yes | Yes | No | No
SN-CBB-Policy | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-International | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-Local | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-LongDistance | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-Premium | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-RoamingInternatnl | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-Transfer | No | No | No | No | Yes | Yes | No | No
SN-CF-Call-Waiting | No | No | No | No | Yes | Yes | No | No
SN-CF-CId-Display | No | No | No | No | Yes | Yes | No | No
SN-CF-CId-Display-Blocked | No | No | No | No | Yes | Yes | No | No
SN-CF-Follow-Me | No | No | No | No | Yes | Yes | No | No
SN-CF-Forward-Busy-Line | No | No | No | No | Yes | Yes | No | No
SN-CF-Forward-No-Answer | No | No | No | No | Yes | Yes | No | No
SN-CF-Forward-Not-Regd | No | No | No | No | Yes | Yes | No | No
SN-CF-Forward-Unconditional | No | No | No | No | Yes | Yes | No | No
SN-CFPolicy-ID | No | No | No | No | Yes | Yes | No | No
SN-Change-Condition | No | No | No | No | Yes | Yes | No | No
SN-Charging-VPN-Name | No | No | No | No | Yes | Yes | No | No
SN-Chrg-Char-Selection-Mode | No | No | No | No | Yes | Yes | No | No
SN-Content-Disposition | No | No | No | No | Yes | Yes | No | No
SN-Content-Length | No | No | No | No | Yes | Yes | No | No
SN-Content-Type | No | No | No | No | Yes | Yes | No | No
SN-CR-International-Cid | No | No | No | No | Yes | Yes | No | No
SN-CR-LongDistance-Cid | No | No | No | No | Yes | Yes | No | No
SN-CSCF-App-Server-Info | No | No | No | No | Yes | Yes | No | No
SN-CSCF-Rf-SDP-Media-Components | No | No | No | No | Yes | Yes | No | No
SN-Cscf-Subscriber-Ip-Address | No | No | No | No | Yes | Yes | No | No
SN-Data-Tunnel-Ignore-DF-Bit | No | No | No | No | Yes | Yes | No | No
SN-DHCP-Lease-Expiry-Policy | No | No | No | No | Yes | Yes | No | No
SN-Direction | No | No | No | No | Yes | Yes | No | No
SN-Disconnect-Reason | No | No | No | No | Yes | Yes | No | No
SN-DNS-Proxy-Intercept-List | No | No | No | No | Yes | Yes | No | No
SN-DNS-Proxy-Use-Subscr-Addr | No | No | No | No | Yes | Yes | No | No
SN-Dynamic-Addr-Alloc-Ind-Flag | No | No | No | No | Yes | Yes | No | No
SN-Ecs-Data-Volume | No | No | No | No | Yes | Yes | No | No
SN-Enable-QoS-Renegotiation | No | No | No | No | Yes | Yes | No | No
SN-Event | No | No | No | No | Yes | Yes | No | No
SN-Ext-Inline-Srvr-Context | No | No | No | No | Yes | Yes | No | No
SN-Ext-Inline-Srvr-Down-Addr | No | No | No | No | Yes | Yes | No | No
SN-Ext-Inline-Srvr-Down-VLAN | No | No | No | No | Yes | Yes | No | No
SN-Ext-Inline-Srvr-Preference | No | No | No | No | Yes | Yes | No | No
SN-Ext-Inline-Srvr-Up-Addr | No | No | No | No | Yes | Yes | No | No
SN-Ext-Inline-Srvr-Up-VLAN | No | No | No | No | Yes | Yes | No | No
SN-Fast-Reauth-Username | No | No | No | No | Yes | Yes | No | No
SN-Firewall-Enabled | No | No | No | No | Yes | Yes | No | No
SN-Firewall-Policy | No | No | No | No | Yes | Yes | No | No
SN-FMC-Location | No | No | No | No | Yes | Yes | No | No
SN-GGSN-Address | No | No | No | No | Yes | Yes | No | No
SN-GGSN-MIP-Required | No | No | No | No | Yes | Yes | No | No
SN-Gratuitous-ARP-Aggressive | No | No | No | No | Yes | Yes | No | No
SN-GTP-Version | No | No | No | No | Yes | Yes | No | No
SN-HA-Send-DNS-Address | No | No | No | No | Yes | Yes | No | No
SN-Home-Behavior | No | No | No | No | Yes | Yes | No | No
SN-Home-Profile | No | No | No | No | Yes | Yes | No | No
SN-Home-Sub-Use-GGSN | No | No | No | No | Yes | Yes | No | No
SN-Ignore-Unknown-HA-Addr-Error | No | No | No | No | Yes | Yes | No | No
SN-IMS-AM-Address | No | No | No | No | Yes | Yes | No | No
SN-IMS-AM-Domain-Name | No | No | No | No | Yes | Yes | No | No
SN-IMS-Charging-Identifier | No | No | No | No | Yes | Yes | No | No
SN-IMSI | No | No | No | No | Yes | Yes | No | No
SN-Inactivity-Time | No | No | No | No | Yes | Yes | No | No
SN-Internal-SM-Index | No | No | No | No | Yes | Yes | No | No
SN-IP-Alloc-Method | No | No | No | No | Yes | Yes | No | No
SN-IP-Filter-In | No | No | No | No | Yes | Yes | No | No
SN-IP-Filter-Out | No | No | No | No | Yes | Yes | No | No
SN-IP-Header-Compression | No | No | No | No | Yes | Yes | No | No
SN-IP-Hide-Service-Address | No | No | No | No | Yes | Yes | No | No
SN-IP-In-ACL | No | No | No | No | Yes | Yes | No | No
SN-IP-In-Plcy-Grp | No | No | No | No | Yes | Yes | No | No
SN-IP-Out-ACL | No | No | No | No | Yes | Yes | No | No
SN-IP-Out-Plcy-Grp | No | No | No | No | Yes | Yes | No | No
SN-IP-Pool-Name | No | No | No | No | Yes | Yes | No | No
SN-IP-Source-Validation | No | No | No | No | Yes | Yes | No | No
SN-IP-Source-Violate-No-Acct | No | No | No | No | Yes | Yes | No | No
SN-IP-Src-Validation-Drop-Limit | No | No | No | No | Yes | Yes | No | No
SN-IPv6-DNS-Proxy | No | No | No | No | Yes | Yes | No | No
SN-IPv6-Egress-Filtering | No | No | No | No | Yes | Yes | No | No
SN-IPv6-Min-Link-MTU | No | No | No | No | Yes | Yes | No | No
SN-IPv6-num-rtr-advt | No | No | No | No | Yes | Yes | No | No
SN-IPv6-Primary-DNS | No | No | No | No | Yes | Yes | No | No
SN-IPv6-rtr-advt-interval | No | No | No | No | Yes | Yes | No | No
SN-IPv6-Secondary-DNS | No | No | No | No | Yes | Yes | No | No
SN-IPv6-Sec-Pool | No | No | No | No | Yes | Yes | No | No
SN-IPv6-Sec-Prefix | No | No | No | No | Yes | Yes | No | No
SN-ISC-Template-Name | No | No | No | No | Yes | Yes | No | No
SN-Is-Unregistered-Subscriber | No | No | No | No | Yes | Yes | No | No
SN-L3-to-L2-Tun-Addr-Policy | No | No | No | No | Yes | Yes | No | No
SN-Local-IP-Address | No | No | No | No | Yes | Yes | No | No
SN-Long-Duration-Action | No | No | No | No | Yes | Yes | No | No
SN-Long-Duration-Notification | No | No | No | No | Yes | Yes | No | No
SN-Long-Duration-Timeout | No | No | No | No | Yes | Yes | No | No
SN-Max-Sec-Contexts-Per-Subs | No | No | No | No | Yes | Yes | No | No
SN-Mediation-Acct-Rsp-Action | No | No | No | No | Yes | Yes | No | No
SN-Mediation-Enabled | No | No | No | No | Yes | Yes | No | No
SN-Mediation-No-Interims | No | No | No | No | Yes | Yes | No | No
SN-Mediation-VPN-Name | No | No | No | No | Yes | Yes | No | No
SN-Min-Compress-Size | No | No | No | No | Yes | Yes | No | No
SN-MIP-AAA-Assign-Addr | No | No | No | No | Yes | Yes | No | No
SN-MIP-ANCID | No | No | No | No | Yes | Yes | No | No
SN-MIP-Dual-Anchor | No | No | No | No | Yes | Yes | No | No
SN-MIP-HA-Assignment-Table | No | No | No | No | Yes | Yes | No | No
SN-MIP-Match-AAA-Assign-Addr | No | No | No | No | Yes | Yes | No | No
SN-MIP-Reg-Lifetime-Realm | No | No | No | No | Yes | Yes | No | No
SN-MIP-Send-Ancid | No | No | No | No | Yes | Yes | No | No
SN-MIP-Send-Correlation-Info | No | No | No | No | Yes | Yes | No | No
SN-MIP-Send-Imsi | No | No | No | No | Yes | Yes | No | No
SN-MIP-Send-Term-Verification | No | No | No | No | Yes | Yes | No | No
SN-MN-HA-Hash-Algorithm | No | No | No | No | Yes | Yes | No | No
SN-MN-HA-Timestamp-Tolerance | No | No | No | No | Yes | Yes | No | No
SN-Mode | No | No | No | No | Yes | Yes | No | No
SN-MS-ISDN | No | No | No | No | Yes | Yes | No | No
SN-NAI-Construction-Domain | No | No | No | No | Yes | Yes | No | No
SN-NAT-IP-Address | No | No | No | No | Yes | Yes | No | No
SN-Node-Functionality | No | No | No | No | Yes | Yes | No | No
SN-NPU-Qos-Priority | No | No | No | No | Yes | Yes | No | No
SN-Ntk-Initiated-Ctx-Ind-Flag | No | No | No | No | Yes | Yes | No | No
SN-Ntk-Session-Disconnect-Flag | No | No | No | No | Yes | Yes | No | No
SN-Nw-Reachability-Server-Name | No | No | No | No | Yes | Yes | No | No
SN-Originating-IOI | No | No | No | No | Yes | Yes | No | No
SN-Overload-Disc-Connect-Time | No | No | No | No | Yes | Yes | No | No
SN-Overload-Disc-Inact-Time | No | No | No | No | Yes | Yes | No | No
SN-Overload-Disconnect | No | No | No | No | Yes | Yes | No | No
SN-PDG-TTG-Required | No | No | No | No | Yes | Yes | No | No
SN-PDIF-MIP-Release-TIA | No | No | No | No | Yes | Yes | No | No
SN-PDIF-MIP-Required | No | No | No | No | Yes | Yes | No | No
SN-PDIF-MIP-Simple-IP-Fallback | No | No | No | No | Yes | Yes | No | No
SN-PDSN-Correlation-Id | No | No | No | No | Yes | Yes | No | No
SN-PDSN-Handoff-Req-IP-Addr | No | No | No | No | Yes | Yes | No | No
SN-PDSN-NAS-Id | No | No | No | No | Yes | Yes | No | No
SN-PDSN-NAS-IP-Address | No | No | No | No | Yes | Yes | No | No
SN-Permit-User-Mcast-PDUs | No | No | No | No | Yes | Yes | No | No
SN-PPP-Accept-Peer-v6Ifid | No | No | No | No | Yes | Yes | No | No
SN-PPP-Always-On-Vse | No | No | No | No | Yes | Yes | No | No
SN-PPP-Data-Compression | No | No | No | No | Yes | Yes | No | No
SN-PPP-Data-Compression-Mode | No | No | No | No | Yes | Yes | No | No
SN-PPP-Keepalive | No | No | No | No | Yes | Yes | No | No
SN-PPP-NW-Layer-IPv4 | No | No | No | No | Yes | Yes | No | No
SN-PPP-NW-Layer-IPv6 | No | No | No | No | Yes | Yes | No | No
SN-PPP-Outbound-Password | No | No | No | No | Yes | Yes | No | No
SN-PPP-Outbound-Username | No | No | No | No | Yes | Yes | No | No
SN-PPP-Progress-Code | No | No | No | No | Yes | Yes | No | No
SN-PPP-Reneg-Disc | No | No | No | No | Yes | Yes | No | No
SN-Prepaid | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Compressed-Count | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Final-Duration-Alg | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Inbound-Octets | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Outbound-Octets | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Preference | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Timeout | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Total-Octets | No | No | No | No | Yes | Yes | No | No
SN-Prepaid-Watermark | No | No | No | No | Yes | Yes | No | No
SN-Primary-DCCA-Peer | No | No | No | No | Yes | Yes | No | No
SN-Primary-DNS-Server | No | No | No | No | Yes | Yes | No | No
SN-Primary-NBNS-Server | No | No | No | No | Yes | Yes | No | No
SN-Proxy-MIP | No | No | No | No | Yes | Yes | No | No
SN-Pseudonym-Username | No | No | No | No | Yes | Yes | No | No
SN-QoS-Background-Class | No | No | No | No | Yes | Yes | No | No
SN-QoS-Class-Background-PHB | No | No | No | No | Yes | Yes | No | No
SN-QoS-Class-Conversational-PHB | No | No | No | No | Yes | Yes | No | No
SN-QoS-Class-Interactive-1-PHB | No | No | No | No | Yes | Yes | No | No
SN-QoS-Class-Interactive-2-PHB | No | No | No | No | Yes | Yes | No | No
SN-QoS-Class-Interactive-3-PHB | No | No | No | No | Yes | Yes | No | No
SN-QoS-Class-Streaming-PHB | No | No | No | No | Yes | Yes | No | No
SN-QoS-Conversation-Class | No | No | No | No | Yes | Yes | No | No
SN-QOS-HLR-Profile | No | No | No | No | Yes | Yes | No | No
SN-QoS-Interactive1-Class | No | No | No | No | Yes | Yes | No | No
SN-QoS-Interactive2-Class | No | No | No | No | Yes | Yes | No | No
SN-QoS-Interactive3-Class | No | No | No | No | Yes | Yes | No | No
SN-QoS-Negotiated | No | No | No | No | Yes | Yes | No | No
SN-QoS-Renegotiation-Timeout | No | No | No | No | Yes | Yes | No | No
SN-QoS-Streaming-Class | No | No | No | No | Yes | Yes | No | No
SN-QoS-Tp-Dnlk | No | No | No | No | Yes | Yes | No | No
SN-QoS-Tp-Uplk | No | No | No | No | Yes | Yes | No | No
SN-QoS-Traffic-Policy | No | No | No | No | Yes | Yes | No | No
SN-Rad-APN-Name | No | No | No | No | Yes | Yes | No | No
SN-Radius-Returned-Username | No | No | No | No | Yes | Yes | No | No
SN-Re-CHAP-Interval | No | No | No | No | Yes | Yes | No | No
SN-Roaming-Behavior | No | No | No | No | Yes | Yes | No | No
SN-Roaming-Profile | No | No | No | No | Yes | Yes | No | No
SN-Roaming-Sub-Use-GGSN | No | No | No | No | Yes | Yes | No | No
SN-ROHC-Flow-Marking-Mode | No | No | No | No | Yes | Yes | No | No
SN-ROHC-Profile-Name | No | No | No | No | Yes | Yes | No | No
SN-Role-Of-Node | No | No | No | No | Yes | Yes | No | No
SN-Routing-Area-Id | No | No | No | No | Yes | Yes | No | No
SN-Rulebase | No | No | No | No | Yes | Yes | No | No
SN-SDP-Session-Description | No | No | No | No | Yes | Yes | No | No
SN-Sec-IP-Pool-Name | No | No | No | No | Yes | Yes | No | No
SN-Secondary-DCCA-Peer | No | No | No | No | Yes | Yes | No | No
SN-Secondary-DNS-Server | No | No | No | No | Yes | Yes | No | No
SN-Secondary-NBNS-Server | No | No | No | No | Yes | Yes | No | No
SN-Service-Address | No | No | No | No | Yes | Yes | No | No
SN-Service-Type | No | No | No | No | Yes | Yes | No | No
SN-Session-Id | No | No | No | No | Yes | Yes | No | No
SN-Simultaneous-SIP-MIP | No | No | No | No | Yes | Yes | No | No
SN-SIP-Method | No | No | No | No | Yes | Yes | No | No
SN-SIP-Request-Time-Stamp | No | No | No | No | Yes | Yes | No | No
SN-SIP-Response-Time-Stamp | No | No | No | No | Yes | Yes | No | No
SN-Software-Version | No | No | No | No | Yes | Yes | No | No
SN-Subs-Acc-Flow-Traffic-Valid | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Accounting | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Acct-Interim | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Acct-Mode | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Acct-Rsp-Action | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Acct-Start | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Acct-Stop | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Class | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Dormant-Activity | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-IP-Hdr-Neg-Mode | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-IP-TOS-Copy | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Nexthop-Address | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-No-Interims | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Permission | No | No | No | No | Yes | Yes | No | No
SN-Subscriber-Template-Name | No | No | No | No | Yes | Yes | No | No
SN-Subs-IMSA-Service-Name | No | No | No | No | Yes | Yes | No | No
SN-Subs-VJ-Slotid-Cmp-Neg-Mode | No | No | No | No | Yes | Yes | No | No
SN-Terminating-IOI | No | No | No | No | Yes | Yes | No | No
SN-Tp-Dnlk-Burst-Size | No | No | No | No | Yes | Yes | No | No
SN-Tp-Dnlk-Committed-Data-Rate | No | No | No | No | Yes | Yes | No | No
SN-Tp-Dnlk-Exceed-Action | No | No | No | No | Yes | Yes | No | No
SN-Tp-Dnlk-Peak-Data-Rate | No | No | No | No | Yes | Yes | No | No
SN-Tp-Dnlk-Violate-Action | No | No | No | No | Yes | Yes | No | No
SN-Tp-Uplk-Burst-Size | No | No | No | No | Yes | Yes | No | No
SN-Tp-Uplk-Committed-Data-Rate | No | No | No | No | Yes | Yes | No | No
SN-Tp-Uplk-Exceed-Action | No | No | No | No | Yes | Yes | No | No
SN-Tp-Uplk-Peak-Data-Rate | No | No | No | No | Yes | Yes | No | No
SN-Tp-Uplk-Violate-Action | No | No | No | No | Yes | Yes | No | No
SN-Traffic-Group | No | No | No | No | Yes | Yes | No | No
SN-TrafficSelector-Class | No | No | No | No | Yes | Yes | No | No
SN-Transparent-Data | No | No | No | No | Yes | Yes | No | No
SN-Tun-Addr-Policy | No | No | No | No | Yes | Yes | No | No
SN-Tunnel-Gn | No | No | No | No | Yes | Yes | No | No
SN-Tunnel-ISAKMP-Crypto-Map | No | No | No | No | Yes | Yes | No | No
SN-Tunnel-ISAKMP-Secret | No | No | No | No | Yes | Yes | No | No
SN-Tunnel-Load-Balancing | No | No | No | No | Yes | Yes | No | No
SN-Tunnel-Password | No | No | No | No | Yes | Yes | No | No
SN-Unclassify-List-Name | No | No | No | No | Yes | Yes | No | No
SN-Virtual-APN-Name | No | No | No | No | Yes | Yes | No | No
SN-Visiting-Behavior | No | No | No | No | Yes | Yes | No | No
SN-Visiting-Profile | No | No | No | No | Yes | Yes | No | No
SN-Visiting-Sub-Use-GGSN | No | No | No | No | Yes | Yes | No | No
SN-Voice-Push-List-Name | No | No | No | No | Yes | Yes | No | No
SN-VPN-ID | No | No | No | No | Yes | Yes | No | No
SN-VPN-Name | No | No | No | No | Yes | Yes | No | No
SN-WiMAX-Auth-Only | No | No | No | No | Yes | Yes | No | No
State | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Terminal-Capability | No | No | No | No | No | No | No | No
Termination-Action | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Transparent-Data | No | No | No | No | No | No | Yes | No
Transparent-VSA | No | No | No | No | No | No | No | No
Tunnel-Assignment-ID | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Client-Auth-ID | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Client-Endpoint | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Medium-Type | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Password | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Preference | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Private-Group-ID | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Server-Auth-ID | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Server-Endpoint | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Tunnel-Type | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
User-Name | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
User-Password | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
WiMAX-Acct-Input-Packets-Giga | No | No | No | No | Yes | No | Yes | No
WiMAX-Acct-Output-Packets-Giga | No | No | No | No | Yes | No | Yes | No
WiMAX-Active-Time | No | No | No | No | Yes | No | Yes | No
WiMAX-Beginning-Of-Session | No | No | No | No | Yes | No | Yes | No
WiMAX-BS-ID | No | No | No | No | Yes | No | Yes | No
WiMAX-Capability | No | No | No | No | Yes | No | Yes | No
WiMAX-Control-Octets-In | No | No | No | No | Yes | No | Yes | No
WiMAX-Control-Octets-Out | No | No | No | No | Yes | No | Yes | No
WiMAX-Control-Packets-In | No | No | No | No | Yes | No | Yes | No
WiMAX-Control-Packets-Out | No | No | No | No | Yes | No | Yes | No
WiMAX-Count-Type | No | No | No | No | Yes | No | Yes | No
WiMAX-Device-Auth-Indicator | No | No | No | No | Yes | No | Yes | No
WiMAX-Flow-Description | No | No | No | No | Yes | No | Yes | No
WiMAX-Home-HNP-PMIP6 | No | No | No | No | Yes | No | Yes | No
WiMAX-Home-IPv4-HoA-PMIP6 | No | No | No | No | Yes | No | Yes | No
WiMAX-Idle-Mode-Transition | No | No | No | No | Yes | No | Yes | No
WiMAX-IP-Technology | No | No | No | No | Yes | No | Yes | No
WiMAX-NAP-ID | No | No | No | No | Yes | No | Yes | No
WiMAX-NSP-ID | No | No | No | No | Yes | No | Yes | No
WiMAX-Packet-Flow-Descriptor | No | No | No | No | Yes | No | Yes | No
WiMAX-Packet-Flow-Descriptor-V2 | No | No | No | No | Yes | No | Yes | No
WiMAX-PDF-ID | No | No | No | No | Yes | No | Yes | No
WiMAX-PPAC | No | No | No | No | Yes | No | Yes | No
WiMAX-PPAQ | No | No | No | No | Yes | No | Yes | No
WiMAX-Prepaid-Indicator | No | No | No | No | Yes | No | Yes | No
WiMAX-Prepaid-Tariff-Switch | No | No | No | No | Yes | No | Yes | No
WiMAX-QoS-Descriptor | No | No | No | No | Yes | No | Yes | No
WiMAX-SDF-ID | No | No | No | No | Yes | No | Yes | No
WiMAX-Session-Continue | No | No | No | No | Yes | No | Yes | No
WiMAX-Session-Term-Capability | No | No | No | No | Yes | No | Yes | No
Win-Call-Id | No | No | No | No | No | No | No | No
Win-Service-Name | No | No | No | No | No | No | No | No
WSType | No | No | No | No | No | No | No | No
XGP-AAA-CoS | No | No | No | No | No | No | No | No
XGP-AAA-QoS-Number | No | No | No | No | No | No | No | No
XGP-AAA-TIME | No | No | No | No | No | No | No | No
XGP-BS-IP-Address | No | No | No | No | No | No | No | No
XGP-FILE-VERSION | No | No | No | No | No | No | No | No
XGP-QoS-Number | No | No | No | No | No | No | No | No
XGP-Sequence-Number | No | No | No | No | No | No | No | No