# LTE Policy Configuration Mode Commands

The LTE Policy Configuration Mode is used to create and manage the LTE policies supporting MME and S-GW configurations on the system.

IMPORTANT:

Available commands or keywords/variables vary based on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
ho-restrict-list

Creates a handover (HO) restriction list or specifies an existing HO restriction list and enters the Handover Restriction List Configuration Mode.
Platform:

ASR 5000
Product:

MME, S-GW
Privilege:

Administrator
Syntax

    [ no ] ho-restrict-list list_name [ -noconfirm ]

no

Removes the specified restriction list from the system.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
list_name

Specifies the name of the HO restriction list. If the entered list name does not refer to an existing list, a new list is created. list_name is an alphanumeric string of 1 through 64 characters.
Usage:

Use this command to enter the Handover Restriction List Configuration Mode for an existing list or for a newly defined list. This command is also used to remove an existing list.

Entering this command results in the following prompt:

    [context_name]hostname(ho-restrict-list)#

Handover Restriction List Configuration Mode commands are defined in the LTE Handover Restriction List Configuration Mode Commands chapter.
Example:
The following command enters the Handover Restriction List Configuration Mode for a new or existing list named ho_restricit_list1:

    ho-restrict-list ho_restrict_list1

subscriber-map

Creates a subscriber map or specifies an existing subscriber map and enters the Subscriber Map Configuration Mode.
Platform:

ASR 5000
Product:

MME, S-GW
Privilege:

Administrator
Syntax

    [ no ] subscriber-map map_name [ -noconfirm ]

no

Removes the specified subscriber map from the system.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
map_name

Specifies the name of the subscriber map. If the map name does not refer to an existing map, a new map is created. map_name must be an alphanumeric string of 1 through 64 characters.
Usage:

Enter the Subscriber Map Configuration Mode for an existing or newly defined map. This command is also used to remove an existing map.

Entering this command results in the following prompt:

    hostname(subscriber-map)#

Subscriber Map Configuration Mode commands are defined in the LTE Subscriber Map Configuration Mode Commands chapter.
Example:
The following command enters the existing Subscriber Map Configuration Mode (or creates it if it does not already exist) for the map named map1:

    subscriber-map map1

tai-mgmt-db

Creates a Tracking Area Identifier (TAI) Management Database or specifies an existing database and enters the TAI Management Database Configuration mode.
Platform:

ASR 5000
Product:

MME, S-GW
Privilege:

Administrator
Syntax

    [ no ] tai-mgmt-db db_name [ -noconfirm ]

no

Removes the specified management database from the system.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
db_name

Specifies the name of the management database. If the name does not refer to an existing database, a new database is created. db_name is an alphanumeric string of 1 through 64 characters.
Usage:

Enter the TAI Management Database Configuration Mode for an existing or newly defined database. This command is also used to remove an existing database.

Entering this command results in the following prompt:

    [context_name]hostname(tai-mgmt-db)#

TAI Management Database Configuration Mode commands are defined in the TAI Management Database Configuration Mode Commands chapter.
Example:
The following command enters the existing TAI Management Database configuration mode (or creates it if it does not already exist) for the database named tai_db1:

    tai-mgmt-db tai_db1