# Remote Address List Configuration Mode Commands

The Remote Address List Configuration Mode is used to configure address lists for the Remote Address-based Accounting feature on a per-context basis.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
address

Configures addresses within a Remote Address List.
Platform:

ASR 5000
Product:

PDSN, HA
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] address ip_address netmask subnet

no

Removes a previously configured address.
ip_address

Specifies the IP address of the remote device.

ip_address is entered using IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation.
netmask subnet

Specifies the subnet mask of the remote device.

subnet is the netmask expressed in IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation.
Usage:

Use this command to configure remote address lists for use with the Remote Address-based accounting feature. A maximum of 10 address can be configured per list.
Example:
The following command adds an IP address of 192.168.100.1 with a subnet mask of 255.255.255.0 to the list:

    address 192.168.100.1
    netmask 255.255.255.0

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.