# Global Configuration Mode Commands (threshold poll commands O - Z)

This section includes the commands threshold poll packets-filtered-dropped interval through threshold poll tpo-rto-timeout.

The Global Configuration Mode is used to configure basic system-wide parameters.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
threshold poll packets-filtered-dropped interval

Configures the polling interval over which to count the filtered/dropped packets.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll packets-filtered-dropped interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPacketsFilteredDropped command in this mode.
Example:
The following command configures the polling interval to 600 seconds for filtered/dropped packets:

    threshold poll packets-filtered-dropped interval
    600

threshold poll packets-forwarded-to-cpu interval

Configures the polling interval over which to count packets forwarded to active system CPUs in the system.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll packets-forwarded-to-cpu interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPacketsForwarded command in this mode.
Example:
The following command configures the polling interval to 600 seconds for packets forwarded to active system CPUs in the system:

    threshold poll packets-forwarded-to-cpu interval
    600

threshold poll pdg-current-active-sessions interval

Configures the polling interval over which to count the total number of currently active Packet Data Gateway/Tunnel Termination Gateway (PDG/TTG) sessions.
Platform:

ASR 5000
Product:

PDG, TTG
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll pdg-current-active-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDGCurrActSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDG/TTG sessions:

    threshold poll pdg-current-active-sessions interval
    600

threshold poll pdg-current-sessions interval

Configures the polling interval over which to count the total number of current Packet Data Gateway/Tunnel Termination Gateway (PDG/TTG) sessions, including inactive sessions.
Platform:

ASR 5000
Product:

PDG, TTG
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll pdg-current-sessions
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDGCurrSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDG/TTG sessions:

    threshold poll pdg-current-sessions
    interval 600

threshold poll pdif-current-active-sessions interval

Configures the polling interval over which to count the total number of currently active Packet Data Interworking Function (PDIF) sessions.
Platform:

ASR 5000
Product:

PDIF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll pdif-current-active-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDIFCurrActSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDIF sessions:

    threshold poll pdif-current-active-sessions interval
    600

threshold poll pdif-current-sessions interval

Configures the polling interval over which to count the total number of current Packet Data Interworking Function (PDIF) sessions, including inactive sessions.
Platform:

ASR 5000
Product:

PDIF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll pdif-current-sessions
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDIFCurrSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDIF sessions:

    threshold poll pdif-current-sessions
    interval 600

threshold poll pdsn-init-rrq-rcvd-rate interval

Configures the polling interval over which to count the total number of current Packet Data Serving Node (PDSN) sessions, including inactive sessions.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll pdsn-init-rrq-rcvd-rate
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNCallSetupRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDSN sessions:

    threshold poll pdsn-init-rrq-rcvd-rate
    interval 600

threshold poll pdsn-svc-init-rrq-rcvd-rate interval

Configures the polling interval over which to count the total number of current Packet Data Serving Node (PDSN) sessions, including inactive sessions.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll pdsn-svc-init-rrq-rcvd-rate interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNSvcCallSetupRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDSN sessions:

    threshold poll pdsn-svc-init-rrq-rcvd-rate interval
    600

threshold poll per-service-asngw-sessions interval

Configures the polling interval in seconds over which to count the number of PDP contexts per ASN-GW service in the system.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-asngw-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceASNGWSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for ASN-GW sessions:

    threshold poll per-service-asngw-sessions interval
    600

threshold poll per-service-ggsn-sessions interval

Configures the polling interval in seconds over which to count the number of PDP contexts per GGSN service in the system.
Platform:

ASR 5000
Product:

GGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-ggsn-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceGGSNSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for GGSN sessions:

    threshold poll per-service-ggsn-sessions interval
    600

threshold poll per-service-gprs-pdp-sessions interval

Configures the polling interval in seconds over which to count the number of 2G-activated PDP contexts per GPRS service.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-gprs-pdp-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceGPRSPDPSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for 2G PDP contexts:

    threshold poll per-service-gprs-pdp-sessions interval
    600

threshold poll per-service-gprs-sessions interval

Configures the polling interval in seconds over which to count the number of 2G-attached subscribers per GPRS service.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-gprs-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceGPRSSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for 2G GPRS sessions:

    threshold poll per-service-gprs-sessions interval
    600

threshold poll per-service-ha-sessions interval

Configures the polling interval in seconds over which to count the number of HA sessions per Home Agent (HA) service in the system.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-ha-sessions
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceHASessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for HA sessions:

    threshold poll per-service-ha-sessions
    interval 600

threshold poll per-service-lns-sessions interval

Configures the polling interval in seconds over which to count the number of L2TP Network Server (LNS) sessions per LNS service in the system.
Platform:

ASR 5000
Product:

LNS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-lns-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceLNSSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for LNS sessions:

    threshold poll per-service-lns-sessions interval
    600

threshold poll per-service-pdg-sessions interval

Configures the polling interval in seconds over which to count the number of Packet Data Gateway (PDG) sessions per PDG/TTG service in the system.
Platform:

ASR 5000
Product:

PDG, TTG
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-pdg-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServicePDGSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDG/TTG sessions:

    threshold poll per-service-pdg-sessions interval
    600

threshold poll per-service-pdsn-sessions interval

Configures the polling interval in seconds over which to count the number of Packet Data Serving Node (PDSN) sessions per PDSN service in the system.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-pdsn-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServicePDSNSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PDSN sessions:

    threshold poll per-service-pdsn-sessions interval
    600

threshold poll per-service-sgsn-pdp-sessions interval

Configures the polling interval in seconds over which to count the number of 3G-activated PDP contexts per SGSN service on the system.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-sgsn-pdp-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceSGSNPDPSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for 3G PDP contexts:

    threshold poll per-service-sgsn-pdp-sessions interval
    600

threshold poll per-service-sgsn-sessions interval

Configures the polling interval in seconds over which to count the number of 3G-attached subscribers per SGSN service in the system.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll per-service-sgsn-sessions interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPerServiceSGSNSessions command in this mode.
Example:
The following command configures the polling interval to 600 seconds for SGSN sessions:

    threshold poll per-service-sgsn-sessions interval
    600

threshold poll phsgw-auth-failure interval

Configures the polling interval in seconds over which to count the number of Personal Handyphone System Gateway (PHSGW) authentication failures.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-auth-failure
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWAuthFail command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW authentication failures:

    threshold poll phsgw-auth-failure
    interval 600

threshold poll phsgw-eapol-auth-failure interval

Configures the polling interval in seconds over which to count the number of authentication failures for a PHSGW service using Extensible Authentication Protocol Over LAN (EAPOL).
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-eapol-auth-failure interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWEAPOLAuthFailure command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW EAPOL failures:

    threshold poll phsgw-eapol-auth-failure interval
    600

threshold poll phsgw-handoff-denial interval

Configures the polling interval in seconds over which to count the number of handoff denials in PHSGW.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-handoff-denial
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWMaxEAPOLRetry command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW handoff denials:

    threshold poll phsgw-handoff-denial
    interval 600

threshold poll phsgw-max-eap-retry interval

Configures the polling interval in seconds over which to count the maximum number of Extensible Authentication Protocol (EAP) retries in PHSGW.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-max-eap-retry
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWMaxEAPRetry command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW EAP retries:

    threshold poll phsgw-max-eap-retry
    interval 600

threshold poll phsgw-max-eapol-retry interval

Configures the polling interval in seconds over which to count the maximum number of Extensible Authentication Protocol Over LAN (EAPOL) retries in PHSGW.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-max-eapol-retry
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWMaxEAPOLRetry command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW EAPOL retries:

    threshold poll phsgw-max-eapol-retry
    interval 600

threshold poll phsgw-network-entry-denial interval

Configures the polling interval in seconds over which to count the number of network entry denials in PHSGW.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-network-entry-denial interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWNWEntryDenial command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW network entry denials:

    threshold poll phsgw-network-entry-denial interval
    600

threshold poll phsgw-session-setup-timeout interval

Configures the polling interval in seconds over which to count the number of PHSGW sessions that timed out during setup.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-session-setup-timeout interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWSessSetupTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW session setup timeouts:

    threshold poll phsgw-session-setup-timeout interval
    600

threshold poll phsgw-session-timeout interval

Configures the polling interval in seconds over which to count the number of PHSGW sessions that timed out.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phsgw-session-timeout
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSGWSessTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSGW session timeouts:

    threshold poll phsgw-session-timeout
    interval 600

threshold poll phspc-session-setup-timeout interval

Configures the polling interval in seconds over which to count the number of Personal Handyphone System - Personal Computer (PHSPC) sessions that timed out during setup.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phspc-session-setup-timeout interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSPCSessSetupTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSPC session setup timeouts:

    threshold poll phspc-session-setup-timeout interval
    600

threshold poll phspc-sleep-mode-timeout interval

Configures the polling interval in seconds over which to count the number of PHSPC sessions that timed out when the personal computer went into sleep mode.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phspc-sleep-mode-timeout interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSPCSleepModeTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSPC sleep mode timeouts:

    threshold poll phspc-sleep-mode-timeout interval
    600

threshold poll phspc-sm-entry-denial interval

Configures the polling interval in seconds over which to count the number of denied PHSPC short message (SM) sessions.
Platform:

ASR 5000
Product:

PHSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll phspc-sm-entry-denial
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPHSPCSmEntryDenial command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PHSPC SM session denials:

    threshold poll phspc-sm-entry-denial
    interval 600

threshold poll port-high-activity interval

Configures the polling interval in seconds over which to measure the overall percentage of port utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Administrator Security Administrator
Syntax

    threshold poll port-high-activity
    interval seconds

interval seconds

Configures the threshold polling interval in multiples of 30 seconds. seconds is an integer from 30 through 60000. Default is 300 seconds.
Usage:

High port activity thresholds generate alerts or alarms based on the peak utilization percentage of each configured port during the specified polling interval. This threshold is configured on a per-port basis. Alerts or alarms are triggered for high port activity based on the following rules:

Enter condition: Actual percent peak utilization of a port is greater than or equal to the high threshold.

Clear condition: Actual percent peak utilization of a port is less than the low threshold.

If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.This threshold is configured on a per-port basis configured using the port port-type slot#/port# command syntax.

IMPORTANT:

This command is not available on all platforms

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPortHighActivity command in this mode.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPortHighActivity command in this mode.
Example:
Use the following example to configure the polling interval over which to measure for high port activity to 300 seconds:

    threshold poll port-high-activity
    interval 300

threshold poll port-rx-utilization interval

Configures the polling interval in seconds over which to measure the overall percentage of incoming traffic received over system ports.
Platform:

ASR 5000
Product:

All
Privilege:

Administrator Security Administrator
Syntax

    threshold poll port-rx-utilization
    interval seconds

interval seconds

Configures the threshold polling interval in multiples of 30 seconds. seconds is an integer from 30 to 60000. Default is 300 seconds.
Usage:

Receive port utilization thresholds generate alerts or alarms based on the utilization percentage of each configured port in relation to data received during the specified polling interval. This threshold is configured on a per-port basis configured using the port port-type slot#/port# command syntax.

IMPORTANT:

This command is not available on all platforms

IMPORTANT:

Ports configured for half-duplex do not differentiate between data received and data transmitted. (The transmitted and received percentages are combined.) Therefore, to avoid redundant alarms, it is recommended that only the receive or transmit utilization threshold be configured.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPortRxUtil command in this mode.
Example:
Use the following example to configure a threshold poll interval of 300 seconds (5 minutes)

    threshold poll port-rx-utilization
    interval 300

threshold poll port-tx-utilization

Configures the polling interval in seconds over which to measure the overall percentage of outgoing traffic sent over system ports.
Platform:

ASR 5000
Product:

All
Privilege:

Administrator Security Administrator
Syntax

    threshold poll port-tx-utilization
    interval seconds

interval seconds

Configures the threshold polling interval in multiples of 30 seconds. seconds is an integer from 30 through 60000. Default is 300 seconds.
Usage:

Transmit port utilization thresholds generate alerts or alarms based on the utilization percentage of each configured port in relation to data transmitted during the specified polling interval. This threshold is configured on a per-port basis configured using the port port-type slot#/port# command syntax.

IMPORTANT:

This command is not available on all platforms

IMPORTANT:

Ports configured for half-duplex do not differentiate between data received and data transmitted. (The transmitted and received percentages are combined.) Therefore, to avoid redundant alarms, it is recommended that only the receive or transmit utilization threshold be configured.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPortTxUtil command in this mode.
Example:
Use the following example to configure a threshold poll interval of 300 seconds (5 minutes)

    threshold poll port-tx-utilization
    interval 300

threshold poll ppp-setup-fail-rate interval

Configures the polling interval in seconds over which to measure for the percentage of point-to-point protocol (PPP) setup failures.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ppp-setup-fail-rate
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPPPSetupFailRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for PPP setup failures:

    threshold poll ppp-setup-fail-rate
    interval 600

threshold poll reg-reply-error interval

Configures the polling interval over which to measure number of registration reply errors for Home Agent (HA) services.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll reg-reply-error
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHASvcRegReplyError command in this mode.
Example:
The following command configures the polling interval to 600 seconds for HA registration errors:

    threshold poll reg-reply-error
    interval 600

threshold poll reg-total-active interval

Configures the polling interval over which to measure CSCF Total Active Registrations.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll reg-total-active
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcTotalActiveReg command in this mode.
Example:
The following command configures the polling interval to 600 seconds for CSCF active registrations:

    threshold poll reg-total-active
    interval 600

threshold poll rereg-reply-error interval

Configures the polling interval over which to measure number of re-registration reply errors for HA services.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll rereg-reply-error
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHASvcReregReplyError command in this mode.
Example:
The following command configures the polling interval to 600 seconds for HA re-registration reply errors:

    threshold poll rereg-reply-error
    interval 600

threshold poll route-service interval

Configures the polling interval over which to count or measure the thresholding value for BGP route services on the system.
Platform:

ASR 5000
Product:

All
Privilege:

Administrator Security Administrator
Syntax

    threshold poll route-service
    interval durdefault threshold poll
    route-service interval

default

Restores the threshold poll interval value to its default value of 900 seconds.
interval time

Default: 900 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is any integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshBGPRoutes command in this mode.
Example:
The following command configures the polling interval for the total BGP routes threshold polling duration value to 600 seconds (10 minutes):

    hreshold poll route-service
    interval 600

threshold poll rp-setup-fail-rate interval

Configures the polling interval over which to measure the percentage of RAN PDSN (RP) setup failures.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Administrator Security Administrator
Syntax

    threshold poll rp-setup-fail-rate
    interval durdefault threshold poll
    route-service interval

default

Restores the threshold poll interval value to its default value of 900 seconds.
interval time

Default: 900 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is any integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshRPSetupFailRate command in this mode.
Example:
The following command configures the polling interval for the RP setup fail rate polling duration value to 600 seconds (10 minutes):

    hreshold poll rp-setup-fail-rate
    interval 600

threshold poll storage-utilization interval

Configures the polling interval over which to measure the percentage of management card flash memory utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Administrator Security Administrator
Syntax

    threshold poll storage-utilization
    interval durdefault threshold poll
    route-service interval

default

Restores the threshold poll interval value to its default value of 900 seconds.
interval time

Default: 900 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is any integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshStorageUtilization command in this mode.
Example:
The following command configures the polling interval for flash memory utilization polling duration value to 600 seconds (10 minutes):

    threshold poll storage-utilization
    interval 600

threshold poll system-capacity interval

Configures the polling interval over which to measure the percentage of current system capacity.
Platform:

ASR 5000
Product:

All
Privilege:

Administrator Security Administrator
Syntax

    threshold poll system-capacity
    interval durdefault threshold poll
    route-service interval

default

Restores the threshold poll interval value to its default value of 900 seconds.
interval time

Default: 900 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is any integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSystemCapacity command in this mode.
Example:
The following command configures the polling interval for flash memory utilization polling duration value to 600 seconds (10 minutes):

    hreshold poll system-capacity
    interval 600

threshold poll total-asngw-sessions interval

Configures the polling interval over which to count or measure the thresholding value for the total number of sessions across all the ASN-GW services on a system to trigger an alert or alarm.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-asngw-sessions
    interval timedefault threshold poll
    total-asngw-sessions interval

default

Restores the threshold polling interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWSessions command in this mode.
Example:
The following command configures the polling interval for counting the total number of ASN-GW sessions across all the ASN-GW services on a system, to 600 seconds (10 minutes):

    threshold poll total-asngw-sessions
    interval 600

threshold poll total-ggsn-sessions interval

Configures the polling interval over which to count or measure the thresholding value for the total number of sessions across all the GGSN services on a system to trigger an alert or alarm.
Platform:

ASR 5000
Product:

GGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-ggsn-sessions
    interval timedefault threshold poll
    total-ggsn-sessions interval

default

Restores the threshold polling interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshGGSNSessions command in this mode.
Example:
The following command configures the polling interval for counting the total number of GGSN sessions across all the GGSN services on a system, to 600 seconds (10 minutes):

    threshold poll total-ggsn-sessions
    interval 600

threshold poll total-gprs-pdp-sessions interval

Configures the polling interval over which to count the total number of 2G-activated PDP contexts per GPRS sessions on the system.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-gprs-pdp-sessions
    interval timedefault threshold poll
    total-gprs-pdp-sessions interval

default

Restores the threshold polling interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshGPRSPDPSessions command in this mode.
Example:
The following command configures the polling interval for counting the total number of 2G-activated PDP contexts per GPRS sessions, to 600 seconds (10 minutes):

    threshold poll total-gprs-pdp-sessions
    interval 600

threshold poll total-gprs-sessions interval

Configures the polling interval over which to count the total number of 2G-attached subscribers on the system.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-gprs-sessions
    interval timedefault threshold poll
    total-gprs-sessions interval

default

Restores the threshold polling interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshGPRSSessions command in this mode.
Example:
The following command configures the polling interval for counting the total number of 2G-attached subscribers, to 600 seconds (10 minutes):

    threshold poll total-gprs-sessions
    interval 600

threshold poll total-ha-sessions interval

Configures the polling interval over which to count the total number of Home Agent (HA) sessions on the system.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-ha-sessions
    interval timedefault threshold poll
    total-ha-sessions interval

default

Restores the threshold polling interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHASessions command in this mode.
Example:
The following command configures the polling interval for counting the total number of HA sessions on the system, to 600 seconds (10 minutes):

    threshold poll total-ha-sessions
    interval 600

threshold poll total-hnbgw-hnb-sessions

Configures the polling interval over which to count or measure the thresholding value for the total number of IuH sessions between the HNB and HNB-GW to count across all the HNB-GW services on a system to trigger an alert or alarm.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-hnbgw-hnb-sessions interval timedefault threshold poll
    total-hnbgw-hnb-sessions interval

default

Restores the threshold polling interval value to its default value of 900 seconds.
interval time

Default: 900 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable SNMP trap for threshold monitoring of this threshold use snmp trap enable ThreshTotalHNBGWHnbSess command in this mode.
Example:
The following command configures the polling interval for counting the total number of HNB sessions between HNB and HNB-GW across all the HNB-GW services on a system, to 600 seconds (10 minutes):

    threshold poll total-hnbgw-hnb-sessions interval
    600

threshold poll total-hnbgw-iu-sessions

Configures the polling interval over which to count or measure the thresholding value for the total number of subscriber sessions on HNB-GW service (over Iu-CS/Iu-PS interface) to count across all the HNB-GW services on a system to trigger alert or alarm.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-hnbgw-iu-sessions
    interval timedefault threshold poll
    total-hnbgw-iu-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an value from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshTotalHNBGWIuSess command in this mode.
Example:
The following command configures the polling interval for counting the total number of subscriber sessions across all the HNB-GW services on a system, to 600 seconds (10 minutes):

    threshold poll total-hnbgw-iu-sessions
    interval 600

threshold poll total-hnbgw-ue-sessions

Configures the polling interval over which to count or measure the thresholding value for the total number of UEs connected to HNB-GW service to count across all the HNB-GW services on a system to trigger alert or alarm.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-hnbgw-ue-sessions
    interval timedefault threshold poll
    total-hnbgw-ue-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshTotalHNBGWUeSess command in this mode.
Example:
The following command configures the polling interval for the total number of UEs connected to an HNB-GW service across all the HNB-GW services on a system, to 600 seconds (10 minutes):

    threshold poll total-hnbgw-ue-sessions
    interval 600

threshold poll total-hsgw-sessions interval

Configures the polling interval over which to count the total number of HRPD Serving Gateway (HSGW) sessions across all services in the system.
Platform:

ASR 5000
Product:

HSGW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-hsgw-sessions
    interval timedefault threshold poll
    total-hsgw-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHSGWSessions command in this mode.
Example:
The following command configures the polling interval for the total number of HSGW sessions across all the HSGW services on a system, to 600 seconds (10 minutes):

    threshold poll total-hsgw-sessions
    interval 600

threshold poll total-lma-sessions interval

Configures the polling interval over which to count the total number of Local Mobility Anchor (LMA) sessions across all services in the system.
Platform:

ASR 5000
Product:

P-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-lma-sessions
    interval timedefault threshold poll
    total-lma-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshLMASessions command in this mode.
Example:
The following command configures the polling interval for the total number of LMA sessions across all the LMA sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-lma-sessions
    interval 600

threshold poll total-lns-sessions interval

Configures the polling interval over which to count the total number of L2TP Network Server (LNS) sessions in the system.
Platform:

ASR 5000
Product:

PDSN, GGSN, HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-lns-sessions
    interval timedefault threshold poll
    total-lns-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshLNSSessions command in this mode.
Example:
The following command configures the polling interval for the total number of LNS sessions across all the LNS sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-lns-sessions
    interval 600

threshold poll total-mme-sessions

Configures the polling interval over which to count or measure the thresholding value for MME sessions on the system.
Platform:

ASR 5000
Product:

MME
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-mme-sessions
    interval timedefault threshold poll
    total-mme-sessions interval

default

Restores the threshold poll interval value to its default value of 900 seconds.
interval time

Default: 900 seconds

Specifies the polling interval (in seconds) for counting the total number of MME sessions on the system.

time must be an ny integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshMMESessions command in this mode.
Example:
The following command configures the polling interval for the total MME session threshold polling duration value to 600 seconds (10 minutes):

    threshold poll total-mme-sessions
    interval 600

threshold poll total-pdsn-sessions interval

Configures the polling interval over which to count the total number of Packet Data Serving Node (PDSN) sessions in the system.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-pdsn-sessions
    interval timedefault threshold poll
    total-pdsn-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNSessions command in this mode.
Example:
The following command configures the polling interval for the total number of PDSN sessions across all the PDSN sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-pdsn-sessions
    interval 600

threshold poll total-pgw-sessions interval

Configures the polling interval over which to count the total number of Packet Data Network Gateway (P-GW) sessions across all services in the system.
Platform:

ASR 5000
Product:

P-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-pgw-sessions
    interval timedefault threshold poll
    total-pgw-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPGWSessions command in this mode.
Example:
The following command configures the polling interval for the total number of P-GW sessions across all the P-GW sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-pgw-sessions
    interval 600

threshold poll total-sgsn-pdp-sessions interval

Configures the polling interval over which to count the total number of PDP contexts for all Serving GPRS Support Node (SGSN) sessions in the system.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-sgsn-pdp-sessions
    interval timedefault threshold poll
    total-sgsn-pdp-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSGSNPDPSessions command in this mode.
Example:
The following command configures the polling interval for the total number of PDP contexts across all the SGSN sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-sgsn-pdp-sessions
    interval 600

threshold poll total-sgsn-sessions interval

Configures the polling interval over which to count the total number of SGSN sessions in the system.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-sgsn-sessions
    interval timedefault threshold poll
    total-sgsn-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSGSNSessions command in this mode.
Example:
The following command configures the polling interval for the total number of SGSN sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-sgsn-sessions
    interval 600

threshold poll total-sgw-sessions interval

Configures the polling interval over which to count the total number of Serving Gateway (S-GW) sessions across all services in the system.
Platform:

ASR 5000
Product:

S-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-sgw-sessions
    interval timedefault threshold poll
    total-sgw-sessions interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSGWSessions command in this mode.
Example:
The following command configures the polling interval for the total number of S-GW sessions on a system, to 600 seconds (10 minutes):

    threshold poll total-sgw-sessions
    interval 600

threshold poll total-subscriber interval

Configures the polling interval over which to count the total number of subscriber sessions across all services in the system.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll total-subscriber
    interval timedefault threshold poll
    total-subscriber interval

default

Restores the threshold poll interval value to its default value of 300 seconds.
interval time

Default: 300 seconds

Specifies the amount of time (in seconds) that comprises the polling interval.

time must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold model and threshold monitoring commands for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSubscriberTotalcommand in this mode.
Example:
The following command configures the polling interval for the total number of subscribers on a system, to 600 seconds (10 minutes):

    threshold poll total-subscriber
    interval 600

threshold poll tpo-dns-failure

Configures the threshold polling interval for monitoring Traffic Performance Optimization (TPO) DNS resolution failures.
Platform:

ASR 5000
Product:

TPO
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll tpo-dns-failure
    interval intervaldefault threshold
    poll tpo-dns-failure interval

default

Configures this command with the default polling interval.

Default: 900 seconds
interval

Specifies the polling interval (in seconds) for monitoring TPO DNS resolution failures.

interval must be an integer from 30 through 60000. The system rounds up the value to the closest multiple of 30.
Usage:

Use this command to configure the threshold polling interval for monitoring TPO DNS resolution failures.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshTpoDnsFailure command in this mode.
Example:
The following command configures the polling interval for TPO DNS resolution failures threshold to 600 seconds:

    threshold poll tpo-dns-failure
    interval 600

threshold poll tpo-low-compression-gain

Configures the threshold polling interval for monitoring TPO low-compression-gain results.
Platform:

ASR 5000
Product:

TPO
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll tpo-low-compression-gain interval intervaldefault threshold
    poll tpo-low-compression-gain interval

default

Configures this command with the default polling interval.

Default: 900 seconds
interval

Specifies the polling interval (in seconds) for monitoring TPO low-compression-gain results.

interval must be an integer from 30 through 60000. The system rounds up the value to the closest multiple of 30.
Usage:

Use this command to configure the threshold polling interval for monitoring TPO low-compression-gain results.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshTpoLowCompressionGain command in this mode.
Example:
The following command configures the polling interval for TPO low-compression-gain results threshold to 600 seconds:

    threshold poll tpo-low-compression-gain interval
    600

threshold poll tpo-rto-timeout

Configures the threshold polling interval for monitoring TPO retransmission timeouts (RTOs).
Platform:

ASR 5000
Product:

TPO
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll tpo-rto-timeout
    interval intervaldefault threshold
    poll tpo-rto-timeout interval

default

Configures this command with the default polling interval.

Default: 900 seconds
interval

Specifies the polling interval (in seconds) for monitoring TPO retransmission timeouts.

interval must be an integer from 30 through 60000. The system rounds up the value to the closest multiple of 30.
Usage:

Use this command to configure the threshold polling interval for monitoring TPO retransmission timeouts.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshTpoRtoTimeout command in this mode.
Example:
The following command configures the polling interval for TPO retransmission timeouts threshold to 600 seconds:

    threshold poll tpo-rto-timeout
    interval 600