# CSCF Last Route Profile Criteria Configuration Mode Commands

The CSCF Last Route Profile Criteria Configuration Mode is used to configure county names and assign them Last Routing Option (LRO) numbers to be used by the CSCF last route profile. The S-CSCF forwards emergency call packets to the correct Public Safety Answering Point (PSAP) based on this criteria, which it receives from a peer server.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
county-name

Configure county names and assign them Last Routing Option (LRO) numbers to be used by the CSCF last route profile.
Platform:

ASR 5000
Product:

SCM (S-CSCF)
Privilege:

Administrator
Syntax

    county-name county_name lro-number value[ no ] county-name county_name

county_name

Specifies the county name.

county_name must be from 1 to 79 alpha and/or numeric characters in length.
lro-number value

Specifies an existing LRO number.

value can be a maximum of ten digits in length.
no county-name county_name

Removes the specified county name.
Usage:

Use this command to configure county names and assign them LRO numbers.

IMPORTANT:

You may configure up to 100 county names.
Example:
The following command creates a county name called norfolk and assigns it an LRO number of 8884384357:

    county-name norfolk lro-number 8884384357

end

Exits the current mode and returns to the Exec Mode.
Product:

All
Privilege:

Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the current mode and returns to the previous mode.
Product:

All
Privilege:

Administrator
Syntax

    exit

Usage:

Return to the previous mode.