# IPv6 ACL Configuration Mode Commands

The IPv6 Access Control List Configuration Mode is used to create and manage IPv6 access privileges.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
deny/permit (by source IP address masking)

Used to filter subscriber sessions based on the IPv6 address mask sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    { deny | permit } [ log ] source_address
    source_wildcardafter { deny | permit } [ log ] source_address
    source_wildcardbefore { deny | permit } [ log ] source_address
    source_wildcardno { deny | permit } [ log ] source_address source_wildcard

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change
no

Removes the rule which exactly matches the options specified.
deny | permit

Specifies the rule is either block (deny) or an allow (permit) filter.

- deny: Indicates the rule, when matched, drops the corresponding packets.
- permit: Indicates the rule, when matched, allows the corresponding packets.

log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
Usage:

Define a rule when any packet from the IP addresses which fall into the group of addresses matching the IP address masking. This allows the reduction of filtering rules as it does not require a rule for each source and destination pair.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide.
Example:
The following command defines two rules with the second logging filtered packets:

    permit 2001:4A2B::1f3F

    deny log 2001:4A2B::1f3F

The following sets the insertion point to before the first rule defined above:

    before permit 2001:4A2B::1f3F

The following command sets the insertion point after the second rule defined above:

    after deny log 2001:4A2B::1f3F

The following deletes the first rule defined above:

    no permit 2001:4A2B::1f3F

deny/permit (any)

Used to filter subscriber sessions based on any packet received. This command is also used to set the access control list insertion point.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    { deny | permit } [ log ] anyafter { deny | permit } [ log ] anybefore { deny | permit } [ log ] anyno { deny | permit } [ log ] any

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
deny | permit

Specifies the rule is either block (deny) or an allow (permit) filter.

- deny: Indicates the rule, when matched, drops the corresponding packets.
- permit: Indicates the rule, when matched, allows the corresponding packets.

log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
any

Indicates all packets will match the filter regardless of source and/or destination.
Usage:

Define a catch all rule to place at the end of the list of rules.

IMPORTANT:

It is suggested that any rule which is added to be a catch all should also have the log option specified. The logged packets may be used to determine if the current list of rules is adequate or needs modification to ensure proper security. The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide.
Example:
The following command defines two rules with the second logging filtered packets:

    permit any

    deny log any

The following sets the insertion point to before the first rule defined above:

    before permit any

The following command sets the insertion point after the second rule defined above:

    after deny log any

The following deletes the first rule defined above:

    no permit any

deny/permit (by host IP address)

Used to filter subscriber sessions based on the targeted host IP address sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    { deny | permit } [ log ] host source_host_addressafter { deny | permit } [ log ] host source_host_addressbefore { deny | permit } [ log ] host source_host_addressno { deny | permit } [ log ] host source_host_address

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
deny | permit

Specifies the rule is either block (deny) or an allow (permit) filter.

- deny: Indicates the rule, when matched, drops the corresponding packets.
- permit: Indicates the rule, when matched, allows the corresponding packets.

log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
Usage:

Define a rule when a very specific remote host is to be blocked. In simplified networks where the access controls need only block a few hosts, this command allows the rules to be very clear and concise.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide.
Example:
The following command defines two rules with the second logging filtered packets:

    permit host 2001:4A2B::1f3F

    deny log host 2001:4A2B::1f3F

The following sets the insertion point to before the first rule defined above:

    before permit host 2001:4A2B::1f3F

The following command sets the insertion point after the second rule defined above:

    after deny log host 2001:4A2B::1f3F

The following deletes the first rule defined above:

    no permit host 2001:4A2B::1f3F

deny/permit (by source ICMP packets)

Used to filter subscriber sessions based on the internet control message protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    { deny | permit } [ log ] icmp { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]after { deny | permit } [ log ] icmp { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]before { deny | permit } [ log ] icmp { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]no { deny | permit } [ log ] icmp { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
deny | permit

Specifies the rule is either block (deny) or an allow (permit) filter.

- deny: Indicates the rule, when matched, drops the corresponding packets.
- permit: Indicates the rule, when matched, allows the corresponding packets.

log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
icmp_type

Specifies that all ICMP packets of a particular type are to be filtered. The type is an integer from 0 through 255.
icmp_code

Specifies that all ICMP packets of a particular code are to be filtered. The type is an integer from 0 through 255.
Usage:

Define a rule to block ICMP packets which can be used for address resolution and possible be a security risk.

The IP filtering allows flexible controls for pairs of individual hosts or groups by IP masking which allows the filtering of entire subnets if necessary.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide.
Example:
The following command defines two rules with the second logging filtered packets:

    permit icmp host 2001:4A2B::1f3F4
    any 168

    deny log icmp 2001:4A2B::1f3F
    2001:4a2b::1f00 host fe80::a02:410 168 11

The following sets the insertion point to before the first rule defined above:

    before permit icmp
    host 2001:4A2B::1f3F any 168

The following command sets the insertion point after the second rule defined above:

    after deny log icmp
    2001:4A2B::1f3F 2001:4a2b::1f00 host fe80::a02:410 168 11

The following deletes the first rule defined above:

    no permit icmp host
    2001:4A2B::1f3F any 168

deny/permit (by IP packets)

Used to filter subscriber sessions based on the internet protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    { deny | permit } [ log ] ip { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocolnum ]after { deny | permit } [ log ] ip { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocolnum ]before { deny | permit } [ log ] ip { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocolnum ]no { deny | permit } [ log ] ip { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocolnum ]

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
deny | permit

Specifies the rule is either block (deny) or an allow (permit) filter.

- deny: indicates the rule, when matched, drops the corresponding packets.
- permit: indicates the rule, when matched, allows the corresponding packets.

log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
fragment

Indicates packet filtering is to be applied to IP packet fragments only.
protocol num

Indicates that the packet filtering is to be applied to a specific protocol number.

num can be any integer ranging from 0 to 255.
Usage:

Block IP packets when the source and destination are of interest.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide.
Example:
The following command defines two rules with the second logging filtered packets:

    permit ip host 2001:4A2B::1f3F
    any fragment

    deny log ip 2001:4A2B::1f3F
    2001:4a2b::1f00 host fe80::a02:410

The following sets the insertion point to before the first rule defined above:

    before permit ip host
    2001:4A2B::1f3F any fragment

The following command sets the insertion point after the second rule defined above:

    after deny log ip
    2001:4A2B::1f3F 2001:4a2b::1f00 host fe80::a02:410

The following deletes the first rule defined above:

    no permit ip host
     2001:4A2B::1f3F any fragment

deny/permit (by TCP/UDP packets)

Used to filter subscriber sessions based on the transmission control protocol/user datagram protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    { deny | permit } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }after { deny | permit } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }before { deny | permit } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }no { deny | permit } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
deny | permit

Specifies the rule is either block (deny) or an allow (permit) filter.

- deny: Indicates the rule, when matched, drops the corresponding packets.
- permit: Indicates the rule, when matched, allows the corresponding packets.

log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
tcp | udp

Specifies the filter is to be applied to IP-based transmission control protocol or the user datagram protocol.

- tcp: Filter applies to TPC packets.
- udp: Filter applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer from 0 through 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer from 0 through 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
Usage:

Block IP packets when the source and destination are of interest but for only a limited set of ports.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide.
Example:
The following command defines four rules with the second and fourth rules logging filtered packets:

    permit tcp host 2001:4A2B::1f3F any

    deny log udp 2001:4A2B::1f3F
    2001:4a2b::1f00 host fe80::a02:410

    permit tcp host 2001:4A2B::1f3F
    gt 1023 any

The following sets the insertion point to before the first rule defined above:

    before permit tcp
    host 2001:4A2B::1f3F any

The following command sets the insertion point after the second rule defined above:

    after deny log udp
    2001:4A2B::1f3F 2001:4a2b::1f00 host fe80::a02:410

The following deletes the third rule defined above:

    no permit tcp host
    2001:4A2B::1f3F gt 1023 any

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
readdress server

Alter the destination address and port number in TCP or UDP packet headers to redirect packets to a different server.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax
after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
redirect_address

The IP address to which the IP packets are redirected. TCP or UDP packet headers are rewritten to contain the new destination address. This must expressed in IPv6 colon-separated-hexadecimal notation.
port port_number

The number of the port at the redirect address where the packets are sent. TCP or UDP packet headers are rewritten to contain the new destination port number.
tcp | udp

Specifies the redirect is to be applied to the IP-based transmission control protocol or the user datagram protocol.

- tcp: Redirect applies to TCP packets.
- udp: Redirect applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer from 0 through 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer from 0 through 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
Usage:

Use this command to define a rule that redirects packets to a different destination address. The TCP and UDP packet headers are modified with the new destination address and destination port.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the server at fe80::c0a8:a04, UDP packets coming from any host with a destination of any host are matched:

    readdress server fe80::c0a8:a04
    udp any any

The following sets the insertion point to before the rule defined above:

    before readdress server
    fe80::c0a8:a04 udp any any

The following deletes the rule defined above:

    no readdress server
    fe80::c0a8:a04 udp any any

redirect context (by IP address masking)

Used to redirect subscriber sessions based on the IP address mask sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect context context_id [ log ] source_address
    source_wildcardafter redirect context context_id [ log ] source_address source_wildcardbefore redirect context context_id [ log ] source_address source_wildcardno redirect context context_id [ log ] source_address source_wildcard

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
context context_id

Specifies the context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

Filters by the IP address(es) from which the packet originated. This option filters all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

Filters packets for a group of addresses specified in conjunction with the source_address option.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
Usage:

Define a rule when any packet from the IP addresses which fall into the group of addresses matching the IP address masking. This allows the reduction of redirect rules as it does not require a rule for each source and destination pair.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the context with the context ID of 23 and the source IP and wildcard of 2002::c6a2:1600 and 2002::c6a2:1600:

    redirect context 23 2002::c6a2:1600 2002::c6a2:1600

The following sets the insertion point to before the first rule defined above:

    before redirect context
    23 2002::c6a2:1600 2002::c6a2:1600

The following command sets the insertion point after the second rule defined above:

    after redirect context
    23 2002::c6a2:1600 2002::c6a2:1600

The following deletes the first rule defined above:

    no redirect context
    23 2002::c6a2:1600 2002::c6a2:1600

redirect context (any)

Used to redirect subscriber sessions based on any packet received. This command is also used to set the access control list insertion point.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect context context_id [ log ] anyafter redirect context context_id [ log ] anybefore redirect context context_id [ log ] anyno redirect context context_id [ log ] any

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
any

Indicates all packets will match the redirect regardless of source and/or destination.
Usage:

Define a catch all rule to place at the end of the list of rules to provide explicit handling of rules which do not fit any other criteria.

IMPORTANT:

It is suggested that any rule which is added to be a catch all should also have the log option specified. The logged packets may be used to determine if the current list of rules is adequate or needs modification to ensure proper security. The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the context with the context ID of 23 and any source IP:

    redirect context 23 any

The following sets the insertion point to before the first rule defined above:

    before redirect context
    23 any

The following command sets the insertion point after the second rule defined above:

    after redirect context
    23 any

The following deletes the first rule defined above:

    no redirect context
    23 any

redirect context (by host IP address)

Used to redirect subscriber sessions based on the targeted host IP address sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect context context_id [ log ] host source_ip_addressafter redirect context context_id [ log ] host source_ip_addressbefore redirect context context_id [ log ] host source_ip_addressno redirect context context_id [ log ] host source_ip_address

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
Usage:

Define a rule when a very specific remote host is to be blocked. In simplified networks where the access controls need only block a few hosts, this command allows the rules to be very clear and concise.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the context with the context ID of 23 and a host IP address of fe80::c0a8:c80b:

    redirect context 23
    host fe80::c0a8:c80b

The following sets the insertion point to before the first rule defined above:

    before redirect context
    23 host fe80::c0a8:c80b

The following command sets the insertion point after the second rule defined above:

    after redirect context
    23 host fe80::c0a8:c80b

The following deletes the first rule defined above:

    no redirect context
    23 host fe80::c0a8:c80b

redirect context (by source ICMP packets)

Used to redirect subscriber sessions based on the internet control message protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect context context_id [ log ] icmp { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]after redirect context context_id [ log ] icmp { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]before redirect context context_id [ log ] icmp { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]no redirect context context_id [ log ] icmp { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
icmp_type

Specifies that all ICMP packets of a particular type are to be filtered. Type is an integer from 0 through 255.
icmp_code

Specifies that all ICMP packets of a particular code are to be filtered type is an integer from 0 through 255.
Usage:

Define a rule to block ICMP packets which can be used for address resolution and possibly be a security risk.

The IP redirecting allows flexible controls for pairs of individual hosts or groups by IP masking which allows the redirecting of entire subnets if necessary.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the context with the context ID of 23, and ICMP packets coming from the host with the IP address 2002::c6a2:6419:

    redirect context 23
    icmp host 2002::c6a2:6419

The following sets the insertion point to before the first rule defined above:

    before redirect context
    23 icmp host 2002::c6a2:6419

The following command sets the insertion point after the second rule defined above:

    after redirect context
    23 icmp host 2002::c6a2:6419

The following deletes the first rule defined above:

    no redirect context
    23 icmp host 2002::c6a2:6419

redirect context (by IP packets)

Used to redirect subscriber sessions based on the internet protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect context context_id [ log ] ip { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocol num ]after redirect context context_id [ log ] ip { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocol num ]before redirect context context_id [ log ] ip { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocol num ]no redirect context context_id [ log ] ip { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocol num ]

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
fragment

Indicates packet redirection is to be applied to IP packet fragments only.
protocol num

Indicates that the packet filtering is to be applied to a specific protocol number.

num is an integer from 0 through 255.
Usage:

Block IP packets when the source and destination are of interest.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the context with the context ID of 23, and IP packets coming from the host with the IP address 2002::c6a2:6419, and fragmented packets for any destination are matched:

    redirect context 23
    ip host 2002::c6a2:6419 any fragment

The following sets the insertion point to before the first rule defined above:

    before redirect context
    23 ip host 198.162.100.25 any fragment

The following command sets the insertion point after the second rule defined above:

    after redirect context
    23 ip host 2002::c6a2:6419 any fragment

The following deletes the first rule defined above:

    no redirect context
    23 ip host 2002::c6a2:6419 any fragment

redirect context (by TCP/UDP packets)

Used to redirect subscriber sessions based on the transmission control protocol/user datagram protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect context context_id [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }after redirect context context_id [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }before redirect context context_id [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }no redirect context context_id [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dst_port ] }

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
tcp | udp

Specifies the redirect is to be applied to IP-based transmission control protocol or the user datagram protocol.

- tcp: Redirect applies to TPC packets.
- udp: Redirect applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer from 0 through 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer from 0 through 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer from 0 through 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer from 0 through 65535.
Usage:

Block IP packets when the source and destination are of interest but for only a limited set of ports.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the context with the context ID of 23, and UDP packets coming from any host are matched:

    redirect context 23
    udp any

The following sets the insertion point to before the rule defined above:

    before redirect context
    23 udp any

The following command sets the insertion point after the rule defined above:

    after redirect context
    23 udp any

The following deletes the rule defined above:

    no redirect context
    23 udp any

redirect css delivery-sequence

This is a restricted command. In StarOS 9.0 and later, this command is obsoleted.
redirect css service (any)

Used to redirect subscriber sessions based on any packet received with Content Service Steering (CSS) enabled. This command is also used to set the access control list insertion point.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] anyafter redirect css
    service svc_name [ log ] anybefore redirect css
    service svc_name [ log ] anyno redirect css service svc_name [ log ] any

after

Indicates all rule definitions defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definitions which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the CSS service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be a string of 1 through 15 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
any

Indicates all packets will match the redirect regardless of source and/or destination.
Usage:

Define a catch all rule definitions to place at the end of the list of rule definitions to provide explicit handling of rule definitions which do not fit any other criteria.

IMPORTANT:

It is suggested that any rule definition which is added to be a catch all should also have the log option specified. The logged packets may be used to determine if the current list of rule definitions is adequate or needs modification to ensure proper security.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL.

IMPORTANT:

Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the CSS service with the name css-svc1 and any source IP:

    redirect css service
    css-svc1 any

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 any

The following command sets the insertion point after the second rule definitions above:

    after redirect css
    service css-svc1 any

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 any

redirect css service (by host IP address)

Used to redirect subscriber sessions based on the targeted host IP address sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] host source_host_addressafter redirect css
    service svc_name [ log ] host source_host_addressbefore redirect css
    service svc_name [ log ] host source_host_addressno redirect css service svc_name [ log ] host source_host_address

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
Usage:

Define a rule definition when a very specific remote host is to be blocked. In simplified networks where the access controls need only block a few hosts, this command allows the rule definitions to be very clear and concise.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the CSS service with the name css-svc1 and a host IP address of fe80::c0a8:c80b:

    redirect css service
    css-svc1 host fe80::c0a8:c80b

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 host fe80::c0a8:c80b

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service css-svc1 host fe80::c0a8:c80b

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 host fe80::c0a8:c80b

redirect css service (by ICMP packets)

Used to redirect subscriber sessions based on the internet control message protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [icmp_type [ icmp_code ] ]after redirect css
    service svc_name [ log ] icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [icmp_type [ icmp_code ] ]before redirect css
    service svc_name [ log ] icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [icmp_type [ icmp_code ] ]no redirect css service svc_name [ log ] icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [icmp_type [ icmp_code ] ]

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured charging services.

svc_name must be an alphanumeric string of 1 through 15 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
icmp_type

Specifies that all ICMP packets of a particular type are to be filtered. The type can be an integer value from 0 through 255.
icmp_code

Specifies that all ICMP packets of a particular code are to be filtered. The type is an integer from 0 through 255.
Usage:

Define a rule definition to block ICMP packets which can be used for address resolution and possibly be a security risk.

The IP redirecting allows flexible controls for pairs of individual hosts or groups by IP masking which allows the redirecting of entire subnets if necessary.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the CSS service named css-svc1, and ICMP packets coming from the host with the IP address 2002::c6a2:6419:

    redirect css service
    css-svc1 icmp host 2002::c6a2:6419

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 icmp host 2002::c6a2:6419

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service css-svc1 icmp host 2002::c6a2:64195

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 icmp host 2002::c6a2:6419

redirect css service (by IP packets)

Used to redirect subscriber sessions based on the internet protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]after redirect css
    service svc_name [ log ] ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]before redirect css
    service svc_name [ log ] ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]no redirect css service svc_name [ log ] ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
fragment

Indicates packet redirection is to be applied to IP packet fragments only.
Usage:

Block IP packets when the source and destination are of interest.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the CSS service named css-svc1, and IP packets coming from the host with the IP address 2002::c6a2:6419, and fragmented packets for any destination are matched:

    redirect css service
    css-svc1 ip host 2002::c6a2:6419 any fragment

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 ip host 2002::c6a2:6419 any fragment

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service css-svc1 ip host 2002::c6a2:6419 any fragment

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 ip host 2002::c6a2:6419 any fragment

redirect css service (by source IP address masking)

Used to redirect subscriber sessions based on the IP address mask sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] source_address
    source_wildcardafter redirect css
    service svc_name [ log ] source_address source_wildcardbefore redirect css
    service svc_name [ log ] source_address source_wildcardno redirect css service svc_name [ log ] source_address source_wildcard

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
Usage:

Define a rule definition when any packet from the IP addresses which fall into the group of addresses matching the IP address masking. This allows the reduction of filtering rule definitions as it does not require a rule definition for each source and destination pair.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL.
Example:
The following command defines a rule definition to redirect packets to a CSS service named css-svc1:

    redirect css service
    css=svc1 2002::c6a2:6419

redirect css service (by TCP/UDP packets)

Used to redirect subscriber sessions based on the transmission control protocol/user datagram protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }after redirect css
    service svc_name [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }after redirect css
    service svc_name [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }no redirect css service svc_name [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured charging services.

svc_name must be an alphanumeric string of 1 through 15 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
tcp | udp

Specifies the redirect is to be applied to IP-based transmission control protocol or the user datagram protocol.

- tcp: Redirect applies to TPC packets.
- udp: Redirect applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer from 0 to 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer from 0 to 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer from 0 to 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer from 0 to 65535.
range start_source_port end_source_port

Specifies that all source TCP ports within a specific range are to be filtered.

start_source_port is the initial port in the range and end_source_port is the final port in the range.

Both start_source_port and end_source_port can be configured to an integer from 0 to 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer from 0 to 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer from 0 to 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer from 0 to 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer from 0 to 65535.
range start_dest_port end_dest_port

Specifies that all destination TCP ports within a specific range are to be filtered.

start_dest_port is the initial port in the range and end_dest_port is the final port in the range.

Both start_dest_port and end_dest_port can be configured to an integer from 0 to 65535
Usage:

Block IP packets when the source and destination are of interest but for only a limited set of ports.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the CSS service named css-svc1, and UDP packets coming from any host are matched:

    redirect css service
    css-svc1 udp any

The following sets the insertion point to before the rule definition above:

    before redirect css
    service css-svc1 udp any

The following command sets the insertion point after the rule definition above:

    after redirect css
    service css-svc1 udp any

The following deletes the rule definition above:

    no redirect css service
    css-svc1 udp any

redirect css service (for downlink, any)

Used to redirect subscriber sessions based on any packet received in the downlink (from the Mobile Node) direction. This command is also used to set the access control list insertion point.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] downlink anyafter redirect css
    service svc_name [ log ] downlink
    anybefore redirect css
    service svc_name [ log ] downlink
    anyno redirect css service svc_name [ log ] downlink any

after

Indicates all rule definitions defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
downlink

Apply this rule definition only to packets in the downlink (from the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
any

Indicates all packets will match the redirect regardless of source and/or destination.
Usage:

Define a catch all rule definition to place at the end of the list of rule definitions to provide explicit handling of rule definitions which do not fit any other criteria.

IMPORTANT:

It is suggested that any rule definition which is added to be a catch all should also have the log option specified. The logged packets may be used to determine if the current list of rule definitions is adequate or needs modification to ensure proper security.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL.

IMPORTANT:

Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the CSS service with the name css-svc1 and any source IP:

    redirect css service
    css-svc1 downlink any

The following sets the insertion point to before the first rule definition above:

    before redirect service
    css-svc1 downlink any

The following command sets the insertion point after the second rule definition above:

    after redirect service
    css-svc1 downlink any chgsvc1 downlink any

The following deletes the first rule definition above:

    no redirect service
    css-svc1 downlink any

redirect css service (for downlink, by host IP address)

Used to redirect subscriber sessions based on the targeted host IP address in the downlink (from the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] downlink
    host source_host_addressafter redirect css
    service svc_name [ log ] downlink
    host source_host_addressbefore redirect css
    service svc_name [ log ] downlink
    host source_host_addressno redirect css service svc_name [ log ] downlink
    host source_host_address

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
downlink

Apply this rule definition only to packets in the downlink (from the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
Usage:

Define a rule definition when a very specific remote host is to be blocked. In simplified networks where the access controls need only block a few hosts, this command allows the rule definitions to be very clear and concise.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service with the name css-svc1 and a host IP address of fe80::c0a8:c80b:

    redirect service css-svc1
    downlink host fe80::c0a8:c80b

The following sets the insertion point to before the first rule definition above:

    before redirect service
    css-svc1 downlink host fe80::c0a8:c80b

The following command sets the insertion point after the second rule definition above:

    after redirect service
    css-svc1 downlink host fe80::c0a8:c80b

The following deletes the first rule definition above:

    no redirect service
    css-svc1 downlink host fe80::c0a8:c80b

redirect css service (for downlink, by ICMP packets)

Used to redirect subscriber sessions based on the internet control message protocol packets in the downlink (from the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] downlink
    icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ icmp_type [ icmp_code ] ]after redirect css
    service svc_name [ log ] downlink
    icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ icmp_type [ icmp_code ] ]before redirect css
    service svc_name [ log ] downlink
    icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ icmp_type [ icmp_code ] ]no redirect css service svc_name [ log ] downlink
    icmp { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ icmp_type [ icmp_code ] ]

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
downlink

Apply this rule definition only to packets in the downlink (from the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
icmp_type

Specifies that all ICMP packets of a particular type are to be filtered. The type can be an integer value from 0 through 255.
icmp_code

Specifies that all ICMP packets of a particular code are to be filtered. The type can be an integer value from 0 through 255.
Usage:

Define a rule definition to block ICMP packets which can be used for address resolution and possibly be a security risk.

The IP redirecting allows flexible controls for pairs of individual hosts or groups by IP masking which allows the redirecting of entire subnets if necessary.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service named css-svc1, and ICMP packets coming in the downlink (from the Mobile Node) direction from the host with the IP address 2002::c6a2:6419:

    redirect css service
    css-svc1 downlink icmp host 2002::c6a2:6419

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 downlink icmp host 2002::c6a2:6419

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service css-svc1 downlink icmp host 2002::c6a2:6419

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 downlink icmp host 2002::c6a2:6419

redirect css service (for downlink, by IP packets)

Used to redirect subscriber sessions based on the internet protocol packets in the downlink (from the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] downlink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]after redirect css
    service svc_name [ log ] downlink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]before redirect css
    service svc_name [ log ] downlink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]no redirect css service svc_name [ log ] downlink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be a string of 1 through 15 characters.
downlink

Apply this rule definition only to packets in the downlink (from the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
fragment

Indicates packet redirection is to be applied to IP packet fragments only.
Usage:

Block IP packets when the source and destination are of interest.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service named css-svc1, and downlink IP packets coming from the host with the IP address 2002::c6a2:6419, and fragmented packets for any destination are matched:

    redirect css service
    css-svc1 downlink ip host 2002::c6a2:6419 any fragment

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 downlink ip host 2002::c6a2:6419 any fragment

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service css-svc1 downlink ip host 2002::c6a2:6419 any fragment

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 downlink ip host 2002::c6a2:6419 any fragment

redirect css service (for downlink, by source IP address masking)

Used to redirect subscriber sessions based on the IP address mask sent by the source in the downlink (from the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] downlink source_address
    source_wildcardafter redirect css
    service svc_name [ log ] downlink source_address source_wildcardbefore redirect css
    service svc_name [ log ] downlink source_address source_wildcardno redirect css service svc_name [ log ] downlink source_address source_wildcard

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
downlink

Apply this rule definition only to packets in the downlink (from the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
Usage:

Define a rule definition when any packet from the IP addresses which fall into the group of addresses matching the IP address masking. This allows the reduction of filtering rule definitions as it does not require a rule definition for each source and destination pair.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL.
Example:
The following command defines a rule definition to redirect packets to a charging service named css-svc1:

    redirect css service
    css-svc1 donwlink fe80::c0a8:a04

redirect css service (for downlink, by TCP/UDP packets)

Used to redirect subscriber sessions to a charging service based on the transmission control protocol/user datagram protocol packets in the downlink (from the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] downlink { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port end_source_port ] } { { dest_address dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }after redirect css
    service svc_name [ log ] downlink { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }after redirect css
    service svc_name [ log ] downlink { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }no redirect css service svc_name [ log ] downlink { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
downlink

Apply this rule definition only to packets in the downlink (from the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
tcp | udp

Specifies the redirect is to be applied to IP-based transmission control protocol or the user datagram protocol.

- tcp: Redirect applies to TPC packets.
- udp: Redirect applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer value from 0 to 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
range start_source_port end_source_port

Specifies that all source TCP ports within a specific range are to be filtered.

start_source_port is the initial port in the range and end_source_port is the final port in the range.

Both start_source_port and end_source_port can be configured to an integer value from 0 to 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
range start_dest_port end_dest_port

Specifies that all destination TCP ports within a specific range are to be filtered.

start_dest_port is the initial port in the range and end_dest_port is the final port in the range.

Both start_dest_port and end_dest_port can be configured to an integer value from 0 to 65535.
Usage:

Block IP packets when the source and destination are of interest but for only a limited set of ports.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service named css-svc1, and UDP packets coming from any host are matched:

    redirect css service
    css-svc1 downlink udp any

The following sets the insertion point to before the rule definition above:

    before redirect css
    service css-svc1 downlink udp any

The following command sets the insertion point after the rule definition above:

    after redirect css
    service css-svc1 downlink udp any

The following deletes the rule definition above:

    no redirect css service
    css-svc1 downlink udp any

redirect css service (for uplink, any)

Used to redirect subscriber sessions based on any packet received in the uplink (to the Mobile Node) direction. This command is also used to set the access control list insertion point.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] uplink anyafter redirect css
    service svc_name [ log ] uplink
    anybefore redirect css
    service svc_name [ log ] uplink
    anyno redirect css service svc_name [ log ] uplink any

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
any

Indicates all packets will match the redirect regardless of source and/or destination.
Usage:

Define a catch all rule definition to place at the end of the list of rule definitions to provide explicit handling of rule definitions which do not fit any other criteria.

IMPORTANT:

It is suggested that any rule definition which is added to be a catch all should also have the log option specified. The logged packets may be used to determine if the current list of rule definitions is adequate or needs modification to ensure proper security.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL.

IMPORTANT:

Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service with the name css-svc1 and any source IP:

    redirect css service
    css-svc1 uplink any

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service css-svc1 uplink any

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service css-svc1 uplink any

The following deletes the first rule definition above:

    no redirect css service
    css-svc1 uplink any

redirect css service (for uplink, by host IP address)

Used to redirect subscriber sessions based on the targeted host IP address in the uplink (to the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] uplink
    host source_host_addressafter redirect css
    service svc_name [ log ] uplink
    host source_host_addressbefore redirect css
    service svc_name [ log ] uplink
    host source_host_addressno redirect css service svc_name [ log ] uplink
    host source_host_address

uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
after

Indicates all rule definitions defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must ben alphanumeric string of 1 through 15 characters.
uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
Usage:

Define a rule definition when a very specific remote host is to be blocked. In simplified networks where the access controls need only block a few hosts, this command allows the rule definitions to be very clear and concise.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service with the name css-svc1 and a host IP address of fe80::c0a8:c80b:

    redirect service css-svc1
    uplink host fe80::c0a8:c80b

The following sets the insertion point to before the first rule definition above:

    before redirect service
    css-svc1 uplink host fe80::c0a8:c80b

The following command sets the insertion point after the second rule definition above:

    after redirect service
    css-svc1 uplink host fe80::c0a8:c80b

The following deletes the first rule definition above:

    no redirect service
    css-svc1 uplink host fe80::c0a8:c80b

redirect css service (for uplink, by ICMP packets)

Used to redirect subscriber sessions based on the internet control message protocol packets in the uplink (to the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

redirect css service svc_name [ log ] uplink icmp { any | host source_host_address | source_address source_wildcard } { any | host dest_host_address | dest_address dest_wildcard } [ icmp_type [ icmp_code ] ]
after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the Content Service Steering (CSS) service to which packets are to be redirected. At the executive mode prompt, use the show css service all command to display the names of all configured CSS services.

svc_name must be an alphanumeric string of 1 through 15 characters.
uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
icmp_type

Specifies that all ICMP packets of a particular type are to be filtered. The type can be an integer value from 0 through 255.
icmp_code

Specifies that all ICMP packets of a particular code are to be filtered. The type can be an integer value from 0 through 255.
Usage:

Define a rule definition to block ICMP packets which can be used for address resolution and possibly be a security risk.

The IP redirecting allows flexible controls for pairs of individual hosts or groups by IP masking which allows the redirecting of entire subnets if necessary.

IMPORTANT:

A maximum of 16 rule definitions can be configured per ACL. Also note that “redirect” rule definitions are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule definition that redirects packets to the charging service named chgsvc1, and ICMP packets in the uplink (to the Mobile Node) direction from the host with the IP address 198.162.100.25:

    redirect css service
    chgsvc1 uplink icmp host 198.162.100.25

The following sets the insertion point to before the first rule definition above:

    before redirect css
    service chgsvc1 uplink icmp host 198.162.100.25

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service chgsvc1 uplink icmp host 198.162.100.25

The following deletes the first rule definition above:

    no redirect css service
    chgsvc1 uplink icmp host 198.162.100.25

redirect css service (for uplink, by IP packets)

Used to redirect subscriber sessions based on the internet protocol packets in the uplink (to the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] uplink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]after redirect css
    service svc_name [ log ] uplink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]before redirect css
    service svc_name [ log ] uplink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]no redirect css service svc_name [ log ] uplink
    ip { any | host source_host_address | source_address
    source_wildcard } { any | host dest_host_address | dest_address
    dest_wildcard } [ fragment ]

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.

IMPORTANT:

If the options specified do not exactly match an existing rule definition, the insertion point does not change.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the active charging service to which packets are to be redirected. At the executive mode prompt, use the show active-charging service all command to display the names of all configured charging services.

svc_name must be a string of 1 through 15 characters.
uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

fragment

Indicates packet redirection is to be applied to IP packet fragments only.
Usage:

Block IP packets when the source and destination are of interest.
Example:
The following command defines a rule definition that redirects packets to the charging service named chgsvc1, and uplink IP packets going to the host with the IP address 198.162.100.25, and fragmented packets for any destination are matched:

    redirect css service
    chgsvc1 uplink ip host 198.162.100.25 any fragment

The following sets the insertion point to before the first rule definition above:

    redirect css service
    chgsvc1 uplink ip host 198.162.100.25 any fragment

The following command sets the insertion point after the second rule definition above:

    after redirect css
    service chgsvc1 uplink ip host 198.162.100.25 any fragment

The following deletes the first rule definition above:

    no redirect css service
    chgsvc1 uplink ip host 198.162.100.25 any fragment

redirect css service (for uplink, by source IP address masking)

Used to redirect subscriber sessions based on the IP address mask sent by the source in the uplink (to the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

redirect css service svc_name [ log ] uplink source_address source_wildcard
after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the active charging service to which packets are to be redirected. At the executive mode prompt, use the show active-charging service all command to display the names of all configured charging services.

svc_name must be a string of 1 through 15 characters.
uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the filter are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

Usage:

Define a rule definition when any packet from the IP addresses which fall into the group of addresses matching the IP address masking. This allows the reduction of filtering rule definitions as it does not require a rule definition for each source and destination pair.
Example:
The following command defines a rule definition to redirect packets to a charging service named chgsvc1:

    redirect css service
    chgsvc1 uplink 1:1:1:1:1:1:1:1

redirect css service (for uplink, by TCP/UDP packets)

Used to redirect subscriber sessions to a charging service based on the transmission control protocol/user datagram protocol packets in the uplink (to the Mobile Node) direction.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect css service svc_name [ log ] uplink { tcp | udp } { { source_address
    source_wildcard | any | source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }after redirect css
    service svc_name [ log ] uplink { tcp | udp } { { source_address
    source_wildcard | any | source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }before redirect css
    service svc_name [ log ] uplink { tcp | udp } { { source_address
    source_wildcard | any | source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }no redirect css service svc_name [ log ] uplink { tcp | udp } { { source_address
    source_wildcard | any | source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port | range start_source_port
    end_source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port | range start_dest_port
    end_dest_port ] }

after

Indicates all rule definitions subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule definition which matches the exact options specified such that new rule definitions will be added, in order, after the matching rule definition.
before

Indicates all rule definitions subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule definition which matches the exact options specified such that new rule definitions will be added, in order, before the matching rule definition.
no

Removes the rule definition which exactly matches the options specified.
css service svc_name

The name of the active charging service to which packets are to be redirected. At the executive mode prompt, use the show active-charging service all command to display the names of all configured charging services.

svc_name must be a string of 1 through 15 characters.
uplink

Apply this rule definition only to packets in the uplink (to the Mobile Node) direction.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
tcp | udp

Specifies the redirect is to be applied to IP-based transmission control protocol or the user datagram protocol.

- tcp: Redirect applies to TPC packets.
- udp: Redirect applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

any

Specifies that the rule definition applies to all packets.
host

Specifies that the rule definition applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer value from 0 to 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
range start_source_port end_source_port

Specifies that all source TCP ports within a specific range are to be filtered.

start_source_port is the initial port in the range and end_source_port is the final port in the range.

Both start_source_port and end_source_port can be configured to an integer value from 0 to 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
range start_dest_port end_dest_port

Specifies that all destination TCP ports within a specific range are to be filtered.

start_dest_port is the initial port in the range and end_dest_port is the final port in the range.

Both start_dest_port and end_dest_port can be configured to an integer value from 0 to 65535.
Usage:

Block IP packets when the source and destination are of interest but for only a limited set of ports.
Example:
The following command defines a rule definition that redirects packets to the charging service named chgsvc1, and UDP packets coming from any host are matched:

    redirect css service
    chgsvc1 uplink udp any

The following sets the insertion point to before the rule definition above:

    before redirect css
    service chgsvc1 uplink udp any

The following command sets the insertion point after the rule definition above:

    after redirect css
    service chgsvc1 uplink udp any

The following deletes the rule definition above:

    no redirect css service
    chgsvc1 uplink udp any

redirect nexthop (by IP address masking)

Used to redirect subscriber sessions based on the IP address mask sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] source_address
    source_wildcardafter redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] source_address source_wildcardbefore redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] source_address source_wildcardno redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] source_address source_wildcard

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
nexthop nexthop_addr

The IP address to which the IP packets are redirected.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
interface interface_name

The name of the logical interface to which the packets should be redirected. interface_name must be an alpha and/or numeric string from 1 to 79 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
Usage:

Define a rule when any packet from the IP addresses which fall into the group of addresses matching the IP address masking. This allows the reduction of redirect rules as it does not require a rule for each source and destination pair.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the next hop host at 192.168.10.4, the context with the context ID of 23 and the source IP and wildcard of 198.162.22.0 and 0.0.0.31:

    redirect nexthop 192.168.10.4
    context 23 198.162.22.0 0.0.0.31

The following sets the insertion point to before the first rule defined above:

    before redirect nexthop
    192.168.10.4 context 23 198.162.22.0 0.0.0.31

The following command sets the insertion point after the second rule defined above:

    after redirect nexthop
    192.168.10.4 context 23 198.162.22.0 0.0.0.31

The following deletes the first rule defined above:

    no redirect nexthop
    192.168.10.4 context 23 198.162.22.0 0.0.0.31

redirect nexthop (any)

Used to redirect subscriber sessions based on any packet received. This command is also used to set the access control list insertion point.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] anyafter redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] anybefore redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] anyno redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] any

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
nexthop nexthop_addr

The IP address to which the IP packets are redirected.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
interface interface_name

The name of the logical interface to which the packets should be redirected. interface_name must be an alpha and/or numeric string from 1 to 79 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
any

Indicates all packets will match the redirect regardless of source and/or destination.
Usage:

Define a catch all rule to place at the end of the list of rules to provide explicit handling of rules which do not fit any other criteria.

IMPORTANT:

It is suggested that any rule which is added to be a catch all should also have the log option specified. The logged packets may be used to determine if the current list of rules is adequate or needs modification to ensure proper security. The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the next hop host at 192.168.10.4, the context with the context ID of 23 and any source IP:

    redirect nexthop 192.168.10.4
    context 23 any

The following sets the insertion point to before the first rule defined above:

    before redirect nexthop
    192.168.10.4 context 23 any

The following command sets the insertion point after the second rule defined above:

    after redirect nexthop
    192.168.10.4 context 23 any

The following deletes the first rule defined above:

    no redirect nexthop
    192.168.10.4 context 23 any

redirect nexthop (by host IP address)

Used to redirect subscriber sessions based on the targeted host IP address sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] host source_ip_addressafter redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] host source_ip_addressbefore redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] host source_ip_addressno redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] host source_ip_address

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
nexthop nexthop_addr

The IP address to which the IP packets are redirected.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
interface interface_name

The name of the logical interface to which the packets should be redirected. interface_name must be an alpha and/or numeric string from 1 to 79 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
Usage:

Define a rule when a very specific remote host is to be blocked. In simplified networks where the access controls need only block a few hosts, this command allows the rules to be very clear and concise.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the next hop host at 192.168.10.4, the context with the context ID of 23 and a host IP address of 192.168.200.11:

    redirect nexthop 192.168.10.4
    context 23 host 192.168.200.11

The following sets the insertion point to before the first rule defined above:

    before redirect nexthop
    192.168.10.4 context 23 host 192.168.200.11

The following command sets the insertion point after the second rule defined above:

    after redirect nexthop
    192.168.10.4 context 23 host 192.168.200.11

The following deletes the first rule defined above:

    no redirect nexthop
    192.168.10.4 context 23 host 192.168.200.11

redirect nexthop (by source ICMP packets)

Used to redirect subscriber sessions based on the internet control message protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] icmp { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]after redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] icmp { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]before redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] icmp { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]no redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] icmp { source_address source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ icmp_type [ icmp_code ] ]

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
nexthop nexthop_addr

The IP address to which the IP packets are redirected.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
interface interface_name

The name of the logical interface to which the packets should be redirected. interface_name must be an alpha and/or numeric string from 1 to 79 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
icmp_type

Specifies that all ICMP packets of a particular type are to be filtered. The type can be an integer value from 0 through 255.
icmp_code

Specifies that all ICMP packets of a particular code are to be filtered. The type can be an integer value from 0 through 255.
Usage:

Define a rule to block ICMP packets which can be used for address resolution and possible be a security risk.

The IP redirecting allows flexible controls for pairs of individual hosts or groups by IP masking which allows the redirecting of entire subnets if necessary.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the next hop host at fe80::c0a8:a04, the context with the context ID of 23, and ICMP packets coming from the host with the IP address 2002::c6a2:64195:

    redirect nexthop fe80::c0a8:a04
    context 23 icmp host 2002::c6a2:6419

The following sets the insertion point to before the first rule defined above:

    before redirect nexthop
    fe80::c0a8:a04 context 23 icmp host 2002::c6a2:6419

The following command sets the insertion point after the second rule defined above:

    after redirect nexthop
    fe80::c0a8:a04 context 23 icmp host 2002::c6a2:6419

The following deletes the first rule defined above:

    no redirect nexthop
    fe80::c0a8:a04 context 23 icmp host 2002::c6a2:6419

redirect nexthop (by IP packets)

Used to redirect subscriber sessions based on the internet protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] ip { source_address
    source_wildcard | any | host source_host_address } { dest_address
    dest_wildcard | any | host dest_host_address } [ fragment ] [ protocol num ]

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to be immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
nexthop nexthop_addr

The IP address to which the IP packets are redirected.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
interface interface_name

The name of the logical interface to which the packets should be redirected. interface_name must be an alphanumeric string from 1 through 79 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
fragment

Indicates packet redirection is to be applied to IP packet fragments only.
protocol num

Indicates that the packet filtering is to be applied to a specific protocol number.

num can be an integer from 0 through 255.
Usage:

Block IP packets when the source and destination are of interest.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
redirect nexthop (by TCP/UDP packets)

Used to redirect subscriber sessions based on the transmission control protocol/user datagram protocol packets sent by the source to the mobile node or the network.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port ] }after redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port ] }before redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port ] }no redirect nexthop nexthop_addr { context context_id | interface interface_name } [ log ] { tcp | udp } { { source_address
    source_wildcard | any | host source_host_address } [ eq source_port | gt source_port | lt source_port | neq source_port ] } { { dest_address
    dest_wildcard | any | host dest_host_address } [ eq dest_port | gt dest_port | lt dest_port | neq dest_port ] }

after

Indicates all rules defined subsequent to this command are to be inserted after the command identified by the exact options listed.

This moves the insertion point to immediately after the rule which matches the exact options specified such that new rules will be added, in order, after the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
before

Indicates all rules defined subsequent to this command are to be inserted before the command identified by the exact options listed.

This moves the insertion point to be immediately before the rule which matches the exact options specified such that new rules will be added, in order, before the matching rule.

IMPORTANT:

If the options specified do not exactly match an existing rule, the insertion point does not change.
no

Removes the rule which exactly matches the options specified.
nexthop nexthop_addr

The IP address to which the IP packets are redirected.
context context_id

The context identification number of the context to which packets are redirected. At the executive mode prompt, use the show context all command to display context names and context IDs.
interface interface_name

The name of the logical interface to which the packets should be redirected. interface_name must be an alphanumeric string from 1 through 79 characters.
log

Default: packets are not logged.

Indicates all packets which match the redirect are to be logged.
tcp | udp

Specifies the redirect is to be applied to IP-based transmission control protocol or the user datagram protocol.

- tcp: Redirect applies to TCP packets.
- udp: Redirect applies to UDP packets.

source_address

The IP address(es) form which the packet originated.

This option is used to filter all packets from a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this option. The range can then be configured using the source_wildcard parameter.
source_wildcard

This option is used in conjunction with the source_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the source_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB).
any

Specifies that the rule applies to all packets.
host

Specifies that the rule applies to a specific host as determined by its IP address.
source_host_address

The IP address of the source host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
dest_host_address

The IP address of the destination host to filter against expressed in IPv6 colon-separated-hexadecimal notation.
eq source_port

Specifies a single, specific source TCP port number to be filtered.

source_port must be configured to an integer value from 0 to 65535.
gt source_port

Specifies that all source TCP port numbers greater than the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
lt source_port

Specifies that all source TCP port numbers less than the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
neq source_port

Specifies that all source TCP port numbers not equal to the one specified are to be filtered.

source_port must be configured to an integer value from 0 to 65535.
dest_address

The IP address(es) to which the packet is to be sent.

This option is used to filter all packets to a specific IP address or a group of IP addresses.

When specifying a group of addresses, the initial address is configured using this parameter. The range can then be configured using the dest_wildcard parameter.
dest_wildcard

This option is used in conjunction with the dest_address option to specify a group of addresses for which packets are to be filtered.

The mask must be entered as a complement:

- Zero-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be identical.
- One-bits in this parameter mean that the corresponding bits configured for the dest_address parameter must be ignored.

IMPORTANT:

The mask must contain a contiguous set of one-bits from the least significant bit (LSB). Therefore, allowed masks are 0, 1, 3, 7, 15, 31, 63, 127, and 255. For example, acceptable wildcards are 0.0.0.3, 0.0.0.255, and 0.0.15.255. A wildcard of 0.0.7.15 is not acceptable since the one-bits are not contiguous.
eq dest_port

Specifies a single, specific destination TCP port number to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
gt dest_port

Specifies that all destination TCP port numbers greater than the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
lt dest_port

Specifies that all destination TCP port numbers less than the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
neq dest_port

Specifies that all destination TCP port numbers not equal to the one specified are to be filtered.

dest_port must be configured to an integer value from 0 to 65535.
Usage:

Block IP packets when the source and destination are of interest but for only a limited set of ports.

IMPORTANT:

The maximum number of rules that can be configured per ACL varies depending on how the ACL is to be used. For more information, refer to the Engineering Rules appendix in the System Administration Guide. Also note that “redirect” rules are ignored for ACLs applied to specific subscribers or all subscribers facilitated by a specific context.
Example:
The following command defines a rule that redirects packets to the next hop host at fe80::c0a8:a04, the context with the context ID of 23, and UDP packets coming from any host are matched:

    redirect nexthop fe80::c0a8:a04
    context 23 udp any

The following sets the insertion point to before the rule defined above:

    before redirect nexthop
    fe80::c0a8:a04 context 23 udp any

The following command sets the insertion point after the rule defined above:

    after redirect nexthop
    fe80::c0a8:a04 context 23 udp any

The following command deletes the first rule defined above:

    no redirect nexthop
    fe80::c0a8:a04 context 23 udp any