# show ps-network

This chapter includes the show ps-network command output tables.
show ps-network all status
Table 1. show ps-network all status Command Output Descriptions

Field | Description
--- | ---
PS Network name | Indicates the name of the Packet Switched (PS) network instance for which status is displayed.
Associated SCCP-Network | Indicates the name of the Signalling Connection Control Part (SCCP) network service instance which in associated with referecned PS network instance.
Associated GTPU Service | Indicates the name of the GTP-U service instance which in associated with referecned PS network instance.
GTPU Context Name | Indicates the name of the context in which GTP-U service instance is configured.
SGSN Point Code | Indicates the address of SGSN in SS7 point code notation which is serving the referenced PS network instance.
Status | Indicates the status of SGSN which is serving the referenced PS network instance.
Network Status | Indicates the status of network in which the referenced PS network instance is placed.
NRI | Indicates the Network Resource Identication (NRI) bit configuration status for the referenced PS network.
IDNNS | Indicates the Intra-Domain NAS Node Selector (IDNNS) configuration status for the referenced PS network to transport the NRI value.
CORE NODE MAP | Indicates the core node mapping configuration status for the referenced PS network.
Ranap Reset Ack Timer | The timer value, in seconds, that defines how long the HNB-GW waits for a RESET ACK message from the SGSN after transmitting a RESET message. This setting is used only if the HNB-GW Initiated RANAP Reset function is enabled.
Ranap Reset Maximum Retransmissions | Sets the maximum number of retries allowed for the HNB-GW to transmit a RANAP RESET message to the SGSN if the RESET ACK timer expires. This setting is used only if the HNB-GW Initiated RANAP Reset function is enabled.
Ranap Reset Guard Timer | The timer that the HNB-GW starts after receiving a RESET message from the PS core network. While this timer is running, the HNB-GW discards any new RESET messages that it receives.
Global RNC-Id | This group displays the information related to global Radio Network Controller settings for use by the PS core network for HNB-GW service(s) on a chassis. It is configured under the PLMN-ID.
MCC | The Mobile Country Code defined for use with this HNB-GW service. It consists of the first 3 digits of the Available Radio Network PLMN ID.
MNC | The Mobile Network Code defined for use with this HNB-GW service. It consists of the last 3 digits of the Available Radio Network PLMN ID.
Id | The Radio Network Controller ID provided to HNBs for use by the PS core network for this HNB-GW service. It is configured under the PLMN-ID