# DLCI Configuration Mode Commands

The DLCI configuration mode provides the commands to configure, bind and manage the DLCI associated with a specific port defined in the parent configuration mode, Channelized Port configuration mode.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
bind link

This command configures an association (binds) between an IP interface or a pre-configured routing SS7/Frame Relay link and the specific port being configured with the Channelized Port configuration commands.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] bind
    link peer-nsei nse_id ns-vci ns-vc_id

peer-nsei nse_id

Defines the end-point network service entity identifier (NSEI). The NSEI must be an integer from 0 to 65535.
ns-vc-id ns-vc_id

Defines the network service virtual circuit identifier (NSVCI). The NSVCI must be an integer from 0 to 65535.
no

Deletes the bind configuration from the Operator Policy.
Usage:

Bind this port to network service entity 2 and network service VC 234.

Example

Example

    bind link peer-nsei 2 ns-vci 234

end

Exits this sub-configuration mode and returns to the Exec mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Change the mode and return to the Exec mode.
exit

Exits the this sub-configuration mode and returns to the parent configuration mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Return to the previous configuration mode.
shaping

Defines egress traffic shaping to control flow for this DLCI.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    shaping typedefault shaping

shaping type
The following types of shaping provide flow management:

- cir: Commited Info Rate
- cir-eir: Commited Info Rate with Excess Rate
- ppr: Peak Packet Rate
- wfq: Weighted Fair Queuing

default

Resets the DLCI configuration to the system default.
Usage:

Use this command to identify the type of signal shaping to be used on the DLCI.

Example

Example

    shaping  cir

shutdown

Terminates all processes supporting the port or blocks the shutting down of the port. Conversely, this command with the no keyword enables the port.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] shutdown

no

Enables the port’s administrative state. When omitted the card is shutdown (removed from service).
Usage:

Shut down a port prior to re-cabling and/or other maintenance activities.

This command with the no keyword is required to bring a port into service.

Example

Example
Use the following command to disable the DLCI:

    no shutdown