# Out-Address Configuration Mode Commands

The Out-Address configuration mode provides the commands to configure the outgoing addresses for SCCP entities.
In this mode, the prompt line will appear similar to:

    [local]hostname(config-gtt-addrmap-outaddr-<name>)#

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the configuration mode and returns to the Exec mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the configuration mode and returns to the Global configuration mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Return to the Global configuration mode.
gt-address

Configures the SCCP short address.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    gt-address  gt_address

gt_address

A string of 1 to 15 digits to define the GT-address
Usage:

Define the GT-address

Example

Example

    gt-address 010405525397

gt-format

The GT-format provides four formats that can be used during GTT.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    gt-format format_num

format_num

1: Selects GT-format 1 options which include nature-of-address and odd/even. Once selected, the system enters GT-Format1 configuration mode.

2: Selects GT-format2 options which include translation-type. Once selected, the system enters GT-Format2 configuration mode.

3: Selects GT-format3 options which include encoding-scheme, numbering-plan3 and translation-type. Once selected, the system enters GT-Format1 configuration mode.

4: Selects GT-format4 options which include encoding-scheme, nature-of-address, numbering-plan, and translation-type. Once selected, the system enters GT-Format4 configuration mode.
Usage:

Select the a GT-format that include encoding-scheme as part of the GTT process.

Example

Example

    gt-format 3

ni-indicator

Configures the National and International indicator to use during the GTT process.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ni-indicator ni_ind

ni_ind
Select one of the following as the appropriate type of national indicator for the address structure:

- national
- international

Usage:

Select the international indicator to be used for out-going addresses.

Example

Example

    ni-indicator international

point-code

Selects and configures the SS7-type point code for use with the out-going address.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    point-code pt_code

pt_code

Enter 1 to 11 digits in the point code format predefined during variant selection of GTT association.
Usage:

Define an ITU point code to be used for out-going address processing.
Example:

    point-code 6.255.6

routing-indicator

Selects the type of routing and the indicator to be included in the out-going message.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    routing-indicator routing_ind

routing_ind
Select one of the following options:

- gt: Inserts an indicator that identifies routing based on global title.
- ssn: Inserts an indicator that identifies routing based on the subsystem number.

Usage:

Select global title as the appropriate routing indicator.

Example

Example

    routing-indicator gt

ssf

Selects the subservice field as factor in the out-going address processing. ssf sets the network indicator in the subservice field for SS7 Message Signal Units (MSUs). The indicator carried in the message’s routing information typically identifies the structure of the point code as a message from within a nation or as a message coming from outside the national - international.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ssf sub_svc_fld

sub_svc_fld
Select one of the following options:

- international: The network indicator identifies the message as international with a point code structure that does not match the national point code structure,
- national: The network indicator identifies the messages as having a national point code structure.
- reserved: Provides an alternate network indicator for national messages.
- spare: Provides an alternate network indicator for international messages.

Usage:

Select the international NI for inclusion in out-going address subservice fields.

Example

Example

    ssf international

ssn

Selects the subsystem number to be included in the out-going message.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ssn sub_sys_num

sub_sys_num

Enter an integer from 1 to 255.
Usage:

Use subsystem number 44 in the out-going address.

Example

Example

    ssn 44