# Global Configuration Mode Commands (threshold poll commands A - N)

This section includes the commands threshold poll 10sec-cpu-utilization interval through threshold poll npu-utilization interval.

The Global Configuration Mode is used to configure basic system-wide parameters.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
threshold poll 10sec-cpu-utilization interval

Configures the polling interval over which to measure a 10-second average of CPU utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll 10sec-cpu-utilization
    interval duration

    default threshold
    poll 10sec-cpu-utilization interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPUUtilization10Sec command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the 10-second CPU utilization threshold:

    threshold poll 10sec-cpu-utilization 600

threshold poll a11-ppp-send-discard interval

Configures the polling interval for PDSN service over which to count the number of packets that the PPP protocol processing layer internally discarded on transmit for any reason.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll a11-ppp-send-discard intervalduration

    default threshold poll
    a11-ppp-send-discard interval

default

Restores the specified parameter to its default value 0 seconds.
interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 900 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNSvcA11PPPSendDiscard command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the A11 PPP send discard threshold:

    threshold poll a11-ppp-send-discard
    interval 600

threshold poll a11-rac-msg-discard interval

Configures the polling interval for PDSN service over which to count the number of Discarded A11 Registration Acknowledgements.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll a11-rac-msg-discard intervalduration

    default threshold poll
    a11-rac-msg-discard interval

default

Restores the specified parameter to its default value 0 seconds.
interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 900 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNSvcA11RACMsgDiscard command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the A11 RAC message discard threshold:

    threshold poll a11-rac-msg-discard
    interval 600

threshold poll aa11-rrp-failure interval

Configures the polling interval for PDSN service over which to count A11 Registration Response failures.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll a11-rrp-failure
    interval duration

    default threshold poll
    a11-rrp-failure interval

default

Restores the specified parameter to its default value 0 seconds.
interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 900 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNSvcA11RRPFailure command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the A11 RRP failure threshold:

    threshold poll a11-rrp-failure
    interval 600

threshold poll a11-rrq-msg-discard interval

Configures the polling interval for PDSN service over which to count how many A11 Registration Request messages are discarded.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll a11-rrq-msg-discard intervalduration

    default threshold poll
    a11-rrq-msg-discard interval

default

Restores the specified parameter to its default value 0 seconds.
interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 900 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshPDSNSvcA11RRQMsgDiscard command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the A11 RRQ message discard threshold:

    threshold poll a11-rrq-msg-discard
    interval 600

threshold poll aaa-acct-archive-size interval

Configures the polling interval over which to count archived AAA accounting messages.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaa-acct-archive-size
    interval duration

    default threshold
    poll aaa-acct-archive-size interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.
Example:
The following command configures the polling interval to 600 seconds for the AAA accounting archive size threshold:

    threshold poll aaa-acct-archive-size
    interval 600

threshold poll aaa-acct-failure interval

Configures the polling interval over which to count failed AAA accounting requests.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaa-acct-failure
    interval duration

    default threshold
    poll aaa-acct-failure interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshAAAAcctFail command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the AAA accounting failure threshold:

    threshold poll aaa-acct-failure
    interval 600

threshold poll aaa-acct-failure-rate interval

Configures the polling interval over which to measure the percentage of AAA accounting failures.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaa-acct-failure-rate
    interval duration

    default threshold
    poll aaa-acct-failure-rate interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshAAAAcctFailRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the AAA accounting failure rate threshold:

    threshold poll aaa-acct-failure-rate
    interval 600

threshold poll aaa-auth-failure interval

Configures the polling interval over which to count failed authentication requests.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaa-auth-failure
    interval duration

    default threshold
    poll aaa-auth-failure interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshAAAAuthFail command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the AAA authentication failure threshold:

    threshold poll aaa-auth-failure
    interval 600

threshold poll aaa-auth-failure-rate interval

Configures the polling interval over which to measure the percentage of AAA authentication failures.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaa-auth-failure-rate
    interval duration

    default threshold
    poll aaa-auth-failure-rate interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshAAAAuthFailRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the AAA authentication failure rate threshold:

    threshold poll aaa-auth-failure-rate
    interval 600

threshold poll aaa-retry-rate interval

Configures the polling interval over which to measure the percent of AAA request message retries.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaa-retry-rate
    interval duration

    default threshold
    poll aaa-retry-rate interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshAAARetryRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the AAA retry rate threshold:

    threshold poll aaa-retry-rate
    interval 600

threshold poll aaamgr-request-queue interval

Configures the polling interval over which to count the number of AAA Manager Requests for each AAA manager process.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll aaamgr-request-queue
    interval duration

    default threshold
    poll aaamgr-request-queue interval

default

Restores the specified parameter to its default value 0 seconds.
interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshAAAMgrQueue command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the AAA manager request queue threshold:

    threshold poll aaamgr-request-queue
    interval 600

threshold poll active-subscriber interval

Configures the polling interval over which to count the total number of active subscriber sessions.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll active-subscriber intervalduration

    default threshold
    poll active-subscriber interval

default

Restores the specified parameter to its default value 300 seconds.
interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSubscriberActive command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the active subscriber threshold:

    threshold poll active-subscriber
    interval 600

threshold poll asngw-auth-failure interval

Configures the polling interval over which to count or measure the thresholding value for ASN Gateway authentication failure.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asngw-auth-failure
    interval durdefault threshold poll
    asngw-auth-failure interval

default

Restores the specified parameter to its default value 300 seconds.
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWAuthFail command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the ASN Gateway authentication failure threshold:

    threshold poll asngw-auth-failure
    interval 600

threshold poll asngw-handoff-denial interval

Configures the polling interval over which to count or measure the thresholding value for ASN Gateway hand-off denial.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asngw-handoff-denial
    interval durdefault threshold poll
    asngw-handoff-denial interval

default

Restores the specified parameter to its default value 300 seconds.
interval dur

Default: 300 seconds.

Specifies the polling interval time in seconds.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWHandoffDenial command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the hand-off denial threshold:

    threshold poll asngw-handoff-denial
    interval 600

threshold poll asngw-max-eap-retry interval

Configures the polling interval over which to count or measure the thresholding value for maximum Extensible Authentication Protocol (EAP) authentication retries.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asngw-max-eap-retry
    interval durdefault threshold poll
    asngw-max-eap-retry interval

default

Restores the specified parameter to its default value 300 seconds.
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWMaxEAPRetry command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the maximum EAP authentication retry threshold:

    threshold poll asngw-max-eap-retry
    interval 600

threshold poll asngw-network-entry-denial interval

Configures the polling interval over which to count or measure the thresholding value for network entry denial to an MS.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asngw-network-entry-denial interval durdefault threshold poll
    asngw-network-entry-denial interval

default

Restores the specified parameter to its default value 300 seconds.
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWNWEntryDenial command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the network entry denial threshold:

    threshold poll asngw-network-entry-denial interval
    600

threshold poll asngw-session-setup-timeout interval

Configures the polling interval over which to count or measure the thresholding value for session setup timeout.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asngw-session-setup-timeout interval durdefault threshold poll
    asngw-session-setup-timeout interval

default

Restores the specified parameter to its default value 300 seconds.
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWSessSetupTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the session setup timeout threshold:

    threshold poll asngw-session-setup-timeout interval
    600

threshold poll asngw-session-timeout interval

Configures the polling interval over which to count or measure the thresholding value for session timeout.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asngw-session-timeout
    interval durdefault threshold poll
    asngw-session-timeout interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNGWSessTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the session timeout threshold:

    threshold poll asngw-session-timeout
    interval 600

threshold poll asnpc-idle-mode-timeout interval

Configures the polling interval over which to count the number of ASNPC Instant Messenger idle mode timeouts.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asnpc-idle-mode-timeout
    interval durdefault threshold poll
    asnpc-idle-mode-timeout interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNPCIdleModeTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the idle mode timeout threshold:

    threshold poll asnpc-idle-mode-timeout
    interval 600

threshold poll asnpc-im-entry-denial interval

Configures the polling interval over which to count the number of ASNPC Instant Messenger entry denials.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asnpc-im-entry-denial
    interval durdefault threshold poll
    asnpc-im-entry-denial interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNPCImEntryDenial command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the IM entry denial threshold:

    threshold poll asnpc-im-entry-denial
    interval 600

threshold poll asnpc-lu-denial interval

Configures the polling interval over which to count the number of ASNPC Location Update (LU) denials.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asnpc-lu-denial
    interval durdefault threshold poll
    asnpc-lu-denial interval interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNPCLuDenial command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the LU denial threshold:

    threshold poll asnpc-lu-denial
    interval 600

threshold poll asnpc-session-setup-timeout interval

Configures the polling interval over which to count the number of times an ASNPC session timed out before setup completion.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll asnpc-session-setup-timeout intervaldurdefault threshold poll
    asnpc-session-setup-timeout interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshASNPCSessSetupTimeout command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the session setup timeout threshold:

    threshold poll asnpc-session-setup-timeout interval
    600

threshold poll available-ip-pool-group interval

Configures the polling interval over which to measure IP pool utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll available-ip-pool-group
    interval durdefault threshold poll
    available-ip-pool-group interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPPoolAvail command in this mode.
Example:
The following command configures the polling interval to 600 seconds for available IP pool threshold:

    threshold poll available-ip-pool-group
    interval 600

threshold poll call-reject-no-resource interval

Configures the polling interval over which to measure IP pool utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll call-reject-no-resource intervaldurdefault threshold poll
    call-reject-no-resource interval

default

Restores the specified parameter to its default value (900 seconds).
interval dur

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCallRejectNoResource command in this mode.
Example:
The following command configures the polling interval to 600 seconds for call reject no-resource threshold:

    threshold poll call-reject-no-resource
    interval 600

threshold poll call-setup interval

Configures the polling interval over which to count the number of calls that were setup.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll call-setup intervaldurdefault threshold poll
    call-setup interval

default

Restores the specified parameter to its default value (900 seconds).
interval dur

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCallSetup command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the call setup threshold:

    threshold poll call-setup
    interval 600

threshold poll call-setup-failure interval

Configures the polling interval over which to count the number of calls that failed to setup.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll call-setup-failure intervaldurdefault threshold poll
    call-setup-failure interval

default

Restores the specified parameter to its default value (900 seconds).
interval dur

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 30 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCallSetupFailure command in this mode.
Example:
The following command configures the polling interval to 600 seconds for call setup failure threshold:

    threshold poll call-setup-failure
    interval 600

threshold poll call-setup-failures interval

Configures the polling interval over which to count the number of CSCF call setup failures.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll call-setup-failures intervaldurdefault threshold poll
    call-setup-failures interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcTotalCallFailure command in this mode.
Example:
The following command configures the polling interval to 600 seconds for CSCF session timeout threshold:

    threshold poll call-setup-failures
    interval 600

threshold poll call-total-active interval

Configures the polling interval over which to count the total number of CSCF active calls.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll call-total-active intervaldurdefault threshold poll
    call-total-active interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcTotalActiveCalls command in this mode.
Example:
The following command configures the polling interval to 600 seconds for session timeout threshold:

    threshold poll call-total-active
    interval 600

threshold poll card-temperature-near-power-off-limit interval

Configures the polling interval over which to count the number of times card temperatures reached the power-off limit.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll card-temperature-near-power-off-limit
    intervaldurdefault threshold poll
    card-temperature-near-power-off-limit interval

default

Restores the specified parameter to its default value (300 seconds).
interval dur

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

dur is an integer from 60 through 60000 in multiples of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCardTemperatureNearPowerOffLimit command in this mode.
Example:
The following command configures the polling interval to 600 seconds for session timeout threshold:

    threshold poll card-temperature-near-power-off-limit
    interval 600

threshold poll cdr-file-space interval

Configures the polling interval for Charging Data Record (CDR) File Space Usage threshold.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cdr-file-space
    interval duration

    default threshold poll
    cdr-file-space interval

default

Uses the default polling interval.

Default: 300 seconds
interval duration

Specifies the polling interval (in seconds) for the CDR File Space Usage threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the polling interval for CDR File Space Usage threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCDRFileSpace command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CDR file space usage threshold:

    threshold poll cdr-file-space
    interval 600

threshold poll contfilt-block interval

Configures the polling interval Content Filtering Block threshold.
Platform:

ASR 5000
Product:

CF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll contfilt-block
    interval duration

    default threshold poll
    contfilt-block interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval duration

Specifies the polling interval (in seconds) for the Content Filtering Block threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the polling interval Content Filtering Block threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshContFiltBlock command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the content filtering blocking threshold:

    threshold poll contfilt-block
    interval 600

threshold poll contfilt-rating interval

Configures the polling interval for the Content Filtering Rating threshold.
Platform:

ASR 5000
Product:

CF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll contfilt-rating
    interval durationdefault threshold poll
    contfilt-rating interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the polling interval (in seconds) for the Content Filtering Rating threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the polling interval for the Content Filtering Rating threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshContFiltRating command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the content filtering rating processing threshold:

    threshold poll contfilt-rating
    interval 600

threshold poll cpu-available-memory interval

Configures the polling interval over which to measure the percentage of total packet processing card CPU memory used.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-available-memory intervaldurationdefault threshold poll
    cpu-available-memory interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPUMemory command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU available memory threshold:

    threshold poll cpu-available-memory
    interval 600

threshold poll cpu-load interval

Configures the polling interval over which to monitor packet processing card CPU loads using a 5-minute average measurement.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-load intervaldurationdefault threshold poll
    cpu-load interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPULoad command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU load threshold:

    threshold poll cpu-load
    interval 600

threshold poll cpu-memory-usage interval

Configures the polling interval over which to measure the percentage of total packet processing card CPU memory used.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-memory-usage
    interval durationdefault threshold poll
    cpu-memory-usage interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPUMemUsage command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU memory usage threshold:

    threshold poll cpu-memory-usage
    interval 600

threshold poll cpu-orbs-crit interval

Configures the polling interval over which to measure the percentage of CPU utilization by the ORBS software task for critical-level alerts.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-orbs-crit
    interval durationdefault threshold poll
    cpu-orbs-crit interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPUOrbsCritical command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU ORBS critical threshold:

    threshold poll cpu-orbs-crit
    interval 600

threshold poll cpu-orbs-warn interval

Configures the polling interval over which to measure the percentage of CPU utilization by the ORBS software task for warning-level alerts.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-orbs-warn
    interval durationdefault threshold poll
    cpu-orbs-warn interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPUOrbsWarn command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU ORBS warning threshold:

    threshold poll cpu-orbs-warn
    interval 600

threshold poll cpu-session-throughput interval

Configures the polling interval over which to measure total throughput for all Session Manager tasks running on each packet processing card CPU.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-session-throughput
    interval durationdefault threshold poll
    cpu-session-throughput interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshSessCPUThroughput command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU session throughput threshold:

    threshold poll cpu-session-throughput
    interval 600

threshold poll cpu-utilization interval

Configures the polling interval over which to measure the percentage of CPU utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cpu-utilization
    interval durationdefault threshold poll
    cpu-utilization interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCPUUtilization command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CPU utilization threshold:

    threshold poll cpu-utilization
    interval 600

threshold poll cscf-invite-rcvd interval

Configures the polling interval in seconds over which to count the invitations received for Call State Control Function (CSCF) calls.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cscf-invite-rcvd
    interval durationdefault threshold poll
    cscf-invite-rcvd interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcCallsPerInterval command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF call invite threshold:

    threshold poll cscf-invite-rcvd
    interval 600

threshold poll cscf-reg-rcvd interval

Configures the polling interval in seconds over which to count the registrations received for Call State Control Function (CSCF) calls.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cscf-reg-rcvd
    interval durationdefault threshold poll
    cscf-reg-rcvd interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcRegPerInterval command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF call registrations threshold:

    threshold poll cscf-reg-rcvd
    interval 600

threshold poll cscf-service-route-failures interval

Configures the polling interval in seconds over which to count the CSCF service route failures.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll cscf-service-route-failures interval durationdefault threshold poll
    cscf-service-route-failures interval

default

Uses the default threshold polling interval.

Default: 300 seconds
interval dur

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcRouteFailures command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF service route failures threshold:

    threshold poll cscf-service-route-failures interval
    600

threshold poll dcca-bad-answers interval

Configures the polling interval for DCCA Bad Answers threshold—invalid or bad response to the system from the Diameter server.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll dcca-bad-answers
    interval duration

    default threshold poll
    dcca-bad-answers interval

default

Uses the default threshold polling interval.

Default: 900 seconds
interval duration

Specifies the polling interval (in seconds) for the DCCA Bad Answers threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the poling interval for DCCA Bad Answers threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholding in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshDCCABadAnswers command in this mode.
Example:
The following command configures the polling interval to 600 seconds for invalid or bad response threshold to the system from Diameter server:

    threshold poll dcca-rating-failed
    interval 600

threshold poll dcca-protocol-error interval

Configures the polling interval for Diameter Credit-Control Application (DCCA) Protocol Error threshold.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll dcca-protocol-error
    interval duration default threshold poll
    dcca-protocol-error interval

default

Uses the default threshold polling interval.

Default: 900 seconds
interval duration

Specifies the polling interval (in seconds) for the DCCA Protocol Error threshold.

duration must be an integer from 60 through 60000.
Usage:

Use this the polling interval for DCCA Protocol Error threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholding in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshDCCAProtocolError command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the DCCA protocol error threshold:

    threshold poll dcca-protocol-error
    interval 600

threshold poll dcca-rating-failed interval

Configures the polling interval for Diameter Credit-Control Application (DCCA) Rating Failed threshold.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll dcca-rating-failed
    interval duration

    default threshold poll
    dcca-rating-failed interval

default

Uses the default polling interval.

Default: 900 seconds
interval duration

Specifies the polling interval (in seconds) for the DCCA Rating Failed threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the polling interval for DCCA Rating Failed threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholding in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshDCCARatingFailed command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the Diameter Credit Control Application (DCCA) Rating Group (content-id) request reject thresholds:

    threshold poll dcca-rating-failed
    interval 600

threshold poll dcca-unknown-rating-group interval

Configures the polling interval for Diameter Credit-Control Application (DCCA) Unknown Rating Group threshold.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll dcca-unknown-rating-group interval duration

    default threshold poll
    dcca-unknown-rating-group interval

default

Uses the default polling interval.

Default: 900 seconds
interval duration

Specifies the polling interval (in seconds) for the DCCA Unknown Rating Group threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the polling interval for DCCA Unknown Rating Group threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholding in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshDCCAUnknownRatingGroup command in this mode.
Example:
The following command configures the polling interval to 600 seconds to threshold for the unknown DCCA Rating Group (content-id) returned by Diameter to system:

    threshold poll dcca-unknown-rating-group interval
    600

threshold poll dereg-reply-error interval

Configures the polling interval to count the number of de-registration reply errors per HA service.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll dereg-reply-error
    interval duration

    default threshold poll
    dereg-reply-error interval

default

Uses the default polling interval.

Default: 300 seconds
interval duration

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000. The input will be rounded up to the closest multiple of 30.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands in this chapter for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHASvcDeregReplyError command in this mode.
Example:
The following command configures the HA de-registration reply error threshold polling interval to 600 seconds:

    threshold poll dereg-reply-error
    interval 600

threshold poll diameter-retry-rate interval

Configures the polling interval for the Diameter Credit-Control Application (DCCA) Diameter Retry Rate threshold.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll diameter-retry-rate
    interval duration

    default threshold poll
    diameter-retry-rate interval

default

Uses the default polling interval.

Default: 300 seconds
interval duration

Specifies the polling interval (in seconds) for the Diameter Retry Rate threshold.

duration must be an integer from 60 through 60000. The input will be rounded up to the closest multiple of 30.
Usage:

This command specifies the polling interval for Diameter Retry Rate threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands in this chapter for additional information on the system’s support for thresholding.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshDiameterRetryRate command in this mode.
Example:
The following command configures the Diameter Retry Rate threshold polling interval to 600 seconds:

    threshold poll diameter-retry-rate
    interval 600

threshold poll edr-file-space interval

Command configures the polling interval for Event Data Record (EDR) File Space Usage threshold.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll edr-file-space
    interval duration

interval duration

Default: 300 seconds.

Specifies the polling interval (in seconds) for the EDR File Space Usage threshold.

duration must be an integer from 60 through 60000.
Usage:

This command configures the polling interval for EDR File Space Usage threshold.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshEDRFileSpace command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the EDR file space usage threshold:

    threshold poll edr-file-space
    interval 600

threshold poll edr-udr-dropped-flow-control interval

Configures the polling interval to count the total number of Event Data Records (EDRs) and Usage Data Records (UDRs) discarded due to ACSMGR flow control.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll edr-udr-dropped-flow-control interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.
Example:
The following command configures the polling interval to 600 seconds for the EDR/UDR drops due to flow control threshold:

    threshold poll edr-udr-dropped-flow-control interval
    600

threshold poll epdg-current-sessions interval

Configures the polling interval to count the total number of subscribers currently in Evolved Packet Date Gateway (ePDG) sessions.
Platform:

ASR 5000
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll epdg-current-sessions
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshEPDGCurrSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the ePDG sessions threshold:

    threshold poll epdg-current-sessions
    interval 600

threshold poll error-no-resource interval

Configures the polling interval in seconds over which to count CSCF No Resource Errors.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll error-no-resource
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcErrorNoResource command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF No Resource Errors threshold:

    threshold poll error-no-resource
    interval 600

threshold poll error-presence interval

Configures the polling interval in seconds over which to count CSCF Presence Errors.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll error-presence
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcErrorPresence command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF Presence Errors threshold:

    threshold poll error-presence
    interval 600

threshold poll error-reg-auth interval

Configures the polling interval in seconds over which to count CSCF Reg-Auth Errors.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll error-reg-auth
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcErrorRegAuth command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF Reg-Auth Errors threshold:

    threshold poll error-reg-auth
    interval 600

threshold poll error-tcp interval

Configures the polling interval in seconds over which to count CSCF TCP Errors.
Platform:

ASR 5000
Product:

SCM
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll error-tcp
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshCSCFSvcErrorTcp command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the CSCF TCP Errors threshold:

    threshold poll error-tcp
    interval 600

threshold poll fa-reg-reply-error interval

Configures the polling interval over which to measure the number of registration reply errors for Foreign Agent (FA) services.
Platform:

ASR 5000
Product:

FA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fa-reg-reply-error
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFASvcRegReplyError command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the FA registration reply errors threshold:

    threshold poll fa-reg-reply-error
    interval 600

threshold poll fng-current-active-sessions interval

Configures the polling interval in seconds over which to count Femto Network Gateway (FNG) current active sessions.
Platform:

ASR 5000
Product:

FNG
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fng-current-active-sessions interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFNGCurrActSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the FNG current active sessions threshold:

    threshold poll fng-current-active-sessions interval
    600

threshold poll fng-current-sessions interval

Configures the polling interval in seconds over which to count Femto Network Gateway (FNG) current sessions, including inactive sessions.
Platform:

ASR 5000
Product:

FNG
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fng-current-sessions
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFNGCurrSess command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the FNG current sessions threshold:

    threshold poll fng-current-sessions
    interval 600

threshold poll fw-deny-rule interval

Configures the Stateful Firewall Deny Rule threshold polling interval.
Platform:

ASR 5000
Product:

PSF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fw-deny-rule
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 900.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFWDenyRule command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the Stateful Firewall Deny Rule threshold:

    threshold poll fw-deny-rule
    interval 600

threshold poll fw-dos-attack interval

Configures the Stateful Firewall Denial of Service (DoS) Attacks threshold polling interval.
Platform:

ASR 5000
Product:

PSF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fw-dos-attack
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 900.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFWDosAttack command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the Stateful Firewall DoS Attacks threshold:

    threshold poll fw-dos-attack
    interval 600

threshold poll fw-drop-packet interval

Configures the Stateful Firewall Drop-Packet threshold polling interval.
Platform:

ASR 5000
Product:

PSF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fw-drop-packet
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 900.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFWDropPacket command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the Stateful Firewall Drop-Packet threshold:

    threshold poll fw-drop-packet
    interval 600

threshold poll fw-no-rule interval

Configures the Stateful Firewall No-Rule threshold polling interval.
Platform:

ASR 5000
Product:

PSF
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll fw-no-rule
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 900.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshFWNoRule command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the Stateful Firewall No-Rule threshold:

    threshold poll fw-no-rule
    interval 600

threshold poll ha-init-rrq-rcvd-rate interval

Configures the polling interval for Home Agent (HA) service over which to measure the average number of calls setup per minute.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ha-init-rrq-rcvd-rate
    interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 900.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHACallSetupRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of HA calls setup per minute:

    threshold poll ha-init-rrq-rcvd-rate
    interval 600

threshold poll ha-svc-init-rrq-rcvd-rate interval

Configures the polling interval over which to measure the average number of calls setup per minute for HA services.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ha-svc-init-rrq-rcvd-rate interval duration

interval duration

Default: 0 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 60 through 900.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshHASvcCallSetupRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of calls setup per minute for HA services:

    threshold poll ha-svc-init-rrq-rcvd-rate interval
    600

threshold poll ip-pool-free interval

Configures the polling interval over which to measure the percentage of the IP pool addresses that are in the Free state.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ip-pool-free
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPPoolFree command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of Free IP pools:

    threshold poll ip-pool-free
    interval interval 600

threshold poll ip-pool-hold interval

Configures the polling interval over which to measure the percentage of the IP pool addresses that are in the Hold state.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ip-pool-hold
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPPoolHold command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of IP pool addresses in Hold state:

    threshold poll ip-pool-hold
    interval 600

threshold poll ip-pool-release interval

Configures the polling interval over which to measure the percentage of IP pool addresses that are in the Release state.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ip-pool-release
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPPoolRelease command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of IP pool addresses in Release state:

    threshold poll ip-pool-release
    interval 600

threshold poll ip-pool-used interval

Configures the polling interval over which to measure the percentage of the IP pool addresses that are used.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ip-pool-used
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPPoolUsed command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of used IP pool addresses:

    threshold poll ip-pool-used
    interval 600

threshold poll ipsec-call-req-rej interval

Configures the polling interval over which to count the IPSec call requests that are rejected.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ipsec-call-req-rej
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPSECCallReqRej command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of rejected IPSec IKE calls:

    threshold poll ipsec-call-req-rej
    interval 600

threshold poll ipsec-ike-failrate interval

Configures the polling interval over which to count the IPSec IKE failure rate.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ipsec-ike-failrate
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPSECIKEFailRate command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average rate for IPSec IKE failures:

    threshold poll ipsec-ike-failrate
    interval 600

threshold poll ipsec-ike-failures interval

Configures the polling interval over which to count the number of IPSec IKE failures.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ipsec-ike-failures
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPSECIKEFailures command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of IPSec IKE failures:

    threshold poll ipsec-ike-failures
    interval 600

threshold poll ipsec-ike-requests interval

Configures the polling interval over which to count the number of IPSec IKE requests.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ipsec-ike-requests
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPSECIKERequests command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the average number of IPSec call requests:

    threshold poll ipsec-ike-requests
    interval 600

threshold poll ipsec-tunnels-established interval

Configures the polling interval over which to count the number of IPSec tunnels that have been established.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ipsec-tunnels-established interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPSECTunEstabl command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the number of established IPSec tunnels:

    threshold poll ipsec-tunnels-established interval
    600

threshold poll ipsec-tunnels-setup interval

Configures the polling interval over which to count the number of IPSec tunnels that have been setup.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll ipsec-tunnels-setup
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshIPSECTunSetup command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the number of IPSec tunnels that have been setup:

    threshold poll ipsec-tunnels-setup
    interval 600

threshold poll license-remaining-session interval

Configures the polling interval over which to measure session license utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll license-remaining-session interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshLicense command in this mode.
Example:
The following command configures the polling interval to 600 seconds for the utilization of session licenses:

    threshold poll license-remaining-session interval
    600

threshold poll mgmt-cpu-memory-usage interval

Configures the polling interval over which to measure management card CPU memory usage.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll mgmt-cpu-memory-usage
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.
Example:
The following command configures the polling interval to 600 seconds for management card CPU memory usage:

    threshold poll mgmt-cpu-memory-usage
    interval 600

threshold poll mgmt-cpu-utilization interval

Configures the polling interval over which to measure management card CPU utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll mgmt-cpu-utilization
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.
Example:
The following command configures the polling interval to 600 seconds for management card CPU memory usage:

    threshold poll mgmt-cpu-utilization
    interval 600

threshold poll mme-attach-failure interval

Configures the polling interval to count the MME Attach Failure messages across all MME services in the system.
Platform:

ASR 5000
Product:

MME
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll mme-attach-failure
    interval durdefault threshold poll
    mme-attach-failure interval

default

Restores the polling interval value to its default value of 900 seconds.
interval dur

Default: 900 seconds.

Specifies the polling interval (in seconds) for counting MME Attach Failure messages across all MME services in the system.

dur must be an integer from 30 through 60000 in multiples of 30.
Usage:

Use this command to configure the polling interval to count the MME Attach Failure messages across all MME services in the system to generate threshold value.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring mme-service and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshMMEAttachFail command in this mode.
Example:
The following command configures the polling interval of 600 seconds to count the MME Attach Failure messages for threshold limit:

    threshold poll mme-attach-failure
    interval 600

threshold poll mme-auth-failure interval

Configures the polling interval to count the MME Authentication Failure messages across all MME services in the system.
Platform:

ASR 5000
Product:

MME
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll mme-auth-failure
    interval durdefault threshold poll
    mme-auth-failure interval

default

Restores the specified poll interval value to its default value of 900 seconds.
interval dur

Default: 900 seconds.

Specifies the polling interval (in seconds) for counting MME Authentication Failure messages across all MME services in the system.

dur must be an integer from 30 through 60000 in multiples of 30.
Usage:

Use this command to configure the polling interval to count the MME Auth Failure messages across all MME services in the system to generate threshold value.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring mme-service and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshMMEAuthFail command in this mode.
Example:
The following command configures the polling interval of 600 seconds to count the MME Auth Failure messages for threshold limit:

    threshold poll mme-auth-failure
    interval 600

threshold poll nat-port-chunks-usage interval

Configures the polling interval over which to measure the percentage of Network Address Translation (NAT) port chunk utilization.
Platform:

ASR 5000
Product:

NAT
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll nat-port-chunks-usage
    interval duration

interval duration

Default: 900 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshNATPortChunksUsage command in this mode.
Example:
The following command configures the polling interval to 600 seconds for (NAT) port chunk utilization:

    threshold poll nat-port-chunks-usage
    interval 600

threshold poll npu-utilization interval

Configures the polling interval over which to measure the percentage of network processing unit (NPU) utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    threshold poll npu-utilization
    interval duration

interval duration

Default: 300 seconds.

Specifies the amount of time (in seconds) that comprises the polling interval.

duration must be an integer from 30 through 60000.
Usage:

This command sets the time period over which to monitor the specified value for threshold crossing.

IMPORTANT:

All configured polling intervals are rounded up to the closest multiple of 30. For example, if a polling interval is configured for 130 seconds, the system uses a polling interval of 150 seconds.

Refer to the threshold monitoring and other threshold commands for additional information on the system’s support for thresholds in this chapter.

IMPORTANT:

To enable an SNMP trap for monitoring this threshold use the snmp trap enable ThreshNPUUtilization command in this mode.
Example:
The following command configures the polling interval to 600 seconds for NPU utilization:

    threshold poll npu-utilization
    interval 600