# show cs-network

This chapter includes the show cs-network command output tables.
show cs-network all status
Table 1. show cs-network all status Command Output Descriptions

Field | Description
--- | ---
CS Network name | Indicates the name of the Circuit Switched (CS) network instance for which status is displayed.
Associated SCCP-Network | Indicates the name of the Signalling Connection Control Part (SCCP) network service instance which in associated with referecned CS network instance.
Associated Alcap-Service | Indicates the name of the Access Link Control Application Protocol (ALCAP) service instance which in associated with referecned CS network instance.
Alcap Context Name | Indicates the name of the context in which ALCAP service instance is configured.
Associated RTP Pool | Indicates the name of the RTP IP pool configured and associated with referecned CS network instance for RTP stream management.
RTP Pool Context Name | Indicates the name of the context in which RTP IP pool is configured for RTP stream management.
MSC Point Code | Indicates the address of MSC in SS7 point code notation which is serving the referenced CS network instance.
Status | Indicates the status of MSC which is serving the referenced CS network instance.
Network Status | Indicates the status of network in which the referenced CS network instance is placed.
RTP IP Addresses | Indicates the session manager instances and associated IP pools with them for RTP stream management support.
NRI | Indicates the Network Resource Identication (NRI) bit configuration status for the referenced CS network.
IDNNS | Indicates the Intra-Domain NAS Node Selector (IDNNS) configuration status for the referenced CS network to transport the NRI value.
Lac range <nnn> to <nnn> MSC Point-code <x.x.x> | Indicates the mapping configured between MSC point-code and range of LAC for multiple MSC selection without Iu-Flex in CS network.
CORE NODE MAP | Indicates the core node mapping configuration status for the referenced CS network.
Ranap Reset Ack Timer | The timer value, in seconds, that defines how long the HNB-GW waits for a RESET ACK message from the MSC after transmitting a RESET message. This setting is used only if the HNB-GW Initiated RANAP Reset function is enabled.
Ranap Reset Maximum Retransmissions | Sets the maximum number of retries allowed for the HNB-GW to transmit a RANAP RESET message to the MSC if the RESET ACK timer expires. This setting is used only if the HNB-GW Initiated RANAP Reset function is enabled.
Ranap Reset Guard Timer | The timer that the HNB-GW starts after receiving a RESET message from the CS core network. While this timer is running, the HNB-GW discards any new RESET messages that it receives.
Global RNC-Id | This group displays the information related to global Radio Network Controller settings for use by the CS core network for HNB-GW service(s) on a chassis. It is configured under the PLMN-ID.
MCC | The Mobile Country Code defined for use with this HNB-GW service. It consists of the first 3 digits of the Available Radio Network PLMN ID.
MNC | The Mobile Network Code defined for use with this HNB-GW service. It consists of the last 3 digits of the Available Radio Network PLMN ID.
Id | The Radio Network Controller ID provided to HNBs for use by the CS core network for this HNB-GW service. It is configured under the PLMN-ID