# Exec Mode show Commands (M-P)

This section includes the commands show mag-service through show ps-network statistics.

The Exec Mode is the initial entry point into the command line interface system. Exec mode show commands are useful in troubleshooting and basic system monitoring.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
show mag-service

Displays statistic and counter information for Mobile Access Gateway (MAG) services on this system.
Platform:

ASR 5000
Product:

HSGW, S-GW
Privilege:

Inspector
Syntax

    show mag-service { all | name service_name | session [ all | callid id | counters | full | ip-address home_ip_address | msid id | summary |
    username name ] | statistics [ name service_name ] } [ |  { grep grep_options | more } ]

all

Displays information for all configured MAG services on this system.
name service_name

Displays configuration information for a specific MAG service configured on this system.

service_name must be an existing MAG service expressed as an alphanumeric string of 1 through 63 characters.
session [ all | callid id | counters | full | ip-address home_ip_address | msid id | summary | username name ]

all: Displays all active MAG sessions using MAG services on the system.

callid id: Displays available session information for the specific call identification number.

id must be an 8-digit hexadecimal number.
counters: Displays counters for all MAG services on the system.This keyword can also be filtered by the following:

- all
- callid
- ip-address
- msid
- summary
- username

Refer to the keyword descriptions in this command for information regarding these filters.
full: Displays additional session information for all active MAG sessions using MAG services on the system. This keyword includes the information in the output of the all keyword plus additional information. This keyword can also be filtered by the following:

- all
- callid
- ip-address
- msid
- summary
- username

Refer to the keyword descriptions in this command for information regarding these filters.

ip-address home_ip_address: Displays available session information for a specific home IPv4 or IPv6 address of a subscriber in a service session.

msid id: Displays available information for a specific mobile station identification number or group of numbers based on wildcard entry.

id must be a valid MSID number and can be a sequence of characters and/or wildcard characters ('$' and/or '*'). The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as wildcard enclose them in single quotes ( ‘). For example: ‘$’.

summary: Displays the number of MAG sessions currently active for MAG services configured on the system.

username name: Displays available session information for a specific user in a service session.

name must be followed by an existing user name expressed as an alphanumeric string of 1 through 127 characters.
statistics [ name service_name ]

name service_name: Displays MAG service statistics for an existing MAG service specified as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

Use this command to view configuration information for MAG services on this system.
Example:
The following command displays service statistics for the MAG service named mag1:

    show mag-service name mag1

show map-service

Displays information configured for the Mobile Application Part (MAP) services, including MAP service features and operational configuration. Also includes some related configuration information for the HLR and EIR configuration parameters.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show map-service [ all | name srvc_name ] [ | { grep grep_options  | more } ]

name srvc_name

Specifies an existing MAP service as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

Use this command to display all MAP service or the statistics for a particular MAP service.
Example:
The following command displays configuration information for the MAP service named map-svc-1:

    show map-service name
    map-srv-1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show map statistics

Displays Mobile Application Part (MAP) statistics.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show map statistics [ name srvc_name [ | { grep grep_options  | more } ]

name srvc_name

Specifies an existing MAP service as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

Use this command to display all MAP statistics or the statistics for a particular MAP service.
Example:
The following command displays statistics for the MAP service named map-svc-1:

    show map statistics
    name map-svc-1

The following command displays combined statistics for all MAP services in the current context:

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show maximum-temperatures

Shows the maximum temperature reached by each card since the last temperature timestamp reset.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show maximum-temperatures [ verbose] [ | { grep grep_options | more } ]

verbose

Indicates that the output is to contain detailed information.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

Verify the maximum temperature reached by components in the chassis since the indicated timestamp.

IMPORTANT:

This command is not supported on all platforms.
Example:

    show maximum-temperatures

    show maximum-tempteratures verbose

show mbms bearer-service

Displays configuration information for bearer services configured for the multimedia broadcast multicast service (MBMS) running on this system.
Platform:

ASR 5000
Product:

GGSN, SGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show mbms bearer-service [ all ] [ apn apn_name mcast-addr ip_address ] [ full ] [ instance instance_id ] [ service-type { broadcast | multicast } ] [ sgsn-sessions ] [ summary ]  [ | { grep
    grep_options | more } ]

all

Displays information on all bearer services configured on the system.
apn apn_name mcast-addr ip_address

Displays bearer service information of the MBMS for a specific Access Point Name (APN). apn_name is bound to a given BM-SC (Broadcast Multicast - Service Center) server address ip_address.

apn_name is the name of the APN expressed as an alphanumeric string of 1 through 62 characters that is case sensitive.

ip_address is the IP address of the BM-SC server in IPv4 dotted-decimal notation bound to the APN.
full

Displays full information for specific or all instances of bearer service in MBMS feature on system.
instance instance_id

Displays session information filtered for an instance of a bearer service running as an MBMS session and specified an integer from 1 through 64.
service-type { broadcast | multicast }

Displays information for a specific type of service for MBMS.

broadcast: Specifies the MBMS service type as broadcast only.

multicast: Specifies the MBMS service type as multicast only.
sgsn-sessions

Displays summary information for all the SGSN multicast sessions.
summary

Displays summary information for specific or all instances of a bearer service.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more options, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

Use this command to verify the configuration of one or all bearer services and active instances of bearer services under MBMS. It is also useful for monitoring or troubleshooting purposes.

If this command is executed from within the local context with the all keyword, information for all bearer service instances running under MBMS will be displayed.
Example:
The following command displays configuration information for all bearer service instances running on system:

    show mbms bearer-service
    full all

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show mipfa

Displays information for specified Mobile IP Foreign Agent (MIP-FA) calls.
Platform:

ASR 5000
Product:

PDSN, GGSN, ASN-GW
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show mipfa { [ [ counters | full | summary ] { all |
    callid call_id | msid ms_id | peer-address [ operator ] peer_address | reverse-tunnel { on | off } |
    username user_name } | statistics [ fa-service fa_name | peer-address [ peer_address | greater-than peer_address | less-than peer_address | > peer_address | < peer_address ] } ] | peers
    fa-service service_name [ current-sessions
     { { > | greater-than } sessions [ < sessions ] |  { < | less-than } sessions [ > sessions ] | sessions } ]  [ peer-address address ] } [ | { grep grep_options | more } ]

counters | full | summary

counters: Displayed output includes the statistical counters.

full: Displays detailed information.

summary: Displays only summary information. this is the default setting.

These options are not available in conjunction with the statistics keyword.
all | callid call_id | msid ms_id | peer-address peer_ip_address | reverse-tunnel { on | off } | username user_name

all: Displays all available information.

callid call_id: Displays information only for calls with the call ID specified as a 4-byte hexadecimal number.

msid ms_id: Displays information for a mobile subscriber ID expressed as a string from 7 to 16 digits for an IMSI, MIN, or RMI and/or characters $ and * for wildcard filter.

show mipha msid 01234567$$

Shows any subscriber with an MSID that matches the upper 8 digits of the supplied MSID, such as 01234567, and any two digits at the remaining two places.

peer-address peer_ip_address: Displays information for the MIP call for the peer IP address specified using IPv4 dotted-decimal notation.

reverse-tunnel { on | off }: Enables the display of reverse IP tunnel information.

username user_name: Displays MIP call user information for the username specified as an alphanumeric string of 1 through 127 characters that may include wildcard characters ($ and *).
statistics [ fa-service fa_name | peer-address [ peer_address | greater-than peer_address | less-than peer_address | > peer_address | < peer_address ]

Displays information for the foreign agent service specified by name or peer IP address.

fa-service fa_name must be an alphanumeric string of 1 through 63 characters.

peer-address peer_address must be specified using IPv4 dotted-decimal notation.

greater-than peer_address: Specifies the range of IPv4 addresses greater than peer_address.

less-than peer_address: Specifies the range of IPv4 addresses less than peer_address.

> peer_address: Specifies the range of IPv4 addresses greater than peer_address.

< peer_address: Specifies the range of IPv4 addresses less than peer_address.
peer-address [ operator ] peer_address

In conjunction with the mipfa [ summary ] peer-address keyword, indicates a range of peers is to be displayed.

peer-address [ operator ] peer_address must be specified using IPv4 dotted-decimal notation.
operator implies how to logically specify a range of peer-address and it must be one of the following:

- <: IP address is less than the specified peer_address
- >: IP address is greater than the specified peer_address
- greater-than: IP address is greater than the specified peer_address
- less-than: IP address is less than the specified peer_address

peers fa-service service_name [ current-sessions { { > | greater-than } sessions [ < sessions ] | { < | less-than } sessions [ > sessions ] | sessions } ] [ peer-address address ]

Displays peer servers for the specified FA service.

fa-service service_name: Specifies the name of an existing FA service for which the associated peer servers are to be displayed as an alphanumeric string of 1 through 63 characters.
current-sessions: Displays only peer servers with current sessions meeting the following criteria:

- > | greater-than sessions: Displays only peer servers currently running sessions higher than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “greater-than” and the “>” symbol are interchangeable in this instance of the command.
- < sessions: Displays only peer servers that are currently running sessions l than the greater-than parameter but less than the value entered in this parameter. sessions must be an integer from 1 to 3000000.
- < | less-than sessions: Displays only peer servers currently running sessions lower than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “less-than” and the “<” symbol are interchangeable in this instance of the command.
- > sessions: Displays only peer servers that are currently running sessions lower than the less-than parameter but more than the value entered in this parameter. sessions must be an integer from 1 to 3000000.
- sessions: Displays only peer servers currently running sessions that are equal to the value entered in this parameter. sessions must be an integer from 1 to 3000000.

peer-address address: Displays only peer servers matching the IP address entered in this parameter. address must be specified using IPv4 dotted-decimal notation and can be followed by the netmask of the address.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

View MIP foreign agent information to support troubleshooting subscriber issues by viewing call information and filtering on the subscriber information using various methods.
Example:
The following displays the call information for all mobile IP FA calls and statistics for fa1, respectively:

    show mipfa all

The following command displays the statistics for the foreign agent service fa1:

    show mipfa statistics
    fa-service fa1

The following commands displays call information for user user6@aaa in full detail and in summary:

    show mipfa full username user6@aaa

    show mipfa summary
    username user1

The following displays MIP FA call information for calls from mobile subscriber 4412345678 and peer address 10.2.3.4, respectively:

    show mipfa msid 4412345678 4412345678

    show mipfa peer-address 10.2.3.4

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show mipha

Displays information for specified Mobile IP Home Agent (MIP-HA) calls.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show mipha { [ [ counters | full | summary ] { all |
    callid call_id | imsi imsi_num | ip-address ip_addr |  msid msid_num | peer-address [ operator ] peer_address | reverse-tunnel { on | off } | username user_name } | statistics [ ha-service ha_name | peer-address peer_address ] } ] | peers
    ha-service service_name [ current-sessions
     { { > | greater-than } sessions [ < sessions ] |  { < | less-than } sessions [ > sessions ] | sessions } ]  [ peer-address address ] } [ | { grep grep_options | more } ]

counters | full | summary

Default: concise output.

counters: Displayed output includes the statistical counters.

full: Displays detailed information.

summary: Displays only summary information.

These options are not available in conjunction with the statistics keyword.
msid msid_num

Displays information for the subscriber with the supplied MSID on HA.

msid msid_num specifies a mobile subscriber ID for which information is to be displayed. ms_id must be from 7 to 16 digits for an IMSI, MIN, or RMI and /or characters $ and * for wildcard filtering.

If enforce imsi-min equivalence is enabled on the chassis and MIN or IMSI numbers are supplied, this keyword/ filter will show subscribers with a corresponding MSID (MIN or IMSI) whose lower 10 digits matches the lower 10 digits of the supplied MSID.

show mipha msid ABCD0123456789 or

show mipha msid 0123456789

Shows any subscriber with a MSID that match the lower 10 digits of MSID supplied, such as 0123456789.

show mipha msid 01234567$$

Shows any subscriber with a MSID that match the upper 8 digits of the supplied MSID, such as 01234567 and any two digits at the remaining two places.
all | callid call_id | imsi imsi_num | ip-address ip_addr | msid msid_num | peer-address [ operator ] peer_address | reverse-tunnel { on | off } | username user_name

all: Displays all available information.

callid call_id: Displays information only for calls with the call ID specified as a 4-byte hexadecimal number.

imsi imsi_num: Specifies an IMSI (international mobile subscriber ID) for which information is to be displayed. The IMSI is a 15-character field which identifies the subscriber’s home country and carrier.

ip-address ip_addr: Displays statistics for a call with the IP address specified in IPv4 dotted-decimal notation.

msid msid_num: Specifies a mobile subscriber ID only for which information is to be displayed. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.

peer-address peer_address: Displays statistical information for the peer IP address specified using IPv4 dotted-decimal notation.

reverse-tunnel { on | off }: Enables the display of reverse IP tunnel information.

username user_name: Displays user MIP call information for the username specified as an alphanumeric string of 1 through 127 characters including wildcard characters ($ and *).
peer-address [ operator ] peer_address

In conjunction with mipha [ summary ] peer-address keyword, indicates a range of peers is to be displayed.

peer_address must be specified using IPv4 dotted-decimal notation.
operator implies how to logically specify a range of peer-addresses and it must be one of the following:

- <: IP address is less than the specified peer_address
- >: IP address is greater than the specified peer_address
- greater-than: IP address is greater than the specified peer_address
- less-than: IP address is less than the specified peer_address

statistics [ ha-service ha_name | peer-address peer_address ]

Displays statistical information for the home agent service specified by its name (an alphanumeric string of 1 through 63 characters) or peer IP address (IPv4 notation).
peers ha-service service_name [ current-sessions { { > | greater-than } sessions [ < sessions ] | { < | less-than } sessions [ > sessions ] | sessions } ] [ peer-address address ]

Displays peer servers for the specified HA service.

ha-service service_name: Specifies the name of an existing HA service for which the associated peer servers are to be displayed as an alphanumeric string of 1 through 63 characters.
current-sessions: Displays only peer servers with current sessions meeting the following criteria:

- > | greater-than sessions: Displays only peer servers currently running sessions higher than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “greater-than” and the “>” symbol are interchangeable in this instance of the command.
- < sessions: Displays only peer servers that are currently running sessions higher than the greater-than parameter but less than the value entered in this parameter. sessions must be an integer from 1 to 3000000.
- < | less-than sessions: Displays only peer servers currently running sessions lower than the value entered in this parameter. sessions must be an integer from 1 to 3000000. Note: the keyword “less-than” and the “<” symbol are interchangeable in this instance of the command.
- > sessions: Displays only peer servers that are currently running sessions lower than the less-than permitter but more than the value entered in this parameter. sessions must be an integer from 1 to 3000000.
- sessions: Displays only peer servers currently running sessions that are equal to the value entered in this parameter. sessions must be an integer from 1 to 3000000.

peer-address address: Displays only peer servers matching the IP address entered in this parameter. address must be specified using IPv4 dotted-decimal notation and can be followed by the netmask of the address.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

View MIP home agent information to support troubleshooting subscriber issues by viewing call information and filtering on the subscriber information using various methods.
Example:
The following displays the call information for all mobile IP HA calls and statistics for ha1, respectively:

    show mipha all

    show mipha statistics
    ha-service ha1

The following commands displays call information for user isp1user1 in full detail and in summary:

    show mipha full username isp1user1

    show mipha summary
    username user1

The following displays MIP-HA call information for calls from mobile subscribers with reverse tunneling off and peer address 10.2.3.4, respectively:

    show mipha reverse-tunnel off

    show mipha peer-address 10.2.3.4

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show mipv6ha

Displays information for specified Mobile IPv6 Home Agent (MIPv6-HA) calls.
Platform:

ASR 5000
Product:

PDSN, HA
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show mipv6ha [ all | callid callid | counters filter | full filter | ipv6-address ip_addr| statistics
    mipv6ha-service mipv6ha-service_name | summary filter | username user_name ]

all

Displays all information for MIPv6-HA calls.
callid call_id

Specifies the Call Identification number as an 8-digit hexadecimal number.
counters [ all | callid | ipv6-address | username ]
Displays the counters associated with the MIPv6-HA service. The following filters are available:

- all
- callid:
- ipv6-address
- username

full [ all | callid | ipv6-address | username ]

Displays all available information for the associated display or filter keyword.
The following filters are available:

- all
- callid:
- ipv6-address
- username

ipv6-address ip_addr
Displays information for subscribers connected via the packet control function for a specific or range of IPv6 addresses. The address must be specified using the IPv6 colon-separated-hexadecimal notation.

- <: Filters output so that only information less than the specified IPv6 address value is displayed.
- >: Filters output so that only information greater than the specified IPv6 address value is displayed.
- less-than: Filters output so that only information less than the specified IPv6 address value is displayed.
- greater-than: Filters output so that only information greater than the specified IPv6 address value is displayed.

statistics [ mipv6ha-service mipv6ha-service_name ]

Displays all information collected for specific protocol since last the restart or clear command.

This can be filtered according to a specified mipv6ha-service.
summary [ all | callid | ipv6-address | username ]

Displays summary information for defined sessions, based on defined parameters.
The following filters are available:

- all
- callid:
- ipv6-address
- username

username user_name

Displays session information for a specific username.
Usage:

View MIPv6 home agent information to support troubleshooting subscriber issues by viewing call information and filtering on the subscriber information using various methods.
Example:
The following displays the call information for all mobile IPv6 HA calls:

    show mipv6ha all

The following command displays call information for user mipv6hauser1 in full detail and in summary:

    show mipv6ha full
    username mipv6hauser1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show mme-service

Displays configuration information for Mobility Management Entity (MME) services on this system.
Platform:

ASR 5000
Product:

MME
Privilege:

Inspector
Syntax

    show mme-service { all | name svc_name [ offload
    statistics ] } [ | { grep grep_options | more } ]

all

Displays configuration information for all MME services configured on this system.
name service_name

Displays configuration information for an existing MME service specified as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to view configuration information for MME services on this system.
Example:
The following command displays service statistics for the MME service named mme1:

    show mme-service name mme1

IMPORTANT:

Output descriptions for these commands are available in the Statistics and Counters Reference.
show mme-service db record

Displays the Mobile Management Entity (MME) database records for MME sessions grouped in session instances on this system and filtered with IMSI or GUTI as criteria.
Platform:

ASR 5000
Product:

MME
Privilege:

Inspector
Syntax

    show mme-service db
    record { all  | call-id call_id | guti plmn plmn_id group-id mme_grp_id code mme_code m-tmsi mtmsi_value| imsi imsi_identifier

all

Displays all database records of a session instance used for MME service.
call-id call_id

Displays database records filtered by the call ID specified as an 8-digit hexadecimal number
guti plmn plmn_id group-id mme_grp_id code mme_code m-tmsi mtmsi_value

Displays database records filtered by the Globally Unique Temporary Identifier (GUTI). The GUTI is constructed from the GUMMEI and the M-TMSI.

The GUMMEI is constructed from the public land mobile network (PLMN) ID [MMC and MNC] and the MME Group ID (MMEGI). Within the MME, the mobile is identified by the M-TMSI.

A GUTI has: 1) a unique identity for the MME which allocated the GUTI; and 2) the unique identity of the UE within the MME that allocated the GUTI.

The MME Identifier (MMEI) is constructed from an MME Group ID (MMEGI) and an MME Code (MMEC).
imsi imsi_identifier

Displays database records filtered by International Mobile Subscriber Identity (IMSI).

imsi_identifier is a 15-character IMSI field which identifies the subscriber’s home country and carrier. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
Usage:

Use this command to view database records for all or a particular instance of session manager for MME services on this system with IMSI or GUTI as a filter criteria.
Example:
The following command displays the summary database records of a session instance for a subscriber having IMSI as 123455432112345 in the MME service:

    show mme-service db
    record imsi 123455432112345

IMPORTANT:

Output descriptions for these commands are available in the Statistics and Counters Reference.
show mme-service db statistics

This command displays the Mobile Management Entity (MME) database statistics for all or specific MME sessions on this system.
Platform:

ASR 5000
Product:

MME
Privilege:

Inspector
Syntax

    show mme-service db
    statistics [ instance smgr_instance ]

instance smgr_instance

Displays MME database statistics for a specific instance of a session manager running the MME service.

smgr_instance is an instance ID specified as an integer from 0 through 4294967295. If an instance is not specified, summary statistics are displayed.
Usage:

Use this command to view database statistics for all or a particular instance of session manager for MME services on this system.
Example:
The following command displays summary database statistics for the MME service running on a system:

    show mme-service db statistics

IMPORTANT:

Output descriptions for these commands are available in the Statistics and Counters Reference.
show mme-service enodeb-association

Displays configuration information for an eNodeB association within an MME service.
Platform:

ASR 5000
Product:

MME
Privilege:

Inspector
Syntax

    show mme-service enodeb-association [ summary | full ] [ all | | ipsec | mme-service-name mme_svc_name | peer-address peer_ip_address | peer-id peer_identifier ] [ | { grep grep_options | more } ]

summary

Displays summarized output for this command.
full

Displays detailed output for this command.
all

Displays information of all eNodeBs associated with MME services on this system.
ipsec

Displays information of all IPSec enabled eNodeBs associated with MME services on this system.
mme-service-name mme_svc_name

Displays summarized or detailed configuration information for eNodeBs associated with an existing MME service specified as an alphanumeric string of 1 through 63 characters.
peer-address peer_ip_address

Displays summarized or detailed configuration information of eNodeBs associated with an existing MME peer IP address configured with an MME service and expressed in IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation.
peer-id peer_identifier

Displays summarized or detailed configuration information for eNodeBs associated with a an existing MME peer ID configured with an MME service and specified as an integer from 1 through 4294967295.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to view configuration information of eNodeBs associated with an MME service on this system.
Example:
The following command displays detailed service statistics for associated eNodeBs within the MME service named mme1:

    show mme-service enodeb-association
    full mme-service-name mme1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show mme-service session

Displays session information for Mobile Management Entity (MME) service(s) running on a peer or local system.
Platform:

ASR 5000
Product:

MME
Privilege:

Inspector
Syntax

    show mme-service session [ summary | full | counters ] [ all
     | callid call_identifier | imei imei_id  | imsi imsi_id | ipsec | mme-service service_name | msisdn number | pdn-address pdn_ip_address | s1-peer s1_peer_ip_address | s11-peer s11_peer_ip_address | vlr-name vlr_name | ue-ecm-state { connected | idle } ] [ | { grep grep_options | more } ]

summary

Displays summarized output for this command.
full

Displays detailed output for this command.
counters

Displays all counters for related events and messages for an MME session running on a system.
all

Displays information for all MME sessions running on this system.
callid call_identifier

Displays summarized or detailed configuration information for an MME session filtered by a call identifier within an MME service configured on this system.

call_identifier must be an existing call identity in 8-digit hexadecimal format running in an MME service on this system.
imei imei_id

Displays summarized or detailed configuration information about MME sessions running and filtered by an International Mobile Equipment Identification (IMEI) number within an MME service configured on this system.

imei_id must be an existing IMEI in an existing MME service on the system. imei_id must contain an 8-digit TAC (Type Allocation Code) and a 6-digit SNR (Serial Number).
imsi imsi_id

Displays summarized or detailed configuration information about MME sessions running and filtered by an International Mobile Subscriber Identity (IMSI) number within an MME service configured on the system.

imsi_id must be an existing IMSI in an existing MME service on the system. imsi_id is a 15-character IMSI field which identifies the subscriber’s home country and carrier.

Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
ipsec

Displays information for all IPSec enabled sessions using MME services on the system.
mme-service service_name

Displays summarized or detailed configuration information about MME sessions running and filtered by an MME service name configured on the system.

service_name must be a configured MME service on the system, expressed as an alphanumeric string of 1 through 63 characters.
msisdn number

Displays summarized or detailed configuration information about MME sessions running and filtered by a Mobile Station International ISDN Number.

number must be a combination of the CC (Country Code) and National (significant) mobile number, not exceeding 15 digits.
pdn-address pdn_ip_address

Displays summarized or detailed configuration information about MME sessions running and filtered by the IP address of a connected PDN(s) within an MME service configured on this system.

pdn_ip_address must be a configured IP address of a PDN expressed in IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation within an existing MME service on the system.
s1-peer s1_peer_ip_address

Displays summarized or detailed configuration information of MME sessions running and filtered by the IP address of a peer connected through an S1 interface within an MME service configured on this system.

s1_peer_ip_address must be a configured IP address of a peer on S1 interface expressed in IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation within an existing MME service on this system.
s11-peer s11_peer_ip_address

Displays summarized or detailed configuration information of MME sessions running and filtered by IP address of a peer connected through S11 interface with an MME service configured on this system.

s11_peer_ip_address must be a configured IP address of a peer on S11 interface expressed in IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation within an existing MME service on this system.
ue-ecm-state { connected | idle }

Displays summarized or detailed configuration information about MME sessions running and filtered by the UE’s EPS Connected Management (ECM) state.

connected: Specifies that summarized or detailed configuration information about MME sessions is to be displayed based on the UE ECM state of “connected”.

idle: Specifies that summarized or detailed configuration information about MME sessions is to be displayed based on the UE ECM state of “idle”.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to view information for MME sessions within MME services on this system.
Example:
The following command displays detailed session statistics for an MME service running on this system:

    show mme-service session full

IMPORTANT:

Output descriptions for these commands are available in the Statistics and Counters Reference.
The following command displays detailed session counters for an MME service running on this system:

    show mme-service session counters

show mme-service statistics

This command displays the service statistics of an MME service specified by various criteria.
Platform:

ASR 5000
Product:

MME
Privilege:

Security Administrator, Administrator
Syntax

    show mme-service statistics [ sctp [ mme-service mme_svc_name ] | s1ap [ mme-service mme_svc_name | peer-id peer_identifier ] | [ emm-only | esm-only ] [ mme-service mme_svc_name | peer-id peer_identifier ] [ verbose ] [ | { grep grep_options | more } ]

emm-only

Filters the output of EPS mobility management (EMM) related statistics by an MME service name or peer MME identifier.
esm-only

Filters the output of EMM related statistics by MME service name or peer MME identifier.
s1ap

Filters the output of S1-AP statistics by MME service name of peer MME identifier.
sctp

Filters the output of SCTP statistics by MME service name of peer MME identifier.
mme-service mme_svc_name

Filters the output of all MME service statistics (such as EMM, ESM, SCTP, S1-AP, and SCTP) by MME service name.
peer-id peer_identifier

Filters the output of all MME service statistics (such as EMM, ESM, SCTP, S1-AP, and SCTP) by MME peer identifier.
verbose

Displays comprehensive information for a specific argument or set of arguments.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

This command is used to display the statistical information of an MME service based on various filter criteria as a local MME service or a peer MME related to EMM, ESM, SCTP, S1-AP, and SCTP.
Example:
The following command displays the service session statistics of all MME service on a system related to all; such as EMM, ESM, SCTP, S1-AP, and SCTP:

    show mme-service statistics

IMPORTANT:

Output descriptions for these commands are available in the Statistics and Counters Reference.
The following command displays the service session statistics of all MME services on a system related to S1-AP:

    show mme-service statistics s1ap

The following command displays the service session statistics of all MME services on a system related to EMM only:

    show mme-service statistics
    emm-only

show mpls ldp

Displays the Multiprotocol Label Switching (MPLS) Label Distribution Protocol (LDP) information.
Platform:

ASR 5000
Product:

GGSN
Privilege:

Security Administrator, Administrator
Syntax

    show mpls ldp { bindings { ldp-id IPv4_add | local [ ldp-id | local | prefix | remote ] | prefix IPv4_addr | remote } | discovery | neighbor { detail | ldp-id
    	 } }

bindings

Displays the MPLS LDP label bindings.
ldp-id

Displays label values for a specific peer LDP ID.
local

Displays locally assigned label values.
prefix

Displays label values for a specific prefix.
remote

Displays remotely assigned label values.
discovery

Displays the MPLS LDP discovery information.
neighbor

Displays the MPLS LDP peer information.
detail

Displays the MPLS LDP peer information in details. The displayed information includes, Local LDP ID, Peer LDP ID, Transport address, State (for example, Established), Role (for example, Active), Uptime, Keepalive negotiated hold time, Proposed Local/Peer, Remaining Keepalive hold time, and Address advertised.
Usage:

This command displays statistical information for an MPLS Label Distribution Protocol configuration. The information includes Prefix, LDP ID, Label, Nexthop, and Egress_if_index for all MPLS LDP Bindings configurations.
Example:
The following command displays information about MPLS LDP protocol related configurations:

    show mpls ldp discovery
    neighbor ldp-id 10.2.3.4 detail bindings ldp-id 31.32.33.34 prefix
    192.168.102.232 local remote

The following command displays the MPLS LDP discovery information, including, LDP Peer IDs, Hold time (in seconds), Proposed Local/Peer, and Remaining (time in seconds):

    show mpls ldp discovery

The following command displays the remotely assigned label values in the MPLS LDP binding configuration:

    show mpls ldp bindings remote

IMPORTANT:

Output descriptions for these commands are available in the Statistics and Counters Reference.
show multicast-sessions

Displays information for multicast sessions defined by the specified keywords.
Platform:

ASR 5000
Product:

PDSN, GGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show multicast-sessions [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more }

command_keyword

The following keywords are base commands that each have a distinct display output. Only one keyword can entered on the command line.
debug-info { callid id | flowid id }

Displays internal call troubleshooting information for multicast sessions defined by the specified keywords.

callid id: Displays subscriber information for the call specified as an 8-digit hexadecimal number.

flowid id: Displays information for a specific BCMCS flow, defined by The flow ID as a hexadecimal number.
full

Displays all available multicast session information. The following filter keywords are valid for this command: active, all, callid, card-num, dormant, flowid, flowid-type, mcast-address, pcf, pdsn-service, grep, more
summary

Only displays a summary of multicast session information. The following commands are valid for this command: active, all, callid, card-num, dormant, flowid, flowid-type, mcast-address, pcf, pdsn-service, grep, more
filter_keywords

The following keywords are filters that modify or filter the output of the Command Keywords. Not all filters are available for all Command Keywords. Multiple Filter Keywords can be entered on a command line.

When multiple Filter Keywords are specified, the output conforms to all of the Filter Keywords specifications.
active

Only displays information for multicast sessions that are currently active.
all

If no keywords are specified before all, information for all multicast sessions is displayed. If keywords are specified before all, all information is displayed with no further options being allowed.
callid id

Displays multicast session information for the call specified by id. The call must be specified as an 8-digit hexadecimal number.
card-num card_num

The slot number of the processing card by which the subscriber session is processed. card_num is a slot number from 1 through 7 or 10 through 16 on the ASR 5000, or 1 through 4 or 7 through 10 on the ASR 5500.
dormant

Shows information for subscriber sessions that are dormant (not transmitting or receiving data).
flowid id

Displays information for a specific BCMCS flow, defined by id. The flow ID must be a hexadecimal number.
flowid-type [ flow | program ]

Displays information for multicast sessions according to the type of flow.

flow: Shows all multicast sessions for the flow ID type “flow”.

program: Shows all multicast sessions for the flow ID type “program”.
mcast-address ipv4_address

Show multicast sessions for a specific multicast address. Must be followed by the IP address of an interface, using IPv4 dotted-decimal notation.
pcf ipv4_address

Displays information for multicast sessions connected via the packet control function, defined by ipv4_address. The address must be specified using IPv4 dotted-decimal notation.
pdsn-service svc_name

Displays information for multicast session connected to the packet data service svc_name.The packet data service must have been previously configured and expressed as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

Please refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter for details on the usage of grep and more.
Usage:

Use this command to view information about multicast sessions.

The output of this command may be considered for part of a periodic system auditing program by verifying active and dormant sessions.
Example:
The following command displays the all broadcast-multicast sessions active in a context/system:

    show multicast-sessions all

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show network-requested-pdp-context

Displays information for the specified network-requested packet data protocol (PDP) context.
Platform:

ASR 5000
Product:

GGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show network-requested-pdp-context
    imsi imsi_value

imsi imsi_value

Specifies that information will be displayed for a particular International Mobile Subscriber Identity (IMSI). imsi_value is an integer from 1 to 15 digits.
Usage:

USe this command to display information pertaining to network-requested PDP contexts.
Example:
The following command displays network-requested PDP context information for a subscriber with an IMSI of 123456789:

    show network-requested-pdp-context
    imsi 123456789

show network-service-entity

Displays information regarding the network service entities (NSEs) in the network.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show network-service-entity { consolidated-status | fr-config [ peer-nsei nsei] | ip-config [ nsvl { all | instance value } }

consolidated-status

Displays Network Service Virtual Connection (NSVC) status information for all network service entities in the network. This keyword is particularly useful for troubleshooting.
fr-config [ peer-nsei nsei]

Displays network service configurations for NSEs using Frame Relay configurations.

peer-nsei nsei limits the display to a specific peer NSE identified as an integer from 0 through 65535.
ip-config [ nsvl { all | instance value }

Displays network service configurations for NSEs using IP configurations.

Including the nsvl keyword limits the display to all or a single (instance 0 to 3) of a network service virtual link.
Usage:

Use this command to display NSE information pertaining to the NSVCs of the NSEs in the networks or NSEs configured for Frame Relay or IP.
Example:
The following command displays the status of all the NSVCs for all the NSEs in the network.

    show network-service-entity
    consolidated-status

show npu utilization

Displays NPU information utilization.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show npu utilization
    table [ | {  grep grep_options | more } ]

| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

View network timing protocol information to troubleshooting system clock issues by displaying the associations and status of the local NTP client.
Example:
The following displays the NPU information.

    show npu utilization table

    show npu utilization
    table | grep  qwe

show ntp

Displays the network timing protocol (NTP) associations and status.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show ntp { associations | status } [ address ip_address ]  [ | { grep grep_options | more } ]

associations

Displays the current NTP server associations and related statistics.
status

Displays the client permeates configured and the synchronization status.
address ip_address

Specifies the IP address of an NTP server/client in the current context in IPv4 dotted-decimal notation.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
Usage:

View network timing protocol information to troubleshooting system clock issues by displaying the associations and status of the local NTP client.
Example:
The following displays the NTP associations and status, respectively.

    show ntp associations show ntp status

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show nw-reachability server

Displays the configuration of network reachability servers for the current context.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show nw-reachability
    server { all | name server_name }

all

Displays configuration information for all network reachability servers in the current context.
name server_name

Displays configuration information for an existing network reachability server specified as an alphanumeric string of 1 through 15 characters.
Usage:

Use this command to display configuration information on network reachability servers configured in the current context.
Example:
The following command displays information on all network reachability servers in the current context:

    show nw-reachability
    server all

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show operator-policy

Displays the information configured for an operator policy.
Platform:

ASR 5000
Product:

MME, SGSN
Privilege:

Inspector
Syntax

    show operator-policy { all | full { all | name op_policy_name } | name op_policy_name } [ | { grep grep_options | more } ]

all

Displays a list of all operator policies configured on the system.
full { all | name op_policy_name }

full:Displays a full set of available information for the specified operator policy (policies).

all: Displays a full set of available information for all operator policies configured on the system.

name op_policy_name: Displays a full set of available information for an existing operator policy specified as an alphanumeric string of 1 through 64 characters.
name op_policy_name Displays a full set of available information for an existing operator policy specified as an alphanumeric string of 1 through 64 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to display information for operator policies configured on the system. Operator policies are configured through the Global Configuration Mode and in the Operator Policy Configuration Mode. For more information regarding operator policy commands, refer to the Operator Policy Configuration Mode Commands chapter.
Example:
The following command displays all available information for an operator policy named policy-5:

    show operator-policy
    full name policy-5

show orbem

Displays information and statistics for the Object Request Broker Element Manager (ORBEM) interface in the current context.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show orbem { client { id client_name | table } | event-notif-service
    filters | session { id session_name |  table } | status } [ | { grep grep_options | more } ]

client { id client_name | table }

Indicates the Common Object Request Broker Architecture (CORBA) client information is to be displayed. The keyword table is used to output to the display information on all configured clients. The keyword id is used to specify a specific client for which information is to be displayed specified as client_name.

client_name must refer to an existing client which is found using the table keyword option.
event-notif-service filters

Displays information pertaining to filters configured for the ORB Notification Service.
session { id session_name | table }

Indicates session information is to be displayed. The keyword table is used to output to the display information on all configured clients. The keyword id is used to specify a specific session for which information is to be displayed specified as session_name.

session_name must refer to an existing session which is found using the table keyword option.
status

Indicates that the ORBEM server status information is to be displayed.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Display current sessions when ORBEM system response may appear sluggish. This command is also useful in periodic verification of the server status.
Example:
The following commands will display the information for all clients.

    show orbem client table

The following commands display the information for the clientName and sessionID, respectively:

    show orbem client
    id clientName

    show orbem session
    id  sessionId

The following command displays the ORBEM server status:

    show orbem status

The following command displays the information for all sessions:

    show orbem session table

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show patch progress

Displays the status of the on-going software patch installation.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show patch progress

Usage:

Use this command to show the status of an on-going software patch installation.

IMPORTANT:

Software Patch Upgrades are not supported in this release.
show pdg-service

Displays configuration information about PDG services configured on the system.
Platform:

ASR 5000
Product:

PDG/TTG
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show pdg-service { all | name service_name }

all

Displays information for all configured Packet Data Gateway/Tunnel Termination Gateway (PDG/TTG) services.
name service_name

Displays information only for an existing PDG service specified as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to display information for PDG services.
Example:
The following command displays available information for all active PDG services:

    show pdg-service all

show pdg-service statistics

Displays statistics for the Packet Data Gateway/Tunnel Termination Gateway (PDG/TTG) since the last restart or clear command. The output includes the number of each type of Extensible Authentication Protocol (EAP) messages.
Platform:

ASR 5000
Product:

PDG/TTG
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show pdg-service statistics [ name service_name | peer-address ipv4_address ]

name service_name

Displays statistics for an existing PDG service specified an alphanumeric string of 1 through 63 characters.
peer-address ipv4_address

Displays statistics for a specific subscriber with the WLAN IP address specified in IPv4 dotted-decimal notation.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to display PDG service statistics.
Example:
The following command displays statistics for all active PDG services:

    show pdg-service statistics

show pdif-service

Displays configuration information about Packet Data Interworking Function (PDIF) services configured on the system.
Platform:

ASR 5000
Product:

PDIF
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show pdif service { all [ counters ] | name name [ counters ] | statistics [ name name | peer-address address ] } [ | { grep grep_options | more } ]

all [ counters ]

Displays configuration information and statistical counters for all PDIF services in the system.
name name [ counters ]

Displays configuration information and statistical counters for an existing PDIF service specified as an alphanumeric string of 1 through 63 characters.
statistics [ name name | peer-address address ]

name name: Displays service statistics for a an existing PDIF service specified as an alphanumeric string of 1 through 63 characters.

peer-address address: Displays service statistics for a peer server IP address specified in IPv4 dotted-decimal notation.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to display configuration information and statistics about PDIF services on the system.
Example:
The following example displays configuration information about a PDIF service named pdif23:

    show pdif service
    name pdif23

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show pdsn-service

Displays information for configured packet data services in the current context.
Platform:

ASR 5000
Product:

PDSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show pdsn-service { all | name pdsn_name } [ pcf-status
     [ address ip_address | filter [ all | icmp-monitored | no-calls | summary | up ] ] ] [ | { grep grep_options | more } ]

all | name pdsn_name

all: Displays information for all configured packet data services.

name pdsn_name: Displays information only for an existing PDSN service specified as an alphanumeric string of 1 through 79 characters.
pcf-status [ address ip_address | filter [ all | icmp-monitored | no-calls | summary | up ] ]

pcf-status: Displays summary information for all Packet Control Functions (PCFs).

address ip_address: Only lists information for the PCF with the IP address specified in IPv4 dotted-decimal notation.
filter: Filters the output so only the specified information is displayed. If a filter is specified with no keywords, summary information for all PCFs is displayed.

- all: Displays information for all the PCFs
- icmp-monitored: Displays information only for PCFs which are ICMP monitored
- no-calls: Displays information only for PCFs which have no active sessions
- summary: Displays only a summary of the status of the PCFs
- up: Displays information only for PCFs which are alive

| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Show the PDSN service information for standard system monitoring or troubleshooting.
Example:
The following will display the information for all configured services and sampleService, respectively:

    show pdsn-service all

    show pdsn-service name sampleService

show pgw-service

Displays configuration information for PDN Gateway (P-GW) services on this system.
Platform:

ASR 5000
Product:

P-GW
Privilege:

Inspector
Syntax

    show pgw-service { all | name service_name | statistics { all | name service_name } [ verbose ] } [ | { grep grep_options | more } ]

all

Displays configuration information for all P-GW services configured on this system.
name service_name

Displays configuration information for an existing P-GW service specified as an alphanumeric string of 1 through 63 characters.
statistics { all | name service_name } [ verbose ]

Displays P-GW service statistics.

all: Displays statistics for all P-GW services on the system.

name service_name: Displays statistics for an existing P-GW service specified as an alphanumeric string of 1 through 63 characters.

If verbose is also specified, the information is displayed in more detail.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to view configuration information for P-GW services on this system.
Example:
The following command displays service statistics for the P-GW service named pgw1:

    show pgw-service name pgw1

show port

Displays information on configured parameters and operational statistics for physical and logical ports in the system.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show port { datalink
    counters [ slot/port ] | info [ slot/port ] [ vlan vlan_id ] | npu
    counters [ slot/port [ tagged | untagged | vlan tag_id ] ] | table  | utilization
    table  } [ | { grep grep_options | more } ]

datalink counters slot/port

Displays the information for all data links or only the one specified by the slot/port location of a previously configured port.
info [ slot/port ] [ vlan vlan_id ]

Displays detailed information for all ports within the chassis or only the one specified by slot/port location of a previously configured port.

vlan vlan_id: Displays detailed information about all Virtual Local Area Networks (VLANs) in the port/slot. If the optional vlan_id is not specified, this keyword displays port information for all VLANs in the slot/port location.
npu counters [ slot/port [ tagged | untagged | vlan tag_id ] ] | bound | unbound ]

Displays the information for Network Processing Unit (NPU) ports. The information for all ports is output or only the one specified by the slot/port location of a previously configured port.

tagged: Display statistics for all tagged packets.

untagged: Display statistics for all untagged packets.

vlan tag_id: Display NPU counters for a previously configured VLAN ID.

bound: Displays individual and cumulative NPU port counters for the bound ports within the current context. If the command is invoked in the local context, all of the bound ports for all contexts and cumulative counter values for all contexts are displayed.

unbound: Displays individual and cumulative NPU port counters for all unbound ports within system.
table

Displays information for all physical ports on rear-installed cards with physical interfaces.
utilization table

Shows average port utilization in Mbps. The output is a table that lists the current utilization average, a 5-minute average, and a 15-minute average, for all enabled ports.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Display port information for troubleshooting of network communications by viewing statistics and configuration information for physical ports.
Example:
The following displays detailed information for port 1 in slot 17:

    show port info 17/1show port table

The following displays information for the data link port 33/1:

    show port datalink counters 33/1

    show port npu counters
    33/1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show power

Displays information about the power on/off status of individual cards and the operating status of installed power filter units.
Platform:

ASR 5000
Product:

All
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show power [ all | chassis | card_num ] [ | { grep grep_options | more } ]

all | chassis | card_num ]

all: Displays power on/off state for all cards in the chassis.

chassis: Displays the operating status of installed power filter units. This is the default setting.

card_num: Displays the power on/off state for a single card specified an integer from 1 through 48 for the ASR 5000 or 1 through 20 for the ASR 5500.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

View power source information to quickly check the power for all cards within a chassis.

IMPORTANT:

On some platforms, only show power is supported with no other keywords or variables.
Example:
The following displays power supply status for the chassis:

    show power

The following command displays the power status for all slots:

    show power all

show ppp

Displays the point-to-point protocol (PPP) information, detailed or summarized, for one or all connections by the use of filtering options.
Platform:

ASR 5000
Product:

PDSN, GGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show ppp { [ counters | full | summary ] { all | callid call_id | imsi id | msid ms_id | username user_name } | statistics
     [ pcf-address [ pcf_ip_addr | all ] |  pdsn-service pdsn_name ] } [ | { grep grep_options | more } ]

counters | full | summary

Filters the output for the level and type of information with the options described below.

counters: Displays PPP statistics.

full: Displays all available information.

summary: Displays only a summary of available information.
all | callid call_id | imsi imsi_id | msid ms_id | username user_name } ]

all: Displays all available information.

callid call_id: Displays PPP information only for the call ID specified as a 4-digit hexadecimal number.

imsi id: Displays PPP information only for the subscriber with the specified IMSI (International Mobile Subscriber Identity). id is a 15-digit field which identifies the subscriber’s home country and carrier.

msid ms_id: Displays information for a mobile subscriber ID specified as 7 to 16 digits for an IMSI, MIN, or RMI.

username user_name: Displays user PPP information for the specified username.
statistics [ pcf-address [ pcf_ip_addr | all ] | pdsn-service pdsn_name ]

Displays statistics for all packet data services.

pcf-address [ pcf_ip_addr | all ]: Displays statistics only for the time the session is connected to the specified PCF (Packet Control Function) or for all PCFs. pcf_ip_addr must be specified using IPv4 dotted-decimal notation.

pdsn-service pdsn_name: Display statistics only for an existing PDSN service specified as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
Usage:

View Point-to-Point Protocol information to support troubleshooting subscriber connections by viewing information on PPP connections for a specific subscriber.
Example:
The following displays the PPP summary for all connections.

    show ppp summary all

The following outputs the point-to-point detailed information for the user user1.

    show ppp full username user1

The following command displays the standard information for the call with ID FF0E11CD.

    show ppp callid ff0e11cd

The following command displays the PPP statistics for pdsn1.

    show ppp statistics
    pdsn-service pdsn1

The following command provides summarized information for the PPP statistics.

    show ppp

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show prepaid 3gpp2

Displays prepaid accounting information for all services or only the service specified.
Platform:

ASR 5000
Product:

PDSN, GGSN
Privilege:

Security Administrator, Administrator, Operator, Inspector
Syntax

    show prepaid 3gpp2
    statistics all [ | { grep grep_options | more } ]

    show prepaid 3gpp2
    statistics { ggsn-service | ha-service | lns-service | pdsn-service { all | name service_name } [ | { grep grep_options | more } ]

    show prepaid 3gpp2 statistics per-service-summary } [ | { grep grep_options | more } ]

all

Displays prepaid statistics for all services.
ggsn-service

Displays statistics for GGSN service(s).
ha-service

Displays statistics for HA service(s).
lns-service

Displays statistics for LNS service(s).
pdsn-service

Displays statistics for PDSN service(s).
{ all | name service_name }

all: Displays statistics for all services of the specified type.

name service_name: Displays statistics for an existing service specified an alphanumeric string of 1 through 63 characters.
per-service-summary

Displays prepaid statistics per service summary for all services.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in the Command Line Interface Reference.
Usage:

Displays Pre-paid statistics for a particular named service or for all services.
Example:
To display statistics for a PDSN service named PDSN1, enter the following command:

    show prepaid 3gpp2
    statistics pdsn-service name PDSN1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show prepaid wimax

This command displays prepaid WiMAX accounting information for all services or only the service specified.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Inspector
Syntax

    show prepaid wimax
    statistics { all | asngw-service { all | name service_name } | ha-service { all | name service_name } | per-service-summary } [ | { s grep_options | more } ]

all

This keyword displays prepaid statistics for all services.
asngw-service

Displays prepaid statistics for Access Service Network-Gateway (ASN-GW) service(s).
ha-service

Displays prepaid accounting statistics for Home Agent (HA) service(s).
{ all | name service_name }

all: Displays statistics for all services of the specified type.

name service_name: Displays statistics for an existing service specified as an alphanumeric string of 1 through 63 characters.
per-service-summary

Displays prepaid statistics per service summary for all services.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to display prepaid WiMAX accounting statistics for named service or for all services.
Example:
The following command displays prepaid WiMAX accounting statistics for an ASN-GW service named asn1:

    show prepaid wimax
    statistics asngw-service name asn1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show profile-id-qci-mapping

Displays QoS Class Identifier-Radio Access Network (QCI-RAN) mapping tables configured on this system.
Platform:

ASR 5000
Product:

HSGW
Privilege:

Inspector
Syntax

    show profile-id-qci-mapping
    table { all | name table_name }  [ | { grep grep_options | more } ]

all

Displays information for all QCI-RAN mapping tables configured on this system.
name table_name

Displays information for an existing QCI-RAN table specified as an alphanumeric string of 1 through 63 characters.
| { grep grep_options | more }

Pipes (sends) the output of the command to the command specified. You must specify a command to which the output will be sent.

For details on the usage of grep and more, refer to the Regulating a Command’s Output section in the Command Line Interface Overview chapter.
Usage:

Use this command to display the contents of a specific QCI-RAN mapping table or all mapping tables configured on this system.
Example:
The following command displays the contents of a QCI-RAN mapping table named table1:

    show profile-id-qci-mapping
    table name table1

show ps-network

Displays statistics for the Packet Switched (PS)-network(s) instance configured on a chassis for HNB-GW service sessions.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Security Administrator, Administrator, Operator
Syntax

    show ps-network { all | name ps_name } [ status ] [ | { grep grep_options | more }]

all

Displays status counters for all PS (packet switched) networks configured for HNB-GW service sessions on a chassis.
name ps_name

Displays status counters for a PS network configured for HNB-GW service specified as an alphanumeric string of 1 through 127 characters that is case sensitive
| { grep grep_options | more }

Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.

Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
Usage:

Use this command to display the status of any or all PS-network(s) instance configured on a chassis for HNB-GW service sessions.
Example:
The following command displays the output for PS network instance status named ps_1_hnb:

    show ps-network name
    ps_1_hnb status

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show ps-network counters

Displays the session counter information for a PS Network associated with Home-NodeB Gateway (HNB-GW) services configured and running on a system.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Inspector
Syntax

    show ps-network counters [ name ps_svc_name [ sgsn sgsn_point_code ] ] [ | { grep grep_options | more } ]

name ps_svc_name

Filters the counter display based on an existing HNB-PS Network service name associated with an HNB-GW service running on system. ps_svc_name is an alphanumeric string of 1 through 63 characters.
sgsn sgsn_point_code

Filters the counter display filtered on the basis of SGSN address provided in the SS7 point code that is connected to a particular HNB-PS Network service. sgsn_point_code must be the address of an SGSN in SS7 point code notation.
| { grep grep_options | more }

Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter.
Usage:

Use this command to view the session counter information for HNB-PS Network services configured and SGSNs connected on a system.
Example:
The following command displays the counters for the HNB-PS Network service named hnb_ps_svc1:

    show ps-network counters
    name hnb_ps_svc1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.
show ps-network statistics

Displays the Packet Switched session statistics for Home-NodeB Gateway (HNB-GW) services configured and running on this system.
Platform:

ASR 5000
Product:

HNB-GW
Privilege:

Inspector
Syntax

    show ps-network statistics [ name ps_svc_name [ sgsn sgsn_point_code]] [ gtpu-only | ranap-only | sccp-only ] [ | { grep grep_options | more } ]

name ps_svc_name

Filters the session statistics display based on an existing HNB-PS Network service name that is associated with an HNB-GW service running on this system. ps_svc_name is an alphanumeric string of 1 through 63 characters.

sgsn sgsn_point_code

Filters the counter display filtered on the basis of SGSN address provided in the SS7 point code that is connected to a particular HNB-PS Network service. sgsn_point_code must be the address of an SGSN in SS7 point code notation.
ranap-only

Filters the session statistics to display only Radio Access Network Application Protocol (RANAP) traffic for an HNB-PS Network service which is configured and associated with an HNB-GW service running on this system.
sccp-only

Filters the session statistics to display only Signaling Connection Control Part (SCCP) traffic for the specified HNB-PS Network service which is configured and associated with an HNB-GW service running on this system.
| { grep grep_options | more }

Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.

For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
Usage:

Use this command to view the session statistics for overall session or in selected part of user session for HNB-GW services configured and running on this system.
Example:
The following command displays the session statistics for the HNB-PS Network service named hnb_ps1:

    show ps-network statistics
    name hnbps1

IMPORTANT:

Output descriptions for commands are available in the Statistics and Counters Reference.