# LTE TAI Management Database Configuration Mode Commands

The LTE TAI Management Database Configuration Mode is used to create and manage the LTE Tracking Area Identifier (TAI) management database configuration for LTE polices configured on this system.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
tai-mgmt-obj

Creates new, or removes/enters existing, LTE Tracking Area Identifier (TAI) object configurations.
Platform:

ASR 5000
Product:

MME
Privilege:

Administrator
Syntax

    [ no ] tai-mgmt-obj object_name [ -noconfirm ]

no

Removes a configured TAI management object from the TAI management database.
-noconfirm

Executes the command without any additional prompt and confirmation from the user.
object_name

Specifies the name of the TAI management object and enters the LTE TAI Management Object Configuration Mode as an alphanumeric string of 1 through 64 characters.
Usage:

Use this command to enter the LTE TAI Management Object Configuration Mode for an existing object or for a newly defined object. This command is also used to remove an existing object.

Entering this command results in the following prompt:

    [context_name]hostname(tai-mgmt-obj)#

LTE TAI Management Object Configuration Mode commands are defined in the LTE TAI Management Object Configuration Mode Commands chapter.
Example:
The following command creates a TAI management object called tai-obj3 and enters the LTE TAI Management Object Configuration Mode:

    tai-mgmt-obj tai-obj3