# Network Service Virtual Connection Configuration Mode Commands

The Network Service Virtual Connection (NSVC) configuration mode is a sub-mode of the Network Service Entity (NSE) - Peer NSEI (for Frame Relay) configuration mode. The NSVC sub-mode creates a configuration instance for a specific NSVC, within the Gb interface, between a BSS and an SGSN in a 2.5G GPRSFrame Relay network connection.
Upon accessing this mode, the prompt will appear similar to:

    [local]hostname(nse-fr-peer-nsei-<nse_id>-nsvci-<nsvc_id>)#

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Return to the Exec mode.
exit

Exits the current configuration mode and returns to the previous configuration mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Returns to the network service entity - frame relay configuration mode.