# Starent Chassis MIB Objects

The following figure displays the hierarchical structure of the management: information base (MIB) for the core platform
MIB Textual Conventions

The following are the supported MIB Objects. Not all entries are supported on all platforms. Some may return a different output than expected.
Object

StarentSlotType

Object ID

N/A

Description

Describes the type of a slot. Each slot in the chassis is build to contain specific type(s) of cards. Only a card of one of the appropriate types can be put into a specific slot.

Syntax

Integer {

unknown(1)

pactac(2)

spc(3)

lc(4)

rcc(5)

spio(6)

}
Object

StarentCardType

Object ID

N/A

Description

Describes the type of a card. Each type represents a physically different card which would have a unique part number.

Syntax

Integer {

none(1)

unknown(2)

spc(3)

pac(4)

spio(5)

rcc(6)

lceth(7)

lcgeth(8)

lcds3

tac(10)

Icoc3(11)

Icoc12(12)

smc(13)

psc(14)

lcqgeth(15)

lctgeth(16)

vmc(17)

vpc(18)

vlceth1p(19)

lcgeth2(20)

lceth2(21)

psc2(22)

psc3(23)

pscA(24), -- Packet Services Card A

ppc(25), -- Packet Processing Card

lcchan3p2(26), -- Channelized Line card 2 Port

fanctrl6(28), -- Fan control revision 6

vioc(29) -- Virtual I/O Card

gpdsp(30) -- GP-DSP Daughter Card

xme(31), --XME Daughter Card

vop(32), -- VOP Daughter Card

edc(33) -- EDC Card

}
Object

StarentVersionNum

Object ID

N/A

Description

Contains the system version identification string.

Syntax

Octet String (0.. 256)
Object

StarRelayState

Object ID

N/A

Description

The state of a Central Office (CO) relay.

Syntax

Integer {

off(1)

on(2)

unknown(3)

}
Object

StarLongDurTimeoutAction

Object ID

N/A

Description

The action taken by the system upon detection of a long-duration session.

Syntax

INTEGER {

unknown(0)

detection(1)

disconnection(2)

notapplicable(3)

dormantdisconnection(4)

dormantdetection(5)

}
Object

StarShortName

Object ID

N/A

Description

short identification string. Follows the same conventions as the DisplayString TEXTUAL-CONVENTION.

Syntax

Octet String (1..32)
Object

StarShortID

Object ID

N/A

Description

An abbreviated form for identifying a service, composed of the first 8 characters of the context name, and the first 8 characters of a service name, separated by (:).

Syntax

OCTET STRING(1..17)
Object

StarMediumID

Object ID

N/A

Description

An abbreviated form for identifying a context-specific object, composed of the first 8 characters of the context name, and the first 16 characters of the object name, separated by (:).

Syntax

OCTET STRING (SIZE (1..25))
Object

StarENBID

Object ID

N/A

Description

An eNodeB identifier in the form aaa:bbb:cccccccc

Syntax

OCTET STRING (SIZE (1..16))
Object

StarQOSTPAction

Object ID

N/A

Description

Traffic Policing Action

Syntax

INTEGER

Enumeration

unknown(0)

notapplicable(1)

transmit(2)

drop(3)

loweripprecedence(4)
Object

StarOSPFNeighborState

Object ID

N/A

Description

OSPF Neighbor State

Syntax

INTEGER

Enumeration

unknown(0),

down(1),

attempt(2),

init(3),

twoway(4),

exstart(5),

exchange(6),

loading(7),

full(8)
starentMIB(8164).starentMIBObjects(1).starentChassis(1)
Object

starChassisCriticalCO

Object ID

enterprises.8164.1.1.1

Description

The current state of the Critical Central Office (CO) relay.

Syntax

StarRelayState

Access

Read-only
Object

starChassisMajorCO

Object ID

enterprises.8164.1.1.2

Description

The current state of the Major Central Office (CO) relay.

Syntax

StarRelayState

Access

Read-only
Object

starChassisMinorCO

Object ID

enterprises.8164.1.1.3

Description

The current state of the Minor Central Office (CO) relay.

Syntax

StarRelayState

Access

Read-only
Object

starChassisAction

Object ID

enterprises.8164.1.1.5

Description

Trigger to perform certain system-wide operations. noaction (1) performs no operation. It is the normal value received when this attribute is read. testled (2) triggers a test of all of the LEDs in the system. aco (3) triggers the Alarm Cut-Off, which shuts off all of the Central Office (CO) audible/visual relays. reset (4) triggers a system-wide restart. It will completely disrupt service on the device.

Syntax

Integer

Access

Read-write

Enumeration

noaction(1)

testled(2)

aco(3)

reset(4)
Object

starTimeTicks

Object ID

enterprises.8164.1.1.6

Description

The number of system clock ticks since the last system Epoch. One system clock tick is 10 milliseconds.

Syntax

Unsigned32

Access

Read-only
Object

starChassisAudibleAlarm

Object ID

enterprises.8164.1.1.7

Description

The current state of the chassis Audible Alarm.

Syntax

StarRelayState

Access

Read-only
Object

starChassisUTCTime

Object ID

enterprises.8164.1.1.8

Description

The current time on the chassis, in UTC format

Syntax

DateAndTime

Access

Read-only
Object

starChassisLocalTime

Object ID

enterprises.8164.1.1.9

Description

The current time on the chassis, converted to the local time zone.

Syntax

DateAndTime

Access

Read-only
Object

starChassisType

Object ID

enterprises.8164.1.1.10

Description

The physical chassis type

Syntax

Integer

Access

Read-only

Enumeration

unknown(0)

ST16(1)

ST40(2)

XT2(3)

st20(4)

asr5000(5)
Object

starChassisDescription

Object ID

enterprises.8164.1.1.11

Description

Chassis description.

Syntax

DisplayString

Access

Read-Only
Object

starChassisSWRevision

Object ID

enterprises.8164.1.1.12

Description

Software revision

Syntax

DisplayString

Access

Read-Only
Object

starChassisPeakCPUUsage

ObjectID

enterprises.8164.1.1.13

Description

Percentage of the system level peak cpu usage. starChassisPeakCpuUsage is the percentage value times 100; for example, 2.3% would be represented as 230.

Syntax

Integer32(1..10000)

Access

Read-only

Object

starChassisPeakMemoryUsage
Object ID

enterprises.8164.1.1.14

Description

The system level peak memory usage, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)

Syntax

Integer32(1..2097152)

Access

Read-Only
starentMIB(8164).starentMIBObjects(1).starentSlots(2)
Object

starSlotTable

Object ID

enterprises.8164.1.2.1

Description

A table containing information on all of the slots.

Syntax

Sequence of StarSlotEntry

Access

Not-accessible
Object

starSlotEntry

Object ID

enterprises.8164.1.2.1.1

Description

Information about a particular slot.

Syntax

StarSlotEntry

Access

Not-accessible

Sequence

starSlotNum

starSlotType

starCardType

starCardOperState

starCardAdminState

starCardRevision

starCardLastStateChange

starCardMode

starCardDesiredMode

starCardPacStandbyPriority

starCardLock

starCardHaltIssued

starCardRebootPending

starCardUsable

starCardSinglePOF

starCardAttachment

starCardTemperature

starSlotVoltage1dot5

starSlotVoltage1dot5LowThresh

starSlotVoltage1dot5HighThresh

starSlotVoltage1dot8

starSlotVoltage1dot8LowThresh

starSlotVoltage1dot8HighThresh

starSlotVoltage2dot5

starSlotVoltage2dot5LowThresh

starSlotVoltage2dot5HighThresh

starSlotVoltage3dot3

starSlotVoltage3dot3LowThresh

starSlotVoltage3dot3HighThresh

starSlotVoltage5dot0

starSlotVoltage5dot0LowThresh

starSlotVoltage5dot0HighThresh

starSlotNumPorts

starSlotVoltageState

starSlotNumCpu

starSlotNum

Object ID

enterprises.8164.1.2.1.1.1

Description

The slot number.

Syntax

Integer32(1..48)

Access

Not-accessible
Object

starSlotType

Object ID

enterprises.8164.1.2.1.1.2

Description

The type of the slot.

Syntax

StarentSlotType

Access

Read-only
Object

starCardType

Object ID

enterprises.8164.1.2.1.1.3

Description

The type of the card which is plugged into a slot.

Syntax

StarentCardType

Access

Read-only
Object

starCardOperState

Object ID

enterprises.8164.1.2.1.1.4

Description

The current operational state of the card.

Syntax

Integer

Access

Read-only

Enumeration

unknown(1)

empty(2)

offline(3)

booting(4)

ready(5)

standby(6)

active(7)

migratefrom(8)

migrateto(9)
Object

starCardAdminState

Object ID

enterprises.8164.1.2.1.1.5

Description

The current administrative state of the card.

Syntax

Integer

Access

Read-only

Enumeration

unknown(1)

enabled(2)

disabled(3)
Object

starCardRevision

Object ID

enterprises.8164.1.2.1.1.6

Description

The revision number of the card that is physically present in this slot.

Syntax

StarentVersionNum

Access

Read-only
Object

starCardLastStateChange

Object ID

enterprises.8164.1.2.1.1.7

Description

The time when the last state change occurred for this row. A manager could poll this variable to determine if information has changed.

Syntax

DateAndTime

Access

Read-only
Object

starCardMode

Object ID

enterprises.8164.1.2.1.1.8

Description

The desired mode of the card. This field is applicable only to slots which can contain packet processing cards.

Syntax

Integer {

unknown(1)

notapplicable(2)

standby(3)

active(4)

activepac(5)

activetac(6)

activepsc(7)

activevpc(8)

}

Access

Read-only
Object

starCardPacStandbyPriority

Object ID

enterprises.8164.1.2.1.1.9

Description

Specifies the standby priority of the packet accelerator card.

Syntax

Gauge32

Access

Read-only
Object

starCardHaltIssued

Object ID

enterprises.8164.1.2.1.1.10

Description

Only applicable to SPC cards.

IMPORTANT:

These cards are no longer supported.

Syntax

Integer

Access

Read-only

Enumeration

notapplicable(1)

yes(2)

no(3)
Object

starCardLock

Object ID

enterprises.8164.1.2.1.1.11

Description

Identifies if the card lock is currently engaged. A value of locked(2) means that the lock is engaged, and thus the card could not be removed from the chassis. A value of unlocked(3) means that the lock is not engaged, and an operator could remove the card from the chassis. A value of unknown(1) should represent that there is no card physically in the slot.

Syntax

Integer

Access

Read-only

Enumeration

unknown(1)

locked(2)

unlocked(3)
Object

starCardRebootPending

Object ID

enterprises.8164.1.2.1.1.12

Description

Identifies if a reboot operation is currently pending for this card.

Syntax

Integer

Access

Read-only

Enumeration

no(1)

yes(2)
Object

starCardUsable

Object ID

enterprises.8164.1.2.1.1.13

Description

Indicates if the card is currently usable.

Syntax

Integer

Access

Read-only

Enumeration

no(1)

yes(2)
Object

starCardSinglePOF

Object ID

enterprises.8164.1.2.1.1.14

Description

Identifies if this card represents a single point of failure (SPOF). A value of no(1) indicates that this card is supported by a redundant card which can take over in the event of a failure. A value of yes(2) indicates that this card does not have a redundant partner, and that a failure of this card could result in service interruption.

Syntax

Integer

Access

Read-only

Enumeration

notapplicable(1)

no(2)

yes(3)
Object

starCardAttachment

Object ID

enterprises.8164.1.2.1.1.15

Description

Identifies if the card is currently attached to another card (a packet processing card attached to a line card, for example)

Syntax

Integer

Access

Read-only

Enumeration

connected(1)

unconnected(2)
Object

starCardTemperature

Object ID

enterprises.8164.1.2.1.1.16

Description

The temperature, in degrees Celsius, as measured on the card. A value of 0 indicates that the temperature cannot be read, or that the card is not present. The maximum measurable temperature is 70 C.

Syntax

Gauge32

Access

Read-only

IMPORTANT:

All of the "voltage"-related starSlot items are obsolete. As systems evolved and different cards have different internal voltages these values had less meaning. Theobject starSlotVoltageState provides an overall state for the card.
Object

starSlotVoltage1dot5

Object ID

enterprises.8164.1.2.1.1.20

Description

The current voltage, in millivolts, of the nominal 1.5V power supply. The working range for this card is the range defined by variables starSlotVoltage1dot5LowThresh and starSlotVoltage1dot5HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage1dot5LowThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.21

Description

The voltage level, in millivolts, which is the lowest allowable value for the nominal 1.5V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage1dot5HighThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.22

Description

The voltage level, in millivolts, which is the highest allowable value for the nominal 1.5V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage1dot8

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification

Object ID

enterprises.8164.1.2.1.1.23

Description

The current voltage, in millivolts, of the nominal 1.8V power supply. The working range for this card is the range defined by variables starSlotVoltage1dot8LowThresh and starSlotVoltage1dot8HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage1dot8LowThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.24

Description

The voltage level, in millivolts, which is the lowest allowable value for the nominal 1.8V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage1dot8HighThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.25

Description

The voltage level, in millivolts, which is the highest allowable value for the nominal 1.8V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage2dot5

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.26

Description

The current voltage, in millivolts, of the nominal 2.5V power supply. The working range for this card is the range defined by variables starSlotVoltage2dot5LowThresh and starSlotVoltage2dot5HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage2dot5LowThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.27

Description

The voltage level, in millivolts, which is the lowest allowable value for the nominal 2.5V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage2dot5HighThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.28

Description

The voltage level, in millivolts, which is the highest allowable value for the nominal 2.5V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage3dot3

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.29

Description

The current voltage, in millivolts, of the nominal 3.3V power supply. The working range for this card is the range defined by variables starSlotVoltage3dot3LowThresh and starSlotVoltage3dot3HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage3dot3LowThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.30

Description

The voltage level, in millivolts, which is the lowest allowable value for the nominal 3.3V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage3dot3HighThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.31

Description

The voltage level, in millivolts, which is the highest allowable value for the nominal 3.3V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage5dot0

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.32

Description

The current voltage, in millivolts, of the nominal 5.0V power supply. The working range for this card is the range defined by variables starSlotVoltage5dot0LowThresh and starSlotVoltage5dot0HighThresh. A value of 0 indicates that the voltage cannot be read, or that the card is not present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage5dot0LowThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification.

Object ID

enterprises.8164.1.2.1.1.33

Description

The voltage level, in millivolts, which is the lowest allowable value for the nominal 5.0V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotVoltage5dot0HighThresh

IMPORTANT:

This alarm is obsolete. System uses starSlotVoltageState alarm for this notification

Object ID

enterprises.8164.1.2.1.1.34

Description

The voltage level, in millivolts, which is the highest allowable value for the nominal 5.0V power supply. A value of 0 indicates that there is no card present.

Syntax

Gauge32

Access

Read-only
Object

starSlotNumPorts

IMPORTANT:

This alarm is obsolete.

Object ID

enterprises.8164.1.2.1.1.35

Description

Number of data ports on this card. This value will be 0 for cards that do not contain ports, or for slots which do not contain a card.

Syntax

Gauge32

Access

Read-only
Object

starSlotAction

Object ID

enterprises.8164.1.2.1.1.36

Description

Trigger to perform certain slot operations. noaction(1) performs no operation. It is the normal value received when this attribute is read. reset(2) causes the slot to be reset.

Syntax

Integer

Access

Read-write

Enumeration

noaction(1)

reset(2)
Object

starSlotVoltageState

Object ID

enterprises.8164.1.2.1.1.37

Description

The state of the voltage supplies on the card. A value of unknown(0) means that the state cannot be identified; normal(1) represents a properly functioning card; outofrange(2) indicates that one or more voltage sources are not within their specified operating range.

Syntax

Integer

Access

Read-only

Enumeration

unknown(0)

normal(1)

outofrange(2)
Object

starSlotNumCpu

Object ID

enterprises.8164.1.2.1.1.38

Description

The number of general purpose CPU on this card.

Syntax

Integer32

Access

Read-only
Object

starSlotPartNumber

Object ID

enterprises.8164.1.2.1.1.39

Description

The part number of this card.

Syntax

DisplayString

Access

Read-only
Object

starSlotPartRevision

Object ID

enterprises.8164.1.2.1.1.40

Description

The revision number of this card.

Syntax

DisplayString

Access

Read-only
Object

starSlotSerialNumber

Object ID

enterprises.8164.1.2.1.1.41

Description

The serial number of this card.

Syntax

DisplayString

Access

Read-only
Object

starSlotCLEICode

Object ID

enterprises.8164.1.2.1.1.42

Description

The CLEI code of this card.

Syntax

DisplayString

Access

Read-only
Object

starSlotCiscoModelName

Object ID

enterprises.8164.1.2.1.1.43

Description

Cisco-defined Product Identifier (PID). The PID is an alphanumeric identifier used to identify specific Cisco product hardware, and may be up to 18 characters in length.

starSlotCiscoModelName will be blank (zero characters) if no PID is available.

Syntax

DisplayString

Access

Read-only
Object

starSlotCiscoHardwareRev

Object ID

enterprises.8164.1.2.1.1.44

Description

Cisco-defined Version Identifier (VID). The VID is used to track the version of the Customer-Orderable Cisco Product Identifier (PID) [starSlotCiscoModelName]. The data convention for VID is 'V' followed by a two digit number. VID numbering typically begins at 'V01' but can be initiated at a higher value.

starSlotCiscoModelName will be blank (zero characters) if no PID is available.

Syntax

DisplayString

Access

Read-only
Object

starSlotCiscoSerialNumber

Object ID

enterprises.8164.1.2.1.1.45

Description

Cisco-defined Serial Number (SN). The SN is an 11 character identifier used in conjunction with the Cisco Product Identifier (PID) [starSlotCiscoModelName] to identify a unique product or Field Replaceable Unit (FRU) of a product.

starSlotCiscoSerialNumber will be blank (zero characters) if no VID is available.

Syntax

DisplayString

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentSlotMapping(3)
Object

starSlotMappingTable

Object ID

enterprises.8164.1.3.1

Description

A table identifying all of the slot mappings.

Syntax

Sequence of StarSlotMappingEntry

Access

Not-accessible
Object

starSlotMappingEntry

Object ID

enterprises.8164.1.3.1.1

Description

Information about a particular slot mapping.

Syntax

StarSlotMappingEntry

Access

Not-accessible

Sequence

starSlotMappingNum Index

starSlotMappingType

starSlotMappingRCCNum

starSlotMappingToSlot
Object

starSlotMappingNum

Object ID

enterprises.8164.1.3.1.1.1

Description

The slot number. This always represents a slot in the back of the chassis.

Syntax

Integer32(17..48)

Access

Not-accessible
Object

starSlotMappingType

Object ID

enterprises.8164.1.3.1.1.2

Description

The type of the slot mapping. The value none(1) represents that there is no mapping, which typically represents that there is no card present in this slot.

Syntax

Integer

Access

Read-only

Enumeration

unknown(1)

none(2)

direct(3)

rcc(4)

cross(5)
Object

starSlotMappingRCCNum

Object ID

enterprises.8164.1.3.1.1.3

Description

Identifies which RCC card is responsible for this mapping. This value is only valid if the value of starSlotMappingType is rcc(3).

Syntax

Integer32(0..2)

Access

Read-only
Object

starSlotMappingToSlot

Object ID

enterprises.8164.1.3.1.1.4

Description

The slot number this slot is mapped to. This always represents a slot in the front of the chassis.

Syntax

Integer32(1..16)

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentFans(4)
Object

starFanTable

Object ID

enterprises.8164.1.4.1

Description

A table containing information on all of the fan controllers.

Syntax

Sequence of StarFanEntry

Access

Not-accessible
Object

starFanEntry

Object ID

enterprises.8164.1.4.1.1

Description

Information about a particular fan controller.

Syntax

StarFanEntry

Access

Not-accessible

Sequence

starFanNum Index

starFanLocation

starFanStatus

starFanSpeed
Object

starFanNum

Object ID

enterprises.8164.1.4.1.1.1

Description

The fan controller number.

Syntax

Integer32(1..2)

Access

Not-accessible
Object

starFanLocation

Object ID

enterprises.8164.1.4.1.1.2

Description

The physical location of the fan controller.

Syntax

Integer

Access

Read-only

Enumeration

upper(1)

lower(2)
Object

starFanStatus

Object ID

enterprises.8164.1.4.1.1.3

Description

A bitmask representing the status of the fan tray. A normal, properly functioning fan tray would show 0x101 (257 decimal), meaning it is present (0x100) and all fans are working (0x1).

Syntax

Integer32

Access

Read-only

Enumeration

0x01 All Fans Good

0x02 Multiple Fans Bad

0x04 Single Fan Bad

0x08 HB Error

0x10 COM A Error

0x20 COM B Error

0x40 COMM Error

0x80 Not Present

0x100 Present

0x200 Filter Clogged

0x400 State Unknown
Object

starFanSpeed

Object ID

enterprises.8164.1.4.1.1.4

Description

The speed of the fans controlled by this fan controller. The values represent the percentage that the speed is running relative to the maximum possible speed, speed100(12)

Syntax

Integer

Access

Read-only

Enumeration

unknown(1)

speed50(2)

speed55(3)

speed60(4)

speed65(5)

speed70(6)

speed75(7)

speed80(8)

speed85(9)

speed90(10)

speed95(11)

speed100(12)
starentMIB(8164).starentMIBObjects(1).starentLogs(5)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starLogTable

Object ID

enterprises.8164.1.5.1

Description

A table containing information about all of the system logs.

Syntax

Sequence of StarLogEntry

Access

Not-accessible
Object

starLogEntry

Object ID

enterprises.8164.1.5.1.1

Description

Information about a particular system log.

Syntax

StarLogEntry

Access

Not-accessible

Sequence

starLogName Index

starLogCurSize

starLogMaxSize

starLogText
Object

starLogName

Object ID

enterprises.8164.1.5.1.1.1

Description

The name of the system log.

Syntax

StarShortName

Access

Not-accessible
Object

starLogCurSize

Object ID

enterprises.8164.1.5.1.1.2

Description

The size, in bytes, of this log.

Syntax

Gauge32

Access

Read-only
Object

starLogMaxSize

Object ID

enterprises.8164.1.5.1.1.3

Description

The maximum size, in bytes, of this log.

Syntax

Gauge32

Access

Read-only
Object

starLogText

Object ID

enterprises.8164.1.5.1.1.4

Description

For use in LogMsg trap.

Syntax

Octet String (SIZE (1..512))

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentAlertMan(8).starentFeedback(1)
Object

starMaxAlertsPerTime

Object ID

enterprises.8164.1.8.1.1

Description

The maximum number of SNMP Traps which will be sent within the time period specified by starWindowTime.

Syntax

Gauge32

Access

Read-only
Object

starWindowTime

Object ID

enterprises.8164.1.8.1.2

Description

The amount of time, in seconds, within which no more than starMaxAlertsPerTime SNMP Traps will be sent.

Syntax

Unsigned32

Access

Read-only
Object

starAlertSendingEnabled

Object ID

enterprises.8164.1.8.1.3

Description

Shows if SNMP traps are currently enabled or disabled. Traps are disabled when more than starMaxAlertsPerTime traps are sent within the starWindowTime time period. A value of true(1) indicates that traps will still be sent. A value of false(2) indicates that traps are no longer being generated

Syntax

TruthValue

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentPower(9)
Object

starPowerTable

Object ID

enterprises.8164.1.9.1

Description

A table containing information about all power filters.

Syntax

Sequence of StarPowerEntry

Access

Not-accessible
Object

starPowerEntry

Object ID

enterprises.8164.1.9.1.1

Description

Information about a particular power filter.

Syntax

StarPowerEntry

Access

Not-accessible

Sequence

starPowerNumber Index

starPowerState
Object

starPowerNumber

Object ID

enterprises.8164.1.9.1.1.1

Description

The identifying number for this power filter.

Syntax

Integer

Access

Not-accessible

Enumeration

powerA(1)

powerB(2)
Object

starPowerState

Object ID

enterprises.8164.1.9.1.1.2

Description

The state of the power filter. The value active(1) means that the power filter is present and operational. The value failed(2) means that the power filter is present, but not operational. The value not-present(3) means that the power filter is not physically present in the system.

Syntax

Integer

Access

Read-only

Enumeration

active(1)

failed(2)

notpresent(3)
starentMIB(8164).starentMIBObjects(1).starentCPU(10)
Object

starCPUTable

Object ID

enterprises.8164.1.10.1

Description

A table containing information about all CPUs

Syntax

Sequence of StarCPUEntry

Access

Not-accessible
Object

starCPUEntry

Object ID

enterprises.8164.1.10.1.1

Description

Information about a particular CPU.

Syntax

StarCPUEntry

Access

Not-accessible

Sequence

starCPUSlot Index

starCPUNumber Index

starCPUUser

starCPUSystem

starCPUIdle

starCPUIO

starCPURQ

starCPULoad1Min

starCPULoad5Min

starCPULoad15Min

starCPUMemTotal

starCPUMemUsed

starCPUNumProcesses

starCPUMemCached
Object

starCPUSlot

Object ID

enterprises.8164.1.10.1.1.1

Description

The slot number of the card holding this CPU.

Syntax

Integer32(1..16)

Access

Not-accessible
Object

starCPUNumber

Object ID

enterprises.8164.1.10.1.1.2

Description

The CPU number within this card. Numbers begin at 0.

Syntax

Integer32(0..3)

Access

Not-accessible
Object

starCPUUser

Object ID

enterprises.8164.1.10.1.1.3

Description

Percentage of the CPU spent running user processes. starCPUUser is the percentage value times 100; for example, 2.3% would be represented as 230

Syntax

Integer32(1..10000)

Access

Read-only
Object

starCPUSystem

Object ID

enterprises.8164.1.10.1.1.4

Description

Percentage of the CPU spent running system processes. starCPUSystem is the percentage value times 100; for example, 2.3% would be represented as 230.

Syntax

Integer32(1..10000)

Access

Read-only
Object

starCPUIdle

Object ID

enterprises.8164.1.10.1.1.6

Description

Percentage of the CPU spent idle. starCPUIdle is the percentage value times 100; for example, 2.3% would be represented as 230.

Syntax

Integer32(1..10000)

Access

Read-only
Object

starCPUIO

Object ID

enterprises.8164.1.10.1.1.7

Description

Percentage of the CPU spent running Input/Output processes. starCPUIO is the percentage value times 100; for example, 2.3% would be represented as 230.

Syntax

Integer32(1..10000)

Access

Read-only
Object

starCPURQ

Object ID

enterprises.8164.1.10.1.1.8

Description

Percentage of the CPU spent running IRQ processes. starCPURQ is the percentage value times 100; for example, 2.3% would be represented as 230.

Syntax

Integer32(1..10000)

Access

Read-only
Object

starCPULoad1Min

Object ID

enterprises.8164.1.10.1.1.11

Description

The average CPU load over the last minute. The CPU load is defined to be the number of processes who are ready to run. starCPULoad1Min is the average number of processes times 100; for example, 2.45 would be represented as 245.

Syntax

Integer32(1..1000000000)

Access

Read-only
Object

starCPULoad5Min

Object ID

enterprises.8164.1.10.1.1.12

Description

The average CPU load over the last 5 minutes. The CPU load is defined to be the number of processes who are ready to run. starCPULoad5Min is the average number of processes times 100; for example, 2.45 would be represented as 245.

Syntax

Integer32(1..1000000000)

Access

Read-only
Object

starCPULoad15Min

Object ID

enterprises.8164.1.10.1.1.13

Description

The average CPU load over the last 15 minutes. The CPU load is defined to be the number of processes who are ready to run. starCPULoad15Min is the average number of processes times 100; for example, 2.45 would be represented as 245.

Syntax

Integer32(1..1000000000)

Access

Read-only
Object

starCPUMemTotal

Object ID

enterprises.8164.1.10.1.1.14

Description

The total amount of memory dedicated to this CPU, in kilobytes.

Syntax

Integer32(1..2097152)

Access

Read-only
Object

starCPUMemUsed

Object ID

enterprises.8164.1.10.1.1.15

Description

The total amount of memory consumed by this CPU, in kilobytes.

Syntax

Integer32(1..2097152)

Access

Read-only
Object

starCPUNumProcesses

Object ID

enterprises.8164.1.10.1.1.16

Description

The total number of processes which exist on this CPU.

Syntax

Integer32(1..4096)

Access

Read-only
Object

starCPUMemCached

Object ID

enterprises.8164.1.10.1.1.17

Description

The total amount of memory consumed by the (reusable) memory cache on this CPU, in kilobytes

Syntax

Integer32(1..2097152)

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentNPUMgr(11)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starNPUMgrTable

Object ID

enterprises.8164.1.11.1

Description

A table containing information about all NPU Managers.

Syntax

Sequence of StarNPUMgrEntry

Access

Not-accessible
Object

starNPUMgrEntry

Object ID

enterprises.8164.1.11.1.1

Description

Information about a particular NPU Manager.

Syntax

StarNPUMgrEntry

Access

Not-accessible

Sequence

starNPUMgrNumber
Object

starNPUMgrNumber

Object ID

enterprises.8164.1.11.1.1.1

Description

The identity of this NPU.

Syntax

Integer32(1..65535)

Access

Not-accessible
starentMIB(8164).starentMIBObjects(1).starentSessInP(12)
Object

starSessInProgCalls

Object ID

enterprises.8164.1.12.1

Description

The number of sessions currently in progress.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgActiveCalls

Object ID

enterprises.8164.1.12.2

Description

The number of sessions with active calls.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgDormantCalls

Object ID

enterprises.8164.1.12.3

Description

The number of sessions associated with dormant calls.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgArrived

Object ID

enterprises.8164.1.12.4

Description

The number of sessions in the arrived state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgLCPNeg

Object ID

enterprises.8164.1.12.5

Description

The number of sessions in the link control protocol negotiation state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgLCPUp

Object ID

enterprises.8164.1.12.6

Description

The number of sessions in the link control protocol up state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgAuthenticating

Object ID

enterprises.8164.1.12.7

Description

The number of sessions in the authenticating state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgAuthenticated

Object ID

enterprises.8164.1.12.8

Description

The number of sessions in the authenticated state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgIPCPUp

Object ID

enterprises.8164.1.12.9

Description

The number of sessions in the IP control protocol up state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgSIPConn

Object ID

enterprises.8164.1.12.10

Description

The number of sessions in the Simple IP connected state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgMIPConn

Object ID

enterprises.8164.1.12.11

Description

The number of sessions in the Mobile IP connected state.

Syntax

Gauge32

Access

Read-only
Object

starSessInProgDisc

Object ID

enterprises.8164.1.12.12

Description

The number of sessions in the disconnecting state.

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentSessMgr(13)
Object

starSessMgrCount

Object ID

enterprises.8164.1.13.1

Description

The total number of session manager instances.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlArrived

Object ID

enterprises.8164.1.13.2

Description

The total number of requested sessions.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlRejected

Object ID

enterprises.8164.1.13.3

Description

The total number of rejected sessions.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlConnected

Object ID

enterprises.8164.1.13.4

Description

The total number of sessions which were connected.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlAuthSucc

Object ID

enterprises.8164.1.13.5

Description

The total number of sessions where authentication was successful.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlAuthFail

Object ID

enterprises.8164.1.13.6

Description

The total number of sessions which failed authentication.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlLCPUp

Object ID

enterprises.8164.1.13.7

Description

The total number of sessions in the link control protocol in the up state.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlIPCPUp

Object ID

enterprises.8164.1.13.8

Description

The total number of sessions in the IP control protocol up state.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlSrcViol

Object ID

enterprises.8164.1.13.9

Description

The total number of sessions which had an invalid source.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlKeepFail

Object ID

enterprises.8164.1.13.10

Description

The total number of sessions which had a keep alive failure.

Syntax

Gauge32

Access

Read-only
Object

starSessTtlOctForwarded

Object ID

enterprises.8164.1.13.11

Description

The total number of octets forwarded (data + control).

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlRPRegAccept

Object ID

enterprises.8164.1.13.12

Description

The total number of Initial RRQ Accepted.

Syntax

Counter32

Access

Read-only
Object

starSessTtlRPRegAcceptInterPDSN

Object ID

enterprises.8164.1.13.13

Description

The total number of Inter PDSN Handoff RRQ Accepted.

Syntax

Counter32

Access

Read-only
Object

starPPPCurrSessions

Object ID

enterprises.8164.1.13.14

Description

The current number of PPP sessions

Syntax

Counter32

Access

Read-only
Object

starSessTtlTxBytes

Object ID

enterprises.8164.1.13.15

Description

The total number of bytes transmitted from mobiles

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlRxBytes

Object ID

enterprises.8164.1.13.16

Description

he total number of bytes received by mobiles

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlSIPTxBytes

Object ID

enterprises.8164.1.13.17

Description

The total number of bytes transmitted from mobiles using SIP

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlSIPRxBytes

Object ID

enterprises.8164.1.13.18

Description

The total number of bytes received by mobiles using SIP

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlMIPTxBytes

Object ID

enterprises.8164.1.13.19

Description

The total number of bytes transmitted from mobiles using MIP

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlMIPRxBytes

Object ID

enterprises.8164.1.13.20

Description

The total number of bytes received by mobiles using MIP

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starSessTtlOctForwardedGB

Object ID

enterprises.8164.1.13.21

Description

The total number of octets forwarded (data + control)

Syntax

Counter32

Units

Gigabytes

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentAAAMgr(14)
Object

starAAAMgrCount

Object ID

enterprises.8164.1.14.1

Description

The total number of AAA manager instances.

Syntax

Gauge32

Access

Read-only
Object

starAAATtlRequests

Object ID

enterprises.8164.1.14.2

Description

The total number of AAA requests.

Syntax

Gauge32

Access

Read-only
Object

starAAATtlAuthRequests

Object ID

enterprises.8164.1.14.3

Description

The total number of AAA authentication requests.

Syntax

Gauge32

Access

Read-only
Object

starAAATtlAcctRequests

Object ID

enterprises.8164.1.14.4

Description

The total number of AAA accounting requests.

Syntax

Gauge32

Access

Read-only
Object

starAAACurRequests

Object ID

enterprises.8164.1.14.5

Description

The current number of AAA requests.

Syntax

Gauge32

Access

Read-only
Object

starAAACurAuthRequests

Object ID

enterprises.8164.1.14.6

Description

The current number of AAA authentication requests.

Syntax

Gauge32

Access

Read-only
Object

starAAACurAcctRequests

Object ID

enterprises.8164.1.14.7

Description

The current number of AAA accounting requests.

Syntax

Gauge32

Access

Read-only
Object

starAAATtlAcctSess

Object ID

enterprises.8164.1.14.8

Description

The total number of AAA accounting sessions.

Syntax

Gauge32

Access

Read-only
Object

starAAACurAcctSess

Object ID

enterprises.8164.1.14.9

Description

The current number of accounting sessions

Syntax

Gauge32

Access

Read-only
Object

starAAATtlAuthSuccess

Object ID

enterprises.8164.1.14.10

Description

The total number of AAA authentication successes.

Syntax

Gauge32

Access

Read-only
Object

starAAATtlAuthFailure

Object ID

enterprises.8164.1.14.11

Description

The total number of AAA authentication failures.

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentA11Mgr(15)
Object

starA11MgrCount

Object ID

enterprises.8164.1.15.1

Description

The total number of A11 manager instances.

Syntax

Gauge32

Access

Read-only
Object

starA11TtlArrived

Object ID

enterprises.8164.1.15.2

Description

The total number of A11 session requests.

Syntax

Gauge32

Access

Read-only
Object

starA11TtlRejected

Object ID

enterprises.8164.1.15.3

Description

The total number of rejected A11 sessions.

Syntax

Gauge32

Access

Read-only
Object

starA11TtlDemultiplexed

Object ID

enterprises.8164.1.15.4

Description

The total number of demultiplexed A11 sessions.

Syntax

Counter32

Access

Read-only
Object

starA11TtlDereg

Object ID

enterprises.8164.1.15.5

Description

The total number of A11 deregistrations.

Syntax

Counter32

Access

Read-only
Object

starA11CurActive

Object ID

enterprises.8164.1.15.6

Description

The current number of active A11 sessions.

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentHAMgr(16)
Object

starHAMgrCount

Object ID

enterprises.8164.1.16.1

Description

The total number of home agent manager instances.

Syntax

Gauge32

Access

Read-only
Object

starHATtlArrived

Object ID

enterprises.8164.1.16.2

Description

The total number of home agent session requests.

Syntax

Counter32

Access

Read-only
Object

starHATtlRejected

Object ID

enterprises.8164.1.16.3

Description

The total number of rejected home agent sessions.

Syntax

Counter32

Access

Read-only
Object

starHATtlDemultiplexed

Object ID

enterprises.8164.1.16.4

Description

The total number of demultiplexed home agent sessions.

Syntax

Counter32

Access

Read-only
Object

starHATtlDereg

Object ID

enterprises.8164.1.16.5

Description

The total number of home agent deregistrations.

Syntax

Counter32

Access

Read-only
Object

starHACurActive

Object ID

enterprises.8164.1.16.6

Description

The current number of active home agent sessions.

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentFAMgr(17)
Object

starFAMgrCount

Object ID

enterprises.8164.1.17.1

Description

The total number of foreign agent manager instances.

Syntax

Gauge32

Access

Read-only
Object

starFATtlArrived

Object ID

enterprises.8164.1.17.2

Description

The total number of foreign agent session requests.

Syntax

Counter32

Access

Read-only
Object

starFATtlRejected

Object ID

enterprises.8164.1.17.3

Description

The total number of rejected foreign agent sessions.

Syntax

Counter32

Access

Read-only
Object

starFATtlDemultiplexed

Object ID

enterprises.8164.1.17.4

Description

The total number of demultiplexed foreign agent sessions.

Syntax

Counter32

Access

Read-only
Object

starFATtlDereg

Object ID

enterprises.8164.1.17.5

Description

The total number of foreign agent deregistrations.

Syntax

Counter32

Access

Read-only
Object

starFACurActive

Object ID

enterprises.8164.1.17.6

Description

The current number of active foreign agent sessions.

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentService(18)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starServiceTable

Object ID

enterprises.8164.1.18.1

Description

A table containing information about all of the service managers.

Syntax

Sequence of StarSvcEntry

Access

Not-accessible
Object

starServiceEntry

Object ID

enterprises.8164.1.18.1.1

Description

Information about a particular service manager.

Syntax

StarSvcEntry

Access

Not-accessible

Sequence

starServiceVpnID Index

starServiceSvcID Index

starServiceVpnName

starServiceServName

starServiceSubLimit

starServiceSubCurrent

starServiceType

starServiceFAIpAddr

starServiceHAIpAddr
Object

starServiceVpnId

Object ID

enterprises.8164.1.18.1.1.1

Description

The internal identification of the VPN (context).

Syntax

Gauge32

Access

Not-accessible
Object

starServiceSvcID

Object ID

enterprises.8164.1.18.1.1.2

Description

The internal identification of the service, unique to the associated context.

Syntax

Gauge32

Access

Not-accessible
Object

starServiceVpnName

Object ID

enterprises.8164.1.18.1.1.3

Description

The name of the VPN (context).

Syntax

DisplayString

Access

Read-only
Object

starServiceServName

Object ID

enterprises.8164.1.18.1.1.4

Description

The name of the service.

Syntax

DisplayString

Access

Read-only
Object

starServiceSubLimit

Object ID

enterprises.8164.1.18.1.1.5

Description

The configured subscriber limit.

Syntax

Unsigned32

Access

Read-only
Object

starServiceSubCurrent

Object ID

enterprises.8164.1.18.1.1.6

Description

Current subscriber limit.

Syntax

Gauge32

Access

Read-only
Object

starServiceType

Object ID

enterprises.8164.1.18.1.1.7

Description

Service type.

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(1)

pdsn(2)

ggsn(3)

ha(4)

fa(5)

l2tpserver(6)

lac(7)

lns(8)

closedrp(9

ecs(10)

cscf(11)

ipsg(12)

evdoreva(13)

pdif(15)

asnpc(16)

mipv6ha(17)

phsgw(18)

phspc(19)

sgw(20)

pgw(21)

mag(22)

gprs(23)

hsgw(24)

sgsn(25)

mme(26)

pdg(27)

standalonefa(28)

imsue(29)

fng(30)

pccpolicy(31)

pccquota(32)

pccaf(33)
Object

starServiceFAIpAddr

Object ID

enterprises.8164.1.18.1.1.8

Description

The IP address for an FA service. Where unknown or not applicable this will contain all zeroes.

Syntax

IpAddress

Access

Read-only
Object

starServiceHAIpAddr

Object ID

enterprises.8164.1.18.1.1.9

Description

The IP address for an HA service. Where unknown or not applicable this will contain all zeroes.

Syntax

IpAddress

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentCLIMgr(19)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starCLITable

Object ID

enterprises.8164.1.19.1

Description

A table containing information about all interactive CLI sessions.

Syntax

Sequence of StarCLIEntry

Access

Not-accessible
Object

starCLIEntry

Object ID

enterprises.8164.1.19.1.1

Description

Information about a particular CLI session.

Syntax

StarSvcEntry

Access

Not-accessible

Sequence

starCLIID

starCLIUsername

starCLITtyname

starCLIPrivs

starCLIType

starCLIRemoteIpAddr

starCLIContext
Object

starCLIID

Object ID

enterprises.8164.1.19.1.1.1

Description

The internal identify of the CLI session.

Syntax

Gauge32

Access

Not-accessible
Object

starCLIUsername

Object ID

enterprises.8164.1.19.1.1.2

Description

The name of the user logged into the CLI sessions or ‘unknown’ if not known.

Syntax

DisplayString

Access

Read-only
Object

starCLITtyname

Object ID

enterprises.8164.1.19.1.1.3

Description

The name of the TTY device used for the CLI session.

Syntax

DisplayString

Access

Read-only
Object

starCLIPrivs

Object ID

enterprises.8164.1.19.1.1.4

Description

The CLI session privilege level.

Syntax

DisplayString

Access

Read-only
Object

starCLIType

Object ID

enterprises.8164.1.19.1.1.5

Description

The CLI type; commandline(1) represents the normal interactive command line; ftp(2) represents an incoming FTP session.

Syntax

INTEGER {

unknown(0)

commandline(1)

ftp(2)

}

Access

Read-only
Object

starCLIRemoteIPAddr

Object ID

enterprises.8164.1.19.1.1.6 (prior to 14.0)

Description

The remote IP address used to access this CLI session. Where unknown or not applicable (such as access through a serial port) this will be 0.

Syntax

InetAddress

Access

Read-only
Object

starCLIContext

Object ID

enterprises.8164.1.19.1.1.7 (Prior to 14.0)

Description

The context (VPN) currently being viewed or managed by the CLI session.

Syntax

DisplayString

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentTaskMgr(20)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starTaskTable

Object ID

enterprises.8164.1.20.1

Description

A table containing information about all of the active tasks.

Syntax

Sequence of StarSvcEntry

Access

Not-accessible
Object

starTaskEntry

Object ID

enterprises.8164.1.20.1.1

Description

Information about a particular task.

Syntax

StarSvcEntry

Access

Not-accessible

Sequence

starTaskFacility Index

starTaskInstance Index

starTaskFacilityName

starTaskCard

starTaskCPU
Object

starTaskFacility

Object ID

enterprises.8164.1.20.1.1.1

Description

The internal identify of the facility.

Syntax

Unsigned32

Access

Not-accessible
Object

starTaskInstance

Object ID

enterprises.8164.1.20.1.1.2

Description

The unique internal instance identifier for the task without a given facility.

Syntax

Unsigned32

Access

Read-only
Object

starTaskFacilityName

Object ID

enterprises.8164.1.20.1.1.3

Description

The name of the facility the task is associated with.

Syntax

DisplayString

Access

Read-only
Object

starTaskCard

Object ID

enterprises.8164.1.20.1.1.4

Description

The slot number of the card where the task is located.

Syntax

Unsigned32

Access

Read-only
Object

starTaskCPU

Object ID

enterprises.8164.1.20.1.1.5

Description

The CPU number where the task is running.

Syntax

Unsigned32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentPPP(21)
Object

starPPPStatTable

Object ID

enterprises.8164.1.21.1

Description

A table containing PPP statistics.

Syntax

Sequence of StarPPPStatEntry

Access

Not-accessible
Object

starPPPStatEntry

Object ID

enterprises.8164.1.21.1.1

Description

The statistics for an individual entry for a PPP context and service.

Syntax

StarPPPStatEntry

Access

Not-accessible

Sequence

starPPPStatVpnID

starPPPStatSvcID Index (Implied)

starPPPStatVpnName

starPPPStatServName

starPPPStatInit

starPPPStatReneg

starPPPStatSuccess

starPPPStatFailed

starPPPStatReleased

starPPPStatReleasedLocal

starPPPStatReleasedRemote

starPPPStatLcpFailMaxRetry

starPPPStatLcpFailOption

starPPPStatIpcpFailMaxRetry

starPPPStatIpcpFailOption

starPPPStatCcpFail

starPPPStatAuthFail

starPPPStatLcpEntered

starPPPStatAuthEntered

starPPPStatIpcpEntered

starPPPStatRenegPdsn

starPPPStatRenegMobil

starPPPStatRenegAddrMismatch

starPPPStatRenegOther

starPPPStatChapAuthAttempt

starPPPStatPapAuthAttempt

starPPPStatMSChapAuthAttempt

starPPPStatChapAuthFail

starPPPStatPapAuthFail

starPPPStatMSChapAuthFail

starPPPStatStacComp

starPPPStatMppcComp

starPPPStatDeflComp

starPPPStatFscErrs

starPPPStatUnknProto

starPPPStatBadAddr

starPPPStatBadCtrl

starPPPStatVjComp

starPPPStatDiscLcpRemote

starPPPStatDiscRpRemote

starPPPStatDiscAdmin

starPPPStatDiscIdleTimeout

starPPPStatDiscAbsTimeout

starPPPStatDiscPPPKeepalive

starPPPStatDiscNoResource

starPPPStatDiscMisc

starPPPStatFailedReneg

starPPPStatLcpFailUnknown

starPPPStatIpcpFailUnknown

starPPPStatAuthAbort

starPPPStatLowerLayerDisc

starPPPStatLcpSuccess

starPPPStatAuthSuccess

starPPPStatRenegLowerLayerHandoff

starPPPStatRenegParamUpdate

starPPPStatChapAuthSuccess

starPPPStatPapAuthSuccess

starPPPStatMSChapAuthSuccess

starPPPStatChapAuthAbort

starPPPStatPapAuthAbort

starPPPStatMSChapAuthAbort

starPPPStatSessSkipAuth

starPPPStatNegComp

starPPPStatCCPNegFailComp

starPPPStatDiscLocalLowerLayer

starPPPStatDiscAddFlowFail

starPPPStatDiscMaxRetriesLCP

starPPPStatDiscMaxRetriesIPCP

starPPPStatDiscMaxSetupTimer

starPPPStatDiscInvalidDestVpn

starPPPStatDiscOptNegFailLCP

starPPPStatDiscOptNegFailIPCP

arPPPStatDiscNoRemoteIpAddr

starPPPStatDiscCallTypeDetectFail

starPPPStatDiscRemoteDiscUpLayer

starPPPStatDiscLongDuraTimeout

starPPPStatDiscAuthFail

starPPPStatLCPEchoTotalReq

starPPPStatLCPEchoReqResent

starPPPStatLCPEchoRepRecved

starPPPStatLCPEchoReqTimeout

starPPPStatRecvErrBadCtrlField

starPPPStatRecvErrBadPacketLen

starPPPStatRemoteTerm

starPPPStatMiscFail
Object

starPPPStatVpnID

Object ID

enterprises.8164.1.21.1.1.1

Description

The internal identification of the PPP VPN (context).

Syntax

Gauge32

Access

Not-accessible
Object

starPPPStatSvcID

Object ID

enterprises.8164.1.21.1.1.2

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

Syntax

StarShortID

Access

Not-accessible
Object

starPPPStatVpnName

Object ID

enterprises.8164.1.21.1.1.3

Description

The name of the PPP VPN (context).

Syntax

DisplayString

Access

Read-only
Object

starPPPStatServName

Object ID

enterprises.8164.1.21.1.1.4

Description

The name of the PPP service.

Syntax

DisplayString

Access

Read-only
Object

starPPPStatInit

Object ID

enterprises.8164.1.21.1.1.5

Description

The number of initialized PPP sessions for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatReneg

Object ID

enterprises.8164.1.21.1.1.6

Description

The number of PPP session renegotiations for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatSuccess

Object ID

enterprises.8164.1.21.1.1.7

Description

The number of PPP session negotiation successes for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatFailed

Object ID

enterprises.8164.1.21.1.1.8

Description

The number of PPP session negotiation failures for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatReleased

Object ID

enterprises.8164.1.21.1.1.9

Description

The number of PPP sessions released for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatReleasedLocal

Object ID

enterprises.8164.1.21.1.1.10

Description

The number of PPP sessions where the release was initiated locally for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatReleasedRemote

Object ID

enterprises.8164.1.21.1.1.11

Description

The number of PPP session where the release was initiated remotely for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLcpFailMaxRetry

Object ID

enterprises.8164.1.21.1.1.12

Description

The number of PPP sessions which failed to bring up the link control protocol due to excessive retries for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLcpFailOption

Object ID

enterprises.8164.1.21.1.1.13

Description

The number of PPP sessions which failed to bring up the Link Control Protocol (LCP) due to an invalid option being received for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatIpcpFailMaxRetry

Object ID

enterprises.8164.1.21.1.1.14

Description

The number of PPP sessions which failed to start the IP Control Protocol (IPCP) due to excessive retries for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatIpcpFailOption

Object ID

enterprises.8164.1.21.1.1.15

Description

The number of PPP sessions which failed to start the IP Control Protocol due to an invalid option being received for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatCcpFail

Object ID

enterprises.8164.1.21.1.1.16

Description

The number of PPP sessions which failed to initialize the CCP.

Syntax

Counter32

Access

Read-only
Object

starPPPStatAuthFail

Object ID

enterprises.8164.1.21.1.1.17

Description

The number of PPP sessions which failed authentication for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLcpEntered

Object ID

enterprises.8164.1.21.1.1.18

Description

The number of PPP sessions which successfully initialized the Link Control Protocol.

Syntax

Counter32

Access

Read-only
Object

starPPPStatAuthEntered

Object ID

enterprises.8164.1.21.1.1.19

Description

The number of PPP sessions which were successfully authenticated.

Syntax

Counter32

Access

Read-only
Object

starPPPStatIpcpEntered

Object ID

enterprises.8164.1.21.1.1.20

Description

The number of PPP sessions which successfully initialized the IP Control Protocol.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRenegPdsn

Object ID

enterprises.8164.1.21.1.1.21

Description

The number of PPP sessions which re-negotiated the PDSN service access.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRenegMobil

Object ID

enterprises.8164.1.21.1.1.22

Description

The number of PPP sessions which re-negotiated the Mobile IP service access.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRenegAddrMismatch

Object ID

enterprises.8164.1.21.1.1.23

Description

The number of PPP sessions which had an IP address mismatch during re-negotiation.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRenegOther

Object ID

enterprises.8164.1.21.1.1.24

Description

The number of PPP sessions which failed renegotiation for reasons other than IP address mismatch.

Syntax

Counter32

Access

Read-only
Object

starPPPStatChapAuthAttempt

Object ID

enterprises.8164.1.21.1.1.25

Description

The number of PPP CHAP authentication attempts for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatPapAuthAttempt

Object ID

enterprises.8164.1.21.1.1.26

Description

The number of PPP PAP authentication attempts for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatMSChapAuthAttempt

Object ID

enterprises.8164.1.21.1.1.27

Description

The number of PPP MSCHAP authentication attempts for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatChapAuthFail

Object ID

enterprises.8164.1.21.1.1.28

Description

The number of PPP CHAP authentication attempt failures for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatPapAuthFail

Object ID

enterprises.8164.1.21.1.1.29

Description

The number of PPP PAP authentication failures for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatMSChapAuthFail

Object ID

enterprises.8164.1.21.1.1.30

Description

The number of PPP MSCHAP authentication failures for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatStacComp

Object ID

enterprises.8164.1.21.1.1.31

Description

The number of PPP sessions which had STAC compression enabled for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatMppcComp

Object ID

enterprises.8164.1.21.1.1.32

Description

The number of PPP sessions which had MPPC compression enabled for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDeflComp

Object ID

enterprises.8164.1.21.1.1.33

Description

The number of PPP sessions which had DEFLATE compression enabled for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatFscErrs

Object ID

enterprises.8164.1.21.1.1.34

Description

The number of PPP forward sequence control errors in messaging.

Syntax

Counter32

Access

Read-only
Object

starPPPStatUnknProto

Object ID

enterprises.8164.1.21.1.1.35

Description

The number of PPP sessions which failed due to an unknown protocol received for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatBadAddr

Object ID

enterprises.8164.1.21.1.1.36

Description

The number of PPP sessions which failed due to a bad address being received for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatBadCtrl

Object ID

enterprises.8164.1.21.1.1.37

Description

The number of PPP sessions in which a bad control sequence was received.

Syntax

Counter32

Access

Read-only
Object

starPPPStatVjComp

Object ID

enterprises.8164.1.21.1.1.38

Description

The number of PPP sessions which had VJ header compression enabled for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscLcpRemote

Object ID

enterprises.8164.1.21.1.1.39

Description

The number of PPP sessions which were disconnected via the link control protocol from the remote end for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscRpRemote

Object ID

enterprises.8164.1.21.1.1.40

Description

The number of PPP sessions which were disconnected by the remote via the R-P interface for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscAdmin

Object ID

enterprises.8164.1.21.1.1.41

Description

The number of PPP sessions which were disconnected by a local administrator for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscIdleTimeout

Object ID

enterprises.8164.1.21.1.1.42

Description

The number of PPP sessions disconnected due to session idle timer expiration for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscAbsTimeout

Object ID

enterprises.8164.1.21.1.1.43

Description

The number of PPP sessions disconnected due to the session absolute timer expiration for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscPPPKeepalive

Object ID

enterprises.8164.1.21.1.1.44

Description

The number of PPP sessions disconnected due to PPP keep alive failure for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscNoResource

Object ID

enterprises.8164.1.21.1.1.45

Description

The number of PPP sessions disconnected due to local resource shortage for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscMisc

Object ID

enterprises.8164.1.21.1.1.46

Description

The number of PPP sessions disconnected due to any cause which does not match any other existing disconnect statistic for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatFailedReneg

Object ID

enterprises.8164.1.21.1.1.47

Description

The number of failed PPP renegotiations the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLcpFailUnknown

Object ID

enterprises.8164.1.21.1.1.48

Description

The number of failed PPP LCP that are due to unknown reasons for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatIpcpFailUnknown

Object ID

enterprises.8164.1.21.1.1.49

Description

The number of failed PPP IPCP that are due to unknown reasons for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatAuthAbort

Object ID

enterprises.8164.1.21.1.1.50

Description

The number of aborted PPP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLowerLayerDisc

Object ID

enterprises.8164.1.21.1.1.51

Description

The number of Failed PPP session due to RP disconnect for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLcpSuccess

Object ID

enterprises.8164.1.21.1.1.52

Description

The number of successful PPP LCPs for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatAuthSuccess

Object ID

enterprises.8164.1.21.1.1.53

Description

The number of successful PPP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRenegLowerLayerHandoff

Object ID

enterprises.8164.1.21.1.1.54

Description

The number of PPP renegotiations for RP handoff for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRenegParamUpdate

Object ID

enterprises.8164.1.21.1.1.55

Description

The number of PPP renegotiations for parameter update for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatChapAuthSuccess

Object ID

enterprises.8164.1.21.1.1.56

Description

The number of successful PPP CHAP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatPapAuthSuccess

Object ID

enterprises.8164.1.21.1.1.57

Description

The number of successful PPP PAP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatMSChapAuthSuccess

Object ID

enterprises.8164.1.21.1.1.58

Description

The number of successful PPP MSCHAP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatChapAuthAbort

Object ID

enterprises.8164.1.21.1.1.59

Description

The number of aborted PPP CHAP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatPapAuthAbort

Object ID

enterprises.8164.1.21.1.1.60

Description

The number of aborted PPP PAP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatMSChapAuthAbort

Object ID

enterprises.8164.1.21.1.1.61

Description

The number of aborted PPP MSCHAP authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatSessSkipAuth

Object ID

enterprises.8164.1.21.1.1.62

Description

The number of PPP sessions that skipped authentications for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatNegComp

Object ID

enterprises.8164.1.21.1.1.63

Description

The number of PPP sessions that negotiated compressions for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatCCPNegFailComp

Object ID

enterprises.8164.1.21.1.1.64

Description

The number of PPP sessions that failed compression negotiation for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscLocalLowerLayer

Object ID

enterprises.8164.1.21.1.1.65

Description

The number of disconnected PPP sessions due to local RP disconnect for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscAddFlowFail

Object ID

enterprises.8164.1.21.1.1.66

Description

The number of disconnected PPP sessions due to failure in adding new flow for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscMaxRetriesLCP

Object ID

enterprises.8164.1.21.1.1.67

Description

The number of disconnected PPP sessions due to max retries for LCP for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscMaxRetriesIPCP

Object ID

enterprises.8164.1.21.1.1.68

Description

The number of disconnected PPP sessions due to max retries for IPCP for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscMaxSetupTimer

Object ID

enterprises.8164.1.21.1.1.69

Description

The number of disconnected PPP sessions due to max setup time out for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscInvalidDestVpn

Object ID

enterprises.8164.1.21.1.1.70

Description

The number of disconnected PPP sessions due to invalid destination VPN for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscOptNegFailLCP

Object ID

enterprises.8164.1.21.1.1.71

Description

The number of disconnected PPP sessions due to invalid destination VPN for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscOptNegFailIPCP

Object ID

enterprises.8164.1.21.1.1.72

Description

The number of disconnected PPP sessions due to failed IPCP option negotiation for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscNoRemoteIpAddr

Object ID

enterprises.8164.1.21.1.1.73

Description

The number of disconnected PPP sessions due to no remote IP address for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscCallTypeDetectFail

Object ID

enterprises.8164.1.21.1.1.74

Description

The number of disconnected PPP sessions due to failure detecting call type for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscRemoteDiscUpLayer

Object ID

enterprises.8164.1.21.1.1.75

Description

The number of disconnected PPP sessions due to failure detecting call type for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscLongDuraTimeout

Object ID

enterprises.8164.1.21.1.1.76

Description

The number of disconnected PPP sessions due to long duration time out for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatDiscAuthFail

Object ID

enterprises.8164.1.21.1.1.77

Description

The number of disconnected PPP sessions due to failed authentication for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLCPEchoTotalReq

Object ID

enterprises.8164.1.21.1.1.78

Description

The total number of PPP LCP echo requests for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLCPEchoReqResent

Object ID

enterprises.8164.1.21.1.1.79

Description

The total number of PPP LCP echo requests resent for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLCPEchoRepRecved

Object ID

enterprises.8164.1.21.1.1.80

Description

The total number of PPP LCP echo replies received for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatLCPEchoReqTimeout

Object ID

enterprises.8164.1.21.1.1.81

Description

The total number of PPP LCP echo requests time out for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRecvErrBadCtrlField

Object ID

enterprises.8164.1.21.1.1.82

Description

The total number of received PPP error due to bad control fields for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRecvErrBadPacketLen

Object ID

enterprises.8164.1.21.1.1.83

Description

The total number of received PPP error due to bad packet length for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatRemoteTerm

Object ID

enterprises.8164.1.21.1.1.84

Description

The total number of PPP remote terminations for the associated VPN service.

Syntax

Counter32

Access

Read-only
Object

starPPPStatMiscFail

Object ID

enterprises.8164.1.21.1.1.85

Description

The number of miscellaneous PPP failures for the associated VPN service.

Syntax

Counter32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentMIPHA(22)
Object

starMIPHAStatTable

Object ID

enterprises.8164.1.22.1

Description

A table containing MIP home agent statistics.

Syntax

Sequence of starMIPHAStatEntry

Access

Not-accessible
Object

starMIPHAStatEntry

Object ID

enterprises.8164.1.22.1.1

Description

The Mobile IP home agent statistics for a specific VPN (context) and service.

Syntax

starMIPHAStatEntry

Access

Not-accessible

Sequence

starMIPHAStatVpnID

starMIPHAStatSvcID Index (Implied)

starMIPHAStatVpnName

starMIPHAStatServName

starMIPHADisconnects

starMIPHAExpiry

starMIPHADereg

starMIPHAAdminDrop

starMIPHARegRecvTotal

starMIPHARegRecvInitial

starMIPHARegRecvRenew

starMIPHARegRecvDereg

starMIPHARegAcceptTotal

starMIPHARegAcceptReg,

starMIPHARegAcceptRenew

starMIPHARegAcceptDereg

starMIPHARegDeniedTotal

starMIPHARegDeniedInitial

starMIPHARegDeniedRenew

starMIPHARegDeniedDereg

starMIPHARegReplyTotal

starMIPHARegReplyAcceptReg

starMIPHARegReplyAcceptDereg

starMIPHARegReplyDenied

starMIPHARegReplyBadReq

starMIPHARegReplyMismatchID

starMIPHARegReplyAdminProhib

starMIPHARegReplyUnspecErr,

starMIPHARegReplyNoResource

starMIPHARegReplyMnAuthFail

starMIPHARegReplyFAAuthFail

starMIPHARegReplySimulBind

starMIPHARegReplyUnknownHA

starMIPHARegReplyRevTunUnavail

starMIPHARegReplyRevTunMand

starMIPHARegReplyEncapUnavail

starMIPHARegReplySendError

starMIPHAStatFARevocations

starMIPHAStatRegAcceptHO

starMIPHAStatRegDeniedHO

starMIPHAStatRegDiscardTotal
Object

starMIPHAStatVpnID

Object ID

enterprises.8164.1.22.1.1.1

Description

The internal identification of the home agent Mobile IP VPN (context).

Syntax

Gauge32

Access

Read-only
Object

starMIPHAStatSvcID

Object ID

enterprises.8164.1.22.1.1.2

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

Syntax

StarShortID

Access

Not-accessible
Object

starMIPHAStatVpnName

Object ID

enterprises.8164.1.22.1.1.3

Description

The name of the VPN (context).

Syntax

DisplayString

Access

Read-only
Object

starMIPHAStatServName

Object ID

enterprises.8164.1.22.1.1.4

Description

The Mobile IP home agent service name.

Syntax

DisplayString

Access

Read-only
Object

starMIPHAStatDisconnects

Object ID

enterprises.8164.1.22.1.1.5

Description

The number of session disconnects for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatExpiry

Object ID

enterprises.8164.1.22.1.1.6

Description

The number of session expirations for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatDereg

Object ID

enterprises.8164.1.22.1.1.7

Description

The number of session deregistrations for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatAdminDrop

Object ID

enterprises.8164.1.22.1.1.8

Description

The number of session disconnects due to administrator actions for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegRecvTotal

Object ID

enterprises.8164.1.22.1.1.9

Description

The number of session registrations received for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegRecvInitial

Object ID

enterprises.8164.1.22.1.1.10

Description

The number of initial session registrations received for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegRecvRenew

Object ID

enterprises.8164.1.22.1.1.11

Description

The number of session registration renewals received for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegRecvDereg

Object ID

enterprises.8164.1.22.1.1.12

Description

The number of session deregistrations received for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegAcceptTotal

Object ID

enterprises.8164.1.22.1.1.13

Description

The number of session registrations accepted for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegAcceptReg

Object ID

enterprises.8164.1.22.1.1.14

Description

The number of session registrations accepted for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegAcceptRenew

Object ID

enterprises.8164.1.22.1.1.15

Description

The number of session registration renewals accepted for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegAcceptDereg

Object ID

enterprises.8164.1.22.1.1.16

Description

The number of session deregistrations accepted for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegDeniedTotal

Object ID

enterprises.8164.1.22.1.1.17

Description

The number of session registrations denied for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegDeniedInitial

Object ID

enterprises.8164.1.22.1.1.18

Description

The number of session initial registrations denied for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegDeniedRenew

Object ID

enterprises.8164.1.22.1.1.19

Description

The number of session registration renewals denied for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegDeniedDereg

Object ID

enterprises.8164.1.22.1.1.20

Description

The number of session deregistrations denied for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyTotal

Object ID

enterprises.8164.1.22.1.1.21

Description

The total number of session registration replies for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyAcceptReg

Object ID

enterprises.8164.1.22.1.1.22

Description

The number of session registration replies accepted indicating registration for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyAcceptDereg

Object ID

enterprises.8164.1.22.1.1.23

Description

The number of session registration replies accepted indicating deregistration for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyDenied

Object ID

enterprises.8164.1.22.1.1.24

Description

The number of session registration replies which were denied for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyBadReq

Object ID

enterprises.8164.1.22.1.1.25

Description

The number of session registration replies indicating a bad request for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyMismatchID

Object ID

enterprises.8164.1.22.1.1.26

Description

The number of session registration replies indicating an ID mismatch for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyAdminProhib

Object ID

enterprises.8164.1.22.1.1.27

Description

The number of session registration replies indicating administrator prohibition for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyUnspecErr

Object ID

enterprises.8164.1.22.1.1.28

Description

The number of session registration replies with an unspecified error for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyNoResource

Object ID

enterprises.8164.1.22.1.1.29

Description

The number of session registration replies indicating no resources for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyMnAuthFail

Object ID

enterprises.8164.1.22.1.1.30

Description

The number of session registration replies indicating mobile number authentication failure for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyFAAuthFail

Object ID

enterprises.8164.1.22.1.1.31

Description

The number of session registration replies indicating a foreign agent authentication failure for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplySimulBind

Object ID

enterprises.8164.1.22.1.1.32

Description

The number of session registration replies indicating a simultaneous bind condition for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyUnknownHA

Object ID

enterprises.8164.1.22.1.1.33

Description

The number of session registration replies indicating unknown home agent for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyRevTunUnavail

Object ID

enterprises.8164.1.22.1.1.34

Description

The number of session registration replies indicating no reverse tunnel available for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyRevTunMand

Object ID

enterprises.8164.1.22.1.1.35

Description

The number of session registration replies indicating reverse tunneling is mandatory for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplyEncapUnavail

Object ID

enterprises.8164.1.22.1.1.36

Description

The number of session registration replies indicating IP encapsulation was not available for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegReplySendError

Object ID

enterprises.8164.1.22.1.1.37

Description

The number of session registration replies indicating a send error occurred for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatFARevocations

Object ID

enterprises.8164.1.22.1.1.38

Description

The number of FA revocations for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegAcceptHO

Object ID

enterprises.8164.1.22.1.1.39

Description

The number of hand over session registrations accepted for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegDeniedHO

Object ID

enterprises.8164.1.22.1.1.40

Description

The number of hand over session registrations denied for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPHAStatRegDiscardTotal

Object ID

enterprises.8164.1.22.1.1.41

Description

The number of session registrations discarded for the associated Mobile IP home agent VPN service.

Syntax

Counter32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentMIPFA(23)
Object

starMIPFAStatTable

Object ID

enterprises.8164.1.23.1

Description

A table containing the Mobile IP Foreign Agent statistics.

Syntax

Sequence of starMIPFAStatEntry

Access

Not-accessible

Description

A table containing MIP FA statistics
Object

starMIPFAStatEntry

Object ID

enterprises.8164.1.23.1.1.

Description

The statistics for a specific foreign agent Mobile IP VPN (context) service.

Syntax

starMIPFAStatEntry

Access

Not-accessible

Sequence

starMIPFAStatVpnID

starMIPFAStatSvcID Index (Implied)

starMIPFAStatVpnName

starMIPFAStatServName

starMIPFAAdvertSend

starMIPFADiscExpiry

starMIPFADiscDereg

starMIPFADiscAdmin

starMIPFAAuthAttempt

starMIPFAAuthSuccess

starMIPFAAuthFailure

starMIPFARegRecvTotal

starMIPFARegRecvInitial

starMIPFARegRecvRenewal

starMIPFARegRecvDereg

starMIPFARegAcceptTotal

starMIPFARegAcceptInitial

starMIPFARegAcceptRenewal

starMIPFARegAcceptDereg

starMIPFARegDenTotal

starMIPFARegDenInitial

starMIPFARegDenRenewal

starMIPFARegDenDereg

starMIPFARegDiscardTotal

starMIPFARegDiscardInitial

starMIPFARegDiscardRenewal

starMIPFARegDiscardDereg

starMIPFARegRelayedTotal

starMIPFARegRelayedInitial

starMIPFARegRelayedRenewal

starMIPFARegRelayedDereg

starMIPFARegAuthFailTotal

starMIPFARegAuthFailInitial

starMIPFARegAuthFailRenewal

starMIPFARegAuthFailDereg

starMIPFARegDenPDSNTotal

starMIPFARegDenPDSNInitial

starMIPFARegDenPDSNRenewal

starMIPFARegDenPDSNDereg

starMIPFARegDenHATotal

starMIPFARegDenHAInitial

starMIPFARegDenHARenewal

starMIPFARegDenHADereg

starMIPFARegDenPDSNUnspec

starMIPFARegDenPDSNTimeout

starMIPFARegDenPDSNAdmin

starMIPFARegDenPDSNResources

starMIPFARegDenPDSNMnAuth

starMIPFARegDenPDSNHAAuth

starMIPFARegDenPDSNTooLong

starMIPFARegDenPDSNBadReq

starMIPFARegDenPDSNEncapUnav

starMIPFARegDenPDSNRevTunUnav

starMIPFARegDenPDSNRevTunMand

starMIPFARegDenHAFAAuth

starMIPFARegDenHABadReq

starMIPFARegDenHAMismatchID

starMIPFARegDenHASimulBind

starMIPFARegDenHAUnknownHA

starMIPFARegDenHARevRunUnavail

starMIPFARegRplRcvTotal

starMIPFARegRplRcvTotalRly

starMIPFARegRplRcvErrors

starMIPFARegRplRcvInitial

starMIPFARegRplRcvInitialRly

starMIPFARegRplRcvRenewal

starMIPFARegRplRcvRenewalRly

starMIPFARegRplRcvDereg

starMIPFARegRplRcvDeregRly

starMIPFARegRplSentTotal

starMIPFARegRplSentAcceptReg

starMIPFARegRplSentAcceptDereg

starMIPFARegRplSentBadReq

starMIPFARegRplSentTooLong

starMIPFARegRplSentMnAuthFail

starMIPFARegRplSentHAAuthFail

starMIPFARegRplSentAdminProhib

starMIPFARegRplSentNoResources

starMIPFARegRplSentRevTunUnavail

starMIPFARegRplSentRevTunMand

starMIPFARegRplSentSendErrors

starMIPFAStatRegDenPDSNBadReply

starMIPFAStatRegDenPDSNMissNAI

starMIPFAStatRegDenPDSNMissHomeAgent

starMIPFAStatRegDenPDSNMissHomeAddr

starMIPFAStatRegDenPDSNUnknChallenge

starMIPFAStatRegDenPDSNMissChallenge

starMIPFAStatRegDenPDSNStaleChallenge

starMIPFAStatRegDenPDSNMNTooDistant

starMIPFAStatRegDenPDSNStyleUnavail

starMIPFAStatRegDenPDSNHANetUnreach

starMIPFAStatRegDenPDSNHAHostUnreach

starMIPFAStatRegDenPDSNHAPortUnreach

starMIPFAStatRegDenPDSNHAUnreach

starMIPFAStatRegDenPDSNInvCOA

starMIPFAStatRegReqSentInitTotal

starMIPFAStatRegReqSentInitResend

starMIPFAStatRegReqSentRenewTotal

starMIPFAStatRegReqSentRenewResend

starMIPFAStatRegReqSentDeregTotal

starMIPFAStatRegReqSentDeregResend

starMIPFAStatRegRplSentMNTooDistant

starMIPFAStatRegRplSentInvCOA

starMIPFAStatRegRplSentHANetUnreach

starMIPFAStatRegRplSentHAHostUnreach

starMIPFAStatRegRplSentHAPortUnreach

starMIPFAStatRegRplSentHAUnreach

starMIPFAStatRegRplSentRegTimeout

starMIPFAStatRegRplSentMissNAI

starMIPFAStatRegRplSentMissHomeAgent

starMIPFAStatRegRplSentMissHomeAddr

starMIPFAStatRegRplSentUnknChallenge

starMIPFAStatRegRplSentMissChallenge

starMIPFAStatRegRplSentStaleChallenge

starMIPFAStatRegRplSentBadReply
Object

starMIPFAStatVpnID

Object ID

enterprises.8164.1.23.1.1.1

Description

Internal identification of the foreign agent Mobile IP VPN (context).

Syntax

Gauge32

Access

Read-only
Object

starMIPFAStatSvcID

Object ID

enterprises.8164.1.23.1.1.2

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

Syntax

StarShortID

Access

Not-accessible
Object

starMIPFAStatVpnName

Object ID

enterprises.8164.1.23.1.1.3

Description

The foreign agent mobile IP VPN (context) name.

Syntax

DisplayString

Access

Read-only
Object

starMIPFAStatServName

Object ID

enterprises.8164.1.23.1.1.4

Description

The Mobile IP foreign agent service name.

Syntax

DisplayString

Access

Read-only
Object

starMIPFAStatAdvertSend

Object ID

enterprises.8164.1.23.1.1.5

Description

The number of advertisements sent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatDiscExpiry

Object ID

enterprises.8164.1.23.1.1.6

Description

The number of session disconnects due to expiration for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatDiscDereg

Object ID

enterprises.8164.1.23.1.1.7

Description

The number of session disconnects due to deregistration requests for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatDiscAdmin

Object ID

enterprises.8164.1.23.1.1.8

Description

The number of session disconnects due to administrator action for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatAuthAttempt

Object ID

enterprises.8164.1.23.1.1.9

Description

The number of session authentication attempts for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatAuthSuccess

Object ID

enterprises.8164.1.23.1.1.10

Description

The number of session authentication successes for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatAuthFailure

Object ID

enterprises.8164.1.23.1.1.11

Description

The number of session authentication failures for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRecvTotal

Object ID

enterprises.8164.1.23.1.1.12

Description

The total number of session registrations received for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRecvInitial

Object ID

enterprises.8164.1.23.1.1.13

Description

The number of initial session registrations received for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRecvRenewal

Object ID

enterprises.8164.1.23.1.1.14

Description

The number of session registration renewals for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRecvDereg

Object ID

enterprises.8164.1.23.1.1.15

Description

The number of session deregistrations for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAcceptTotal

Object ID

enterprises.8164.1.23.1.1.16

Description

The total number of session registrations accepted for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAcceptInitial

Object ID

enterprises.8164.1.23.1.1.17

Description

The number of initial session registrations accepted for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAcceptRenewal

Object ID

enterprises.8164.1.23.1.1.18

Description

The number of session registration renewals accepted for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAcceptDereg

Object ID

enterprises.8164.1.23.1.1.19

Description

The number of session deregistrations accepted for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenTotal

Object ID

enterprises.8164.1.23.1.1.20

Description

The total number of session registrations denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenInitial

Object ID

enterprises.8164.1.23.1.1.21

Description

The number of initial session registrations denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenRenewal

Object ID

enterprises.8164.1.23.1.1.22

Description

The number of session registration renewals denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenDereg

Object ID

enterprises.8164.1.23.1.1.23

Description

The number of session deregistrations denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDiscardTotal

Object ID

enterprises.8164.1.23.1.1.24

Description

The total number of session registrations discarded for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDiscardInitial

Object ID

enterprises.8164.1.23.1.1.25

Description

The number of initial session registrations discarded for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDiscardRenewal

Object ID

enterprises.8164.1.23.1.1.26

Description

The number of session registration renewals discarded for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDiscardDereg

Object ID

enterprises.8164.1.23.1.1.27

Description

The number of session deregistrations discarded for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRelayedTotal

Object ID

enterprises.8164.1.23.1.1.28

Description

The total number of session registrations relayed for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRelayedInitial

Object ID

enterprises.8164.1.23.1.1.29

Description

The number of initial session registrations relayed for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRelayedRenewal

Object ID

enterprises.8164.1.23.1.1.30

Description

The number of session registration renewals relayed for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRelayedDereg

Object ID

enterprises.8164.1.23.1.1.31

Description

The number of session deregistrations relayed for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAuthFailTotal

Object ID

enterprises.8164.1.23.1.1.32

Description

The total number of session registration authentication failures for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAuthFailInitial

Object ID

enterprises.8164.1.23.1.1.33

Description

The number of initial session registration failures for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAuthFailRenewal

Object ID

enterprises.8164.1.23.1.1.34

Description

The number of session registration renewal failures for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegAuthFailDereg

Object ID

enterprises.8164.1.23.1.1.35

Description

The number of session deregistration authentication failures for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNTotal

Object ID

enterprises.8164.1.23.1.1.36

Description

The total number of PDSN session registrations denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNInitial

Object ID

enterprises.8164.1.23.1.1.37

Description

The number of initial PDSN session registrations denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNRenewal

Object ID

enterprises.8164.1.23.1.1.38

Description

The number of PDSN session registration renewals denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNDereg

Object ID

enterprises.8164.1.23.1.1.39

Description

The number of PDSN session deregistrations denied for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHATotal

Object ID

enterprises.8164.1.23.1.1.40

Description

The total number of session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHAInitial

Object ID

enterprises.8164.1.23.1.1.41

Description

The number of initial session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHARenewal

Object ID

enterprises.8164.1.23.1.1.42

Description

The number of session registration renewals denied by the home agent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHADereg

Object ID

enterprises.8164.1.23.1.1.43

Description

The number of session deregistrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNUnspec

Object ID

enterprises.8164.1.23.1.1.44

Description

The number of PDSN session registrations denied for an unspecified reason for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNTimeout

Object ID

enterprises.8164.1.23.1.1.45

Description

The number of PDSN session registrations denied due to timer expiration for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNAdmin

Object ID

enterprises.8164.1.23.1.1.46

Description

The number of PDSN session registration denied due administrator prohibition for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNResources

Object ID

enterprises.8164.1.23.1.1.47

Description

The number of PDSN session registrations denied due to no resources for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNMnAuth

Object ID

enterprises.8164.1.23.1.1.48

Description

The number of PDSN session registrations denied due to mobile number authentication failure for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNHAAuth

Object ID

enterprises.8164.1.23.1.1.49

Description

The number of PDSN session registrations denied by the home agent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNTooLong

Object ID

enterprises.8164.1.23.1.1.50

Description

The number of PDSN session registrations denied due to a life too lone indication for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNBadReq

Object ID

enterprises.8164.1.23.1.1.51

Description

The number of PDSN session registration denied due to a bad request indication for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNEncapUnav

Object ID

enterprises.8164.1.23.1.1.52

Description

The number of PDSN session registration denied due to no IP encapsulation available for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDeniedPDSNRevTunUnav

Object ID

enterprises.8164.1.23.1.1.53

Description

The number of PDSN session registrations denied due to no reverse tunnel available for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNRevTunMand

Object ID

enterprises.8164.1.23.1.1.54

Description

The number of PDSN session registration denied due to reverse tunneling being mandatory for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHAFAAuth

Object ID

enterprises.8164.1.23.1.1.55

Description

The number of session registrations denied by the home agent due to authentication failure for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHABadReq

Object ID

enterprises.8164.1.23.1.1.56

Description

The number of session registration denied by the home agent due to the request being invalid for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHAMismatchID

Object ID

enterprises.8164.1.23.1.1.57

Description

The number of session registrations denied by the home agent due to an ID mismatch for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHASimulBind

Object ID

enterprises.8164.1.23.1.1.58

Description

The number of session registrations denied by the home agent due to a simultaneous bind attempt for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHAUnknownHA

Object ID

enterprises.8164.1.23.1.1.59

Description

The number of session registrations denied by the home agent for an unknown reason for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenHARevRunUnavail

Object ID

enterprises.8164.1.23.1.1.60

Description

The number of session registrations denied by the home agent due to no reverse tunnel being available for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvTotal

Object ID

enterprises.8164.1.23.1.1.61

Description

The total number of session registration replies received for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvTotalRly

Object ID

enterprises.8164.1.23.1.1.62

Description

The total number of session registration replies relayed for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvErrors

Object ID

enterprises.8164.1.23.1.1.63

Description

The number of session registration replies received indicating errors for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvInitial

Object ID

enterprises.8164.1.23.1.1.64

Description

The number of initial session registration replies received for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvInitialRly

Object ID

enterprises.8164.1.23.1.1.65

Description

The number of initial session registration replies relayed for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvRenewal

Object ID

enterprises.8164.1.23.1.1.66

Description

The number of session registration renewal replies received for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvRenewalRly

Object ID

enterprises.8164.1.23.1.1.67

Description

The number of session registration replies relayed received for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvDereg

Object ID

enterprises.8164.1.23.1.1.68

Description

The number of session registration replies received indicating deregistration for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplRcvDeregRly

Object ID

enterprises.8164.1.23.1.1.69

Description

The number of session registration replies relayed indicating deregistration for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentTotal

Object ID

enterprises.8164.1.23.1.1.70

Description

The total number of session registration replies sent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentAcceptReg

Object ID

enterprises.8164.1.23.1.1.71

Description

The number of session registration replies which were sent and accepted for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentAcceptDereg

Object ID

enterprises.8164.1.23.1.1.72

Description

The number of session registration replies which were sent and accepted indicating deregistration for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentBadReq

Object ID

enterprises.8164.1.23.1.1.73

Description

The number of session registration replies which were sent indicating the request was invalid for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentTooLong

Object ID

enterprises.8164.1.23.1.1.74

Description

The number of session registration replies which were sent indicating life too long for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentMnAuthFail

Object ID

enterprises.8164.1.23.1.1.75

Description

The number of session registration replies which were sent indicating mobile number authentication failure for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentHAAuthFail

Object ID

enterprises.8164.1.23.1.1.76

Description

The number of session registration replies which were sent indicating for home agent authentication failure the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentAdminProhib

Object ID

enterprises.8164.1.23.1.1.77

Description

The number of session registration replies which were sent indicating prohibited by the administrator for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentNoResources

Object ID

enterprises.8164.1.23.1.1.78

Description

The number of session registration replies which were sent indicating no resources available for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentRevTunUnavail

Object ID

enterprises.8164.1.23.1.1.79

Description

The number of session registration replies which were sent indicating no reverse tunnel available for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentRevTunMand

Object ID

enterprises.8164.1.23.1.1.80

Description

The number of session registration replies which were sent indicating reverse tunneling was mandatory for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentSendErrors

Object ID

enterprises.8164.1.23.1.1.81

Description

The number of session registration replies which were sent indicating there were errors in transmission for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNBadReply

Object ID

enterprises.8164.1.23.1.1.82

Description

The number of session registrations denied by PDSN due to bad reply from HA for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNMissNAI

Object ID

enterprises.8164.1.23.1.1.83

Description

The number of session registrations denied by PDSN due to missing NAI for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNMissHomeAgent

Object ID

enterprises.8164.1.23.1.1.84

Description

The number of session registrations denied by PDSN due to missing home agent for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNMissHomeAddr

Object ID

enterprises.8164.1.23.1.1.85

Description

The number of session registrations denied by PDSN due to missing home address for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNUnknChallenge

Object ID

enterprises.8164.1.23.1.1.86

Description

The number of session registrations denied by PDSN due to unknown challenge for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNMissChallenge

Object ID

enterprises.8164.1.23.1.1.87

Description

The number of session registrations denied by PDSN due to missing challenge for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNStaleChallenge

Object ID

enterprises.8164.1.23.1.1.88

Description

The number of session registrations denied by PDSN due to stale challenge for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNMNTooDistant

Object ID

enterprises.8164.1.23.1.1.89

Description

The number of session registrations denied by PDSN due to MN too distant for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNStyleUnavail

Object ID

enterprises.8164.1.23.1.1.90

Description

The number of session registration denied by PDSN due to style not available for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNHANetUnreach

Object ID

enterprises.8164.1.23.1.1.91

Description

The number of session registrations denied by PDSN due to HA network unreachable for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNHAHostUnreach

Object ID

enterprises.8164.1.23.1.1.92

Description

The number of session registrations denied by PDSN due to HA host unreachable for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNHAPortUnreach

Object ID

enterprises.8164.1.23.1.1.93

Description

The number of session registrations denied by PDSN due to HA port unreachable for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNHAUnreach

Object ID

enterprises.8164.1.23.1.1.94

Description

The number of session registrations denied by PDSN due to HA unreachable for miscellaneous reasons for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegDenPDSNInvCOA

Object ID

enterprises.8164.1.23.1.1.95

Description

The number of session registrations denied by PDSN due to invalid COA for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegReqSentInitTotal

Object ID

enterprises.8164.1.23.1.1.96

Description

The number of initial session registrations for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegReqSentInitResend

Object ID

enterprises.8164.1.23.1.1.97

Description

The number of initial session registrations retried for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegReqSentRenewTotal

Object ID

enterprises.8164.1.23.1.1.98

Description

The number of renewal session registrations for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegReqSentRenewResend

Object ID

enterprises.8164.1.23.1.1.99

Description

The number of renewal session registrations retried for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegReqSentDeregTotal

Object ID

enterprises.8164.1.23.1.1.100

Description

The number of session deregistrations for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegReqSentDeregResend

Object ID

enterprises.8164.1.23.1.1.101

Description

The number of session deregistrations retried for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentMNTooDistant

Object ID

enterprises.8164.1.23.1.1.102

Description

The number of session registration reply that indicate MN too distant for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentInvCOA

Object ID

enterprises.8164.1.23.1.1.103

Description

The number of session registration reply that indicate invalid COA for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentHANetUnreach

Object ID

enterprises.8164.1.23.1.1.104

Description

The number of session registration reply that indicate HA network unreachable for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentHAHostUnreach

Object ID

enterprises.8164.1.23.1.1.105

Description

The number of session registration reply that indicate HA host unreachable for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentHAPortUnreach

Object ID

enterprises.8164.1.23.1.1.106

Description

The number of session registration reply that indicate HA port unreachable for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentHAUnreach

Object ID

enterprises.8164.1.23.1.1.107

Description

The number of session registration reply that indicate HA unreachable due to miscellaneous reasons for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentRegTimeout

Object ID

enterprises.8164.1.23.1.1.108

Description

The number of session registration reply that indicate registration time out for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentMissNAI

Object ID

enterprises.8164.1.23.1.1.109

Description

The number of session registration reply that indicate NAI missing for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentMissHomeAgent

Object ID

enterprises.8164.1.23.1.1.110

Description

The number of session registration reply that indicate HA missing for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentMissHomeAddr

Object ID

enterprises.8164.1.23.1.1.111

Description

The number of session registration reply that indicate home address missing for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentUnknChallenge

Object ID

enterprises.8164.1.23.1.1.112

Description

The number of session registration reply that indicate unknown challenge for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentMissChallenge

Object ID

enterprises.8164.1.23.1.1.113

Description

The number of session registration reply that indicate challenge missing for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentStaleChallenge

Object ID

enterprises.8164.1.23.1.1.114

Description

The number of session registration reply that indicate stale challenge for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
Object

starMIPFAStatRegRplSentBadReply

Object ID

enterprises.8164.1.23.1.1.115

Description

The number of session registration reply that indicate bad reply for the associated Mobile IP foreign agent VPN service.

Syntax

Counter32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentRP(24)
Object

starRPStatTable

Object ID

enterprises.8164.1.24.1

Description

A table containing the R-P interface statistics.

Syntax

Sequence of starMIPFAStatEntry

Access

Not-accessible

Description

A table containing MIP FA statistics
Object

starRPStatEntry

Object ID

enterprises.8164.1.24.1.1

Description

The statistics for a specific R-P VPN (context) service.

Syntax

starRPStatEntry

Access

Not-accessible

Sequence

starRPStatVpnID

starRPStatSvcID Index (Implied)

starRPStatVpnName

starRPStatServName

starRPRegRecvTotal

starRPRegAcceptTotal

starRPRegDeniedTotal

starRPRegDiscardTotal

starRPRegAcceptInitial

starRPRegAcceptIntraPDSN

starRPRegAcceptInterPDSN

starRPRegDeniedInitial

starRPRegAcceptRenew

starRPRegDeniedRenew

starRPRegAcceptDereg

starRPRegDeniedDereg

starRPRegSendError

starRPRegHashError

starRPRegDecodeError

starRPRegUnhandled

starRPRegAirlinkSeqError

starRPRegDenyUnspec

starRPRegDenyAdminProhib

starRPRegDenyNoResource

starRPRegDenyAuth

starRPRegDenyMismatchID

starRPRegDenyBadRequest

starRPRegDenyUnknownPDSN

starRPRegDenyRevTunUnav

starRPRegDenyRevTunReq

starRPRegDenyUnrecogVend

starRPRegUpdTotal

starRPRegUpdAccept

starRPRegUpdDenied

starRPRegUpdUnack

starRPRegUpdTrans

starRPRegUpdRetrans

starRPRegUpdReceived

starRPRegUpdDiscard

starRPRegUpdSendError

starRPRegUpdUplyrInit

starRPRegUpdOther

starRPRegUpdHandoff

starRPRegUpdDenyUnspec

starRPRegUpdDenyAdminProhib

starRPRegUpdDenyAuth

starRPRegUpdDenyMismatchID

starRPRegUpdDenyBadRequest

starRPSecViolations

starRPSecBadAuth

starRPSecBadID

starRPSecBadSpi

starRPSecMissingMnHAAuth

starRPSecMissingRegUpdate

starRPRegRecvInitial

starRPRegAcceptActvStartIntraPDSN

starRPRegAcceptActvStopIntraPDSN

starRPRegRecvRenew

starRPRegActvStartRenew

starRPRegActvStopRenew

starRPRegRecvDereg

starRPRegAcceptActvStopDereg

starRPDiscSessAbsent

starRPDiscNoMemory

starRPDiscMalformed

starRPDiscAuthFail

starRPDiscInternalBounce

starRPDiscInpuQueueExceeded

starRPDiscMismatchedId

starRPDiscInvPacketLen

starRPDiscMisc
Object

starRPStatVpnID

Object ID

enterprises.8164.1.24.1.1.1

Description

The internal identification of the R-P VPN (context).

Syntax

Gauge32

Access

Read-only
Object

starRPStatSvcID

Object ID

enterprises.8164.1.24.1.1.2

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

Syntax

StarShortID

Access

Not-accessible
Object

starRPStatVpnName

Object ID

enterprises.8164.1.24.1.1.3

Description

The R-P VPN (context) name.

Syntax

DisplayString

Access

Read-only
Object

starRPStatServName

Object ID

enterprises.8164.1.24.1.1.4

Description

The R-P service name.

Syntax

DisplayString

Access

Read-only
Object

starRPRegRecvTotal

Object ID

enterprises.8164.1.24.1.1.5

Description

The total number of session registrations received for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptTotal

Object ID

enterprises.8164.1.24.1.1.6

Description

The total number of session registrations accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDeniedTotal

Object ID

enterprises.8164.1.24.1.1.7

Description

The total number of session registrations denied for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDiscardTotal

Object ID

enterprises.8164.1.24.1.1.8

Description

The total number of session registrations discarded for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptInitial

Object ID

enterprises.8164.1.24.1.1.9

Description

The total number of initial session registrations accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptIntraPDSN

IMPORTANT:

Status of this alarm is obsolete.

Object ID

enterprises.8164.1.24.1.1.10

Description

The number of Intra-PDSN session registrations accepted for the associated R-P VPN service.

Syntax

Gauge32

Access

Read-only
Object

starRPRegAcceptInterPDSN

Object ID

enterprises.8164.1.24.1.1.11

Description

The number of Inter-PDSN session registrations accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDeniedInitial

Object ID

enterprises.8164.1.24.1.1.12

Description

The number of initial session registrations denied for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptRenew

Object ID

enterprises.8164.1.24.1.1.13

Description

The number of session registration renewals accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDeniedRenew

Object ID

enterprises.8164.1.24.1.1.14

Description

The number of session registration renewals denied for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptDereg

Object ID

enterprises.8164.1.24.1.1.15

Description

The number of session deregistrations accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDeniedDereg

Object ID

enterprises.8164.1.24.1.1.16

Description

The number of session deregistrations denied accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegSendError

Object ID

enterprises.8164.1.24.1.1.17

Description

The number of session registrations with errors in transmission for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegHashError

Object ID

enterprises.8164.1.24.1.1.18

Description

The number of session registrations with hash errors for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDecodeError

Object ID

enterprises.8164.1.24.1.1.19

Description

The number of session registrations with decode errors for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUnhandled

Object ID

enterprises.8164.1.24.1.1.20

Description

The number of session registrations not processed for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAirlinkSeqError

Object ID

enterprises.8164.1.24.1.1.21

Description

The number of session registrations with air link sequence errors for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyUnspec

Object ID

enterprises.8164.1.24.1.1.22

Description

The number of session registrations denied for an unspecified reason for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyAdminProhib

Object ID

enterprises.8164.1.24.1.1.23

Description

The number of session registrations denied due to administrator prohibition for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyNoResource

Object ID

enterprises.8164.1.24.1.1.24

Description

The number of session registrations denied due to no resources available for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyAuth

Object ID

enterprises.8164.1.24.1.1.25

Description

The number of session registrations denied due to authentication failure for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyMismatchID

Object ID

enterprises.8164.1.24.1.1.26

Description

The number of session registrations denied due to an ID mismatch for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyBadRequest

Object ID

enterprises.8164.1.24.1.1.27

Description

The number of session registrations denied due to the request being invalid for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyUnknownPDSN

Object ID

enterprises.8164.1.24.1.1.28

Description

The number of session registrations denied due to the packet data service not being recognized for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyRevTunUnav

Object ID

enterprises.8164.1.24.1.1.29

Description

The number of session registrations denied due to no reverse tunnel being available for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyRevTunReq

Object ID

enterprises.8164.1.24.1.1.30

Description

The number of session registrations denied due to reverse tunneling being mandatory for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegDenyUnrecogVend

Object ID

enterprises.8164.1.24.1.1.31

Description

The number of session registrations denied due to the vendor not being recognized for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdTotal

Object ID

enterprises.8164.1.24.1.1.32

Description

The total number of session registration updates for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdAccept

Object ID

enterprises.8164.1.24.1.1.33

Description

The number of session registration updates which were accepted for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDenied

Object ID

enterprises.8164.1.24.1.1.34

Description

The number of session registration updates denied for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdUnack

Object ID

enterprises.8164.1.24.1.1.35

Description

The number of session registration updates which were not acknowledged for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdTrans

Object ID

enterprises.8164.1.24.1.1.36

Description

The number of session registration updates sent for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdRetrans

Object ID

enterprises.8164.1.24.1.1.37

Description

The number of session registration updates resent for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdReceived

Object ID

enterprises.8164.1.24.1.1.38

Description

The number of session registration updates received for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDiscard

Object ID

enterprises.8164.1.24.1.1.39

Description

The number of session registration updates discarded for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdSendError

Object ID

enterprises.8164.1.24.1.1.40

Description

The number of session registration updates with errors in transmission for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdUplyrInit

Object ID

enterprises.8164.1.24.1.1.41

Description

The number of session registration updates with up-link re-initializations.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdOther

Object ID

enterprises.8164.1.24.1.1.42

Description

The number of session registration updates with a reason of ‘other’ for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdHandoff

Object ID

enterprises.8164.1.24.1.1.43

Description

The number of session registration updates due to a mobile hand-off for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDenyUnspec

Object ID

enterprises.8164.1.24.1.1.44

Description

The number of session registration updates denied for an unspecified reason for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDenyAdminProhib

Object ID

enterprises.8164.1.24.1.1.45

Description

The number of session registration updates denied due to administrator prohibition for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDenyAuth

Object ID

enterprises.8164.1.24.1.1.46

Description

The number of session registration updates denied due to authentication failure for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDenyMismatchID

Object ID

enterprises.8164.1.24.1.1.47

Description

The number of session registration updates denied due to an ID mismatch for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegUpdDenyBadRequest

Object ID

enterprises.8164.1.24.1.1.48

Description

The number of session registration updates denied due to the request being invalid for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPSecViolations

Object ID

enterprises.8164.1.24.1.1.49

Description

The total number of session security violations for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPSecBadAuth

Object ID

enterprises.8164.1.24.1.1.50

Description

The total number of session security authentication violations for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPSecBadID

Object ID

enterprises.8164.1.24.1.1.51

Description

The total number of session security ID violations for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPSecBadSpi

Object ID

enterprises.8164.1.24.1.1.52

Description

The total number of session security SPI violations for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPSecMissingMnHAAuth

Object ID

enterprises.8164.1.24.1.1.53

Description

The total number of session security missing mobile number home agent authentication violations for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPSecMissingRegUpdate

Object ID

enterprises.8164.1.24.1.1.54

Description

The total number of session missing registration update violations for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegRecvInitial

Object ID

enterprises.8164.1.24.1.1.55

Description

The total number of initial session registration for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptActvStartIntraPDSN

Object ID

enterprises.8164.1.24.1.1.56

Description

The number of accepted registration request during intra-PDSN handoffs which contains active start for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptActvStopIntraPDSN

Object ID

enterprises.8164.1.24.1.1.57

Description

The number of accepted registration request during intraPDSN handoff which contains active stop for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegRecvRenew

Object ID

enterprises.8164.1.24.1.1.58

Description

The number of received renew registration request for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegActvStartRenew

Object ID

enterprises.8164.1.24.1.1.59

Description

The number of received renew registration request that contains active start for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegActvStopRenew

Object ID

enterprises.8164.1.24.1.1.60

Description

The number of received renew registration request that contains active stop for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegRecvDereg

Object ID

enterprises.8164.1.24.1.1.61

Description

The number of received deregistration request for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPRegAcceptActvStopDereg

Object ID

enterprises.8164.1.24.1.1.62

Description

The number of accepted deregistration request that contains active stop for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscSessAbsent

Object ID

enterprises.8164.1.24.1.1.63

Description

The number of registration request discarded due to no session for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscNoMemory

Object ID

enterprises.8164.1.24.1.1.64

Description

The number of registration request discarded due to no memory for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscMalformed

Object ID

enterprises.8164.1.24.1.1.65

Description

The number of registration request discarded because malformed for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscAuthFail

Object ID

enterprises.8164.1.24.1.1.66

Description

The number of registration request discarded because authentication failed for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscInternalBounce

Object ID

enterprises.8164.1.24.1.1.67

Description

The number of registration request discarded because internal bounce for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscInpuQueueExceeded

Object ID

enterprises.8164.1.24.1.1.68

Description

The number of registration request discarded because internal queue exceeded for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscMismatchedId

Object ID

enterprises.8164.1.24.1.1.69

Description

The number of registration request discarded because mismatched ID for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscInvPacketLen

Object ID

enterprises.8164.1.24.1.1.70

Description

The number of registration request discarded because invalid packet length for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRPDiscMisc

Object ID

enterprises.8164.1.24.1.1.71

Description

The number of registration request discarded due to misc. reasons for the associated R-P VPN service.

Syntax

Counter32

Access

Read-only
Object

starRP1xTxBytes

Object ID

enterprises.8164.1.24.1.1.72

Description

The number of 1x bytes transmitted, in megabytes.

Syntax

Counter32

Access

Read-only
Object

starRPDiscMisc

Object ID

enterprises.8164.1.24.1.1.73

Description

The number of 1x bytes received, in megabytes.

Syntax

Counter32

Access

Read-only
Object

starRP1xTxPackets

Object ID

enterprises.8164.1.24.1.1.74

Description

The number of 1x packets transmitted, in thousands.

Syntax

Counter32

Access

Read-only
Object

starRP1xRxPackets

Object ID

enterprises.8164.1.24.1.1.75

Description

The number of 1x packets received, in thousands.

Syntax

Counter32

Access

Read-only
Object

starRPDoTxBytes

Object ID

enterprises.8164.1.24.1.1.76

Description

The number of Do bytes transmitted, in megabytes.

Syntax

Counter32

Access

Read-only
Object

starRPDoRxBytes

Object ID

enterprises.8164.1.24.1.1.77

Description

The number of Do bytes received, in megabytes.

Syntax

Counter32

Access

Read-only
Object

starRPDoTxPackets

Object ID

enterprises.8164.1.24.1.1.78

Description

The number of Do packets transmitted, in thousands.

Syntax

Counter32

Access

Read-only
Object

starRPDoRxPackets

Object ID

enterprises.8164.1.24.1.1.79

Description

The number of Do packets received, in thousands.

Syntax

Counter32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentSubscriber(26)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starSubTable

Object ID

enterprises.8164.1.26.1

Description

A table containing subscriber information.

Syntax

SEQUENCE OF starSubEntry

Access

Not-accessible
Object

starSubEntry

Object ID

enterprises.8164.1.26.1.1

Description

Information for a specific Subscriber.

Syntax

starSubEntry

Access

Not-accessible

Sequence

starSubContext

starSubMSID Index

starSubName Index

starSubTimerDuration

starSubLongDurTimeoutAction

starSubSetupTime

starSubHomeAddr

starSubHomeAddrv6
Object

starSubContext

Object ID

enterprises.8164.1.26.1.1.1

Description

The context the subscriber is in.

Syntax

DisplayString

Access

accessible-for-notify
Object

starSubMSID

Object ID

enterprises.8164.1.26.1.1.2

Description

The MSID of the subscriber.

Syntax

OCTET STRING (SIZE (1..16))

Access

Not-accessible
Object

starSubName

Object ID

enterprises.8164.1.26.1.1.3

Description

The name of the subscriber.

Syntax

OCTET STRING (SIZE (1..128))

Access

Not-accessible
Object

starSubTimerDuration

Object ID

enterprises.8164.1.26.1.1.4

Description

The length of the long-duration timer in seconds

Syntax

Unsigned32

Access

Read-only
Object

starSubLongDurTimeoutAction

Object ID

enterprises.8164.1.26.1.1.5

Description

he action taken by the system upon detection of a long-duration session.

Syntax

StarLongDurTimeoutAction

Access

Read-only
Object

starSubSetupTime

Object ID

enterprises.8164.1.26.1.1.6

Description

The time when the call was setup.

Syntax

DateAndTime

Access

Read-only
Object

starSubHomeAddr

Object ID

enterprises.8164.1.26.1.1.7

Description

The IPv4 home address.

Syntax

IPv4Address

Access

Read-only
Object

starSubHomeAddrv6

Object ID

enterprises.8164.1.26.1.1.8

Description

The IPv6 home address.

Syntax

IPv6Address

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentEISServer(27)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starEISServerTable

Object ID

enterprises.8164.1.27.1

Description

A table containing EIS Server information.

Syntax

SEQUENCE OF StarEISServerEntry

Access

Not-accessible
Object

starEISServerEntry

Object ID

enterprises.8164.1.27.1.1

Description

Information for a specific EIS Server.

Syntax

StarEISServerEntry

Access

Not-accessible

Sequence

starEISServerVPNID Index

starEISServerAddr Index

starEISServerVPNName
Object

starEISServerVPNID

Object ID

enterprises.8164.1.27.1.1.1

Description

The VPN ID for the EIS Server.

Syntax

Gauge32

Access

Not-accessible
Object

starEISServerAddr

Object ID

enterprises.8164.1.27.1.1.2

Description

The IP Address for the EIS Server.

Syntax

IpAddress

Access

Not-accessible
Object

starEISServerVPNName

Object ID

enterprises.8164.1.27.1.1.3

Description

The VPN Name for this EIS Server.

Syntax

DisplayString

Access

Accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starentThresholds(28)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starThreshMeasuredPct

Object ID

enterprises.8164.1.28.1

Description

The measured value of a thresholded parameter.

Syntax

INTEGER32(0..100)

Access

Accessible-for-notify
Object

starThreshPct

Object ID

enterprises.8164.1.28.2

Description

The configured value of a thresholded parameter.

Syntax

INTEGER32(0..100)

Access

Accessible-for-notify
Object

starThreshMeasuredInt

Object ID

enterprises.8164.1.28.3

Description

The measured value of a thresholded parameter.

Syntax

Guage32

Access

Accessible-for-notify
Object

starThreshInt

Object ID

enterprises.8164.1.28.4

Description

The configured value of a thresholded parameter.

Syntax

Unsigned32

Access

Accessible-for-notify
Object

starThreshMeasuredMB

Object ID

enterprises.8164.1.28.5

Description

The measured value of a thresholded parameter.

Syntax

Guard32

Units

Megabytes

Access

Accessible-for-notify
Object

starThreshMB

Object ID

enterprises.8164.1.28.6

Description

The configured value of a thresholded parameter

Syntax

Unsigned32

Units

Megabytes

Access

Accessible-for-notify
Object

starThreshMeasuredGB

Object ID

enterprises.8164.1.28.7

Description

The configured value of a thresholded parameter.

Syntax

Gauge32

Units

Gigabytes

Access

Accessible-for-notify
Object

starThreshGB

Object ID

enterprises.8164.1.28.8

Description

The configured value of a thresholded parameter.

Syntax

Unsigned32

Units

Gigabytes

Access

Accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starentPort(29)
Object

starPortTable

Object ID

enterprises.8164.1.29.1

Description

A table containing Port information.

Syntax

SEQUENCE OF starPortEntry

Access

Not-accessible
Object

starPortEntry

Object ID

enterprises.8164.1.29.1.1

Description

Information for a specific Port

Syntax

starPortEntry

Access

Not-accessible

Sequence

starPortSlot Integer32

starPortNum integer32

starPortType INTEGER

starPortTypeDescr DisplayString

starPortAdminState INTEGER

starPortOperState INTEGER

starPortOperMode INTEGER

starPortLinkState INTEGER

starRedundantPortSlot integer32

starRedundantPortNum integer32

starPortRXByte Counter32

starPortTXByte Counter32

starPortRXFrames Counter32

starPortTXFrames Counter32

starPortRxDiscards Counter32

starPortTxDiscards Counter32

starPortRxErrors Counter32

starPortTxErrors Counter32
Object

starPortSlot

Object ID

enterprises.8164.1.29.1.1.1

Description

The Slot number for this port.

Syntax

Integer32(1..48)

Access

Not-accessible
Object

starPortNum

Object ID

enterprises.8164.1.29.1.1.2

Description

The Port number within this slot.

Syntax

Integer32(1..8)

Access

Not-accessible
Object

starPortType

Object ID

enterprises.8164.1.29.1.1.3

Description

The port type.

Syntax

INTEGER {

none(0)

ethernet10100(1)

ethernet1000dualmedia(2)

ethernet1000(3)

ds3(4)

oc3(5)

oc3atm(6)

ds3e(7)

rs232(8)

bits1e1(9)

virtualEthernet(10)

}

Access

Read-only
Object

starPortTypeDescr

Object ID

enterprises.8164.1.29.1.1.4

Description

A textual representation of the starPortType attribute

Syntax

DisplayString

Access

Read-only
Object

starPortAdminState

Object ID

enterprises.8164.1.29.1.1.5

Description

The administrative start of the port

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

enabled(1)

disabled(2)
Object

starPortOperState

Object ID

enterprises.8164.1.29.1.1.6

Description

The operation status of the port

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

up(1)

down(2)

notapplicable(3)
Object

starPortOperMode

Object ID

enterprises.8164.1.29.1.1.7

Description

The operation mode of the port

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

active(1)

standby(2)
Object

starPortLinkState

Object ID

enterprises.8164.1.29.1.1.8

Description

The link status of the port

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

up(1)

down(2)
Object

starRedundantPortSlot

Object ID

enterprises.8164.1.29.1.1.9

Description

The slot number of the redundant port for the current port.

Syntax

Integer32(1..48)

Access

Read-only
Object

starRedundantPortNum

Object ID

enterprises.8164.1.29.1.1.10

Description

The port number of the redundant port for the current port

Syntax

Integer32(1..8)

Access

Read-only
Object

starPortRXBytes

Object ID

enterprises.8164.1.29.1.1.11

Description

The number of bytes successfully received, in megabytes.

For ports of type rs232(8) for bitst1e1(9) this value will always be zero.

Syntax

Counter32

Access

Read-only
Object

starPortTXBytes

Object ID

enterprises.8164.1.29.1.1.12

Description

The number of bytes successfully transmitted in megabytes. For ports of type rs232(8) for bitst1e1(9) this value will always be zero.

Syntax

Counter32

Access

Read-only
Object

starPortRXFrames

Object ID

enterprises.8164.1.29.1.1.13

Description

The number of frames successfully received, in thousands. For ports of type rs232(8) for bitst1e1(9) this value will always be zero and for ports of type oc3atm(5) and oc12atm(6) this is the count of cells received.

Syntax

Counter32

Access

Read-only
Object

starPortTXFrames

Object ID

enterprises.8164.1.29.1.1.14

Description

The number of frames successfully transmitted, in thousands. For ports of type rs232(8) for bitst1e1(9) this value will always be zero and for ports of type oc3atm(5) and oc12atm(6) this is the count of cells received..

Syntax

Counter32

Access

Read-only
Object

starPortRxDiscards

Object ID

enterprises.8164.1.29.1.1.15

Description

The number of inbound packets which were chosen to be discarded even though no errors had been detected to prevent their being deliverable to a higher-layer protocol. One possible reason for discarding such a packet could be to free up buffer space.

Syntax

Counter32

Access

read-only
Object

starPortTxDiscards

Object ID

enterprises.8164.1.29.1.1.16

Description

The number of outbound packets which were chosen to be discarded even though no errors had been detected to prevent their being transmitted. One possible reason for discarding such a packet could be to free up buffer space.

Syntax

Counter32

Access

read-only
Object

starPortRxErrors

Object ID

enterprises.8164.1.29.1.1.17

Description

The number of inbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.

Syntax

Counter32

Access

read-only
Object

starPortTxErrors

Object ID

enterprises.8164.1.29.1.1.18

Description

The number of outbound packets that could not be transmitted because of errors.

Syntax

Counter32

Access

read-only

Units

Thousands
starentMIB(8164).starentMIBObjects(1).starentIPPool(30)
Object

starIPPoolTable

Object ID

enterprises.8164.1.30.1

Description

A table containing IP Pool information.

Syntax

SEQUENCE OF StarIPPoolEntry

Access

Not-accessible
Object

starIPPoolEntry

Object ID

enterprises.8164.1.30.1.1

Description

Information for a specific IP Pool

Syntax

StarIPPoolEntry

Access

Not-accessible

Sequence

starIPPoolVpnID Gauge32

starIPPoolID StarMediumID

starIPPoolContext DisplayString

starIPPoolGroup DisplayString

starIPPoolName OCTET STRING

starIPPoolType INTEGER

starIPPoolState INTEGER

starIPPoolStartAddr IpAddress

starIPPoolMaskorEndAddr IpAddress

starIPPoolPriority Integer32

starIPPoolUsed Gauge32

starIPPoolHold Gauge32

starIPPoolRelease Gauge32

starIPPoolFree Gauge32
Object

starIPPoolVpnID

Object ID

enterprises.8164.1.30.1.1.1

Description

The context ID for this pool.

Syntax

Gauge32

Access

Read-only
Object

starIPPoolID

Object ID

enterprises.8164.1.30.1.1.2

Description

The service identification is made up from first 16 chars of context name and first 8 chars of pool name separated by (:).

Syntax

StarMediumID

Access

Not-accessible
Object

starIPPoolContext

Object ID

enterprises.8164.1.30.1.1.3

Description

The context for this pool.

Syntax

DisplayString

Access

Not-accessible
Object

starIPPoolGroup

Object ID

enterprises.8164.1.30.1.1.4

Description

The name of the group to which the IP pool belongs.

Syntax

DisplayString

Access

Not-accessible
Object

starIPPoolName

Object ID

enterprises.8164.1.30.1.1.5

Description

The name of the IP pool.

Syntax

OCTET STRING (SIZE (1..32))

Access

Not-accessible
Object

starIPPoolType

Object ID

enterprises.8164.1.30.1.1.6

Description

The type of the pool.

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

private(1)

public(2)

static(3)

resource(4),

nat(5)
Object

starIPPoolState

Object ID

enterprises.8164.1.30.1.1.7

Description

The state of the pool.

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

good(1)

pendingdelete(2)

alarm(3)

resize(4)

inactive(5)
Object

starIPPoolStartAddr

Object ID

enterprises.8164.1.30.1.1.8

Description

The start IP address of the pool.

Syntax

IpAddress

Access

Read-only
Object

starIPPoolMaskorEndAddr

Object ID

enterprises.8164.1.30.1.1.9

Description

The mask or end IP address of the pool.

Syntax

IpAddress

Access

Read-only
Object

starIPPoolPriority

Object ID

enterprises.8164.1.30.1.1.10

Description

The priority of the pool.

Syntax

Integer32

Access

Read-only
Object

starIPPoolUsed

Object ID

enterprises.8164.1.30.1.1.11

Description

The number of IP addresses in USED state in the pool.

Syntax

Gauge32

Access

Read-only
Object

starIPPoolHold

Object ID

enterprises.8164.1.30.1.1.12

Description

The number of IP addresses in HOLD state in the pool.

Syntax

Gauge32

Access

Read-only
Object

starIPPoolRelease

Object ID

enterprises.8164.1.30.1.1.13

Description

The number of IP addresses in RELEASE state in the pool.

Syntax

Gauge32

Access

Read-only
Object

starIPPoolFree

Object ID

enterprises.8164.1.30.1.1.14

Description

The number of IP addresses in FREE state in the pool.

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentTrapData(31)
Object

starCongestionPolicy

Object ID

enterprises.8164.1.31.1

Description

The policy invoked for congestion events.

Syntax

INTEGER

Access

Not-accessible

Objects

reject(1)

redirect(2)

drop(3)
Object

starCongestionResourceType

Object ID

enterprises.8164.1.31.2

Description

The resource type for a congestion event.

Syntax

INTEGER

Access

Not-accessible

Objects

systemcpu(1)

servicecpu(2)

averagememory(3)

queuesize(4)

queuedelay(5)

license(6)

portutil(7)

rxportutill(8)

txportutil(9)

rxperportutil(10)

txperportutil(11)

servicecapacity(12)
Object

starPTACConfig

Object ID

enterprises.8164.1.31.3

Description

The number of packet processing cards configured in the system.

Syntax

Integer32(0..14)

Access

Not-accessible
Object

starPTACActive

Object ID

enterprises.8164.1.31.4

Description

The number of packet processing cards active in the system.

Syntax

Integer32(0..14)

Access

Not-accessible
Object

starContextName

Object ID

enterprises.8164.1.31.5

Description

The name of a context configured on the system.

Syntax

DisplayString

Access

Not-accessible
Object

starInterfaceName

Object ID

enterprises.8164.1.31.6

Description

The name of an interface.

Syntax

DisplayString

Access

Not-accessible
Object

starPCFAddress

Object ID

enterprises.8164.1.31.7

Description

The IP address of a PCF.

Syntax

IpAddress

Access

Not-accessible
Object

starPeerAddress

Object ID

enterprises.8164.1.31.8

Description

Peer Address

Syntax

IpAddress

Access

Not-accessible
Object

starLicensedSessions

Object ID

enterprises.8164.1.31.9

Description

The number of sessions enabled by the software license.

Syntax

Unsigned32

Access

Accessible-for-notify
Object

starCurrentSessions

Object ID

enterprises.8164.1.31.10

Description

The number of current sessions in use against a software license.

Syntax

Gauge32

Access

Accessible-for-notify
Object

starL3Address

Object ID

enterprises.8164.1.31.11

Description

L3 Address

Syntax

IpAddress

Access

Not-accessible
Object

starUDPPortNum

Object ID

enterprises.8164.1.31.12

Description

UDP Port Number

Syntax

Integer32(1..65535)

Access

Not-accessible
Object

starSRPIPAddress

Object ID

enterprises.8164.1.31.13

Description

SRP IP Address

Syntax

IpAddress

Access

Not-accessible
Object

starBGPPeerIPAddress

Object ID

enterprises.8164.1.31.14

Description

BGP Peer IP Address

Syntax

IpAddress

Access

Not-accessible
Object

starContFiltCFFilename

Object ID

enterprises.8164.1.31.15

Description

File name for the Optimized Content Rating Database (OPTCMDB)

Syntax

DisplayString

Access

Not-accessible
Object

starContFiltCFErrorCode

Object ID

enterprises.8164.1.31.16

Description

Error code.

Syntax

Integer32

Access

Not-accessible
Object

starFetchedFromAAAMgr

Object ID

enterprises.8164.1.31.17

Description

The total number of calls fetched from AAA Manager

Syntax

Integer32

Access

Read-only
Object

starPriorToAudit

Object ID

enterprises.8164.1.31.18

Description

The number calls prior to audit

Syntax

Integer32

Access

Read-only
Object

starPassedAudit

Object ID

enterprises.8164.1.31.19

Description

The number calls prior to audit

Syntax

Integer32

Access

Read-only
Object

starCallsRecovered

Object ID

enterprises.8164.1.31.20

Description

The number calls recovered

Syntax

Integer32

Access

Read-only
Object

starA11CallLines

Object ID

enterprises.8164.1.31.21

Description

The number of A11 call lines

Syntax

Integer32

Access

Read-only
Object

starElapsedMs

Object ID

enterprises.8164.1.31.22

Description

The audit time elapsed in milli-seconds

Syntax

Integer32

Access

Read-only
Object

starCDRFilename

Object ID

enterprises.8164.1.31.23

Description

The name of a CDR (EDR/UDR) file.

Syntax

DisplayString

Access

Not-accessible
Object

starDiameterVpnName

Object ID

enterprises.8164.1.31.24

Description

Diameter VPN (Context) Name

Syntax

DisplayString

Access

Accessible-for-notify
Object

starDiameterPeerAddr

Object ID

enterprises.8164.1.31.25

Description

Diameter Peer Address

Syntax

IpAddress

Access

Accessible-for-notify
Object

starDiameterEndpointName

Object ID

enterprises.8164.1.31.26

Description

Diameter Endpoint Name

Syntax

DisplayString

Access

Accessible-for-notify
Object

starInterfaceIPAddress

Object ID

enterprises.8164.1.31.27

Description

Interface IP Address

Syntax

IpAddress

Access

Accessible-for-notify
Object

starOSPFNeighborRouterID

Object ID

enterprises.8164.1.31.28

Description

Interface IP Address

Syntax

IpAddress

Access

Accessible-for-notify
Object

starOSPFFromState

Object ID

enterprises.8164.1.31.29

Description

FROM state for OSPF Neighbor

Syntax

StarOSPFNeighborState

Access

Accessible-for-notify
Object

starOSPFToState

Object ID

enterprises.8164.1.31.30

Description

TO state for OSPF Neighbor

Syntax

StarOSPFNeighborState

Access

Accessible-for-notify
Object

starDiameterEncoderString

Object ID

enterprises.8164.1.31.31

Description

Diameter Cause Code String

Syntax

DisplayString

Access

Accessible-for-notify
Object

starDiameterECode

Object ID

enterprises.8164.1.31.33

Description

Diameter Cause code

Syntax

Integer

Access

Accessible-for-notify

Enumeration

notcomplete(1)

hostnamemismatch(2)

hostrealmismatch(3)

securitymismatch(4)

tlscertificateerror(5)

tlshandshakeerror(6)

authappidmismatch(7)
Object

starDiameterPeerAddrIpv6

Object ID

enterprises.8164.1.31.34

Description

Diameter Peer Address

Syntax

Ipv6Address

Access

accessible-for-notify
Object

starContFiltCFUpgradeFilename

Object ID

enterprises.8164.1.31.35

Description

File name for the Full or Incremental OPTCMDB

Syntax

DisplayString

Access

not-accessible
Object

starContFiltCFUpgradeErrorCode

Object ID

enterprises.8164.1.31.36

Description

Error code

Syntax

unknownerror(1)

upgradefullfailure(2)

upgradeincrfailure(3)

Access

not-accessible
Object

starBLUpgradeFilename

Object ID

enterprises.8164.1.31.37

Description

File name for the Full OPTBLDB

Syntax

DisplayString

Access

not-accessible
Object

starBLUpgradeErrorCode

Object ID

enterprises.8164.1.31.38

Description

Error code

Syntax

unknownerror(1)

upgradefullfailure(2)

Access

not-accessible
Object

starDynPkgFilename

Object ID

enterprises.8164.1.31.39

Description

File name for the DynPkg

Syntax

DisplayString

Access

not-accessible
Object

starDynCFErrorCode

Object ID

enterprises.8164.1.31.40

Description

Error code

Syntax

unknownerror(1)

notavailable(2)

loadfailure(3)

Access

not-accessible
Object

starDynPkgUpgradeFilename

Object ID

enterprises.8164.1.31.41

Description

File name for the Full DynPkg

Syntax

DisplayString

Access

not-accessible
Object

starDynCFUpgradeErrorCode

Object ID

enterprises.8164.1.31.42

Description

Error code

Syntax

unknownerror(1)

upgradefullfailure(2)

Access

not-accessible
Object

starCscfSessCongestionResourceType

Object ID

enterprises.8164.1.31.43

Description

Cscf Session resource type for a congestion event

Syntax

cpu(1)

memory(2)

Access

not-accessible
Object

starSmgrId

Object ID

enterprises.8164.1.31.44

Description

Session Manager Instance ID

Syntax

Integer32

Access

not-accessible
Object

starEGTPVpnName

Object ID

enterprises.8164.1.31.45

Description

The name of this VPN (context)

Syntax

DisplayString

Access

accessible-for-notify
Object

starEGTPServName

Object ID

enterprises.8164.1.31.46

Description

The name of this service

Syntax

DisplayString

Access

accessible-for-notify
Object

starEGTPInterfaceType

Object ID

enterprises.8164.1.31.47

Description

Egtp interface type

Syntax

INTEGER

Access

accessible-for-notify
Object

starEGTPSelfPort

Object ID

enterprises.8164.1.31.48

Description

The Port number of the EGTP

Syntax

Gauge32

Access

accessible-for-notify
Object

starEGTPSelfAddr

Object ID

enterprises.8164.1.31.49

Description

The IP Address of the EGTP

Syntax

IpAddress

Access

accessible-for-notify
Object

starEGTPPeerPort

Object ID

enterprises.8164.1.31.50

Description

The Port number of the PeerNode

Syntax

Gauge32

Access

accessible-for-notify
Object

starEGTPPeerAddr

Object ID

enterprises.8164.1.31.51

Description

The IP Address of the PeerNode

Syntax

IpAddress

Access

accessible-for-notify
Object

starEGTPPeerOldRstCnt

Object ID

enterprises.8164.1.31.52

Description

EGTP peer old restart counter

Syntax

Gauge32

Access

accessible-for-notify
Object

starEGTPPeerNewRstCnt

Object ID

enterprises.8164.1.31.53

Description

EGTP peer new restart counter

Syntax

Gauge32

Access

accessible-for-notify
Object

starEGTPPeerSessCnt

Object ID

enterprises.8164.1.31.54

Description

EGTP peer session count

Syntax

Gauge32

Access

accessible-for-notify
Object

starEGTPFailureReason

Object ID

enterprises.8164.1.31.55

Description

Egtp path failure reason

Syntax

INTEGER

Access

accessible-for-notify
Object

starGSSCDRLossConfigured

Object ID

enterprises.8164.1.31.56

Description

The configured value of threshold CDR Loss at GSS

Syntax

Unsigned32

Access

accessible-for-notify
Object

starGSSCDRLossMeasured

Object ID

enterprises.8164.1.31.57

Description

The Measured value of CDR Loss at GSS

Syntax

Unsigned32

Access

accessible-for-notify
Object

starLicenseKey

Object ID

enterprises.8164.1.31.58

Description

The license key

Syntax

Unsigned32

Access

accessible-for-notifyaccessible-for-notify
Object

starLicenseExpiryDate

Object ID

enterprises.8164.1.31.59

Description

The license expiration date/time

Syntax

DateAndTime

Access

accessible-for-notify
Object

starLicenseDaysRemaining

Object ID

enterprises.8164.1.31.60

Description

The number of days remaining before the license expires

Syntax

Unsigned32

Access

accessible-for-notify
Object

starLicenseDaysafterExpiry

Object ID

enterprises.8164.1.31.61

Description

The number of days after the license has expired

Syntax

Unsigned32

Access

accessible-for-notify
Object

starNPUSlot

Object ID

enterprises.8164.1.31.62

Description

The NPU slot number

Syntax

Integer32

Access

accessible-for-notify
Object

starSPRServerIpAddr

Object ID

enterprises.8164.1.31.63

Description

The IP Address of the SSC Server

Syntax

IpAddress

Access

accessible-for-notify
Object

starMVGEndpointName

Object ID

enterprises.8164.1.31.66

Description

MVG Endpoint Name.

Syntax

DisplayString

Access

accessible-for-notify
Object

starMVGProtocolType

Object ID

enterprises.8164.1.31.68

Description

MVG Protocol Types.

Syntax

INTEGER { protocolhttp(1), protocoltcp(2), protocolicmp(3) }

Access

accessible-for-notify
Object

starMVGCauseCode

Object ID

enterprises.8164.1.31.69

Description

MVG Cause Code.

Syntax

INTEGER {

servernotreachable(1)

servicereachable(2)

}

Access

accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starentGGSNService(32)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starGGSNSerTable

Object ID

enterprises.8164.1.32.1

Description

A table containing GGSN related information

Syntax

SEQUENCE OF StarGGSNSerEntry

Access

Not-accessible
Object

starGGSNSerEntry

Object ID

enterprises.8164.1.32.1.1

Description

The statistics for a specific GGSN service

Syntax

StarGGSNSerEntry

Access

Not-accessible

Sequence

starGGSNSerVpnID

starGGSNSerSvcID

starSessGGSNVpnName

starSessGGSNServName

starSessGGSNPeerPort

starSessGGSNPeerAddr

starSessGGSNImsi

starSessGGSNSubsName

starSessGGSNAPNName
Object

starGGSNSerVpnID

Object ID

enterprises.8164.1.32.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

Not-accessible
Object

starGGSNSerSvcID

Object ID

enterprises.8164.1.32.1.1.2

Description

The internal identification of this service; unique within a specific context

Syntax

Gauge32

Access

Not-accessible
Object

starSessGGSNVpnName

Object ID

enterprises.8164.1.32.1.1.3

Description

The name of this VPN (context)

Syntax

DisplayString

Access

Read-only
Object

starSessGGSNServName

Object ID

enterprises.8164.1.32.1.1.4

Description

The name of this service

Syntax

DisplayString

Access

Read-only
Object

starSessGGSNPeerPort

Object ID

enterprises.8164.1.32.1.1.5

Description

The Peer Port for which PATH Failure has occurred

Syntax

Gauge32

Access

Accessible-for-notify
Object

starSessGGSNPeerAddr

Object ID

enterprises.8164.1.32.1.1.6

Description

The Peer Address for which PATH Failure has occurred

Syntax

IpAddress

Access

Read-only
Object

starSessGGSNImsi

Object ID

enterprises.8164.1.32.1.1.7

Description

The IMSI of the subscriber.

Syntax

OCTET STRING (SIZE (1..8))

Access

Accessible-for-notify
Object

starSessGGSNSubsName

Object ID

enterprises.8164.1.32.1.1.8

Description

The name of the subscriber.

Syntax

OCTET STRING (SIZE (1..128))

Access

Accessible-for-notify
Object

starSessGGSNAPNName

Object ID

enterprises.8164.1.32.1.1.9

Description

The name of the APN.

Syntax

OCTET STRING (SIZE (1..64))

Access

Accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starentL2TP(33)
Object

starL2TPTable

Object ID

enterprises.8164.1.33.1

Description

A table containing L2TP related information

Syntax

SEQUENCE OF starL2TPEntry

Access

Not-accessible
Object

starL2TPEntry

Object ID

enterprises.8164.1.33.1.1

Description

The statistics for a L2TP entry

Syntax

starL2TPEntry

Access

Not-accessible

Sequence

starL2TPLocalTunnelID

starL2TPPeerTunnelID

starL2TPContextName

starL2TPServiceName

starL2TPServiceTypeName

starL2TPLocalAddress

starL2TPPeerAddress
Object

starL2TPLocalTunnelID

Object ID

enterprises.8164.1.33.1.1.1

Description

The internal identification of the L2TP local tunnel ID

Syntax

Unsigned32

Access

Not-accessible
Object

starL2TPPeerTunnelID

Object ID

enterprises.8164.1.33.1.1.2

Description

The internal identification of the L2TP peer tunnel ID

Syntax

Unsigned32

Access

Not-accessible
Object

starL2TPContextName

Object ID

enterprises.8164.1.33.1.1.3

Description

The name of the context

Syntax

DisplayString

Access

Accessible-for-notify
Object

starL2TPServiceName

Object ID

enterprises.8164.1.33.1.1.4

Description

The name of the service

Syntax

DisplayString

Access

Accessible-for-notify
Object

starL2TPServiceTypeName

Object ID

enterprises.8164.1.33.1.1.5

Description

The name of the service type

Syntax

DisplayString

Access

Accessible-for-notify
Object

starL2TPLocalAddress

Object ID

enterprises.8164.1.33.1.1.6

Description

The local address of the service

Syntax

IpAddress

Access

Accessible-for-notify
Object

starL2TPPeerAddress

Object ID

enterprises.8164.1.33.1.1.7

Description

The peer address of the service

Syntax

IpAddress

Access

Accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starSessSub1(34)

Use a SET pdu to provide the keys to lookup. Set one or more of the fields starSessSub1Context, starSessSub1NAI, starSessSub1MSID, starSessSub1IpAddr.

The SET pdu returns once the query is complete. This query can takes some time especially on large systems, so do not use small retry timers.

Use a GET pdu to retrieve the data.

IMPORTANT:

Note that in some cases, multiple subscribers might watch the given search criteria. The starSessSub1LastResult field identifies if zero, one or multiple matches were found. If multiple matches are found, data is returned for one of them.
Object

starSessSub1Context

Object ID

enterprises.8164.1.34.1

Description

The name of the context for this subscriber. If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills-in the various objects in this row.

Syntax

DisplayString

Access

Read-write
Object

starSessSub1NAI

Object ID

enterprises.8164.1.34.2

Description

The NAI for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

Syntax

OCTET STRING (SIZE (1..128))

Access

Read-write
Object

starSessSub1MSID

Object ID

enterprises.8164.1.34.3

Description

The MSID for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

Syntax

OCTET STRING (SIZE (1..16))

Access

Read-write
Object

starSessSub1IpAddr

Object ID

enterprises.8164.1.34.4

Description

The remote IP address for this subscriber If a SET is received, triggers a lookup for a subscriber that matches the specified search criteria and fills in the various objects in this row.

Syntax

IpAddress

Access

Read-write
Object

starSessSub1LastResult

Object ID

enterprises.8164.1.34.5

Description

The result of the last search. A value of unknown(0) means that the query wasn't created properly, or that no query has been performed; error(1) indicates an internal error performing the query, this is an abnormal condition that shouldn't normally be seen; nomatch(2) means that the query did not find a matching subscriber; onematch(3) means that the query found exactly one subscriber; multimatch(4) means that more than one subscriber matched; the information for one (random) subscriber was fetched

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

error(1)

nomatch(2)

onematch(3)

multimatch(4)
Object

starSessSub1ServiceName

Object ID

enterprises.8164.1.34.6

Description

The service name of the subscriber.

Syntax

OCTET STRING (SIZE (1..63))

Access

Read-only
Object

starSessSub1HAIpAddr

Object ID

enterprises.8164.1.34.7

Description

The HA IP address for FA MIP connections

Syntax

IpAddress

Access

Read-only
Object

starSessSub1PeerIpAddr

Object ID

enterprises.8164.1.34.8

Description

The remote IP address of the peer. The type of peer depends on the session type:

Session Type | Peer
--- | ---
PDSN | PCF
GGSN | SGSN
HA Mobile IP/HA IPSEC | FA
LAC | LNS
LNS | LAC

Syntax

IpAddress

Access

Read-only
Object

starSessSub1InPackets

Object ID

enterprises.8164.1.34.9

Description

The number of incoming packets for the subscriber

Syntax

Counter32

Access

Read-only
Object

starSessSub1InPacketsDropped

Object ID

enterprises.8164.1.34.10

Description

The number of incoming packets dropped for the subscriber

Syntax

Counter32

Access

Read-only
Object

starSessSub1InBytes

Object ID

enterprises.8164.1.34.11

Description

The count of incoming bytes for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes

Syntax

Counter32

Units

KB

Access

Read-only
Object

starSessSub1OutPackets

Object ID

enterprises.8164.1.34.12

Description

The number of outgoing packets for the subscriber

Syntax

Counter32

Access

Read-only
Object

starSessSub1OutPacketsDropped

Object ID

enterprises.8164.1.34.13

Description

The number of outgoing packets dropped for the subscriber

Syntax

Counter32

Access

Read-only
Object

starSessSub1OutBytes

Object ID

enterprises.8164.1.34.14

Description

The count of outgoing bytes for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes.

Syntax

Counter32

Units

KB

Access

Read-only
Object

starSessSub1Activity

Object ID

enterprises.8164.1.34.15

Description

TBD

Syntax

Gauge32

Units

%

Access

Read-only
Object

starSessSub1State

Object ID

enterprises.8164.1.34.16

Description

The state of the subscriber

Syntax

INTEGER

Access

Read-only

Enumeration

Unknown(0)

Connecting(1)

Connected(2)

Disconnecting(3)
Object

starSessSub1CallID

Object ID

enterprises.8164.1.34.17

Description

The internal call ID of the subscriber

Syntax

Integer32

Access

Read-only
Object

starSessSub1ConnectTime

Object ID

enterprises.8164.1.34.18

Description

The connect time for the subscriber, in UTC. The UNIX epoch (Jan. 1, 1970) is used if no value is available

Syntax

DateAndTime

Access

Read-only
Object

starSessSub1CallDuration

Object ID

enterprises.8164.1.34.19

Description

The duration of the call, in seconds

Syntax

Counter32

Units

Seconds

Access

Read-only
Object

starSessSub1TimeIdle

Object ID

enterprises.8164.1.34.20

Description

The idle time of the call, in seconds

Syntax

Gauge32

Units

Seconds

Access

Read-only
Object

starSessSub1AccessType

Object ID

enterprises.8164.1.34.21

Description

The access type for the subscriber.

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

pdsnsimpleip(1)

pdsnmobileip(2)

hamobileip(3)

ggsnpdptypeipv4(4)

ggsnpdptypeppp(5)

ggsnpdptypeipv6(6)

lnsl2tp(7)

haipsec(8)

ipsg(9)

pdsnsipmip(10)

mipproxyfa(11)

imsa(12)

bcmcs(13)

ggsnmip(14)

ipprobe(15)

ansgw(16)
Object

starSessSub1AccessTech

Object ID

enterprises.8164.1.34.22

Description

The access technology for the subscriber.

Syntax

INTEGER

Access

Read-only

Sequence

unknown(0)

cdma1xrtt(1)

cdmaevdo(2)

cdmaother(3)

wcdmautran(4)

gprsgeran(5)

gprsother(6)

wirelesslan(7)

ipsg(8)

wimax(9)

sip(10)

other(11)

cdmaevdoreva(12)

pdif(13)

phs(14)

ehrpd(15)

eutran(16)

gan(17)

hspa(18)
Object

starSessSub1LinkStatus

Object ID

enterprises.8164.1.34.23

Description

The link status for the subscriber.

Syntax

INTEGER

Enumeration

Read-only

Sequence

unknown(0)

active(1)

dormant(2)
Object

starSessSub1NetworkType

Object ID

enterprises.8164.1.34.24

Description

The network type for the subscriber.

Syntax

INTEGER

Access

Read-only

Sequence

unknown(0)

ip(1)

mobileip(2)

l2tp(3)

proxymobileip(4)

ipinip(5)

gre(6)

ipv6inipv4(7)
Object

starSessSub1CarrierID

Object ID

enterprises.8164.1.34.25

Description

Carrier ID

Syntax

OCTET STRING (SIZE (0..6))

Access

Read-only
Object

starSessSub1ESN

Object ID

enterprises.8164.1.34.26

Description

Electronic Serial Number

Syntax

OCTET STRING (SIZE (0..15))

Access

Read-only
Object

starSessSub1GMTTimezoneOffset

Object ID

enterprises.8164.1.34.27

Description

Timezone offset from GMT, in seconds. This is a signed value

Syntax

Integer32

Units

Seconds

Access

Read-only
Object

starSessSub1SessMgr

Object ID

enterprises.8164.1.34.28

Description

The instance number of the session manager for this subscriber.

Syntax

Unsigned32

Access

Read-only
Object

starSessSub1RemoteIPAddr

Object ID

enterprises.8164.1.34.29

Description

Remote IP Address

Syntax

IpAddress

Access

Read-only
Object

starSessSub1Card

Object ID

enterprises.8164.1.34.30

Description

The card holding the session manager for this session. Use in combination with starSessSub1CPU.

Syntax

Integer32(1..16)

Access

Read-only
Object

starSessSub1CPU

Object ID

enterprises.8164.1.34.31

Description

The CPU holding the session manager for this session. Use in combination with starSessSub1Card

Syntax

Integer32(0..3)

Access

Read-only
Object

starSessSub1TimeIdleLeft

Object ID

enterprises.8164.1.34.32

Description

The remaining idle time of the call, in seconds. A value of 0xffffffff is used if the call does not have an idle timeout

Syntax

Gauge32

Units

Seconds

Access

Read-only
Object

starSessSub1TimeLeft

Object ID

enterprises.8164.1.34.33

Description

The remaining session time of the call, in seconds. A value of 0xffffffff is used if the call does not have a session timeout.

Syntax

Gauge32

Units

Seconds

Access

Read-only
Object

starSessSub1TimeLongDurLeft

Object ID

enterprises.8164.1.34.34

Description

The remaining long duration time of the call, in seconds. A value of 0xffffffff is used if the call does not have a long duration timer

Syntax

Gauge32

Units

Seconds

Access

Read-only
Object

starSessSub1LongDurAction

Object ID

enterprises.8164.1.34.35

Description

The action to take when the long duration timer is reached

Syntax

StarLongDurTimeoutAction

Access

Read-only
Object

starSessSub1AlwaysOn

Object ID

enterprises.8164.1.34.36

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

enabled(1)

disabled(2)
Object

starSessSub1IPPoolName

Object ID

enterprises.8164.1.34.37

Syntax

OCTET STRING (SIZE(0..31))

Access

Read-only
Object

starSessSub1VLANID

Object ID

enterprises.8164.1.34.38

Description

0 is returned if this is not applicable

Syntax

Unsigned32

Access

Read-only
Object

starSessSub1LNSIPAddr

Object ID

enterprises.8164.1.34.39

Description

Only valid if starSessSub1NetworkType is l2tp(3), otherwise 0.0.0.0

Syntax

IpAddress

Access

Read-only
Object

starSessSub1ProxyMIP

Object ID

enterprises.8164.1.34.40

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

enabled(1)

disabled(2)
Object

starSessSub1GGSNMIP

Object ID

enterprises.8164.1.34.41

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

enabled(1)

disabled(2)
Object

starSessSub1HomeAgentIpAddr

Object ID

enterprises.8164.1.34.42

Description

The IP address of the Home Agent. This value is applicable only if one of the following is true:

- The value of starSessSub1AccessType is pdsnmobileip(2)
- The value of starSessSub1ProxyMIP is enabled(1)
- The value of starSessSub1GGSNMIP is enabled(1)

If not applicable, a value of 0.0.0.0 will be returned

Syntax

IpAddress

Access

Read-only
Object

starSessSub1LocalIPAddr

Object ID

enterprises.8164.1.34.43

Description

The Local IP address of the Home Agent. This value is applicable only if one of the following is true:

- The value of starSessSub1AccessType is pdsnsimpleip(1)
- The value of starSessSub1AccessType is ggsnpdptypeppp(5)
- The value of starSessSub1AccessType is lnsl2tp(7)

If not applicable, a value of 0.0.0.0 will be returned

Syntax

IpAddress

Access

Read-only
Object

starSessSub1FAServiceName

Object ID

enterprises.8164.1.34.44

Description

The FA service name for the subscriber. This value is applicable only if one of the following is true:

- The value of starSessSub1AccessType is pdsnmobileip(2)
- The value of starSessSub1ProxyMIP is enabled(1)
- The value of starSessSub1GGSNMIP is enabled(1)

Syntax

OCTET STRING (SIZE (1..63))

Access

Read-only
Object

starSessSub1FAVPNName

Object ID

enterprises.8164.1.34.45

Description

The FA VPN (Context) name. This value is applicable only if one of the following is true:

- The value of starSessSub1AccessType is pdsnmobileip(2)
- The value of starSessSub1ProxyMIP is enabled(1)
- The value of starSessSub1GGSNMIP is enabled(1)

Syntax

DisplayString

Access

Read-only
Object

starSessSub1SourceVPN

Object ID

enterprises.8164.1.34.46

Description

The Source VPN (Context) name.

Syntax

DisplayString

Access

Read-only
Object

starSessSub1DestVPN

Object ID

enterprises.8164.1.34.47

Description

The Destination VPN (Context) name.

Syntax

DisplayString

Access

Read-only
Object

starSessSub1AAAVPN

Object ID

enterprises.8164.1.34.48

Syntax

DisplayString

Access

Read-only
Object

starSessSub1AAADomain

Object ID

enterprises.8164.1.34.49

Syntax

DisplayString

Access

Read-only
Object

starSessSub1AAAStart

Object ID

enterprises.8164.1.34.50

Syntax

Counter32

Access

Read-only
Object

starSessSub1AAAStop

Object ID

enterprises.8164.1.34.51

Syntax

Counter32

Access

Read-only
Object

starSessSub1AAAInterim

Object ID

enterprises.8164.1.34.52

Syntax

Counter32

Access

Read-only
Object

starSessSub1AcctSessionID

Object ID

enterprises.8164.1.34.53

Syntax

OCTET STRING (SIZE(0..23))

Access

Read-only
Object

starSessSub1AAARadiusGroup

Object ID

enterprises.8164.1.34.54

Syntax

OCTET STRING (SIZE(0..63))

Access

Read-only
Object

starSessSub1AAARadiusAuthServerIPAddr

Object ID

enterprises.8164.1.34.55

Syntax

IpAddress

Access

Read-only
Object

starSessSub1AAARadiusAcctServerIPAddr

Object ID

enterprises.8164.1.34.56

Syntax

IpAddress

Access

Read-only
Object

starSessSub1NASIPAddr

Object ID

enterprises.8164.1.34.57

Syntax

IpAddress

Access

Read-only
Object

starSessSub1NexthopIPAddr

Object ID

enterprises.8164.1.34.58

Syntax

IpAddress

Access

Read-only
Object

starSessSub1ActiveInACL

Object ID

enterprises.8164.1.34.59

Syntax

OCTET STRING (SIZE(0..79))

Access

Read-only
Object

starSessSub1ActiveOutACL

Object ID

enterprises.8164.1.34.60

Syntax

OCTET STRING (SIZE(0..79))

Access

Read-only
Object

starSessSub1ECSRulebase

Object ID

enterprises.8164.1.34.61

Syntax

OCTET STRING (SIZE(0..63))

Access

Read-only
Object

starSessSub1InPlcyGrp

Object ID

enterprises.8164.1.34.62

Syntax

OCTET STRING (SIZE(0..15))

Access

Read-only
Object

starSessSub1OutPlcyGrp

Object ID

enterprises.8164.1.34.63

Syntax

OCTET STRING (SIZE(0..15))

Access

Read-only
Object

starSessSub1DownTrafPolState

Object ID

enterprises.8164.1.34.64

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

enabled(1)

disabled(2)
Object

starSessSub1DownCommDataRate

Object ID

enterprises.8164.1.34.65

Description

Downlink committed data rate, in bps. This value is only valid if starSessSub1DownTrafPolState is enabled(1)

Syntax

Unsigned32

Units

bps

Access

Read-only
Object

starSessSub1DownPeakDataRate

Object ID

enterprises.8164.1.34.66

Description

Downlink peak data rate, in bps. This value will be 0 if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

Syntax

Unsigned32

Units

bps

Access

Read-only
Object

starSessSub1DownBurstSize

Object ID

enterprises.8164.1.34.67

Description

Downlink burst size, in bytes. This value will be 0 if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

Syntax

Unsigned32

Units

bytes

Access

Read-only
Object

starSessSub1DownExceedAction

Object ID

enterprises.8164.1.34.68

Description

Downlink Exceed Action. This value will be notapplicable(1) if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

Syntax

StarQOSTPAction

Access

Read-only
Object

starSessSub1DownViolateAction

Object ID

enterprises.8164.1.34.69

Description

Downlink Violate Action. This value will be notapplicable(1) if the value of starSessSub1DownTrafPolState is anything other than enabled(1)

Syntax

StarQOSTPAction

Access

Read-only
Object

starSessSub1DownExceed

Object ID

enterprises.8164.1.34.70

Description

Downlink packets exceeded bandwidth parameters

Syntax

Counter32

Units

packets

Access

Read-only
Object

starSessSub1DownViolate

Object ID

enterprises.8164.1.34.71

Description

Downlink packets violated bandwidth parameters

Syntax

Counter32

Units

packets

Access

Read-only
Object

starSessSub1UpTrafPolState

Object ID

enterprises.8164.1.34.72

Description

Uplink traffic policing state

Syntax

INTEGER

Access

Read-only

Enumeration

unknown(0)

enabled(1)

disabled(2)
Object

starSessSub1UpCommDataRate

Object ID

enterprises.8164.1.34.73

Description

Uplink committed data rate, in bps. This value is only valid if starSessSub1UpTrafPolState is enabled(1)

Syntax

Unsigned32

Units

bps

Access

Read-only
Object

starSessSub1UpPeakDataRate

Object ID

enterprises.8164.1.34.74

Description

Uplink peak data rate, in bps. This value will be 0 if the value of starSessSub1UpTrafPolState is anything other than enabled(1)

Syntax

Unsigned32

Units

bps

Access

Read-only
Object

starSessSub1UpBurstSize

Object ID

enterprises.8164.1.34.75

Description

Uplink burst size, in bytes. This value will be 0 if the value of starSessSub1UpTrafPolState is anything other than enabled(1

Syntax

Unsigned32

Units

bytes

Access

Read-only
Object

starSessSub1UpExceedAction

Object ID

enterprises.8164.1.34.76

Description

Uplink Exceed Action. This value will be notapplicable(1) if the value of starSessSub1UpTrafPolState is anything other than enabled(1)

Syntax

StarQOSTPAction

Access

Read-only
Object

starSessSub1UpViolateAction

Object ID

enterprises.8164.1.34.77

Description

Uplink Violate Action. This value will be notapplicable(1) if the value of starSessSub1UpTrafPolState is anything other than enabled(1)

Syntax

StarQOSTPAction

Access

Read-only
Object

starSessSub1UpExceed

Object ID

enterprises.8164.1.34.78

Description

Uplink packets exceeded bandwidth parameters

Syntax

Counter32

Units

packets

Access

Read-only
Object

starSessSub1UpViolate

Object ID

enterprises.8164.1.34.79

Description

Uplink packets violated bandwidth parameters

Syntax

Counter32

Units

packets

Access

Read-only
Object

starSessSub1L3TunnelingState

Object ID

enterprises.8164.1.34.80

Description

Identifies if L3 tunneling is enabled. This value should be enabled(1) if starSessSub1NetworkType is ipinip(5) or gre(6).

Syntax

Integer

Access

Read-only
Object

starSessSub1L3TunLocalIPAddr

Object ID

enterprises.8164.1.34.81

Description

L3 tunnel local address. This value is valid only if starSessSub1L3TunnelState is enabled(1), other it will be 0.0.0.0.

Syntax

IpAddress

Access

Read-only
Object

starSessSub1L3TunRemoteIPAddr

Object ID

enterprises.8164.1.34.82

Description

L3 tunnel remote address. This value is valid only if starSessSub1L3TunnelState is enabled(1), other it will be 0.0.0.0

Syntax

IpAddress

Access

Read-only
Object

starSessSub1AddrViaDHCP

Object ID

enterprises.8164.1.34.83

Syntax

Integer

Access

Read-only
Object

starSessSub1DHCPServName

Object ID

enterprises.8164.1.34.84

Description

DHCP service name. This value is only valid if starSessSub1DHCPAddrViaDHCP is enabled(1)

Syntax

Octet string

Access

Read-only
Object

starSessSub1DHCPServIPAddr

Object ID

enterprises.8164.1.34.85

Description

DHCP service IP address. This value is only valid if starSessSub1DHCPAddrViaDHCP is enabled(1), otherwise it will be 0.0.0.0

Syntax

IpAddress

Access

Read-only
Object

starSessSub1AccessLinkIPFrag

Object ID

enterprises.8164.1.34.86

Syntax

Integer

Access

Read-only
Object

starSessSub1IgnoreDFBit

Object ID

enterprises.8164.1.34.87

Description

Ignore DF-bit data-tunnel

Syntax

Integer

Access

Read-only
Object

starSessSub1MIPGratARPMode

Object ID

enterprises.8164.1.34.88

Description

This field is only applicable if starSessSub1AccessType is hamobileip(3) or haipsec(8)

Syntax

Integer

Access

Read-only
Object

starSessSub1ExtInlSrvrProc

Object ID

enterprises.8164.1.34.89

Description

The state of external inline server processing

Syntax

Integer

Access

Read-only
Object

starSessSub1ExtInlSrvrIngrIPAddr

Object ID

enterprises.8164.1.34.90

Description

The external inline server ingress IP address. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

IP Address

Access

Read-only
Object

starSessSub1ExtInlSrvrIngrVLANTag

Object ID

enterprises.8164.1.34.91

Description

The external inline server ingress VLAN tag. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

Unsigned32

Access

Read-only
Object

starSessSub1ExtInlSrvrEgrIPAddr

Object ID

enterprises.8164.1.34.92

Description

The external inline server egress IP address. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

IpAddress

Access

Read-only
Object

starSessSub1ExtInlSrvrEgrVLANTag

Object ID

enterprises.8164.1.34.93

Description

The external inline server egress VLAN tag. This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

Unsigned32

Access

Read-only
Object

starSessSub1ExtInlSrvrVPNName

Object ID

enterprises.8164.1.34.94

Description

The external inline server context (VPN). This value is only valid if starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

DisplayString

Access

Read-only
Object

starSessSub1RadAcctMode

Object ID

enterprises.8164.1.34.95

Description

Radius Accounting Mode

Syntax

Integer

Access

Read-only
Object

starSessSub1InBytesDropped

Object ID

enterprises.8164.1.34.96

Description

The count of incoming bytes dropped for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)

Syntax

Counter32

Access

Read-only
Object

starSessSub1OutBytesDropped

Object ID

enterprises.8164.1.34.97

Description

The count of outgoing bytes dropped for the subscriber, in kilobytes, rounded down (i.e. 1023 bytes = 0 kilobytes)

Syntax

Counter32

Access

Read-only
Object

starSessSub1PeakBPSTx

Object ID

enterprises.8164.1.34.98

Description

Peak rate from user, in bytes per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1PeakBPSRx

Object ID

enterprises.8164.1.34.99

Description

Peak rate to user, in bytes per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1AveBPSTx

Object ID

enterprises.8164.1.34.100

Description

Average rate from user, in bytes per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1AveBPSRx

Object ID

enterprises.8164.1.34.101

Description

Average rate to user, in bytes per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1SustBPSTx

Object ID

enterprises.8164.1.34.102

Description

Sustained rate from user, in bytes per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1SustBPSRx

Object ID

enterprises.8164.1.34.103

Description

Sustained rate to user, in bytes per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1PeakPPSTx

Object ID

enterprises.8164.1.34.104

Description

Peak rate from user, in packets per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1PeakPPSRx

Object ID

enterprises.8164.1.34.105

Description

Peak rate to user, in packets per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1AvePPSTx

Object ID

enterprises.8164.1.34.106

Description

Average rate from user, in packets per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1AvePPSRx

Object ID

enterprises.8164.1.34.107

Description

Average rate to user, in packets per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1SustPPSTx

Object ID

enterprises.8164.1.34.108

Description

Sustained rate from user, in packets per second.

Syntax

Gauge32

Access

Read-only
Object

starSessSub1SustPPSRx

Object ID

enterprises.8164.1.34.109

Description

Sustained rate to user, in packets per second

Syntax

Gauge32

Access

Read-only
Object

starSessSub1ActivePct

Object ID

enterprises.8164.1.34.110

Description

Link online/active percentage.

Syntax

Integer32(0..100)

Access

Read-only
Object

starSessSub1IPv4BadHdr

Object ID

enterprises.8164.1.34.111

Description

IPv4 Bad Headers

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4TtlExceeded

Object ID

enterprises.8164.1.34.112

Description

IPv4 Total Exceeded

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4FragSent

Object ID

enterprises.8164.1.34.113

Description

IPv4 Fragments sent

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4FragFail

Object ID

enterprises.8164.1.34.114

Description

IPv4 Could Not Fragment errors

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4InACLDrop

Object ID

enterprises.8164.1.34.115

Description

IPv4 Input ACL Drops

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4OutACLDrop

Object ID

enterprises.8164.1.34.116

Description

IPv5 Output ACL Drops

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4InCSSDownDrop

Object ID

enterprises.8164.1.34.117

Description

IPv4 Input CSS Down Drops

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4OutCSSDownDrop

Object ID

enterprises.8164.1.34.118

Description

IPv4 Output CSS Down Drops

Syntax

Counter-32

Access

Read-only
Object

starSessSub1IPv4OutXOFFDropPkt

Object ID

enterprises.8164.1.34.119

Description

IPv4 Output XOFF Packets Drop

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4OutXOFFDropByte

Object ID

enterprises.8164.1.34.120

Description

IPv4 Output XOFF Bytes Drop

Syntax

Counter-32

Access

Read-only
Object

starSessSub1IPv4SrcViol

Object ID

enterprises.8164.1.34.121

Description

IPv4 Source Violations

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4ProxyDNSRedir

Object ID

enterprises.8164.1.34.122

Description

IPv4 Proxy-DNS Redirect

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4SrcProxyDNSPThru

Object ID

enterprises.8164.1.34.123

Description

IPv4 Proxy-DNS Pass-Thru

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4ProxyDNSDrop

Object ID

enterprises.8164.1.34.124

Description

IPv4 Proxy-DNS Drop

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4SrcViolNoAcct

Object ID

enterprises.8164.1.34.125

Description

IPv4 Source Violations No Account

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4SrcViolIgnored

Object ID

enterprises.8164.1.34.126

Description

IPv4 Source Violations Ignored

Syntax

Counter32

Access

Read-only
Object

starSessSub1ExtInlSrvrTxPkt

Object ID

enterprises.8164.1.34.127

Description

Packets transmitted to inline server. This value is valid only if the value of starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

Counter32

Access

Read-only
Object

starSessSub1ExtInlSrvrRxPkt

Object ID

enterprises.8164.1.34.128

Description

Packets received from inline server. This value is valid only if the value of starSessSub1ExtInlSrvrProc is enabled(1)

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPv4ICMPDropPkt

Object ID

enterprises.8164.1.34.129

Description

IPv4 ICMP Packets dropped

Syntax

Counter32

Access

Read-only
Object

starSessSub1TunnelType

Object ID

enterprises.8164.1.34.130

Description

Tunnel Type

Syntax

Integer

Access

Read-only
Object

starSessSub1IPSECTunDownDropPkt

Object ID

enterprises.8164.1.34.131

Description

Pool IPSEC tunnel down packets dropped. This value is only valid if the value of starSessSub1TunnelType is esp(6)

Syntax

Counter32

Access

Read-only
Object

starSessSub1IPSECFlowID

Object ID

enterprises.8164.1.34.132

Description

IP Pool IPSEC flow id. This value is only valid if the value of starSessSub1TunnelType is esp(6)

Syntax

Integer32

Access

Read-only
Object

starSessSub1DormancyTotal

Object ID

enterprises.8164.1.34.133

Description

Dormancy total. This value is not valid if the value of starSessSub1AccessType is ggsnpdptypeipv4(4) or ggsnpdptypeppp(5)

Syntax

Counter32

Access

Read-only
Object

starSessSub1HandoffTotal

Object ID

enterprises.8164.1.34.134

Description

Handoff total. This value is not valid if the value of starSessSub1AccessType is ggsnpdptypeipv4(4) or ggsnpdptypeppp(5)

Syntax

Counter32

Access

Read-only
Object

starSessSub1AccessFlows

Object ID

enterprises.8164.1.34.135

Description

Access flows

Syntax

Gauge32

Access

Read-only
Object

starSessSub1TFT

Object ID

enterprises.8164.1.34.136

Description

Number of TFTs

Syntax

Gauge32

Access

Read-only
Object

starSessSub1NASPort

Object ID

enterprises.8164.1.34.137

Description

NAS port

Syntax

Integer32

Access

Read-only
Object

starSessSub1CorrID

Object ID

enterprises.8164.1.34.139

Description

ThreeGPP2-correlation-id (C2)

Syntax

Octet String

Access

Read-only
Object

starSessSub1L2TPPeerIPAddr

Object ID

enterprises.8164.1.34.140

Description

L2TP Peer address. This value is only valid if the value of starSessSub1NetworkType is l2tp(3)

Syntax

IpAddress

Access

Read-only
Object

starSessSub1IPv4EarlyPDURecv

Object ID

enterprises.8164.1.34.141

Description

IPv4 early PDU received

Syntax

Counter32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentNwReachServer(35)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starNwReachTable

Object ID

enterprises.8164.1.35.1

Description

A table containing Network Reachable Server information

Syntax

SEQUENCE OF StarNwReachEntry

Access

Not-accessible
Object

starNwReachEntry

Object ID

enterprises.8164.1.35.1.1

Description

Information for a specific Ntw Reachable Server

Syntax

StarNwReachEntry

Access

Not-accessible

Sequence

starNwReachName

starNwReachSrvrAddr
Object

starNwReachName

Object ID

enterprises.8164.1.35.1.1.1

Description

The Name for this Network Reachable Server

Syntax

OCTET STRING (SIZE (1..16))

Access

Not-accessible
Object

starNwReachSrvrAddr

Object ID

enterprises.8164.1.35.1.1.2

Description

The IP Address for the Network Reachable Server

Syntax

IpAddress

Access

Not-accessible
starentMIB(8164).starentMIBObjects(1).starentIPSEC(36)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starIPSECContextName

Object ID

enterprises.8164.1.36.1

Description

The name of a context

Syntax

DisplayString

Access

Accessible-for-notify
Object

starIPSECGroupName

Object ID

enterprises.8164.1.36.2

Description

The name of a crypto map

Syntax

DisplayString

Access

Accessible-for-notify
Object

starIPSECTunLocalIPAddr

Object ID

enterprises.8164.1.36.3

Description

The local IP Address for an IPSEC tunnel

Syntax

DisplayString

Access

Accessible-for-notify
Object

starIPSECTunRemoteIPAddr

Object ID

enterprises.8164.1.36.4

Description

The local IP Address for an IPSEC tunnel

Syntax

DisplayString

Access

Accessible-for-notify
Object

starIPSECPolicyName

Object ID

enterprises.8164.1.36.5

Description

An IPSEC policy name

Syntax

DisplayString

Access

Accessible-for-notify
Object

starIPSECDynPolicyType

Object ID

enterprises.8164.1.36.6

Description

An IPSEC dynamic policy type. Note that the value test(5) is used only forinternal testing

Syntax

Integer

Access

Accessible-for-notify

Enumeration

unknown(0)

manual(1)

isakmp(2)

subscribertemplate(3)

subscribertunnel(4)

test(5)

dynamic(6)
Object

starIPSECDynPolicyPayloadType

Object ID

enterprises.8164.1.36.7

Description

An IPSEC dynamic policy payload type

Syntax

Integer

Access

Accessible-for-notify
Object

starIPSECLocalGateway

Object ID

enterprises.8164.1.36.8

Description

IP address of IPSec local gateway

Syntax

IpAddress

Access

Accessible-for-notify
Object

starIPSECRemoteGateway

Object ID

enterprises.8164.1.36.9

Description

IP address of IPSec remote gateway

Syntax

IpAddress

Access

Accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starentSIPRoute(37)
Object

starSIPRouteTable

Object ID

enterprises.8164.1.37.1

Description

A table containing SIPRoute related information

Syntax

SEQUENCE OF StarSIPRouteEntry

Access

Not-accessible
Object

starSIPRouteEntry

Object ID

enterprises.8164.1.37.1.1

Description

The statistics for a specific SIPRoute service

Syntax

StarSIPRouteEntry

Access

Not-accessible

Sequence

starSIPRouteVpnID Index

starSIPRouteVpnName Index

starSIPRouteVmgName

starSIPRouteAsName

starSIPRouteDestPartyNum

starSIPRouteReqNum
Object

starSIPRouteVpnID

Object ID

enterprises.8164.1.37.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

Not-accessible
Object

starSIPRouteVpnName

Object ID

enterprises.8164.1.37.1.1.2

Description

The name of this VPN (context)

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteVmgName

Object ID

enterprises.8164.1.37.1.1.3

Description

The name of this VMG (context)

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteAsName

Object ID

enterprises.8164.1.37.1.1.4

Description

The name of this AS (context)

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteDestPartyNum

Object ID

enterprises.8164.1.37.1.1.5

Description

The dest. party number

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteReqNum

Object ID

enterprises.8164.1.37.1.1.6

Description

The request number

Syntax

DisplayString

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentRPServiceOption(38)
Object

starRPServiceOptionTable

Object ID

enterprises.8164.1.38.1

Syntax

SEQUENCE OF StarRPServiceOptionEntry

Access

Not-accessible
Object

starRPServiceOptionEntry

Object ID

enterprises.8164.1.38.1.1

Syntax

StarRPServiceOptionEntry

Access

Not-accessible

Sequence

starRPServiceOptionNum

starRPServiceOptionCalls
Object

starRPServiceOptionNum

Object ID

enterprises.8164.1.38.1.1.1

Syntax

Integer32(1..255)

Access

Not-accessible
Object

starRPServiceOptionCalls

Object ID

enterprises.8164.1.38.1.1.2

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentPCFStats(39)
Object

starPCFStatTable

Object ID

enterprises.8164.1.39.1

Description

A table containing per-PCF statistics.

Syntax

SEQUENCE OF StarPCFStatEntry

Access

Not-accessible
Object

starPCFStatEntry

Object ID

enterprises.8164.1.39.1.1

Description

The statistics for a specific PCF.

Syntax

StarPCFStatsEntry

Access

Not-accessible

Sequence

starPCFStatVpnID Index

starPCFStatIpAddr

starPCFStatVpnName

starPCFStatRxPkts

starPCFStatTxPkts

starPCFStatRxBytes

starPCFStatTxBytes

starPCFStatTotalSessions

starPCFStatCurrentSessions

starPCFStatCurrentActiveSessions

starPCFStatCurrentDormantSessions

starPCFStatCurrentSIPConnected

starPCFStatCurrentMIPConnected

starPCFStatCurrentPMIPConnected

starPCFStatCurrentL2TPLACConnected

starPCFStatCurrentOtherConnected
Object

starPCFStatVpnID

Object ID

enterprises.8164.1.39.1.1.1

Description

The internal identification of the VPN (context).

Syntax

Guage32

Access

Not-accessible
Object

starPCFStatIpAddr

Object ID

enterprises.8164.1.39.1.1.2

Description

The IP address of the specific PCF.

Syntax

IpAddress

Access

Not-accessible
Object

starPCFStatVpnName

Object ID

enterprises.8164.1.39.1.1.3

Description

The name of the VPN (context).

Syntax

DisplayString

Access

Read-only
Object

starPCFStatRxPkts

Object ID

enterprises.8164.1.39.1.1.4

Description

Total packets received.

Syntax

Counter32

Units

Millions

Access

Read-only
Object

starPCFStatTxPkts

Object ID

enterprises.8164.1.39.1.1.5

Description

total packets transferred.

Syntax

Counter32

Units

Millions

Access

Read-only
Object

starPCFStatRxBytes

Object ID

enterprises.8164.1.39.1.1.6

Description

Total bytes received.

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starPCFStatTxBytes

Object ID

enterprises.8164.1.39.1.1.7

Description

Total bytes send.

Syntax

Counter32

Units

Megabytes

Access

Read-only
Object

starPCFStatTotalSessions

Object ID

enterprises.8164.1.39.1.1.8

Description

Total number of sessions.

Syntax

Counter32

Access

Read-only
Object

starPCFStatCurrentSessions

Object ID

enterprises.8164.1.39.1.1.9

Description

Total current sessions.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentActiveSessions

Object ID

enterprises.8164.1.39.1.1.10

Description

Total number of current active sessions.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentDormantSessions

Object ID

enterprises.8164.1.39.1.1.11

Description

Total Numbers of current dormant sessions.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentSIPConnected

Object ID

enterprises.8164.1.39.1.1.12

Description

Total number of Simple IP sessions connected.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentMIPConnected

Object ID

enterprises.8164.1.39.1.1.13

Description

Total number of Mobile IP sessions connected.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentPMIPConnected

Object ID

enterprises.8164.1.39.1.1.14

Description

Total number of Proxy Mobile IP sessions connected.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentL2TPLACConnected

Object ID

enterprises.8164.1.39.1.1.15

Description

Total number of current L2TP LAC connected.

Syntax

Gauge32

Access

Read-only
Object

starPCFStatCurrentOtherConnected

Object ID

enterprises.8164.1.39.1.1.16

Description

Total number of other connections.

Syntax

Gauge32

Access

Read-only
Object

starPCFTable

Object ID

enterprises.8164.1.39.2

Description

A table of per service PCF statistics

Syntax

Gauge32

Access

Read-only
Object

starPCFEntry

Object ID

enterprises.8164.1.39.2.1

Description

The statistics for a specific PCF per service

Syntax

StarPCFEntry

Access

not-accessible
Object

starPCFSvcID

Object ID

enterprises.8164.1.39.2.1.1

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:) with the length of this structure at the beginning.

Syntax

StarShortID

Access

Read-only
Object

starPCFIpAddr

Object ID

enterprises.8164.1.39.2.1.2

Description

The PCF IP address

Syntax

IpAddress

Access

Read-only
Object

starPCFVpnID

Object ID

enterprises.8164.1.39.2.1.3

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

Read-only
Object

starPCFVpnName

Object ID

enterprises.8164.1.39.2.1.4

Description

The VPN (context) name

Syntax

DisplayString

Access

Read-only
Object

starPCFServName

Object ID

enterprises.8164.1.39.2.1.5

Description

The name of this service.

Syntax

DisplayString

Access

Read-only
Object

starPCFRrqRcvd

Object ID

enterprises.8164.1.39.2.1.6

Description

Number of rrq received.

Syntax

StarShortID

Access

Read-only
Object

starPCFRrqAccepted

Object ID

enterprises.8164.1.39.2.1.7

Description

Number of rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFRrqDenied

Object ID

enterprises.8164.1.39.2.1.8

Description

Number of rrq denied

Syntax

Counter32

Access

Read-only
Object

starPCFRrqDiscarded

Object ID

enterprises.8164.1.39.2.1.9

Description

Number of rrq discarded.

Syntax

Counter32

Access

Read-only
Object

starPCFInitialRrqRcvd

Object ID

enterprises.8164.1.39.2.1.10

Description

Initial rrq received.

Syntax

Counter32

Access

Read-only
Object

starPCFInitialRrqAccepted

Object ID

enterprises.8164.1.39.2.1.11

Description

Initial rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFIntraPDSNActiveHORrqAccepted

Object ID

enterprises.8164.1.39.2.1.12

Description

Intra PDSN active handoff rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFIntraPDSNDormantHORrqAccepted

Object ID

enterprises.8164.1.39.2.1.13

Description

Intra PDSN dormant handoff rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFInterPDSNHORrqAccepted

Object ID

enterprises.8164.1.39.2.1.14

Description

Inter PDSN handoff rrq accpted.

Syntax

Counter32

Access

Read-only
Object

starPCFInitialRrqDenied

Object ID

enterprises.8164.1.39.2.1.15

Description

Intial rrq denied.

Syntax

Counter32

Access

Read-only
Object

starPCFInitialRrqDiscarded

Object ID

enterprises.8164.1.39.2.1.16

Description

Intial rrq discarded.

Syntax

Counter32

Access

Read-only
Object

starPCFRenewRrqRcvd

Object ID

enterprises.8164.1.39.2.1.17

Description

Renew rrq received.

Syntax

Counter32

Access

Read-only
Object

starPCFRenewRrqAccepted

Object ID

enterprises.8164.1.39.2.1.18

Description

Renew rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFRenewActiveRrqAccepted

Object ID

enterprises.8164.1.39.2.1.19

Description

Renew active rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFRenewDormantRrqAccepted

Object ID

enterprises.8164.1.39.2.1.20

Description

Renew dormant rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFRenewRrqDenied

Object ID

enterprises.8164.1.39.2.1.21

Description

Renew rrq denied.

Syntax

Counter32

Access

Read-only
Object

starPCFRenewRrqDiscarded

Object ID

enterprises.8164.1.39.2.1.22

Description

Renew rrq discarded.

Syntax

Counter32

Access

Read-only
Object

starPCFDeregRrqRcvd

Object ID

enterprises.8164.1.39.2.1.23

Description

Deregistration rrq received.

Syntax

Counter32

Access

Read-only
Object

starPCFDeregRrqAccepted

Object ID

enterprises.8164.1.39.2.1.24

Description

Deregistration rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFDeregDormantRrqAccepted

Object ID

enterprises.8164.1.39.2.1.25

Description

Deregistration dormant rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFDeregRrqDenied

Object ID

enterprises.8164.1.39.2.1.26

Description

Deregistration rrq denied.

Syntax

Counter32

Access

Read-only
Object

starPCFDeregRrqDiscarded

Object ID

enterprises.8164.1.39.2.1.27

Description

Deregistration rrq discarded.

Syntax

Counter32

Access

Read-only
Object

starPCFIntraPDSNActiveAnidHORrqAccepted

Object ID

enterprises.8164.1.39.2.1.28

Description

Intra PDSN active anid handoff rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFIntraPDSNDormantAnidHORrqAccepted

Object ID

enterprises.8164.1.39.2.1.29

Description

Intra PDSN dormant anidhandoff rrq accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedUnSpeReason

Object ID

enterprises.8164.1.39.2.1.30

Description

Denied unspecified reason.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedAdmProh

Object ID

enterprises.8164.1.39.2.1.31

Description

Denied admin prohibited.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedAdmProh

Object ID

enterprises.8164.1.39.2.1.32

Description

Denied insufficient resources.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedMobNodeAuthFail

Object ID

enterprises.8164.1.39.2.1.33

Description

Denied mobile node authentication failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedIdentMismatch

Object ID

enterprises.8164.1.39.2.1.34

Description

Denied identification mismatch.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedPoorFormedReq

Object ID

enterprises.8164.1.39.2.1.35

Description

Denied poor formed request.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedUnknownPDSNAddr

Object ID

enterprises.8164.1.39.2.1.36

Description

Denied unknown PDSN address.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedRevTunnelUnavail

Object ID

enterprises.8164.1.39.2.1.37

Description

Denied rev tunnel unavilable.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedRevTunnelRequire

Object ID

enterprises.8164.1.39.2.1.38

Description

Denied rev tunnel required.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedUnrecogVendorId

Object ID

enterprises.8164.1.39.2.1.39

Description

Denied unrecognized vendor id.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedSessionClosed

Object ID

enterprises.8164.1.39.2.1.40

Description

Denied session closed.

Syntax

Counter32

Access

Read-only
Object

starPCFDeniedBsnSessionInfoUnavail

Object ID

enterprises.8164.1.39.2.1.41

Description

Denied bsn session information unavilable.

Syntax

Counter32

Access

Read-only
Object

starPCFegUpdTransmitted

Object ID

enterprises.8164.1.39.2.1.42

Description

Registration updates transmitted.

Syntax

Counter32

Access

Read-only
Object

starPCFRegUpdAccepted

Object ID

enterprises.8164.1.39.2.1.43

Description

Registration updates accepted.

Syntax

Counter32

Access

Read-only
Object

starPCFRegUpdateRpLifetimeExpiry

Object ID

enterprises.8164.1.39.2.1.44

Description

Registration update rp life time expiry.

Syntax

Counter32

Access

Read-only
Object

starPCFRegUpdateUpperLayerIntiated

Object ID

enterprises.8164.1.39.2.1.45

Description

Registration update upper layer intiated

Syntax

Counter32

Access

Read-only
Object

starPCFRegUpdateOtherReason

Object ID

enterprises.8164.1.39.2.1.46

Description

Registration update other reason.

Syntax

Counter32

Access

Read-only
Object

starPCFRegUpdateHORelease

Object ID

enterprises.8164.1.39.2.1.47

Description

Registration update handoff release.

Syntax

Counter32

Access

Read-only
Object

starPCFRegUpdateSessmgrDied

Object ID

enterprises.8164.1.39.2.1.48

Description

Registration update sessmgr denied.

Syntax

Counter32

Access

Read-only
Object

starPCFAuxA10ConnectionsSetup

Object ID

enterprises.8164.1.39.2.1.49

Description

Aux a10 connections setup.

Syntax

Counter32

Access

Read-only
Object

starPCFSessionsDenied

Object ID

enterprises.8164.1.39.2.1.50

Description

Number of sessions denied.

Syntax

Counter32

Access

Read-only
Object

starPCFSessionsInit

Object ID

enterprises.8164.1.39.2.1.51

Description

Number of sessions initiated.

Syntax

Counter32

Access

Read-only
Object

starPCFSessionsReneg

Object ID

enterprises.8164.1.39.2.1.52

Description

Number of PCF sessions renegotiated.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscLcpRemote

Object ID

enterprises.8164.1.39.2.1.53

Description

Disconnect reason lcp remote.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscRpRemote

Object ID

enterprises.8164.1.39.2.1.54

Description

Disconnect reason rp remote.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscRpLocal

Object ID

enterprises.8164.1.39.2.1.55

Description

Disconnect reason rp local.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscMaxIpcpRetr

Object ID

enterprises.8164.1.39.2.1.56

Description

Disconnect reason ppp maximum ipcp retries.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscMaxIpv6cpRetr

Object ID

enterprises.8164.1.39.2.1.57

Description

Disconnect reason max ipv6cp retries.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscMaxLcpRetr

Object ID

enterprises.8164.1.39.2.1.58

Description

Disconnect reason max lcp retries.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscAuthFail

Object ID

enterprises.8164.1.39.2.1.59

Description

Disconnect reason authentication failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscSessSetupTimeout

Object ID

enterprises.8164.1.39.2.1.60

Description

Disconnect reason session setup timeout.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscFlowAddFail

Object ID

enterprises.8164.1.39.2.1.61

Description

Disconnect reason flow add failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscInvDestContext

Object ID

enterprises.8164.1.39.2.1.62

Description

Disconnect reason invalid destination context.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscLcpOptFail

Object ID

enterprises.8164.1.39.2.1.63

Description

Disconnect reason lcp option failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscIpcpOptFail

Object ID

enterprises.8164.1.39.2.1.64

Description

Disconnect reason lcp option failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscIpv6cpOptFail

Object ID

enterprises.8164.1.39.2.1.65

Description

Disconnect reason ipv6cp option failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscNoRemIpAddr

Object ID

enterprises.8164.1.39.2.1.66

Description

Disconnect reason no ip remote ip address.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscDetectionFail

Object ID

enterprises.8164.1.39.2.1.67

Description

Disconnect reason detection failure.

Syntax

Counter32

Access

Read-only
Object

starPCFDiscMisc

Object ID

enterprises.8164.1.39.2.1.68

Description

Disconnect reason misallaneous.

Syntax

Counter32

Access

Read-only
Object

starPCFCurrentSessions

Object ID

enterprises.8164.1.39.2.1.69

Description

Current sessions.

Syntax

Counter32

Access

Read-only
Object

starPCFSessionsSetup

Object ID

enterprises.8164.1.39.2.1.70

Description

Session setup.

Syntax

Counter32

Access

Read-only
Object

starPCFSessionsRelsese

Object ID

enterprises.8164.1.39.2.1.71

Description

Sessions release.

Syntax

Counter32

Access

Read-only
Object

starPCFCurrentRevaSessions

Object ID

enterprises.8164.1.39.2.1.72

Description

Current reva sessions.

Syntax

Counter32

Access

Read-only
Object

starPCFRevaSessionsSetup

Object ID

enterprises.8164.1.39.2.1.73

Description

Reva session setup.

Syntax

Counter32

Access

Read-only
Object

starPCFRevaSessionsRelsese

Object ID

enterprises.8164.1.39.2.1.74

Description

Reva session release

Syntax

Counter32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentSIPRouteServer(40)
Object

starSIPRouteServerTable

Object ID

enterprises.8164.1.40.1

Description

A table containing SIPRouteServer related information

Syntax

SEQUENCE OF StarSIPRouteServerEntry

Access

Not-accessible
Object

starSIPRouteServerEntry

Object ID

enterprises.8164.1.40.1.1

Description

The statistics for a specific SIPRouteServer.

Syntax

StarSIPRouteServerEntry

Access

Not-accessible

Sequence

starSIPRouteServerVpnID Index

starSIPRouteServerVpnName

starSIPRouteServerVmgName

starSIPRouteServerAsName

starSIPRouteServerIpAddr
Object

starSIPRouteServerVpnID

Object ID

enterprises.8164.1.40.1.1.1

Description

The internal identification of the VPN (context).

Syntax

Gauge32

Access

Not-accessible
Object

starSIPRouteServerVpnName

Object ID

enterprises.8164.1.40.1.1.2

Description

The name of the VPN (context).

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteServerVmgName

Object ID

enterprises.8164.1.40.1.1.3

Description

The name of the VMG (context).

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteServerAsName

Object ID

enterprises.8164.1.40.1.1.4

Description

The name of the AS (context).

Syntax

DisplayString

Access

Read-only
Object

starSIPRouteServerIpAddr

Object ID

enterprises.8164.1.40.1.1.5

Description

The SIP Route Server IP address.

Syntax

IP Address in dotted decimal notation

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentVIMService(41)
Object

starVIMServiceTable

Object ID

enterprises.8164.1.41.1

Description

A table containing VIM's Service related information

Syntax

SEQUENCE OF StarVIMServiceEntry

Access

Not-accessible
Object

starVIMServiceEntry

Object ID

enterprises.8164.1.41.1.1

Description

The statistics for a specific VIM's Service

Syntax

StarVIMServiceEntry

Access

Not-accessible

Sequence

starVIMServiceVpnID

starVIMServiceVpnName

starVIMServiceInstanceId

starVIMServiceFMDMaxCallRate

starVIMServiceFMDContinuousLoadCount
Object

starVIMServiceVpnID

Object ID

enterprises.8164.1.41.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

Not-accessible
Object

starVIMServiceVpnName

Object ID

enterprises.8164.1.41.1.1.2

Description

The name of this VPN (context)

Syntax

DisplayString

Access

Read-only
Object

starVIMServiceInstanceId

Object ID

enterprises.8164.1.41.1.1.3

Description

The VIM Instance ID

Syntax

Unsigned32

Access

Not-accessible
Object

starVIMServiceFMDMaxCallRate

Object ID

enterprises.8164.1.41.1.1.4

Description

Configured FMD max call rate

Syntax

Unsigned32

Units

Calls per Minute

Access

Read-only
Object

starVIMServiceFMDContinuousLoadCount

Object ID

enterprises.8164.1.41.1.1.5

Description

Configured FMD continuous load count

Syntax

Unsigned32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentGSS(42)

The GTPP Storage Server is an external entity, but the chassis reports notifications on its behalf. The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starGSSClusterName

Object ID

enterprises.8164.1.42.1

Description

The name of the Storage Server Cluster

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterNodeName

Object ID

enterprises.8164.1.42.2

Description

The name of a node within a Storage Server Cluster

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterRgName

Object ID

enterprises.8164.1.42.3

Description

The name of the Storage Server Cluster Resource Group

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterRsName

Object ID

enterprises.8164.1.42.4

Description

The name of the Storage Server Cluster Resource

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterNodeState

Object ID

enterprises.8164.1.42.5

Description

Status of the Storage Server Cluster node

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterPrevOnlineNode

Object ID

enterprises.8164.1.42.6

Description

Name of the previous node of the Storage Server Cluster which was online/active

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterFromNode

Object ID

enterprises.8164.1.42.7

Description

Information from Storage Server Cluster to node

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSClusterToNode

Object ID

enterprises.8164.1.42.8

Description

Information from node to Storage Server Cluster

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSDiskPath

Object ID

enterprises.8164.1.42.9

Description

Path information of Storage Server disk

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSTransportPath

Object ID

enterprises.8164.1.42.10

Description

Path information of Storage Server for data transportation

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSIPMPGroupName

Object ID

enterprises.8164.1.42.11

Description

Name of the IPMP group for GSS

Syntax

DisplayString

Access

Accessible-for-notify
Object

starGSSInterfaceName

Object ID

enterprises.8164.1.42.12

Description

Name of the GSS interface

Syntax

DisplayString

Access

Accessible-for-notify
starentMIB(8164).starentMIBObjects(1).starentPDIFSys(43)
Object

starPDIFSysStatus

Object ID

enterprises.8164.1.43.1

Description

The overall status of the chassis as a PDIF service. A value of noservice(1) means that the chassis is not configured/licensed for PDIF; active(2) indicates that at least one PDIF service is available for processing sessions; temporary(3) indicates that PDIF is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no PDIF service is currently active, but one or more PDIF services are configured

Syntax

INTEGER

unknown(0)

noservice(1)

active(2)

temporary(3)

outofservice(4)

Access

Read-only
Object

starPDIFSysNumService

Object ID

enterprises.8164.1.43.2

Description

The number of PDIF services configured

Syntax

Unsigned32

Units

Services

Access

Read-only
Object

starPDIFSysSessCurrent

Object ID

enterprises.8164.1.43.3

Description

The number of current PDIF sessions for this chassis

Syntax

Gauge32

Access

Read-only
Object

starPDIFSysSessCurrActive

Object ID

enterprises.8164.1.43.4

Description

The number of currently active PDIF sessions for this chassis

Syntax

Gauge32

Access

Read-only
Object

starPDIFSysSessCurrDormant

Object ID

enterprises.8164.1.43.5

Description

The number of currently dormant PDIF sessions for this chassis

Syntax

Gauge32

Access

Read-only
Object

starPDIFSysSessTtlSetup

Object ID

enterprises.8164.1.43.6

Description

The cumulative total number of PDIF sessions that have been setup.

Syntax

Counter32

Access

Read-only
Object

starPDIFSysChildSACurrent

Object ID

enterprises.8164.1.43.7

Description

Number of current PDIF child SAs for the chassis

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentPDIFService(44)
Object

starPDIFTable

Object ID

enterprises.8164.1.44.1

Description

A table of per-service PDIF information

Syntax

SEQUENCE OF StarPDIFEntry

Access

Not-accessible
Object

starPDIFEntry

Object ID

enterprises.8164.1.44.1.1

Description

The information for a PDIF service

Syntax

StarPDIFEntry

Access

Not-accessible

Sequence

starPDIFSvcID

StarShortID

starPDIFVpnID Gauge32

starPDIFVpnName DisplayString

starPDIFServName DisplayString

starPDIFStatus INTEGER

starPDIFSessCurrent Gauge32

starPDIFSessRemain Gauge32

starPDIFSessCurrentActive Gauge32

starPDIFSessCurrentDormant Gauge32

starPDIFSessCurrentIpv6Active Gauge32

starPDIFSessCurrentIpv6Dormant Gauge32

starPDIFSessCurrentIpv4Active Gauge32

starPDIFSessCurrentIpv4Dormant Gauge32

starPDIFBindIpAddress IpAddress

starPDIFBindIpPort Integer32

starPDIFBindSlot Integer32

starPDIFBindPort Integer32
Object

starPDIFSvcID

Object ID

enterprises.8164.1.44.1.1.1

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:).

Syntax

StarShortID

Access

Not-accessible
Object

starPDIFVpnID

Object ID

enterprises.8164.1.44.1.1.2

Description

The internal VPN (context) ID.

Syntax

Gauge32

Access

Read-only
Object

starPDIFVpnName

Object ID

enterprises.8164.1.44.1.1.3

Description

The VPN (context) name.

Syntax

DisplayString

Access

Read-only
Object

starPDIFServName

Object ID

enterprises.8164.1.44.11.1.4

Description

The name of this service

Syntax

DisplayString

Access

Read-only
Object

starPDIFStatus

Object ID

enterprises.8164.1.44.1.1.5

Description

The state of this PDIF service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.

Syntax

INTEGER

unknown(0)

inservice(1)

outofservice(2)

Access

Read-only
Object

starPDIFSessCurrent

Object ID

enterprises.8164.1.44.1.1.6

Description

The number of current sessions for this PDIF service.

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessRemain

Object ID

enterprises.8164.1.44.1.1.7

Description

A count of the remaining capacity for this PDIF service, in terms of sessions. If a session limit is configured for this PDIF service, starPDIFSessRemain will identify the difference between this limit and starPDIFSessCurrent. If no individual limit has been configured for this service, starPDIFSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starPDIFSessRemain cannot be summed across multiple services.

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessCurrentActive

Object ID

enterprises.8164.1.44.1.1.8

Description

The number of currently active sessions for this PDIF service

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessCurrentDormant

Object ID

enterprises.8164.1.44.1.1.9

Description

The number of currently dormant sessions for this PDIF service

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessCurrentIpv6Active

Object ID

enterprises.8164.1.44.1.1.10

Description

The number of currently active IPv6 sessions for this PDIF service

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessCurrentIpv6Dormant

Object ID

enterprises.8164.1.44.1.1.11

Description

The number of currently dormant IPv6 sessions for this PDIF service.

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessCurrentIpv4Active

Object ID

enterprises.8164.1.44.1.1.12

Description

The number of currently active IPv4 sessions for this PDIF service.

Syntax

Gauge32

Access

Read-only
Object

starPDIFSessCurrentIpv4Dormant

Object ID

enterprises.8164.1.44.1.1.13

Description

The number of currently dormant IPv4 sessions for this PDIF service.

Syntax

Gauge32

Access

Read-only
Object

starPDIFBindIpAddress

Object ID

enterprises.8164.1.44.1.1.14

Description

The bind IP address for this PDIF service

Syntax

IpAddress

Access

Read-only
Object

starPDIFBindIpPort

Object ID

enterprises.8164.1.44.1.1.15

Description

The bind IP port for this PDIF service

Syntax

Integer32

Access

Read-only
Object

starPDIFBindSlot

Object ID

enterprises.8164.1.44.1.1.16

Description

The physical slot number for the physical port which holds the interface bound to the starPDIFBindIpAddress address.

Syntax

Integer32

Access

Read-only
Object

starPDIFBindPort

Object ID

enterprises.8164.1.44.1.1.17

Description

The physical port number for the physical port which holds the interface bound to the starPDIFBindIpAddress address.

Syntax

SYNTAX Integer32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentSGSNService(45)
Object

starSGSNSerTable

Object ID

enterprises.8164.1.45.1

Description

A table containing SGSN related information.

Syntax

SEQUENCE OF StarSGSNSerEntry

Access

Not-accessible
Object

starSGSNSerEntry

Object ID

enterprises.8164.1.45.1.1

Description

The statistics for a specific SGSN service.

Syntax

StarSGSNSerEntry

Access

Not-accessible

Sequence

starSGSNSerVpnID Gauge32

starSGSNSerSvcID Gauge32

starSessSGSNVpnName DisplayString

starSessSGSNServName DisplayString

starLinkM3UASs7rdId Gauge32

starSS7Pc Gauge32

starLinkM3UAPsId Gauge32
Object

starSGSNSerVpnID

Object ID

enterprises.8164.1.45.1.1.1

Description

The internal identification of the VPN (context).

Syntax

Gauge32

Access

not-accessible
Object

starSGSNSerSvcID

Object ID

enterprises.8164.1.45.1.1.2

Description

The internal identification of this service; unique within a specific context.

Syntax

Gauge32

Access

not-accessible
Object

starSessSGSNVpnName

Object ID

enterprises.8164.1.45.1.1.3

Description

The name of this VPN (context).

Syntax

DisplayString

Access

read-only
Object

starSessSGSNServName

Object ID

enterprises.8164.1.45.1.1.4

Description

The name of this service.

Syntax

DisplayString

Access

read-only
Object

starSessSGSNMcc

Object ID

enterprises.8164.1.45.1.1.5

Description

Mobile country code

Syntax

Octet String (size1..3))

Access

Read-only
Object

starSessSGSNMnc

Object ID

enterprises.8164.1.45.1.1.6

Description

Mobile network code

Syntax

Octet String (size1..3))

Access

Read-only
Object

starSessSGSNRncId

Object ID

enterprises.8164.1.45.1.1.7

Description

The RNC id

Syntax

Gauge32

Access

Read-only
Object

starSessSGSNHlrNum

Object ID

enterprises.8164.1.45.1.1.8

Description

The HLR id

Syntax

Octet String (Size(1..16))

Access

Read-
starentMIB(8164).starentMIBObjects(1).starentSS7Rd(46)
Object

starSS7RdTable

Object ID

enterprises.8164.1.46.1

Description

Table containing SS7Rd-related information

Syntax

Sequence of StarSS7RdEntry

Access

Not-Accessible
Object

starSS7RdEntry

Object ID

enterprises.8164.1.46.1.1

Description

The statistics for a specific ss7rd

Syntax

StarSS7RdEntry

Access

Not-Accessible

Sequence

starSS7rdId Index

starSS7Pc

starSS7M3UAPsId

starSS7M3UAPspId

starSS7MTP3LinkSetId

starSS7MTP3LinkId

starSS7SCTPSelfAddr

starSS7SCTPPeerAddr

starSS7SCTPSelfPort

starSS7SCTPPeerPort
Object

starSS7rdid

Object ID

enterprises.8164.1.46.1.1.1

Description

SS7 Routing Domain identification.

Syntax

Gauge32

Access

Not accessible
Object

starSS7Pc

Object ID

enterprises.8164.1.46.1.1.2

Description

Point Code.

Syntax

Gauge32

Access

not-accessible
Object

starSS7M3UAPsId

Object ID

enterprises.8164.1.46.1.1.3

Description

Peer Server identification.

Syntax

Gauge32

Access

Read-only
Object

starSS7M3UAPspid

Object ID

enterprises.8164.1.46.1.1.4

Description

Peer Server Process Identification

Syntax

Gauge32

Access

Read-only
Object

starSS7MTP3LinkSetId

Object ID

enterprises.8164.1.46.1.1.5

Description

MTP3 LinkSet Identifier

Syntax

Gauge32

Access

Read-only
Object

starSS7MTP3LinkId

Object ID

enterprises.8164.1.46.1.1.6

Description

MTP3 Link Identifier

Syntax

Gauge32

Access

Read-only
Object

starSS7SCTPSelfAddr

Object ID

enterprises.8164.1.46.1.1.7

Description

Self-End-Point IP Address

Syntax

IpAddress

Access

Read-only
Object

starSS7SCTPPeerAddr

Object ID

enterprises.8164.1.46.1.1.8

Description

Peer Node IP Address

Syntax

IpAddress

Access

Read-Only
Object

starSS7SCTPSelfPort

Object ID

enterprises.8164.1.46.1.1.9

Description

Self end-point sctp port

Syntax

Gauge32

Access

Read-Only
Object

starSS7SCTPPeerPort

Object ID

enterprises.8164.1.46.1.1.10

Description

Peer end-point SCTP Port

Syntax

Gauge32

Access

Read-Only
starentMIB(8164).starentMIBObjects(1).starentSccpNw(47)
Object

starSccpNwTable

Object ID

enterprises.8164.1.47.1

Description

Table containing Sccp Network-related information

Syntax

Sequence of StarSccpNwEntry

Access

Not-accessible
Object

starSccpNwEntry

Object ID

enterprises.8164.1.47.1.1

Description

Statistics for a specific Sccp Network

Syntax

StarSccpNwEntry

Access

Not-accessible

Sequence

starSccpNwld Gauge32

starSccpSsn Gauge32
Object

starSccpNwId

Object ID

enterprises.8164.1.47.1.1.1

Description

SCCP Network ID

Syntax

Gauge32

Access

Not accessible
Object

starSccpSsn

Object ID

enterprises.8164.1.47.1.1.2

Description

Sub-system number

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentSGTPService(48)
Object

starSGTPSerTable

Object ID

enterprises.8164.1.48.1

Description

Table containing SGTP Service-related info

Syntax

Sequence of StarSGTPSerEntry

Access

Not-accessible
Object

starSGTPSerEntry

Object ID

enterprises.8164.1.48.1.1

Description

Statistics for a specific SGTP Service

Syntax

StarSGTPSerEntry

Access

Not-accessible

Sequence

starSGTPSerVpnID Gauge32

starSGTPSerSvcID Gauge32

starSGTPVpnName Display String

starSGTPServName Display String

starSGTPSelfAddr IpAddress

starSGTPPeerAddr IpAddress

starSGTPSelfPort Gauge32

starSGTPPeerPort Gauge32
Object

starSGTPSerVpnID

Object ID

enterprises.8164.1.48.1.1.1

Description

Internal ID of the VPN (Context)

Syntax

Gauge32

Access

Not accessible
Object

starSGTPSerSvcID

Object ID

enterprises.8164.1.48.1.1.2

Description

Internal service ID unique within this context

Syntax

Gauge32

Access

Not-accessible
Object

starSGTPVpnName

Object ID

enterprises.8164.1.48.1.1.3

Description

Name of this VPN (Context)

Syntax

DisplayString

Access

Read-only
Object

starSGTPServName

Object ID

enterprises.8164.1.48.1.1.4

Description

Name of this service

Syntax

DisplayString

Access

Read-only
Object

starSGTPSelfAddr

Object ID

enterprises.8164.1.48.1.1.5

Description

SGSN IP Address

Syntax

IP Address

Access

Read-only
Object

starSGTPPeerAddr

Object ID

enterprises.8164.1.48.1.1.6

Description

IP Address for the PeerNode

Syntax

IPAddress

Access

Read-only
Object

starSGTPSelfPort

Object ID

enterprises.8164.1.48.1.1.7

Description

The self end point SGTP port

Syntax

Gauge32

Access

Read-only
Object

starSGTPPeerPort

Object ID

enterprises.8164.1.48.1.1.8

Description

The peer end point SGTP port

Syntax

Gauge32

Access

Read-only
starentMIB(8164).starentMIBObjects(1).starentIPMSServer(49)
Object

starIPMSServerTable

Object ID

enterprises.8164.1.49.1

Description

Table containing information on IPMS servers

Syntax

Sequence of StarIPMSServerEntry

Access

Not-accessible

Sequence

starIPMSServerVpnIDGauge32

starIPMSServerAddrIpAddress

starIPMSServerVpnNameDisplayString
Object

starIPMSServerEntry

Object ID

enterprises.8164.1.49.1.1

Description

Information about a particular IPMS Server.

Syntax

Sequence of StarIPMSServerEntry

Access

Not-accessible

Sequence

starIPMSServerVpnID Gauge32

starIPMSServerAddr Address

starIPMSServerVpnName DisplayString
Object

starIPMSServerVpnID

Object ID

enterprises.8164.1.49.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

Not-accessible
Object

starIPMSServerAddr

Object ID

enterprises.8164.1.49.1.1.2

Description

The IP address of the IPMS server within this VPN (context)

Syntax

IpAddress

Access

Not-accessible
Object

starIPMSServerVpnName

Object ID

enterprises.8164.1.49.1.1.3

Description

The name of this VPN (context)

Syntax

DisplayString

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentCert(50)
Object

starCertTable

Object ID

enterprises.8164.1.50.1

Description

Table containing information on X.509 certificates

Syntax

Sequence of StarCertEntry

Access

Not-accessible
Object

starCertEntry

Object ID

enterprises.8164.1.50.1.1

Description

Information on a particular X.509 Certificate

Syntax

StarCertEntry

Access

Not-accessible

Sequence

starCertSerialNumber Display-String

starCertExpiryTime DateAndTime

starCertIssuer Display-String
Object

starCertSerialNumber

Object ID

enterprises.8164.1.50.1.1.1

Description

Certificate serial number

Syntax

DisplayString

Access

Not-accessible
Object

starCertExpiryTime

Object ID

enterprises.8164.1.50.1.1.2

Description

Certificate expiration date and time

Syntax

DateAndTime

Access

Read-only
Object

starCertIssuer

Object ID

enterprises.8164.1.50.1.1.3

Description

The certificate issuing agency

Syntax

DisplayString

Access

Read-0nly
starentMIB(8164).starentMIBObjects(1).starentFile(51)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starFileTable

Object ID

enterprises.8164.1.51.1

Description

A table of files stored on a mass storage device

Syntax

SEQUENCE OF StarFileEntry

Access

Not-accessible
Object

starFileEntry

Object ID

enterprises.8164.1.51.1.1

Description

Information about a particular file on a mass storage device

Syntax

StarFileEntry

Access

Not-accessible

Sequence

starFileName DisplayString,

starFileApplication INTEGER
Object

starFileName

Object ID

enterprises.8164.1.51.1.1.1

Description

The name (full path) of the file

Syntax

DisplayString

Access

Not-accessible
Object

starFileApplication

Object ID

enterprises.8164.1.51.1.1.2

Description

The application that owns this file

Syntax

Integer

Access

Read-only

Enumeration

unknown(0)

systemfile(1)

cdrmod(2)
starentMIB(8164).starentMIBObjects(1).starentFTPServ(52)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starFTPServTable

Object ID

enterprises.8164.1.52.1

Description

A table of FTP servers configured

Syntax

SEQUENCE OF StarFTPServEntry

Access

Not-accessible
Object

starFTPServEntry

Object ID

enterprises.8164.1.52.1.1

Description

Information about a particular FTP Server

Syntax

StarFTPServEntry

Access

Not-accessible

Sequence

starFTPServVpnID Unsigned32,

starFTPServIpAddr IpAddress,

starFTPServVpnName DisplayString
Object

starFTPServVpnID

Object ID

enterprises.8164.1.52.1.1.1

Description

The internal identification of the VPN (context) used to reach this FTP server

Syntax

Unsigned32

Access

Not-accessible
Object

starFTPServIpAddr

Object ID

enterprises.8164.1.52.1.1.2

Description

The IP address of the FTP server

Syntax

IpAddress

Access

Not-accessible
Object

starFTPServVpnName

Object ID

enterprises.8164.1.52.1.1.3

Description

The name of the VPN (context)

Syntax

DisplayString

Access

Not-accessible
starentMIB(8164).starentMIBObjects(1).starentCSCFPeerServer(53)
Object

starCSCFPeerServerTable

Object ID

enterprises.8164.1.53.1

Description

A table containing PeerServer related information

Syntax

SEQUENCE OF StarCSCFPeerServerEntry

Access

Not Accessible
Object

starCSCFPeerServerEntry

Object ID

enterprises.8164.1.53.1.1

Description

The statistics for a specific CSCF service

Syntax

StarCSCFPeerServerEntry

Access

Not Accessible

Sequence

starCSCFPeerServerVpnID Gauge32,

starCSCFPeerServerSvcID Gauge32,

starCSCFPeerServerVpnName DisplayString,

starCSCFPeerServerSvcName DisplayString,

starCSCFPeerServerListName DisplayString
Object

starCSCFPeerServerVpnID

Object ID

enterprises.8164.1.53.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

Not Accessible
Object

starCSCFPeerServerSvcID

Object ID

enterprises.8164.1.53.1.1.2

Description

The internal identification of this CSCF service; unique

Syntax

Gauge32

Access

Not Accessible
Object

starCSCFPeerServerVpnName

Object ID

enterprises.8164.1.53.1.1.3

Description

The name of this VPN (context)

Syntax

DisplayString

Access

Read-Only
Object

starCSCFPeerServerSvcName

Object ID

enterprises.8164.1.53.1.1.4

Description

The name of this CSCF-service

Syntax

DisplayString

Access

Read-Only
Object

starCSCFPeerServerListName

Object ID

enterprises.8164.1.53.1.1.5

Description

The name of the cscf-peer-server

Syntax

DisplayString
Object

starCSCFPeerServerName

Object ID

enterprises.8164.1.53.1.1.6

Description

The name of the cscf-peer-server

Syntax

DisplayString
Object

starCSCFPeerServerState

Object ID

enterprises.8164.1.53.1.1.7

Description

The state of the cscf-peer-server.

Syntax

DisplayString
starentMIB(8164).starentMIBObjects(1).starentSDH(54)
Object

starSDHTable

Object ID

enterprises.8164.1.54.1

Description

Table containing SDH information

Syntax

SEQUENCE OF StarSDHEntry

Access

Not Accessible
Object

starSDHEntry

Object ID

enterprises.8164.1.54.1.1

Description

Statistical data

Syntax

StarSDHEntry

Access

Not Accessible

Sequence

starSDHSlot Index

starSDHPort Index

starSDHOperState
Object

starSDHSlot

Object ID

enterprises.8164.1.54.1.1.1

Description

The slot number for this port

Syntax

Integer32(17..48)

Access

Not Accessible
Object

starSDHPort

Object ID

enterprises.8164.1.54.1.1.2

Description

The port number within this slot

Syntax

Integer32(1..8)

Access

Not Accessible
Object

starSDHOperState

Object ID

enterprises.8164.1.54.1.1.3

Description

A bitmask indicating the state of SDH layer SCT.

0x0000 Good

0x0001 lais

0x0002 linesd

0x0004 linesf

0x0010 lof

0x0020 los

0x0040 msrdi

Syntax

Integer32

Access

Read-Only
starentMIB(8164).starentMIBObjects(1).starentSDHPath(55)
Object

starSDHPathTable

Object ID

enterprises.8164.1.55.1

Description

Table for SDH Path data

Syntax

SEQUENCE OF starSDHPathEntry

Access

Not Accessible
Object

starSDHPathEntry

Object ID

enterprises.8164.1.55.1.1

Description

Table statistical data

Syntax

starSDHPathEntry

Access

Not Accessible

Sequence

starSDHPathSlot Integer32

starSDHPathPort Integer32

starSDHPathNum Integer32

starSDHPathOperState Integer32
Object

starSDHPathSlot

Object ID

enterprises.8164.1.55.1.1.1

Description

Slot number for this port

Syntax

Integer32(17..48)

Access

Not Accessible
Object

starSDHPathPort

Object ID

enterprises.8164.1.55.1.1.2

Description

Port number within this slot

Syntax

Integer32(1..8)

Access

Not Accessible
Object

starSDHPathNum

Object ID

enterprises.8164.1.55.1.1.3

Description

Path number

Syntax

Integer32(1..3)

Access

Not Accessible
Object

starSDHPathOperState

Object ID

enterprises.8164.1.55.1.1.4

Description

A bitmask indicating the state of SDH Path HOP

0x0000 Good

0x0001 hopathsd

0x0002 hopathsf

0x0020ppdi

0x0040 prdi

0x0080 perdi

0x0100 perdival

0x0200 perdivaloff

Syntax

Integer32

Access

Read-Only
starentMIB(8164).starentMIBObjects(1).starentE1Trib(56)
Object

starE1TribTable

Object ID

enterprises.8164.1.56.1

Description

Table for E1Trib data

Syntax

SEQUENCE OF StarE1TribEntry

Access

Not Accessible
Object

starE1TribEntry

Object ID

enterprises.8164.1.56.1.1

Description

Statistical data for table

Syntax

StarE1TribEntry

Access

Not Accessible

Sequence

starE1TribSlot Index

starE1TribPort Index

starE1TribPath Index

starE1TribTug2 Integer32

starE1TribTu12 Integer32

starE1TribOperStateLOP Integer32

starE1TribOperState Integer32
Object

starE1TribSlot

Object ID

enterprises.8164.1.56.1.1.1

Description

The slot number for this port

Syntax

Integer32(17..48)

Access

Not Accessible
Object

starE1TribPort

Object ID

enterprises.8164.1.56.1.1.2

Description

The port number within this slot

Syntax

Integer32(1..8)

Access

Not Accessible
Object

starE1TribPath

Object ID

enterprises.8164.1.56.1.1.3

Description

Not shown

Syntax

Integer32(1..3)

Access

Not Accessible
Object

starE1TribTug2

Object ID

enterprises.8164.1.56.1.1.4

Description

Not shown

Syntax

Integer32(1..7)

Access

Not Accessible
Object

starE1TribTu12

Object ID

enterprises.8164.1.56.1.1.5

Description

Not shown

Syntax

Integer32(1..3)

Access

Not Accessible
Object

starE1TribOperStateLOP

Object ID

enterprises.8164.1.56.1.1.6

Description

A bitmask indicating the stare of SDH layer LOP

0x0000 Good

0x0001 lopathsd

0x0002 lopathsf

0x0100 erdi

0x0200 rdi

0x0400 lop

0x0800 ais

0x1000 lom

Syntax

Integer32

Access

Read Only
Object

starE1TribOperState

Object ID

enterprises.8164.1.56.1.1.7

Description

A bitmask indicating the state of the E1 Tributary

0x0000 Good

0x0001 inf0x0002 insmf

0x0004 incmf

0x0008 ooof

0x0010 raiccrc

0x0020 cfebe

0x0040 rai

0x0080 rmai

0x0100 aisd

0x0200 red

0x0400 ais

0x0800 ts16aisd

Syntax

Integer32

Access

Read Only
starentMIB(8164).starentMIBObjects(1).starentGPRSLink(57)
Object

starGPRSLinkTable

Object ID

enterprises.8164.1.57.1

Description

A table containing GPRS Service Link related information.

Syntax

SEQUENCE of StarGPRSLinkEntry

Access

Not Accessible
Object

starGPRSLinkEntry

Object ID

enterprises.8164.1.57.1.1

Description

The link statistics for a specific GPRS service.

Syntax

StarGPRSLinkEntry

Sequence

starGPRSNsei Gauge32,

starGPRSNsvci Gauge32,

starGPRSBvci Gauge32,
Object

starGPRSNsei

Object ID

enterprises.8164.1.57.1.1.1

Description

Network Service Entity Identifier

Syntax

Gauge32

Access

Read-Only
Object

starGPRSNsvci

Object ID

enterprises.8164.1.57.1.1.2

Description

Network Service Virtual Circuit Identifier

Syntax

Gauge32

Access

Read-Only
Object

starGPRSBvci

Object ID

enterprises.8164.1.57.1.1.3

Description

Base Station System GPRS (General Packet Radio Service) Protocol Virtual Circuit Identifier.

Syntax

Gauge32

Access

Read-Only
starentMIB(8164).starentMIBObjects(1).starentFractE1Trib(58)
Object

starFractE1TribTable

Object ID

enterprises.8164.1.58.1

Description

A table ...

Syntax

SEQUENCE of StarFractTribEntry

Access

Not Accessible
Object

starFractE1TribEntry

Object ID

enterprises.8164.1.58.1.1

Description

Information about a specific Entry

Syntax

starFractE1TribEntry

Sequence

starFractE1TribSlot Integer32,

starFractE1TribPort I Integer32,

starFractE1TribPath Integer32,

starFractE1TribTug2 Integer32,

starFractE1TribTu12 Integer32

starFractE1TribBundNum Integer32,

starFractE1TribTimeslots DisplayString
Object

starFractE1TribSlot

Object ID

enterprises.8164.1.58.1.1.1

Description

Slot number for this port

Syntax

Integer32(17..48)

Access

Not Accessible
Object

starFractE1TribPort

Object ID

enterprises.8164.1.58.1.1.2

Description

Port number within slot

Syntax

Integer32(1..8)

Access

Not Accessible
Object

starFractE1TribPath

Object ID

enterprises.8164.1.58.1.1.3

Description

Not shown

Syntax

Integer32(1..3)
Object

starFractE1TribTug2

Object ID

enterprises.8164.1.58.1.1.4

Description

Not shown

Syntax

Integer32(1..84)

Access

Not Accessible
Object

starFractE1TribTu12

Object ID

enterprises.8164.1.58.1.1.5

Syntax

Integer32(1..3)

Access

not-accessible
Object

starFractE1TribBundNum

Object ID

enterprises.8164.1.58.1.1.6

Description

Not Given

Syntax

Integer32(0..31)

Access

Not Accessible
Object

starFractE1TribTimeslots

Object ID

enterprises.8164.1.58.1.1.7

Description

Not Given

Syntax

Display/String

Access

Read-Only
starentMIB(8164).starentMIBObjects(1).starentStorage(59)

The objects in this table are not accessible via SNMP. They are intended for use within traps.
Object

starStorageTable

Object ID

enterprises.8164.1.59.1

Description

A table of mass storage devices

Syntax

SEQUENCE OF StarStorageEntry

Access

Not Accessible
Object

starStorageEntry

Object ID

enterprises.8164.1.59.1.1

Description

Information about a particular file on a mass storage device

Syntax

StarStorageEntry

Access

Not Accessible

Sequence

starStorageSlot Integer32,

starStorageName DisplayString,

starStorageDeviceType INTEGER
Object

starStorageSlot

Object ID

enterprises.8164.1.59.1.1.1

Description

The slot number of the card holding this storage device

Syntax

Integer32(1..16)

Access

Not Accessible
Object

starStorageName

Object ID

enterprises.8164.1.59.1.1.2

Description

The name of the storage device

Syntax

DisplayString

Access

Not Accessible
Object

starStorageDeviceType

Object ID

enterprises.8164.1.59.1.1.3

Description

The storage device type. A value of independent(1) means that the device can be accessed as a standalone device, and is not part of a raid array. A value of raid(2) means that this device is a raid array. A value of raidmember(3) means the device is part of a raid array, and thus cannot be read/written to outside of the raid array

Syntax

INTEGER

Access

Not Accessible

Enumeration

unknown(0),

independent(1),

raid(2),

raidmember(3)
starentMIB(8164).starentMIBObject(1).FNGSys(60)
Object

starFNGSysStatus

Object ID

8164.1.60.1

Description

The overall status of the chassis as a FNG service. A value of noservice(1) means that the chassis is not configured/licensed for FNG; active(2) indicates that at least one NG service is available for processing sessions; temporary(3) indicates that FNG is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no FNG service is currently active, but one or more FNG services are configured.

Syntax

unknown(0)

noservice(1)

active(2)

temporary(3)

outofservice(4)

Access

read-only
Object

starFNGSysNumService

Object ID

8164.1.60.2

Description

The number of FNG services configured

Syntax

Gauge32

Access

read-only
Object

starFNGSysSessCurrent

Object ID

8164.1.60.3

Description

The number of current FNG sessions for this chassis

Syntax

Gauge32

Access

read-only
Object

starFNGSysSessCurrActive

Object ID

8164.1.60.4

Description

The number of currently active FNG sessions for this chassis

Syntax

current

Access

read-only
Object

starFNGSysSessCurrDormant

Object ID

8164.1.60.5

Description

The number of currently dormant FNG sessions for this chassis

Syntax

Gauge32

Access

read-only
Object

starFNGSysSessTtlSetup

Object ID

8164.1.60.6

Description

he cumulative total number of FNG sessions that has been setup

Syntax

Counter32

Access

read-only
Object

starFNGSysChildSACurrent

Object ID

8164.1.60.7

Description

The number of current FNG child SAs for this chassis

Syntax

Gauge32

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentFNGService(61)
Object

starFNGTable

Object ID

8164.1.61.1

Description

A table of per-service FNG information

Syntax

SEQUENCE OF StarFNGEntry

Access

not-accessible
Object

starFNGEntry

Object ID

8164.1.61.1.1

Description

The information for a FNG service

Syntax

StarFNGEntry

Access

not-accessible
Object

starFNGSvcID

Sequence

starFNGSvcID StarShortID

starFNGVpnID Gauge32

starFNGVpnName DisplayString

starFNGServName DisplayString

starFNGStatus INTEGER

starFNGSessCurrent Gauge32

starFNGSessRemain Gauge32

starFNGSessCurrentActive Gauge32

starFNGSessCurrentDormant Gauge32

starFNGSessCurrentIpv6Active Gauge32

starFNGSessCurrentIpv6Dormant Gauge32

starFNGSessCurrentIpv4Active Gauge32

starFNGSessCurrentIpv4Dormant Gauge32

starFNGBindIpAddress IpAddress

starFNGBindIpPort Integer32

starFNGBindIpPort Integer32

starFNGBindSlot Integer32

starFNGBindPort Integer32

Object ID

8164.1.61.1.1.1

Description

The service identification is made up from first 8 chars of context name and the first 8 chars of service name separated by (:)

Syntax

StarShortID

Access

not-accessible
Object

starFNGVpnID

Object ID

8164.1.61.1.1.2

Description

The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the FNG device; in general starFNGVpnName should be used to identify the VPN (context).

Syntax

Gauge32

Access

read-only
Object

starFNGVpnName

Object ID

8164.1.61.1.1.3

Description

he VPN (context) name

Syntax

DisplayString

Access

read-only
Object

starFNGServName

Object ID

8164.1.61.1.1.4

Description

he name of this service

Syntax

DisplayString

Access

read-only
Object

starFNGStatus

Object ID

8164.1.61.1.1.5

Description

The state of this FNG service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.

Syntax

unknown(0)

inservice(1)

outofservice(2)

Access

read-only
Object

starFNGSessCurrent

Object ID

8164.1.61.1.1.6

Description

The number of current sessions for this FNG service.

Syntax

Gauge32

Access

read-only
Object

starFNGSessRemain

Object ID

8164.1.61.1.1.7

Description

A count of the remaining capacity for this FNG service, in terms of sessions. If a session limit is configured for this FNG service, starFNGSessRemain will identify the difference between this limit and starFNGSessCurrent. If no individual limit has been configured for this service, starFNGSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starFNGSessRemain cannot be summed across multiple services.

Syntax

Gauge32

Access

read-only
Object

starFNGSessCurrentActive

Object ID

8164.1.61.1.1.8

Description

The number of currently active sessions for this FNG service

Syntax

Gauge32

Access

read-only
Object

starFNGSessCurrentDormant

Object ID

8164.1.61.1.1.9

Description

The number of currently dormant sessions for this FNG service.

Syntax

Gauge32

Access

read-only
Object

starFNGSessCurrentIpv6Active

Object ID

8164.1.61.1.1.10

Description

The number of currently active IPv6 sessions for this FNG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.

Syntax

Gauge32

Access

read-only
Object

starFNGSessCurrentIpv6Dormant

Object ID

8164.1.61.1.1.11

Description

The number of currently dormant IPv6 sessions for this FNG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.

Syntax

Gauge32

Access

read-only
Object

starFNGSessCurrentIpv4Active

Object ID

8164.1.61.1.1.12

Description

The number of currently active IPv4 sessions for this FNG service. Note that all FNG sessions are currently identified as 'active', and the value for starFNGSessCurrentIPv4Dormant will always be zero.

Syntax

Gauge32

Access

read-only
Object

starFNGSessCurrentIpv4Dormant

Object ID

8164.1.61.1.1.13

Description

The number of currently dormant IPv4 sessions for this FNG service. Note that all FNG sessions are currently identified as 'active', so the value for starFNGSessCurrentIPv4Dormant will always be zero.

Syntax

Gauge32

Access

read-only
Object

starFNGBindIpAddress

Object ID

8164.1.61.1.1.14

Description

The bind IP address for this FNG service.

Syntax

IpAddress

Access

read-only
Object

starFNGBindIpPort

Object ID

8164.1.61.1.1.15

Description

The bind IP port for this FNG service.

Syntax

Integer32

Access

read-only
Object

starFNGBindSlot

Object ID

8164.1.61.1.1.16

Description

he physical slot number for the physical port which holds the interface bound to the starFNGBindIpAddress address.

Syntax

Integer32

Access

read-only
Object

starFNGBindPort

Object ID

8164.1.61.1.1.17

Description

The physical port number for the physical port which holds the interface bound to the starFNGBindIpAddress address.

Syntax

Integer32

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentPDGSys(62)
Object

starPDGSysStatus

Object ID

8164.1.62.1

Description

The overall status of the chassis as a PDG service. A value of noservice(1) means that the chassis is not configured/licensed for PDG; active(2) indicates that at least one PDG service is available for processing sessions; temporary(3) indicates that PDG is running in a temporary capacity, such as running in standby mode during an online upgrade; outofservice(4) indicates that no PDG service is currently active, but one or more PDG services are configured.

Syntax

unknown(0)

noservice(1)

active(2)

temporary(3)

outofservice(4)

Access

read-only
Object

starPDGSysNumService

Object ID

8164.1.62.2

Description

The number of PDG services configured

Syntax

Unsigned32

Access

read-only

Units

Services
Object

starPDGSysSessCurrent

Object ID

8164.1.62.3

Description

The number of current PDG sessions for this chassis

Syntax

Gauge32

Access

read-only
Object

starPDGSysSessCurrActive

Object ID

8164.1.62.4

Description

he number of currently active PDG sessions for this chassis.

Syntax

Gauge32

Access

read-only
Object

starPDGSysSessCurrDormant

Object ID

8164.1.62.5

Description

The number of currently dormant PDG sessions for this chassis

Syntax

Gauge32

Access

read-only
Object

starPDGSysSessTtlSetup

Object ID

8164.1.62.6

Description

The cumulative total number of PDG sessions that has been setup

Syntax

Counter32

Access

read-only
Object

starPDGSysChildSACurrent

Object ID

8164.1.62.7

Description

The number of current PDG child SAs for this chassis

Syntax

Gauge32

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentPDGService(63)
Object

starPDGTable

Object ID

8164.1.63.1

Description

A table of per-service PDG information

Syntax

SEQUENCE OF StarPDGEntry

Access

not-accessible
Object

starPDGEntry

Object ID

8164.1.63.1.1

Description

The information for a PDG service

Syntax

StarPDGEntry

Access

not-accessible

Sequence

starPDGSvcID

starPDGVpnID

starPDGVpnName

starPDGServName

starPDGStatus

starPDGSessCurrent

starPDGSessRemain

starPDGSessCurrentActive

starPDGSessCurrentDormant

starPDGSessCurrentIpv6Active

starPDGSessCurrentIpv6Dormant

starPDGSessCurrentIpv4Active

starPDGSessCurrentIpv4Dormant

starPDGBindIpAddress

starPDGBindIpPort
Object

starPDGSvcID

Object ID

8164.1.63.1.1.1

Description

The service identification is made up from first 8 chars of context name and first 8 chars of service name separated by (:)

Syntax

StarShortID

Access

not-accessible
Object

starPDGVpnID

Object ID

8164.1.63.1.1.2

Description

The internal identification of the VPN (context). Note that this identifier can change due to configuration changes and/or the restart of the PDG device; in general starPDGVpnName should be used to identify the VPN (context).

Syntax

Gauge32

Access

read-only
Object

starPDGVpnName

Object ID

8164.1.63.1.1.3

Description

The VPN (context) name

Syntax

DisplayString

Access

read-only
Object

starPDGServName

Object ID

8164.1.63.1.1.4

Description

The name of this service

Syntax

DisplayString

Access

read-only
Object

starPDGStatus

Object ID

8164.1.63.1.1.5

Description

The state of this PDG service. The value unknown(0) indicates that the system is unable to determine the status; inservice(1) indicates that the service is available for processing sessions; outofservice(2) indicates that the service is configured, but unavailable, either due to operator action or due to a fault.

Syntax

unknown(0)

inservice(1)

outofservice(2)

Access

read-only
Object

starPDGSessCurrent

Object ID

8164.1.63.1.1.6

Description

The number of current sessions for this PDG service.

Syntax

Gauge32

Access

read-only
Object

starPDGSessRemain

Object ID

8164.1.63.1.1.7

Description

A count of the remaining capacity for this PDG service, in terms of sessions. If a session limit is configured for this PDG service, starPDGSessRemain will identify the difference between this limit and starPDGSessCurrent. If no individual limit has been configured for this service, starPDGSessRemain will identify the remaining capacity for the entire chassis. Note that in this latter case, the value for starPDGSessRemain cannot be summed across multiple services.

Syntax

Gauge32

Access

read-only
Object

starPDGSessCurrentActive

Object ID

8164.1.63.1.1.8

Description

The number of currently active sessions for this PDG service

Syntax

Gauge32

Access

read-only
Object

starPDGSessCurrentDormant

Object ID

8164.1.63.1.1.9

Description

The number of currently dormant sessions for this PDG service

Syntax

Gauge32

Access

read-only
Object

starPDGSessCurrentIpv6Active

Object ID

8164.1.63.1.1.10

Description

The number of currently active IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.

Syntax

Gauge32

Access

read-only
Object

starPDGSessCurrentIpv6Dormant

Object ID

8164.1.63.1.1.11

Description

The number of currently dormant IPv6 sessions for this PDG service. Note that this value will always be 0, as the current system does not support IPv6 sessions.

Syntax

Gauge32

Access

read-only
Object

starPDGSessCurrentIpv4Active

Object ID

8164.1.63.1.1.12

Description

The number of currently active IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', and the value for starPDGSessCurrentIPv4Dormant will always be zero.

Syntax

Gauge32

Access

read-only
Object

starPDGSessCurrentIpv4Dormant

Object ID

8164.1.63.1.1.13

Description

The number of currently dormant IPv4 sessions for this PDG service. Note that all PDG sessions are currently identified as 'active', so the value for starPDGSessCurrentIPv4Dormant will always be zero.

Syntax

Gauge32

Access

read-only
Object

starPDGBindIpAddress

Object ID

8164.1.63.1.1.14

Description

The bind IP address for this PDG service

Syntax

IpAddress

Access

read-only
Object

starPDGBindIpPort

Object ID

8164.1.63.1.1.15

Description

The bind IP port for this PDG service

Syntax

Integer32

Access

read-only
Object

starPDGBindSlot

Object ID

8164.1.63.1.1.16

Description

The bind IP port for this PDG service

Syntax

Integer32

Access

read-only
Object

starPDGBindPort

Object ID

8164.1.63.1.1.17

Description

The physical port number for the physical port which holds the interface bound to the starPDGBindIpAddress address.

Syntax

Integer32

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentIPPoolGroup(64)
Object

starIPPoolGroupTable

Object ID

8164.1.64.1

Description

A table containing IP Pool Group information

Syntax

SEQUENCE OF StarIPPoolGroupEntry

Access

not-accessible
Object

starIPPoolGroupEntry

Object ID

8164.1.64.1.1

Description

Information for a specific IP Pool Group

Syntax

StarIPPoolGroupEntry

Access

not-accessible
Object

starIPPoolGroupVpnID

Object ID

8164.1.63.1.1.1

Description

The context ID for this pool group

Syntax

Gauge32

Access

not-accessible
Object

starIPPoolGroupID

Object ID

8164.1.64.1.1.2

Description

The service identification is made up from first 8 chars of context name and first 16 chars of pool group name separated by (:)

Syntax

StarMediumID

Access

not-accessible
Object

starIPPoolGroupName

Object ID

8164.1.64.1.1.3

Description

The name of the IP pool group

Syntax

DisplayString

Access

read-only
Object

starIPPoolGroupVpnName

Object ID

8164.1.64.1.1.4

Description

The context name string for this pool group

Syntax

DisplayString

Access

read-only
Object

starIPPoolGroupUsed

Object ID

8164.1.64.1.1.5

Description

The number of IP addresses in USED state in the pool group

Syntax

Gauge32

Access

read-only
Object

starIPPoolGroupHold

Object ID

8164.1.64.1.1.6

Description

The number of IP addresses in HOLD state in the pool group

Syntax

Gauge32

Access

read-only
Object

starIPPoolGroupRelease

Object ID

8164.1.64.1.1.7

Description

The number of IP addresses in RELEASE state in the pool group

Syntax

Gauge32

Access

read-only
Object

starIPPoolGroupFree

Object ID

8164.1.64.1.1.8

Description

The number of IP addresses in FREE state in the pool group

Syntax

Gauge32

Access

read-only
Object

starIPPoolGroupPctUsed

Object ID

8164.1.64.1.1.9

Description

The context name string for this pool group

Syntax

Integer32(0..10000)

Access

read-only
Object

starIPPoolGroupAvail

Object ID

8164.1.64.1.1.10

Description

The context name string for this pool group

Syntax

Gauge32

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentHNBGWService(65)
Object

starHNBGWServTable

Object ID

8164.1.65.1

Description

The statistics for a specific HNBGW service

Syntax

StarHNBGWSerEntry

Access

not-accessible
Object

starHNBGWSerEntry

Object ID

8164.1.65.1.1

Description

The statistics for a specific HNBGW service

Syntax

StarHNBGWSerEntry

Access

not-accessible
Object

starHNBGWSerVpnID

Object ID

8164.1.65.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

not-accessible
Object

starHNBGWSerSvcID

Object ID

8164.1.65.1.1.2

Description

The internal identification of this service; unique within a specific context

Syntax

Gauge32

Access

not-accessible
Object

starSessHNBGWVpnName

Object ID

8164.1.65.1.1.3

Description

The name of this VPN (context)

Syntax

DisplayString

Access

read-only
Object

starSessHNBGWServName

Object ID

8164.1.65.1.1.4

Description

The name of this Service

Syntax

DisplayString

Access

read-only
Object

starSessHNBGWCsNwName

Object ID

8164.1.65.1.1.5

Description

The name of the CS NW

Syntax

DisplayString

Access

read-only
Object

starSessHNBGWPsNwName

Object ID

8164.1.65.1.1.6

Description

The name of the PS NW

Syntax

DisplayString

Access

read-only
Object

starSessHNBGWSgsnPtCd

Object ID

8164.1.65.1.1.7

Description

SGSN Point Code

Syntax

Integer32

Access

read-only
Object

starSessHNBGWMscPtCd

Object ID

8164.1.65.1.1.8

Description

MSC Point Code

Syntax

Integer32

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentALCAPService(66)
Object

starALCAPServTable

Object ID

8164.1.66.1

Description

A table containing ALCAP relate information.

Syntax

StarALCAPSerEntry

Access

not-accessible
Object

starALCAPSerEntry

Object ID

8164.1.66.1.1

Description

The statistics for a specific ALCAP service

Syntax

StarALCAPSerEntry

Access

not-accessible
Object

starALCAPSerVpnID

Object ID

8164.1.66.1.1.1

Description

The internal identification of the VPN (context)

Syntax

Gauge32

Access

not-accessible
Object

starALCAPSerSvcID

Object ID

8164.1.66.1.1.2

Description

The internal identification of this service; unique within a specific context.

Syntax

Gauge32

Access

not-accessible
Object

starSessALCAPVpnName

Object ID

8164.1.66.1.1.3

Description

The name of this VPN (context).

Syntax

DisplayString

Access

read-only
Object

starSessALCAPServName

Object ID

8164.1.66.1.1.4

Description

The name of this Service.

Syntax

DisplayString

Access

read-only
Object

starSessALCAPAAL2NodeName

Object ID

8164.1.66.1.1.5

Description

The name of the AAL2 Node.

Syntax

DisplayString

Access

read-only
Object

starSessALCAPPathId

Object ID

8164.1.66.1.1.6

Description

The path id of AAL2 path.

Syntax

Integer32

Access

read-only