# CSCF Service Configuration Mode Commands

The CSCF Service Configuration Mode is used to create and manage CSCF services within the current context.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
access-service

Configures the name of the P-CSCF/A-BG access service from which the system receives requests and sends responses. The access service lets the core service know where a packet needs to be routed.
Platform:

ASR 5000
Product:

SCM (P-CSCF, A-BG)
Privilege:

Administrator
Syntax

    access-service name nameno access-service [ name name ]

no

Removes the access service.
name name

Specifies the name of the P-CSCF/A-BG access service from which the system receives requests and sends responses.

name must be from 1 to 63 alpha and/or numeric characters.

IMPORTANT:

This command should only be issued in the core service configuration, however, multiple access services may be configured per core service.
Usage:

Use this command to identify the name of the P-CSCF/A-BG access service from which the system receives requests and sends responses from/to the UEs. This command is used in systems that deploy two P-CSCF/A-BG services in bridging (Back-to-Back User Agent) mode configurations where an access service P-CSCF/A-BG faces the UE network and a core P-CSCF/A-BG faces the public network.
Example:
The following command identifies the P-CSCF/A-BG access service named to the CSCF/A-BG core service:

    access-service name HA3

access-type

Specifies the access types for IMS core.
Platform:

ASR 5000
Product:

SCM (P-CSCF, A-BG)
Privilege:

Administrator
Syntax

    access-type { type } access-profile { default | name access_profile_name } | ue-ip-address-range
    name ue_ip_name  { address ip_address_mask | range start_ip_address
    end_ip_address }no access-type { type } [ access-profile | ue-ip-address-range
     [ name ue_ip_name ] ]

no

Removes the specified access type from a CSCF access profile or UE IP address/range.
access-type { type }

3gpp-e-utran-fdd: 3GPP Access Type

3gpp-e-utran-tdd: 3GPP Access Type

3gpp-geran: 3GPP Access Type

3gpp-utran-fdd: 3GPP Access Type

3gpp-utran-tdd: 3GPP Access type

3gpp2-1x: 3GPP2 Access Type

3gpp2-1x-hrpd: 3GPP2 Access Type

3gpp2-umb: 3GPP2-UMB

adsl: FixedLine Access Type

adsl2: FixedLine Access Type

adsl2p: FixedLine Access Type ADSL2+

docsis: DOCSIS

gshdsl: FixedLine Access Type G.SHDSL

hdsl: FixedLine Access Type

hdsl2: FixedLine Access Type

idsl: FixedLine Access Type

ieee-80211: WLAN Access Type

ieee-80211a: WLAN Access Type

ieee-80211b: WLAN Access Type

ieee-80211g: WLAN Access Type

ieee-80211n: WLAN Access Type

ieee-80216e: Wireless MAN Access Type

ieee-8023: Ethernet Access Type

ieee-8023a: Ethernet Access Type

ieee-8023ab: Ethernet Access Type

ieee-8023ae: Ethernet Access Type

ieee-8023ak: Ethernet Access Type

ieee-8023an: Ethernet Access Type

ieee-8023aq: Ethernet Access Type

ieee-8023e: Ethernet Access Type

ieee-8023i: Ethernet Access Type

ieee-8023j: Ethernet Access Type

ieee-8023u: Ethernet Access Type

ieee-8023y: Ethernet Access Type

ieee-8023z: Ethernet Access Type

radsl: FixedLine Access Type

sdsl: FixedLine Access Type

vdsl: FixedLine Access Type
access-profile { default | name access_profile_name }

Associates an access type with a CSCF access profile. Different access types can refer to the same access profile.
ue-ip-address-range name ue_ip_name { address ip_address_mask | range start_ip_address end_ip_address }

Configures UE IP address/range for a specific access type.

ue_ip_name must be from 1 to 79 alpha and/or numeric characters.

address ip_address_mask: Specifies a combined IP address subnet mask bits to indicate what IP addresses the specific access-type applies to. ip_address_mask must be specified using the form “IP Address/Mask Bits” where the IP address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6, and the mask bits are a numeric value, which is the number of bits in the subnet mask.
range start_ip_address end_ip_address: Configure UE IP range for specific access-type.

- start_ip_address specifies the beginning of the range of addresses.
- end_ip_address specifies the end of the range of addresses.
- ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

Usage:

Use this command to associated the access types for a specified CSCF access profile or UE IP address/range name.

IMPORTANT:

Use the sip-header command to enable SIP P-Access-Network-Info (PANI) header insertion. CSCF Proxy-CSCF Configuration Mode commands are defined in the CSCF Proxy-CSCF Configuration Mode Commands chapter in this guide.
Example:
The following command identifies the access type adsl and assigns it to access profile ap1:

    access-type adsl access-profile
    name ap1

allow-dereg

Allows the CSCF to send de-registration requests. Feature is disabled by default.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] allow-dereg

no

Disables the feature.
Usage:

Use this command to allow the CSCF service to send de-registration requests.

If the UE stops sending keepalive packets, which ends the connection between the UE and the proxy, UE information is cleared from the Proxy-CSCF (P-CSCF) or Access Border Gateway (A-BG). If de-registration requests are enabled, any UE-related information that is shared with the Serving-CSCF (S-CSCF) will also be cleared.
bind

Binds the CSCF service to a logical IP interface and specifies the maximum number of sessions that can access this service over the specified interface.
Platform:

ASR 5000
Product:

SCM (P-CSCF, A-BG)
Privilege:

Administrator
Syntax

    bind address ip_address [ cscf-hostname host_name ] [ ipsec-crypto-template template ] [ max-sessions max# ]  [ port number ] [ reserved-call-capacity percentage ] [ tls-crypto-template template [ tls-port number ] ] [ transport
    tcp ] [ use-serviceport-towards-network ]no bind address

no

Removes the binding of the service to a specified interface.
address ip_address

Specifies the IP address of the interface to which the service is being bound.

ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.
cscf-hostname host_name

Specifies the local host name of the CSCF service.

host_name must be an existing CSCF service name and be from 1 to 127 alpha and/or numeric characters.

Configuring this keyword associates the CSCF service with the AOR domain configured in the default-aor-domain command and uses the domain name in SIP headers.

IMPORTANT:

If this keyword is not configured, SIP headers will contain the IP address of the CSCF service instead of the domain name.
ipsec-crypto-template template

Specifies the name of an existing IPSec CSCF crypto template to be used for accessing CSCF service by user equipment. Valid only for P-CSCF or A-BG.

template must be an existing IPSec CSCF crypto template and be from 1 to 127 alpha and/or numeric characters.

IMPORTANT:

The IPSec CSCF crypto template should be configured in the same context in which the P-CSCF is configured.
max-sessions max#

Default: 500,000

Specifies the maximum number of sessions managed by this service on this interface.

max# must be configured to any integer value from 0 to 500,000.

IMPORTANT:

The total session capacity of the system is 500,000. max-sessions is also limited by the capacity in the license generated for the service. If licenses for PDSN/GGSN/HA are generated for x number of sessions, then the license for the CSCF service will be generated at 500,000-x. Hardware configuration and installed features can also affect the maximum number of sessions that can be supported.
port number

Default: 5060

Specifies the UDP port number.

number must be an integer value from 1 to 65534.
reserved-call-capacity percentage

Default: 10

Specifies the call capacity percentage per session manager (sessmgr).

percentage must be an integer value from 1 to 50.
tls-crypto-template template [ tls-port number ]

Specifies the name of an existing Transport Layer Security (TLS) crypto template to enable TLS functionality. Valid only for P-CSCF or A-BG.

template must be an existing TLS crypto template and be from 1 to 127 alpha and/or numeric characters.

Default: 5061

Specifies the TLS port number.

number must be an integer value from 1 to 65534.

IMPORTANT:

When the tls-crypto-template is configured, TCP transport must be enabled, otherwise this command will throw an error. The configured tls-crypto-template should be should be configured in the same context in which the P-CSCF service is configured and must be complete with all certificate and cipher suite configuration. If the tls-crypto-template is not present or not completely configured, the P-CSCF service will not be started.
transport tcp

Enables TCP transport for the address.
use-serviceport-towards-network

Enables use of service port for sending and receiving UDP messages from network elements.
Usage:

Use this command to associated the service with a specific logical IP address. This command also configures the identity of the CSCF in SIP headers as either the domain name of the CSCF service or the IP address.

IMPORTANT:

Multiple keywords can be used per bind command.
Example:
The following command binds the CSCF service to a logical interface with an IP address of 1.2.3.4 and sets the maximum number of supported sessions for this interface at 250000:

    bind address 1.2.3.4
    max-sessions 250000

charging

Enables Rf charging in this CSCF service for SIP messages.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ default | no ] charging

default | no

Disables Rf charging in this CSCF service for SIP messages.
Usage:

Use this command to enable the RF charging feature in this service and enter the CSCF Charging Configuration Mode.

Entering this command results in the following prompt:

    [context_name]hostname(config-cscf-charging)#

CSCF Charging Configuration Mode commands are defined in the CSCF Charging Configuration Mode Commands chapter in this guide.
cnsa-media-profile

Configures the media profile id to be set for a previously created service policy.
Platform:

ASR 5000
Product:

SCM (S-CSCF)
Privilege:

Administrator
Syntax

    [ no ] cnsa-media-profile profile_id cscf-service-policy policy_name content-type { application-3gpp-ims-xml | application-pidf-diff-xml | application-pidf-partial-xml | application-pidf-xml | application-reginfo-xml | application-sdp | application-xml | message-sipfrag | multipart-mixed | multipart-related | text-plain }

no

Removes the media profile from the service policy.
cnsa-media-profile profile_id

Specifies the media profile id.

profile_id must be an integer from 0 to 10 and be an existing media profile id in the system. CNSA media profile ids are created and maintained in the CSCF ISC Template Configuration Mode.
cscf-service-policy policy_name

Assigns the media profile id to a service policy.

policy_name must be from 1 to 63 alpha and/or numeric characters and be an existing policy name in the system. Service policies are created and maintained in the CSCF Policy Configuration Mode.
content-type { application-3gpp-ims-xml | application-pidf-diff-xml | application-pidf-partial-xml | application-pidf-xml | application-reginfo-xml | application-sdp | application-xml | message-sipfrag | multipart-mixed | multipart-related | text-plain }

Specifies the content type(s).

application-3gpp-ims-xml - format for exchanging information in SIP Requests and Responses as used within the 3GPP IM CN Subsystem

application-pidf-diff-xml - contains changed presence elements. Contains full presence document when there are many changes

application-pidf-partial-xml - contains only changed parts of PIDF-based presence information

application-pidf-xml - XML MIME entity that contains presence information

application-reginfo-xml - used in Notifications to SIP user agents about registration expiry

application-sdp - SDP session description

application-xml - content type for generic xml documents

message-sipfrag - contains subsets of well formed SIP messages

multipart-mixed - intended for use when the body parts are independent and need to be bundled in a particular order

multipart-related - intended for compound objects consisting of several inter-related body parts

text-plain - plain text

IMPORTANT:

You may specify multiple types of content.
Usage:

Use this command to assign a media profile id to a service policy. The policies defined in the service policy apply to all subscribers using this service.

CNSA media profile ids are created and maintained in the CSCF ISC Template Configuration Mode. Service policies are created and maintained in the CSCF Policy Configuration Mode.
Example:
The following command defines the media profile id as 2 and assigns it to serv_policy3 with plain text content type.

    cnsa-media-profile 2
    cscf-service-policy serv_policy3 content-type text-plain

core-service

Configures a core service if:

- CSCF services are run in bridging (Back-to-Back User Agent) mode
- A-BG is an Application-level Gateway (ALG) for Network Address Translation (NAT)

By default, no core-service name will be present.
Platform:

ASR 5000
Product:

SCM (CSCF, A-BG)
Privilege:

Administrator
Syntax

    [ no ] core-service
    name service_name

no

Removes the core service.
name service_name

Specifies the name of the core service.

service_name must be from 1 to 80 alpha and/or numeric characters.
Usage:

Use this command to assign a core service to the CSCF/A-BG service.
Example:
The following command identifies the core service:

    core-service name service1

default-aor-domain

Configures the domain name of the service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] default-aor-domain alias

no

Removes the domain name from the service.
alias

Specifies the domain name for the service.

alias is the name of the domain for this service and must be from 1 to 79 alpha and/or numeric characters in length.
Usage:

Use this command to define the domain name of the service.
Example:
The following command defines the domain name of the CSCF service as business.com:

    default-aor-domain business.com

emergency-cscf

Enables the Emergency-CSCF for the service and enters the Emergency-CSCF Configuration Mode. Default is disabled.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] emergency-cscf

no

Disables the E-CSCF for the service.
Usage:

Use this command to enable the Emergency-CSCF feature and enter the Emergency-CSCF Configuration Mode.

Entering this command results in the following prompt:

    [context_name]hostname(config-cscf-service-emergency-cscf)#

Emergency-CSCF Configuration Mode commands are defined in the CSCF Emergency-CSCF Configuration Mode Commands chapter in this guide.

IMPORTANT:

Only one function (P-CSCF, S-CSCF, E-CSCF, SIP Proxy, or A-BG) can be enabled per service.
end

Exits the current mode and returns to the Exec Mode.
Product:

All
Privilege:

Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the current mode and returns to the previous mode.
Product:

All
Privilege:

Administrator
Syntax

    exit

Usage:

Return to the previous mode.
history-info

Enables the addition of the history-info header to SIP requests in order to capture request URI information. By default, this command is disabled.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ default | no ] history-info

default | no

Disables the inclusion of the history-info header.
Usage:

Use this command to include the history-info header in SIP requests to capture the request URI information for routing or translation.
interface statistics sip

Enables interface SIP statistic collection in this CSCF service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ default | no ] interface
    statistics sip

default | no

Disables interface SIP statistic collection for this service.
Usage:

Use this command to enable or disable the collection of interface SIP statistics in this service.
interrogating-cscf

This command is not supported in this release.
ipv4-ipv6-interworking

Allows the P-CSCF to provide IPv4-IPv6 interworking when UEs are IPv6-only and the IMS core network is IPv4-only. Feature is disabled by default.
Platform:

ASR 5000
Product:

SCM (P-CSCF)
Privilege:

Administrator
Syntax

    [ no ] ipv4-ipv6-interworking

no

Disables the feature.
Usage:

Use this command to allow IPv4-IPv6 interworking functionality.
keepalive

Configures the CSCF to receive and respond to different types of keep-alive requests.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    keepalive [ expire-timer sec [ max-retry num ] | max-retry num  [ expire-timer sec ] | method { crlf | stun }  [ expire-timer sec [ max-retry num ] | max-retry num  [ expire-timer sec ] ] ]default keepalive [ expire-timer | max-retry [ expire-timer ] | method [ expire-timer | max-retry ] ]no keepalive [ method { crlf | stun } ]

default

Returns the command to the default settings. All methods are enabled by default. See keywords above for specific defaults.
no

Disables the specified method of keepalive messages.
expire-timer sec

Default: 29

This value is used according to timed-keepalives parameter present in Path header. UEs are expected to send keepalive messages according to this time interval.

sec must be an integer from 24 to 150.
max-retry num

Default: 3

Specifies the maximum number of times the CSCF waits for the UE to send a keepalive request before it deletes the user information.

num must be an integer from 1 to 10.
method { crlf | stun }

Default: both methods enabled.

Specifies the method of keepalive messages supported by the CSCF.

crlf: “\r\n” string (CRLF packets) sent by UE

stun: STUN protocol messages (rfc3489-bis)
Usage:

Use this command to configure how the CSCF manages keepalive requests.
Example:
The following example sets the expire timer to 40 and the maximum retry parameter to 5:

    keepalive expire-timer
    40 max-retry 5

lawful-intercept

Enables Lawful Intercept (LI) in this CSCF service. Feature is disabled by default.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ]
    lawful-intercept

no

Disables the feature.
Usage:

Refer to the Lawful Intercept Configuration Guide for more information on LI.
li-packet-cable

Refer to the Lawful Intercept Configuration Guide for a description of this command.
max-sipmsg-size

Configures the maximum SIP message size.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    max-sipmsg-size limit[ default | no ] max-sipmsg-size

default | no

Returns/sets the maximum SIP message size to 4096 bytes.
limit

Default: 4096

Configures the SIP message size limit in bytes.

limit must be an integer from 1024 to 65535.

IMPORTANT:

Maximum SIP message size should be more than the message-max-size set in the CSCF Proxy-CSCF Configuration Mode.
Usage:

Use this command to configure the maximum SIP message size.
Example:
The following command limits the SIP message size to 4500 bytes:

    max-sipmsg-size 4500

media-bridging

Enables SDP modification that terminate media on CSCF. Feature is disabled by default.
Platform:

ASR 5000
Product:

SCM (P-CSCF)
Privilege:

Administrator
Syntax

    media-bridgingno media-bridging

no

Disables the feature.
Usage:

Use this command to allow termination of media on CSCF.
monitoring

Enables thresholds alerting for this CSCF service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    monitoring

Usage:

Use this command to enable thresholds alerting for this CSCF service.
nat-policy

Configures a NAT (Network Address Translation) policy for the service if the CSCF service is performing one of the following functions:

- CSCF services are run in bridging (Back-to-Back User Agent) mode
- A-BG is an Application-level Gateway (ALG) for NAT

Platform:

ASR 5000
Product:

SCM(CSCF, A-BG)
Privilege:

Administrator
Syntax

    nat-policy policy_name { private-address ( address ip_address_mask| default | range start_ip_address end_ip_address }  | bridge-network { address ip_address_mask | range start_ip_address end_ip_address }no nat-policy policy_name

no

Removes the specified NAT policy from the service.
policy_name

Specifies a name for the NAT policy.

policy_name must be from 1 to 79 alpha and/or numeric characters.
private-address { address ip_address_mask | default|range start_ip_address end_ip_address }

Specifies the private-address policy type for nat-pool.

address ip_address_mask: Address for nat-policy policy type for nat-pool. Specifies a combined IP address subnet mask bits to indicate what IP addresses the specific policy type applies to. ip_address_mask must be specified using the form “IP Address/Mask Bits” where the IP address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6, and the mask bits are a numeric value, which is the number of bits in the subnet mask.
default: Default for nat-policy policy type for nat-pool. Default is defined as the address range specified by rfc1918.

- 10.0.0.0 - 10.255.255.255 (10/8 prefix)
- 172.16.0.0 - 172.31.255.255 (172.16/12 prefix)
- 192.168.0.0 - 192.168.255.255 (192.168/16 prefix)

range start_ip_address end_ip_address: Range for nat-policy policy type for nat-pool.

- start_ip_address specifies the beginning of the range of addresses.
- end_ip_address specifies the end of the range of addresses .
- ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

bridge-network { address ip_address_mask | range start_ip_address end_ip_address }

Specifies the bridge-network policy type for S-CSCF bridging.

address ip_address_mask: Address for bridge-network policy type for S-CSCF bridging. Specifies a combined IP address subnet mask bits to indicate what IP addresses the specific policy type applies to. ip_address_mask must be specified using the form “IP Address/Mask Bits” here the IP address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6, and the mask bits are a numeric value, which is the number of bits in the subnet mask.
range start_ip_address end_ip_address: Range for bridge-network policy type for S-CSCF bridging.

- start_ip_address specifies the beginning of the range of addresses.
- end_ip_address specifies the end of the range of addresses.
- ip_address must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

Usage:

Generally, if a SIP packet has a VIA address (physical address that identifies where the service is located) different from the Source address, ALG functionality is invoked. Even if the VIA and Source addresses are the same, however, this command allows the ALG functionality to be started. For ALG to start, the VIA address should belong to one of the nat-policy address ranges.
Example:
The following command identifies the NAT policy named policy1 with a private-address policy type of 10.10.10.10 255.255.255.0:

    nat-policy policy1 private-address
    address 10.10.10.10 255.255.255.0

The following command identifies the NAT policy named policy2 with a private-address range policy type of 172.162.23.23 172.162.23.230:

    nat-policy policy2 private-address
    address 172.162.23.23 172.162.23.230

The following command identifies the NAT policy named policy3 with a default policy type:

    nat-policy policy3 private-address default

nat-pool

Configures a NAT (Network Address Translation) pool for the service if the CSCF service is performing one of the following functions:

- P-CSCF services are run in bridging (Back-to-Back User Agent) mode
- A-BG is an Application-level Gateway (ALG) for NAT

By default, no nat-pool name will be present.
Platform:

ASR 5000
Product:

SCM(P-CSCF, A-BG)
Privilege:

Administrator
Syntax

    nat-pool name pool_name [ signalling-pool signalling_pool_name ]no nat-pool name pool_name

no

Removes the NAT pool from the service.
name pool_name

Specifies the name of an existing NAT pool.

pool_name must be from 1 to 32 alpha and/or numeric characters.

IMPORTANT:

NAT pools are created in Context Configuration Mode with the ip pool command.
signalling-pool signalling_pool_name

Specifies the name of an existing IP pool from where IP addresses will be used to fill in signalling headers only.

signalling_pool_name must be from 1 to 32 alpha and/or numeric characters.

IMPORTANT:

If signalling-pool is not specified, service IP:port will be filled in signalling headers.
Usage:

Use this command to assign a NAT pool to the P-CSCF/A-BG service.
Example:
The following command identifies the NAT pool:

    nat-pool name pool2

policy

Enables or disables early media support and IBCF capability in P-CSCF/A-BG. In addition, configures Interim-Interval value for CSCF accounting sessions, overload response, and the congestion control threshold and tolerance values that are to be monitored on this CSCF service.
Platform:

ASR 5000
Product:

SCM (P-CSCF, A-BG)
Privilege:

Administrator
Syntax

    policy { accounting interim-interval value |  allow-early-media | ibcf-capability domain domain/name | overload [ drop | redirect IPv4_address1 [ weight weight1 ] [ IPv4_address2 [ weight weight2 ] ] ... | reject ] | threshold
    congestion-control { system-cpu-utilization percent | tolerance percent } }default policy { allow-early-media | overload | threshold congestion-control { system-cpu-utilization | tolerance } }no policy { accounting interim-interval | allow-early-media | ibcf-capability domain domain/name | overload [ redirect IPv4_address1 ] [ IPv4_address2 ] ... | threshold
    congestion-control { system-cpu-utilization | tolerance } }

default

Returns the command to the default settings. See keywords above for specific defaults.
no

Disables the specified functionality.
accounting interim-interval value

Default: Disabled

Used to configure Interim-Interval value for CSCF accounting sessions.

value can be configured to any integer value from 50 to 7200. This value is sent in the “Acct-Interim-Interval” AVP of the accounting message. Based on the response message from accounting server, Interim-Interval timer is started.
allow-early-media

Default: Enabled

Allows early media by doing QoS commit during QoS Authorization (with PCRF) in P-CSCF.
ibcf-capability domain domain/name

Enables IBCF capability to support Mx reference point in CSCF.

IBCF capability domain name must be entered using from 1 to 80 alpha and/or numeric characters.

IMPORTANT:

This CLI can be repeated to add/delete multiple entities to/from the ibcf-capability domain table. An ibcf-capability domain can be removed by using the no keyword; using the no keyword without giving any domain name will delete all entries from the list.
overload [ drop | redirect IPv4_address1 [ weight weight1 ] [ IPv4_address2 [ weight weight2 ] ] ... | reject ]

Configures the overload response for this policy. When the P-CSCF/A-BG becomes congested, this overload policy is used to drop/reject subsequent sessions or redirect them to another server.

drop: Specifies that upon policy overload, the system will drop the session.
redirect: Specifies that upon policy overload, the system will redirect the session to another CSCF.

- IPv4_address1 must be expressed in dotted decimal notation.
- weight weight1: Defines the priority of the redirect address.weight1 must be an integer from 1 to 10. Default is 1.

reject: Specifies that upon policy overload, the system will reject the session with 503 (Service Unavailable) SIP error response. This is the default setting.
threshold congestion-control { system-cpu-utilization percent | tolerance percent}
Enables congestion control. CSCF performs congestion control based on the memory usage inside every sessmgr at two levels.

- Level 1: For every new call/event received, the system checks if sessmgr memory-usage is above a threshold value (such as 95 percent). If it is, memory-congestion is triggered and new call messages are rejected with 500 SIP response. Memory congestion is disabled when memory usage drops by a tolerance value (default is 10 percent).
- Level 2: If the sessmgr usage reaches 100 percent, all newly received SIP messages are dropped at the socket layer in that sessmgr except for the BYE message. The new SIP messages are not processed until the memory reaches the threshold value (95 percent).

A trap is also generated whenever sessmgr is in congestion state

system-cpu-utilization percent: The average percent utilization of a CPU in a PSC/PSC2/PSC3 running the CSCF service as measured in 10 second intervals.

percent can be configured to any integer value from 0 to 100. This value becomes the upper threshold for triggering the CPU-based congestion for CSCF services. Default is 80

tolerance percent: The percentage under a configured threshold that dictates the point at which the condition is cleared.

percent is an integer value from 1 to 25. Default is 5
Usage:
Use this command to set the following policy for this CSCF service:

- Configure Interim-Interval value for CSCF accounting sessions.
- Set QoS support during either the initial SDP response or the 200OK response to the INVITE. When allow-early-media is enabled, QoS commit is done during initial SDP answer. When disabled, QoS commit is done during 200OK INVITE. By default, this command is enabled.
- Enable or disable IBCF capability.
- Define the response to an overload condition.
- Set thresholds to dictate the conditions for which congestion control is to be enabled and establish limits for defining the state of the CSCF service (congested or clear). The tolerance parameter establishes the threshold at which the condition is cleared.

IMPORTANT:

When congestion is triggered, new CSCF calls are not rejected.
Example:
The following command sets the upper threshold for CPU utilization for triggering congestion control at 90%.

    policy threshold congestion-control
    system-cpu-utilization 90

The following command sets the tolerance to its default value of 5.

    default policy threshold
    congestion-control tolerance

policy-name

Assigns a previously created service policy to this service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    policy-name nameno policy-name

no

Remove the assigned service policy from this service.
name

Specifies the name of the service policy being assigned to this service.

name must be from 1 to 79 alpha and/or numeric characters and be an existing policy name in the system. Service policies are created and maintained in the CSCF Policy Configuration Mode.
Usage:

Use this command to assign a service policy to this service. The policies defined in the service policy apply to all subscribers using this service. Service policies are created and maintained in the CSCF Policy Configuration Mode.
Example:
The following command assigns a service policy named serv_policy3 to this service:

    policy-name serv_policy3

proxy-cscf

Enables the Proxy-CSCF for the service and enters the Proxy-CSCF Configuration Mode. Default is disabled.
Platform:

ASR 5000
Product:

SCM (P-CSCF)
Privilege:

Administrator
Syntax

    [ no ] proxy-cscf

no

Disables the P-CSCF for the service.
Usage:

Use this command to enable the Proxy-CSCF feature and enter the Proxy-CSCF Configuration Mode.

Entering this command results in the following prompt:

    [context_name]hostname(config-cscf-service-proxy-cscf)#

Proxy-CSCF Configuration Mode commands are defined in the CSCF Proxy-CSCF Configuration Mode Commands chapter in this guide.

IMPORTANT:

The Proxy-CSCF is a license-enabled function of the Session Control Manager. Only one function (P-CSCF, S-CSCF, E-CSCF, SIP Proxy, or A-BG) can be enabled per service.
proxy-serving-cscf

This command is not supported in this release.
recurse-on-redirect-resp

Enables the 3xx recursion feature. If enabled, the service will send further invites to the contacts specified upon receiving a 3xx redirect response. Default is disabled.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] recurse-on-redirect-resp

no

Disables the 3xx recursion feature.
Usage:

When enabled and on receipt of a 3xx response, the service will collect the SIP URIs present in the Contact header(s) of 3xx and recursively contact each one of them until the call succeeds. The contacts are tried serially. There is a maximum implementation limit of 50 URIs. Each contact, in turn, can send a 3xx response. The service will honor them and append the new contacts. When disabled, the service treats a 3xx response as the final failure response and declares the call attempt “failed”. By default, this feature is disabled.
Example:
Enable recursion on 3xx:

    recurse-on-redirect-resp

Disable recursion on 3xx:

    no recurse-on-redirect-resp

reject-on-cnsa-failure

Enables rejection of messages on Core Network Service Authorization failure. Default is disabled.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] reject-on-cnsa-failure

no

Disables the rejection of messages on Core Network Service Authorization failure.
Usage:

Enables rejection of messages on Core Network Service Authorization failure. By default, this feature is disabled.

In a mobile originating case, S-CSCF checks for the presence of P-Preferred-Service (PPS) header. If the header is present, media profile authentication is successful and if the incoming ICSI (IMS Communication Service Identifier) value also matches with one of the values in the service_id list, then the request will be forwarded after replacing the PPS header with PAS (P-Asserted-Service). If media profile authentication fails, S-CSCF will check reject-on-cnsa-failure. If enabled, then call is rejected with 403 message. If disabled, a default ICSI is selected from the service_id list and will be put into PAS while forwarding the request by the S-CSCF on service authentication failure.

In PPS is not received by the S-CSCF and media profile authentication is successful, an ICSI from the service_id list, if present, is selected and will be added in PAS header. If media profile authentication fails, reject-on-cnsa-failure is checked. If enabled, call is rejected with 403 message. If disabled, PAS header is added if service_id list is present with an ICSI value.
Example:
Enable rejection of messages on Core Network Service Authorization failure:

    reject-on-cnsa-failure

Disable rejection of messages on Core Network Service Authorization failure:

    no reject-on-cnsa-failure

release-call-on-media-loss

Release call on detection of media loss.
Platform:

ASR 5000
Product:

SCM (P-CSCF, A-BG)
Privilege:

Administrator
Syntax

    release-call-on-media-loss
    media-type audiono release-call-on-media-loss

no

Disables the release of SIP calls upon the detection of media loss.
media-type audio

Enables the release of SIP calls upon the detection of media loss on media-type audio.
Usage:

Use this command to enable the release of SIP calls upon the detection of media loss.
Example:
Enables the release of SIP calls upon the detection of media loss:

    release-call-on-media-loss
    media-type audio

Enables the release of SIP calls upon the detection of media loss:

    no release-call-on-media-loss

rfc3261-proxy

Enables RFC3261 proxy (SIP Proxy) for this service and enters the SIP Proxy Configuration Mode. Default is disabled.
Platform:

ASR 5000
Product:

SCM (SIP Proxy)
Privilege:

Administrator
Syntax

    [ default | no ] rfc3261-proxy

default | no

Disables RFC3261 proxy in this service.
Usage:

Use this command to enable the Sip Proxy feature and enter the SIP Proxy Configuration Mode.

Entering this command results in the following prompt:

    [context_name]hostname(config-cscf-service-rfc3261-proxy)#

SIP Proxy Configuration Mode commands are defined in the CSCF SIP Proxy Configuration Mode Commands chapter in this guide.

IMPORTANT:

The SIP Proxy is a license-enabled function of the Session Control Manager. Only one function (P-CSCF, S-CSCF, E-CSCF, SIP Proxy, or A-BG) can be enabled per service.
serving-cscf

Enables Serving-CSCF for the service and enters the Serving-CSCF Command Mode. Default is disabled.
Platform:

ASR 5000
Product:

SCM (S-CSCF)
Privilege:

Administrator
Syntax

    [ no ] serving-cscf

no

Disables S-CSCF for the service.
Usage:

Use this command to enable the Serving-CSCF feature and enter the Serving-CSCF Configuration Mode.

Entering this command results in the following prompt:

    [context_name]hostname(config-cscf-service-serving-cscf)#

Serving-CSCF Configuration Mode commands are defined in the CSCF Serving-CSCF Configuration Mode Commands chapter in this guide.

IMPORTANT:

The Serving-CSCF is a license-enabled function of the Session Control Manager. Only one function (P-CSCF, S-CSCF, E-CSCF, SIP Proxy, or A-BG) can be enabled per service.
serving-cscf-list

Configure a list of Serving CSCFs and their capabilities.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] serving-cscf-list
    server { address address | domain domain } { capability value | port num { capability value } }

no

Removes an entry from this list.
server { address address | domain domain }

Specifies the S-CSCF server.

address address: IP addresses must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6.

domain domain: Domain names must be entered using from 1 to 80 alpha and/or numeric characters.
capability value

Specifies the capability of the S-CSCF server. value is assigned by the Service Provider and may be an integer from 1 to 999999.
port num

Specifies the port at which service is provided by the S-CSCF server. num may be an integer from 1 to 65535.
Usage:

Use this command to configure a list of Serving CSCFs and their capabilities.

IMPORTANT:

This command can be entered multiple times to identify multiple Serving CSCFs.
Example:
The following command adds a S-CSCF with an IP address of 1.2.3.4 and a capability value of 75 to this service’s list:

    serving-cscf-list server
    address 1.2.3.4 capability 75

session-timer

Configures the session expiry for sessions (Session will expire at the configured value unless refreshed.) and the minimum number of seconds in a session timer (session-expires) value the system will allow.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    session-timer { min-se sec [ session-expires sec ] | session-expires sec [ min-se sec ] }default session-timer [ min-se ] [ session-expires ]no session-timer

default

Returns the command to the default settings.
no

Disables the session timer.
min-se sec

Default: 90

Specifies the minimum number of seconds the system will allow a session-expires value in a session request.

sec must be an integer value between 90 and the value of the session-expires command.
session-expires sec

Default: 1800 (30 minutes)

Specifies the number of seconds a session is allowed exist before it expires.

sec must be an integer value between 90 and 18000.
Usage:

Use this command to set a session expiry value for all invites generated by the SCM and a minimum value for a session request session timer the system will allow. If a session is requested with a timer of less than this command’s value, the system will reject the request with a “422 Session Interval Too Small” response code.

Example

Example
The following command sets the session expiry for all sessions generated by the SCM to 60 minutes:

    session-timer session-expires 3600

strict-outbound

When enabled, the CSCF rejects registration without outbound parameters from an already registered AoR (the AoR would have included outbound parameters in a previous registration). When disabled, the CSCF allows registration without outbound parameters from the previously registered AoR.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] strict-outbound

no

Disables the feature. This is the default behavior.
Usage:

Use this command to reject registration from a previously registered AoR if the AoR fails to register with outbound parameters but included them in the previous registration.
subscriber-policy-override

Configures the system to allow the subscriber-based policy to override the service-based policy. Default is disabled.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ default | no ] subscriber-policy-override

default | no

Removes the subscriber policy override from the service.
Usage:

By default, if a conflict occurs between the subscriber-based policy and the service-based policy, the service policy takes precedence. Use this command to override the default behavior of the system and allow the subscriber-based policy to overrule the service policy.
subscription

Enables the registration event package for the service and configures a system-wide subscription lifetime for all subscribers to the service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    subscription package
    reg [ lifetime { default sec |  max sec [ default sec ] | min sec [ max sec ]  [ default sec ] } ][ default | no ] subscription
    package reg

default

Returns the command to the default settings.
no

Disables the registration event package for the service.
package reg [ lifetime { default sec | max sec ] | min sec }

default sec: Specifies the default amount of time that a subscription can exist on the system. sec must be an integer from 60 to max sec -1.

Default: 3761

IMPORTANT:

default sec must be < or = to max sec and > or = to min sec.

The following keywords are specific to the S-CSCF functionality:

max sec: Specifies the maximum amount of time that a subscription can exist on the system.

sec must be an integer from 60 to 2147483646.

Default: 86400

IMPORTANT:

max sec must be > or = to min sec.

min sec: Specifies the minimum amount of time that a subscription can exist on the system.

sec must be an integer from 60 to max sec -1.

Default: 60

IMPORTANT:

min sec must be < or = to max sec.
Usage:

Use this command to enable the registration event package for the service and control the amount of time subscriptions are allowed to exist on this service.

The system responds to subscriptions in the following manner:
Using default values:

- If a subscription with an expiration value lower than the service’s minimum (60) is received, the service will respond with a 423 Interval Too Small message.
- If a subscription with an expiration value higher than the service’s maximum (2147483646) is received, the service will automatically reduce the expiration value to the default value.

If a subscription is received missing the “Expires” value, or the value is malformed, the service will automatically respond with 3761 in the 200OK message.
Example:
The following command configures the maximum subscription lifetime to 43200 (12 hours):

    subscription package
    reg lifetime max 43200

support-content-type any

Validates Content-Type in this CSCF service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] support-content-type any

no

Disables the feature. If disabled, CSCF service rejects unsupported Content-Type with “415 Unsupported Media Type”.
Usage:

Use this command to either allow any type of Content-Type or reject unsupported Content-Type.
Example:
Allows any type of Content-Type for the CSCF service:

    support-content-type any

Rejects unsupported Content-Type for the CSCF service:

    no support-content-type any

tcp-proxy

Enables SIP TCP proxy for the CSCF service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    tcp-proxy [ port port_number ]no tcp-proxy

no

Disables SIP TCP proxy for the CSCF service
port port_number

Default: 5062

Specifies the port used for SIP TCP proxy connections.

port_number must be an integer from 1 to 65534.
Usage:

Use this command to enable SIP TCP proxy for the CSCF service.
Example:
Enables SIP TCP proxy for the CSCF service on port 5062:

    tcp-proxy port5062

Disables SIP TCP proxy for the CSCF service:

    no tcp-proxy

threshold

Enables thresholds alerting and configuration of thresholds for CSCF Service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    threshold { { call-setup-failures | call-total-active | error-no-resource |
    error-presence | error-reg-auth | error-tcp | invite-rcvd-rate | monitoring | reg-rcvd-rate |
    reg-total-active | route-failures } high_thresh [ clear low_thresh ] | monitoring }[ default | no ] threshold monitoring

default

Returns the command to the default settings.
no

Disables thresholds alerting for CSCF Service.
{ call-setup-failures | call-total-active | error-no-resource | error-presence | error-reg-auth | error-tcp | invite-rcvd-rate | reg-rcvd-rate | reg-total-active | route-failures } high_thresh clear low_thresh

call-setup-failures: Number of CSCF call setup failures.

Default: 0

call-total-active: Number of total active CSCF calls.

Default: 0

error-no-resource: Number of CSCF call setup failures due to no-resource.

Default: 0

error-presence: Number of CSCF Presence errors.

Default: 0

error-reg-auth: Number of CSCF Registration Authentication failures.

Default: 0

error-tcp: Number of CSCF call setup failures due to TCP error.

Default: 0

invite-rcvd-rate: Number of CSCF calls per polling interval.

Default: 0

reg-rcvd-rate: Number of CSCF registrations per polling interval.

Default: 0

reg-total-active: Number of total CSCF active registrations.

Default: 0

route-failures: Maximum number of route-failures, after which the alarm/alert will be raised. Default: 5

high_thresh: The high threshold number that must be met or exceeded within the polling interval to generate an alert or alarm. Can be configured to any integer value between 0 and 2000000 (0 and 60000 for route-failures).

clear low_thresh: The low threshold number that must be met or exceeded within the polling interval to clear an alert or alarm. Can be configured to any integer value between 0 and 2000000 (0 and 60000 for route-failures).

IMPORTANT:

This value is ignored for the Alert model. In addition, if this value is not configured for the Alarm model, the system assumes it is identical to the high threshold.
monitoring

Enables thresholds alerting for CSCF Service.
Usage:
Use this command to:

- enable/disable thresholds alerting for CSCF Service
- set an alert or an alarm when a threshold exceeds the configured level

Alerts or alarms are triggered for the number of registration reply errors on the following rules:

- Enter condition: Actual number > High Threshold
- Clear condition: Actual number < Low Threshold

Example:
The following command configures a route failures threshold of 1000 and a low threshold of 500 for a system using the Alarm thresholding model:

    threshold route-failures
    1000 clear 500

timeout

Sets timeout values for CSCF and SIP transactions.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    timeout { hss-wait sec | map-slr-response sec | policy-interface sec | sip { 3gpp-d sec | 3gpp-t1 msec | 3gpp-t2 sec | 3gpp-t4 sec | d sec | idle-tcp-connection msec  [ cleanup-timer msec ] | invite-expiry sec | t1 msec | t2 sec | t4 sec } }default timeout { hss-wait | no-answer | policy-interface | sip { 3gpp-d | 3gpp-t1 | 3gpp-t2 | 3gpp-t4 | d | idle-tcp-connection | invite-expiry | t1 | t2 | t4 } }

default

Returns the command to the default settings. See keywords above for specific defaults.
hss-wait sec

Default: 5

This timer is used by S-CSCF with HSS interface for timeout.

sec must be an integer from 0 to 2147483646.
no-answer sec

Default: 100

This timer is specially used for No-Answer Call Feature executed by S-CSCF. The timer will be started as soon as 180 Ringing response is received and No-Answer call feature is enabled. The value of this timer should be always less than INVITE Timeout used by DC-SIP.

sec must be an integer from 0 to 2147483646.
policy-interface sec

Default: 5

This timer is used by the P-CSCF/A-BG with Policy interface for timeout.

sec must be an integer from 0 to 2147483646.
sip { 3gpp-d sec | 3gpp-t1 msec | 3gpp-t2 sec | 3gpp-t4 sec | d sec | idle-tcp-connection msec [ cleanup-timer msec ] | invite-expiry sec | t1 msec | t2 sec | t4 sec }
Sets transaction and expiry timers for SIP.

- 3gpp-d sec: This timer is used to control the retransmission of 200OK messages to INVITEs after an ACK is sent. The ACK transaction is cleared after this period. This timer is applicable only for unreliable transport. sec must be an integer from 0 to 2147483646. Default: 64*T1 (128 seconds, recommended minimum)
- 3gpp-t1 msec: This timer is used to control the time interval between each retransmission. The interval doubles after each retransmission. This is used by P-CSCF/A-BG only when it sending message toward the UE. Example: T1, 2T1, 4T2, etc. This timer is applicable only for unreliable transport. msec must be an integer from 0 to 4294967294. Default: 2000 ms (2 secs, recommended minimum).
- 3gpp-t2 sec: This timer is used to control the period for which the request continues to get retransmitted. This is used by P-CSCF/A-BG only when it sending message toward the UE. This timer is applicable both for reliable and unreliable transport. sec must be an integer from 0 to 2147483646. Default: 16 seconds (recommended minimum).
- 3gpp-t4 sec: This timer is used to control the period for which the final response to non-invite transaction should be buffered. The buffered response for the retransmitted non-invite request should be sent within that interval. This timer is applicable only for unreliable transport. sec must be an integer from 0 to 2147483646. Default: 17 seconds (recommended minimum).
- d sec: This timer is used to control the retransmission of 200OK to INVITE after ACK is sent. The ACK transaction will be cleared after this interval. This timer is applicable only for unreliable transport. sec must be an integer from 0 to 2147483646. Default: 64*T1 (32 seconds, recommended minimum)
- idle-tcp-connection msec: This timer is used for closing idle TCP connections. If there is not activity in the TCP connection for the configuration duration, then the connection will be closed. msec must be an integer from 1000 (recommended minimum) to 4294967294. Default: 42000 milliseconds.
- cleanup-timer msec: This timer is used to control how often to check for idle TCP connections. msec must be an integer from 2000 to 2147483646. Default: 2000 milliseconds.
- invite-expiry sec: This timer is used by SIP while acting as UA Role and no final response is received for the INVITE request sent. This timer is applicable for both reliable and unreliable transport. sec must be an integer from 0 to 2147483646. Default: 100 seconds (recommended minimum).
- t1 msec: Specifies the time interval (in microseconds) between each retransmission. The interval doubles after each retransmission, for example: T1, 2T1, 4T2, etc. This timer is applicable only for unreliable transport. msec must be an integer from 0 to 2147483646. Default: 500 milliseconds (recommended minimum).
- t2 sec: This timer is used to control the period for which the request keeps getting retransmitted. This timer is applicable both for reliable and unreliable transport. sec must be an integer from 0 to 2147483646. The recommended minimum value for this parameter is 4 seconds. Default: 64*T1 (32 seconds)
- t4 sec: This timer is used to control the period for which the final response to non-invite transaction should be buffered so as to send the buffered response for the retransmitted non-invite request within that interval. This timer is applicable only for unreliable transport. sec must be an integer from 0 to 2147483646. Default: 5 seconds (recommended minimum).

Usage:

Use this command to configure SIP Stack timers and CSCF service specific timers.
Example:
The following command sets the SIP d timer to 64 seconds:

    timeout sip d 64

transport-switching

Sets the message size that triggers a transport protocol switch.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    transport-switching
    policy protocol tcp trigger msg-size sizedefault transport-switching
    policy protocol tcp trigger msg-size

default

Returns the size of the SIP message beyond which transport changes to TCP to 1300 bytes.
policy protocol tcp trigger msg-size size

Default: 1300

Specifies the size of the SIP message beyond which transport changes to TCP.

size can be configured to any integer value between 1300 and 65535.
Usage:

Use this command to configure the size of the SIP message beyond which transport changes to TCP.
Example:
Switch to TCP transport protocol when the SIP message size is 4000 bytes or more:

    transport-switching
    policy protocol tcp trigger msg-size 4000

trusted-domain-entity

Adds trusted network nodes (or entities) to a table used by this service to identify those nodes that can be trusted with subscriber information.
Platform:

ASR 5000
Product:

SCM (S-CSCF)
Privilege:

Administrator
Syntax

    trusted-domain-entity address [ foreign-network ] [ private-network ]no trusted-domain-entity address

no

Removes an entry from this service’s trusted domain table.
address

Specifies the IP address of the network node identified as a trusted entity by this service. address must be either an IP address or a domain name. IP addresses must be expressed in dotted decimal notation for IPv4 or colon notation for IPv6. Domain names must be entered using from 1 to 80 alpha and/or numeric characters.
foreign-network

Entity belongs to Foreign Network.
private-network

Entity belongs to Private Network.
Usage:

Use this command to identify to the service the network entities that can be trusted with subscriber information by this service.

IMPORTANT:

This command can be entered multiple times to identify multiple trusted network entities. In StarOS v12.x and earlier, a maximum of 50 entries can be configured per CSCF service.
Example:
The following command adds a network node with an IP address of 1.2.3.4 to this service’s trusted domain table:

    trusted-domain-entity 1.2.3.4