# RADIUS Dictionaries and Attribute Definitions

This chapter presents information on RADIUS dictionary types and attribute definitions.

For the quick reference table, see the RADIUS Attribute Quick Reference appendix.

RADIUS Dictionaries

This section presents information on RADIUS dictionary types.

Dictionary Types

The CLI command to specify the RADIUS dictionary is:

    radius dictionary [ 3gpp | 3gpp2 | 3gpp2-835 | custom XX | standard | starent | starent-835 | starent-vsa1 | starent-vsa1-835 ]

Keyword | Description
--- | ---
custom XX | These dictionaries can be customized. Customization information can be obtained by contacting your local service representative. XX is the integer value of the custom dictionary. IMPORTANT: RADIUS dictionary custom23 should be used in conjunction with Enhanced Charging Service (ECS).
standard | This dictionary consists only of the attributes specified in RFC 2865, RFC 2866, and RFC 2869. It also supports 3GPP release 4 and 3GPP Release 5 - extended QoS format.
3gpp | This dictionary consists not only of all of the attributes in the standard dictionary, but also all of the attributes specified in 3GPP 32.015.
3gpp2 | This dictionary consists of all of the attributes in the standard dictionary, and all of the attributes specified in IS-835-A.
3gpp2-835 | This dictionary consists of all of the attributes in the standard dictionary, and all of the attributes specified in IS-835.
starent-vsa1 | This dictionary consists of the 3GPP2 dictionary, and includes the vendor-specific attributes (VSAs) as well. The VSAs in this dictionary support a one-byte wide VSA Type field in order to support certain RADIUS applications. The one-byte limit allows support for only 256 VSAs (0 - 255) as shown in the following figure. This is the default dictionary. IMPORTANT: In 12.0 and later releases, no new RADIUS/Diameter attributes can be added to the starent-vsa1 dictionary. If there are any new attributes to be added, these can be added to the starent dictionary.
starent-vsa1-835 | This dictionary consists of the 3GPP2-835 dictionary, and includes the vendor-specific attributes (VSAs) as well. The VSAs in this dictionary support a one-byte wide VSA Type field in order to support certain RADIUS applications. The one-byte limit allows support for only 256 VSAs (0 - 255) as shown in the following figure.
starent | This dictionary consists of all of the attributes in the starent-vsa1 dictionary and incorporates additional VSAs by using a two-byte VSA Type field as shown in the following figure. This dictionary is the master-set of all of the attributes in all of the dictionaries supported by the system.
starent-835 | This dictionary consists of all of the attributes in the starent-vsa1-835 dictionary and incorporates additional VSAs by using a two-byte VSA Type field. This dictionary is the master-set of all of the attributes in all of the -835 dictionaries supported by the system.

Figure 1. Difference in VSA Value Lengths per Dictionary

IMPORTANT:

Customer-specific attributes are not documented in this reference. For information on customer-specific attributes, contact your Cisco account representative.

IMPORTANT:

The length documented for each attribute is the length of the attribute’s Value field (data portion) and not length of the attribute (Type + Length + Value fields).

RADIUS Attribute Definitions

This section presents RADIUS attribute definitions.

IMPORTANT:

RADIUS attributes received by the system from the RADIUS server always take precedence over local-subscriber attributes and parameters configured on the system.
3GPP-Allocate-IPType

This attribute indicates whether the Access-Request is sent for user authentication only and/or for allocation of IPv4 and/or IPv6 address.

Type

26

Vendor ID

10415

VSA Type

27

Length

4

Value

Enumerated integer. Supported values are:

- none = 0
- ipv4 = 1
- ipv6 = 2
- ipv4-or-ipv6 = 3

3GPP-CAMEL-Charging-Info

This attribute contains the received CAMEL charging information. CAMEL charging information is applicable to GGSN.

Type

26

Vendor ID

10415

VSA Type

24

Length

1–255

Value

String
3GPP-CG-Address

This attribute identifies the charging gateway address.

Type

26

Vendor ID

10415

VSA Type

4

Length

4

Value

IPv4 address
3GPP-Charging-ID

This attribute contains the charging ID for the PDP Context. This together with the GGSN-Address constitutes a unique identifier for the PDP context.

Type

26

Vendor ID

10415

VSA Type

2

Length

4

Value

Unsigned integer
3GPP-Chrg-Char

This attribute contains the charging characteristics for this PDP Context received in the Create PDP Context Request Message (only available in R99 and later releases).

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

10415

VSA Type

13

Length

4

Value

Opaque value
3GPP-GGSN-Address

This attribute contains IPv4 address of the GGSN.

Type

26

Vendor ID

10415

VSA Type

7

Length

4

Value

IPv4 address
3GPP-GGSN-IPv6-Address

For GGSN, it represents the GGSN IPv6 address that is used by the GTP control plane for thecontext establishment. For P-GW, it represents the P-GW IPv6 address that is used on S5/S8, S2a, S2b, or S2c control plane for the IP-CAN session establishment.

Type

26

Vendor ID

10415

VSA Type

16

Length

16

Value

Opaque value
3GPP-GGSN-Mcc-Mnc

This attribute contains the MCC-MNC of the network the GGSN belongs to.

Type

26

Vendor ID

10415

VSA Type

9

Length

1–6

Value

Opaque value
3GPP-IMEISV

This attribute identifies the International Mobile Equipment Identity and Software Version (IMEISV) number received from the mobile node (MN). It is sent in RADIUS authentication and accounting messages by GGSN.

Type

26

Vendor ID

10415

VSA Type

20

Length

16

Value

Opaque value
3GPP-IMSI

This attribute contains the IMSI identifying the mobile unit.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

10415

VSA Type

1

Length

1–15

Value

Opaque value
3GPP-IMSI-Mcc-Mnc

This attribute contains the MCC and MNC extracted from the user's IMSI (first 5 or 6 digits, as applicable from the presented IMSI).

Type

26

Vendor ID

10415

VSA Type

8

Length

1–6

Value

Opaque value
3GPP-IPv6-DNS-Servers

This attribute contains list of IPv6 DNS server addresses.

Type

26

Vendor ID

10415

VSA Type

17

Length

16–240

Value

Opaque value
3GPP-MS-TimeZone

This attribute indicates the offset between universal time and local time in steps of 15 minutes of where the MS currently resides.

Type

26

Vendor ID

10415

VSA Type

23

Length

2

Value

Opaque value
3GPP-Negotiated-DSCP

This attribute is used to mark IP packets of PDP context on the Gi interface.

Type

26

Vendor ID

10415

VSA Type

26

Length

1

Value

Unsigned integer
3GPP-Negotiated-QoS-Profile

This attribute specifies the QoS profile to be used for the subscriber.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

10415

VSA Type

5

Length

In 10.2 and earlier releases: 1–35

In 11.0 and later releases: 1–39

Value

Opaque value
3GPP-NSAPI

This attribute specifies the value of the NSAPI of the PDP context that the RADIUS message is related to. It is encoded as its hexadecimal representation, using 1 UTF-8 encoded digit.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

10415

VSA Type

10

Length

1

Value

Opaque value
3GPP-Packet-Filter

This compound attribute specifies the Packet Filter used for the PDP context.

Type

26

Vendor ID

10415

VSA Type

25

Length

65

Value

Contains the following subattributes:
Identifier

Identifier of the packet filter.

Type

1

Length

1

Value

Unsigned integer
Eval-Precedence

Evaluation precedence of the packet filter.

Type

2

Length

1

Value

Unsigned integer
Length

Length of the packet filter.

Type

3

Length

1

Value

Unsigned integer
Direction

Direction of the packet filter.

Type

4

Length

1

Value

Unsigned integer
IPv4-Address-Type

This is a compound attribute specifying the IPv4 source address and netmask if the direction is downlink, or destination address and netmask if the direction is downlink, or destination address and netmask if the direction is uplink.

Type

5

Length

8

Value

Contains the following two subattributes:
Address

This attribute contains source address if direction value is set to Downlink, and destination address if direction value is set to Uplink.

Type

1

Length

4

Value

IPv4 address
Netmask

This attribute contains netmask of the IPv4 address.

Type

2

Length

4

Value

IPv4 address
IPv6-Address-Type

This is a compound attribute specifying the IPv6 source address and netmask if the direction is Downlink, or Destination Address and Netmask if the direction is Downlink, or Destination Address and Netmask if the direction is Uplink.

Type

6

Length

32

Value

Contains the following two subattributes:
Address

This attribute contains source address if direction value is set to Downlink, and destination address if direction value is set to Uplink.

Type

1

Length

16

Value

Opaque value
Netmask

This attribute contains the Netmask of the IPv6 address.

Type

2

Length

16

Value

Opaque value
Protocol-Identifier-Or-Next-Header

Specifies the IPv4 Protocol Identifier or IPv6 Next Header.

Type

7

Length

1

Value

Unsigned integer
Destination-Port

Specifies the Destination Port number of the packet filter.

Type

8

Length

2

Value

An integer in network byte order
Destination-Port-Range

This is a compound attribute and specifies the destination port range.

Type

9

Length

4

Value

Contains the following two subattributes:
Lower

Specifies the lower range of the destination port of the packet filter.

Type

1

Length

2

Value

Unsigned integer
Higher

Specifies the higher range of the destination port of the packet filter.

Type

2

Length

2

Value

Unsigned integer
Source-Port

Specifies the source port number of the packet filter.

Type

10

Length

2

Value

Unsigned integer
Source-Port-Range

Specifies the source port range.

Type

11

Length

4

Value

Contains the following two subattributes:
Lower

Specifies lower range of the source port of the packet filter.

Type

1

Length

2

Value

Unsigned integer
Higher

Specifies higher range of the source port of the packet filter.

Type

2

Length

2

Value

Unsigned integer
Security-Parameter-Index

Specifies the IPSec Security Parameter Index(IPv6).

Type

12

Length

4

Value

Unsigned integer
Type-Of-Service

This is a compound attribute and specifies the Type of Service/ Traffic Class.

Type

13

Length

2

Value

Contains the following two subattributes:
Value

Specifies the Type of Service/Traffic Class Value.

Type

1

Length

1

Value

Unsigned integer
Mask

Specifies the Type of Service/Traffic Class Mask.

Type

2

Length

1

Value

Unsigned integer
Flow-Label

Specifies the IPv6 Flow Label.

Type

14

Length

3

Value

Opaque value
3GPP-PDP-Type

This attribute identifies the PDP Context type.

Type

26

Vendor ID

10415

VSA Type

3

Length

4

Value

Enumerated integer. Supported values are:

- ipv4 = 0
- ppp = 1
- ipv6 = 2
- ipv4-or-ipv6 = 3

3GPP-RAT-Type

This attribute indicates which Radio Access Technology is currently serving the UE.

Type

26

Vendor ID

10415

VSA Type

21

Length

1

Value

Opaque value
3GPP-Selection-Mode

This attribute contains the selection mode for this PDP Context received in the Create PDP Context Request message as an UTF-8 encoded character.

Type

26

Vendor ID

10415

VSA Type

12

Length

1

Value

Opaque value
3GPP-Session-Stop-Ind

The presence of this attribute indicates to the AAA server that the last PDP context of a session is released and that the PDP session has been terminated.

Type

26

Vendor ID

10415

VSA Type

11

Length

1

Value

Opaque value
3GPP-SGSN-Address

This attribute contains IPv4 address of the SGSN.

Type

26

Vendor ID

10415

VSA Type

6

Length

4

Value

IPv4 address
3GPP-SGSN-IPv6-Address

For GGSN, it represents the SGSN IPv6 address that is used by the GTP control plane for the handling of control messages. For P-GW, it represents the IPv6 address of the S-GW, trusted non-3GPP IP access or ePDG that is used on S5/S8, S2a, or S2b for the handling of control messages. The address may beused to identify the PLMN to which the user is attached.

Type

26

Vendor ID

10415

VSA Type

15

Length

16

Value

Opaque value
3GPP-SGSN-Mcc-Mnc

For GPRS the MCC and the MNC of the SGSN.

Type

26

Vendor ID

10415

VSA Type

18

Length

1–6

Value

String
3GPP-Teardown-Indicator

If this value is set to 1 in disconnect-request, the whole correlated sessions would be disconnected.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

16

Vendor ID

10415

VSA Type

19

Length

1

Value

Opaque value
3GPP-User-Location-Info

GTP user location information attribute for the subscriber session.

Type

26

Vendor ID

10415

VSA Type

22

Length

In 10.2 and earlier releases: 8

In 11.0, 12.0 and 12.1 releases: 37

Value

Opaque value
3GPP2-835-Release-Indicator

3GPP2-895- Standard Release-Indicator, reason/cause for session release.

Type

26

Vendor ID

5535

VSA Type

24

Length

4

Value

Enumerated integer. Supported values are:

- Unknown = 0
- PPP-Timeout = 1
- Handoff = 2
- PPP-Termination = 3
- Mobile-IP-Registration-Failure = 4
- Active-To-Dormant = 5

3GPP2-Acct-Session-Time

The total amount of time spent in the Active state, in seconds. This attribute has the same type as Acct-Session-Time, and thus conforms to IS-835.

Type

46

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
3GPP2-Active-Time

The total period of time spent in the Active state, in seconds.

Type

26

Vendor ID

5535

VSA Type

49

Length

4

Value

Unsigned integer
3GPP2-Active-Time-Corrected

3GPP2 Active session time value.

Type

26

Vendor ID

5535

VSA Type

49

Length

4

Value

Unsigned integer
3GPP2-Airlink-Record-Type

This attribute indicates the most recent type of Airlink Record to be received for this subscriber's connection.

Type

26

Vendor ID

5535

VSA Type

40

Length

4

Value

Enumerated integer. Supported values are:

- Connection-Setup = 1
- Active-Start = 2
- Active-Stop = 3
- SDB = 4
- BCMCS-Connection-Setup = 5
- BCMCS-Active-Start = 6
- BCMCS-Active-Stop = 7

3GPP2-Airlink-Sequence-Number

This represents the sequence number of an Airlink Record and is incremented (modulo 256) by the PCF for each Airlink Record. The sequence number is unique for a given RP Session ID, PCF ID, and MSID.

Type

26

Vendor ID

5535

VSA Type

42

Length

4

Value

Unsigned integer
3GPP2-Air-QOS

This attribute identifies airlink QOS associated with the user data. The least significant 4 bits hold the QOS priority as defined in C.S0001-A in the subscriber profile.

Type

26

Vendor ID

5535

VSA Type

39

Length

4

Value

Unsigned integer
3GPP2-Allowed-Diffserv

This attribute specifies if the user is able to mark packets with AF and/or EF. The Max Class specifies that the user may mark packets with a Class Selector Code Point that is less then or equal to Max Class.

Type

26

Vendor ID

5535

VSA Type

73

Length

24

Value

Contains the following three subattributes:
Flags

Allowed DSCP flag.

Type

1

Length

2

Value

Enumerated integer. Supported values are:

- Allow_AF_EF_Exp = 0xE000
- Allow_AF_EF = 0xC000
- Allow_AF_Exp = 0xA000
- Allow_EF_Exp = 0x6000
- Allow_AF = 0x8000
- Allow_EF = 0x4000
- Allow_Exp = 0x2000
- Allow_None = 0x0

Max-Class

Allowed max dscp.

Type

2

Length

2

Value

Enumerated integer. Supported values are:

- Best-Effort = 0x0
- AF11 = 0x2800
- AF12 = 0x3000
- AF13 = 0x3800
- AF21 = 0x4800
- AF22 = 0x5000
- AF23 = 0x5800
- AF31 = 0x6800
- AF32 = 0x7000
- AF33 = 0x7800
- AF41 = 0x8800
- AF42 = 0x9000
- AF43 = 0x9800
- EF = 0xb800
- Class1 = 0x2000
- Class2 = 0x4000
- Class3 = 0x6000
- Class4 = 0x8000
- Class5 = 0xa000
- Class6 = 0xc000
- Class7 = 0xe000

RT-Marking

Allowed max dscp rev. tun.

Type

3

Length

2

Value

Enumerated integer. Supported values are:

- Best-Effort = 0x0
- AF11 = 0x2800
- AF12 = 0x3000
- AF13 = 0x3800
- AF21 = 0x4800
- AF22 = 0x5000
- AF23 = 0x5800
- AF31 = 0x6800
- AF32 = 0x7000
- AF33 = 0x7800
- AF41 = 0x8800
- AF42 = 0x9000
- AF43 = 0x9800
- EF = 0xb800
- Class1 = 0x2000
- Class2 = 0x4000
- Class3 = 0x6000
- Class4 = 0x8000
- Class5 = 0xa000
- Class6 = 0xc000
- Class7 = 0xe000

3GPP2-Allowed-Persistent-TFTs

This attribute displays the 3GPP2 Allowed Persistent Traffic Flow Templates.

Type

26

Vendor ID

5535

VSA Type

89

Length

4

Value

Unsigned integer
3GPP2-Alternate-Billing-ID

This attribute is currently not supported.
3GPP2-Always-On

This attribute, when set to Active, indicates that the subscriber's session should be kept up regardless of the idle time as long as the subscriber is reachable. Reachability is ascertained using LCP keepalive messages.

Type

26

Vendor ID

5535

VSA Type

78

Length

4

Value

Enumerated integer. Supported values are:

- Inactive = 0
- Active = 1

3GPP2-Auth-Flow-Profile-Id

This compound attribute is a list of flow profile IDs.

Type

26

Vendor ID

5535

VSA Type

131

Length

6

Value

Contains the following three subattributes:
Profile-Id-Forward

This attribute specifies a list of Forward Flow Profile IDs that the user is allowed to specify/request in a QoS Sub Blob.

Type

1

Length

2

Value

Unsigned integer
Profile-Id-Reverse

This attribute specifies a list of Reverse Flow Profile IDs that the user is allowed to specify/request in a QoS Sub Blob.

Type

2

Length

2

Value

Unsigned integer
Profile-Id-Bi-Direction

This attribute specifies the list of Bi-Direction Flow Profile IDs that the user is allowed to specify/request in a QoS Sub Blob.

Type

3

Length

2

Value

Unsigned integer
3GPP2-Auth-QoS-Profile-Id

This attribute specifies the authorized QOS profile ID.

Type

26

Vendor ID

5535

VSA Type

131

Length

1

Value

1
3GPP2-Bad-PPP-Frame-Count

The total number of PPP frames from the MS dropped by the PDSN due to uncorrectable errors.

Type

26

Vendor ID

5535

VSA Type

25

Length

4

Value

Unsigned integer
3GPP2-BCMCS-Auth-Parameters

This is a grouped AVP with Authentication signature, Sequence number, and timestamp required to validate each flow in a BCMCS flow registration request. Each flow is validated using the procedure described in 3GPP2 standard C.S0054-0_v1.0. This information is configured on a per subscriber basis.

Type

26

Vendor ID

5535

VSA Type

99

Length

38

Value

Contains the following three subattributes:
BAK-Sequence-Number

Type

1

Length

1

Value

Opaque value
Timestamp

Type

2

Length

33

Value

Opaque value
Auth-Signature

Type

3

Length

4

Value

Unsigned integer
3GPP2-BCMCS-BSN-Session-Info

This is a grouped AVP containing information about the established flows. This includes the multicast address, port, compression status of the flow, and the content server address.

Type

26

Vendor ID

5535

VSA Type

103

Length

46

Value

Contains the following 11 subattributes:
Flow-ID

Type

1

Length

2-4

Value

Opaque value
Mcast-IP-Addr

Type

2

Length

4

Value

IPv4 address
Mcast-Port

Type

3

Length

2

Value

Unsigned integer
Header-Compression-Algorithm

Type

4

Length

4

Value

Enumerated integer. Supported values are:

- No_header_compression = 0
- ROHC_U_Mode = 1

CID-Type-Attribute

Type

5

Length

4

Value

Enumerated integer. Supported values are:

- Small_CID = 0
- Large_CID = 1

MAX-CID

Type

6

Length

2

Value

Unsigned integer
Compression-Profile

Type

7

Length

2

Value

Unsigned integer
MAX-Header-Size

Type

8

Length

2

Value

Unsigned integer
MRRU

Type

9

Length

2

Value

Unsigned integer
Content-Server-Source-IP-Address

Type

10

Length

4

Value

IPv4 address
Content-Server-Source-IPv6-Address

Type

11

Length

16

Value

Opaque value
3GPP2-BCMCS-Capability

This AVP defines the specific BCMCS protocol revision the PDSN supports.

Type

26

Vendor ID

5535

VSA Type

101

Length

4

Value

Contains the following subattribute:
BCMCS-Protocol-Revision

Type

1

Length

2

Value

Enumerated integer. Supported value is:

- Release_0 = 1

3GPP2-BCMCS-Common-Session-Info

This is a grouped AVP which specifies the program start time, end time and the allowed registration time on a per flow basis.

Type

26

Vendor ID

5535

VSA Type

102

Length

18

Value

Contains the following five subattributes:
Flow-ID

Type

1

Length

2–4

Value

Opaque value
Program-Start-Time

Type

2

Length

4

Value

Unsigned integer
Program-End-Time

Type

3

Length

4

Value

Unsigned integer
Program-Allowed-Registration-Time

Type

4

Length

4

Value

Unsigned integer
Auth-Required-Flag

Type

5

Length

2

Value

Enumerated integer. Supported values are:

- Authorization_not_required = 0
- Authorization_required = 1

3GPP2-BCMCS-Flow-ID

This attribute specifies the BCMCS_FLOW_ID.

Type

26

Vendor ID

5535

VSA Type

100

Length

2–4

Value

String
3GPP2-BCMCS-Flow-Transmit-Time

The total BCMCS flow transmission time in seconds.

Type

26

Vendor ID

5535

VSA Type

107

Length

4

Value

Unsigned integer
3GPP2-BCMCS-Mcast-IP-Addr

This attribute contains the multicast IP address of the BCMCS flow as it would appear in the source or destination field of an IP header.

Type

26

Vendor ID

5535

VSA Type

109

Length

4

Value

IPv4 address
3GPP2-BCMCS-Mcast-Port

The multicast port for the BCMCS flow.

Type

26

Vendor ID

5535

VSA Type

110

Length

2

Value

Unsigned integer
3GPP2-BCMCS-Reason-Code

This attribute specifies the reason to send the RADIUS Access-Accept message.

Type

26

Vendor ID

5535

VSA Type

105

Length

1

Value

Opaque value
3GPP2-BCMCS-RN-Session-Info

This is a grouped AVP which contains the encryption mechanism, BAK (Broadcast access key), BAK_ID, BAK expire time and authorization required flag. This attribute specifies the session information that needs to be known only by the RN.

Type

26

Vendor ID

5535

VSA Type

104

Length

31

Value

Contains the following six subattributes:
Flow-ID

Type

1

Length

2-4

Value

Opaque value
BCMCS-Encryption-Mechanism-Attribute

Type

2

Length

2

Value

Enumerated integer. Supported values are:

- High_layer_encryption_in_CS = 0
- Link_layer_encryption_in_RN = 1

BCMCS-BAK-ID-Attribute

Type

3

Length

1

Value

Unsigned integer
BCMCS-BAK

Type

4

Length

16

Value

Opaque value
BCMCS-BAK-Expire-Time

Type

5

Length

4

Value

Unsigned integer
BCMCS-Session-Bandwidth-attribute

Type

6

Length

2

Value

Unsigned integer
3GPP2-BCMCS-Subnet-VSA-Format

This attribute is deprecated.
3GPP2-Beginning-Session

3GPP2 Beginning Session will be TRUE or FALSE depending on if this is a new session.

Type

26

Vendor ID

5535

VSA Type

51

Length

4

Value

Enumerated integer. Supported values:

- False = 0
- True = 1

3GPP2-BSID

The base station ID.

Type

26

Vendor ID

5535

VSA Type

10

Length

6–12

Value

Opaque value
3GPP2-Carrier-ID

A 5 or 6-byte identifier of the visited PDSN comprising of a 3 byte Mobile Country Code (MCC) followed by a 2 or 3 byte Mobile Network Code (MNC) of the visited carrier. This value is configured locally in the visited carrier's PDSN.

Type

26

Vendor ID

5535

VSA Type

142

Length

5–6

Value

Opaque value
3GPP2-Comp-Tunnel-Indicator

This attribute indicates the invocation of a compulsory tunnel established on behalf of the MS for providing private network and/or ISP access during a single packet data connection. Normal PPP sessions will show No Tunnel. L2TP, IPinIP, and IP-GRE tunnels will show Non-Secure-Tunnel. IPSEC support will show Secure-Tunnel.

Type

26

Vendor ID

5535

VSA Type

23

Length

4

Value

Enumerated integer. Supported values are:

- No Tunnel = 0
- Non-Secure-Tunnel = 1
- Secure-Tunnel = 2

3GPP2-Container

A compound attribute that encapsulates the User Data Record for an Airlink Event.

Type

26

Vendor ID

5535

VSA Type

6

Length

Varies

Value

Embedded attributes as defined in “Wireless IP Network Standard – 3GPP2.P.S0001-A-1” [6].

Format of the 3GPP2-Container attribute:
Embedded attributes will contain 0 or 1 of the following attributes:

- 3GPP2-User-Zone
- 3GPP2-Air-QOS
- NAS-IP-Address
- 3GPP2-Serving-PCF
- 3GPP2-BSID
- Acct-Output-Octets
- Acct-Output-Gigawords
- Acct-Input-Octets
- Acct-Input-Gigawords
- SNA1-PPP-Unfr-data-In-Oct
- SNA1-PPP-Unfr-data-Out-Oct
- 3GPP2-Bad-PPP-Frame-Count
- 3GPP2-Active-Time
- 3GPP2-Number-Active-Transitions
- 3GPP2-SDB-Input-Octets
- 3GPP2-SDB-Output-Octets
- 3GPP2-Num-SDB-Input
- 3GPP2-Num-SDB-Output
- 3GPP2-Num-Bytes-Received-Total
- 3GPP2-MIP-Sig-Octet-Count-In
- 3GPP2-MIP-Sig-Octet-Count-Out

Embedded attributes inside the 3GPP2-Container attribute have the same format as those outside the 3GPP2-Container attribute.
3GPP2-Correlation-Id

This attribute contains an ID that correlates all accounting sessions authorized for this NAI by this access request.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

26

Vendor ID

5535

VSA Type

44

Length

1–253

Value

String
3GPP2-Correlation-Id-Old

Custom-11 style correlation ID.

Type

26

Vendor ID

5535

VSA Type

40

Length

1–251

Value

Opaque value
3GPP2-DCCH-Frame-Size

Specifies the DCCH frame size.

Type

26

Vendor ID

5535

VSA Type

50

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- 5s = 1
- 20ms = 2

3GPP2-Diff-Service-Class-Option

This is the DSCP (Differentiated Service Code Point) value as defined in the 3GPP2 standard. The DSCP values are assigned for different classes of traffic so that each traffic class can be given different priorities (QoS).

Type

26

Vendor ID

5535

VSA Type

5

Length

4

Value

Unsigned integer
3GPP2-Disconnect-Reason

This attribute indicates the reason for disconnecting the user. This attribute may be present in the RADIUS Disconnect-request Message from Home RADIUS server to the PDSN.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

5535

VSA Type

96

Length

4

Value

Enumerated integer. Supported values are:

- MS_Mobility_Detection = 1
- All other values are reserved.

3GPP2-DNS-Server-IP-Address

DNS server IP address. Used in custom dictionary.

Type

26

Vendor ID

5535

VSA Type

117

Value

Contains the following four subattributes:
Primary-DNS-Server-IP

Primary DNS Server IP address.

Type

1

Length

4

Value

IPv4 address
Secondary-DNS-Server-IP

Secondary DNS Server IP address.

Type

2

Length

4

Value

IPv4 address
Flag

M bit set to 1 indicates to the PDSN that primary and secondary IP addresses provided by the Home RADIUS server should override the primary and secondary IP addresses provided also by the visited RADIUS server.

Type

3

Length

1

Value

Unsigned integer
Entity-Type

Network Entity that inserted in the DNS server ID address. Currently the following types are defined. HAAA = 1, VAAA = 1.

Type

4

Length

1

Value

Unsigned integer
3GPP2-DNS-Server-IPV6-Addr

DNS server IPv6 address.

Type

26

Vendor ID

5535

VSA Type

214

Length

0–50

Value

Contains the following four subattributes:
Primary-DNS-Server-IPV6

Primary DNS server IPv6 address.

Type

1

Length

2

Value

Opaque value
Secondary-DNS-Server-IPV6

Secondary IPv6 DNS server IP address.

Type

2

Length

2

Value

Opaque value
Flag-IPV6

M bit set to 1 indicates to the PDSN that Primary and Secondary IPv6 addresses provided by the Home RADIUS server should override the Primary and Secondary IPv6 addresses provided also by the visited RADIUS server.

Type

3

Length

1

Value

Unsigned integer
Entity-Type-IPV6

Network Entity that inserted in the DNS server ID address. Either HAAA = 1, VAAA = 1.

Type

4

Length

1

Value

Unsigned integer
3GPP2-DNS-Update-Required

This attribute indicates whether the HA needs to send the DNS update to the DNS server.

Type

26

Vendor ID

5535

VSA Type

75

Length

4

Value

Enumerated integer. Supported values are:

- No = 0 — HA does not need to send DNS update
- Yes = 1 — HA needs to send DNS update

3GPP2-ESN

This attribute contains the Electronic Serial Number (ESN) of the Mobile Station.

Type

26

Vendor ID

5535

VSA Type

52

Length

1–15

Value

Opaque value
3GPP2-FA-Address

This attribute indicates if compulsory tunneling is to be employed on behalf of a subscriber. Usually compulsory tunneling is employed when a subscriber cannot initiate a tunnel itself, usually because the subscriber's device does not support tunneling. Contains an IP address as it would appear in the IP header.

Type

26

Vendor ID

5535

VSA Type

79

Length

4

Value

IPv4 address
3GPP2-FEID

This attribute specifies the FEID value.

Type

26

Vendor ID

5535

VSA Type

216

Length

0–16

Value

Opaque value
3GPP2-Flow-Id

This attribute displays the 3GPP2-Flow-Id-parameter.

Type

26

Vendor ID

5535

VSA Type

144

Value

Contains the following two subattributes:
Direction

This attribute identifies the IP flow id direction.

Type

1

Length

2

Value

Enumerated integer. Supported values are:

- Forward = 0
- Reverse = 1
- Both = 2

Flow-Id

This attribute identifies the IP flow.

Type

2

Length

2

Value

Unsigned integer
3GPP2-Flow-Status

This attribute displays the 3GPP2 Flow Status.

Type

26

Vendor ID

5535

VSA Type

145

Length

4

Value

Enumerated integer. Supported values are:

- Active = 0
- Inactive = 1

3GPP2-Forward-Fundamental-Rate

As defined in “Wireless IP Network Standard – 3GPP2.P.S0001-A-1”.

Type

26

Vendor ID

5535

VSA Type

14

Length

4

Value

Unsigned integer
3GPP2-Forward-Fundamental-RC

The format and structure of the RADIUS channel in the forward direction. A set of forward transmission formats that are characterized by data rates, modulation characterized, and spreading rates.

Type

26

Vendor ID

5535

VSA Type

20

Length

4

Value

Unsigned integer
3GPP2-Forward-Mux-Option

Forward direction multiplexer option.

Type

26

Vendor ID

5535

VSA Type

12

Length

4

Value

Unsigned integer
3GPP2-Forward-Traffic-Type

Specifies the forward traffic type.

Type

26

Vendor ID

5535

VSA Type

17

Length

4

Value

Enumerated integer. Supported values are:

- Primary = 0
- Secondary = 1

3GPP2-Fundamental-Frame-Size

This attribute indicates the fundamental frame size. The fundamental channel has the choice of 5 or 20 ms size. The 5 ms frame size allows fast response for short signaling messages (short frame can be decoded quickly). However, depending on configuration, the fundamental may not be present.

Type

26

Vendor ID

5535

VSA Type

19

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- 5ms = 1
- 20ms = 2

3GPP2-Fwd-Dcch-Mux-Option

This attribute specifies Forward DCCH Mux option.

Type

26

Vendor ID

5535

VSA Type

84

Length

4

Value

Unsigned integer
3GPP2-Fwd-Dcch-Rc

This attribute specifies Radio Configuration of the Forward Packet Data Channel.

Type

26

Vendor ID

5535

VSA Type

86

Length

4

Value

Unsigned integer
3GPP2-Fwd-Pdch-Rc

This attribute specifies Radio Configuration of the Forward Packet Data Channel.

Type

26

Vendor ID

5535

VSA Type

83

Length

4

Value

Unsigned integer
3GPP2-GMT-Timezone-Offset

GMT-Time-Zone-Offset is 4-octet string that is interpreted as a 4-byte signed integer that indicates the current offset in seconds from GMT at the visited carrier's PDSN. The offset should be adjusted to reflect standard time or daylight saving time.

Type

26

Vendor ID

5535

VSA Type

143

Length

4

Value

Integer
3GPP2-Granted-QoS

This attribute displays the 3GPP2-Granted-QoS-Parameter.

Type

26

Vendor ID

5535

VSA Type

132

Value

Contains the following subattributes:
Direction

This attribute specifies the Granted QoS parameters received from the RAN for the flow identified by direction.

Type

1

Length

2

Value

Enumerated integer. Supported values are:

- Forward = 0
- Reverse = 1
- Both = 2

Flow-Id

This attribute specifies the Granted QoS parameters received from the RAN for the flow identified by FLOW_ID.

Type

2

Length

2

Value

Unsigned integer
Attribute-Set-Id

This attribute specifies the Granted QoS parameters received from the RAN for flow verbose or non-verbose.

Type

3

Length

2

Value

Unsigned integer
Flow-Profile-Id

This attribute specifies the Granted QoS parameters received from the RAN for the flow profile ID.

Type

4

Length

2

Value

Unsigned integer
Traffic-Class

This attribute specifies the Granted QoS parameters received from the RAN for the flow traffic class.

Type

5

Length

2

Value

Enumerated integer. Supported values are:

- Unknown = 0
- Conversational = 1
- Streaming = 2
- Interactive = 3
- Background = 4

Peak-Rate

This attribute specifies the Granted QoS parameters received from the RAN for the flow Peak Rate.

Type

6

Length

2

Value

Unsigned integer
Bucket-Rate

This attribute specifies the Granted QoS parameters received from the RAN for the flow Bucket Rate.

Type

7

Length

2

Value

Unsigned integer
Token-Rate

This attribute specifies the Granted QoS parameters received from the RAN for the flow Token Rate.

Type

8

Length

2

Value

Unsigned integer
Max-Latency

This attribute specifies the Granted QoS parameters received from the RAN for the flow Max Latency.

Type

9

Length

2

Value

Unsigned integer
Max-IP-Packet-Loss-Rate

This attribute specifies the Granted QoS parameters received from the RAN for the flow Packet Loss Rate.

Type

10

Length

2

Value

Unsigned integer
Packet-Size

This attribute specifies the Granted QoS parameters received from the RAN for the flow Packet Size.

Type

11

Length

2

Value

Unsigned integer
Delay-Var-Sensitive

This attribute specifies the Granted QoS parameters received from the RAN for the flow Delay Var Sensitive.

Type

12

Length

2

Value

Enumerated integer. Supported values are:

- Not-Specified = 0
- Sensitive = 1

3GPP2-IKE-Secret

This attribute contains the FA/HA shared secret for the IKE protocol. This attribute is salt-encrypted.

Type

26

Vendor ID

5535

VSA Type

3

Length

1-247

Value

Opaque value
3GPP2-IKE-Secret-Request

This attribute indicates if the IKE secret for the FA/HA pair is to be returned for the subscriber.

Type

26

Vendor ID

5535

VSA Type

1

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

3GPP2-IKE-Secret-Unencrypted

IKE Secret key from RADIUS server in Access Accept message

Type

26

Vendor ID

5535

VSA Type

3

Length

1–247

Value

Opaque value
3GPP2-IMSI

This is the calling Station-ID attribute. IMSI value of the mobile is being filled in. This is sent when Custom11 dictionary is selected.

Type

26

Vendor ID

5535

VSA Type

1

Length

1–253

Value

Opaque value
3GPP2-Interconnect-IP

This attribute is currently not supported.
3GPP2-Interconnect-QOS

This attribute is currently not supported.
3GPP2-Inter-User-Priority

This attribute displays the 3GPP2-Inter-User-Priority.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

5535

VSA Type

139

Length

4

Value

Unsigned integer
3GPP2-IP-QOS

This attribute defines the differentiated Services code points associated with the user data.

Type

26

Vendor ID

5535

VSA Type

36

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- CS1 = 8
- AF11 = 10
- AF12 = 12
- AF13 = 14
- CS2 = 16
- AF21 = 18
- AF22 = 20
- AF23 = 22
- CS3 = 24
- AF31 = 26
- AF32 = 28
- AF33 = 30
- CS4 = 32
- AF41 = 34
- AF42 = 36
- AF43 = 38
- CS5 = 40
- EF = 46
- CS6 = 48
- CS7 = 56

3GPP2-IP-Services-Authorized

This attribute specifies the type of IP services (IPv4/CMIPv4/IPv6/CMIPv6/PMIPv4/PMIPv6, etc.) authorized.

Type

26

Vendor ID

5535

VSA Type

185

Length

4

Value

In 11.0 and earlier releases: Unsigned integer
In 12.0 and later releases: Enumerated integer. Supported values are:

- SIP4 = 1
- SIP6 = 2
- MIP4 = 4
- MIP6 = 8
- IP4_PMIP4 = 16
- IP6_PMIP4 = 32
- IP4_PMIP6 = 64
- IP6_PMIP6= 128

3GPP2-IP-Technology

This attribute identifies whether we are using Simple IP, Mobile IP, or another technology.

Type

26

Vendor ID

5535

VSA Type

22

Length

4

Value

Enumerated integer. Supported values are:

- Simple IP = 1
- Mobile IP = 2

3GPP2-IP-Services-Authorized

This attribute specifies the type of IP services (IPv4/CMIPv4/IPv6/CMIPv6/PMIPv4/PMIPv6..etc) authorized.

Type

26

Vendor ID

5535

VSA Type

185

Length

4

Value

Unsigned integer
3GPP2-KeyID

This attribute contains the opaque IKE Key Identifier for the FA/HA shared IKE secret. The first eight bytes is the network-order FA IP address in hexadecimal characters. The next eight bytes is the network-order HA IP address in hexadecimal characters. The final four bytes is a timestamp in network order, indicating when the key was created, and is the number of seconds since January 1, 1970, UTC.

Type

26

Vendor ID

5535

VSA Type

8

Length

20

Value

Opaque value
3GPP2-Last-Activity

This attribute contains timestamp of the last user activity. This attribute is same as the 3GPP2-Last-User-Activity-Time standard attribute.

Type

26

Vendor ID

5535

VSA Type

80

Length

4

Value

Unsigned integer
3GPP2-Max-Auth-Aggr-Bw-BET

This attribute contains the maximum authorized aggregate bandwidth for Best Effort Traffic.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

5535

VSA Type

130

Length

4

Value

Unsigned integer
3GPP2-Max-Per-Fl-Pri-ForTheUser

The maximum per flow priority for the user.

Type

26

Vendor ID

5535

VSA Type

133

Length

4

Value

Unsigned integer
3GPP2-MEID

Mobile Equipment Identifier (MEID) uniquely identifies the mobile equipment.

Type

26

Vendor ID

5535

VSA Type

116

Length

0–14

Value

Opaque value
3GPP2-MIP-HA-Address

The IP address of the MIP Home Agent.

Type

26

Vendor ID

5535

VSA Type

7

Length

4

Value

IPv4 address
3GPP2-MIP-Lifetime

This VSA should be included in the RADIUS Access-Request message from the HA to the Home RADIUS/PPS if the HA is PrePaid capable. It may be included in the RADIUS Access-Accept message from the Home RADIUS/PPS to HA, in which case, the HA should include the received value in the MIP RRP sent to the PDSN.

Type

26

Vendor ID

5535

VSA Type

92

Length

Variable, greater than 8

Value

Contains the following two subattributes:
RRQ-Lifetime

Should be included in the initial RADIUS Access-Request message and subsequent on-line RADIUS Access-Request if duration based PrePaid is provided for the session. It contains the MIP RRQ integer value lifetime received in the MIP RRQ message. In the RADIUS Access-Accept message, it contains the MIP RRQ integer value lifetime that should be used in the MIP RRP.

Type

1

Length

4

Value

Unsigned integer
Used-Lifetime

Should be included in the RADIUS Access-Request message at re-registration and updated RRQ (new CoA) if duration based PrePaid is provided for the session, it contains the used MIP RRQ lifetime value from an existing MIP session with the same NAI and Home Address.

Type

1

Length

4

Value

Unsigned integer
3GPP2-MIP-Rev-Tunnel-Required

Indicates to the PDSN if MIP Reverse Tunneling is required.

Type

26

Vendor ID

5535

VSA Type

4

Length

4

Value

Enumerated integer. Supported values are:

- NotRequired = 0
- Required = 1

3GPP2-MIP-Sig-Octet-Count-In

The total number of octets in registration requests and solicitations sent by the mobile.

Type

26

Vendor ID

5535

VSA Type

46

Length

4

Value

Unsigned integer
3GPP2-MIP-Sig-Octet-Count-Out

The total number of octets in registration replies and agent advertisements, sent to the mobile.

Type

26

Vendor ID

5535

VSA Type

47

Length

4

Value

Unsigned integer
3GPP2-MIP6-Authenticator

The MN-AAA authenticator obtained from the MN-AAA authentication mobility option in the BU.

Type

26

Vendor ID

5535

VSA Type

134

Length

12

Value

Opaque value
3GPP2-MIP6-CoA

MIPv6 CoA received in binding update.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

5535

VSA Type

119

Length

16

Value

Opaque value
3GPP2-MIP6-HA

MIPv6 Home Agent address received in binding update.

Type

26

Vendor ID

5535

VSA Type

118

Length

16

Value

Opaque value
3GPP2-MIP6-HoA

MIPv6 HoA received in binding update.

Type

26

Vendor ID

5535

VSA Type

141

Length

16

Value

Opaque value
3GPP2-MIP6-HoA-Not-Authorized

Value of 1 indicates to the HA that the HoA is not authorized to be used by HA.

Type

26

Vendor ID

5535

VSA Type

120

Length

4

Value

Enumerated integer. Supported value is:

- UnAuthorized = 1

3GPP2-MIP6-Home-Address

Carries the assigned Home Address during MIP6 bootstrapping.

Type

26

Vendor ID

5535

VSA Type

129

Length

18

Value

Opaque value
3GPP2-MIP6-Home-Agent

Carries the assigned MIPv6 Home Agent address received during MIPv6 bootstrapping.

Type

26

Vendor ID

5535

VSA Type

140

Length

18

Value

Opaque value
3GPP2-MIP6-Home-Link-Prefix

Carries the assigned Home Link Prefix during MIP6 bootstrapping.

Type

26

Vendor ID

5535

VSA Type

128

Length

2–18

Value

Opaque value
3GPP2-MIP6-MAC-Mobility-Data

The hashed Mobility Data from the HA to the Home RADIUS server so that the Home RADIUS server can validate the MN-AAA authenticator.

Type

26

Vendor ID

5535

VSA Type

138

Length

20

Value

Opaque value
3GPP2-MIP6-Mesg-ID

Value of Message ID from Mobility message replay protection option in Binding Update.

Type

26

Vendor ID

5535

VSA Type

123

Length

8

Value

Opaque value
3GPP2-MIP6-Session-Key

This VSA carries the Integrity Key (IK) in its encrypted form, from the Home RADIUS server to the HA.

Type

26

Vendor ID

5535

VSA Type

121

Length

16–64

Value

Opaque value
3GPP2-MN-AAA-Removal-Indication

This attribute, when set to “Not Required”, indicates that the system, when acting as a Mobile-IP Foreign Agent, should remove the MN-FA challenge and the MN-AAA Authentication Extensions, when present, from the RRQ before relaying the RRQ to the Mobile-IP Home Agent.

Vendor ID

26

VSA Type

5535

Length

4

Value

Enumerated integer. Supported values are:

- Allowed = 0
- Not-Required = 1

3GPP2-MN-HA-Shared-Key

A shared key for MN-HA authentication. The MN-HA shared key is encrypted using a method based on MD5.

Type

26

Vendor ID

5535

VSA Type

58

Length

1–251

Value

Opaque value
3GPP2-MN-HA-Shared-Key-No-Enc

This attribute contains the MN-HA shared key in plain format.

Type

26

Vendor ID

5535

VSA Type

58

Length

1–251

Value

Opaque value
3GPP2-MN-HA-SPI

The SPI for the MN-HA authentication shared key.

Type

26

Vendor ID

5535

VSA Type

57

Length

4

Value

Unsigned integer
3GPP2-Mobile-Term-Orig-Ind

Tells whether the call is mobile originated (Call initiated from mobile side) or mobile terminated (Call initiated from external towards mobile).

Type

26

Vendor ID

5535

VSA Type

45

Length

1

Value

Enumerated integer. Supported values are:

- Mobile-Originated = 0
- Mobile-Terminated = 1

3GPP2-Number-Active-Transitions

This attribute counts the total number of non-active to active transitions by the user.

Type

26

Vendor ID

5535

VSA Type

30

Length

4

Value

Unsigned integer
3GPP2-Num-Bytes-Received-Total

This attribute counts all bytes received in the reverse direction by the HDLC layer in the PDSN.

Type

26

Vendor ID

5535

VSA Type

43

Length

4

Value

Unsigned integer
3GPP2-Num-SDB-Input

This attribute counts the total number of Short Data Burst transactions to the user.

Type

26

Vendor ID

5535

VSA Type

33

Length

4

Value

Unsigned integer
3GPP2-Num-SDB-Output

This attribute counts the total number of Short Data Burst transactions from the user.

Type

26

Vendor ID

5535

VSA Type

34

Length

4

Value

Unsigned integer
3GPP2-PMIP-Capability

This attribute specifies the AGW's PMIP capability.

Type

26

Vendor ID

5535

VSA Type

193

Length

4

Value

Enumerated integer. Supported values are:

- PMIPv4_ONLY = 1
- PMIPv6_ONLY = 2
- PMIPv4_PMIPv6 = 3

3GPP2-PMIP-NAI

This attribute specifies the PMIP NAI provided by AAA.

Type

26

Vendor ID

5535

VSA Type

192

Length

1–128

Value

Opaque value
3GPP2-PMIP-IPv4Session-Info

This attribute specifies PMIP information for IPv4 session.

Type

26

Vendor ID

5535

VSA Type

194

Length

0–160

Value

Contains the following subattributes:
VAAA-IPv4Session-HA-Addr

An IPv4 address or IPv6 Address of the local HA assigned by the AGW/VAAA for AT's IPv4 Address assignment.

Type

1

Length

0–16

Value

Opaque value
HAAA-IPv4Session-HA-Addr

An IPv4 address or IPv6 Address of the home or local HA assigned by the HAAA for AT's IPv4 Address assignment.

Type

2

Length

0–16

Value

Opaque value
PMN-HA-KEY

256 bits value of network PMIP MN-HA key.

Type

3

Length

0–32

Value

Opaque value
PMN-HA-SPI

32 bits value of network PMIP MN-HA SPI value.

Type

4

Length

4

Value

Unsigned integer
VAAA-IPv4Session-LMA-Addr

An IPv4 address or IPv6 Address of the local LMA assigned by the AGW/VAAA for AT's IPv4 Address assignment

Type

5

Length

0–16

Value

Opaque value
HAAA-IPv4Session-LMA-Addr

An IPv4 address or IPv6 Address of the home or local LMA assigned by the HAAA for AT's IPv4 Address assignment.

Type

6

Length

0–16

Value

Opaque value
3GPP2-PMIP-IPv6Session-Info

This attribute specifies the PMIP information for IPv6 session.

Type

26

Vendor ID

5535

VSA Type

195

Length

0–160

Value

Contains the following subattributes:
VAAA-IPv6Session-HA-Addr

Type

1

Length

0–16

Value

Opaque value
HAAA-IPv6Session-HA-Addr

Type

2

Length

0–16

Value

Opaque value
PMN-HA-KEY

Type

3

Length

0–32

Value

Opaque value
PMN-HA-SPI

Type

4

Length

4

Value

Unsigned integer
VAAA-IPv6Session-LMA-Addr

An IPv4 address or IPv6 Address of the local LMA assigned by the AGW/VAAA for AT's IPv6 Address assignment.

Type

5

Length

0–16

Value

Opaque value
HAAA-IPv6Session-LMA-Addr

An IPv4 address or IPv6 Address of the home or local LMA assigned by the HAAA for AT's IPv6 Address assignment.

Type

6

Length

0–16

Value

Opaque value
3GPP2-Pre-Paid-Accounting-Quota

This attribute specifies the characteristics for PrePaid accounting of the volume and/or duration of a packet data session. It should be present in all on-line RADIUS Access-Request and on-line RADIUS Access-Accept messages and may be included in other RADIUS Access-Accept messages. Non-used Sub-Types by the PPC and PPS should be omitted.

Type

26

Vendor ID

5535

VSA Type

90

Length

Variable, greater than 8.

Value

Contains the following nine subattributes:
Quota-Identifier

The Quota-IDentifier Sub-Type is generated by the PrePaid server at allocation of a Volume and/or Duration Quota. The on-line quota update RADIUS Access-Request message sent from the PPC to the PPS should include a previously received Quota-Identifier.

Type

1

Length

8

Value

Unsigned integer
Volume-Quota

The optional Volume-Quota Sub-Type is only present if Volume Based charging is used. In RADIUS Access-Accept message (PPS to PPC direction), it indicates the Volume (in octets) allocated for the session by the PrePaid server. In on-line RADIUS Access-Request message (PPC to PPS direction), it indicates the total used volume (in octets) for both forward and reverse traffic applicable to PrePaid accounting13. If a Tariff Switch condition was reached during the session, this Sub-Type contains the complete (before and after) volume used, while the VolumeUsedAfterTariffSwitch attribute contains the volume used after the tariff switch condition.

Type

2

Length

4

Value

Unsigned integer
Volume-Quota-Overflow

The optional Volume-Quota-Overflow Sub-Type is used to indicate how many times the VolumeQuota counter has wrapped around 2^32 over the course of the service being provided.

Type

3

Length

2

Value

Unsigned integer
Volume-Threshold

The Volume-Threshold Sub-Type should always be present if VolumeQuota is present in a RADIUS Access-Accept message (PPS to PPC direction). It is generated by the PrePaid server and indicates the volume (in octets) that should be used before requesting quota update. This threshold should not be larger than the VolumeQuota.

Type

4

Length

4

Value

Unsigned integer
Volume-Threshold-Overflow

The optional Volume-Threshold-Overflow Sub-Type is used to indicate how many times the VolumeThreshold counter has wrapped around 2^32 over the course of the service being provided.

Type

5

Length

2

Value

Unsigned integer
Duration-Quota

The optional Duration-Quota Sub-Type is only present if Duration Based charging is used. In RADIUS Access-Accept message (PPS to PPC direction), it indicates the Duration (in seconds) allocated for the session by the PrePaid server. In on-line RADIUS Access-Accept message (PPC to PPS direction), it indicates the total Duration (in seconds) since the start of the accounting session related to the QuotaID.

Type

6

Length

4

Value

Unsigned integer
Duration-Threshold

The Duration-Threshold Sub-Type should always be present if DurationQuota is present in a RADIUS Access-Accept message (PPS to PPC direction). It represents the duration (in seconds) that should be used by the session before requesting quota update. This threshold should not be larger than the DurationQuota and should always be sent with the DurationQuota.

Type

7

Length

4

Value

Unsigned integer
Update-Reason

The Update-Reason Sub-Type should be present in the on-line RADIUS Access-Request message (PPC to PPS direction). It indicates the reason for initiating the on-line quota update operation. Update reasons 4, 5, 6, 7 and 8 indicate that the associated resources are released at the client side, and therefore the PPS should not allocate a new quota in the RADIUS Access-Accept message.

Type

8

Length

2

Value

Enumerated integer. Supported values are:

- Pre-Initialization = 1
- Initial-Request = 2
- Threshold-Reached = 3
- Quota-Reached = 4
- Remote-Forced-Disconnect = 5
- Client-Service-Termination = 6
- Main-SI-Released = 7
- Service-Instance-Not-Established = 8
- Tariff-Switch-Update = 9
- Incorrect-Quota-Type-Received = 10
- Poorly-Formed-Quota-Attribute = 11

Pre-Paid-Server

The optional, multi-value Pre-Paid-Server indicates the address of the serving PrePaid System. If present, the Home RADIUS server uses this address to route the message to the serving PrePaid Server. The attribute may be sent by the Home RADIUS server. If present in the incoming RADIUS Access-Accept message, the PDSN should send this attribute back without modifying it in the subsequent RADIUS Access-Request message, except for the first one. If multiple values are present, the PDSN should not change the order of the attributes.

Type

9

Length

4

Value

IPv4 address
3GPP2-Pre-Paid-Acct-Capability

This attribute specifies the capability for PrePaid accounting for a packet data session. It contains the possible capabilities of the PrePaid client and the selected (by the PrePaid server) capability for the session. The absence of this VSA indicates that the client is not capable of PrePaid Accounting and the session should not use PrePaid accounting.

Type

26

Vendor ID

5535

VSA Type

91

Length

Variable, greater than 8

Value

Contains the following two subattributes:
Available-In-Client

The optional Available-In-Client Sub-Type, generated by the PrePaid client, indicates the PrePaid Accounting capabilities of the client in the PDSN or HA and should be bitmap encoded.

Type

1

Length

4

Value

Enumerated integer. Supported values are:

- Supported_None = 0
- Supported_Volume = 1 — PrePaid Accounting for Volume supported
- Supported_Duration = 2 — PrePaid Accounting for Duration supported
- Supported_Volume_And_Duration = 3 — PrePaid Accounting for Volume and Duration supported (non concurrently)

Selected-For-Session

The optional Selected-For-Session Sub-Type, generated by the PrePaid server, indicates the PrePaid Accounting capability to be used for a given session.

Type

2

Length

4

Value

Enumerated integer. Supported values are:

- Usage_None = 0 — PrePaid Accounting not used
- Usage_Volume = 1 — Usage of PrePaid Accounting for Volume (only possible if the AvailableInClient supports PrePaid Accounting for Volume).
- Usage_Duration = 2 — Usage of PrePaid Accounting for Duration (only possible if the AvailableInClient supports PrePaid Accounting for Duration).
- Usage_Volume_And_Duration = 3 — Usage of PrePaid Accounting for Volume and Duration (non concurrent) (only possible if the AvailableInClient supports PrePaid Accounting for Volume and duration).

3GPP2-Pre-Paid-TariffSwitch

Type

26

Vendor ID

5535

VSA Type

98

Length

Compound

Value

Contains the following subattributes:
Quota-Identifier

Quota-Identifier

Type

1

Length

4

Value

Unsigned integer
Volume-Used-After-Tariff-Switch

Volume Quota used after Tariff Switch happened.

Type

2

Length

4

Value

Unsigned integer
Volume-Used-ATS-Overflow

Indicates how many times the VUATS counter has wrapped around 2^32 over the course of the service being provided.

Type

3

Length

2

Value

Unsigned integer
Tariff-Switch-Interval

Indicates Tariff Switch Interval in seconds.

Type

4

Length

4

Value

Unsigned integer
Time-Interval-After-Tariff-Switch-Update

Duration after TSI where an on-line RADIUS Access-Request is sent by PrePaid client to report VUATS before the next TS condition is triggered.

Type

5

Length

4

Value

Unsigned integer
3GPP2-QoS-Service-Opt-Profile

The attribute specifies the unauthorized packet data service options, the maximum number of simultaneous service instances of the given service option number and the total maximum number of simultaneous service instances.

Type

26

Vendor ID

5535

VSA Type

74

Length

8-247

Value

Opaque value
3GPP2-Release-Indicator

This attribute specifies reasons for sending a stop record. The enumeration of this attribute conforms to IS-835-1.

Type

26

Vendor ID

5535

VSA Type

24

Length

4

Value

Enumerated integer. Supported values are:

- Unknown = 0
- PPP-Timeout = 1
- Handoff = 2
- PPP-Termination = 3
- Mobile-IP-Registration-Failure = 4
- Abnormal-Terminations = 5
- Termation-Dueto-Resource-Mgmt = 6
- Service-Instance-Released = 7
- VolumeQuota-Reached = 8
- DurationQuota-Reached = 9
- Incompatible-Prepaid = 10
- Airlink-Parameter-Change = 11
- TOD-Timer-Expiry = 12
- Active-To-Dormant = 13
- Flow-Deactivated = 15
- PPP-Renegotiation = 1001
- MIP-Lifetime-Expired = 1002
- A11-Lifetime-Expired = 1003
- MIP-Remote-Dereg = 1004
- Tarrif-Boundary = 1006
- PPP-Renegotiation-Handoff = 1007
- MIP-Registration-Revocation = 1008

3GPP2-Release-Indicator-custom9

3GPP2 Release Indicator for custom9, reason/cause for session release.

Type

26

Vendor ID

5535

VSA Type

24

Length

4

Value

Enumerated integer. Supported values are:

- Unknown = 0
- PPP-Timeout = 1
- Handoff = 2
- PPP-Termination = 3
- Mobile-IP-Registration-Failure = 4
- PPP-Renegotiation = 5
- MIP-Registration-Revocation = 6
- VolumeQuota-Reached = 8
- DurationQuota-Reached = 9
- Incompatible-Prepaid = 10

3GPP2-Release-Indicator-Old

3GPP2 old Standard Release Indicator, reason/cause for session release.

Type

26

Vendor ID

5535

VSA Type

24

Length

4

Value

Enumerated integer. Supported values are:

- Unknown = 0
- PPP-Timeout = 1
- Handoff = 2
- PPP-Protocol-Failure = 3
- PPP-Abnormal-Release = 4
- PPP-Termination = 5
- Mobile-IP-Registration-Failure = 6
- Active-To-Dormant = 7

3GPP2-Remote-Addr-Table-Index

This attribute contains the Remote Address Table Index used to generate remote address accounting records. Supported range is 1–65535. Only one 3GPP2-Remote-Addr-Table-Index can be associated with a session.

Type

26

Vendor ID

5535

VSA Type

71

Length

4

Value

Contains the following two subattributes:
Table-Index

Table-Index

Type

1

Length

2

Value

Unsigned integer
Qualifier

Qualifier

Type

2

Length

2

Value

Enumerated integer. Supported values are:

- Exempt-From-Prepaid = 1
- Summarize-Octet-Count = 2
- Both = 3

3GPP2-Remote-IPv4-Address

This attribute allows the HA or PDSN to identify any IP address to be used for remote address-based accounting for the user. Up to 20 instances of the attribute are supported in the access response.

Type

26

Vendor ID

5535

VSA Type

59

Length

12

Value

Contains the following three subattributes:
Address

This attribute contains an IPv4 address to be used for remote address based accounting for the user. The address is used in conjunction with the Remote-Address-Mask subattribute to define the range of addresses to be monitored.

Type

1

Length

4

Value

IPv4 address
Netmask

This attribute contains an IPv4 address mask that defines the set of remote addresses to be used for remote address based accounting.

Type

2

Length

4

Value

IPv4 address
Qualifier

Qualifier

Type

3

Length

2

Value

Enumerated integer. Supported values are:

- Exempt-From-Prepaid = 1
- Summarize-Octet-Count = 2
- Both = 3

3GPP2-Remote-IPv4-Addr-Octets

This attribute allows the HA or PDSN to identify any IP address to be used for remote address based accounting for the user. Up to 10 instances of the attribute are supported.

Type

26

Vendor ID

5535

VSA Type

72

Length

26

Value

Contains the following subattributes:
Address

This attribute contains an IPv4 address to be used for remote address based accounting for the user. The address is used in conjunction with the Netmask subattribute to define the range of addresses to be monitored.

Type

1

Length

4

Value

IPv4 address
Netmask

This attribute contains an IPv4 address mask that defines the set of remote addresses to be used for remote address based accounting.

Type

2

Length

4

Value

An IP Netmask specified in IP address format.
Octets-Out

Indicates how many bytes have been sent to the remote address specification (corresponds to forward traffic direction).

Type

3

Length

4

Value

Unsigned integer
Octets-In

Indicates how many bytes have been received from the remote address specification (corresponds to reverse traffic direction).

Type

4

Length

4

Value

Unsigned integer
Table-Index

Table-Index

Type

5

Length

2

Value

Unsigned integer
Octets-Overflow-Out

Indicates how many times the forward octet overflow counter has wrapped around 2^32 over the course of the service being provided.

Type

6

Length

2

Value

Unsigned integer
Octets-Overflow-In

Indicates how many times the reverse octets overflow counter has wrapped around 2^32 over the course of the service being provided.

Type

7

Length

2

Value

Unsigned integer
3GPP2-Rev-Dcch-Mux-Option

This attribute specifies Reverse DCCH Mux option.

Type

26

Vendor ID

5535

VSA Type

85

Length

4

Value

Unsigned integer
3GPP2-Rev-Dcch-Rc

This attribute specifies the Radio Configuration of the Reverse Packet Data Channel.

Type

26

Vendor ID

5535

VSA Type

87

Length

4

Value

Unsigned integer
3GPP2-Reverse-Fundamental-Rate

As defined in “Wireless IP Network Standard - 3GPP2.P.S0001-A-1[4]”.

Type

26

Vendor ID

5535

VSA Type

15

Length

4

Value

Unsigned integer
3GPP2-Reverse-Fundamental-RC

The format and structure of the RADIUS channel in the reverse direction. A set of forward transmission formats that are characterized by data rates, modulation characterized, and spreading rates.

Type

26

Vendor ID

5535

VSA Type

21

Length

4

Value

Unsigned integer
3GPP2-Reverse-Mux-Option

Forward direction multiplexer option.

Type

26

Vendor ID

5535

VSA Type

13

Length

4

Value

Unsigned integer
3GPP2-Reverse-Traffic-Type

Specifies the reverse traffic type.

Type

26

Vendor ID

5535

VSA Type

18

Length

4

Value

Enumerated integer. Supported values are:

- Primary = 0
- Secondary = 1

3GPP2-Rev-Pdch-Rc

This attribute displays the 3GPP2-Rev-Pdch-Rc.

Type

26

Vendor ID

5535

VSA Type

114

Length

4

Value

Unsigned integer
3GPP2-RP-Session-ID

This represents the GRE key selected by the PCF that identifies the A10 traffic for a user session.

Type

26

Vendor ID

5535

VSA Type

41

Length

4

Value

Unsigned integer
3GPP2-Rsvp-Signal-In-Count

This attribute specifies the RSVP signaling octets sent by the MS.

Type

26

Vendor ID

5535

VSA Type

162

Length

4

Value

Unsigned integer
3GPP2-Rsvp-Signal-In-Packets

This attribute specifies the Number of RSVP signaling packets sent by the MS.

Type

26

Vendor ID

5535

VSA Type

164

Length

4

Value

Unsigned integer
3GPP2-Rsvp-Signal-Out-Count

This attribute specifies the RSVP signaling octets sent to the MS.

Type

26

Vendor ID

5535

VSA Type

163

Length

4

Value

Unsigned integer
3GPP2-Rsvp-Signal-Out-Packets

This attribute specifies the Number of RSVP signaling packets sent to the MS.

Type

26

Vendor ID

5535

VSA Type

165

Length

4

Value

Unsigned integer
3GPP2-S

This attribute contains the 'S' secret parameter used to make the IKE pre-shared secret.

Type

26

Vendor ID

5535

VSA Type

54

Length

1–247

Value

A binary string of the value of 'S'.
3GPP2-SDB-Input-Octets

This attribute counts the total number of octets sent to the user via Short Data Bursts.

Type

26

Vendor ID

5535

VSA Type

31

Length

4

Value

Unsigned integer
3GPP2-SDB-Output-Octets

This attribute counts the total number of octets sent by the user via Short Data Bursts.

Type

26

Vendor ID

5535

VSA Type

32

Length

4

Value

Unsigned integer
3GPP2-Security-Level

This attribute indicates the type of security that the home network mandates on the visited network.

Type

26

Vendor ID

5535

VSA Type

2

Length

4

Value

Enumerated integer. Supported values are:

- IPSec = 3—IPSec for tunnels and registration messages
- None = 4

3GPP2-Service-Option

This attribute indicates the service option used for CDMA air interface.

Type

26

Vendor ID

5535

VSA Type

16

Length

4

Value

Enumerated integer. Supported values are:

- HSPD = 0x21
- HRPD = 0x3b
- LLAROHC = 0x3d
- HRPD-AUX = 0x40
- HRPD-AUX-IP = 0x43
- eHRPD = 0x252
- LTE = 0x253
- UTRAN = 0x254
- GERAN = 0x255
- WIFI = 0x806c

3GPP2-Service-Option-Profile

This attribute specifies the authorized packet data service options, the maximum number of simultaneous service instances of the given service option number (n), and the total maximum number of simultaneous service instances. This attribute may appear in a RADIUS Access-Accept message.

Type

26

Vendor ID

5535

VSA Type

74

Length

4

Value

Unsigned integer Supported values are:

- Maximum Service Instances total: The maximum number of service instances the user is allowed to establish regardless of the service option numbers. '1' represents one service instance, i.e., the main service instance. '0' is not an allowed value.
- Sub-Type ( = 1): Sub-Type for service option length for service option attribute in octets (4 octets)Service Option n: Service Option number: Maximum Number of Service instances of service option n. Sub-Type 1 may be repeated, once for each authorized service option.

3GPP2-Service-Reference-ID

Specifies the reference ID of the service instance as received in the A11 Registration Request. If the service instance is the main service instance, the main SI Indicator Sub-Type should be included.

Type

26

Vendor ID

5535

VSA Type

94

Length

4

Value

Contains two subattributes:
SR-ID

The SR_ID value received in the A11 Registration-Request message.

Type

1

Length

2

Value

Unsigned integer
Main-SI-Indicator

Only included for the main service instance.

Type

2

Length

2

Value

Enumerated integer. Supported value is:

- Main-SI = 1

3GPP2-Serving-PCF

IP address of the serving PCF.

Type

26

Vendor ID

5535

VSA Type

9

Length

4

Value

IPv4 address
3GPP2-Session-Continue

This attribute when set to True means it is not the end of a session, and an Accounting Stop is immediately followed by an Account Start Record. False means end of a session.

Type

26

Vendor ID

5535

VSA Type

48

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

3GPP2-Session-Term-Capability

This attribute should be included in a RADIUS Access-request message to the Home RADIUS server and should contain the value 3 to indicate that the PDSN and HA support both Dynamic authorization with RADIUS and Registration Revocation for Mobile Ipv4. The attribute should also be included in the RADIUS Access-Accept message and should contain the preferred resource management mechanism by the home network, which should be used for the session and may include values 1 to 3.

Type

26

Vendor ID

5535

VSA Type

88

Length

4

Value

Enumerated integer. Supported values are:

- Only_Dynamic_Auth_Extn_to_Radius = 0x00000001 = 1
- Only_Reg_Revocation_in_MIP = 0x00000002 = 2
- Both_Dynamic_Auth_And_Reg_Revocation_in_MIP = 0x00000003 = 3

3GPP2-S-Key

This attribute contains the HA IKE key in encrypted format.

Type

26

Vendor ID

5535

VSA Type

54

Length

1–247

Value

Opaque value
3GPP2-S-Lifetime

This attribute contains the lifetime of the 'S' secret parameter used to make the IKE pre-shared secret. indicating the time in seconds since January 1, 1970 00:00 UTC. Note that this is equivalent to the UNIX operating system expression of time.

Type

26

Vendor ID

5535

VSA Type

55

Length

4

Value

Unsigned integer
3GPP2-S-Request

This attribute indicates whether the HA requests a shared secret 'S'.

Type

26

Vendor ID

5535

VSA Type

55

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1 — 'S' secret requested for IKE

3GPP2-Subnet

This attribute specifies the Subnet information of the HRPD RAN.

Type

26

Vendor ID

5535

VSA Type

108

Value

Contains the following subattributes:
Rev-A-Subnet

This attribute specifies the Subnet information of the HRPD RAN.

Type

1

Length

In StarOS 8.1 and earlier: 118; In StarOS 9.0 and later: 119

Value

Opaque value
Rev-A-Sector-Id

This attribute specifies the Sector ID information of the HRPD RAN.

Type

2

Length

In StarOS 8.1 and earlier: 119; In StarOS 9.0 and later: 118

Value

Opaque value
3GPP2-S-Unencrypted

This attribute contains the HA IKE key in plain format.

Type

26

Vendor ID

5535

VSA Type

54

Length

1–247

Value

Opaque value
3GPP2-User-Zone

This attribute describes the Tiered Services user zone. The least significant 16 bits are the user zone ID, the next significant 15 bits are the user zone system ID, and the most significant bit is zero.

Type

26

Vendor ID

5535

VSA Type

11

Length

4

Value

Unsigned integer
AAA-Session-ID

A unique per realm identifier assigned to WiMAX session by the Home network during network entry.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

4

Length

1–246

Value

Opaque value
Access-In-Subs

This attribute is used in a custom dictionary, and the VSA type is not standard. Opaque 1 byte value received in Access Accept. This will be included in accounting messages for this session.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

224

Length

1

Value

Opaque value
Acct-Authentic

This attribute is included in Accounting-Request packets to indicate how the session was authenticated (RADIUS or locally).

Type

45

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- None = 0 — Authentication was not required for the session
- RADIUS = 1 — The session was authenticated via RADIUS
- Local = 2 — The session was authenticated locally
- Remote = 3
- Diameter = 4

Acct-Delay-Time

This attribute indicates how many seconds the chassis has been trying to send this record for. The standard behavior is that this AVP will be visible in the Accounting Request message only if it has a non-zero value.

Type

41

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Input-Gigawords

This attribute indicates how many times the Acct-Input-Octets attribute has wrapped within its 32-bit field length. In effect, the number of octets received is a 64-bit integer, with this attribute representing the high 32 bits, and the Acct-Input-Octets attribute representing the low 32 bits. This attribute is not included unless it has a non-zero value.

Type

52

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Input-Octets

This attribute indicates how many octets have been received in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the Acct-Input-Gigawords attribute will be incremented. In effect, the number of octets received is a 64-bit integer, with the Acct-Input-Gigawords attribute representing the high 32 bits, and this attribute representing the low 32 bits.

IMPORTANT:

RADIUS reports what is going through the air interface. For uplink traffic, it reports all packets including those dropped/filtered by ACS. For downlink traffic, it reports what is going to the MS after ACS filtering. When DCCA is enabled, packets may be dropped due to unavailability of quota. Therefore, for pre-paid calls, accounting attributes “Acct-Input-Octets” and “Acct-Output-Octets” will not match totals of “dataVolumeGPRSUplink” and “dataVolumeGPRSDownlink” respectively from generated eG-CDRs.

Type

42

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Input-Packets

This attribute indicates how many PPP packets have been received during the session.

Type

47

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Interim-Interval

This attribute indicates the time (in seconds) between updates to session counters (log file on RADIUS or AAA event log) during the session. Note that the setting for this attribute always takes precedence over interim interval settings configured on the system.

CAUTION:

To avoid increasing network traffic unnecessarily and potentially reducing network and system performance, do not set this parameter to a value less than 50.

If this AVP is present in Access Accept message, the locally configured RADIUS accounting interim interval value in AAA group will be overriden. If there are no values configured in the RADIUS and AAA group the accounting interim is disabled.

Type

85

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Multi-Session-Id

This attribute is a unique Accounting ID to make it easy to link together multiple related sessions in a log file. Each session linked together would have a unique Acct-Session-Id but the same Acct-Multi-Session-Id. It is strongly recommended that the Acct-Multi-Session-Id contain UTF-8 encoded characters.

Type

50

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

String
Acct-Output-Gigawords

This attribute indicates how many times the Acct-Output-Octets attribute has wrapped within its 32-bit field length. In effect, the number of octets received is a 64-bit integer, with this attribute representing the high 32 bits, and the Acct-Output-Octets attribute representing the low 32 bits. This attribute is not included unless it has a non-zero value.

Type

53

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Output-Octets

This attribute indicates how many octets have been sent in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the Acct-Output-Gigawords attribute will be incremented. In effect, the number of octets received is a 64-bit integer, with the Acct-Output-Gigawords attribute representing the high 32 bits, and this attribute representing the low 32 bits.

IMPORTANT:

RADIUS reports what is going through the air interface. For uplink traffic, it reports all packets including those dropped/filtered by ACS. For downlink traffic, it reports what is going to the MS after ACS filtering. When DCCA is enabled, packets may be dropped due to unavailability of quota. Therefore, for pre-paid calls, accounting attributes “Acct-Input-Octets” and “Acct-Output-Octets” will not match totals of “dataVolumeGPRSUplink” and “dataVolumeGPRSDownlink” respectively from generated eG-CDRs.

Type

43

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Output-Packets

This attribute indicates how many PPP packets have been sent during the session.

Type

48

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Acct-Session-Id

This attribute is a session ID. Combined with the identification of the chassis (NAS-IP-Address or NAS-Identifier), this uniquely describes a session. For a given chassis, there will never be another session (even across boots) with this same session ID. The Acct-Session-ID AVP is sent on both Gx and Gy messages.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

44

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

String
Acct-Session-Id-Long

This attribute contains long format account session ID. This is supported only for custom2 dictionary.

Type

44

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

String
Acct-Session-Time

This attribute indicates the duration of the session in seconds.

Type

46

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Integer
Acct-Status-Type

This attribute indicates the event for the session.

Type

40

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- Start = 1 — The session has started, or the service has been delivered
- Stop = 2 — The session has completed, or the user has released service
- Interim-Update = 3 — The session or service is still ongoing. Usage details are given in other RADIUS attributes.
- Accounting-On = 7 — The chassis sends this message to the RADIUS server upon boot.
- Accounting-Off = 8 — The chassis sends this message to the RADIUS server when it shuts down in a normal fashion.
- Tunnel-Start = 9
- Tunnel-Stop = 10
- Tunnel-Reject = 11
- Tunnel-Link-Start = 12
- Tunnel-Link-Stop = 13
- Tunnel-Link-Reject = 14
- Failed = 15

Acct-Termination-Cause

This attribute indicates why the session was terminated.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

49

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- User_Request = 1 — The user requested termination
- Lost_Carrier = 2
- Lost_Service = 3 — The chassis session terminated abnormally
- Idle_Timeout = 4 — The session idle timeout expired
- Session_Timeout = 5 — The session timeout expired
- Admin_Reset = 6 — The Service Provisioning system terminated the session
- Admin_Reboot = 7 — The Service Provisioning system rebooted the chassis
- Port_Error = 8 — PAC error, requiring the session to be terminated
- NAS_Error = 9 — Error other than PAC error, requiring session to be terminated
- NAS_Request = 10 — Session terminated for any other non error reason by PDSN
- NAS_Reboot = 11 — The chassis rebooted abnormally.
- Port_Unneeded = 12
- Port_Preempted = 13 — Duplicate Home Address Requested. Call aborted.
- Port_Suspended = 14 — PPP restart or RP-A11 disconnect without active Stop conditions
- Service_Unavailable = 15 — The chassis could not provide the service requested
- Callback = 16
- User_Error = 17 — A non-compliant PPP client required the chassis to terminate the session
- Host_Request = 18 — Inter-PDSN handoff, Active->Dormant transition, PPP re-nego-tiation, Active Start Parameter change, Accounting Tariff Boundary
- Supplicant_Restart = 19
- Reauthentication_Failure = 20
- Port_Reinitialized = 21
- Port_Administratively_Disabled = 22
- Inter-PDSN-Handoff = 99 — Customer-specific implementation
- Long-Duration-Timeout = 1001
- Invalid-Source-Address = 1002
- Duplicate-IMSI = 1003
- Interim-Update = 1004
- Hotlining-Status-Change=1005

BU-CoA-Ipv6

The IPv6 address extracted from the Careof Address field in the BU and sent in Access Request from HA for WiMAX call.

Type

26

Vendor ID

24757

VSA Type

51

Length

16

Value

Opaque value
Callback-Id

This attribute contains the name of the place to be called, to be interpreted by NAS.

Type

20

Length

1-253

Value

Opaque value
Called-Station-ID

For PDSN, the value of this attribute is a single zero byte for custom6/7/8 dictionaries. For other dictionaries, this attribute will not be present for PDSN calls.

Type

30

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

For GGSN, a UTF-8 encoded string identifying the target network. For PDSN, a single zero byte.
Calling-Station-Id

This attribute indicates the Mobile Station Identifier in PDSN, and MSISDN in GGSN.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

31

Vendor ID

N/A

VSA Type

N/A

Length

1–15

Value

ASCII string
Calling-Subscriber-Type

Opaque one byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

218

Length

1

Value

The system does not interpret this value, it is only copied in accounting messages.
CHAP-Challenge

This attribute contains the CHAP Challenge that was sent by the chassis to the other end of the PPP link, when CHAP authentication is being used.

Type

60

Vendor ID

N/A

VSA Type

N/A

Length

1-253

Value

Opaque value
CHAP-Password

This attribute contains the CHAP ID and the CHAP Response when CHAP authentication is used.

Type

3

Vendor ID

N/A

VSA Type

N/A

Length

17

Value

Bit string. First byte is the CHAP ID. Next 16 bytes is the CHAP Response.
Charging-Id

Same as 3GPP-Charging-ID standard attribute; non-standard behavior for use in custom dictionary.

Type

225

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Class

This attribute may be sent by the RADIUS server to the chassis in an Access-Accept packet. The chassis will include this attribute in all subsequent Accounting-Request messages sent to the RADIUS Accounting server for this user’s session. This attribute is included to support the RADIUS protocol and should not be human-interpreted.

Type

25

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

The format of the value is server-dependent. The chassis will interpret it as simply a bit string to be reflected in Accounting-Request messages.
CUI

Chargeable User Identity is a unique temporary handle to the user responsible for paying bill. Set to NULL in Initial Access request and set to value sent by AAA in subsequent messages.

Type

89

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

Opaque value
DHCP-RK

DHCP-RK is a 160-bit randomly generated for every DHCP server, the DHCP Key is derived from this.

Type

26

Vendor ID

24757

VSA Type

40

Length

1–250

Value

Opaque value
DHCP-RK-Key-ID

An integer uniquely identifying the DHCP-RK within the scope of a single DHCP server.

Type

26

Vendor ID

24757

VSA Type

41

Length

4

Value

Unsigned Integer
DHCP-RK-Lifetime

Lifetime of the DHCP-RK and derived keys.

Type

26

Vendor ID

24757

VSA Type

42

Length

4

Value

Unsigned Integer
DHCPMSG-Server-IP

The IPv4 address of the DHCP server.

Type

26

Vendor ID

24757

VSA Type

43

Length

4

Value

IPv4 address
Digest-AKA-Auts

This attribute holds the auts parameter that is used in the Digest AKA calculation.

Type

118

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Algorithm

This parameter holds the algorithm parameter that influences the HTTP Digest calculation.

Type

111

Vendor ID

N/A

VSA Type

N/A

Length

0–253

Value

Opaque value
Digest-Auth-Param

This attribute is a placeholder for future extensions.

Type

117

Vendor ID

N/A

VSA Type

N/A

Length

0–253

Value

Opaque value
Digest-CNonce

This attribute holds the client nonce that is used in the digest calculation.

Type

113

Vendor ID

N/A

VSA Type

N/A

Length

0–253

Value

Opaque value
Digest-Domain

This attribute consists of single URI that defines a protection space component.

Type

119

Vendor ID

N/A

VSA Type

N/A

Length

0-256

Value

Opaque value
Digest-Entity-Body-Hash

This attribute holds the hexadecimal representation of H(entity-body). This hash is required when quality of protection is set to “auth-int”.

Type

112

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

Hexadecimal string
Digest-HA1

This attribute contains the hexadecimal representation on H(A1) as described in RFC 2617.

Type

121

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Method

This attribute holds the method value to be used in the HTTP digest calculation.

Type

108

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Nextnonce

This attribute holds a nonce to be used in the HTTP digest calculation.

Type

107

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

Hexadecimal string
Digest-Nonce-Count

This attribute holds the nonce count parameter that is used to detect replay attacks.

Type

114

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Opaque

This attribute holds the opaque parameter that is passed to the SIP client.

Type

116

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Qop

This attribute holds the quality of protection parameter that influences the HTTP digest calculation.

Type

110

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Realm

This attribute describes a protection space component of the RADIUS server.

Type

104

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Response-Auth

This enables the RADIUS server to prove possession of the password.

Type

106

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

Hexadecimal string.
Digest-Stale

This attribute is sent by RADIUS server in order to notify the RADIUS client whether it has accepted a nonce.

Type

120

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string. The following are valid values for this attribute:

- False = 0
- True = 1

Digest-URI

This attribute is used to transport the contents of the URI of the SIP request.

Type

109

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
Digest-Username

This attribute holds the user name used in the HTTP Digest calculation.

Type

115

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

ASCII string
DNS

IPv4/IPv6 address of the DNS server to be conveyed to the MS via DHCP.

Type

26

Vendor ID

24757

VSA Type

52

Length

4–16

Value

Opaque value
EAP-Message

The EAP exchanged transported over RADIUS.

Type

79

Vendor ID

N/A

VSA Type

N/A

Length

0-253

Value

Opaque value
Error-Cause

It is possible that the NAS cannot honor Disconnect-Request or CoA-Request messages for some reason. The Error-Cause Attribute provides more detail on the cause of the problem. It may be included within Disconnect-ACK, Disconnect-NAK, and CoA-NAK messages.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

101

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- Residual-Session-Context-Remove = 201
- Invalid-EAP-Packet = 202
- Unsupported-Attribute = 401
- Missing-Attribute = 402
- NAS-Identification-Mismatch = 403
- Invalid-Request = 404
- Unsupported-Service = 405
- Unsupported-Extension = 406
- Administratively-Prohibited = 501
- Request-Not-Routable = 502
- Session-Context-Not-Found = 503
- Session-Context-Not-Removable = 504
- Other-Proxy-Processing-Error = 505
- Resources-Unavailable = 506
- Request-Initiated = 507
- Session-Context-Not-Removable-Dormant = 599

Event-Timestamp

This attribute is a timestamp of when the event being logged occurred, indicating the time in seconds since January 1, 1970 00:00 UTC. Note that this is equivalent to the UNIX operating system expression of time.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

55

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
FA-RK-KEY

This attribute contains the encrypted FA-RK-KEY. The FA-RK determined during EAP authentication by the RADIUS server and passed on to the NAS upon successful EAP authentication. It is used by the NAS to generate MN-FA keys.

Type

26

Vendor ID

24757

VSA Type

14

Length

1–244

Value

Opaque value
FA-RK-SPI

SPI used for the FA-RK associated with FA-RK Key for generating MN-FA key for WiMAX call

Type

26

Vendor ID

24757

VSA Type

61

Length

4

Value

Unsigned integer
Filter-Id

This attribute identifies the IP access-list/filter by name.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

By default, a Filter-Id is applied in both directions. To apply a filter in a single direction, add the prefix “in:” or “out:” to the access-list name in the Filter-Id. Syntax:

in:<filter_name>

This assigns an input filter identified by filter_name

out:<filter_name>

This assigns an output filter identified by filter_name <filter_name>

If the Filter-Id value in the Access Accept message is invalid this value will not be applied to the session.

If this AVP is missing in the Access Accept message the value configured in the APN / subscriber template, if any, will be taken.

Type

11

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

ASCII string
Framed-Compression

This attribute indicates the compression protocol to be used.

Type

13

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- None = 0 — Do not use compression
- VJ_TCP_IP_header_compression = 1 — Use VJ TCP/IP header compression
- IPX_header_compression = 2
- Stac_LZS_compressions = 3 — Use Stac-LZS compression

Framed-Interface-Id

This attribute contains the value of IPv6 Interface ID.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

96

Vendor ID

N/A

VSA Type

N/A

Length

8

Value

Opaque value
Framed-IP-Address

This attribute indicates the IP address to be configured for the user.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

8

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

An IP address as it would appear in the source or destination field of an IP header. Special values are:

- 255.255.255.255 — User selected address
- 255.255.255.254 — Assign address from a pool (see Framed-Pool and SN-IP-Pool-Name)

Framed-IP-Netmask

This attribute indicates the IP netmask to be configured for the session when the PPP connection is to a router servicing a network.

Type

9

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

An IP netmask specified in IPv4 address format.
Framed-IPv6-Pool

This attribute contains the IPv6 pool name.

Type

100

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

String
Framed-IPv6-Prefix

This attribute contains IPv6 prefix.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

97

Vendor ID

N/A

VSA Type

N/A

Length

2–18

Value

Opaque value
Framed-MTU

This attribute indicates the Maximum Transmission Unit that was configured for the PPP session.

Type

12

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Integer. Supported values are from 64 through 4096.
Framed-Pool

This standard attribute indicates the name of the IP pool from which an IP address should be allocated to the subscriber. Also, see SN-IP-Pool-Name, which is a vendor-specific attribute accomplishing the same.

Type

88

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

String
Framed-Protocol

This attribute describes the framed protocol that the user is granted to use (Access-Accept), when Service-Type = Framed. Note that PPP is the only framed protocol supported.

Type

7

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- PPP = 1
- SLIP = 2
- ARAP = 3
- Gandalf_proprietary___ = 4
- Xylogics_proprietary_IPX_SLIP = 5
- X_75_Synchronous = 6
- GPRS_PDP_Context = 7

Framed-Route

This attribute specifies the subnet route to be installed in GGSN for the mobile router.

If the GGSN receives a packet with a destination address matching the Framed-Route, the packet is forwarded to the mobile router through the associated PDP context.

This attribute is accepted in the Access-Accept message and can appear multiple times. The format of value to be assigned to the Framed-Route attribute should be as follows:

<dest-ip>/<net-mask> <gateway-ip> hops

- or -

<dest-ip> <subnet-mask> <gateway-ip> hops

For example, Framed-Route = 40.40.41.0/24

IMPORTANT:

Note that the <gateway-ip> and hops are optional.

If the gateway_ip is 0.0.0.0 then the mobile node's (user's) IP is considered as the Gateway IP.

IMPORTANT:

The maximum number of framed routes allowed per subscriber is 10.

These framed routes are established at the time of call setup and deleted when the call is terminated.

Type

61

Vendor ID

N/A

VSA Type

N/A

Length

In StarOS 8.x and earlier: 16; in StarOS 9.0 and later: 1–64

Value

Opaque value
Geographical-Location

This attribute contains the information of geographical location as reported by HNB.

Type

26

Vendor ID

9

VSA Type

114

Length

10

Value

Opaque value
GGSN-GTP-IP-Address

Same as 3GPP-GGSN-Address standard attribute; non-standard behavior for use in custom dictionary.

Type

230

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

IPv4 address
HA-IP-MIP4

IPv4 address of the HA.

Type

26

Vendor ID

24757

VSA Type

6

Length

4

Value

IPv4 address
HA-IP-MIP6

IPv6 address of the HA for CMIP4.

Type

26

Vendor ID

24757

VSA Type

7

Length

4–16

Value

Opaque value
HA-RK-KEY

The HA-RK-KEY determined during EAP authentication by the RADIUS server and passed to the NAS upon successful EAP authentication. It is used by the NAS to generate FA-HA keys.

Type

26

Vendor ID

24757

VSA Type

15

Length

1–244

Value

Opaque value
HA-RK-Lifetime

Lifetime of the HA-RK and derived keys.

Type

26

Vendor ID

24757

VSA Type

17

Length

4

Value

Unsigned integer
HA-RK-SPI

The SPI associated with the HA-RK for generating MN-HA key for WiMAX call.

Type

26

Vendor ID

24757

VSA Type

16

Length

4

Value

Unsigned integer
hLMA-IPv6-PMIP6

MIPv6 Home Agent address received in binding update.

Type

26

Vendor ID

24757

VSA Type

127

Length

2

Value

Opaque value
HNB-Internet-Information

This attribute contains public IP address (either IPv4 or IPv6 address) of HNB assigned through the broadband connection.

Type

26

Vendor ID

9

VSA Type

115

Length

4–16

Value

Opaque value
HNB-Parameters

This attribute contains PLMN ID, LAC, RAC, SAC, and Cell ID of the HNB as reported to HNB-GW in RADIUS Access-Request during authentication.

Type

26

Vendor ID

9

VSA Type

112

Length

12

Value

Opaque value
Hotline-Indicator

This attribute in a RADIUS Accounting-Request message indicates to back-office systems (billing audit systems) that the session has been hot lined.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

24

Length

In 10.2 and earlier releases: 1–246

In 11.0 and later releases: 1–54

Value

In 10.2 and earlier releases: Opaque value

In 11.0 and later releases: String
Hotline-Profile-ID

A unique identifier of a hotline profile to be applied to the session.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

53

Length

In 10.2 and earlier releases: 1–246

In 11.0 and later releases: 1–64

Value

In 10.2 and earlier releases: Opaque value

In 11.0 and later releases: String
Hotline-Session-Timer

The time period, in seconds, the session can remain hotlined.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

56

Length

4

Value

Unsigned Integer
HTTP-Redirection-Rule

An HTTP redirection rule.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

54

Length

1–246

Value

Opaque value
Idle-Timeout

This attribute sets the maximum idle session time, in seconds. A session is idle when there is no IP traffic on the link. After the connection has been idle for the indicated amount of time, the chassis will tear down the session.

Type

28

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Integer
IMSI

Same as 3GPP-IMSI standard attribute; non-standard behavior for use in custom dictionary.

Type

224

Vendor ID

N/A

VSA Type

N/A

Length

1–6

Value

ASCII string
IMSI-MCC-MNC

Same as 3GPP-IMSI-Mcc-Mnc standard attribute; non-standard behavior for use in custom dictionary.

Type

226

Vendor ID

N/A

VSA Type

N/A

Length

1–6

Value

String.
In-Packet-Period

Opaque 4 byte value received in Access Accept. This will be included in accounting messages for the session. Used in custom dictionary.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

247

Length

Unsigned integer
IP-Redirection-Rule

This attribute is used to specify which packet flow to redirect and where to redirect it.

Type

26

Vendor ID

24757

VSA Type

55

Length

1–246

Value

Opaque value
Macro-Coverage-Information

This attribute contains the marco coverage information as reported by HNB which could be a GERAN or UTRAN cell information.

Type

26

Vendor ID

9

VSA Type

113

Length

8–11

Value

Opaque value
MN-HA-MIP4-KEY

MN-HA key for SPI value in the Access request if present.

Type

26

Vendor ID

24757

VSA Type

10

Length

1–244

Value

Opaque value
MN-HA-MIP4-SPI

SPI associated with the MN-HA-MIP4 key. This attribute needs to be sent in the Access Request to fetch the corresponding MN-HA keys.

Type

26

Vendor ID

24757

VSA Type

11

Length

4

Value

Unsigned integer
MN-HA-MIP6-KEY

Used to calculate AUTH for MIP6 BU during PMIP6 on ASN and to validate and compute AUTH for MIP6 Binding Answer on HA.

Type

26

Vendor ID

24757

VSA Type

12

Length

1–244

Value

Opaque value
MN-HA-MIP6-SPI

SPI associated with the MN-HA-MIP6-KEY.

Type

26

Vendor ID

24757

VSA Type

12

Length

4

Value

Unsigned integer
MSISDN

MSIDSN of the call. Used in custom dictionary.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

222

Length

1-256

Value

String
MSK

The Master Session Key determined during EAP authentication by the RADIUS server and passed to the NAS upon successful EAP authentication.

Type

26

Vendor ID

24757

VSA Type

5

Length

1–246

Value

Opaque value
NAS-Filter-Rule

Indicates filter rules to be applied for the user.

Type

92

Vendor ID

N/A

VSA Type

N/A

Length

1–246

Value

Opaque value
NAS-Identifier

This attribute identifies the NAS generating the record.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

32

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

ASCII string
NAS-IP-Address

This attribute identifies the serving NAS.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

4

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

An IP address as it would appear in the source or destination field of an IP header.
NAS-Port

This attribute describes the assigned resource number to the user session. It is guaranteed to be unique at a particular instance in time for a particular chassis.

Type

5

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
NAS-Port-Type

This attribute indicates the physical layer that the session is using.

Type

61

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- Async = 0
- Sync = 1
- ISDN_Sync = 2
- ISDN_Async_V_120 = 3
- ISDN_Async_V_110 = 4
- Virtual = 5 – MGMT
- PIAFS = 6
- HDLC_Clear_Channel = 7
- X_25 = 8
- X_75 = 9
- G_3_Fax = 10
- SDSL_Symmetric_DSL = 11
- ADSL_CAP = 12
- ADSL_DMT = 13
- IDSL = 14
- Ethernet = 15
- xDSL = 16
- Cable = 17
- Wireless_Other = 18 – Other wireless
- Wireless_IEEE_802_11 = 19 – Wireless IEEE 802.11
- Token_Ring = 20
- FDDI = 21
- Wireless_CDMA2000 = 22
- Wireless_UMTS = 23
- HRPD = 24 — High Rate Packet Data. HRPD is only available if included in the custom dictionary. None of the standard dictionaries include it.
- IAPP = 25
- FTTP = 26
- Wireless_IEEE_802_16 = 27
- Wireless_IEEE_802_20 = 28
- Wireless_IEEE_802_22 = 29
- Wireless_XGP=36

PMIP-Authenticated-Nwk-Id

The real user identifier returned by hAAA after successful authentication.

Type

26

Vendor ID

24757

VSA Type

In 10.2 and earlier releases: 58

In 11.0 and later releases: 78

Length

1–246

Value

Opaque value
PMIP6-RK-KEY

The PMIP6-RK-KEY sent by the RADIUS Server to the ASN and hCSN LMA for PMIP6. It is used to calculate the individual LMA-MAG key being the base for PBU and PBA messages protection through mobility authentication options.

Type

26

Vendor ID

24757

VSA Type

131

Length

1–251

Value

Opaque value
PMIP6-RK-SPI

The SPI associated with the PMIP6-RK-KEY.

Type

26

Vendor ID

24757

VSA Type

132

Length

1–251

Value

Opaque value
PMIP6-Service-Info

Indicates which PMIPv6 features are supported and enabled on ASN/LMA.

Type

26

Vendor ID

24757

VSA Type

126

Length

2

Value

Unsigned Integer
Price-Plan

Opaque 1 byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

196

Length

1

Value

The system does not interpret this value, but it is copied in accounting messages.
Primary-DNS-Server

Same as SN1-Primary-DNS-Server standard attribute; non-standard behavior for use in custom dictionary.

Type

135

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

IPv4 address
Prohibit-Payload-Compression

Flag to prohibit SGSN from compressing user data on per APN basis.

Type

26

Vendor ID

8164

VSA Type

237

Length

2

Value

Enumerated integer. Supported values are:

- Allowed = 0
- Prohibited = 1

Prohibit-Payload-Compression1

Flag to prohibit SGSN from compressing user data on per APN basis.

Type

26

Vendor ID

8164

VSA Type

237

Length

2

Value

Enumerated integer. Supported values are:

- Allowed = 0
- Prohibited = 1

Reject-Cause

This attribute indicates the cause for sending Access-Reject.

Type

26

Vendor ID

9

VSA Type

116

Length

1

Value

Opaque value
Reply-Message

This attribute indicates the text to be displayed to a user upon completion of authentication, whether successful or not.

Type

18

Vendor ID

N/A

VSA Type

N/A

Length

1–2048

Value

An ASCII string to be displayed to the user. This attribute may appear more than once, in which case the string displayed to the user is a concatenation of the Reply-Message attributes in the order in which they appear in the RADIUS response message.
RRQ-MN-HA-KEY

MN-HA key computed using RRQ-HA-IP if sent in Access request.

Type

26

Vendor ID

24757

VSA Type

19

Length

1–244

Value

Opaque value
Secondary-DNS-Server

Same as SN1-Secondary-DNS-Server standard attribute; non-standard behavior for use in custom dictionary.

Type

136

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

IPv4 address
Selection-Mode

Same as 3GPP-Selection-Mode standard attribute; non-standard behavior for use in custom dictionary.

Type

229

Vendor ID

N/A

VSA Type

N/A

Length

1

Value

Opaque value
Service-Type

This attribute identifies the service that the user is attempting to use (Access-Request), or is granted to use (Access-Accept).

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

6

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. Supported values are:

- Framed = 2—PPP or HA session
- Administrative = 6—Configuration administration CLI session
- Authenticate_Only = 8
- Inspector = 19650516—Configuration/statistics read-only CLI session
- Security_Admin = 19660618—Security administration CLI session

The following values are not supported, used only for display/decoding purposes:

- Login = 1
- Callback_Login = 3
- Callback_Framed = 4
- Outbound = 5
- NAS_Prompt = 7—CLI session
- Callback_NAS_Prompt = 9
- Call_Check = 10
- Callback_Administrative = 11
- Voice = 12
- Fax = 13
- Modem_Relay = 14
- IAPP_Register = 15
- IAPP_AP_Check = 16
- Authorize_Only = 17—RADIUS Change of Authorize/Disconnect/Prepaid Access Requests

Session-Timeout

This attribute sets the maximum session time in seconds. After this session time expires the chassis will tear down the session.

Type

27

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
SGSN-IP-Address

Same as 3GPP-SGSN-Address standard attribute; non-standard behavior for use in custom dictionary.

Type

228

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

IPv4 address
SIP-AOR

This attribute identifies the URI, the use of which must be authenticated and authorized.

Type

122

Vendor ID

N/A

VSA Type

N/A

Length

0–253

Value

ASCII string
SN-Access-link-IP-Frag

This attribute specifies what to do when data received for the subscriber on the Access link that needs to be fragmented and the DF bit is either set or unset. The default is Normal.

Type

26

Vendor ID

8164

VSA Type

63

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0 — Data to be fragmented is not fragmented if the DF bit is set
- DF-Ignore = 1 — Fragment regardless
- DF-Fragment-ICMP-Notify = 2 — Fragment regardless, and ICMP Notify if DF bit is set

SN-Acct-Input-Giga-Dropped

This attribute contains the number of input gigawords dropped if the number of input bytes is greater than 2^32 - 1.

Type

26

Vendor ID

8164

VSA Type

230

Length

4

Value

Unsigned integer
SN-Acct-Input-Octets-Dropped

This attribute indicates how many octets received have been dropped in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the SN-Acct-Input-Giga-Dropped attribute will be incremented.

Type

26

Vendor ID

8164

VSA Type

228

Length

8

Value

Unsigned integer
SN-Acct-Input-Packets-Dropped

This attribute indicates how many PPP packets received have been dropped during the session.

Type

26

Vendor ID

8164

VSA Type

226

Length

4

Value

Unsigned integer
SN-Acct-Output-Giga-Dropped

This attribute contains the number of output gigawords dropped if the number of output bytes is greater than 2^32 - 1.

Type

26

Vendor ID

8164

VSA Type

231

Length

4

Value

Unsigned integer
SN-Acct-Output-Octets-Dropped

This attribute indicates how many octets have been dropped in the PPP session. Since the value field is 32 bits, it is possible that the number of octets will exceed the 32-bit field length. If this happens, this attribute will “wrap” back to 0. Each time the “wrap” occurs, the SN-Acct-Output-Giga-Dropped attribute will be incremented.

Type

26

Vendor ID

8164

VSA Type

229

Length

8

Value

Unsigned integer
SN-Acct-Output-Packets-Dropped

This attribute indicates how many output PPP packets have been dropped during the session.

Type

26

Vendor ID

8164

VSA Type

227

Length

4

Value

Unsigned integer
SN-Acs-Credit-Control-Group

This attribute contains the Diameter Credit Control Group name. It is used to send the Credit Control Group name from APN config to the ACS module.

Type

26

Vendor ID

8164

VSA Type

301

Length

1–63

Value

String
SN-Admin-Expiry

This attribute contains the date/time the administrative user account expires. It is an integer value specifying the number of seconds since the UNIX epoch at which time the account will expire.

Type

26

Vendor ID

8164

VSA Type

204

Length

4

Value

Integer
SN-Admin-Permission

This attribute indicates the services allowed to be delivered to the administrative user. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.

Type

26

Vendor ID

8164

VSA Type

21

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- CLI = 1
- FTP = 2
- CLI-FTP = 3
- Intercept = 4
- CLI-Intercept = 5
- CLI-Intercept-FTP = 7
- ECS = 8
- CLI-ECS = 9
- CLI-FTP-ECS = 11
- CLI-Intercept-ECS = 13
- CLI-Intercept-FTP-ECS = 15

SN-ANID

This attribute contains the Access Network ID.

Type

26

Vendor ID

5535

VSA Type

178

Length

10

Value

Opaque value
SN-Assigned-VLAN-ID

This attribute contains the Assigned VLAN ID.

Type

26

Vendor ID

8164

VSA Type

152

Length

2

Value

Unsigned integer
SN-Authorised-Qos

This attribute contains the authorized QoS.

Type

26

Vendor ID

8164

VSA Type

266

Length

4

Value

ASCII string
SN-Bandwidth-Policy

This attribute contains the Traffic Policy value.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this policy will not be applied.

Type

26

Vendor ID

8164

VSA Type

300

Length

1–63

Value

String
SN-Call-Id

This attribute contains the Call ID.

Type

26

Vendor ID

8164

VSA Type

251

Length

4

Value

Unsigned integer
SN-Cause-Code

This attribute includes the termination cause code value from IMS node.

Type

26

Vendor ID

8164

VSA Type

267

Length

4

Value

Enumerated integer. Supported values are:

- Normal_End_Of_Session = 0
- Successful_Transaction = 1
- End_Of_Subscriber_Dialog = 2
- 3XX_Redirection = 3
- 4XX_Request_Failure = 4
- 5XX_Server_Failure = 5
- 6XX_Global_Failure = 6
- Unspecified_Error = 7
- Unsuccessful_Session_Setup = 8
- Internal_Error = 9

SN-Cause-For-Rec-Closing

This attribute contains the GGSN Specific Record Closing Reason Value.

Type

26

Vendor ID

8164

VSA Type

139

Length

4

Value

Unsigned integer
SN-CBB-Policy

This attribute contains the CBB policy name.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this policy will not be applied.

Type

26

Vendor ID

8164

VSA Type

302

Length

1–63

Value

String
SN-CF-Call-International

This attribute contains enable/disable config for CF call restriction and dialing permission for international calls.

Type

26

Vendor ID

8164

VSA Type

293

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Call-Local

This attribute contains enable/disable config for CF call restriction and dialing permission for local calls.

Type

26

Vendor ID

8164

VSA Type

291

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Call-LongDistance

This attribute contains enable/disable config for CF call restriction and dialing permission for long distance calls.

Type

26

Vendor ID

8164

VSA Type

292

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Call-Premium

This attribute contains enable/disable config for CF call restriction and dialing permission for premium calls.

Type

26

Vendor ID

8164

VSA Type

294

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Call-RoamingInternatnl

This attribute contains enable/disable config for CSCF call restriction and dialing permission - Roaming International call.

Type

26

Vendor ID

8164

VSA Type

298

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Call-Transfer

This attribute contains enable/disable config for CSCF call feature - call transfer.

Type

26

Vendor ID

8164

VSA Type

285

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Call-Waiting

This attribute contains enable/disable config for CSCF call feature - call waiting.

Type

26

Vendor ID

8164

VSA Type

284

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-CId-Display

This attribute contains enable/disable config for CSCF call feature — caller ID display.

Type

26

Vendor ID

8164

VSA Type

282

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-CId-Display-Blocked

This attribute contains enable/disable config for CSCF call feature — caller ID display blocked.

Type

26

Vendor ID

8164

VSA Type

283

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-CF-Follow-Me

This attribute contains URIs for CSCF call feature — follow me.

Type

26

Vendor ID

8164

VSA Type

281

Length

0–255

Value

ASCII string
SN-CF-Forward-Busy-Line

This attribute contains URI for CSCF call feature — forward busy line.

Type

26

Vendor ID

8164

VSA Type

279

Length

0–255

Value

ASCII string
SN-CF-Forward-No-Answer

This attribute contains URI for CSCF call feature — forward no answer.

Type

26

Vendor ID

8164

VSA Type

278

Length

0–255

Value

ASCII string
SN-CF-Forward-Not-Regd

This attribute contains URI for CSCF call feature — forward not registered.

Type

26

Vendor ID

8164

VSA Type

280

Length

0–255

Value

ASCII string
SN-CF-Forward-Unconditional

This attribute contains URI for CSCF call feature — forward unconditional.

Type

26

Vendor ID

8164

VSA Type

277

Length

0–255

Value

ASCII string
SN-CFPolicy-ID

This attribute contains the Content Filtering policy ID.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

220

Length

4

Value

Unsigned integer
SN-Change-Condition

The change condition that triggered this record for a GGSN session.

Type

26

Vendor ID

8164

VSA Type

140

Length

4

Value

Enumerated integer. Supported values are:

- QOSCHANGE = 0
- TARIFFTIMECHANGE = 1
- SGSNCHANGE = 500

SN-Charging-VPN-Name

The Charging Context Name for GGSN sessions.

Type

26

Vendor ID

8164

VSA Type

137

Length

1–252

Value

ASCII string
SN-Chrg-Char-Selection-Mode

SN-Chrg-Char-Selection-Mode

Type

26

Vendor ID

8164

VSA Type

138

Length

4

Value

Unsigned integer
SN-Content-Disposition

This attribute indicates how the SIP message body or a message body part is to be interpreted.

Type

26

Vendor ID

8164

VSA Type

272

Length

4

Value

ASCII string
SN-Content-Length

This attribute contains size of the SIP message body.

Type

26

Vendor ID

8164

VSA Type

271

Length

4

Value

ASCII string
SN-Content-Type

This attribute contains the media type of the SIP message body.

Type

26

Vendor ID

8164

VSA Type

270

Length

4

Value

ASCII string
SN-CR-International-Cid

Carrier ID for routing international calls.

Type

26

Vendor ID

8164

VSA Type

295

Length

4

Value

Unsigned integer
SN-CR-LongDistance-Cid

Carrier ID for routing long distance calls.

Type

26

Vendor ID

8164

VSA Type

296

Length

4

Value

Unsigned integer
SN-CSCF-App-Server-Info

This is a compound attribute and contains information about application servers.

Type

26

Vendor ID

8164

VSA Type

275

Length

4

Value

Contains the following two subattributes:
App-Server

Holds URL of the application server.

Type

1

Length

4

Value

ASCII string
AS-Called-Party-Address

Holds the called party addresses determined by the application server.

Type

2

Length

4

Value

ASCII string
SN-CSCF-Rf-SDP-Media-Components

This is a compound attribute for IMS SDP media components.

Type

26

Vendor ID

8164

VSA Type

273

Value

Contains the following subattributes:
Media-Name

Name of the media as available in the SDP data.

Type

1

Length

0–128

Value

String
Media-Description

Holds the attributes of the media as available in the SDP data.

Type

2

Length

0–128

Value

String
Authorised-QoS

Holds the 3GPP Authorised QoS string.

Type

3

Length

0–128

Value

String
3GPP-Charging-Id

Holds the 3GPP charging ID.

Type

4

Length

0–253

Value

String
Access-Network-Charging-Identifier-Value

Holds the access network charging identifier value.

Type

5

Length

1–256

Value

Opaque value
SN-Cscf-Subscriber-Ip-Address

This attribute contains the IP address of subscriber, used for early IMS authentication procedures.

Type

26

Vendor ID

8164

VSA Type

287

Length

4

Value

IPv4 address
SN-Data-Tunnel-Ignore-DF-Bit

This attribute specifies if the PDSN/FA or HA should ignore the DF bit in the IPv4 header when encapsulating the IPv4 packet in MIP, and therefore fragmenting the resulting tunneled packet if necessary. The default is not to ignore the DF bit.

Type

26

Vendor ID

8164

VSA Type

49

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not ignore DF bit
- Enabled = 1 — Ignore DF bit

SN-DHCP-Lease-Expiry-Policy

This attribute specifies whether to renew or disconnect on expiry of IP address lease time.

Type

26

Vendor ID

8164

VSA Type

157

Length

4

Value

Enumerated integer. Supported values are:

- auto-renew = 0
- disconnect = 1

SN-DHCP-Options

Specific information to be sent from the DHCP server to the client.

Type

26

Vendor ID

8164

VSA Type

309

Length

1–245

Value

Opaque value
SN-Direction

ROHC protocol control that specifies in which direction to enable Robust Header Compression (ROHC).

Type

26

Vendor ID

8164

VSA Type

153

Length

4

Value

Enumerated integer. Supported values are:

- Any = 0
- Uplink = 1
- Downlink = 2

SN-Disconnect-Reason

This attribute indicates the reason the user was disconnected from service.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

3

Length

4

Value

Enumerated integer. Supported values are:

- Not-Defined = 0
- Admin-Disconnect = 1
- Remote-Disconnect = 2
- Local-Disconnect = 3
- Disc-No-Resource = 4
- Disc-Excd-Service-Limit = 5
- PPP-LCP-Neg-Failed = 6
- PPP-LCP-No-Response = 7
- PPP-LCP-Loopback = 8
- PPP-LCP-Max-Retry = 9
- PPP-Echo-Failed = 10
- PPP-Auth-Failed = 11
- PPP-Auth-Failed-No-AAA-Resp = 12
- PPP-Auth-No-Response = 13
- PPP-Auth-Max-Retry = 14
- Invalid-AAA-Attr = 15
- Failed-User-Filter = 16
- Failed-Provide-Service = 17
- Invalid-IP-Address-AAA = 18
- Invalid-IP-Pool-AAA = 19
- PPP-IPCP-Neg-Failed = 20
- PPP-IPCP-No-Response = 21
- PPP-IPCP-Max-Retry = 22
- PPP-No-Rem-IP-Address = 23
- Inactivity-Timeout = 24
- Session-Timeout = 25
- Max-Data-Excd = 26
- Invalid-IP-Source-Address = 27
- MSID-Auth-Failed = 28
- MSID-Auth-Failed-No-AAA-Resp = 29
- A11-Max-Retry = 30
- A11-Lifetime-Expired = 31
- A11-Message-Integrity-Failure = 32
- PPP-lcp-remote-disc = 33
- Session-setup-timeout = 34
- PPP-keepalive-failure = 35
- Flow-add-failed = 36
- Call-type-detection-failed = 37
- Wrong-ipcp-params = 38
- MIP-remote-dereg = 39
- MIP-lifetime-expiry = 40
- MIP-proto-error = 41
- MIP-auth-failure = 42
- MIP-reg-timeout = 43
- Invalid-dest-context = 44
- Source-context-removed = 45
- Destination-context-removed = 46
- Req-service-addr-unavailable = 47
- Demux-mgr-failed = 48
- Internal-error = 49
- AAA-context-removed = 50
- invalid-service-type = 51
- mip-relay-req-failed = 52
- mip-rcvd-relay-failure = 53
- ppp-restart-inter-pdsn-handoff = 54
- gre-key-mismatch = 55
- invalid_tunnel_context = 56
- no_peer_lns_address = 57
- failed_tunnel_connect = 58
- l2tp-tunnel-disconnect-remote = 59
- l2tp-tunnel-timeout = 60
- l2tp-protocol-error-remote = 61
- l2tp-protocol-error-local = 62
- l2tp-auth-failed-remote = 63
- l2tp-auth-failed-local = 64
- l2tp-try-another-lns-from-remote = 65
- l2tp-no-resource-local = 66
- l2tp-no-resource-remote = 67
- l2tp-tunnel-disconnect-local = 68
- l2tp-admin-disconnect_remote = 69
- l2tpmgr-reached-max-capacity = 70
- MIP-reg-revocation = 71
- path-failure = 72
- dhcp-relay-ip-validation-failed = 73
- gtp-unknown-pdp-addr-or-pdp-type = 74
- gtp-all-dynamic-pdp-addr-occupied = 75
- gtp-no-memory-is-available = 76
- dhcp-relay-static-ip-addr-not-allowed = 77
- dhcp-no-ip-addr-allocated = 78
- dhcp-ip-addr-allocation-tmr-exp = 79
- dhcp-ip-validation-failed = 80
- dhcp-static-addr-not-allowed = 81
- dhcp-ip-addr-not-available-at-present = 82
- dhcp-lease-expired = 83
- lpool-ip-validation-failed = 84
- lpool-static-ip-addr-not-allowed = 85
- static-ip-validation-failed = 86
- static-ip-addr-not-present = 87
- static-ip-addr-not-allowed = 88
- radius-ip-validation-failed = 89
- radius-ip-addr-not-provided = 90
- invalid-ip-addr-from-sgsn = 91
- no-more-sessions-in-aaa = 92
- ggsn-aaa-auth-req-failed = 93
- conflict-in-ip-addr-assignment = 94
- apn-removed = 95
- credits-used-bytes-in = 96
- credits-used-bytes-out = 97
- credits-used-bytes-total = 98
- prepaid-failed = 99
- l2tp-ipsec-tunnel-failure = 100
- l2tp-ipsec-tunnel-disconnected = 101
- mip-ipsec-sa-inactive = 102
- Long-Duration-Timeout = 103
- proxy-mip-registration-failure = 104
- proxy-mip-binding-update = 105
- proxy-mip-inter-pdsn-handoff-require-ip-address = 106
- proxy-mip-inter-pdsn-handoff-mismatched-address = 107
- Local-purge = 108
- failed-update-handoff = 109
- closed_rp-handoff-complete = 110
- closed_rp-duplicate-session = 111
- closed_rp-handoff-session-not-found = 112
- closed_rp-handoff-failed = 113
- pcf-monitor-keep-alive-failed = 114
- call-internal-reject = 115
- call-restarted = 116
- a11-mn-ha-auth-failure = 117
- a11-badly-formed = 118
- a11-t-bit-not-set = 119
- a11-unsupported-vendor-id = 120
- a11-mismatched-id = 121
- mipha-dup-home-addr-req = 122
- mipha-dup-imsi-session = 123
- ha-unreachable = 124
- IPSP-addr-in-use = 125
- mipfa-dup-home-addr-req = 126
- mipha-ip-pool-busyout = 127
- inter-pdsn-handoff = 128
- active-to-dormant = 129
- ppp-renegotiation = 130
- active-start-param-change = 131
- tarrif-boundary = 132
- a11-disconnect-no-active-stop = 133
- nw-reachability-failed-reject = 134
- nw-reachability-failed-redirect = 135
- container-max-exceeded = 136
- static-addr-not-allowed-in-apn = 137
- static-addr-required-by-radius = 138
- static-addr-not-allowed-by-radius = 139
- mip-registration-dropped = 140
- counter-rollover = 141
- constructed-nai-auth-fail = 142
- inter-pdsn-service-optimize-handoff-disabled = 143
- gre-key-collision = 144
- inter-pdsn-service-optimize-handoff-triggered = 145
- intra-pdsn-handoff-triggered = 146
- delayed-abort-timer-expired = 147
- Admin-AAA-disconnect = 148
- Admin-AAA-disconnect-handoff = 149
- PPP-IPV6CP-Neg-Failed = 150
- PPP-IPV6CP-No-Response = 151
- PPP-IPV6CP-Max-Retry = 152
- PPP-Restart-Invalid-source-IPV4-address = 153
- a11-disconnect-handoff-no-active-stop = 154
- call-restarted-inter-pdsn-handoff = 155
- call-restarted-ppp-termination = 156
- mipfa-resource-conflict = 157
- failed-auth-with-charging-svc = 158
- mipha-dup-imsi-session-purge = 159
- mipha-rev-pending-newcall = 160
- volume-quota-reached = 161
- duration-quota-reached = 162
- gtp-user-authentication-failed = 163
- MIP-reg-revocation-no-lcp-term = 164
- MIP-private-ip-no-rev-tunnel = 165
- Invalid-Prepaid-AAA-attr-in-auth-response = 166
- mipha-prepaid-reset-dynamic-newcall = 167
- gre-flow-control-timeout = 168
- mip-paaa-bc-query-not-found = 169
- mipha-dynamic-ip-addr-not-available = 170
- a11-mismatched-id-on-handoff = 171
- a11-badly-formed-on-handoff = 172
- a11-unsupported-vendor-id-on-handoff = 173
- a11-t-bit-not-set-on-handoff = 174
- MIP-reg-revocation-i-bit-on = 175
- A11-RRQ-Deny-Max-Count = 176
- Dormant-Transition-During-Session-Setup = 177
- PPP-Rem-Reneg-Disc-Always-Cfg = 178
- PPP-Rem-Reneg-Disc-NAI-MSID-Mismatch = 179
- mipha-subscriber-ipsec-tunnel-down = 180
- mipha-subscriber-ipsec-tunnel-failed = 181
- mipha-subscriber-ipsecmgr-death = 182
- flow-is-deactivated = 183
- ecsv2-license-exceeded = 184
- IPSG-Auth-Failed = 185
- driver-initiated = 186
- ims-authorization-failed = 187
- service-instance-released = 188
- flow-released = 189
- ppp-renego-no-ha-addr = 190
- intra-pdsn-handoff = 191
- overload-disconnect = 192
- css-service-not-found = 193
- Auth-Failed = 194
- dhcp-client-sent-release = 195
- dhcp-client-sent-nak = 196
- msid-dhcp-chaddr-mismatch = 197
- link-broken = 198
- prog-end-timeout = 199
- qos-update-wait-timeout = 200
- css-synch-cause = 201
- Gtp-context-replacement = 202
- PDIF-Auth-failed = 203
- l2tp-unknown-apn = 204
- ms-unexpected-network-reentry = 205
- r6-invalid-nai = 206
- eap-max-retry-reached = 207
- vbm-hoa-session-disconnected = 208
- vbm-voa-session-disconnected = 209
- in-acl-disconnect-on-violation = 210
- eap-msk-lifetime-expiry = 211
- eap-msk-lifetime-too-low = 212
- mipfa-inter-tech-handoff = 213
- r6-max-retry-reached = 214
- r6-nwexit-recd = 215
- r6-dereg-req-recd = 216
- r6-remote-failure = 217
- r6r4-protocol-errors = 218
- wimax-qos-invalid-aaa-attr = 219
- npu-gre-flows-not-available = 220
- r4-max-retry-reached = 221
- r4-nwexit-recd = 222
- r4-dereg-req-recd = 223
- r4-remote-failure = 224
- ims-authorization-revoked = 225
- ims-authorization-released = 226
- ims-auth-decision-invalid = 227
- mac-addr-validation-failed = 228
- excessive-wimax-pd-flows-cfgd = 229
- sgsn-canc-loc-sub = 230
- sgsn-canc-loc-upd = 231
- sgsn-mnr-exp = 232
- sgsn-ident-fail = 233
- sgsn-sec-fail = 234
- sgsn-auth-fail = 235
- sgsn-glu-fail = 236
- sgsn-imp-det = 237
- sgsn-smgr-purge = 238
- sgsn-subs-handed-to-peer = 239
- sgsn-dns-fail-inter-rau = 240
- sgsn-cont-rsp-fail = 241
- sgsn-hlr-not-found-for-imsi = 242
- sgsn-ms-init-det = 243
- sgsn-opr-policy-fail = 244
- sgsn-duplicate-context = 245
- hss-profile-update-failed = 246
- sgsn-no-pdp-activated = 247
- asnpc-idle-mode-timeout = 248
- asnpc-idle-mode-exit = 249
- asnpc-idle-mode-auth-failed = 250
- asngw-invalid-qos-configuration = 251
- sgsn-dsd-allgprswithdrawn = 252
- r6-pmk-key-change-failure = 253
- sgsn-illegal-me = 254
- sess-termination-timeout = 255
- sgsn-sai-fail = 256
- sgsn-rnc-removal = 257
- sgsn-rai-removal = 258
- sgsn-init-deact = 259
- ggsn-init-deact = 260
- hlr-init-deact = 261
- ms-init-deact = 262
- sgsn-detach-init-deact = 263
- sgsn-rab-rel-init-deact = 264
- sgsn-iu-rel-init-deact = 265
- sgsn-gtpu-path-failure = 266
- sgsn-gtpc-path-failure = 267
- sgsn-local-handoff-init-deact = 268
- sgsn-remote-handoff-init-deact = 269
- sgsn-gtp-no-resource = 270
- sgsn-rnc-no-resource = 271
- sgsn-odb-init-deact = 272
- sgsn-invalid-ti = 273
- sgsn-ggsn-ctxt-non-existent = 274
- sgsn-apn-restrict-vio = 275
- sgsn-regular-deact = 276
- sgsn-abnormal-deact = 277
- sgsn-actv-rejected-by-peer = 278
- sgsn-err-ind = 279
- asngw-non-anchor-prohibited = 280
- asngw-im-entry-prohibited = 281
- session-idle-mode-entry-timeout = 282
- session-idle-mode-exit-timeout = 283
- asnpc-ms-power-down-nwexit = 284
- asnpc-r4-nwexit-recd = 285
- sgsn-iu-rel-before-call-est = 286
- ikev2-subscriber-ipsecmgr-death = 287
- All-dynamic-pool-addr-occupied = 288
- mip6ha-ip-addr-not-available = 289
- bs-monitor-keep-alive-failed = 290
- sgsn-att-in-reg-state = 291
- sgsn-inbound-srns-in-reg-state = 292
- dt-ggsn-tun-reestablish-failed = 293
- sgsn-unknown-pdp = 294
- sgsn-pdp-auth-failure = 295
- sgsn-duplicate-pdp-context = 296
- sgsn-no-rsp-from-ggsn = 297
- sgsn-failure-rsp-from-ggsn = 298
- sgsn-apn-unknown = 299
- sgsn-serv-req-init-deact = 300
- sgsn-attach-on-attch-init-abort = 301
- sgsn-iu-rel-in-israu-init-abort = 302
- sgsn-smgr-init-abort = 303
- sgsn-mm-ctx-cleanup-init-abort = 304
- sgsn-unknown-abort = 305
- sgsn-guard-timeout-abort = 306
- vpn-bounce-dhcpip-validate-req = 307
- mipv6-id-mismatch = 308
- aaa-session-id-not-found = 309
- x1-max-retry-reached = 310
- x1-nwexit-recd = 311
- x1-dereg-req-recd = 312
- x1-remote-failure = 313
- x1x2-protocol-errors = 314
- x2-max-retry-reached = 315
- x2-nwexit-recd = 316
- x2-dereg-req-recd = 317
- x2-remote-failure = 318
- x1-pmk-key-change-failure = 319
- sa-rekeying-failure = 320
- sess-sleep-mode-entry-timeout = 321
- phsgw-non-anchor-prohibited = 322
- asnpc-pc-relocation-failed = 323
- asnpc-pc-relocation = 324
- auth_policy_mismatch = 325
- sa-lifetime-expiry = 326
- asnpc-del-ms-entry-recd = 327
- phspc-sleep-mode-timeout = 328
- phspc-sleep-mode-exit = 329
- phspc-sleep-mode-auth-failed = 330
- phspc-ms-power-down-nwexit = 331
- phspc-x2-nwexit-recd = 332
- invalid-nat-config = 333
- asngw-tid-entry-not-found = 334
- No-NAT-IP-Address = 335
- excessive-phs-pd-flows-cfgd = 336
- phsgw-invalid-qos-configuration = 337
- Interim-Update = 338
- sgsn-attach-abrt-rad-lost = 339
- sgsn-inbnd-irau-abrt-rad-lost = 340
- ike-keepalive-failed = 341
- sgsn-attach-abrt-ms-suspend = 342
- sgsn-inbnd-irau-abrt-ms-suspend = 343
- duplicate-session-detected = 344
- sgsn-xid-response-failure = 345
- sgsn-nse-cleanup = 346
- sgsn-gtp-req-failure = 347
- sgsn-imsi-mismatch = 348
- sgsn-bvc-blocked = 349
- sgsn-attach-on-inbound-irau = 350
- sgsn-attach-on-outbound-irau = 351
- sgsn-incorrect-state = 352
- sgsn-t3350-expiry = 353
- sgsn-page-timer-expiry = 354
- phsgw-tid-entry-not-found = 355
- phspc-del-ms-entry-recd = 356
- sgsn-pdp-local-purge = 357
- phs-invalid-nai = 358
- session-sleep-mode-exit-timeout = 359
- sgsn-offload-phase2 = 360
- phs-thirdparty-auth-fail = 361
- remote-error-notify = 362
- no-response = 363
- PDG-Auth-failed = 364
- mme-s1AP-send-failed=365
- mme-egtpc-connection-failed=366
- mme-egtpc-create-session-failed=367
- mme-authentication-failure=368
- mme-ue-detach=369
- mme-mme-detach=370
- mme-hss-detach=371
- mme-pgw-detach=372
- mme-sub-validation-failure=373
- mme-hss-connection-failure=374
- mme-hss-user-unknown=375
- dhcp-lease-mismatch-detected=376
- nemo-link-layer-down=377
- eapol-max-retry-reached = 378
- sgsn-offload-phase3 = 379
- mbms-bearer-service-disconnect = 380
- disconnect-on-violation-odb = 381
- disconn-on-violation-focs-odb = 382
- CSCF-REG-Admin-disconnect = 383
- CSCF-REG-User-disconnect = 384
- CSCF-REG-Inactivity-timeout = 385
- CSCF-REG-Network-disconnect = 386
- CSCF-Call-Admin-disconnect = 387
- CSCF-CAll-User-disconnect = 388
- CSCF-CALL-Local-disconnect = 389
- CSCF-CALL-No-Resource = 390
- CSCF-CALL-No-Respone = 391
- CSCF-CALL-Inactivity-timeout = 392
- CSCF-CALL-Media-Auth-Failure = 393
- CSCF-REG-No-Resource = 394
- ms-unexpected-idle-mode-entry = 395
- re-auth-failed = 396
- sgsn-pdp-nse-cleanup = 397
- sgsn-mm-ctxt-gtp-no-resource = 398
- unknown-apn = 399
- gtpc-path-failure = 400
- gtpu-path-failure = 401
- actv-rejected-by-sgsn = 402
- sgsn-pdp-gprs-camel-release = 403
- sgsn-check-imei-failure = 404
- sgsn-sndcp-init-deact = 405
- sgsn-pdp-inactivity-timeout = 406
- fw-and-nat-policy-removed = 407
- FNG-Auth-failed = 408
- ha-stale-key-disconnect = 409
- No-IPV6-address-for-subscriber = 410
- prefix-registration-failure = 411
- disconnect-from-policy-server = 412
- s6b-auth-failed = 413
- gtpc-err-ind = 414
- gtpu-err-ind = 415
- invalid-pdn-type = 416
- aaa-auth-req-failed = 417
- apn-denied-no-subscription = 418
- Sgw-context-replacement = 419
- dup-static-ip-addr-req = 420
- apn-restrict-violation = 421
- invalid-wapn = 422
- ttg-nsapi-allocation-failed = 423
- mandatory-gtp-ie-missing = 424
- aaa-unreachable = 425
- asngw-service-flow-deletion = 426
- CT-PMIP-RRQ-NVSE-Value-Change = 427
- tcp-read-failed = 428
- tcp-write-failed = 429
- ssl-handshake-failed = 430
- ssl-renegotiate-failed = 431
- ssl-bad-message = 432
- ssl-alert-received = 433
- ssl-disconnect = 434
- ssl-migration = 435
- sgsn-ard-failure = 436
- sgsn-camel-release = 437
- Hotlining-Status-Change=447
- ggsn-no-rsp-from-sgsn = 448
- diameter-protocol-error=449
- diameter-request-timeout=450
- operator-policy=451
- spr-connection-timeout=452
- mipha-dup-wimax-session = 453
- invalid-version-attr = 454
- sgsn-zone-code-failure = 455
- invalid-qci = 456
- no_rules = 457
- mme-init-ctxt-setup-failure = 459
- mme-driver-initiated = 460
- mme-s1ap-connection-down = 461
- mme-s1ap-reset-recd = 462
- mme-s6a-response-timeout = 463
- mme-s13-response-timeout = 464
- mme-Illegal-equipment = 465
- mme-unexpected-attach = 466
- mme-sgw-selection-failure = 467
- mme-pgw-selection-failure = 468
- mme-reselection-to-sgsn = 469
- mme-relocation-to-sgsn = 470
- mme-reselection-to-mme = 471
- mme-relocation-to-mme = 472
- mme-tau-attach-collision = 473
- mme-old-sgsn-resolution-failure = 474
- mme-old-mme-resolution-failure = 475
- mme-reloc-ho-notify-timeout = 476
- mme-reloc-ho-req-ack-timeout = 477
- mme-create-session-timeout = 478
- mme-create-session-failure = 479
- mme-s11-path-failure = 480
- mme-policy-no-ue-irat = 481
- mme-x2-handover-failed = 482
- mme-attach-restrict = 483
- mme-regional-zone-code = 484
- mme-no-response-from-ue = 485
- mme-sgw-relocation-failed = 486
- mme-implicit-detach = 487
- sgsn-detach-notify = 488
- emergency-inactivity-timeout = 489
- policy-initiated-release = 490
- gy-result-code-system-failure = 491
- mme-zone-code-validation-failed = 492
- sgsn-pgw-init-deact = 493
- s6b-ip-validation-failed = 494
- sgsn-failure-rsp-from-sgw = 495
- tcp-remote-close = 496
- tcp-reset-received = 497
- tcp-socket-error = 498
- ptmsi-signature-mismatch = 499

SN-DNS-Proxy-Intercept-List

This attribute is used to specify the list name which contains the rules to intercept and redirect DNS requires received from mobile. This attribute can be configured using either local subscriber template or returned from Access-Accept.

Type

26

Vendor ID

8164

VSA Type

214

Length

1–253

Value

ASCII string
SN-DNS-Proxy-Use-Subscr-Addr

This attribute is used to convey whether to use the subscriber's address as the source address for DNS Proxy.

Type

26

Vendor ID

8164

VSA Type

25

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-Dynamic-Addr-Alloc-Ind-Flag

This attribute indicates whether the IP address is allocated statically or dynamically from SGW perspective.

Type

26

Vendor ID

8164

VSA Type

141

Length

1

Value

Opaque value
SN-Ecs-Data-Volume

Compound attribute indicating downlink and uplink octet usage for a PDP context per rating group.

Type

26

Vendor ID

8164

VSA Type

176

Length

12

Value

Contains the following subattributes:
Rating-Group-Id

Rating Group Id in a PDP context.

Type

1

Length

4

Value

Unsigned integer
GPRS-Uplink

Uplink octet usage for a PDP context per rating group.

Type

2

Length

4

Value

Unsigned integer
GPRS-Downlink

Downlink octet usage for a PDP context per rating group.

Type

3

Length

4

Value

Unsigned integer
SN-Enable-QoS-Renegotiation

This attribute configures the enabling of dynamic QoS renegotiation.

Type

26

Vendor ID

8164

VSA Type

144

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN-Event

This attribute contains the type of SIP event for which the accounting-request message is generated.

Type

26

Vendor ID

8164

VSA Type

255

Length

4

Value

ASCII string
SN-Ext-Inline-Srvr-Context

This attribute configures the context name in which the External In-line server resides.

Type

26

Vendor ID

8164

VSA Type

41

Length

1–247

Value

String

IMPORTANT:

This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
SN-Ext-Inline-Srvr-Down-Addr

This attribute configures the IP address of the Downstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

56

Length

4

Value

IPv4 address

IMPORTANT:

This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
SN-Ext-Inline-Srvr-Down-VLAN

This attribute configures the IP address of the Downstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

59

Length

4

Value

The VLAN tag to apply.

IMPORTANT:

This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
SN-Ext-Inline-Srvr-Preference

This attribute configures the preference for the tagged group of External In-line Servers. This attribute is required, although it doesn't actually assign a preference right now. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

57

Length

4

Value

Unsigned integer

IMPORTANT:

This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
SN-Ext-Inline-Srvr-Up-Addr

This attribute configures the IP address of the Upstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group

Type

26

Vendor ID

8164

VSA Type

55

Length

4

Value

IPv4 address

IMPORTANT:

This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
SN-Ext-Inline-Srvr-Up-VLAN

This attribute configures the VLAN tag to be applied to Upstream packets and forwarded to the External In-line server. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

58

Length

4

Value

The VLAN tag to apply.

IMPORTANT:

This attribute is used in conjunction with the External In-line Server feature, which is not supported in StarOS 9.0 and later releases.
SN-Fast-Reauth-Username

Fast re-authentication user name.

Type

26

Vendor ID

8164

VSA Type

304

Length

1–128

Value

Opaque value
SN-Firewall-Enabled

Firewall for subscriber enabled.

Type

26

Vendor ID

8164

VSA Type

198

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

SN-Firewall-Policy

This attribute contains the firewall policy name.

IMPORTANT:

This AVP was deprecated in StarOS 8.0, and was later reintroduced in StarOS 8.1.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this policy will not be applied.

Type

26

Vendor ID

8164

VSA Type

239

Length

1–63

Value

String
SN-FMC-Location

MAC address and CDMA location information.

Type

26

Vendor ID

8164

VSA Type

171

Length

1–247

Value

String
SN-GGSN-Address

The control plane IP address of the GGSN that handles one or more media component(s) of an IMS session.

Type

26

Vendor ID

8164

VSA Type

264

Length

4

Value

IPv4 address
SN-GGSN-MIP-Required

This attribute specifies if MIP is required for the GGSN subscriber.

Type

26

Vendor ID

8164

VSA Type

68

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-Gratuitous-ARP-Aggressive

This attribute specifies whether to generate a gratuitous ARP message whenever a MIP handoff or re-registration occurs. A non-zero of this attribute also configures the mode of operation when sending the gratuitous ARP, although only one mode (Aggressive) is supported at this time.

Type

26

Vendor ID

8164

VSA Type

54

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not send Gratuitous ARP
- Enabled = 1 — Send Gratuitous ARP in Aggressive mode

SN-GTP-Version

This attribute indicates the version of GTP the subscriber is using.

Type

26

Vendor ID

8164

VSA Type

62

Length

4

Value

Enumerated integer. Supported values are:

- GTP_VERSION_0 = 0
- GTP_VERSION_1 = 1
- GTP_VERSION_2 = 2

SN-HA-Send-DNS-ADDRESS

This attribute specifies if the HA should send the DNS address in the Mobile IP RRP message. The default is not to send the DNS address.

Type

26

Vendor ID

8164

VSA Type

47

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not send
- Enabled = 1 — Send

SN-Handoff-Indicator

This attribute indicates whether the Accounting Interim is sent because of the interim or not.

Type

26

Vendor ID

8164

VSA Type

310

Length

1

Value

Enumerated integer. Supported values are:

- Active-Handoff = 0
- Location-Update = 1

SN-Home-Behavior

This attribute specifies the configuration for the behavior bits settings for a home subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for “home” subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by “Or”ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

119

Length

4

Value

Unsigned integer
SN-Home-Profile

This attribute specifies the configuration for the profile bits settings for a home subscriber in an APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

109

Length

4

Value

Unsigned integer
SN-Home-Sub-Use-GGSN

This attribute configures GGSN to accept GGSN's charging characteristics for home subscribers defined for the APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

106

Length

4

Value

Enumerated integer. Supported values are:

- Deny = 0
- Accept = 1

SN-IMS-AM-Address

IMS application manager address.

Type

26

Vendor ID

8164

VSA Type

167

Length

4

Value

IPv4 address
SN-IMS-AM-Domain-Name

IMS application manager domain name.

Type

26

Vendor ID

8164

VSA Type

168

Length

1–64

Value

String
SN-IMS-Charging-Identifier

This attribute holds the IMS Charging Identifier (ICID) as generated by an IMS node for a SIP session.

Type

26

Vendor ID

8164

VSA Type

260

Length

4

Value

ASCII string
SN-IMSI

SN-IMSI

Type

26

Vendor ID

8164

VSA Type

252

Length

1–8

Value

Opaque value
SN-Inactivity-Time

This attribute contains the inactivity time duration for a subscriber session under long time duration timer configuration.

Type

26

Vendor ID

8164

VSA Type

232

Length

4

Value

Integer
SN-Internal-SM-Index

SN-Internal-SM-Index

Type

26

Vendor ID

8164

VSA Type

122

Length

4

Value

Unsigned integer
SN-IP-Alloc-Method

This attribute specifies the method for allocating an IP address. This feature only applies to the GGSN service.

Type

26

Vendor ID

8164

VSA Type

53

Length

4

Value

Enumerated integer. Supported values are:

- Alloc_Local_Pool = 0
- Alloc_Dhcp_Client = 1
- Alloc_Radius = 2
- Alloc_No_Alloc = 3
- Alloc_Static_Alloc = 4
- Alloc_Dhcp_Relay = 5

SN-IP-Filter-In

This attribute specifies the IP input filter rules to determine whether the traffic should undergo DPI processing.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this value will not be applied to the session.

Type

26

Vendor ID

8164

VSA Type

10

Length

1–253

Value

String
SN-IP-Filter-Out

This attribute specifies the IP output filter rules to determine whether the traffic should undergo DPI processing.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this value will not be applied to the session.

Type

26

Vendor ID

8164

VSA Type

11

Length

1–253

Value

String
SN-IP-Header-Compression

Specifies the IP header compression method to use.

Type

Type 26

Vendor ID

8164

VSA Type

150

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- VJ = 1
- ROHC = 2
- VJ_ROHC = 3

SN-IP-Hide-Service-Address

This attribute prevents subscribers from using traceroute to discover the public domain network addresses configured on HA and other services on the system.

Type

26

Vendor ID

8164

VSA Type

60

Length

4

Value

Enumerated integer. Supported values are:

- No = 0 — Disabled
- Yes = 1 — Enabled

SN-IP-In-ACL

This attribute contains a definition for one Input IP Access Control List, which is used to filter the IP packets coming from the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.

Type

26

Vendor ID

8164

VSA Type

17

Length

1–253

Value

ASCII string
SN-IP-In-Plcy-Grp

This attribute specifies the name of the policy group configuration applied in the uplink direction.

Type

26

Vendor ID

8164

VSA Type

193

Length

1–15

Value

String
SN-IP-Out-ACL

This attribute contains a definition for one Output IP Access Control List, which is used to filter the IP packets sent to the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.

Type

26

Vendor ID

8164

VSA Type

18

Length

1–253

Value

ASCII string
SN-IP-Out-Plcy-Grp

This attribute specifies the name of the policy group configuration applied in the downlink direction.

Type

26

Vendor ID

8164

VSA Type

194

Length

1–15

Value

String
SN-IP-Pool-Name

This vendor-specific attribute indicates the name of the IP pool from which an IP address should be allocated to the subscriber. Also, see Framed-Pool, which is the standard attribute accomplishing the same.

Type

26

Vendor ID

8164

VSA Type

8

Length

1–253

Value

ASCII string
SN-IP-Source-Validation

This attribute indicates if the source IP address should be validated before forwarding the IP packet.

Type

26

Vendor ID

8164

VSA Type

14

Length

4

Value

Enumerated integer. Supported values are:

- No = 0 — No Validation
- Yes = 1 — Validated

SN-IP-Source-Violate-No-Acct

This attribute excludes the Source Violated IP packets and byte counts when reporting the Octet and Packet count in an accounting message.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this value will not be applied to the session.

Type

26

Vendor ID

8164

VSA Type

196

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-IP-Src-Validation-Drop-Limit

Maximum number of packet drops entertained before disconnecting the session for source violated packets for the session.

Type

26

Vendor ID

8164

VSA Type

110

Length

4

Value

Unsigned integer
SN-IPv6-DNS-Proxy

IPV6 DNS proxy enabled or disabled setting for the session.

Type

26

Vendor ID

8164

VSA Type

126

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-IPv6-Egress-Filtering

This attribute enables egress filtering to make sure that packets being sent to the mobile device have an interface ID that matches that of the mobile device. This feature is meant to protect the Mobile from receiving unwanted packets from the Internet.

Type

26

Vendor ID

8164

VSA Type

103

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-IPv6-Min-Link-MTU

IPV6 MTU size.

Type

26

Vendor ID

8164

VSA Type

136

Length

4

Value

Unsigned integer
SN-IPv6-num-rtr-advt

This attribute indicates the IPv6 number of Initial Router Advertisements. The default value is 3.

Type

26

Vendor ID

8164

VSA Type

97

Length

4

Value

Unsigned integer
SN-IPv6-Primary-DNS

This attribute specifies a Primary DNS server address that the Router Advertisement message sent by the PDSN will include.

Type

26

Vendor ID

8164

VSA Type

101

Length

2

Value

IPv6 address
SN-IPv6-rtr-advt-interval

This attribute indicates the IPv6 Initial Router Advertisement Interval specified in milliseconds. The default value is 3000.

Type

26

Vendor ID

8164

VSA Type

96

Length

4

Value

Unsigned integer
SN-IPv6-Secondary-DNS

This attribute specifies a Secondary DNS server address that the Router Advertisement message sent by the PDSN will include.

Type

26

Vendor ID

8164

VSA Type

102

Length

16

Value

Opaque value
SN-IPv6-Sec-Pool

IPv6 secondary pool names.

Type

26

Vendor ID

8164

VSA Type

124

Length

1–253

Value

String
SN-IPv6-Sec-Prefix

IPv6 Secondary Pool name prefix.

Type

26

Vendor ID

8164

VSA Type

125

Length

2–18

Value

Opaque value
SN-ISC-Template-Name

This attribute contains name of the CSCF ISC template to be used for a subscriber.

Type

26

Vendor ID

8164

VSA Type

276

Length

0-255

Value

ASCII string
SN-Is-Unregistered-Subscriber

This attribute specifies if a subscriber is registered or not.

Type

26

Vendor ID

8164

VSA Type

269

Length

4

Value

ASCII string
SN-L3-to-L2-Tun-Addr-Policy

This attribute specifies the address allocation policy.

Type

26

Vendor ID

8164

VSA Type

43

Length

4

Value

Enumerated integer. Supported values are:

- no-local-alloc-validate = 0 — Do not locally allocate, do not validate
- local-alloc = 1 — Locally allocate
- local-alloc-validate = 2 — Locally allocate and validate

SN-Local-IP-Address

This attribute indicates the IP address of the local interface on the chassis for the user’s session.

Type

26

Vendor ID

8164

VSA Type

13

Length

4

Value

IPv4 address
SN-Long-Duration-Action

This attribute specifies the action to take place when the long duration timeout expires for a subscriber session.

Type

26

Vendor ID

8164

VSA Type

45

Length

4

Value

Enumerated integer. Supported values are:

- Detection = 1 — Detect the session and alert the administrator
- Disconnection = 2 — Disconnect the session
- Dormant-Only-Disconnection = 3
- Dormant-Only-Detection = 4

SN-Long-Duration-Notification

SN-Long-Duration-Notification.

Type

26

Vendor ID

8164

VSA Type

253

Length

4

Value

Enumerated integer. Supported values are:

- Suppress = 0
- Send = 1

SN-Long-Duration-Timeout

This attribute is used to detect and if necessary disconnect sessions connected to the PDSN. This attribute configures the time period, in seconds, before either alerting the administrator or disconnecting the subscriber.

Type

26

Vendor ID

8164

VSA Type

44

Length

4

Value

Integer
SN-Max-Sec-Contexts-Per-Subs

Maximum secondary PDP contexts per subscriber.

Type

26

Vendor ID

8164

VSA Type

290

Length

2

Value

Unsigned integer
SN-Mediation-Acct-Rsp-Action

When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the Mediation Accounting server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the Mediation Accounting server. When set to Delay_GTP_Response, the system does not send a GTP create PDP response to the GGSN until a response for the accounting start message is received from the Mediation Accounting server. If the AVP is not present in Access Accept message or if the AVP value is invalid, the value “None” is assumed.

Type

26

Vendor ID

8164

VSA Type

105

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- No_Early_PDUs = 1
- Delay_GTP_Response = 2

SN-Mediation-Enabled

This attribute indicates whether the Mediation Accounting configuration is enabled or disabled for GGSN.

If this AVP is not present in Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

123

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-Mediation-No-Interims

This attribute is used to disable or enable Mediation Interim Accounting Records for the session.

If this AVP is not present in Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

146

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-Mediation-VPN-Name

This attribute specifies the Mediation Context name for the session.

If this AVP is not received in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

104

Length

1–128

Value

String
SN-Min-Compress-Size

This attribute specifies the minimum size (in octets) a data packet can have in order to be compressed.

Type

26

Vendor ID

8164

VSA Type

23

Length

4

Value

Unsigned integer
SN-MIP-AAA-Assign-Addr

This attribute specifies if the PDSN/FA will allow AAA to assign the home address. The default is to not allow AAA to assign the home address.

Type

26

Vendor ID

8164

VSA Type

50

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not allow AAA to assign home address
- Enabled = 1 — Allow AAA to assign home address

SN-MIP-ANCID

Accounting correlation ID created by IPGW, received by VBM and HBM.

Type

26

Vendor ID

8164

VSA Type

166

Length

12

Value

Opaque value
SN-MIP-Dual-Anchor

Enable/disable dual-anchor service for a subscriber.

Type

26

Vendor ID

8164

VSA Type

165

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-MIP-HA-Assignment-Table

MIP-HA Assignment Table name. When this is received in an Access Accept message, the system uses this local table to get the HA Address.

Type

26

Vendor ID

8164

VSA Type

154

Length

1–253

Value

ASCII string
SN-MIP-Match-AAA-Assign-Addr

This attribute specifies if the PDSN/FA will enforce that a non-zero AAA-specified home address must match the home address present in the MIP RRQ from the mobile node, and disconnect the subscriber session if a match is not present. The default is not to force the addresses to match.

Type

26

Vendor ID

8164

VSA Type

51

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not force the AAA-specified home address to match RRQ
- Enabled = 1 — Force the AAA-specified home address to match RRQ

SN-MIP-Reg-Lifetime-Realm

Configure the maximum MIP registration lifetime for a subscriber/realm.

Type

26

Vendor ID

8164

VSA Type

175

Length

2

Value

Unsigned integer
SN-MIP-Send-Ancid

This attribute enables/disables sending ANCID from FA to HA in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

163

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-MIP-Send-Correlation-Info

This attribute enables/disables sending of correlation-id from FA to HA in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

188

Length

4

Value

Enumerated integer. In StarOS 8.1 and earlier, supported values are:

- Disabled = 0
- Enabled = 1

In StarOS 8.3 and later, supported values are:

- Disabled = 0
- NVSE_Starent = 1
- NVSE_CUstom1 = 2
- NVSE_Custom2 = 3

SN-MIP-Send-Host-Config

This attribute is used to enable/disable Host Config Extension in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

311

Length

1

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-MIP-Send-Imsi

AAA attribute to enable/disable sending IMSI from FA to HA in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

164

Length

4

Value

Enumerated integer. In StarOS and 8.1 and earlier, supported values are:

- None = 0
- Starent_NVSE = 1
- Custom1_NVSE = 2

In StarOS 8.3 and later, supported values are:

- Disabled = 0
- NVSE_Starent = 1
- NVSE_Custom1 = 2
- NVSE_Custom2 = 3

SN-MIP-Send-Term-Verification

This attribute specifies whether the PDSN/FA should send the Terminal Verification Normal Vendor/Organization Specific Extension (NVSE) in the Mobile IP RRQ message to the HA. The default is not to send the Terminal Verification NVSE.

Type

26

Vendor ID

8164

VSA Type

48

Length

4

Value

Enumerated integer. In StarOS 8.1 and earlier, supported values are:

- Disabled = 0 — Do not send
- Enabled = 1 — Send

In StarOS 8.3 and later, supported values are:

- Disabled = 0
- NVSE_Custom1 = 1 — Send custom NVSE
- NVSE_Custom2 = 2 — Send custom NVSE
- NVSE_Starent = 3 — Send custom NVSE

SN-MN-HA-Hash-Algorithm

This attribute contains the hash algorithm to use for MN-HA authentication.

Type

26

Vendor ID

8164

VSA Type

99

Length

4

Value

Enumerated integer. Supported values are:

- MD5 = 1
- MD5-RFC2002 = 2
- HMAC-MD5 = 3

SN-MN-HA-Timestamp-Tolerance

This attribute indicates the duration of timestamp tolerance, in seconds, to use for MN-HA authentication.

Type

26

Vendor ID

8164

VSA Type

30

Length

4

Value

Unsigned integer
SN-Mode

Robust Header Compression (ROHC) Mode. Reliable mode means each ROHC control needs to be Acknowledged. Optimistic mode is a modified version to reduce the number of control messages and bandwidth consumption. Unidirectional assumes a one way link without any Feedback from the decompressor.

Type

26

Vendor ID

8164

VSA Type

151

Length

4

Value

Enumerated integer. Supported values are:

- Reliable = 0
- Optimistic = 1
- Unidirectional = 2

SN-MS-ISDN

SN-MS-ISDN.

Type

26

Vendor ID

8164

VSA Type

248

Length

1–9

Value

Opaque value
SN-MSK-Lifetime

This attribute is currently not supported.
SN-NAI-Construction-Domain

This attribute specifies the domain name to use when constructing the NAI.

Type

26

Vendor ID

8164

VSA Type

37

Length

1–247

Value

String
SN-NAT-IP-Address

This attribute includes the NAT (public) IP address used for the call.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

297

Length

4

Value

IPv4 address
SN-Node-Functionality

This attribute includes the functionality identifier of the IMS node where the cause code was generated.

Type

26

Vendor ID

8164

VSA Type

268

Length

4

Value

Enumerated integer. Supported values are:

- S-CSCF = 0
- P-CSCF = 1
- I-CSCF = 2

SN-NPU-Qos-Priority

This attribute configures Inter-Subscriber priority Queueing based on class of service offered. Gold has highest priority and Best_effort lowest priority. From DSCP, means the priority queueing will be done based on the DSCP marking the incoming subscriber packet carries.

Type

26

Vendor ID

8164

VSA Type

98

Length

4

Value

Enumerated integer. Supported values are:

- Best_Effort = 0
- Bronze = 1
- Silver = 2
- Gold = 3
- From_DSCP = 4

SN-Ntk-Initiated-Ctx-Ind-Flag

Indicates whether the GGSN call is a network initiated PDP Context.

Type

26

Vendor ID

8164

VSA Type

142

Length

1

Value

Opaque value
SN-Ntk-Session-Disconnect-Flag

SN-Ntk-Session-Disconnect-Flag.

Type

26

Vendor ID

8164

VSA Type

143

Length

4

Value

Enumerated integer. Supported value is:

- Session-Disconnect = 1

SN-Nw-Reachability-Server-Name

This attribute specifies the name of the Network Reachability Detection Server.

Type

26

Vendor ID

8164

VSA Type

65

Length

1–16

Value

String
SN-Originating-IOI

This attribute holds the Inter Operator Identifier for the originating network in the home network of the originating end user.

Type

26

Vendor ID

8164

VSA Type

261

Length

1–253

Value

ASCII string
SN-Overload-Disc-Connect-Time

This attribute provides inactivity time for session to become candidate for disconnection during overload.

Type

26

Vendor ID

8164

VSA Type

233

Length

4

Value

Unsigned integer
SN-Overload-Disc-Inact-Time

This attribute provides inactivity time for session to become candidate for disconnection during overload.

Type

26

Vendor ID

8164

VSA Type

234

Length

4

Value

Unsigned integer
SN-Overload-Disconnect

This attribute enables (if one) and disables the overload-disconnect feature for a subscriber.

Type

26

Vendor ID

8164

VSA Type

235

Length

4

Value

Unsigned integer
SN-PDG-TTG-Required

TTG mode of operation Required for PDG.

Type

26

Vendor ID

8164

VSA Type

299

Length

1

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN-PDIF-MIP-Release-TIA

PDIF mobile IP release TIA.

Type

26

Vendor ID

8164

VSA Type

172

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN-PDIF-MIP-Required

PDIF mobile IP required.

Type

26

Vendor ID

8164

VSA Type

170

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN-PDIF-MIP-Simple-IP-Fallback

PDIF mobile IP simple IP fallback.

Type

26

Vendor ID

8164

VSA Type

173

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN-PDSN-Correlation-Id

Correlation ID received from PDSN to HA.

Type

26

Vendor ID

8164

VSA Type

189

Length

8

Value

Opaque value
SN-PDSN-Handoff-Req-IP-Addr

This attribute specifies if the PDSN should reject and terminate the subscriber session when the proposed address in IPCP by the mobile does not match the existing address in the PDSN. The default (Disabled) is not to reject these sessions.

Type

26

Vendor ID

8164

VSA Type

46

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not reject
- Enabled = 1 — Reject

SN-PDSN-NAS-Id

NAS Identifier received from PDSN to HA

Type

26

Vendor ID

8164

VSA Type

190

Length

1–253

Value

String
SN-PDSN-NAS-IP-Address

NAS IP address received from PDSN to HA.

Type

26

Vendor ID

8164

VSA Type

191

Length

4

Value

IPv4 address
SN-Permit-User-Mcast-PDUs

Specifies whether or not to let the subscriber discard multicast PDUs.

Type

26

Vendor ID

8164

VSA Type

134

Length

2

Value

Enumerated integer. Supported values are:

- disabled = 0
- enabled = 1

SN-PPP-Accept-Peer-v6Ifid

This attribute indicates the acceptance of the interface ID provided by peer during PPP IPv6CP if the ID is valid. The default is disabled.

Type

26

Vendor ID

8164

VSA Type

95

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not accept interface ID
- Enabled = 1 — Accept interface ID

SN-PPP-Always-On-Vse

SN-PPP-Always-On-Vse.

Type

26

Vendor ID

8164

VSA Type

130

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-PPP-Data-Compression

This attribute indicates the PPP data compression algorithm to use for the PPP session. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.

Type

26

Vendor ID

8164

VSA Type

9

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Stac-LZS = 1
- MPPC = 2
- Deflate = 4

SN-PPP-Data-Compression-Mode

This attribute indicates the PPP data compression mode to use for the PPP session when PPP data compression is used.

Type

26

Vendor ID

8164

VSA Type

19

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Stateless = 1

SN-PPP-Keepalive

This attribute indicates the interval for the PPP keepalive, in seconds.

Type

26

Vendor ID

8164

VSA Type

16

Length

4

Value

Unsigned integer
SN-PPP-NW-Layer-IPv4

This attribute indicates the PPP IPCP negotiation for IPv4. The default is enabled.

Type

26

Vendor ID

8164

VSA Type

92

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — IPCP negotiation for IPv4 is disabled.
- Enabled = 1 — IPCP negotiation for IPv4 is enabled.
- Passive = 2 — Start the negotiation only if peer initiates it.

SN-PPP-NW-Layer-IPv6

This attribute indicates the PPP IPv6CP negotiation for IPv6. The default is enabled.

Type

26

Vendor ID

8164

VSA Type

93

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — IPCP negotiation for IPv6 is disabled.
- Enabled = 1 — IPCP negotiation for IPv6 is enabled.
- Passive = 2 — Start the negotiation only if peer initiates it.

SN-PPP-Outbound-Password

This attribute indicates the password to be used when the user side of the PPP connection requires authentication.

Type

26

Vendor ID

8164

VSA Type

15

Length

1–247

Value

ASCII string
SN-PPP-Outbound-Username

This attribute indicates the username to be used when the user side of the PPP connection requires authentication.

Type

26

Vendor ID

8164

VSA Type

61

Length

1–247

Value

ASCII string
SN-PPP-Progress-Code

This attribute provides information about the “state” of the PPP connection, when the connection was terminated.

Type

26

Vendor ID

8164

VSA Type

4

Length

4

Value

Enumerated integer. Supported values are:

- Not-Defined = 0
- Call-Lcp-Down = 10
- Call-Disconnecting = 20
- Call-Ppp-Renegotiating = 30
- Call-Arrived = 40
- Call-Pdg-Tcp-Connecting = 45
- Call-Pdg-Ssl-Connecting = 46
- Call-Lcp-Up = 50
- Call-Authenticating = 60
- Call-Bcmcs-Authenticating = 70
- Call-Authenticated = 80
- Call-Tunnel-Connecting = 85
- Call-Ipcp-Up = 90
- Call-Imsa-Authorizing = 95
- Call-Imsa-Authorized = 97
- Call-MBMS-UE-Authorizing = 98
- Call-MBMS-Bearer-Authorizing = 99
- Call-Simple-IP-Connected = 100
- Call-Mobile-IP-Connected = 110
- Call-Tunnel-Connected = 115
- Call-Pdp-Type-IP-Connected = 120
- Call-Pdp-Type-IPv6-Connected = 125
- Call-Pdp-Type-PPP-Connected = 130
- Call-Proxy-Mobile-IP-Connected = 140
- Call-Pdg-Connected = 142
- Call-Pdg-Ssl-Connected = 141
- Call-Pdg-Connected = 142
- Call-Pdg-Connected = 142
- Call-Ipsg-Connected = 145
- Call-Bcmcs-Connected = 150
- Call-MBMS-UE-Connected = 155
- Call-MBMS-Bearer-Connected = 156
- Call-Pending-Addr-From-DHCP = 160
- Call-Got-Addr-From-DHCP = 170
- Call-HA-IPSEC-Tunnel-Connecting = 180
- Call-HA-IPSEC-Connected = 190
- Call-ASN-Non-Anchor-Connected = 200
- Call-ASNPC-Connected = 210
- Call-Mobile-IPv6-Connected = 220
- Call-PMIPv6-Connected = 221
- Call-PHSPC-Connected = 230
- Call-GTP-IPv4-Connected = 235
- Call-GTP-IPv6-Connected = 236
- Call-GTP-IPv4-IPv6-Connected = 237
- Call-SGW-Connected = 245
- Call-MME-Attached = 246
- Call-Auth-Only-Connected = 247

SN-PPP-Reneg-Disc

PPP remote reneg disconnect policy

Type

26

Vendor ID

8164

VSA Type

187

Length

4

Value

Enumerated integer. Supported values are:

- Never = 0
- Always = 1
- NAI_Prefix_MSID_Mismatch = 2

SN-Prepaid

Prepaid

Type

26

Vendor ID

8164

VSA Type

128

Length

4

Value

Enumerated integer. Supported values are:

- no_prepaid = 0
- custom_prepaid = 1
- standard_prepaid = 2
- wimax_prepaid = 4

SN-Prepaid-Compressed-Count

This attribute indicates if a Pre-paid subscriber's byte usage should be counted on the basis of compressed or uncompressed byte data over the subscriber's PPP connection to the system. If not present, the default is to count uncompressed byte data.

Type

26

Vendor ID

8164

VSA Type

31

Length

4

Value

Enumerated integer. Supported values are:

- Uncompressed = 0
- Compressed = 1

SN-Prepaid-Final-Duration-Alg

For prepaid, final duration is calculated based on the algorithm specified by the value of this attribute.

If this AVP is not received in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

135

Length

4

Value

Enumerated integer. Supported values are:

- current_time = 0
- last-user-layer3-activity-time = 1
- last-airlink-activity-time = 2
- last-airlink-activity-time-last-reported = 3

SN-Prepaid-Inbound-Octets

In an Access-Accept, this indicates how many additional inbound (bytes delivered to the subscriber) byte credits should be granted to the subscriber. In an Accounting- Request, this indicates how many total inbound byte credits have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on an inbound octet basis.

Type

26

Vendor ID

8164

VSA Type

32

Length

4

Value

Unsigned integer
SN-Prepaid-Outbound-Octets

Type

26

Vendor ID

8164

VSA Type

33

Length

4

Value

Unsigned integer
SN-Prepaid-Preference

This attribute specifies whether prepaid is volume based or duration based.

Type

26

Vendor ID

8164

VSA Type

129

Length

4

Value

Enumerated integer. Supported values are:

- prepaid_duration = 0
- prepaid_volume = 1

SN-Prepaid-Timeout

This attribute indicates how much time may elapse before a new request for more pre-paid credits is issued. If the specified time has elapsed since the prior grant of credits was received from the RADIUS server, then a new request for credits is issued. This attribute is primarily used to periodically update the subscriber of new credits issued since the subscriber was connected. Note that credit requests will still be made on behalf of the subscriber when the subscriber drops down to the low watermark of credits (or zero if there is no low watermark). The presence or absence of this attribute does not affect that mechanism in any way. However, this timer is re-set whenever any grant of credits is received on behalf of the subscriber, regardless of why the grant of credits was requested.

Type

26

Vendor ID

8164

VSA Type

35

Length

4
SN-Prepaid-Total-Octets

In an Access-Accept, this attribute indicates how many additional byte credits (combining both inbound and outbound counts) should be granted to the subscriber. In an Accounting- Request, this indicates how many total bytes credits (combined inbound and outbound) have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on a combined inbound and outbound octet-count basis.

Type

26

Vendor ID

8164

VSA Type

34

Length

4

Value

Unsigned integer
SN-Prepaid-Watermark

This attribute Indicates the percentage of remaining granted credits that will trigger a new request to grant credits from the RADIUS server. For example, if 1GB of credits was granted to a user, and the value of SN-Prepaid-Watermark was 10, then when 100 MB of credits are remaining (900 MB have been used) to the subscriber, a new request for any new byte credits is issued on behalf of the subscriber. Note that when calculating the pre-paid low watermark, the total credits granted for the subscriber's entire session is used.

Type

26

Vendor ID

8164

VSA Type

36

Length

4

Value

Unsigned integer
SN-Primary-DCCA-Peer

This attribute indicates the name of the primary DCCA peer and primary DCCA realm.

If this AVP is received in Access Accept message, the primary DCCA peer is used for Gy functionality. If not present in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

223

Length

1-192

Value

A colon separated string, like “primary_peer : primary_realm”
SN-Primary-DNS-Server

This attribute indicates the IP address of the primary DNS server that should be used for the session.

Type

26

Vendor ID

8164

VSA Type

5

Length

4

Value

IPv4 address
SN-Primary-NBNS-Server

Primary NBNS Server IP address.

Type

26

Vendor ID

8164

VSA Type

148

Length

4

Value

IPv4 address
SN-Proxy-MIP

This attribute specifies if the PDSN/FA will perform compulsory Proxy-MIP tunneling for a Simple-IP PDSN subscriber. This feature is licensed. The default is not to perform compulsory Proxy-MIP.

Type

26

Vendor ID

8164

VSA Type

52

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not perform compulsory Proxy-MIP
- Enabled = 1 — Perform compulsory Proxy-MIP

SN-Proxy-MIPV6

Enable/disable PMIPv6 for a subscriber.

Type

26

Vendor ID

8164

VSA Type

65530

Length

8

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-Pseudonym-Username

This attribute contains the pseudonym user name generated by AAA server.

Type

26

Vendor ID

8164

VSA Type

305

Length

1-256

Value

Opaque value
SN-QoS-Background-Class

This attribute defines the QOS Background Traffic Class.

Type

26

Vendor ID

8164

VSA Type

91

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN-QoS-Class-Background-PHB

Quality of Service DSCP classification value.

Type

26

Vendor ID

8164

VSA Type

113

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN-QoS-Class-Conversational-PHB

Quality of Service DSCP classification value.

Type

26

Vendor ID

8164

VSA Type

111

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN-QoS-Class-Interactive-1-PHB

Interactive-1 class PHB value.

Type

26

Vendor ID

8164

VSA Type

114

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN-QoS-Class-Interactive-2-PHB

Interactive-2 class PHB.

Type

26

Vendor ID

8164

VSA Type

115

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN-QoS-Class-Interactive-3-PHB

Interactive-3 class PHB.

Type

26

Vendor ID

8164

VSA Type

115

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN-QoS-Class-Streaming-PHB

Quality of Service DSCP classification value.

Type

26

Vendor ID

8164

VSA Type

112

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN-QoS-Conversation-Class

This attribute defines the QOS Conversation Traffic Class.

Type

26

Vendor ID

8164

VSA Type

86

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN-QOS-HLR-Profile

QoS with Allocation Retention bit. QoS structured as per 29.002.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

303

Length

1–35

Value

Opaque value
SN-QoS-Interactive1-Class

This attribute defines the QOS Interactive TrafficClass.

Type

26

Vendor ID

8164

VSA Type

88

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN-QoS-Interactive2-Class

This attribute defines the QOS Interactive2 Traffic Class.

Type

26

Vendor ID

8164

VSA Type

89

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN-QoS-Interactive3-Class

This attribute defines the QOS Interactive3 Traffic Class.

Type

26

Vendor ID

8164

VSA Type

90

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN-QoS-Negotiated

Negotiated QoS for GGSN sessions.

Type

26

Vendor ID

8164

VSA Type

147

Length

In 10.2 and earlier releases: 4–17

In 11.0 and later releases: 4–20

Value

ASCII string
SN-QoS-Renegotiation-Timeout

This attribute configures the timeout duration of dampening time for dynamic QoS renegotiation.

Type

26

Vendor ID

8164

VSA Type

145

Length

4

Value

Unsigned integer
SN-QoS-Streaming-Class

This attribute defines the QOS Streaming Traffic Class.

Type

26

Vendor ID

8164

VSA Type

87

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN-QoS-Tp-Dnlk

This attribute enables/disables Traffic Policing/Shaping in downlink direction.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

73

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Policing = 1
- Shaping = 2

SN-QoS-Tp-Uplk

This attribute enables/disables Traffic Policing/Shaping in uplink direction.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

79

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Policing = 1
- Shaping = 2

SN-QoS-Traffic-Policy

This compound attribute simplifies sending QoS values for Traffic Class, Direction, Burst-Size, Committed-Data-Rate, Peak-Data-Rate, Exceed-Action, and Violate-Action from the RADIUS server. When the SN-QoS-Traffic-Policy attribute is sent along with Acct-Session-ID attribute, the system matches the particular PDP context, and applies the new policy and retains the policy with the subscriber profile for future use. The next time the system sends a CoA request with a new policy and a different Acct-Session-ID for the same subscriber, the previously received policy is also applied to the matching PDP context along with the new policy.

IMPORTANT:

This attribute is specific to the GGSN service.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

177

Value

Contains the following subattributes:
Direction

Direction of traffic.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

1

Length

1

Value

Unsigned integer Supported values are:

- Downlink = 0
- Uplink = 1

Class

Traffic class.

Type

2

Length

1

Value

Unsigned integer Supported values are:

- Undefined = 0
- Conversational = 1
- Streaming = 2
- Interactive TP 1 = 4
- Interactive TP 2 = 5
- Interactive TP 3 = 6
- Background = 7

Burst-Size

Peak burst size.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

3

Length

4

Value

Unsigned integer
Committed-Data-Rate

Committed data rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

4

Length

4

Value

Unsigned integer
Peak-Data-Rate

Peak data rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

5

Length

4

Value

Unsigned integer
Exceed-Action

Action to take on packets that exceed the Committed-Data-Rate but do not violate the Peak-Data-Rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

6

Length

1

Value

Unsigned integer Supported values are:

- Transmit = 0
- Drop = 1
- Lower IP Precedence = 2

Violate-Action

Violate action.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

7

Length

1

Value

Unsigned integer Supported values are:

- Transmit = 0
- Drop = 1
- Lower IP Precedence = 2
- Buffer = 3
- Buffer-Transmit-On-Full = 4

Auto-Readjust-Enabled

Available only in StarOS 8.1 and later. Auto-readjust enabled.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

8

Length

1

Value

Unsigned integer
Auto-Readjust-Duration

Available only in StarOS 8.1 and later. Auto-readjust duration.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

9

Length

4

Value

Unsigned integer
Qci

Available only in 11.0 and later releases. QOS QCI accepted values are 1 (qci 1), 2 (qci 2), 3 (qci 3), 4 (qci 4), 5 (qci 5), 6 (qci 6), 7 (qci 7), 8 (qci 8), 9 (qci 9).

Type

10

Length

1

Value

Unsigned integer
SN-Rad-APN-Name

This attributes specifies the RADIUS returned APN name.

If this AVP is not present in the Access Accept message or if the AVP value is invalid, the SGSN supplied APN value in create PDP context will be used for the session.

Type

26

Vendor ID

8164

VSA Type

162

Length

1–64

Value

Opaque value
SN-Radius-Returned-Username

This attribute is used to prefer RADIUS returned user name over constructed user name in the accounting messages.

Type

26

Vendor ID

8164

VSA Type

236

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN-Re-CHAP-Interval

The Periodic CHAP authentication interval for PPP, in seconds.

Type

26

Vendor ID

8164

VSA Type

7

Length

4

Value

Unsigned integer
SN-Roaming-Behavior

This attribute specifies the configuration for the behavior bits settings for a roaming subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for "roaming" subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by "Or"ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

121

Length

4

Value

Unsigned integer
SN-Roaming-Profile

This attribute specifies the configuration for the profile bits settings for a roaming subscriber in an APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

118

Length

4

Value

Unsigned integer
SN-Roaming-Sub-Use-GGSN

This attribute configures GGSN to accept GGSN's charging characteristics for roaming subscribers defined for the APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

108

Length

4

Value

Enumerated integer. Supported values are:

- Deny = 0
- Accept = 1

SN-ROHC-Flow-Marking-Mode

Configure ROHC compression for marked flows only.

Type

26

Vendor ID

8164

VSA Type

274

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

SN-ROHC-Mode

ROHC Mode.

Type

26

Vendor ID

8164

VSA Type

151

Length

4

Value

An integer in network order. Supported values are:

- Reliable = 0
- Optimistic = 1
- Unidirectional = 2

SN-ROHC-Profile-Name

Specifies the ROHC profile to use for the subscriber.

Type

26

Vendor ID

8164

VSA Type

238

Length

1–64

Value

ASCII string
SN-Role-Of-Node

This attribute denotes the role of the CSCF.

Type

26

Vendor ID

8164

VSA Type

256

Length

4

Value

Enumerated integer. Supported values are:

- ORIGINATING_ROLE = 0
- TERMINATING_ROLE = 1

SN-Routing-Area-Id

For GGSN calls this indicates the Routing Area ID of the subscriber.

Type

26

Vendor ID

8164

VSA Type

249

Length

3

Value

String
SN-Rulebase

When the session is active charging enabled, Rulebase name will specify one of the pre configured ECSv2 rulebases in active charging subsystem.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN, this value will not be applied to the session.

Type

26

Vendor ID

8164

VSA Type

249

Length

1–64

Value

String
SN-SDP-Media-Components

This attribute is currently not supported. See SN-CSCF-Rf-SDP-Media-Components.
SN-SDP-Session-Description

This attribute contains the Session portion of the SDP data exchanged between the User Agents in the SIP transaction.

Type

26

Vendor ID

8164

VSA Type

263

Length

4

Value

ASCII string
SN-Sec-IP-Pool-Name

Available only in StarOS 8.1 and later. This attribute contains the secondary IP pool name.

Type

26

Vendor ID

8164

VSA Type

265

Length

1–253

Value

String
SN-Secondary-DCCA-Peer

This attribute indicates the name of the Secondary DCCA peer and Secondary DCCA realm.

If this AVP is received in Access Accept message the secondary DCCA peer is used for Gy functionality. If not present in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

224

Length

1–192

Value

A colon separated string, like “secondary_peer : secondary_realm”.
SN-Secondary-DNS-Server

This attribute indicates the IP address of the secondary DNS server that should be used for the session.

Type

26

Vendor ID

8164

VSA Type

6

Length

4

Value

IPv4 address
SN-Secondary-NBNS-Server

Secondary NBNS server IP address.

Type

26

Vendor ID

8164

VSA Type

149

Length

4

Value

IPv4 address
SN-Served-Party-Address

This attribute is currently not supported.
SN-Service-Address

Used to send bind IP address of the service in RADIUS messages.

Type

26

Vendor ID

8164

VSA Type

169

Length

4

Value

IPv4 address
SN-Service-Type

This attribute indicates the service type that the user is accessing.

Type

26

Vendor ID

8164

VSA Type

24

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- PDSN = 1
- Management = 2
- HA = 3
- GGSN = 4
- LNS = 5
- IPSG = 6
- CSCF = 7
- ASNGW = 8
- PDIF = 9
- STANDALONE_FA = 10
- SGSN = 11
- PHSGW = 12
- PDG = 13
- MIPV6HA = 14
- PGW = 15
- SGW = 16
- FNG = 17
- OGW = 18 — NOTE: Applicable only in release 12.0.
- HNBGW = 19
- BNG = 20

SN-Session-Id

This attribute contains Call-ID of the SIP session.

Type

26

Vendor ID

8164

VSA Type

257

Length

4

Value

ASCII string
SN-Simultaneous-SIP-MIP

This attribute indicates if a PDSN Subscriber can simultaneously be given Simple IP and Mobile IP service.

Type

26

Vendor ID

8164

VSA Type

22

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-SIP-Method

This attribute identifies the SIP-method for which acct request is sent.

Type

26

Vendor ID

8164

VSA Type

254

Length

4

Value

ASCII string
SN-SIP-Request-Time-Stamp

This attribute specifies the time of initial SIP request.

Type

26

Vendor ID

8164

VSA Type

258

Length

4

Value

ASCII string
SN-SIP-Response-Time-Stamp

This attribute specifies the time of response to initial SIP request.

Type

26

Vendor ID

8164

VSA Type

259

Length

4

Value

ASCII string
SN-Software-Version

Provides the Software version. This contains the major version number, minor version number and build number.

Type

26

Vendor ID

8164

VSA Type

288

Length

1–32

Value

ASCII string
SN-Subs-Acc-Flow-Traffic-Valid

This attribute indicates the subscriber account flow traffic is valid.

Type

26

Vendor ID

8164

VSA Type

225

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN-Subscriber-Accounting

This attribute specifically enables or disables subscriber accounting. Note that if enabled, subscriber accounting still needs to be enabled in the subscriber's AAA context for accounting to be performed.

The AVP value 0 means no accounting; 1 indicates RADIUS accounting; and 2 indicates GTPP accounting. If an invalid value is received or if the AVP is not present in the Access Accept message, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

64

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Radius = 1
- GTPP = 2

SN-Subscriber-Acct-Interim

This attribute specifies if accounting INTERIM messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context (along with a specific INTERIM interval), if accounting INTERIM messages are to be sent.

The AVP value 0 represents normal or enabled for generating accounting START messages. The value 1 represents enabled for suppressing RADIUS accounting START messages.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

70

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Suppress = 1

SN-Subscriber-Acct-Mode

This attribute contains the subscriber accounting mode.

Type

26

Vendor ID

8164

VSA Type

192

Length

4

Value

Enumerated integer. Supported values are:

- flow-based-auxilliary = 0
- flow-based-all = 1
- flow-based-none = 2
- session-based = 3
- main-a10-only = 4

SN-Subscriber-Acct-Rsp-Action

When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the RADIUS server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the RADIUS server. When set to Delay_GTP_Response, the system does not send a GTP create response to the GGSN until a response for the accounting start message is received from the RADIUS server.

Type

26

Vendor ID

8164

VSA Type

100

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- No_Early_PDUs = 1
- Delay_GTP_Response = 2

SN-Subscriber-Acct-Start

This attribute specifies if accounting START messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting START messages are to be sent.

The AVP value 0 represents normal or enabled for generating accounting START messages. The value 1 represents enabled for suppressing RADIUS accounting START messages.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

69

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Suppress = 1

SN-Subscriber-Acct-Stop

This attribute specifies if accounting STOP messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting STOP messages are to be sent.

The AVP value 0 represents normal or enabled for generating accounting STOP messages. The value 1 represents enabled for suppressing RADIUS accounting STOP messages.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

71

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Suppress = 1

SN-Subscriber-Class

Customer-specific attribute to support specific subscriber billing behavior.

Type

26

Vendor ID

8164

VSA Type

219

Length

4

Value

Enumerated integer. Supported values are:

- Normal_Subscriber = 0
- Ting_100 = 1
- Ting_500 = 2
- Ting_Buddy = 3
- Ting_Star = 4
- Ting_Nolimit_SMS = 5
- Kids_Locator = 6
- Ting_2000 = 7
- Handicapped_Welfare = 8
- Reserved = 9

SN-Subscriber-Dormant-Activity

This attribute specifies whether to treat dormant packets routed to the mobile as activity for idle timeout purposes. The default is Enabled. Disabled means dormant packets routed to the mobile is not treated as activity for idle timeout purposes.

Type

26

Vendor ID

8164

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-Subscriber-IP-Hdr-Neg-Mode

This attribute specifies whether to wait (detect) for IP header compression to be requested by the mobile before responding, or not to wait (force). Force is the default.

Type

26

Vendor ID

8164

VSA Type

67

Length

4

Value

Enumerated integer. Supported values are:

- Force = 0
- Detect = 1

SN-Subscriber-IP-TOS-Copy

This attribute controls the copying of the IP TOS octet value from IPv4 datagrams to the IP header in tunnel encapsulation.

Type

26

Vendor ID

8164

VSA Type

85

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Access-Tunnel = 1
- Data-Tunnel = 2
- Both = 3

SN-Subscriber-Nexthop-Address

This attribute specifies the nexthop gateway address to be returned by AAA on a per subscriber basis.

Type

26

Vendor ID

8164

VSA Type

127

Length

4

Value

IPv4 address
SN-Subscriber-No-Interims

This is a GGSN specific attribute. When set to 0 (disabled) interim accounting is generated. When set to 1 (enabled) interim accounting generation is disabled.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

133

Length

4

Value

Enumerated integer. Supported values are:

- Enabled = 0
- Disabled = 1

SN-Subscriber-Permission

This attribute indicates the services allowed to be delivered to the subscriber. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.

Type

26

Vendor ID

8164

VSA Type

20

Length

4

Value

Enumerated integer. In StarOS 8.1 and earlier, supported values are:

- None = 0
- Simple-IP = 1
- Mobile-IP = 2
- Simple-IP-Mobile-IP = 3
- HA-Mobile-IP = 4
- Simple-IP-HA-Mobile-IP = 5
- Mobile-IP-HA-Mobile-IP = 6
- All = 7

In StarOS 8.3 and later, supported values are:

- None = 0
- Simple-IP = 1
- Mobile-IP = 2
- Simple-IP-Mobile-IP = 3
- HA-Mobile-IP = 4
- Simple-IP-HA-Mobile-IP = 5
- Mobile-IP-HA-Mobile-IP = 6
- SIP-MIP-HA-MIP = 7
- GGSN-PDP-TYPE-IP = 0x08, # see SessSubscriberPermission in sess_common.x
- GGSN-PDP-TYPE-PPP = 0x10, # see SessSubscriberPermission in sess_common.x
- Network-Mobility = 0x20
- FA-HA-NEMO = 0x26
- All = 0x3F

SN-Subscriber-Template-Name

RADIUS returned subscriber template.

Type

26

Vendor ID

8164

VSA Type

158

Length

1–127

Value

String
SN-Subs-IMSA-Service-Name

IMS authorization service name.

Type

26

Vendor ID

8164

VSA Type

159

Length

1–128

Value

String
SN-Subs-VJ-Slotid-Cmp-Neg-Mode

Enable/Disable slot ID compression in either direction when using VJ compression.

Type

26

Vendor ID

8164

VSA Type

221

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Receive = 1
- Transmit = 2
- Both = 3

SN-Transparent-Data

This AVP is used by RADIUS to provide Global Title information for the GGSN to use in CDRs and Quota Auth.

Type

26

Vendor ID

8164

VSA Type

247

Length

In StarOS 8.1 and later: 1–247

In StarOS 8.0: 1–237

Value

Opaque value
SN-Terminating-IOI

This attribute holds the Inter Operator Identifier for the originating network in the home network of the terminating end user.

Type

26

Vendor ID

8164

VSA Type

262

Length

4

Value

ASCII string
SN-Tp-Dnlk-Burst-Size

This attribute specifies the Traffic Policing downlink burst size in bytes.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

76

Length

4

Value

Unsigned integer
SN-Tp-Dnlk-Committed-Data-Rate

This attribute specifies the Traffic Policing downlink committed data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

74

Length

4

Value

Unsigned integer
SN-Tp-Dnlk-Exceed-Action

This attribute specifies the action to take on Traffic Policing downlink packets that exceed the committed-data-rate but do not violate the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

77

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN-Tp-Dnlk-Peak-Data-Rate

This attribute specifies the Traffic Policing downlink peak data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

75

Length

4

Value

Unsigned integer
SN-Tp-Dnlk-Violate-Action

This attribute specifies the action to take on Traffic Policing downlink packets that exceed both the committed-data-rate and the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

78

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN-Tp-Uplk-Burst-Size

This attribute specifies the Traffic Policing uplink burst size in bytes.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

82

Length

4

Value

Unsigned integer
SN-Tp-Uplk-Committed-Data-Rate

This attribute specifies the Traffic Policing uplink committed data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

80

Length

4

Value

Unsigned integer
SN-Tp-Uplk-Exceed-Action

This attribute specifies the action to take on Traffic Policing uplink packets that exceed the committed-data-rate but do not violate the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

83

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN-Tp-Uplk-Peak-Data-Rate

This attribute specifies the Traffic Policing Uplink Peak Data Rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

81

Length

4

Value

Unsigned integer
SN-Tp-Uplk-Violate-Action

This attribute specifies the action to take on Traffic Policing uplink packets that exceed both the committed-data-rate and the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

84

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN-TPO-Policy

This attribute contains the TPO policy name.

Type

26

Vendor ID

8164

VSA Type

308

Length

1–63

Value

String
SN-Traffic-Group

This attribute is used to assign a tag to an FA or a group of FAs, so that traffic policy can be enforced based on the tag value.

Type

26

Vendor ID

8164

VSA Type

161

Length

2

Value

Unsigned integer
SN-TrafficSelector-Class

The ipsec traffic selector class.

Type

26

Vendor ID

8164

VSA Type

307

Length

4

Value

Unsigned integer
SN-Tun-Addr-Policy

Describes IP address validation policy for non L2TP tunneled calls.

Type

26

Vendor ID

8164

VSA Type

156

Length

4

Value

Enumerated integer. Supported values are:

- no-local-alloc-validate = 0
- local-alloc = 1
- local-alloc-validate = 2

SN-Tunnel-Gn

Used to enable/disable Gn interface from PDG/TTG to GGSN.

Type

26

Vendor ID

8164

VSA Type

174

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN-Tunnel-ISAKMP-Crypto-Map

This attribute specifies the system-defined crypto map to use for the subscriber's Mobile-IP connection, when IPSec is used to protect the Mobile-IP connection. This attribute is salt-encrypted.

Type

26

Vendor ID

8164

VSA Type

38

Length

1–128

Value

String
SN-Tunnel-ISAKMP-Secret

This attribute specifies the secret to use for IKE.

Type

26

Vendor ID

8164

VSA Type

39

Length

1–128

Value

String
SN-Tunnel-Load-Balancing

This attribute specifies the load-balancing algorithm to use when tunneling is employed.

Type

26

Vendor ID

8164

VSA Type

27

Length

4

Value

Enumerated integer. Supported values are:

- random = 1
- balanced = 2
- prioritized = 3

SN-Tunnel-Password

This attribute contains a secret for tunneling usage. Currently this is only used for L2TP. It is recommended that you use the Tunnel-Password attribute if your RADIUS server supports salt-encryption of attributes.

Type

26

Vendor ID

8164

VSA Type

26

Length

1–240

Value

Opaque value
SN-Unclassify-List-Name

Unclassify List Name.

Type

26

Vendor ID

8164

VSA Type

132

Length

1–32

Value

An ASCII string
SN-Virtual-APN-Name

This attribute contains the virtual APN name.

Type

26

Vendor ID

8164

VSA Type

94

Length

1–64

Value

ASCII string
SN-Visiting-Behavior

This attribute specifies the configuration for the behavior bits settings for a visiting subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for "home" subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by "Or"ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

120

Length

4

Value

Unsigned integer
SN-Visiting-Profile

This attribute specifies the configuration for the profile bits settings for a visiting subscriber in an APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

117

Length

4

Value

Unsigned integer
SN-Visiting-Sub-Use-GGSN

This attribute configures GGSN to accept GGSN's charging characteristics for visiting subscribers defined for the APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

107

Length

4

Value

Enumerated integer. Supported values are:

- Deny = 0
- Accept = 1

SN-Voice-Push-List-Name

SN-Voice-Push-List-Name.

Type

26

Vendor ID

8164

VSA Type

131

Length

1–32

Value

ASCII string
SN-VPN-ID

This attribute contains the Destination VPN of the user, specified by a 32-bit identifier.

Type

26

Vendor ID

8164

VSA Type

1

Length

4

Value

Unsigned integer
SN-VPN-Name

This attribute contains the name of the user’s Destination VPN.

Type

26

Vendor ID

8164

VSA Type

2

Length

1–253

Value

ASCII string
SN-WiMAX-Auth-Only

Specifies whether the call is established for Authentication Mode Only.

Type

26

Vendor ID

8164

VSA Type

306

Length

1

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Access-link-IP-Frag

This attribute specifies what to do when data received for the subscriber on the Access link that needs to be fragmented and the DF bit is either set or unset. The default is Normal.

Type

26

Vendor ID

8164

VSA Type

63

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0 — Data to be fragmented is not fragmented if the DF bit is set
- DF-Ignore = 1 — Fragment regardless
- DF-Fragment-ICMP-Notify = 2 — Fragment regardless, and ICMP Notify if DF bit is set

SN1-Acct-Input-Giga-Dropped

This attribute contains the number of input gigawords dropped if the number of input bytes is greater than 2^32 - 1

Type

26

Vendor ID

8164

VSA Type

230

Length

4

Value

Unsigned integer
SN1-Acct-Input-Octets-Dropped

This attribute contains the number of input bytes dropped.

Type

26

Vendor ID

8164

VSA Type

228

Length

4

Value

Unsigned integer
SN1-Acct-Input-Packets-Dropped

This attribute contains the number of input packets dropped.

Type

26

Vendor ID

8164

VSA Type

226

Length

4

Value

Unsigned integer
SN1-Acct-Output-Giga-Dropped

This attribute contains the number of output gigawords dropped if the number of output bytes is greater than 2^32 - 1.

Type

26

Vendor ID

8164

VSA Type

231

Length

4

Value

integer
SN1-Acct-Output-Octets-Dropped

This attribute contains the number of output bytes dropped.

Type

26

Vendor ID

8164

VSA Type

229

Length

4

Value

Integer
SN1-Acct-Output-Packets-Dropped

This attribute contains the number of output packets dropped.

Type

26

Vendor ID

8164

VSA Type

227

Length

4

Value

Integer
SN1-Admin-Expiry

This attribute contains the date/time the administrative user account expires. It is an integer value specifying the number of seconds since the UNIX epoch at which time the account will expire.

Type

26

Vendor ID

8164

VSA Type

72

Length

4

Value

Integer
SN1-Admin-Permission

This attribute indicates the services allowed to be delivered to the administrative user. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.

Type

26

Vendor ID

8164

VSA Type

21

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- CLI = 1
- FTP = 2
- CLI-FTP = 3
- Intercept = 4
- CLI-Intercept = 5
- CLI-Intercept-FTP = 7
- ECS = 8
- CLI-ECS = 9
- CLI-FTP-ECS = 11
- CLI-Intercept-ECS = 13
- CLI-Intercept-FTP-ECS = 15

SN1-Assigned-VLAN-ID

The VLAN ID assigned to the subscriber.

Type

26

Vendor ID

8164

VSA Type

152

Length

4

Value

Unsigned integer
SN1-Call-Id

Internal system generated call ID number for the session.

Type

26

Vendor ID

8164

VSA Type

251

Length

4

Value

Unsigned integer
SN1-Cause-For-Rec-Closing

This attribute contains a reason for the release of the CDR.

Type

26

Vendor ID

8164

VSA Type

139

Length

4

Value

Enumerated integer. Supported values are:

- normalRelease = 0
- abnormalRelease = 4
- volumeLimit = 16
- timeLimit = 17
- SGSNChange = 18
- maxChangeCond = 19
- managementIntervention = 20

SN1-CFPolicy-ID

This attribute contains the Content Filtering policy ID.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

220

Length

4

Value

Unsigned integer
SN1-Change-Condition

This attribute defines the reason for closing the container.

Type

26

Vendor ID

8164

VSA Type

140

Length

4

Value

Enumerated integer. Supported values are:

- QOSCHANGE = 0
- TARIFFTIMECHANGE = 1
- SGSNCHANGE = 500

SN1-Charging-VPN-Name

Charging VPN Name.

Type

26

Vendor ID

8164

VSA Type

137

Length

1–252

Value

String
SN1-Chrg-Char-Selection-Mode

This attribute contains the charging characteristics type that the GSNs applied to the CDR.

Type

26

Vendor ID

8164

VSA Type

138

Length

4

Value

Integer. Supported values are:

- SGSN = 0
- HOME = 3
- ROAMING = 4
- VISITING = 5

SN1-Data-Tunnel-Ignore-DF-Bit

This attribute specifies if the PDSN/FA or HA should ignore the DF bit in the IPv4 header when encapsulating the IPv4 packet in MIP, and therefore fragmenting the resulting tunneled packet if necessary. The default is not to ignore the DF bit.

Type

26

Vendor ID

8164

VSA Type

49

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not ignore DF bit
- Enabled = 1 — Ignore DF bit

SN1-DHCP-Lease-Expiry-Policy

This attribute specifies whether to renew or disconnect on expiry of IP address lease time.

Type

26

Vendor ID

8164

VSA Type

157

Length

4

Value

Enumerated integer. Supported values are:

- auto-renew = 0
- disconnect = 1

SN1-Disconnect-Reason

This attribute contains the reason the user was disconnected from service.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

3

Length

4

Value

Enumerated integer. Supported values are:

- Not-Defined = 0
- Admin-Disconnect = 1
- Remote-Disconnect = 2
- Local-Disconnect = 3
- Disc-No-Resource = 4
- Disc-Excd-Service-Limit = 5
- PPP-LCP-Neg-Failed = 6
- PPP-LCP-No-Response = 7
- PPP-LCP-Loopback = 8
- PPP-LCP-Max-Retry = 9
- PPP-Echo-Failed = 10
- PPP-Auth-Failed = 11
- PPP-Auth-Failed-No-AAA-Resp = 12
- PPP-Auth-No-Response = 13
- PPP-Auth-Max-Retry = 14
- Invalid-AAA-Attr = 15
- Failed-User-Filter = 16
- Failed-Provide-Service = 17
- Invalid-IP-Address-AAA = 18
- Invalid-IP-Pool-AAA = 19
- PPP-IPCP-Neg-Failed = 20
- PPP-IPCP-No-Response = 21
- PPP-IPCP-Max-Retry = 22
- PPP-No-Rem-IP-Address = 23
- Inactivity-Timeout = 24
- Session-Timeout = 25
- Max-Data-Excd = 26
- Invalid-IP-Source-Address = 27
- MSID-Auth-Failed = 28
- MSID-Auth-Failed-No-AAA-Resp = 29
- A11-Max-Retry = 30
- A11-Lifetime-Expired = 31
- A11-Message-Integrity-Failure = 32
- PPP-lcp-remote-disc = 33
- Session-setup-timeout = 34
- PPP-keepalive-failure = 35
- Flow-add-failed = 36
- Call-type-detection-failed = 37
- Wrong-ipcp-params = 38
- MIP-remote-dereg = 39
- MIP-lifetime-expiry = 40
- MIP-proto-error = 41
- MIP-auth-failure = 42
- MIP-reg-timeout = 43
- Invalid-dest-context = 44
- Source-context-removed = 45
- Destination-context-removed = 46
- Req-service-addr-unavailable = 47
- Demux-mgr-failed = 48
- Internal-error = 49
- AAA-context-removed = 50
- invalid-service-type = 51
- mip-relay-req-failed = 52
- mip-rcvd-relay-failure = 53
- ppp-restart-inter-pdsn-handoff = 54
- gre-key-mismatch = 55
- invalid_tunnel_context = 56
- no_peer_lns_address = 57
- failed_tunnel_connect = 58
- l2tp-tunnel-disconnect-remote = 59
- l2tp-tunnel-timeout = 60
- l2tp-protocol-error-remote = 61
- l2tp-protocol-error-local = 62
- l2tp-auth-failed-remote = 63
- l2tp-auth-failed-local = 64
- l2tp-try-another-lns-from-remote = 65
- l2tp-no-resource-local = 66
- l2tp-no-resource-remote = 67
- l2tp-tunnel-disconnect-local = 68
- l2tp-admin-disconnect_remote = 69
- l2tpmgr-reached-max-capacity = 70
- MIP-reg-revocation = 71
- path-failure = 72
- dhcp-relay-ip-validation-failed = 73
- gtp-unknown-pdp-addr-or-pdp-type = 74
- gtp-all-dynamic-pdp-addr-occupied = 75
- gtp-no-memory-is-available = 76
- dhcp-relay-static-ip-addr-not-allowed = 77
- dhcp-no-ip-addr-allocated = 78
- dhcp-ip-addr-allocation-tmr-exp = 79
- dhcp-ip-validation-failed = 80
- dhcp-static-addr-not-allowed = 81
- dhcp-ip-addr-not-available-at-present = 82
- dhcp-lease-expired = 83
- lpool-ip-validation-failed = 84
- lpool-static-ip-addr-not-allowed = 85
- static-ip-validation-failed = 86
- static-ip-addr-not-present = 87
- static-ip-addr-not-allowed = 88
- radius-ip-validation-failed = 89
- radius-ip-addr-not-provided = 90
- invalid-ip-addr-from-sgsn = 91
- no-more-sessions-in-aaa = 92
- ggsn-aaa-auth-req-failed = 93
- conflict-in-ip-addr-assignment = 94
- apn-removed = 95
- credits-used-bytes-in = 96
- credits-used-bytes-out = 97
- credits-used-bytes-total = 98
- prepaid-failed = 99
- l2tp-ipsec-tunnel-failure = 100
- l2tp-ipsec-tunnel-disconnected = 101
- mip-ipsec-sa-inactive = 102
- Long-Duration-Timeout = 103
- proxy-mip-registration-failure = 104
- proxy-mip-binding-update = 105
- proxy-mip-inter-pdsn-handoff-require-ip-address = 106
- proxy-mip-inter-pdsn-handoff-mismatched-address = 107
- Local-purge = 108
- failed-update-handoff = 109
- closed_rp-handoff-complete = 110
- closed_rp-duplicate-session = 111
- closed_rp-handoff-session-not-found = 112
- closed_rp-handoff-failed = 113
- pcf-monitor-keep-alive-failed = 114
- call-internal-reject = 115
- call-restarted = 116
- a11-mn-ha-auth-failure = 117
- a11-badly-formed = 118
- a11-t-bit-not-set = 119
- a11-unsupported-vendor-id = 120
- a11-mismatched-id = 121
- mipha-dup-home-addr-req = 122
- mipha-dup-imsi-session = 123
- ha-unreachable = 124
- IPSP-addr-in-use = 125
- mipfa-dup-home-addr-req = 126
- mipha-ip-pool-busyout = 127
- inter-pdsn-handoff = 128
- active-to-dormant = 129
- ppp-renegotiation = 130
- active-start-param-change = 131
- tarrif-boundary = 132
- a11-disconnect-no-active-stop = 133
- nw-reachability-failed-reject = 134
- nw-reachability-failed-redirect = 135
- container-max-exceeded = 136
- static-addr-not-allowed-in-apn = 137
- static-addr-required-by-radius = 138
- static-addr-not-allowed-by-radius = 139
- mip-registration-dropped = 140
- counter-rollover = 141
- constructed-nai-auth-fail = 142
- inter-pdsn-service-optimize-handoff-disabled = 143
- gre-key-collision = 144
- inter-pdsn-service-optimize-handoff-triggered = 145
- intra-pdsn-handoff-triggered = 146
- delayed-abort-timer-expired = 147
- Admin-AAA-disconnect = 148
- Admin-AAA-disconnect-handoff = 149
- PPP-IPV6CP-Neg-Failed = 150
- PPP-IPV6CP-No-Response = 151
- PPP-IPV6CP-Max-Retry = 152
- PPP-Restart-Invalid-source-IPV4-address = 153
- a11-disconnect-handoff-no-active-stop = 154
- call-restarted-inter-pdsn-handoff = 155
- call-restarted-ppp-termination = 156
- mipfa-resource-conflict = 157
- failed-auth-with-charging-svc = 158
- mipha-dup-imsi-session-purge = 159
- mipha-rev-pending-newcall = 160
- volume-quota-reached = 161
- duration-quota-reached = 162
- gtp-user-authentication-failed = 163
- MIP-reg-revocation-no-lcp-term = 164
- MIP-private-ip-no-rev-tunnel = 165
- Invalid-Prepaid-AAA-attr-in-auth-response = 166
- mipha-prepaid-reset-dynamic-newcall = 167
- gre-flow-control-timeout = 168
- mip-paaa-bc-query-not-found = 169
- mipha-dynamic-ip-addr-not-available = 170
- a11-mismatched-id-on-handoff = 171
- a11-badly-formed-on-handoff = 172
- a11-unsupported-vendor-id-on-handoff = 173
- a11-t-bit-not-set-on-handoff = 174
- MIP-reg-revocation-i-bit-on = 175
- A11-RRQ-Deny-Max-Count = 176
- Dormant-Transition-During-Session-Setup = 177
- PPP-Rem-Reneg-Disc-Always-Cfg = 178
- PPP-Rem-Reneg-Disc-NAI-MSID-Mismatch = 179
- mipha-subscriber-ipsec-tunnel-down = 180
- mipha-subscriber-ipsec-tunnel-failed = 181
- mipha-subscriber-ipsecmgr-death = 182
- flow-is-deactivated = 183
- ecsv2-license-exceeded = 184
- IPSG-Auth-Failed = 185
- driver-initiated = 186
- ims-authorization-failed = 187
- service-instance-released = 188
- flow-released = 189
- ppp-renego-no-ha-addr = 190
- intra-pdsn-handoff = 191
- overload-disconnect = 192
- css-service-not-found = 193
- Auth-Failed = 194
- dhcp-client-sent-release = 195
- dhcp-client-sent-nak = 196
- msid-dhcp-chaddr-mismatch = 197
- link-broken = 198
- prog-end-timeout = 199
- qos-update-wait-timeout = 200
- css-synch-cause = 201
- Gtp-context-replacement = 202
- PDIF-Auth-failed = 203
- l2tp-unknown-apn = 204
- ms-unexpected-network-reentry = 205
- r6-invalid-nai = 206
- eap-max-retry-reached = 207
- vbm-hoa-session-disconnected = 208
- vbm-voa-session-disconnected = 209
- in-acl-disconnect-on-violation = 210
- eap-msk-lifetime-expiry = 211
- eap-msk-lifetime-too-low = 212
- mipfa-inter-tech-handoff = 213
- r6-max-retry-reached = 214
- r6-nwexit-recd = 215
- r6-dereg-req-recd = 216
- r6-remote-failure = 217
- r6r4-protocol-errors = 218
- wimax-qos-invalid-aaa-attr = 219
- npu-gre-flows-not-available = 220
- r4-max-retry-reached = 221
- r4-nwexit-recd = 222
- r4-dereg-req-recd = 223
- r4-remote-failure = 224
- ims-authorization-revoked = 225
- ims-authorization-released = 226
- ims-auth-decision-invalid = 227
- mac-addr-validation-failed = 228
- excessive-wimax-pd-flows-cfgd = 229
- sgsn-canc-loc-sub = 230
- sgsn-canc-loc-upd = 231
- sgsn-mnr-exp = 232
- sgsn-ident-fail = 233
- sgsn-sec-fail = 234
- sgsn-auth-fail = 235
- sgsn-glu-fail = 236
- sgsn-imp-det = 237
- sgsn-smgr-purge = 238
- sgsn-subs-handed-to-peer = 239
- sgsn-dns-fail-inter-rau = 240
- sgsn-cont-rsp-fail = 241
- sgsn-hlr-not-found-for-imsi = 242
- sgsn-ms-init-det = 243
- sgsn-opr-policy-fail = 244
- sgsn-duplicate-context = 245
- hss-profile-update-failed = 246
- sgsn-no-pdp-activated = 247
- asnpc-idle-mode-timeout = 248
- asnpc-idle-mode-exit = 249
- asnpc-idle-mode-auth-failed = 250
- asngw-invalid-qos-configuration = 251
- sgsn-dsd-allgprswithdrawn = 252
- r6-pmk-key-change-failure = 253
- sgsn-illegal-me = 254
- sess-termination-timeout = 255
- sgsn-sai-fail = 256
- sgsn-rnc-removal = 257
- sgsn-rai-removal = 258
- sgsn-init-deact = 259
- ggsn-init-deact = 260
- hlr-init-deact = 261
- ms-init-deact = 262
- sgsn-detach-init-deact = 263
- sgsn-rab-rel-init-deact = 264
- sgsn-iu-rel-init-deact = 265
- sgsn-gtpu-path-failure = 266
- sgsn-gtpc-path-failure = 267
- sgsn-local-handoff-init-deact = 268
- sgsn-remote-handoff-init-deact = 269
- sgsn-gtp-no-resource = 270
- sgsn-rnc-no-resource = 271
- sgsn-odb-init-deact = 272
- sgsn-invalid-ti = 273
- sgsn-ggsn-ctxt-non-existent = 274
- sgsn-apn-restrict-vio = 275
- sgsn-regular-deact = 276
- sgsn-abnormal-deact = 277
- sgsn-actv-rejected-by-peer = 278
- sgsn-err-ind = 279
- asngw-non-anchor-prohibited = 280
- asngw-im-entry-prohibited = 281
- session-idle-mode-entry-timeout = 282
- session-idle-mode-exit-timeout = 283
- asnpc-ms-power-down-nwexit = 284
- asnpc-r4-nwexit-recd = 285
- sgsn-iu-rel-before-call-est = 286
- ikev2-subscriber-ipsecmgr-death = 287
- All-dynamic-pool-addr-occupied = 288
- mip6ha-ip-addr-not-available = 289
- bs-monitor-keep-alive-failed = 290
- sgsn-att-in-reg-state = 291
- sgsn-inbound-srns-in-reg-state = 292
- dt-ggsn-tun-reestablish-failed = 293
- sgsn-unknown-pdp = 294
- sgsn-pdp-auth-failure = 295
- sgsn-duplicate-pdp-context = 296
- sgsn-no-rsp-from-ggsn = 297
- sgsn-failure-rsp-from-ggsn = 298
- sgsn-apn-unknown = 299
- sgsn-serv-req-init-deact = 300
- sgsn-attach-on-attch-init-abort = 301
- sgsn-iu-rel-in-israu-init-abort = 302
- sgsn-smgr-init-abort = 303
- sgsn-mm-ctx-cleanup-init-abort = 304
- sgsn-unknown-abort = 305
- sgsn-guard-timeout-abort = 306
- vpn-bounce-dhcpip-validate-req = 307
- mipv6-id-mismatch = 308
- aaa-session-id-not-found = 309
- x1-max-retry-reached = 310
- x1-nwexit-recd = 311
- x1-dereg-req-recd = 312
- x1-remote-failure = 313
- x1x2-protocol-errors = 314
- x2-max-retry-reached = 315
- x2-nwexit-recd = 316
- x2-dereg-req-recd = 317
- x2-remote-failure = 318
- x1-pmk-key-change-failure = 319
- sa-rekeying-failure = 320
- sess-sleep-mode-entry-timeout = 321
- phsgw-non-anchor-prohibited = 322
- asnpc-pc-relocation-failed = 323
- asnpc-pc-relocation = 324
- auth_policy_mismatch = 325
- sa-lifetime-expiry = 326
- asnpc-del-ms-entry-recd = 327
- phspc-sleep-mode-timeout = 328
- phspc-sleep-mode-exit = 329
- phspc-sleep-mode-auth-failed = 330
- phspc-ms-power-down-nwexit = 331
- phspc-x2-nwexit-recd = 332
- invalid-nat-config = 333
- asngw-tid-entry-not-found = 334
- No-NAT-IP-Address = 335
- excessive-phs-pd-flows-cfgd = 336
- phsgw-invalid-qos-configuration = 337
- Interim-Update = 338
- sgsn-attach-abrt-rad-lost = 339
- sgsn-inbnd-irau-abrt-rad-lost = 340
- ike-keepalive-failed = 341
- sgsn-attach-abrt-ms-suspend = 342
- sgsn-inbnd-irau-abrt-ms-suspend = 343
- duplicate-session-detected = 344
- sgsn-xid-response-failure = 345
- sgsn-nse-cleanup = 346
- sgsn-gtp-req-failure = 347
- sgsn-imsi-mismatch = 348
- sgsn-bvc-blocked = 349
- sgsn-attach-on-inbound-irau = 350
- sgsn-attach-on-outbound-irau = 351
- sgsn-incorrect-state = 352
- sgsn-t3350-expiry = 353
- sgsn-page-timer-expiry = 354
- phsgw-tid-entry-not-found = 355
- phspc-del-ms-entry-recd = 356
- sgsn-pdp-local-purge = 357
- phs-invalid-nai = 358
- session-sleep-mode-exit-timeout = 359
- sgsn-offload-phase2 = 360
- phs-thirdparty-auth-fail = 361
- remote-error-notify = 362
- no-response = 363
- PDG-Auth-failed = 364
- mme-s1AP-send-failed=365
- mme-egtpc-connection-failed=366
- mme-egtpc-create-session-failed=367
- mme-authentication-failure=368
- mme-ue-detach=369
- mme-mme-detach=370
- mme-hss-detach=371
- mme-pgw-detach=372
- mme-sub-validation-failure=373
- mme-hss-connection-failure=374
- mme-hss-user-unknown=375
- dhcp-lease-mismatch-detected=376
- nemo-link-layer-down=377
- eapol-max-retry-reached = 378
- sgsn-offload-phase3 = 379
- mbms-bearer-service-disconnect = 380
- disconnect-on-violation-odb = 381
- disconn-on-violation-focs-odb = 382
- CSCF-REG-Admin-disconnect = 383
- CSCF-REG-User-disconnect = 384
- CSCF-REG-Inactivity-timeout = 385
- CSCF-REG-Network-disconnect = 386
- CSCF-Call-Admin-disconnect = 387
- CSCF-CAll-User-disconnect = 388
- CSCF-CALL-Local-disconnect = 389
- CSCF-CALL-No-Resource = 390
- CSCF-CALL-No-Respone = 391
- CSCF-CALL-Inactivity-timeout = 392
- CSCF-CALL-Media-Auth-Failure = 393
- CSCF-REG-No-Resource = 394
- ms-unexpected-idle-mode-entry = 395
- re-auth-failed = 396
- sgsn-pdp-nse-cleanup = 397
- sgsn-mm-ctxt-gtp-no-resource = 398
- unknown-apn = 399
- gtpc-path-failure = 400
- gtpu-path-failure = 401
- actv-rejected-by-sgsn = 402
- sgsn-pdp-gprs-camel-release = 403
- sgsn-check-imei-failure = 404
- sgsn-sndcp-init-deact = 405
- sgsn-pdp-inactivity-timeout = 406
- fw-and-nat-policy-removed = 407
- FNG-Auth-failed = 408
- ha-stale-key-disconnect = 409
- No-IPV6-address-for-subscriber = 410
- prefix-registration-failure = 411
- disconnect-from-policy-server = 412
- s6b-auth-failed = 413
- gtpc-err-ind = 414
- gtpu-err-ind = 415
- invalid-pdn-type = 416
- aaa-auth-req-failed = 417
- apn-denied-no-subscription = 418
- Sgw-context-replacement = 419
- dup-static-ip-addr-req = 420
- apn-restrict-violation = 421
- invalid-wapn = 422
- ttg-nsapi-allocation-failed = 423
- mandatory-gtp-ie-missing = 424
- aaa-unreachable = 425
- asngw-service-flow-deletion = 426
- CT-PMIP-RRQ-NVSE-Value-Change = 427
- tcp-read-failed = 428
- tcp-write-failed = 429
- ssl-handshake-failed = 430
- ssl-renegotiate-failed = 431
- ssl-bad-message = 432
- ssl-alert-received = 433
- ssl-disconnect = 434
- ssl-migration = 435
- sgsn-ard-failure = 436
- sgsn-camel-release = 437
- Hotlining-Status-Change=447
- ggsn-no-rsp-from-sgsn = 448
- diameter-protocol-error=449
- diameter-request-timeout=450
- operator-policy=451
- spr-connection-timeout=452
- mipha-dup-wimax-session = 453
- invalid-version-attr = 454
- sgsn-zone-code-failure = 455
- invalid-qci = 456
- no_rules = 457
- mme-init-ctxt-setup-failure = 459
- mme-driver-initiated = 460
- mme-s1ap-connection-down = 461
- mme-s1ap-reset-recd = 462
- mme-s6a-response-timeout = 463
- mme-s13-response-timeout = 464
- mme-Illegal-equipment = 465
- mme-unexpected-attach = 466
- mme-sgw-selection-failure = 467
- mme-pgw-selection-failure = 468
- mme-reselection-to-sgsn = 469
- mme-relocation-to-sgsn = 470
- mme-reselection-to-mme = 471
- mme-relocation-to-mme = 472
- mme-tau-attach-collision = 473
- mme-old-sgsn-resolution-failure = 474
- mme-old-mme-resolution-failure = 475
- mme-reloc-ho-notify-timeout = 476
- mme-reloc-ho-req-ack-timeout = 477
- mme-create-session-timeout = 478
- mme-create-session-failure = 479
- mme-s11-path-failure = 480
- mme-policy-no-ue-irat = 481
- mme-x2-handover-failed = 482
- mme-attach-restrict = 483
- mme-regional-zone-code = 484
- mme-no-response-from-ue = 485
- mme-sgw-relocation-failed = 486
- mme-implicit-detach = 487
- sgsn-detach-notify = 488
- emergency-inactivity-timeout = 489
- policy-initiated-release = 490
- gy-result-code-system-failure = 491
- mme-zone-code-validation-failed = 492
- sgsn-pgw-init-deact = 493
- s6b-ip-validation-failed = 494
- sgsn-failure-rsp-from-sgw = 495
- tcp-remote-close = 496
- tcp-reset-received = 497
- tcp-socket-error = 498

SN1-DNS-Proxy-Intercept-List

DNS proxy list.

Type

26

Vendor ID

8164

VSA Type

214

Length

1–253

Value

String
SN1-DNS-Proxy-Use-Subscr-Addr

This attribute is used to convey whether to use the subscriber's address as the source address for DNS Proxy.

Type

26

Vendor ID

8164

VSA Type

25

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN1-Dynamic-Addr-Alloc-Ind-Flag

This attribute indicates that the PDP address has been dramatically allocated for that particular PDP context. This field is missing if the address is static (e.g., part of the PDP context subscription). Dynamic address allocation might be relevant for charging (e.g., the duration of PDP context as one resource offered and possibly owned by the network operator).

Type

26

Vendor ID

8164

VSA Type

141

Length

1

Value

Integer.

Dynamic address allocation = 1
SN1-Ecs-Data-Volume

Compound attribute indicating downlink and uplink octet usage for a PDP context per rating group.

Type

26

Vendor ID

8164

VSA Type

176

Length

12

Value

Contains the following subattributes:
Rating-Group-Id

Rating Group Id in a PDP context.

Type

1

Length

4

Value

Unsigned integer
GPRS-Uplink

Uplink octet usage for a PDP context per rating group.

Type

2

Length

4

Value

Unsigned integer
GPRS-Downlink

Downlink octet usage for a PDP context per rating group.

Type

3

Length

4

Value

Unsigned integer
SN1-Enable-QoS-Renegotiation

This attribute configures the enabling of dynamic QoS renegotiation.

Type

26

Vendor ID

8164

VSA Type

144

Length

1

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN1-Ext-Inline-Srvr-Context

This attribute configures the context name in which the External In-line server resides. The value is an ASCII string naming the In-line Server Context.

Type

26

Vendor ID

8164

VSA Type

41

Length

1–247

Value

ASCII string
SN1-Ext-Inline-Srvr-Down-Addr

This attribute configures the IP address of the Downstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

56

Length

4

Value

IPv4 address
SN1-Ext-Inline-Srvr-Down-VLAN

This attribute configures the IP address of the downstream external in-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

59

Length

4

Value

Unsigned integer
SN1-Ext-Inline-Srvr-Preference

This attribute configures the preference for the tagged group of External In-line Servers. This attribute is required, although it doesn't actually assign a preference right now. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

57

Length

4

Value

Unsigned integer
SN1-Ext-Inline-Srvr-Up-Addr

This attribute configures the IP address of the Upstream External In-line server to forward VLAN-tagged packets to. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

55

Length

4

Value

IPv4 address
SN1-Ext-Inline-Srvr-Up-VLAN

This attribute configures the VLAN tag to be applied to Upstream packets and forwarded to the External In-line server. It can be tagged, in which case it is treated as part of an external in-line server group.

Type

26

Vendor ID

8164

VSA Type

58

Length

4

Value

The VLAN tag to apply.
SN1-Firewall-Enabled

Firewall for subscriber enabled.

Type

26

Vendor ID

8164

VSA Type

198

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

SN1-Firewall-Policy

This attribute is obsoleted.
SN1-FMC-Location

MAC address and CDMA location information.

Type

26

Vendor ID

8164

VSA Type

171

Length

1–247

Value

String
SN1-GGSN-MIP-Required

This attribute specifies if MIP is required for the GGSN subscriber.

Type

26

Vendor ID

8164

VSA Type

68

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Gratuitous-ARP-Aggressive

This attribute specifies whether to generate a gratuitous ARP message whenever a MIP handoff or re-registration occurs. A non-zero of this attribute also configures the mode of operation when sending the gratuitous ARP, although only one mode (Aggressive) is supported at this time.

Type

26

Vendor ID

8164

VSA Type

54

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Gratuitous-ARP-Mode

This attribute specifies whether to generate a gratuitous ARP message whenever a MIP handoff or re-registration occurs. A non-zero of this attribute also configures the mode of operation when sending the gratuitous ARP, although only one mode (Aggressive) is supported at this time.

Type

26

Vendor ID

8164

VSA Type

54

Length

4

Value

An integer in network order. Supported values are:

- Disabled = 0 — Do not send Gratuitous ARP
- Aggressive = 1 — Send Gratuitous ARP in Aggressive mode

SN1-GTP-Version

This attribute contains the version of GTP the subscriber is using.

Type

26

Vendor ID

8164

VSA Type

62

Length

4

Value

Enumerated integer. Supported values are:

- GTP_VERSION_0 = 0
- GTP_VERSION_1 = 1
- GTP_VERSION_2 = 2

SN1-HA-Send-DNS-Address

This attribute specifies if the HA should send the DNS address in the Mobile IP RRP message. The default is not to send the DSN Address.

Type

26

Vendor ID

8164

VSA Type

47

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not send
- Enabled = 1 — Send

SN-Home-Behavior

This attribute specifies the configuration for the behavior bits settings for a home subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for “home” subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by “Or”ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

119

Length

4

Value

Unsigned integer
SN1-Home-Behavior

This attribute specifies the configuration for the behavior bits settings for a home subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for “home” subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by “Or”ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

119

Length

4

Value

Unsigned integer
SN1-Home-Profile

This attribute specifies the configuration for the profile bits settings for a home subscriber in an APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

109

Length

4

Value

Unsigned integer
SN1-Home-Sub-Use-GGSN

This attribute configures GGSN to accept GGSN's charging characteristics for home subscribers defined for the APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

106

Length

4

Value

Enumerated integer. Supported values are:

- Deny = 0
- Accept = 1

SN1-Ignore-Unknown-HA-Addr-Err

Value of 1 enables HA to ignore unknown HA address error for incoming RRQ.

Type

26

Vendor ID

8164

VSA Type

160

Length

1

Value

Unsigned integer
SN1-IMSI

This is the IMSI that identifies the mobile subscriber.

Type

26

Vendor ID

8164

VSA Type

252

Length

1–8

Value

ASCII string
SN1-IMS-AM-Address

IMS application manager address.

Type

26

Vendor ID

8164

VSA Type

167

Length

4

Value

IPv4 address
SN1-IMS-AM-Domain-Name

IMS application manager domain name.

Type

26

Vendor ID

8164

VSA Type

168

Length

1 - 64

Value

String
SN1-Internal-SM-Index

GGSN charging service, internally used.

Type

26

Vendor ID

8164

VSA Type

122

Length

4

Value

Unsigned integer
SN1-Inactivity-Time

This attribute contains the inactivity time duration for a subscriber session under long time duration timer configuration.

Type

26

Vendor ID

8164

VSA Type

232

Length

1

Value

1
SN1-IP-Alloc-Method

This attribute specifies the method for allocating an IP address. This feature only applies to the GGSN Service.

Type

26

Vendor ID

8164

VSA Type

53

Length

4

Value

Enumerated integer. Supported values are:

- Alloc_Local_Pool = 0
- Alloc_Dhcp_Client = 1
- Alloc_Radius = 2
- Alloc_No_Alloc = 3
- Alloc_Static_Alloc = 4
- Alloc_Dhcp_Relay = 5

SN1-IP-Filter-In

This attribute is deprecated. To select an IP access list that is already defined in the destination context, use the IETF standard Filter-Id attribute. The filter ID is used to identify the IP access list by name.
SN1-IP-Filter-Out

This attribute is deprecated. To select an IP access list that is already defined in the destination context, use the IETF standard Filter-Id attribute. The filter ID is used to identify the IP access list by name.
SN1-IP-Header-Compression

Specifies the IP header compression method to use.

Type

Type 26

Vendor ID

8164

VSA Type

150

Length

2

Value

Enumerated integer. Supported values are:

- None = 0
- VJ = 1
- ROHC = 2
- VJ_ROHC = 3

SN1-IP-Hide-Service-Address

This attribute prevents the IP address bound to a call service from responding to ping and IMCP error packets.

Type

26

Vendor ID

8164

VSA Type

60

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN1-IP-In-ACL

This attribute contains a definition for one Input IP Access Control List, which is used to filter the IP packets coming from the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.

Type

26

Vendor ID

8164

VSA Type

17

Length

1–253

Value

ASCII string
SN1-IP-In-Plcy-Grp

This attribute specifies the name of the policy group config applied in the uplink direction.

Type

26

Vendor ID

8164

VSA Type

193

Length

1–16

Value

String.
SN1-IP-Out-ACL

This attribute contains a definition for one Output IP Access Control List, which is used to filter the IP packets sent to the user. Note that more than one of these attributes can be included, in which case they are processed in the order in which they appear in the RADIUS Access-Accept.

Type

26

Vendor ID

8164

VSA Type

18

Length

1–253

Value

ASCII string
SN1-IP-Out-Plcy-Grp

This attribute specifies the name of the policy group config applied in the downlink direction.

Type

26

Vendor ID

8164

VSA Type

194

Length

1–16

Value

String.
SN1-IP-Pool-Name

This attribute contains the name of the IP pool, configured on the chassis, from which an IP address should be chosen for the user.

Type

26

Vendor ID

8164

VSA Type

8

Length

1–253

Value

ASCII string
SN1-IP-Source-Validation

This attribute indicates if the source IP address should be validated before forwarding the IP packet.

Type

26

Vendor ID

8164

VSA Type

14

Length

4

Value

Enumerated integer. Supported values are:

- No = 0 — No Validation
- Yes = 1 — Validated
- VSA1 vendor specific.

SN1-IP-Source-Violate-No-Acct

This attribute excludes the Source Violated IP packets and byte counts when reporting the Octet and Packet count in an accounting message.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN this value will not be applied to the session.

Type

26

Vendor ID

8164

VSA Type

196

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-IP-Src-Valid-Drop-Limit

Maximum number of packet drops entertained before disconnecting the session for source violated packets for the session

Type

26

Vendor ID

8164

VSA Type

110

Length

1

Value

Unsigned integer
SN1-IPv6-DNS-Proxy

IPV6 DNS Proxy Enabled or Disabled Setting for the session.

Type

26

Vendor ID

8164

VSA Type

126

Length

2

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-IPv6-Egress-Filtering

This attribute enables egress filtering to make sure that packets being sent to the mobile device have an interface ID that matches that of the mobile device. This feature is meant to protect the Mobile from receiving unwanted packets from the Internet.

Type

26

Vendor ID

8164

VSA Type

103

Length

1

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-IPv6-Min-Link-MTU

SN1-IPv6-Min-Link-MTU

Type

26

Vendor ID

8164

VSA Type

136

Length

2

Value

Unsigned integer
SN1-IPv6-num-rtr-advt

This attribute contains the IPv6 number of Initial Router Advertisements. Default value is 3.

Type

26

Vendor ID

8164

VSA Type

97

Length

4

Value

Unsigned integer
SN1-IPv6-Primary-DNS

This attribute specifies a Primary DNS server address that the Router Advertisement message sent by the PDSN will include.

Type

26

Vendor ID

8164

VSA Type

101

Length

4

Value

IPv6 address
SN1-IPv6-rtr-advt-interval

This attribute contains the IPv6 Initial Router Advertisement Interval, specified in milliseconds. The default value is 3000.

Type

26

Vendor ID

8164

VSA Type

96

Length

4

Value

Unsigned integer
SN1-IPv6-Sec-Pool

This attribute contains the IPv6 secondary pool name.

Type

26

Vendor ID

8164

VSA Type

124

Length

1–253

Value

String
SN1-IPv6-Sec-Prefix

IPv6 Secondary Pool name prefix.

Type

26

Vendor ID

8164

VSA Type

125

Length

2–18

Value

Opaque value
SN1-IPv6-Secondary-DNS

This attribute specifies a Secondary DNS server address that the Router Advertisement message sent by the PDSN will include.

Type

26

Vendor ID

8164

VSA Type

102

Length

4

Value

IPv6 address
SN1-L3-to-L2-Tun-Addr-Policy

This attribute specifies the address allocation policy.

Type

26

Vendor ID

8164

VSA Type

43

Length

4

Value

Enumerated integer. Supported values are:

- no-local-alloc-validate = 0 — Do not locally allocate, do not validate
- local-alloc = 1 — Locally allocate
- local-alloc-validate = 2 — Locally allocate and validate

SN1-Local-IP-Address

This attribute contains the IP address of the local interface on the chassis for the user’s session.

Type

26

Vendor ID

8164

VSA Type

13

Length

4

Value

IPv4 address
SN1-Long-Duration-Action

This attribute specifies the action to take place when the long duration timeout expires for a subscriber session.

Type

26

Vendor ID

8164

VSA Type

45

Length

4

Value

Enumerated integer. Supported values are:

- Detection = 1 — Detect the session and alert the administrator
- Disconnection = 2 — Disconnect the session
- Dormant-Only-Disconnection = 3
- Dormant-Only-Detection = 4

SN1-Long-Duration-Notification

Long Duration Notification.

Type

26

Vendor ID

8164

VSA Type

253

Length

4

Value

Enumerated integer. Supported values are:

- Suppress = 0
- Send = 1

SN1-Long-Duration-Timeout

This attribute is used to detect and if necessary disconnect sessions connected to the PDSN. This attribute configures the time period before either alerting the administrator or disconnecting the subscriber.

Type

26

Vendor ID

8164

VSA Type

44

Length

4

Value

An integer in network order which is the number of seconds for the long duration timer.
SN1-Mediation-Acct-Rsp-Action

When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the Mediation Accounting server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the Mediation Accounting server. When set to Delay_GTP_Response, the system does not send a GTP create PDP response to the GGSN until a response for the accounting start message is received from the Mediation Accounting server. If the AVP is not present in Access Accept message or if the AVP value is invalid, the value “None” is assumed.

Type

26

Vendor ID

8164

VSA Type

105

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- No_Early_PDUs = 1
- Delay_GTP_Response = 2

SN1-Mediation-Enabled

This attribute indicates whether the Mediation Accounting configuration is enabled or disabled for GGSN.

If the AVP is not present in Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

123

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Mediation-No-Interims

This attribute is used to disable or enable Mediation Interim Accounting Records for the session.

If this AVP is not present in Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

146

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Mediation-VPN-Name

This attribute specifies the Mediation Context name for the session.

If this AVP is not received in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

104

Length

1–128

Value

String
SN1-Min-Compress-Size

This attribute contains the minimum size (in octets) a data packet can have in order to be compressed.

Type

26

Vendor ID

8164

VSA Type

23

Length

4

Value

Unsigned integer
SN1-MIP-AAA-Assign-Addr

This attribute specifies if the PDSN/FA will allow AAA to assign the home address. The default is to not allow AAA to assign the home address.

Type

26

Vendor ID

8164

VSA Type

50

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not allow AAA to assign home address
- Enabled = 1 — Allow AAA to assign home address

SN1-MIP-ANCID

Accounting correlation ID created by IPGW, received by VBM and HBM.

Type

26

Vendor ID

8164

VSA Type

166

Length

12

Value

Opaque value
SN1-MIP-Dual-Anchor

Enable/disable dual-anchor service for a subscriber.

Type

26

Vendor ID

8164

VSA Type

165

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-MIP-HA-Assignment-Table

MIP-HA Assignment Table name. When this is received in an Access Accept message, the system uses this local table to get the HA Address.

Type

26

Vendor ID

8164

VSA Type

154

Length

1–253

Value

ASCII string
SN1-MIP-Match-AAA-Assign-Addr

This attribute specifies if the PDSN/FA will enforce that a non-zero AAA-specified home address must match the home address present in the MIP RRQ from the mobile node, and disconnect the subscriber session if a match is not present. The default is not to force the addresses to match.

Type

26

Vendor ID

8164

VSA Type

51

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not force the AAA-specified home address to match RRQ
- Enabled = 1 — Force the AAA-specified home address to match RRQ

SN1-MIP-Reg-Lifetime-Realm

Configure the maximum MIP registration lifetime for a subscriber/realm.

Type

26

Vendor ID

8164

VSA Type

175

Length

2

Value

Unsigned integer
SN1-MIP-Send-Ancid

AAA attribute to enable/disable sending ANCID from FA to HA in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

163

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-MIP-Send-Correlation-Info

This attribute enables/disables sending of correlation-id from FA to HA in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

188

Length

4

Value

Enumerated integer. In StarOS 8.1 and earlier, supported values are:

- Disabled = 0
- Enabled = 1

In StarOS 8.3 and later, supported values are:

- Disabled = 0
- NVSE_Starent = 1
- NVSE_CUstom1 = 2
- NVSE_Custom2 = 3

SN1-MIP-Send-Imsi

Attribute to enable/disable sending IMSI from FA to HA in MIP RRQ.

Type

26

Vendor ID

8164

VSA Type

164

Length

4

Value

Enumerated integer. In StarOS 8.1 and earlier, supported values are:

- None = 0
- Starent_NVSE = 1
- Custom1_NVSE = 2

In StarOS 8.3 and later, supported values are:

- Disabled = 0,
- NVSE_Starent = 1,
- NVSE_Custom1 = 2,
- NVSE_Custom2 = 3

SN1-MIP-Send-Term-Verification

This attribute specifies whether the PDSN/FA should send the Terminal Verification Normal Vendor/Organization Specific Extension (NVSE) in the Mobile IP RRQ message to the HA. The default is not to send the Terminal Verification NVSE.

Type

26

Vendor ID

8164

VSA Type

48

Length

4

Value

Enumerated integer. In StarOS 8.1 and earlier, supported values are:

- Disabled = 0 — Do not send
- Enabled = 1 — Send

In StarOS 8.3 and later, supported values are:

- Disabled = 0
- NVSE_Custom1 = 1 — Send custom NVSE
- NVSE_Custom2 = 2 — Send custom NVSE
- NVSE_Starent = 3 — Send custom NVSE

SN1-MN-HA-Hash-Algorithm

This attribute contains the hash algorithm to use for MN-HA authentication.

Type

26

Vendor ID

8164

VSA Type

28

Length

4

Value

Enumerated integer. Supported values are:

- MD5 = 1
- MD5-RFC2002 = 2
- HMAC-MD5 = 3

SN1-MN-HA-Timestamp-Tolerance

This attribute contains the duration of timestamp tolerance, in seconds, to use for MN-HA authentication.

Type

26

Vendor ID

8164

VSA Type

30

Length

4

Value

Unsigned integer
SN1-MS-ISDN

SN1-MS-ISDN.

Type

26

Vendor ID

8164

VSA Type

248

Length

1–9

Value

Opaque value
SN1-MSK-Lifetime

This attribute is currently not supported.
SN1-NAI-Construction-Domain

This attribute specifies the domain name to use when constructing the NAI.

Type

26

Vendor ID

8164

VSA Type

37

Length

1–247

Value

An ASCII string specifying the domain to use when constructed NAI is used.
SN1-NAT-Bind-Record

This attribute contains the NAT Binding Record.

Type

26

Vendor ID

8164

VSA Type

216

Length

Compound

Value

Contains the following subattributes:
NAT-IP-Address

NAT IP Address.

Type

1

Length

4

Value

IPv4 address
NAT-Port-Block-Start

Start port of the port chunk.

Type

2

Length

2

Value

Unsigned integer
NAT-Port-Block-End

End port of the port chunk.

Type

3

Length

2

Value

Unsigned integer
Alloc-Flag

Port chunk status. Accepted Values are 0(De-Allocated) and 1(Allocated).

Type

4

Length

1

Value

Unsigned integer
Correlation-Id

Correlation ID.

Type

5

Length

1–253

Value

String
Loading-Factor

Indicates maximum number of users per NAT IP address.

Type

6

Length

2

Value

Unsigned integer
Binding-Timer

Port chunk hold timer.

Type

7

Length

4

Value

Unsigned integer
SN1-NAT-Info-Record

NAT-Record-Info.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

246

Length

Compound

Value

Contains the following subattributes:
Framed-IP-Address

Framed IP address.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

1

Length

4

Value

IPv4 address
NAT-IP-Address

NAT IP address.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

2

Length

4

Value

IPv4 address
NAT-Port-Block-Start

Start port of the port chunk

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

3

Length

2

Value

Unsigned integer
NAT-Port-Block-End

End port of the port chunk.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

4

Length

2

Value

Unsigned integer
Acct-Session-Id

Accounting Session ID.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

5

Length

1–17

Value

String
User-Name

User name.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

6

Length

1–128

Value

String
Correlation-Id

Correlation ID.

This attribute is also accepted in CoA response message to be used in a currently active subscriber session.

Type

7

Length

1–17

Value

String
SN1-NAT-IP-Address

This attribute includes the NAT (public) IP address used for the call.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

217

Length

4

Value

IPv4 address
SN1-NAT-IP-Address-Old

Public IP address used for the call

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

0

Length

4

Value

IPv4 address
SN1-NPU-Qos-Priority

This attribute configures Inter-Subscriber priority Queueing based on class of service offered. Gold has highest priority and Best_effort lowest priority. From DSCP, means the priority queueing will be done based on the DSCP marking the incoming subscriber packet carries.

Type

26

Vendor ID

8164

VSA Type

98

Length

4

Value

Enumerated integer. Supported values are:

- Best_Effort = 0
- Bronze = 1
- Silver = 2
- Gold = 3
- From_DSCP = 4

SN1-Ntk-Initiated-Ctx-Ind-Flag

This attribute indicates that the PDP context is network initiated. The attribute is missing for a mobile activated PDP context.

Type

26

Vendor ID

8164

VSA Type

142

Length

1

Value

Opaque value
SN1-Ntk-Session-Disconnect-Flag

SN1-Ntk-Session-Disconnect-Flag.

Type

26

Vendor ID

8164

VSA Type

143

Length

4

Value

Enumerated integer. Supported value is:

- Session-Disconnect = 1

SN1-Ntk-Session-Disconnect-Reason

SN1-Ntk-Session-Disconnect-Reason.

Type

26

Vendor ID

8164

VSA Type

143

Length

4

Value

Enumerated integer. Supported value is:

- Session-Disconnect = 1

SN1-Nw-Reachability-Server-Name

This attribute specifies the name of a network reachability server (defined in the destination context of the subscriber) that must respond as reachable, or the user is be redirected.

Type

26

Vendor ID

8164

VSA Type

65

Length

1–247

Value

An ASCII string representing the name of the Network Reachability Detection Server.
SN1-Overload-Disconnect

Enables/disables the overload-disconnect feature (if 1) and disables if 0

Type

26

Vendor ID

8164

VSA Type

235

Length

4

Value

Unsigned Integer
SN1-Overload-Disc-Connect-Time

Provides the connect time for a session. When this time expires, the session may become a candidate for disconnection.

Type

26

Vendor ID

8164

VSA Type

233

Length

1

Value

Integer
SN1-Overload-Disc-Inact-Time

Provides inactivity time for a session after which it may become candidate for disconnection.

Type

26

Vendor ID

8164

VSA Type

234

Length

1

Value

Integer
SN1-PDIF-MIP-Release-TIA

PDIF mobile IP release TIA.

Type

26

Vendor ID

8164

VSA Type

172

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN1-PDIF-MIP-Required

PDIF mobile IP required.

Type

26

Vendor ID

8164

VSA Type

170

Length

4

Value

Enumerated Integer. Supported values are:

- No = 0
- Yes = 1

SN1-PDIF-MIP-Simple-IP-Fallback

PDIF mobile IP simple IP fallback.

Type

26

Vendor ID

8164

VSA Type

173

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN1-PDSN-Correlation-Id

Correlation ID received from PDSN to HA.

Type

26

Vendor ID

8164

VSA Type

189

Length

8

Value

Opaque value
SN1-PDSN-Handoff-Req-IP-Addr

This attribute specifies if the PDSN should reject and terminate the subscriber session when the proposed address in IPCP by the mobile does not match the existing address in the PDSN. The default (Disabled) is not to reject these sessions.

Type

26

Vendor ID

8164

VSA Type

46

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not reject
- Enabled = 1 — Reject

SN1-PDSN-NAS-Id

NAS Identifier received from PDSN to HA.

Type

26

Vendor ID

8164

VSA Type

190

Length

1–253

Value

String
SN1-PDSN-NAS-IP-Address

NAS IP address received from PDSN to HA.

Type

26

Vendor ID

8164

VSA Type

191

Length

4

Value

IPv4 address
SN1-Permit-User-Mcast-PDUs

Specifies whether or not to let the subscriber discard multicast PDUs.

Type

26

Vendor ID

8164

VSA Type

134

Length

2

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-PPP-Accept-Peer-v6Ifid

This attribute indicates the acceptance of the interface ID provided by peer during PPP IPv6CP if the ID is valid. The default is disabled.

Type

26

Vendor ID

8164

VSA Type

95

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not accept interface ID
- Enabled = 1 — Accept interface ID

SN1-PPP-Always-On-Vse

SN1-PPP-Always-On-Vse.

Type

26

Vendor ID

8164

VSA Type

130

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-PPP-Data-Compression

This attribute indicates the PPP data compression algorithm to use for the PPP session. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.

Type

26

Vendor ID

8164

VSA Type

9

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Stac-LZS = 1
- MPPC = 2
- Deflate = 4

SN1-PPP-Data-Compression-Mode

This attribute indicates the PPP data compression mode to use for the PPP session when PPP data compression is used.

Type

26

Vendor ID

8164

VSA Type

19

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Stateless = 1

SN1-PPP-Keepalive

This attribute indicates the interval for the PPP keepalive, in seconds.

Type

26

Vendor ID

8164

VSA Type

16

Length

4

Value

Unsigned integer
SN1-PPP-NW-Layer-IPv4

This attribute indicates the PPP IPCP negotiation for IPv4. The default is enabled.

Type

26

Vendor ID

8164

VSA Type

92

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — IPCP negotiation for IPv4 is disabled.
- Enabled = 1 — IPCP negotiation for IPv4 is enabled.
- Passive = 2 — Start the negotiation only if peer initiates it.

SN1-PPP-NW-Layer-IPv6

This attribute indicates the PPP IPv6CP negotiation for IPv6. The default is enabled.

Type

26

Vendor ID

8164

VSA Type

93

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — IPCP negotiation for IPv6 is disabled.
- Enabled = 1 — IPCP negotiation for IPv6 is enabled.
- Passive = 2 — Start the negotiation only if peer initiates it.

SN1-PPP-Outbound-Password

This attribute indicates the password to be used when the user side of the PPP connection requires authentication.

Type

26

Vendor ID

8164

VSA Type

15

Length

1–253

Value

ASCII string
SN1-PPP-Outbound-Username

This attribute indicates the username to be used when the user side of the PPP connection requires authentication.

Type

26

Vendor ID

8164

VSA Type

61

Length

1–253

Value

ASCII string
SN1-PPP-Progress-Code

This attribute provides information about the “state” of the PPP connection, when the connection was terminated.

Type

26

Vendor ID

8164

VSA Type

4

Length

4

Value

Enumerated integer. Supported values are:

- Not-Defined = 0
- Call-Lcp-Down = 10
- Call-Disconnecting = 20
- Call-Ppp-Renegotiating = 30
- Call-Arrived = 40
- Call-Pdg-Tcp-Connecting = 45
- Call-Pdg-Ssl-Connecting = 46
- Call-Lcp-Up = 50
- Call-Authenticating = 60
- Call-Bcmcs-Authenticating = 70
- Call-Authenticated = 80
- Call-Tunnel-Connecting = 85
- Call-Ipcp-Up = 90
- Call-Imsa-Authorizing = 95
- Call-Imsa-Authorized = 97
- Call-MBMS-UE-Authorizing = 98
- Call-MBMS-Bearer-Authorizing = 99
- Call-Simple-IP-Connected = 100
- Call-Mobile-IP-Connected = 110
- Call-Tunnel-Connected = 115
- Call-Pdp-Type-IP-Connected = 120
- Call-Pdp-Type-IPv6-Connected = 125
- Call-Pdp-Type-PPP-Connected = 130
- Call-Proxy-Mobile-IP-Connected = 140
- Call-Pdg-Connected = 142
- Call-Pdg-Ssl-Connected = 141
- Call-Pdg-Connected = 142
- Call-Pdg-Connected = 142
- Call-Ipsg-Connected = 145
- Call-Bcmcs-Connected = 150
- Call-MBMS-UE-Connected = 155
- Call-MBMS-Bearer-Connected = 156
- Call-Pending-Addr-From-DHCP = 160
- Call-Got-Addr-From-DHCP = 170
- Call-HA-IPSEC-Tunnel-Connecting = 180
- Call-HA-IPSEC-Connected = 190
- Call-ASN-Non-Anchor-Connected = 200
- Call-ASNPC-Connected = 210
- Call-Mobile-IPv6-Connected = 220
- Call-PMIPv6-Connected = 221
- Call-PHSPC-Connected = 230
- Call-GTP-IPv4-Connected = 235
- Call-GTP-IPv6-Connected = 236
- Call-GTP-IPv4-IPv6-Connected = 237
- Call-SGW-Connected = 245
- Call-MME-Attached = 246
- Call-Auth-Only-Connected = 247

SN1-PPP-Reneg-Disc

PPP remote reneg disconnect policy.

Type

26

Vendor ID

8164

VSA Type

187

Length

1

Value

Enumerated integer. Supported values are:

- Disc_no = 0
- Always = 1
- NAI_Prefix_MSID_Mismatch = 2

SN1-Prepaid

Prepaid.

Type

26

Vendor ID

8164

VSA Type

128

Length

1

Value

Enumerated integer. Supported values are:

- no_prepaid = 0
- custom_prepaid = 1
- standard_prepaid = 2
- wimax_prepaid = 4

SN1-Prepaid-Compressed-Count

This attribute indicates if a Pre-paid subscriber's byte usage should be counted on the basis of compressed or uncompressed byte data over the subscriber's PPP connection to the system. If not present, the default is to count uncompressed byte data.

Type

26

Vendor ID

8164

VSA Type

31

Length

4

Value

Enumerated integer. Supported values are:

- Uncompressed = 0
- Compressed = 1

SN1-Prepaid-Final-Duration-Alg

For prepaid, final duration is calculated based on the algorithm specified by the value of this attribute.

If this AVP is not received in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

135

Length

4

Value

Enumerated integer. Supported values are:

- current_time = 0
- last-user-layer3-activity-time = 1
- last-airlink-activity-time = 2
- last-airlink-activity-time-last-reported = 3

SN1-Prepaid-Inbound-Octets

In an Access-Accept, this indicates how many additional inbound (bytes delivered to the subscriber) byte credits should be granted to the subscriber. In an Accounting- Request, this indicates how many total inbound byte credits have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on an inbound octet basis.

Type

26

Vendor ID

8164

VSA Type

32

Length

4

Value

Unsigned integer
SN1-Prepaid-Outbound-Octets

SN1-Prepaid-Outbound-Octets.

Type

26

Vendor ID

8164

VSA Type

33

Length

4

Value

Unsigned integer
SN1-Prepaid-Preference

This attribute specifies whether prepaid is volume based or duration based.

Type

26

Vendor ID

8164

VSA Type

129

Length

1

Value

Enumerated integer. Supported values are:

- prepaid_duration = 0
- prepaid_volume = 1

SN1-Prepaid-Profile

Do not do prepaid, regardless of the Rulebase configuration.

Type

26

Vendor ID

8164

VSA Type

155

Length

4

Value

Enumerated integer. Supported values are:

- Use-Rulebase-Config = 0
- Prohibit = 1

SN1-Prepaid-Total-Octets

In an Access-Accept, this attribute indicates how many additional byte credits (combining both inbound and outbound counts) should be granted to the subscriber. In an Accounting- Request, this indicates how many total bytes credits (combined inbound and outbound) have been granted to the subscriber. When this attribute is not present in the Access-Accept, then pre-paid usage checking is disabled on a combined inbound and outbound octet-count basis.

Type

26

Vendor ID

8164

VSA Type

34

Length

4

Value

Unsigned integer
SN1-Prepaid-Timeout

This attribute indicates how much time may elapse before a new request for more pre-paid credits is issued. If the specified time has elapsed since the prior grant of credits was received from the RADIUS server, then a new request for credits is issued. This attribute is primarily used to periodically update the subscriber of new credits issued since the subscriber was connected. Note that credit requests will still be made on behalf of the subscriber when the subscriber drops down to the low watermark of credits (or zero if there is no low watermark). The presence or absence of this attribute does not affect that mechanism in any way. However, this timer is re-set whenever any grant of credits is received on behalf of the subscriber, regardless of why the grant of credits was requested.

Type

26

Vendor ID

8164

VSA Type

35

Length

4

Value

Unsigned integer
SN1-Prepaid-Watermark

This attribute Indicates the percentage of remaining granted credits that will trigger a new request to grant credits from the RADIUS server. For example, if 1GB of credits was granted to a user, and the value of SN-Prepaid-Watermark was 10, then when 100 MB of credits are remaining (900 MB have been used) to the subscriber, a new request for any new byte credits is issued on behalf of the subscriber. Note that when calculating the pre-paid low watermark, the total credits granted for the subscriber's entire session is used.

Type

26

Vendor ID

8164

VSA Type

36

Length

4

Value

Unsigned integer
SN1-Primary-DCCA-Peer

This attribute indicates the name of the primary DCCA peer and primary DCCA realm.

If the AVP is received in Access Accept message, the primary DCCA peer is used for Gy functionality. If not present in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

223

Length

1-192

Value

A colon separated string, like “primary_peer : primary_realm”
SN1-Primary-DNS-Server

This attribute indicates the IP address of the primary DNS server that should be used for the session.

Type

26

Vendor ID

8164

VSA Type

5

Length

4

Value

IPv4 address
SN1-Primary-NBNS-Server

Primary NBNS Server IP address.

Type

26

Vendor ID

8164

VSA Type

148

Length

4

Value

IPv4 address
SN1-Proxy-MIP

This attribute specifies if the PDSN/FA will perform compulsory Proxy-MIP tunneling for a Simple-IP PDSN subscriber. This feature is licensed. The default is not to perform compulsory Proxy-MIP.

Type

26

Vendor ID

8164

VSA Type

52

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0 — Do not perform compulsory Proxy-MIP
- Enabled = 1 — Perform compulsory Proxy-MIP

SN1-QoS-Background-Class

This attribute defines the QOS Background Traffic Class.

Type

26

Vendor ID

8164

VSA Type

91

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN1-QoS-Class-Background-PHB

SN1-QoS-Class-Background-PHB

Type

26

Vendor ID

10415

VSA Type

113

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN1-QoS-Class-Converstional-PHB

SN1-QoS-Class-Converstional-PHB.

Type

26

Vendor ID

10415

VSA Type

111

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN1-QoS-Class-Interactive-1-PHB

SN1-QoS-Class-Interactive-1-PHB

Type

26

Vendor ID

10415

VSA Type

114

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN1-QoS-Class-Interactive-2-PHB

SN1-QoS-Class-Interactive-2-PHB

Type

26

Vendor ID

10415

VSA Type

115

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN1-QoS-Class-Interactive-3-PHB

SN1-QoS-Class-Interactive-3-PHB

Type

26

Vendor ID

10415

VSA Type

116

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN1-QoS-Class-Streaming-PHB

SN1-QoS-Class-Streaming-PHB

Type

26

Vendor ID

10415

VSA Type

112

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort = 0
- Pass-Through = 1
- AF11 = 10
- AF12 = 12
- AF13 = 14
- AF21 = 18
- AF22 = 20
- AF23 = 22
- AF31 = 26
- AF32 = 28
- AF33 = 30
- AF41 = 34
- AF42 = 36
- AF43 = 38
- EF = 46

SN1-QoS-Conversation-Class

This attribute defines the QOS Conversation Traffic Class.

Type

26

Vendor ID

8164

VSA Type

86

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN1-QoS-Interactive1-Class

This attribute defines the QOS Interactive Traffic Class.

Type

26

Vendor ID

8164

VSA Type

88

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN1-QoS-Interactive2-Class

This attribute defines the QOS Interactive2 Traffic Class.

Type

26

Vendor ID

8164

VSA Type

89

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN1-QoS-Interactive3-Class

This attribute defines the QOS Interactive3 Traffic Class.

Type

26

Vendor ID

8164

VSA Type

90

Length

28 bytes

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN1-QoS-Negotiated

Negotiated QoS for GGSN sessions.

Type

26

Vendor ID

8164

VSA Type

147

Length

In 10.2 and earlier releases: 4–17

In 11.0 and later releases: 4–20

Value

String
SN1-QoS-Renegotiation-Timeout

This attribute configures the timeout duration of dampening time for dynamic QoS renegotiation.

Type

26

Vendor ID

8164

VSA Type

145

Length

1

Value

1
SN1-QoS-Streaming-Class

This attribute defines the QOS Streaming Traffic Class.

Type

26

Vendor ID

8164

VSA Type

87

Length

28 byte

Value

Opaque value encoded in the following format:

- Byte 16 Bit 1 - Uplink Traffic Policing Enable/Disable
- Byte 16 Bit 2 - Downlink Traffic Policing Enable/Disable
- Byte 16 Bits 3,4 - Uplink Exceed Action
- Byte 16 Bits 5,6 - Downlink Exceed Action
- Byte 16 Bits 7,8 - Uplink Violate Action
- Byte 15 Bits 1,2 - Downlink Violate Action
- Byte 15 Bit 3 - Downlink Ext Peak Data Rate
- Byte 15 Bit 4 - Downlink Ext Committed Data Rate
- Byte 14 - Uplink Peak Data Rate
- Byte 13 - Downlink Peak Data Rate
- Byte 12 - Uplink Committed Data Rate
- Byte 11 - Downlink Committed Data Rate
- Byte 5-8 - Uplink Burst Size (in Network Byte Order)
- Byte 1-4 - Downlink Burst Size (in Network Byte Order)

SN1-QoS-Tp-Dnlk

This attribute enables/disables Traffic Policing/Shaping in downlink direction.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

73

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Policing = 1
- Shaping = 2

SN1-QoS-Tp-Uplk

This attribute enables/disables Traffic Policing/Shaping in uplink direction.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

79

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Policing = 1
- Shaping = 2

SN1-QoS-Traffic-Policy

This compound attribute simplifies sending QoS values for Traffic Class, Direction, Burst-Size, Committed-Data-Rate, Peak-Data-Rate, Exceed-Action, and Violate-Action from the RADIUS server. When the SN1-QoS-Traffic-Policy attribute is sent along with the Acct-Session-ID attribute, the system matches the particular PtDP context, and applies the new policy and retains the policy with the subscriber profile for future use. The next time the system sends a CoA request with a new policy and a different Acct-Session-ID for the same subscriber, the previously received policy is also applied to the matching PDP context along with the new policy.

IMPORTANT:

This attribute is specific to the GGSN service.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

177

Value

Contains the following subattributes:
Direction

Direction of traffic.

Type

1

Length

1

Value

Unsigned integer Supported values are:

- Downlink = 0
- Uplink = 1

Class

Traffic class.

Type

2

Length

1

Value

Unsigned integer Supported values are:

- Undefined = 0
- Conversational = 1
- Streaming = 2
- Interactive TP 1 = 4
- Interactive TP 2 = 5
- Interactive TP 3 = 6
- Background = 7

Burst-Size

Peak burst size.

Type

3

Length

4

Value

Unsigned integer
Committed-Data-Rate

Committed data rate.

Type

4

Length

4

Value

Unsigned integer
Peak-Data-Rate

Peak data rate.

Type

5

Length

4

Value

Unsigned integer
Exceed-Action

Action to take on packets that exceed the Committed-Data-Rate but do not violate the Peak-Data-Rate.

Type

6

Length

1

Value

Unsigned integer Supported values are:

- Transmit = 0
- Drop = 1
- Lower IP Precedence = 2

Violate-Action

Violate action.

Type

7

Length

1

Value

Unsigned integer Supported values are:

- Transmit = 0
- Drop = 1
- Lower IP Precedence = 2
- Buffer = 3
- Buffer-Transmit-On-Full = 4

Auto-Readjust-Enabled

Available only in StarOS 8.1 and later. Auto-readjust enabled.

Type

8

Length

1

Value

Unsigned integer
Auto-Readjust-Duration

Available only in StarOS 8.1 and later. Auto-readjust duration.

Type

9

Length

4

Value

Unsigned integer
Qci

Available only in 11.0 and later releases. QOS QCI accepted values are 1 (qci 1), 2 (qci 2), 3 (qci 3), 4 (qci 4), 5 (qci 5), 6 (qci 6), 7 (qci 7), 8 (qci 8), 9 (qci 9).

Type

10

Length

1

Value

Unsigned integer
SN1-Rad-APN-Name

This attributes specifies the RADIUS returned APN name.

If this AVP is not present in the Access Accept message or if the AVP value is invalid, the SGSN supplied APN value in create PDP context will be used for the session.

Type

26

Vendor ID

8164

VSA Type

162

Length

1–64

Value

Opaque value
SN1-Radius-Returned-Username

This attribute is used to prefer RADIUS returned user name over constructed username in the accounting messages.

Type

26

Vendor ID

8164

VSA Type

236

Length

4

Value

Enumerated integer. Supported values are:

- No = 0
- Yes = 1

SN1-Re-CHAP-Interval

The Periodic CHAP authentication interval for PPP, in seconds.

Type

26

Vendor ID

8164

VSA Type

7

Length

4

Value

Integer.
SN1-Roaming-Behavior

This attribute specifies the configuration for the behavior bits settings for a roaming subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for "roaming" subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by "Or"ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

121

Length

4

Value

Unsigned integer
SN1-Roaming-Profile

This attribute specifies the configuration for the profile bits settings for a roaming subscriber in an APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

118

Length

4

Value

Unsigned integer
SN1-Roaming-Sub-Use-GGSN

This attribute configures GGSN to accept GGSN's charging characteristics for roaming subscribers defined for the APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

108

Length

4

Value

Enumerated integer. Supported values are:

- Deny = 0
- Accept = 1

SN1-ROHC-Direction

Specifies in which direction to apply Robust Header Compression (ROHC).

Type

Type 26

Vendor ID

Vendor-ID 8164

VSA Type

VSA-Type 153

Length

4

Value

Enumerated integer. Supported values are:

- Any = 0
- Uplink = 1
- Downlink = 2

SN1-ROHC-Flow-Marking-Mode

Configure ROHC compression for marked flows only.

Type

26

Vendor ID

8164

VSA Type

216

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

SN1-ROHC-Mode

Sets the mode of operation for Robust Header Compression for IP.

Type

26

Vendor ID

8164

VSA Type

151

Length

4

Value

Enumerated integer. Supported values are:

- Reliable = 0
- Optimistic = 1
- Unidirectional = 2

SN1-ROHC-Profile-Name

Specifies the ROHC profile name to use for the subscriber.

Type

26

Vendor ID

8164

VSA Type

238

Length

1–64

Value

ASCII string
SN1-Routing-Area-Id

For GGSN calls this indicates the Routing Area ID of the subscriber.

Type

26

Vendor ID

8164

VSA Type

249

Length

3

Value

Opaque value
SN1-Rulebase

When the session is active charging enabled, Rulebase name will specify one of the pre configured ECSv2 rulebases in active charging subsystem.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

If this AVP is present in Access Accept message the locally configured APN value will be overridden. If there is no value configured in the APN, this value will not be applied to the session.

Type

26

Vendor ID

8164

VSA Type

249

Length

1–64

Value

String
SN1-Secondary-DCCA-Peer

This attribute indicates the name of the Secondary DCCA peer and Secondary DCCA realm.

If this AVP is received in Access Accept message the secondary DCCA peer is used for Gy functionality. If not present in the Access Accept message or if the AVP value is invalid, the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

224

Length

1–192

Value

A colon separated string, like “secondary_peer : secondary_realm”.
SN1-Secondary-DNS-Server

This attribute indicates the IP address of the secondary DNS server that should be used for the session.

Type

26

Vendor ID

8164

VSA Type

6

Length

4

Value

IPv4 address
SN1-Secondary-NBNS-Server

Secondary NBNS Server IP Address.

Type

26

Vendor ID

8164

VSA Type

149

Length

4

Value

IPv4 address
SN1-Service-Address

Used to send the bind IP address of the service in RADIUS messages.

Type

26

Vendor ID

8164

VSA Type

169

Length

4

Value

IPv4 address
SN1-Service-Type

This attribute signifies the type that the user is accessing.

Type

26

Vendor ID

8164

VSA Type

24

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- PDSN = 1
- Management = 2
- HA = 3
- GGSN = 4
- LNS = 5
- IPSG = 6
- CSCF = 7
- ASNGW = 8
- PDIF = 9
- STANDALONE_FA = 10
- SGSN = 11
- PHSGW = 12
- PDG = 13
- MIPV6HA = 14
- PGW = 15
- SGW = 16
- FNG = 17
- OGW = 18 — NOTE: Applicable only in release 12.0.
- HNBGW = 19

SN1-Simultaneous-SIP-MIP

This attribute indicates if a PDSN Subscriber can simultaneously be given Simple IP and Mobile IP service.

Type

26

Vendor ID

8164

VSA Type

22

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Subscriber-Acct-Mode

SN1-Subscriber-Acct-Mode

Type

26

Vendor ID

8164

VSA Type

192

Length

4

Value

Enumerated integer. Supported values are:

- flow-based-auxilliary = 0
- flow-based-all = 1
- flow-based-none = 2
- session-based = 3
- main-a10-only = 4

SN1-Subscriber-Accounting

This attribute specifically enables or disables subscriber accounting. Note that if enabled, subscriber accounting still needs to be enabled in the subscriber's AAA context for accounting to be performed.

The AVP value 0 means no accounting; 1 indicates RADIUS accounting; and 2 indicates GTPP accounting. If an invalid value is received or if the AVP is not present in the Access Accept message, then the locally configured APN value will be used.

Type

26

Vendor ID

8164

VSA Type

64

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Radius = 1
- GTPP = 2

SN1-Subscriber-Acct-Interim

This attribute specifies if accounting INTERIM messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context (along with a specific INTERIM interval), if accounting INTERIM messages are to be sent.

The AVP value 0 represents normal or enabled for generating accounting INTERIM messages. The value 1 represents enabled for suppressing RADIUS accounting INTERIM messages.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

70

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Suppress = 1

SN1-Subscriber-Acct-Rsp-Action

When this attribute is set to None, there is no action taken while waiting for a response for the accounting start message from the RADIUS server. When this attribute is set to No-Early-PDUs the system buffers all packets from the user (uplink) until a response for the accounting start message is received from the RADIUS server. When set to Delay_GTP_Response, the system does not send a GTP create response to the GGSN until a response for the accounting start message is received from the RADIUS server.

Type

26

Vendor ID

8164

VSA Type

100

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- No_Early_PDUs = 1
- Delay_GTP_Response = 2

SN1-Subscriber-Acct-Start

This attribute specifies if accounting START messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting START messages are to be sent.

The AVP value 0 represents normal or enabled for generating accounting START messages. The value 1 represents enabled for suppressing RADIUS accounting START messages.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

69

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Suppress = 1

SN1-Subscriber-Acct-Stop

This attribute specifies if accounting STOP messages are enabled for the subscriber. Note that accounting must also be globally enabled for the subscriber (SN-Subscriber-Accounting), and enabled for the subscriber's AAA context, if accounting STOP messages are to be sent.

The AVP value 0 represents normal or enabled for generating accounting STOP messages. The value 1 represents enabled for suppressing RADIUS accounting STOP messages.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

71

Length

4

Value

Enumerated integer. Supported values are:

- Normal = 0
- Suppress = 1

SN1-Subscriber-Class

Customer-requested attribute for supporting specific behavior for their subscriber billing.

Type

26

Vendor ID

8164

VSA Type

219

Length

4

Value

Enumerated integer. Supported values are:

- Normal_Subscriber = 0
- Ting_100 = 1
- Ting_500 = 2
- Ting_Buddy = 3
- Ting_Star = 4
- Ting_Nolimit_SMS = 5
- Kids_Locator = 6
- Ting_2000 = 7
- Handicapped_Welfare = 8
- Reserved = 9

SN1-Subscriber-Dormant-Activity

This attribute specifies whether to treat dormant packets routed to the mobile as activity for idle timeout purposes. The default is Enabled. Disabled means dormant packets routed to the mobile are not treated as activity for idle timeout purposes.

Type

26

Vendor ID

8164

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Subscriber-IP-Hdr-Neg-Mode

This attribute specifies whether to wait for (detect) IP header compression to be requested by the mobile before responding, or not to wait (force). Force is the default.

Type

26

Vendor ID

8164

VSA Type

67

Length

4

Value

Enumerated integer. Supported values are:

- Force = 0
- Detect = 1

SN1-Subscriber-IP-TOS-Copy

This attribute enables copying of TOS bits from outer IP headers into inner tunneled IP headers. The default is Both.

Type

26

Vendor ID

8164

VSA Type

85

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Access-Tunnel = 1
- Data-Tunnel = 2
- Both = 3

SN1-Subscriber-Nexthop-Address

This attribute specifies the nexthop gateway address to be returned by AAA on a per subscriber basis.

Type

26

Vendor ID

8164

VSA Type

127

Length

6

Value

IPv4 address
SN1-Subscriber-No-Interims

This is a GGSN specific attribute. When set to 0 (disabled) interim accounting is generated. When set to 1 (enabled) interim accounting generation is disabled.

If the AVP is not present in the Access Accept message or if the AVP value is invalid, the value 0 is assumed.

Type

26

Vendor ID

8164

VSA Type

133

Length

4

Value

Enumerated integer. Supported values are:

- Enabled = 0
- Disabled = 1

SN1-Subscriber-Permission

This attribute indicates the services allowed to be delivered to the subscriber. The attribute value is a bit field, and many algorithms can be specified to indicate that one of these may be chosen by the user.

Type

26

Vendor ID

8164

VSA Type

20

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Simple-IP = 1
- Mobile-IP = 2
- Simple-IP-Mobile-IP = 3
- HA-Mobile-IP = 4
- Simple-IP-HA-Mobile-IP = 5
- Mobile-IP-HA-Mobile-IP = 6
- All = 7

In StarOS 8.3 and later, supported values are:

- None = 0
- Simple-IP = 1
- Mobile-IP = 2
- Simple-IP-Mobile-IP = 3
- HA-Mobile-IP = 4
- Simple-IP-HA-Mobile-IP = 5
- Mobile-IP-HA-Mobile-IP = 6
- SIP-MIP-HA-MIP = 7
- GGSN-PDP-TYPE-IP = 0x08, # see SessSubscriberPermission in sess_common.x
- GGSN-PDP-TYPE-PPP = 0x10, # see SessSubscriberPermission in sess_common.x
- Network-Mobility = 0x20
- FA-HA-NEMO = 0x26
- All = 0x3F

SN1-Subscriber-Template-Name

RADIUS returned subscriber template.

Type

26

Vendor ID

8164

VSA Type

158

Length

1–127

Value

String
SN1-Subs-Acc-Flow-Traffic-Valid

This attribute indicates the subscriber account flow traffic is valid.

Type

26

Vendor ID

8164

VSA Type

225

Length

4

Value

Enumerated integer. Supported values are:

- Disable = 0
- Enable = 1

SN1-Subs-IMSA-Service-Name

IMS Authorization Service name.

Type

26

Vendor ID

8164

VSA Type

159

Length

1–128

Value

ASCII string
SN1-Subs-VJ-Slotid-Cmp-Neg-Mode

Enable/Disable slotid compression in either direction when using VJ compression.

Type

26

Vendor ID

8164

VSA Type

221

Length

4

Value

Enumerated integer. Supported values are:

- None = 0
- Receive = 1
- Transmit = 2
- Both = 3

SN1-Tp-Dnlk-Burst-Size

This attribute specifies the Traffic Policing downlink burst size in bytes.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

76

Length

4

Value

Unsigned integer
SN1-Tp-Dnlk-Committed-Data-Rate

This attribute specifies the Traffic Policing downlink committed data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

74

Length

4

Value

Unsigned integer
SN1-Tp-Dnlk-Exceed-Action

This attribute specifies the action to take on Traffic Policing downlink packets that exceed the committed-data-rate but do not violate the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

77

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN1-Tp-Dnlk-Peak-Data-Rate

This attribute specifies the Traffic Policing downlink peak data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

75

Length

4

Value

Unsigned integer
SN1-Tp-Dnlk-Violate-Action

This attribute specifies the action to take on Traffic Policing downlink packets that exceed both the committed-data-rate and the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

78

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN1-Tp-Uplk-Burst-Size

This attribute specifies the Traffic Policing uplink burst size in bytes.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

82

Length

4

Value

Unsigned integer
SN1-Tp-Uplk-Committed-Data-Rate

This attribute specifies the Traffic Policing uplink committed data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

80

Length

4

Value

Unsigned integer
SN1-Tp-Uplk-Exceed-Action

This attribute specifies the action to take on Traffic Policing uplink packets that exceed the committed-data-rate but do not violate the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

83

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN1-Tp-Uplk-Peak-Data-Rate

This attribute specifies the Traffic Policing uplink peak data rate in bps.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

81

Length

4

Value

Unsigned integer
SN1-Tp-Uplk-Violate-Action

This attribute specifies the action to take on Traffic Policing uplink packets that exceed both the committed-data-rate and the peak-data-rate.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

8164

VSA Type

84

Length

4

Value

Enumerated integer. Supported values are:

- Transmit = 0
- Drop = 1
- Lower-IP-Precedence = 2
- Buffer = 3
- Transmit-On-Buffer-Full = 4

SN1-Traffic-Group

This attribute is used to assign a tag to a FA or a group of FAs, so that traffic policy can be enforced based on the tag value.

Type

26

Vendor ID

8164

VSA Type

161

Length

2

Value

Unsigned integer
SN1-Transparent-Data

This AVP is used by RADIUS to provide Global Title information for the GGSN to use in CDRs and Quota Auth.

Type

26

Vendor ID

8164

VSA Type

247

Length

In StarOS 8.1 and later: 1–247 In StarOS 8.0: 1–237

Value

Opaque value
SN1-Tun-Addr-Policy

Describes IP address validation policy for non L2TP tunneled calls.

Type

26

Vendor ID

8164

VSA Type

156

Length

4

Value

Enumerated integer. Supported values are:

- no-local-alloc-validate = 0
- local-alloc = 1
- local-alloc-validate = 2

SN1-Tunnel-Gn

Used to enable/disable Gn interface from PDG/TTG to GGSN.

Type

26

Vendor ID

8164

VSA Type

174

Length

4

Value

Enumerated integer. Supported values are:

- Disabled = 0
- Enabled = 1

SN1-Tunnel-ISAKMP-Crypto-Map

This attribute specifies the system-defined crypto map to use for the subscriber's Mobile-IP connection, when IPSec is used to protect the Mobile-IP connection. This attribute is salt-encrypted.

Type

26

Vendor ID

8164

VSA Type

38

Length

1–128

Value

String
SN1-Tunnel-ISAKMP-Secret

This attribute specifies the secret to use for IKE.

Type

26

Vendor ID

8164

VSA Type

39

Length

1–128

Value

String
SN1-Tunnel-Load-Balancing

Specifies the load-balancing algorithm to use when tunneling is employed.

Type

26

Vendor ID

8164

VSA Type

27

Length

4

Value

Enumerated integer. Supported values are:

- random = 1
- balanced = 2
- prioritized = 3

SN1-Tunnel-Password

This attribute contains a secret for tunneling usage. Currently this is only used for L2TP. It is recommended that if your RADIUS server supports salt-encryption of attributes, that you use the Tunnel-Password attribute instead.

Type

26

Vendor ID

8164

VSA Type

26

Length

1–247

Value

A bitstring which is the tunnel secret.
SN1-Unclassify-List-Name

SN1-Unclassify-List-Name.

Type

26

Vendor ID

8164

VSA Type

132

Length

1–132

Value

String
SN1-Virtual-APN-Name

This attribute indicates the virtual APN name.

Type

26

Vendor ID

8164

VSA Type

94

Length

1–64

Value

Opaque value
SN1-Visiting-Behavior

This attribute specifies the configuration for the behavior bits settings for a visiting subscriber in an APN.

When GGSN is configured to reject the charging characteristics sent by the SGSN for "home" subscribers, it uses the profile index specified by cc-home behavior <bits> profile <index> command to determine the appropriate CCs to use.

Multiple behavior bits can be configured for a single profile index by "Or"ing the bit strings together and convert the result to hexadecimal. The properties of the actual CC profile index are configured as part of the GGSN service using the cc profile command.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

120

Length

4

Value

Unsigned integer
SN1-Visiting-Profile

This attribute specifies the configuration for the profile bits settings for a visiting subscriber in an APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

117

Length

4

Value

Unsigned integer
SN1-Visiting-Sub-Use-GGSN

This attribute configures GGSN to accept GGSN's charging characteristics for visiting subscribers defined for the APN.

If this AVP is present in Access Accept message the locally configured APN value will be overridden.

Type

26

Vendor ID

8164

VSA Type

107

Length

4

Value

Enumerated integer. Supported values are:

- Deny = 0
- Accept = 1

SN1-Voice-Push-List-Name

SN1-Voice-Push-List-Name.

Type

26

Vendor ID

8164

VSA Type

131

Length

1–32

Value

String
SN1-VPN-ID

This attribute indicates the Destination VPN of the user, specified by a 32-bit identifier.

Type

26

Vendor ID

8164

VSA Type

1

Length

4

Value

Unsigned integer
SN1-VPN-Name

This attribute indicates the name of the user’s destination VPN.

Type

26

Vendor ID

8164

VSA Type

2

Length

1–253

Value

ASCII string
SNA-Input-Gigawords

This attribute contains the total number of input gigawords.

Type

26

Vendor ID

8164

VSA Type

206

Length

4

Value

Unsigned integer
SNA-Output-Gigawords

This attribute contains the total number of output gigawords.

Type

26

Vendor ID

8164

VSA Type

207

Length

4

Value

Unsigned integer
SNA-PPP-Bad-Addr

This attribute contains the total number of frames received with bad address field in the HDLC header field, for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1011

Length

4

Value

Unsigned integer
SNA-PPP-Bad-Ctrl

This attribute contains the total number of frames received with bad control field in the HDLC header field, for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1012

Length

4

Value

Unsigned integer
SNA-PPP-Bad-FCS

This attribute contains the number of frames received, for the user’s PPP session, with bad FCS.

Type

26

Vendor ID

8164

VSA Type

1014

Length

4

Value

Unsigned integer
SNA-PPP-Ctrl-Input-Octets

This attribute contains the number of PPP Control Octets received for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1001

Length

4

Value

Unsigned integer
SNA-PPP-Ctrl-Input-Packets

This attribute contains the number of PPP Control packets received for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1003

Length

4

Value

Unsigned integer
SNA-PPP-Ctrl-Output-Octets

This attribute contains the number of PPP Control Octets sent to the user during the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1002

Length

4

Value

Unsigned integer
SNA-PPP-Ctrl-Output-Packets

This attribute contains the number of PPP Control packets sent to the user during the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1004

Length

4

Value

Unsigned integer
SNA-PPP-Discards-Input

This attribute contains the number of PPP input frames that were discarded during the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1007

Length

4

Value

Unsigned integer
SNA-PPP-Discards-Output

This attribute contains the number of PPP output frames that were discarded during the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1008

Length

4

Value

Unsigned integer
SNA-PPP-Echo-Req-Input

This attribute contains the number of LCP echo packets received, for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1015

Length

4

Value

Unsigned integer
SNA-PPP-Echo-Req-Output

This attribute contains the number of LCP echo packets sent, for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1016

Length

4

Value

Unsigned integer
SNA-PPP-Echo-Rsp-Input

This attribute contains the number of LCP echo response packets received, for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1017

Length

4

Value

Unsigned integer
SNA-PPP-Echo-Rsp-Output

This attribute contains the number of LCP echo response packets sent, for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1018

Length

4

Value

Unsigned integer
SNA-PPP-Errors-Input

This attribute contains the number of PPP input de-framing errors for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1009

Length

4

Value

Unsigned integer
SNA-PPP-Errors-Output

This attribute contains the number of PPP output framing errors for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1010

Length

4

Value

Unsigned integer
SNA-PPP-Framed-Input-Octets

This attribute contains the number of PPP octets received (without framing overhead) for the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1005

Length

4

Value

Unsigned integer
SNA-PPP-Framed-Output-Octets

This attribute contains the number of PPP octets sent (without framing overhead) to the user during the user’s PPP session.

Type

26

Vendor ID

8164

VSA Type

1006

Length

4

Value

Unsigned integer
SNA-PPP-Packet-Too-Long

This attribute contains the total number of frames received, for the user’s PPP session, that exceeds the MTU of the interface.

Type

26

Vendor ID

8164

VSA Type

1013

Length

4

Value

Unsigned integer
SNA-PPP-Unfr-Data-In-Gig

This attribute contains the total number of PPP gigawords without framing sent for the subscriber's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing send for the subscriber's session.

Type

26

Vendor ID

8164

VSA Type

202

Length

4

Value

Unsigned integer
SNA-PPP-Unfr-Data-Out-Gig

This attribute contains the total number of PPP octets without framing received for the user's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing received for the subscriber's session.

Type

26

Vendor ID

8164

VSA Type

203

Length

4

Value

Unsigned integer
SNA-PPP-Unfr-data-In-Oct

This attribute contains the total number of PPP octets without framing sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

200

Length

4

Value

Unsigned integer
SNA-PPP-Unfr-data-Out-Oct

This attribute contains the total number of PPP octets without framing received for the user’s session.

Type

26

Vendor ID

8164

VSA Type

201

Length

4

Value

Unsigned integer
SNA-RPRAK-Rcvd-Acc-Ack

This attribute contains the total number of A11 registration ACK accepted for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1028

Length

4

Value

Unsigned integer
SNA-RPRAK-Rcvd-Mis-ID

This attribute contains the total number of A11 registration ACK messages received with ID-mismatch for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1030

Length

4

Value

Unsigned integer
SNA-RPRAK-Rcvd-Msg-Auth-Fail

This attribute contains the total number of message auth failures for A11 registration ACK messages for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1029

Length

4

Value

Unsigned integer
SNA-RPRAK-Rcvd-Total

This attribute contains the total number of A11 registration ACK received for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1027

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Acc-Dereg

This attribute contains the number of Accept A11 registration reply sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1033

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Acc-Reg

This attribute contains the number of Accept A11 registration reply sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1032

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Bad-Req

This attribute contains the number of A11 registration reply sent for bad requests for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1034

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Denied

This attribute contains the number of denied A11 registration reply sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1035

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Mis-ID

This attribute contains the number of A11 registration reply sent for mismatched ID for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1036

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Send-Err

This attribute contains the number of A11 registration reply sent with send errors for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1037

Length

4

Value

Unsigned integer
SNA-RP-Reg-Reply-Sent-Total

This attribute contains the total number A11 registration reply sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1031

Length

4

Value

Unsigned integer
SNA-RP-Reg-Upd-Re-Sent

This attribute contains the total number of A11 registration update re-sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1039

Length

4

Value

Unsigned integer
SNA-RP-Reg-Upd-Send-Err

This attribute contains the total number of A11 registration update send errors for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1040

Length

4

Value

Unsigned integer
SNA-RP-Reg-Upd-Sent

This attribute contains the total number of A11 registration update sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1038

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-Acc-Dereg

This attribute contains the number of A11 De-registration Requests accepted for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1021

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-Acc-Reg

This attribute contains the number of A11 Registration Requests accepted for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1020

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-Badly-Formed

This attribute contains the number of badly formed A11 registration requests received for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1024

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-Mis-ID

This attribute contains the number of A11 registration requests received with ID-mismatch for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1023

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-Msg-Auth-Fail

This attribute contains the number of message authentication failures for A11 registration requests for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1022

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-T-Bit-Not-Set

This attribute contains the number of A11 registration requests received with T-Bit not set for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1026

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-Total

This attribute contains the number of A11 Registration Requests received for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1019

Length

4

Value

Unsigned integer
SNA-RPRRQ-Rcvd-VID-Unsupported

This attribute contains the number of A11 registration requests received with an unsupported Vendor ID for the user’s session.

Type

26

Vendor ID

8164

VSA Type

1025

Length

4

Value

Unsigned integer
SNA1-PPP-Unfr-data-In-Gig

This attribute contains the total number of PPP gigawords without framing sent for the subscriber's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing send for the subscriber's session.

Type

26

Vendor ID

8164

VSA Type

202

Length

4

Value

Unsigned integer
SNA1-PPP-Unfr-data-Out-Gig

This attribute contains the total number of PPP octets without framing received for the user's session. When combined with the attribute SNA-PPP-Unfr-data-In-Oct, a 64-bit value can be formed which is the total number of PPP octets without framing received for the subscriber's session.

Type

26

Vendor ID

8164

VSA Type

203

Length

4

Value

Unsigned integer
SNA1-PPP-Unfr-data-In-Oct

This attribute contains the total number of PPP octets without framing sent for the user’s session.

Type

26

Vendor ID

8164

VSA Type

200

Length

4

Value

Unsigned integer
SNA1-PPP-Unfr-data-Out-Oct

This attribute contains the total number of PPP octets without framing received for the user’s session.

Type

26

Vendor ID

8164

VSA Type

201

Length

4

Value

Unsigned integer
Terminal-Capability

Opaque one byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

219

Length

1

Value

The system does not interpret this value, but it is copied in accounting messages.
Termination-Action

Indicates what action the NAS should take when the service is completed. AAAmgr passes this attribute to Sessmgr only for ASN-GW calls. The combination of Session-Timeout and Termination-Action attributes received in Access-Accept or Access-Challenge determines how NAS should interpret it.

Type

29

Vendor ID

N/A

VSA Type

N/A

Length

6

Value

Enumerated integer. Supported values are:

- Default = 0 — Indicates that the session should terminate.
- RADIUS-Request = 1 — Indicates that re-authentication should occur on expiration of the Session-Time. Upon termination of the specified service the NAS may send a new Access-Request to the RADIUS server, including the State attribute if any.

Tunnel-Assignment-ID

This attribute indicates the tunnel to which the session is to be assigned.

Type

82

Vendor ID

N/A

VSA Type

N/A

Length

1–247

Value

ASCII string. It can be tagged.
Tunnel-Client-Auth-ID

This attribute contains the name of the client for the purposes of tunnel authentication.

Type

90

Vendor ID

N/A

VSA Type

N/A

Length

1–247

Value

ASCII string. It can be tagged.
Tunnel-Client-Endpoint

This attribute is an identifier of the Tunnel client. When Tunnel-Medium-Type = IPv4, then this attribute is in the form of an IP address string in “dotted-decimal” notation.

Type

66

Vendor ID

N/A

VSA Type

N/A

Length

1–250

Value

Opaque value. It can be tagged.
Tunnel-Medium-Type

This attribute indicates the protocol medium over which the tunneling protocol runs. It is used to describe the format of the attributes Tunnel-Client-Endpoint and Tunnel-Server-Endpoint.

Type

65

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. It can be tagged. Supported values are:

- IPv4 = 1
- IPv6 = 2
- NSAP = 3
- HDLC = 4
- BBN-1822 = 5
- IEEE-802 = 6
- E-163 = 7
- E-164 = 8
- F-69 = 9
- X-121 = 10
- IPX = 11
- Appletalk = 12
- Decnet-IV = 13
- Banyan-Vines = 14
- E-164-NSAP-Subaddress = 15

Tunnel-Password

This attribute contains a shared secret for the Tunnel connection. It is salt-encrypted.

Type

69

Vendor ID

N/A

VSA Type

N/A

Length

1–240

Value

Opaque value
Tunnel-Preference

This attribute indicates the priority given to the tunnel group. The tunnel group is defined as those tunnel attributes that have the same tag.

Type

82

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Unsigned integer
Tunnel-Private-Group-ID

This attribute contains the context of the tunnel.

Type

81

Vendor ID

N/A

VSA Type

N/A

Length

1–252

Value

ASCII string. It can be tagged.
Tunnel-Server-Auth-ID

This attribute contains the name of the server for the purposes of tunnel authentication.

Type

91

Vendor ID

N/A

VSA Type

N/A

Length

1–252

Value

Opaque value
Tunnel-Server-Endpoint

This attribute is an identifier of the Tunnel server. When Tunnel-Medium-Type = IPv4, then this attribute is in the form of an IP address string in “dotted-decimal” notation.

Type

67

Vendor ID

N/A

VSA Type

N/A

Length

1–250

Value

A string identifying the Tunnel server. It can be tagged.

IMPORTANT:

This attribute is used in conjunction with L2TP functionality. Refer to the RFC 2868 Tunneling Attributes section for additional information on this and other attributes added in support of this functionality.
Tunnel-Type

This attribute indicates the type of tunnel used by the subscriber.

Type

64

Vendor ID

N/A

VSA Type

N/A

Length

4

Value

Enumerated integer. It can be tagged. Supported values are:

- PPTP = 1
- L2F = 2
- L2TP = 3
- ATMP = 4
- VTP = 5
- AH = 6
- IP-IP = 7
- MIN-IP-IP = 8
- ESP = 9
- GRE = 10
- DVS = 11
- MIP = 12
- VLAN = 13

User-Name

This attribute indicates the name of the user to be authenticated. This field can contain a stand-alone user name, or a user name and domain name. The format of this field is variable and configurable on a per-context basis. Separation of user and domain names is delineated by a special character, which can be %, -, @, \, #, and /. The user name may appear before the domain name or after. If this attribute is included in the Access-Accept, then the value of that attribute will be the value of the User-Name attribute in subsequent Accounting-Request messages for that particular session.

This attribute is also accepted in CoA request and response messages to be used in a currently active subscriber session.

Type

1

Vendor ID

N/A

VSA Type

N/A

Length

1–253

Value

String
User-Password

This attribute contains the encrypted password of the user, when simple password authentication is being used.

Type

2

Vendor ID

N/A

VSA Type

N/A

Length

1–128

Value

String
White-List

This attribute contains the list of IMSIs which are allowed to access through an HNB.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

9

VSA Type

117

Length

3–251

Value

Opaque value
WiMAX-Acct-Input-Packets-Giga

Number of packets incremented each time Acct-Input-Packets(47) overflows.

Type

26

Vendor ID

24757

VSA Type

48

Length

4

Value

Unsigned integer
WiMAX-Acct-Output-Packets-Giga

Number of packets incremented each time Acct-Output-Packets(48) overflows.

Type

26

Vendor ID

24757

VSA Type

49

Length

4

Value

Unsigned integer
WiMAX-Active-Time

The period of time the session was NOT in idle state.

Type

26

Vendor ID

24757

VSA Type

39

Length

4

Value

Unsigned integer
WiMAX-Beginning-Of-Session

This attribute indicates whether the session is new or a continuation of previous flow.

Type

26

Vendor ID

24757

VSA Type

22

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

WiMAX-BS-ID

Uniquely identifies an NAP and a Base Station within that NAP. The first three octets representing the NAP operator identifier, and the next three the Base Station ID.

Type

26

Vendor ID

24757

VSA Type

46

Length

6–12

Value

Opaque value
WiMAX-Capability

This compound attribute identifies the supported WiMAX capabilities.

Type

26

Vendor ID

24757

VSA Type

1

Length

1–246

Value

Contains the following subattributes:
WiMAX-Release

Specifies WiMAX release of the sender.

Type

1

Length

4

Value

ASCII string
Accounting-Capabilities

Describes accounting capabilities supported for the session.

Type

2

Length

1

Value

0x00 = No accounting. Only valid at the HA.

- 0x01 = IP-Session-based accounting. Default value for the ASN.
- 0x02 = Flow-based accounting

Hotlining-Capabilities

Supported hotline capabilities.

Type

3

Length

1

Value

- Not-Supported = 0x00 — Hotlining is not supported
- Hotline-Profile-Id = 0x01 — Profile-based Hot lining is supported (using Hotline-Profile-ID VSA)
- NAS-Filter = 0x02 — Rule-based Hot lining is supported using NAS-Filter-Rule
- HTTP-Redirection = 0x04 — Hot lining HTTP Redirection is supported.
- Profile-Id-based-and-HTTP-Redirection-Rule-based = 0x05
- IP-Redirection = 0x08 — Rule-based Hot lining is supported using IP-Redirection rule.

Idle-Mode-Notification-Capabilities

Describes idle mode notification capabilities.

Type

4

Length

1

Value

0x00 = Idle Mode notification is not supported or is not required.

- 0x01 = Idle Mode notification is supported or is required.

ROHC-Support

Describes ROHC capability support for the session

Type

11

Length

1

Value

Enumerated integer. Supported values are:

- Not-Supported = 0x00
- Supported = 0x01

WiMAX-Control-Octets-In

Octet counts for incoming Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.

Type

26

Vendor ID

24757

VSA Type

4

Length

13

Value

Unsigned integer
WiMAX-Control-Octets-Out

Octet counts for outgoing Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.

Type

26

Vendor ID

24757

VSA Type

34

Length

4

Value

Unsigned integer
WiMAX-Control-Packets-In

Packet counts for incoming Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.

Type

26

Vendor ID

24757

VSA Type

4

Length

13

Value

Unsigned integer
WiMAX-Control-Packets-Out

Packet counts for outgoing Mobile IP, DHCP, ICMP messages for IPv4 and IPv6.

Type

26

Vendor ID

24757

VSA Type

33

Length

4

Value

Unsigned Integer
WiMAX-Count-Type

Indicates if the record represents compressed counts over-the-air.

Type

26

Vendor ID

24757

VSA Type

59

Length

4

Value

Enumerated integer. Supported values are:

- Uncompressed = 0
- Compressed = 1

WiMAX-Device-Auth-Indicator

Indicates whether NAS performed device authentication successfully or not.

Type

26

Vendor ID

24757

VSA Type

2

Length

1

Value

Unsigned octet.
WiMAX-Flow-Description

Describes a flow classifier.

Type

26

Vendor ID

24757

VSA Type

50

Length

1–240

Value

String
WiMAX GMT-Time-Zone-Offset

The current offset in seconds of the local time at the NAS with respect to GMT time.

Type

26

Vendor ID

24757

VSA Type

3

Length

4

Value

Unsigned integer
WiMAX-Home-HNP-PMIP6

The IPv6 Home Network Prefix assigned by the AAA in HCSN to the MS for PMIP6 mobility session.

Type

26

Vendor ID

24757

VSA Type

133

Length

2–18

Value

Opaque value
WiMAX-Home-IPv4-HoA-PMIP6

The IPv4 Home Address assigned by the CSN to the MS for PMIP6-IPv4 mobility session.

Type

26

Vendor ID

24757

VSA Type

135

Length

4

Value

IPv4 Address
WiMAX-Idle-Mode-Transition

A flag indicating whether the mobile node is in idle mode or not. When the mobile node enters or exits idle mode, an interim accounting message that includes WiMAX-Idle-Mode-Transition(26/44) attribute is generated instantly. The value of this attribute is 1 when mobile enters idle mode, and 0 when mobile exits idle mode. If accounting mode is flow based, then the asynchronous interim message is generated only for an ISF and not for all the flows in the session. Regular interim accounting if enabled, is not affected by idle mode entry. Also, the regular interim messages will not include WiMAX-Idle-Mode-Transition attribute.

Type

26

Vendor ID

24757

VSA Type

44

Length

1

Value

Enumerated integer. Supported values are:

- In idle mode = 0x01
- Not in idle mode = 0x00

WiMAX-IP-Technology

Indicates the type of WiMAX session being used.

Type

26

Vendor ID

24757

VSA Type

23

Length

4

Value

Enumerated integer. Supported values are:

- SIP = 1
- PMIP4 = 2
- CMIP4 = 3
- CMIP6 = 4
- Ethernet-CS = 5
- PMIP6 = 6

WiMAX-NAP-ID

Uniquely identifies the Network Access Provider.

Type

26

Vendor ID

24757

VSA Type

45

Length

3

Value

String
WiMAX-NSP-ID

Uniquely identifies the Network Service Provider.

Type

26

Vendor ID

24757

VSA Type

57

Length

3

Value

Opaque value
WiMAX-Packet-Flow-Descriptor

This compound attribute describes a packet flow. A packet flow may describe uni-directional flow and bi-directional flow. The packet flow descriptor may be pre-provisioned. A packet flow descriptor references one or two QoS specifications.

Type

26

Vendor ID

24757

VSA Type

28

Length

4–1400

Value

Contains the following subattributes:
PDF-ID

Used to match all records from the same Packet Data Flow.

Type

1

Length

2

Value

Unsigned integer
SDF-ID

Used to match all PDFs from the same Service Data Flow.

Type

2

Length

2

Value

Unsigned integer
Service-Profile-ID

Identifies a pre configured Flow Descriptor at the NAS.

Type

3

Length

4

Value

Unsigned integer
Direction

Direction of the PDF.

Type

4

Length

1

Value

Enumerated integer. Supported values are:

- Uplink = 1
- Downlink = 2
- Bi-Directional = 3

Activation-Trigger

Specifies the trigger to be used for the activation of Service Flow.

Type

5

Length

1

Value

Enumerated integer. Supported values are:

- Provisioned = 0x01
- Admit = 0x02
- Provisioned-Admit = 0x03
- Activate = 0x04
- Provisioned-Activate = 0x05
- Admit-Activate = 0x06
- Provisioned-Admit-Activate = 0x07
- Dynamic = 0x08
- Dynamic-Admit = 0x0a
- Dynamic-Activate = 0x0c
- Dynamic-Admit-Activate = 0x0e

Transport-Type

Type of transport (IP, Ethernet).

Type

6

Length

1

Value

Enumerated integer
Uplink-QoS-ID

Identifier of the QoS Descriptor for Uplink or Bidirection.

Type

7

Length

1

Value

Unsigned integer
Downlink-QoS-ID

Identifier of the QoS Descriptor for Downlink.

Type

8

Length

1

Value

Unsigned integer
Uplink-Classifier

Classifier to match for traffic flowing in Uplink Direction.

Type

9

Length

1–240

Value

String
Downlink-Classifier

Classifier to match for traffic flowing in Downlink Direction.

Type

10

Length

1–240

Value

String
WiMAX-Packet-Flow-Descriptor-V2

Describes a Unidirectional or Bidirectional Packet Flow Descriptor Version 2.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

84

Length

4–1400

Value

Contains the following subattributes:
PDF-ID

Used to match all records from the same Packet Data Flow.

Type

1

Length

2

Value

Unsigned integer
SDF-ID

Used to match all PDFs from the same Service Data Flow.

Type

2

Length

2

Value

Unsigned integer
Service-Profile-ID

Identifies a pre-configured Flow Descriptor at the NAS.

Type

3

Length

4

Value

Unsigned integer
Direction

Direction of the PDF.

Type

4

Length

1

Value

Enumerated integer. Supported values are:

- Uplink = 1
- Downlink = 2
- Bi-Directional = 3

Activation-Trigger

Specifies the trigger to be used for the activation of Service Flow.

Type

5

Length

1

Value

Enumerated integer. Supported values are:

- Provisioned = 0x01
- Admit = 0x02
- Activate = 0x04
- Dynamic = 0x08

Transport-Type

Type of transport (IP, Ethernet).

Type

6

Length

1

Value

Enumerated integer. Supported values are:

- IPv4-CS = 1
- IPv6-CS = 2
- Ethernet = 3

Uplink-QoS-ID

Identifier of the QoS Descriptor for Uplink or Bidirection.

Type

7

Length

1

Value

Unsigned integer
Downlink-QoS-ID

Identifier of the QoS Descriptor for Downlink.

Type

8

Length

1

Value

Unsigned integer
WiMAX-Packet-Flow-Classifier

Describes Packet Flow Classifiers.

Type

9

Value

Contains the following subattributes:
Classifier-ID

WiMAX Classifier ID.

Type

1

Length

1

Value

Unsigned integer
Priority

WiMAX Classifier Priority.

Type

2

Length

1

Value

Unsigned integer
Protocol

WiMAX Classifier Protocol, i.e TCP/UDP.

Type

3

Length

1

Value

In StarOS 10.0 and earlier, enumerated integer. Supported values are:

- ICMP = 1
- TCP = 6
- UDP = 17

In StarOS 10.2 and later, Unsigned integer
Direction

Direction of the PDF.

Type

4

Length

1

Value

Enumerated integer. Supported values are:

- Uplink = 1
- Downlink = 2
- Bi-Directional = 3

Source-Specification

Identifies WiMAX classifier rule params for source specification.

Type

5

Value

Contains the following subattributes:
IP-Address

This attribute contains source/destination address.

Type

1

Length

4

Value

IPv4 address.
IP-Address-Range

WiMAX Packet Classifier IP Address Range.

Type

2

Length

1

Value

Opaque value
IP-Address-Mask

WiMAX Packet Classifier IP Address Mask.

Type

3

Length

5

Value

Opaque value
Port

WiMAX Packet Classifier Port.

Type

4

Length

2

Value

Unsigned integer
Port-Range

WiMAX Packet Classifier Port Range.

Type

5

Length

4

Value

Unsigned integer
Inverted

WiMAX Classifier Inverted.

Type

6

Length

1

Value

Enumerated integer. Supported values are:

- FALSE = 0
- TRUE = 1

Assigned

WiMAX Classifier Assigned.

Type

7

Length

1

Value

Enumerated integer. Supported values are:

- Src_Assigned = 1
- Dest_Assigned = 2
- Src_Dest_Assigned = 3

Destination-Specification

Identifies WiMAX classifier rule params for destination specification.

Type

6

Value

Contains the following subattributes:
IP-Address

This attribute contains source/destination address.

Type

1

Length

4

Value

IPv4 address.
IP-Address-Range

WiMAX Packet Classifier IP Address Range.

Type

2

Length

8

Value

Opaque value
IP-Address-Mask

WiMAX Packet Classifier IP Address Mask.

Type

3

Length

5

Value

Opaque value
Port

WiMAX Packet Classifier Port.

Type

4

Length

2

Value

Unsigned integer
Port-Range

WiMAX Packet Classifier Port Range.

Type

5

Length

4

Value

Unsigned integer
Inverted

WiMAX Classifier Inverted.

Type

6

Length

1

Value

Enumerated integer. Supported values are:

- FALSE = 0
- TRUE = 1

Assigned

WiMAX Classifier Assigned.

Type

7

Length

1

Value

Enumerated integer. Supported values are:

- Src_Assigned = 1
- Dest_Assigned = 2
- Src_Dest_Assigned = 3

IP-TOS-DSCP-Range-And-Mask

WiMAX Classifier WiMAX-IP-TOS-DSCP-Range-And-Mask.

Type

7

Length

1–3

Value

Opaque value
Action

WiMAX Classifier Action.

Type

8

Length

1

Value

Enumerated integer. Supported values are:

- Reserved = 0
- Permit = 1
- Deny = 2

Paging-Preference

WiMAX Paging Preference.

Type

10

Length

1

Value

Enumerated integer. Supported values are:

- FALSE = 0
- TRUE = 1

WiMAX-PDF-ID

The value of this attribute matches all records from the same packet data flow. PDFID is assigned by the CSN and remains constant through all handover scenarios.

Type

26

Vendor ID

24757

VSA Type

26

Length

2

Value

Unsigned integer
WiMAX-PPAC

The Prepaid-Accounting-Capability (PPAC) attribute is sent in the Access-Request message by a prepaid capable ASNGW, and is used to describe the prepaid capabilities of the ASNGW. The absence of this attribute indicates that the client is not capable of prepaid accounting and the session should not use prepaid accounting.

Type

26

Vendor ID

24757

VSA Type

35

Value

Contains the following subattribute:
Available-In-Client

The optional Available-In-Client subtype, generated by the PPC, indicates the metering capabilities of the NAS and is be bitmap encoded.

Type

1

Length

4

Value

Enumerated integer. Supported values are:

- Supported_None = 0
- Supported_Volume = 1
- Supported_Duration = 2
- Supported_Volume_And_Duration = 3

WiMAX-PPAQ

Prepaid Quota, used for charging, report usage, and request quota. This attribute specifies the characteristics for pre-paid accounting of the volume and/or duration of a packet data session. It should be present in all on-line RADIUS Access-Request and on-line RADIUS Access-Accept messages and may be included in other RADIUS Access-Accept messages. In Authorize-Only Access-Request messages, it is used for one-time charging, report usage and the request for further quota. In an Access-Accept message it is used in order to allocate the (initial and subsequent) quotas.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

37

Value

Contains the following subattributes:
Quota-Identifier

Is generated by the PPS together with the allocation of new quota.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

1

Length

1-4

Value

Opaque value
Volume-Quota

Indicates the volume in octets excluding control data.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

2

Length

4-12

Value

Opaque value
Volume-Threshold

Is generated by the PPS and indicates the volume (in octets) that be consumed before a new quota should be requested.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

3

Length

4-12

Value

Opaque value
Duration-Quota

3GPP2 PrePaid Duration Quota. This is optionally present if duration-based charging is used. In RADIUS Access-Accept message, it indicates the duration (in seconds) allocated for the session by the PPS. In an on-line RADIUS Access-Accept message, it indicates the total duration (in seconds) since the start of the accounting session related to the QuotaID of the PPAQ in which it occurs.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

4

Length

4

Value

Unsigned integer
Duration-Threshold

3GPP2 PrePaid Duration Quota Threshold. This is optionally present if Duration-Quota is present in a RADIUS Access-Accept message. It is generated by the PPS and indicates the duration (in seconds) that should be consumed before a new quota should be requested. This threshold should not be larger than the Duration-Quota.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

5

Length

4

Value

Unsigned integer
Update-Reason

Reason for initiating online quota update operation. This should be present in the Authorize-Only RADIUS Access-Request message. It indicates the reason for initiating the on-line quota update operation. Update reasons 6, 7, 8, and 9 indicate that the associated resources are released at the client side, and that therefore the PPS should not allocate a new quota in the RADIUS Access Accept message.

Type

8

Length

1

Value

Enumerated integer. Supported values are:

- Pre-Initialization = 1
- Initial-Request = 2
- Threshold-Reached = 3
- Quota-Reached = 4
- TITSU-Approaching = 5
- Remote-Forced-Disconnect = 6
- Client-Service-Termination = 7
- Access-Service-Terminated = 8
- Service-Not-Established = 9
- One-Time-Charging = 10

Pre-Paid-Server

PrePaid server IP address. This optional subtype indicates the address IPv4 of the serving PPS. If present, the Home RADIUS server uses this address to route the message to the serving PPS. The attribute may be sent by the Home RADIUS server. Multiple instances of this subtype may be present in a single PPAQ. If present in the incoming RADIUS Access-Accept message, the ASNGW should send this attribute back without modifying it in the subsequent RADIUS Access-Request message.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

9

Length

4

Value

IPv4 address
Service-ID

This value is a string that uniquely describes the service instance to which prepaid metering should be applied.

Type

10

Length

1-246

Value

Opaque value
Rating-Group-ID

Rating-Group-ID for which the WiMAX PPAQ is allocated or reported.

Type

11

Length

4

Value

Unsigned integer
Termination-Action

Describes action to take when PPS does not grant additional quota.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

12

Length

4

Value

Enumerated integer. Supported values are:

- Reserved = 0
- Terminate = 1
- Request-more-quota = 2
- Redirect/Filter = 3

WiMAX-Prepaid-Indicator

Indicates that this session was associated with a prepaid user (online accounting).

Type

26

Vendor ID

24757

VSA Type

25

Length

1

Value

Enumerated integer. Supported values are:

- Offline = 0
- Online = 1

WiMAX-Prepaid-Tariff-Switch

Attribute to indicate Tariff-Switch-Interval / Time-Interval-After-Tariff-Switch-Update by the PPS and Volume-Used-After-Tariff-Switch by the PPC.

Type

26

Vendor ID

24757

VSA Type

38

Value

Contains the following subattributes:
Quota-Identifier

It is generated by the PPS together with the allocation of new quota.

Type

1

Length

1-4

Value

Opaque value
Volume-Used-After-Tariff-Switch

Volume Quota used after Tariff Switch Happened

Type

2

Length

4

Value

Unsigned integer
Tariff-Switch-Interval

Tariff Switch Interval in seconds

Type

3

Length

4

Value

Unsigned integer
Time-Interval-After-Tariff-Switch-Update

Duration after TSI where an on-line RADIUS Access-Request is sent by PrePaid client to report VUATS before the next TS condition is triggered

Type

4

Length

4

Value

Unsigned integer
WiMAX-QoS-Descriptor

This attribute describes over the air QoS parameter that are associated with a flow. The QoS-Descriptor is only valid for the actual RADIUS transaction.

This attribute is also accepted in CoA request message to be used in a currently active subscriber session.

Type

26

Vendor ID

24757

VSA Type

29

Length

6–700

Value

Contains the following 17 subattributes:
QoS-ID

Unique ID for the QoS specification in the packet

Type

1

Length

1

Value

Unsigned integer
Global-Service-Class-Name

Represents Global Service Class Name as defined in IEEE802.16e

Type

2

Length

6

Value

String
Service-Class-Name

Represents Service Class Name as defined in IEEE802.16e

Type

3

Length

2–127

Value

String
Schedule-Type

Specifies Uplink granted scheduling type.

Type

4

Length

1

Value

Enumerated integer. Supported values are:

- Best-Effort = 2
- nrtPS = 3
- rtPS = 4
- Extended-rtPS = 5
- UGS = 6

Traffic-Priority

Specifies the priority assigned to a Service Flow.

Type

5

Length

1

Value

Unsigned integer
Maximum-Sustained-Traffic-Rate

Defines Peak Information Rate of the service in bits/second.

Type

6

Length

4

Value

Unsigned integer
Minimum-Reserved-Traffic-Rate

Defines Minimum Rate reserved for the Service Flow in bits/second.

Type

7

Length

4

Value

Unsigned integer
Maximum-Traffic-Burst

Defines Maximum Burst Size accommodated for the Service in bytes/second

Type

8

Length

4

Value

Unsigned integer
Tolerated-Jitter

Represents Maximum Delay Variation in milliseconds.

Type

9

Length

4

Value

Unsigned integer
Maximum-Latency

Represents Maximum Latency in milliseconds.

Type

10

Length

4

Value

Unsigned integer
Reduced-Resources-Code

Indicates that requesting entity will accept reduced resources if requested resources are unavailable.

Type

11

Length

1

Value

Unsigned integer
Media-Flow-Type

Describes the application type, used as a hint in admission decisions.

Type

12

Length

1

Value

Enumerated integer. Supported values are:

- VoIP = 1
- Robust-Browser = 2
- Secure-Browser/VPN = 3
- Streaming-Video-On-Demand = 4
- Streaming-Live-TV = 5
- Music-Photo-Download = 6
- Multi-Player-Gaming = 7
- Location-Based-Services = 8
- Text-Audio-Books-With-Graphics = 9
- Video-Conversation = 10
- Message = 11
- Control = 12
- Data = 13

Unsolicited-Grant-Interval

Specifies nominal interval between successive data grant opportunities for the Service Flow, in milliseconds.

Type

13

Length

2

Value

Unsigned integer
SDU-Size

Represents the number of bytes in the fixed size SDU.

Type

14

Length

1

Value

Unsigned integer
Unsolicited-Polling-Interval

Specifies maximal nominal interval between successive polling grant opportunities for the Service Flow.

Type

15

Length

2

Value

Unsigned integer
Transmission-Policy

Include options for PDU formation, and for uplink service flows, restrictions on the types of bandwidth request options that may be use.

Type

17

Length

In StarOS 9.0 and earlier releases: 4

In StarOS 10.0 and later releases: 1

Value

In StarOS 10.0 and earlier releases: enumerated integer. Supported values are:

- no-bcast = 0x01
- no-mcast = 0x02
- no-piggy-back = 0x04
- no-fragment = 0x08
- no-sup-payload-header = 0x10
- no-multiple-sdu = 0x20
- no-crc = 0x40
- no-rohc-compression = 0x80

In StarOS 10.2 and later releases: Unsigned integer
DSCP

DSCP

Type

18

Length

4

Value

Enumerated integer. Supported values are:

- Best-Effort=0
- AF11=10
- AF12=12
- AF13=14
- AF21=18
- AF22=20
- AF23=22
- AF31=26
- AF32=28
- AF33=30
- AF41=34
- AF42=36
- AF43=38
- EF=46

WiMAX-RRQ-HA-IP

IPv4 or IPv6 address of the HA as contained in the MIP Registration Request or the BU.

Type

26

Vendor ID

24757

VSA Type

18

Length

4-16

Value

Opaque value
WiMAX-SDF-ID

The value of this attribute matches all records from the same packet data flow. SDFID is assigned by the CSN and remains constant through all handover scenarios.

Type

26

Vendor ID

24757

VSA Type

27

Length

2

Value

Unsigned integer
WiMAX-Session-Continue

The value of this attribute matches all records from the same packet data flow. SDFID is assigned by the CSN and remains constant through all handover scenarios.

Type

26

Vendor ID

24757

VSA Type

21

Length

4

Value

Enumerated integer. Supported values are:

- False = 0
- True = 1

WiMAX-Session-Term-Capability

WiMAX session term capability. This attribute is included in a RADIUS Access-Request message to the RADIUS server and indicates whether or not the NAS supports Dynamic Authorization.

Type

26

Vendor ID

24757

VSA Type

36

Length

4

Value

Enumerated integer. Supported values are:

- Only_Dynamic_Auth_Extn_to_Radius = 0x00000001
- Only_Reg_Revocation_in_MIP = 0x00000002
- Both_Dynamic_Auth_And_Reg_Revocation_in_MIP = 0x00000003

Win-Call-Id

Customer-specific attribute used in custom dictionary. Contains opaque 1 byte value received from customer RADIUS server in access request.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

205

Length

1

Value

The system does not interpret this value, but it is copied in accounting messages.
Win-Service-Name

Opaque value value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages. Used in custom dictionary.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

206

Length

1 – 256

Value

The system does not interpret this value, but it is copied in accounting messages.
WSType

Opaque one byte value received from customer RADIUS server in access request. We need to retain this value and return it back in all future accounting messages.

Type

136

Vendor ID

5535 (Reusing the 3GPP2 VID in a non-standard way.)

VSA Type

197

Length

1

Value

The system does not interpret this value, but it is copied in accounting messages.

Attribute Notes

This section contains notes that apply to groups of attributes that have been included in support of specific features and/or functionality.

RFC 2868 Tunneling Attributes

Tunnel attributes may be tagged, which means the leading byte in the value field may be used to group attributes together. This is used to return a number of different tunnel configurations that are available to the subscriber. The tagged group with the highest tunnel preference (the lowest value of the Tunnel-Preference attribute) has precedence over other tunnel configurations.

Tags can be a value from 1 through 31. Any value outside of this range for the leading byte means the attribute is not tagged, and the leading byte is then interpreted as part of the attribute value. Integer attributes that are tagged are three bytes in length (the leading byte is ignored), but are four bytes in length when not tagged (the leading byte is incorporated).

If Tunnel attributes appear more than once in the RADIUS Accept-Accept but are not tagged, then the system treats the attributes as having an implicit tag. The first instance of the attribute has a tag value of 32, the second instance has a tag value of 33, etc.