# RNC Configuration Mode Commands

The RNC (radio network controller) configuration mode defines the parameters related to the SGSN connection with an RNC.
This mode is accessed from the IuPS Service configuration mode and the command prompt for this mode will appear similar to:

    [<context_name>]hostname(config-ctx-iups-service-rnc)#

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
associate-gtpu-bind-address

This command defines the GTP-U loopback address and associates (binds) this address with a particular interface (non-loopback) address.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] associate-gtpu-bind-address ip_address to-interface-address ip_address

no

Removes the loopback address definition and interface association from the current RNC configuration.
ip_address

ip_address: Must be specified using the standard IPv4 dotted decimal notation.
Usage:

Use this command to setup associations between loopback GTP-U addresses and a non-loopback addresses.

Example

Example
Bind the GTP-U loopback address of 123.1.1.1 to interface address 222.1.1.1:

    associate-gtpu-bind-address
    123.1.1.1  to-interface-address 222.1.1.1

description

This command defines an alphanumeric string that is intended to provide descriptive information about the radio network controller (RNC). This is used for operator reference only.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    description stringno description

no

Removes the description string from the current RNC configuration.
string

Specifies the alphanumeric string that is stored. must be from 1 through 255 alphanumeric characters. Strings with spaces must be enclosed in double-quotes. See the example below.
Usage:

Use this command to set a description for reference by operators.
Example:
The following command sets the description to identify a particular RNC and carrier in Uganda “RNC1 Carrier2 Uganda”:

    description “RNC1
    Carrier2 Uganda”

direct-tunnel

This command enables/disables the direct tunnel feature through the interface to the radio network controller (RNC).
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    direct-tunnel not-permitted-by-rncdefault direct-tunnel

default

Sets the direct tunnel support on RNC to default mode; i.e. enabling direct tunnel.
not-permitted-by-rnc

Default: enabled

Disables the direct-tunnel support on radio network controller (RNC).
Usage:

Use this command to disable/enable the direct-tunnel function through the interface to the RNC.
Example:
Following command disables the direct tunnel support to the RNC:

    direct-tunnel not-permitted-by-rnc

end

Exits the configuration mode and returns to the Exec mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Change the mode to the Exec mode.
exit

Exits the current configuration mode and returns to the IuPS Service configuration mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Return to the previous configuration mode.
lac

This command identifies a Local Area Concentrator (LAC) and a Remote Area Concentrator (RAC) and associates them with this RNC definition.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] lac lac_id rac rac_id

no

Deletes the LAC and RAC information from the system configuration.
lac_id

A unique numeric identifier for the LAC associated with the RNC.

lac_id must be an integer between 1 and 65535.
rac_id

A unique numeric identifier for the RLAC associated with the RNC.

rac_id must be an integer between 1 and 255.
Usage:

Creates an association with a specific LAC and RAC.

Example

Example
Associate LAC 545 and RAC 23 with this RNC:

    lac 545 rac 23

mbms

Configures RNC options for multimedia broadcast multicast service.

IMPORTANT:

This feature and command are currently under development and are not supported.
Platform:

ASR 5000
Product:

SGSN
overload-action disable

This command maps an action to be taken if traffic reaches or exceeds defined levels.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    overload-action disable { activate | attach | auth-challenge | modify-request | paging-downlink-data | ptmsi-reallocation | service-request-data | sms } traffic-level traffic-level [ no | default ] overload-action
    disable { activate | attach | auth-challenge | modify-request | paging-downlink-data | ptmsi-reallocation | service-request-data | sms }

no

Removes the defined overload action from configuration.
default

Resets the traffic level to the default level for the associated overload action.
activate traffic-level traffic-level

The system rejects new requests to activate PDP contexts if the defined traffic-level is exceeded.

traffic-level: An integer 1 to 15.

Default: 14
attach traffic-level traffic-level

The system rejects new requests for GPRS attach if the defined traffic-level is exceeded.

traffic-level: An integer 1 to 15.

Default: 15
auth-challenge traffic-level traffic-level

The system skips performing authentication challenges if the defined traffic-level is exceeded.

traffic-level: An integer 1 to 15.

Default: 4
modify-request traffic-level

The system rejects requests to modify a PDP context if the defined traffic-level is exceeded.

traffic-level: An integer 1 to 15.

Default: 12
paging-downlink-data traffic-level traffic-level

If the defined traffic-level is exceeded, then paging is not performed for data during downlinks if RABs are not available.

traffic-level: An integer 1 to 15.

Default: 11
ptmsi-reallocation traffic-level traffic-level

The system skips performing ptmsi-reallocation if the defined traffic-level is reached or exceeded.

traffic-level: An integer from 1 to 15.

Default: 4
service-request-data traffic-level traffic-level

The system rejects service requests to accept data and establish new RABs if the defined traffic-level is reached or exceeded.

traffic-level: An integer from 1 to 15.

Default: 10
sms traffic-level traffic-level

The system rejects SMS signaling if the defined traffic-level is reached or exceeded.

traffic-level: An integer 1 to 15.

Default: 8
Usage:

This command defines traffic levels and the actions to take if traffic exceeds the defined levels. The command can be re-entered multiple times to create individual definitions for each type of traffic level and action.

Example

Example
Use the following to instruct the system to reject service requests to establish new RABs if the traffic level reaches 3:

    overload-action disable
    service-request-data traffic-level 3

paging-non-searching-indication

This command instructs the SGSN to include the non-searching indicator flag in the page-request message.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    paging-non-searching-indication { non-searching | searching }[ no | default ] paging-non-searching-indication

no | default

This is the default. Entering no or default with this command disables the inclusion of the flag.
non-searching

Set the non-searching-indication to non-searching in the page-request message.
searching

Set the non-searching-indication to searching in the page-request message.
Usage:

Use this command to determine which type of search indicator flag will be included in the page-request message.

Example

Example
Use this command to include the non-searching flag in page-request messages:

    paging-non-searching-indication
    non-searching

pointcode

Configures the point code of the RNC.

The access protocol that is part of the IuPS Service configuration mode must be configured prior to defining the RNC’s point code.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    pointcode pt_code

    no pointcode

no

Deletes the RNC’s point code information from the system configuration.
pt_code
Point code in dotted-decimal format :

- ITU Range 0.0.1 to 7.255.7
- ANSI Range 0.0.1 to 255.255.255
- TTC Range 0.0.1 to 15.31.255
- string of 1 to 11 characters

Usage:

Use this command to identify the point code of the associated RNC.

Example

Example
Identify the pointcode for this RNC as 1.234.2:

    pointcode 1.234.2

pooled

Configure an RNC as either ‘pooled’ or ‘non-pooled’.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    pooled[ default | no ] pooled

default | no

Entering either default or no returns the RNC configuration to the default ‘non-pooled’ state.
Usage:

Each RNC, one-at-a-time, can be identified as ‘pooled’ -- as participating within an SGSN pool -- or ‘non-pooled’. Pooled RNCs can co-exist with non-pooled RNCs.

Example

Example
Identify this RNC as being part of an SGSN pool:

    pooled

rab-asymmetry-indicator

Configures the SGSN to force “Asymmetric-Bidirecitonal” as the RAB Asymmetry Indicator when uplink/downlink bitrates are equal.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    rab-asymmetry-indicator
    symmetric-bidirectional force-asymmetric-bidirectionalno rab-asymmetry-indicator
    symmetric-bidirectional force-asymmetric-bidirectionaldefault rab-asymmetry-indicator

default | no

Disables the override and sets the indicator based on the symmetry of the bitrates as described for the Default Functionality below.
Usage:

This command defines an override that uses “Asymmetric-Bidirecitonal” as the RAB Asymmetry Indicator when uplink/downlink bitrates are equal (default functionality item #1). This overrides the default functionality (see below) for the RAB indicator in the RAB Assignment Request.

As a result of using this override command, two sets of bitrates, one for downlink and one for uplink, will be included in RAB Assignment Requests for establish or modify per 3GPP TS 25.413.

Default Functionality: The SGSN sets the value of the RAB Asymmetry Indicator based on symmetry of negotiated maximum bitrates in the following manner:

- If the uplink and downlink bitrates are equal, then it is set to “Symmetric-Bidirectional”.
- If uplink bitrate is set to 0 kbps, then it is set to “Asymmetric-Unidirectional-Downlink”.
- If downlink bitrate is set to 0 kbps, then it is set to “Asymmetric-Unidirectional-Uplink”.
- If the uplink and downlink bitrates are non-zero and different, then it is set to “Asymmetric-Bidirectional”.

Example

Example
Override the use of the “Symmetric-Bidirectional” RAB Asymmetry Indicator for equal up/downlink bitrates with the following command:

    rab-asymmetry-indicator
    symmetric-bidirectional force-asymmetric-bidirectional

Disable the override with the following command:

    no rab-asymmetry-indicator
    symmetric-bidirectional force-asymmetric-bidirectional

rab-modify-procedure

This command configures how the RAB (radio access bearer) assignment procedure will be modified
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    rab-modify-procedure { normal-modify | release-and-establish }default rab-modify-procedure

default

Returns the configuration to the default setting for this command parameter.
normal-modify

Selects the normal RAB modify procedure.
release-and-establish

Instructs the system to release and establish the RAB procedure.
Usage:

Set the procedure to establish the radio access bearer (RAB).

Example

Example

    rab-modify-procedure
    normal-modify

ranap global-cn-id

This command configures the SGSN to use include the Global Core Network ID IE in the various messages.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ranap global-cn-id { paging-request | relocation-request | reset-procedure | reset-resource-procedure } [ network-sharing
    selected-plmn ][ default | no ] ranap
    global-cn-id { paging-request | relocation-request }

default

Returns the configuration to the default setting and sends the common-plmn in the Global CN ID IE.
no

Disables sending the Global CN ID IE.
paging-request

Instructs the SGSN to send the Global CN ID IE in the Paging Request message.
relocation-request

Instructs the SGSN to send the Global CN ID IE in the Relocation Request message.
reset-procedure

Instructs the SGSN to send the Global CN ID IE in the Reset/Ack message.
reset-resource-procedure

Instructs the SGSN to send the Global CN ID IE in the Reset-Resource/Ack message.
network-sharing selected-plmn

Instructs the SGSN to send the selected-plmn in the Global CN ID IE if network sharing has been enabled.
Usage:

Use this command to configure the SGSN to use ‘selected-plmn’ in the Global Core Network ID IE in various messages when network sharing is enabled.

Example

Example
Use the following command to include the global-cn-id IE in a Paging Request with the common PLMN when network sharing is enabled :

    default ranap global-cn-id
    paging-request

Use the following command to include global-cn-id IE in Relocation Request with the selected-plmn (assumes network sharing has been enabled):

    ranap global-cn-id relocation-request
    network-sharing selected-plmn

ranap paging-area-id

This command configures the SGSN to use include the Paging Area ID IE in the Paging Request message.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ranap paging-area-id
    paging-request [ network-sharing selected-plmn ][ default | no ] ranap
    paging-area-id paging-request [ network-sharing selected-plmn ]

default

Returns the configuration to the default setting and sends the common-plmn in the Paging Area ID IE.
no

Disables sending the Paging Area ID IE.
paging-request

Instructs the SGSN to send the Paging Area ID IE in the Paging Request message.
network-sharing selected-plmn

Instructs the SGSN to send the selected-plmn in the Paging Area ID IE if network sharing has been enabled.
Usage:

Use this command to configure the SGSN to use ‘selected-plmn’ in the Paging Area ID IE in the Paging Request message when network sharing is enabled.

Example

Example
Use the following command to include the paging-area-id IE in a Paging Request with the common PLMN when network sharing is enabled :

    default ranap paging-area-id
    paging-request

Use the following command to include global-cn-id IE in Paging Request with the selected-plmn (assumes network sharing has been enabled):

    ranap global-cn-id paging-request
    network-sharing selected-plmn

ranap paging-cause-ie

This command sets the paging cause value and either includes or suppresses the Paging Cause IE in responses to Paging Requests due to various sources. This command is available in releases 8.1 and higher.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ranap { paging-cause-ie { all | background-data [ value ] | conversational-data
     [ value ] | gmm-signalling
     [ value ] | gs-signalling
     [ value ] | interactive-data
     [ value ] | sm-signalling
     [ value ] | sms-signalling
     [ value ] | streaming-data
     [ value ] }[ default | no ] ranap { paging-cause-ie { all | background-data
     | conversational-data  | gmm-signalling  | gs-signalling
     | interactive-data  | sm-signalling  | sms-signalling
     | streaming-data  }

default

Resets the specific parameters value to default.
no

Suppresses the Paging Cause IE so that it is not included in responses to Paging Requests from respective sources.
all

Using all sets the action for the Paging Cause IE value for all paging due to all sources.
background-data [ value ]

Default: 3 (terminating background call)

Set the Paging Cause IE value for paging due to background data.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
conversational-data [ value ]

Default: 5 (terminating high priority signaling)

Set the Paging Cause IE value for paging due to conversational data.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
gmm-signalling [ value ]

Default: 5 (terminating high priority signaling)

Set the Paging Cause IE value for paging due to gmm-signaling.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
gs-signalling [ value ]

Default: 5 (terminating high priority signaling)

Set the Paging Cause IE value for paging due to VLR Paging Request.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
interactive-data [ value ]

Default: 2 (terminating interactive call)

Set the Paging Cause IE value for paging due to interactive data.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
sm-signalling [ value ]

Default: 5 (terminating high priority signaling)

Set the Paging Cause IE value for paging due to SM signaling.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
sms-signalling [ value ]

Default: 4 (terminating low priority signaling)

Set the Paging Cause IE value for paging due to SMS signaling.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
streaming-data [ value ]

Default: 5 (terminating high priority signaling)

Set the Paging Cause IE value for paging due to streaming data.

value : Must be an integer from 0 to 5. See Paging Cause value mapping in Usage section.
Usage:

This command can be used to set the value (meaning) of the Paging Cause IE included in responses to Paging Requests or it can be used to suppress the inclusion of the Paging Cause IE in the responses. These actions can be configured for paging for all sources or for a specified source.
The following values are applicable to all Paging Cause IEs:

- 0 - Terminating conversational call
- 1 - Terminating streaming call
- 2 - Terminating interactive call
- 3 - Terminating background call
- 4 - Terminating low priority signaling
- 5 - Terminating high priority signaling

Example

Example
Use the following command to set Paging Cause value to 3 for paging due to GMM signaling without affecting cause values for other sources:

    ranap paging-cause-ie
    gmm-signalling 3

Use the following command to suppress the Paging Cause IE from all Paging Requests to the RNC:

    no ranap paging-cause-ie all

Either of the following commands will cause the Paging Cause IE to be included in Paging Requests with the default value for SM signaling without affecting the cause for other sources:

    ranap paging-cause-ie
    sm-signalling

    default ranap paging-cause-ie
    sm-signalling

ranap signalling-indication-ie

This command enables/disables the inclusion of the Signaling Indication IE in either or both the RAB Assignment Request and/or the Relocation Request RANAP messages.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    ranap signalling-indication-ie { rab-assignment-request [ relocation-request ] | relocation-request [ rab-assignment-request ] }

    no ranap signalling-indication-ie

    default ranap signalling-indication-ie

no

Sets the configuration so that the SGSN never includes the IE.
default

Resets the configuration to the default - the SGSN includes the IE in the messages if preconditions are met (see Usage section).
rab-assignment-request | relocation-request

Including one or both of these keywords configures what type of RANAP message will include the IE.
Usage:

The command enables the operator to determine whether the signalling indication information element is included in either or both the RAB Assignment Request and Relocation Request messages during the PDP context setup procedure.
For this command configuration to work so that the IE is included, two preconditions must be met:

- Received QoS traffic class for the context must be interactive
- Received QoS has a signalling indication value as optimized

When an RNC receives this IE, the RNC assumes that the customer is using IMS signaling and allocates massive amounts of bandwidth, potentially causing cell congestion. This command enables the operator to determine the usage of this IE which provides the operator with additional session management control.

Example

Example
Use the following command to include the signalling indication IE in the RAB Assignment Request:

    ranap signalling-indication-ie rab-assignment-request

release-compliance

This command allows the SGSN to set support based on the RNC’s 3GPP release compliance and to define per RNC QoS overrides.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    release-compliance { pre-release-7 | release-7 } [ gbr-down gbr_dn_val | gbr-up gbr_up_val | mbr-down mbr_dn_val | mbr-up mbr_up_val ] + default release-compliance

default

Returns the configuration to the default value, release-7.
pre-release-7

Enables support for an RNC with capabilities compliant with releases prior to Release 7, such as HSPA in R6.
release-7

Enables support for RNC with capabilities compliant with 3GPP Release 7 or later, such as HSPA+ available in R7.
gbr-down gbr_dn_val
Defines a guaranteed kbps bit rate for downlink direction,

- options for pre-release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000. Default cap is 16000.
- options for release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000, 21000, 28000, 42000. See default cap information below.

gbr-up gbr_up_val
Defines a guaranteed kbps bit rate for uplink direction,

- options for pre-release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000. Default cap is 16000.
- options for release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000, 21000, 28000, 42000. See default cap information below.

mbr-down mbr_dn_val
Defines a maximum kbps bit rate for downlink direction,

- options for pre-release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000. Default cap is 16000.
- options for release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000, 21000, 28000, 42000. See default cap information below.

mbr-up mbr_up_val
Defines a maximum kbps bit rate for uplink direction,

- options for pre-release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000. Default cap is 16000.
- options for release-7 include: 16, 32, 64, 128, 256, 512, 1024, 2048, 4096, 8192, 11500, 16000, 21000, 28000, 42000. See default cap information below.

Usage:

Use this command to match the 3GPP release support by the RNC. As the 3GPP releases each support differing data rate options - R6 supports HSPA and R7 supports HSPA+ - then selecting the compliance is a method of preforming data rate management on a per RNC basis.

Also use this command to set QoS capping overrides for each RNC separately. Default caps for Release 7 RNC will vary depending upon which overrides are set.

IMPORTANT:

Once caps are set for an RNC, if the RNC release level changes the capping remains the same until the QoS override values are changed for that RNC. Values do not automatically change to the default values appropriate for that release .

Example

Example
Enable HSPA fallback to R6 compliance:

    release-compliance pre-release-7

reset-resource

This command enables the operator to control message length by configuring the number of IuConIDs sent in each RANAP Reset Resource messages.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    reset-resource max-iuconid-per-msg numberdefault reset-resource
    max-iuconid-per-msg

default

Resets the number of Iu connection Ids included in the Reset Resource messages. Default is 250.
max-iuconid-per-msg number

Sets the number of Iu connection Ids to be included in the Reset Resource messages.

number: Integer from 1 to 250.

Default: 250
Usage:

Id numbers for each Iu connection are included in the RANAP Reset Resource messages. Including this potentially long stream of numbers can make the message very long. With this command, the operator can control the size of the messages by controlling the number of Id messages included in the messages.

Example

Example
Limit the number of Iu connection IDs to 30:

    reset-resource max-iuconid-per-msg 30