# show sgsn-service

This chapter describes the output of the show sgsn-service command.

show sgsn-service all

Table 1. show sgsn-service all Command Output Descriptions

Field | Description
--- | ---
Service name | The SGSN service that is running in this session.
Context | The name of the context in which SGSN service is running.
Status | Status of the SGSN service.
Accounting Context Name | The name of the context in which accounting interface is configured for this SGSN service.
SGSN Number | The number of SGSN system in current network.
Network-sharing | Specifies whether network sharing is enabled or disabled.
Nri bits | Specifies whether network resource identifier (NRI) bit is configured or not in this SGSN service.
SGTP Context | The name of the context in which SGTP service is running.
SGTP Service | The SGTP service that is running the SGTP session in this SGSN service.
MAP Context | The name of the context in which mobile application part (MAP) service, configured in this SGSN service, is running.
MAP Service | The service that is running the MAP session in this SGSN service.
IuPS Context | The name of the context in which UMTS Packet Switch Iu interface (IuPS) service is running.
IuPS Service | The service that is running the IuPS session.
SM-T3385 Timeout | The time-out duration in seconds for GPRS session management timer - T3385 on network side for PDP context activation.
SM-T3386 Timeout | The time-out duration in seconds for GPRS session management timer - T3386 on network side for PDP context modification.
SM-T3395 Timeout | The time-out duration in seconds for GPRS session management timer - T3395 on network side for PDP context deactivation.
SM-Max Activate Retries | Total number of retries for PDP context activation from GPRS session manager.
SM-Max Modify Retries | Total number of retries for PDP context modification from GPRS session manager.
SM-Max Deactivate Retries | Total number of retries for PDP context deactivation from GPRS session manager.
GMM-T3302 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3302 on MS side for GPRS attach procedure or RAU procedure.
GMM-T3322 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3322 on network side for GPRS detach request procedure.
GMM-T3350 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3350 on network side GPRS attach accept/RAU accept/REALLOC request procedure sent with P-TMSI and/or TMSI.
GMM-Mobil-Reachable Timeout | The time-out duration in seconds for GPRS mobility management timer - Mobile Reachable on network side.
GMM-Implicit-Detach Timeout | The time-out duration in seconds for GPRS mobility management timer - Implicit-Detach on network side.
GMM-Purge Timeout | The time-out duration in seconds for GPRS mobility management timer - Purge to hold the detach of MM context on network side.
GMM-T3313 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3313 on network side for paging procedure initiation.
GMM-Max Page Retries | Maximum number of retries for paging procedure from GPRS mobility manager.
GMM-T3312 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3313 on network side for RAU procedure initiation.
GMM-T3370 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3370 on network side for identity request procedure.
GMM-Max Identity Retries | Maximum number of retries for identity request procedure from GPRS mobility manager.
GMM-T3360 Timeout | The time-out duration in seconds for GPRS mobility management timer - T3360 on network side for Authentication and Cipher request procedure.
GMM-Max Auth Retries | Maximum number of retries for authentication request procedure from GPRS mobility manager.
GMM-Max PTMSI RELOC Retries | Maximum number of retries for Packet-Temporary Mobile Subscriber Identity (P-TMSI) relocation procedure from GPRS mobility manager.
GMM-Perform-Identity-After-Auth | Specifies whether “perform identity after authentication” procedure is enabled or not.
Max simultaneous pdp contexts per MS | Maximum number of simultaneous PDP context allowed on one MS.
SUPER CHARGER | Specifies whether “super charger” feature is enabled or not.
Accounting cdr-types | Specifies type of accounting CDRs configured in this SGSN service.
Charging Characteristics (CC) Profiles | This group provides the charging characteristics profiles configured in this SGSN service.
Profile | Specifies the charging characteristic profile configured in this SGSN service
Bucket | Specifies the charging bucket configured for charging characteristic in this SGSN service
Inform RNC before UE during QOS Modification | Specifies if operator has enabled or disabled the SGSN functionality to inform RNC before UE during QoS modification.