# show aaa group name

Table 1. show aaa group name Command Output Descriptions

Field | Description
--- | ---
Group name | The AAA server group name.
Context | The context name.
Diameter config:
Authentication:
Dictionary | The Diameter dictionary used for authentication.
Endpoint name | The Diameter endpoint used for authentication.
Max-transmissions | The maximum number of transmission attempts for Diameter authentication.
Max-retries | The number of retry attempts for Diameter authentication requests.
Request-timeout | The Diameter authentication request timeout period.
Redirect-host-avp | Indicates whether to use just one returned AVP, or use the first returned AVP as selecting the primary host and the second returned AVP as selecting the secondary host.
Accounting:
Dictionary | The Diameter dictionary used for accounting.
Endpoint name | The Diameter endpoint used for accounting.
Max-transmissions | The maximum number of transmission attempts for Diameter accounting.
Max-retries | The number of retry attempts for Diameter accounting requests.
Request-timeout | The Diameter accounting request timeout period.
Radius Config:
Dictionary | The RADIUS dictionary.
Strip-domain | Indicates whether the domain is stripped from the user name prior to authentication or accounting.
Authenticator-validation | Indicates whether the MD5 authentication of RADIUS user is enabled.
Allow authentication-down | Indicates whether the system allows subscriber sessions when RADIUS authentication is unavailable.
Allow accounting-down | Indicates whether the system allows subscriber sessions when RADIUS accounting is unavailable.
Attributes:
Nas-identifier | The attribute name by which the system is identified in Access-Request messages.
Nas-ip | The AAA interface IP address(es) used to identify the system.
Nas-ip backup | The IP address of the secondary interface to use in the current context.
Nexthop | The next hop IP address for this NAS IP address.
MPLS-label | Indicates the MPLS label used for traffic from the specified RADIUS client NAS IP address.
VRF | The Virtual Routing and Forwarding (VRF) Context instance associated with this AAA group.
Authentication
called-station-id | Indicates whether RADIUS authentication attribute for called station id is enabled. The attribute must also be supported in the configured RADIUS dictionary.
calling-station-id | Indicates whether RADIUS authentication attribute for calling station id is enabled. The attribute must also be supported in the configured RADIUS dictionary.
imsi | Indicates whether RADIUS authentication attribute for IMSI is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-pdp-type | Indicates whether RADIUS authentication attribute for 3GPP PDP type is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-cg-address | Indicates whether RADIUS authentication attribute for 3GPP CG address is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-gprs-qos-negotiated-profile | Indicates whether RADIUS authentication attribute for 3GPP GPRS QoS negotiated profile is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-sgsn-address | Indicates whether RADIUS authentication attribute for 3GPP SGSN address is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-ggsn-address | Indicates whether RADIUS authentication attribute for 3GPP GGSN address is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-imsi-mcc-mnc | Indicates whether RADIUS authentication attribute for 3GPP IMSI MCC MNC is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-ggsn-mcc-mnc | Indicates whether RADIUS authentication attribute for 3GPP GGSN MCC MNC is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-nsapi | Indicates whether RADIUS authentication attribute for 3GPP NSAPI is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-select-mode | Indicates whether RADIUS authentication attribute for 3GPP select mode is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-charging-characteristics | Indicates whether RADIUS authentication attribute for 3GPP charging characteristics is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-sgsn-mcc-mnc | Indicates whether RADIUS authentication attribute for 3GPP SGSN MCC MNC is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-imeisv | Indicates whether RADIUS authentication attribute for 3GPP imeisv is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-rat-type | Indicates whether RADIUS authentication attribute for 3GPP RAT type is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-user-location-info | Indicates whether RADIUS authentication attribute for 3GPP user location information is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-ms-timezone | Indicates whether RADIUS authentication attribute for 3GPP ms timezone is enabled. The attribute must also be supported in the configured RADIUS dictionary.
Accounting
called-station-id | Indicates whether RADIUS accounting attribute for called station id is enabled. The attribute must also be supported in the configured RADIUS dictionary.
calling-station-id | Indicates whether RADIUS accounting attribute for calling station id is enabled. The attribute must also be supported in the configured RADIUS dictionary.
acct-input-octets | Indicates whether RADIUS accounting attribute for accounting input octets is enabled. The attribute must also be supported in the configured RADIUS dictionary.
acct-input-packets | Indicates whether RADIUS accounting attribute for accounting input packets is enabled. The attribute must also be supported in the configured RADIUS dictionary.
acct-session-time | Indicates whether RADIUS accounting attribute for accounting session time is enabled. The attribute must also be supported in the configured RADIUS dictionary.
acct-output-octets | Indicates whether RADIUS accounting attribute for accounting output octets is enabled. The attribute must also be supported in the configured RADIUS dictionary.
acct-output-packets | Indicates whether RADIUS accounting attribute for accounting output packets is enabled. The attribute must also be supported in the configured RADIUS dictionary.
event-timestamp | Indicates whether RADIUS accounting attribute for event timestamp is enabled. The attribute must also be supported in the configured RADIUS dictionary.
imsi | Indicates whether RADIUS accounting attribute for IMSI is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-charging-id | Indicates whether RADIUS accounting attribute for 3GPP charging ID is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-pdp-type | Indicates whether RADIUS accounting attribute for 3GPP PDP type is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-cg-address | Indicates whether RADIUS accounting attribute for 3GPP CG address is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-gprs-qos-negotiated-profile | Indicates whether RADIUS accounting attribute for 3GPP GPRS QoS negotiated profile is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-sgsn-address | Indicates whether RADIUS accounting attribute for 3GPP SGSN address is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-ggsn-address | Indicates whether RADIUS accounting attribute for 3GPP GGSN address is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-imsi-mcc-mnc | Indicates whether RADIUS accounting attribute for 3GPP IMSI MCC MNC is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-ggsn-mcc-mnc | Indicates whether RADIUS accounting attribute for 3GPP GGSN MCC MNC is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-nsapi | Indicates whether RADIUS accounting attribute for 3GPP NSAPI is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-select-mode | Indicates whether RADIUS accounting attribute for 3GPP select mode is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-charging-characteristics | Indicates whether RADIUS accounting attribute for 3GPP charging characteristics is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-sgsn-mcc-mnc | Indicates whether RADIUS accounting attribute for 3GPP SGSN MCC MNC is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-imeisv | Indicates whether RADIUS accounting attribute for 3GPP imeisv is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-rat-type | Indicates whether RADIUS accounting attribute for 3GPP RAT type is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-user-location-info | Indicates whether RADIUS accounting attribute for 3GPP user location information is enabled. The attribute must also be supported in the configured RADIUS dictionary.
3gpp-ms-timezone | Indicates whether RADIUS accounting attribute for 3GPP ms timezone is enabled. The attribute must also be supported in the configured RADIUS dictionary.
Authentication:
Algorithm | The RADIUS authentication server selection algorithm for the current context.
Deadtime | The time period to wait before changing the state of a RADIUS server from “Down” to “Active”, in minutes.
Max-outstanding | The maximum number of messages a AAA manager will queue.
Max-retries | The maximum number of times communication with a AAA server is attempted before it is marked as “Not Responding” and the detect dead server’s consecutive failures count is incremented.
Max-transmissions | The maximum number of re-transmissions for RADIUS authentication requests.
Timeout | The time period to wait for a response from the RADIUS server before re-sending the messages, in seconds.
Apn-to-be-included | The APN name included for RADIUS authentication.
Authenticate null-username | Indicates whether authentication of user names that are blank or empty is enabled.
Probe:
Interval | The time period between two RADIUS authentication probes.
Timeout | The timeout period for HAGR to wait for a response for RADIUS authentication probes.
Max-retries | The maximum number of retries for RADIUS authentication probe response.
Keepalive:
Interval | The time period between two keepalive access requests.
Timeout | The time period between two keepalive access request retries.
Retries | The number of times the keepalive access request is sent before marking the server as unreachable.
consecutive-response | The number of consecutive authentication responses after which the server is marked as reachable.
Username | The user name used for authentication.
Calling-station-id | The calling station ID used for keepalive authentication.
Password | The password used for authentication.
Allow access-reject | Indicates whether both access-accept and access-reject are considered as success for the keepalive authentication request.
Detect-dead-server:
Consecutive-failures | The number of consecutive failures, for any AAA manager, before a server’s state is changed from “Active” to “Down”.
Response-timeout | The time period for any AAA manager to wait for a response to any message before a server’s state is changed from “Active” to “Down”, in seconds.
Keepalive | Indicates whether the AAA server alive-dead detect mechanism based on sending keepalive authentication messages to all authentication servers is enabled.
Accounting:
Algorithm | The RADIUS accounting server selection algorithm for the current context.
Deadtime | The time period to wait before changing the state of a RADIUS server from “Down” to “Active”, in minutes.
Fire-And-Forget | Displays whether or not the Fire-and-Forget feature is enabled in the AAA Group configuration.
Max-outstanding | The maximum number of messages a AAA manager will queue.
Max-retries | The maximum number of times communication with a AAA server will be attempted before it is marked as “Not Responding” and the detect dead server’s consecutive failures count is incremented.
Max-transmissions | The maximum number of re-transmissions for RADIUS accounting requests.
Max-pdu-size | The maximum sized packet data unit which can be accepted/generated, in bytes.
Interim-timeout | The timeout period for sending accounting INTERIM-UPDATE records, in seconds.
Interim-downlink-volume | The downlink volume limit that triggers RADIUS interim accounting, in bytes.
Interim-uplink-volume | The uplink volume limit that triggers RADIUS interim accounting, in bytes.
Interim-total-volume | The total volume limit for RADIUS interim accounting, in bytes.
Timeout | The time period to wait for a response from a RADIUS server before retransmitting a request.
Remote-address | Indicates whether remote IP address lists are configured, and collection of accounting data for the addresses in those lists on a per-subscriber basis is enabled.
Archive | Indicates whether archiving of RADIUS Accounting messages in the system after the accounting message has exhausted retries to all available RADIUS Accounting servers is enabled.
Apn-to-be-included | The APN name included for RADIUS accounting.
R-P originated:
Trigger active-start | Indicates whether when an Active-Start is received from the PCF and there has been a parameter change, an R-P event occurs.
Trigger active-handoff | Indicates whether when an Active PCF-to-PFC Handoff occurs, a single or two R-P events will occur (one for the Connection Setup, and the second for the Active-Start).
Trigger active-stop | Indicates whether when an Active-Stop is received from the PCF, an R-P event occurs.
Trigger policy | the overall accounting policy for R-P sessions.
Trigger stop-start | Indicates whether a stop/start RADIUS accounting pair is sent to the RADIUS server when an applicable R-P event occurs.
Handoff policy | The overall accounting policy for R-P sessions.
TOD | The time of day a RADIUS event is generated for accounting.
GTP originated:
Trigger policy | The RADIUS accounting policy for GTP.
MIP HA:
Policy | The RADIUS accounting policy for Mobile IP HA calls.
Keepalive:
Interval | The time period between the two keepalive access requests.
Timeout | The time period between each keepalive access request retries.
Retries | The number of times the keepalive access request is sent before marking the server as unreachable.
consecutive-response | The number of consecutive authentication response after which the server is marked as reachable.
Username | The user name used for authentication.
Calling-station-id | The calling station ID used for keepalive authentication.
Framed-ip-address | The framed-ip-address used for keepalive accounting.
Detect-dead-server:
Consecutive-failures | The number of consecutive failures, for any AAA manager, before a server’s state is changed from “Active” to “Down”.
Response-timeout | The time period for any AAA manager to wait for a response to any message before a server’s state is changed from “Active” to “Down”, in seconds.
Keepalive | Indicates whether the AAA server alive-dead detect mechanism based on sending keepalive authentication messages to all authentication servers is enabled.
Charging:
Auth-algorithm | The RADIUS authentication algorithm.
Acct-algorithm | The RADIUS accounting algorithm.
Deadtime | The time period to wait before changing the state of a RADIUS server from “Down” to “Active”, in minutes.
Max-outstanding | The maximum number of messages a AAA manager will queue.
Max-retries | The maximum number of times communication with a AAA server will be attempted before it is marked as “Not Responding” and the detect dead server’s consecutive failures count is incremented.
Max-transmissions | The maximum number of re-transmissions for RADIUS requests.
Timeout | The time period to wait for a response from a RADIUS server before retransmitting a request.
Detect-dead-server:
Consecutive-failures | The number of consecutive failures, for any AAA manager, before a server’s state is changed from “Active” to “Down”.
Response-timeout | The time period for any AAA manager to wait for a response to any message before a server’s state is changed from “Active” to “Down”, in seconds.