# QCI - RAN ID Mapping Configuration Mode Commands

The QoS Class Index (QCI) Mapping Configuration Mode is used to map RAN profile IDs to QoS Class Indexes via the HRPD Serving Gateway (HSGW) in an eHRPD network.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current mode and returns to the Exec Mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the current mode and returns to the previous mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Return to the previous mode.
profile-id

Maps a QCI ID to a RAN profile ID and modifies data flow bit rate ranges.
Platform:

ASR 5000
Product:

HSGW
Privilege:

Administrator
Syntax

    profile-id id qci num [ uplink { gbr rate [ mbr rate ] |
    mbr rate [ gbr rate ] } downlink { gbr rate [ mbr rate ] |
    mbr rate [ gbr rate ] ]no profile-id id

no

Removes the specified profile ID entry from this map.
id

Specifies the profile ID to which a QCI ID will be mapped. id must be an integer value from 1 to 65535.
qci num

Specifies the QCI number to which the profile ID will be mapped. num must be an integer value from 1 to 255.
uplink

Specifies that the guaranteed bit rate (GBR) and/or maximum bite rate (MBR) setting that follow this keyword will be applied to the uplink data flow.
downlink

Specifies that the guaranteed bit rate (GBR) and/or maximum bite rate (MBR) settings that follow this keyword will be applied to the downlink data flow.
gbr rate

Specifies the guaranteed bit rate for the uplink or downlink data flow. rate must be an integer value from 0 to 4294967295.
mbr rate

Specifies the maximum bit rate for the uplink or downlink data flow. rate must be an integer value from 0 to 4294967295.
Usage:

Use this command to map a QCI ID to a RAN profile ID and, optionally, modify data flow bit rate ranges.
Example:
The following command maps a QCI ID (1) to a profile ID (10) and sets the uplink guaranteed bite rate to 10000 and the downlink guaranteed bit rate to 20000:

    profile-id 10 qci 1
    uplink gbr 10000 downlink gbr 20000