# HNBGW-RTP Schema Statistics

The HNBGW-RTP schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HNB-GW.
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the HNBGW-RTP Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context in which HNB-GW service is configured. This is a key variable. | String
vpnid | The identity number of the context in which HNB-GW service is configured. This is a key variable. | String
servname | The name of the HNB-GW service for which statistics are collected. This is a key variable. | String
rtp-uplink-pkts-rx | Indicates the total number of RTP Uplink Packets received. Trigger: When RTP Uplink Packets are received by HNB-GW. Availability: Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-pkts-good-rx | Indicates the total number of RTP Uplink Packets (good) received. Trigger: When RTP Uplink Packets(good) are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-byts-rx | Indicates the total number of RTP Uplink Bytes received. Trigger: When RTP Uplink Bytes are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-pkts-dropped | Indicates the total number of RTP Uplink Packets dropped. Trigger: When RTP Uplink Packets are dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-pkts-drop-rab_not-in_conn_state | Indicates the total number of RTP Uplink Packets dropped with cause RAB not in CONNETED state. Trigger: When RTP Uplink Packets are dropped by HNB-GW with cause RAB not in CONNETED state. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-pkts-dropped-misc | Indicates the total number of RTP Uplink Packets dropped with cause Miscellaneous. Trigger: When RTP Uplink Packets are dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-byts-dropped | Indicates the total number of RTP Uplink Bytes dropped. Trigger: When RTP Uplink Bytes are dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-byts-drop-rab_not-in_conn_state | Indicates the total number of RTP Uplink Bytes dropped with cause RAB not in CONNETED state. Trigger: When RTP Uplink Bytes are dropped with cause RAB not in CONNETED state. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-uplink-byts-dropped-misc | Indicates the total number of RTP Uplink Bytes dropped with cause Miscellaneous. Trigger: When RTP Uplink Bytes are dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-downlink-pkts-tx | Indicates the total number of RTP Downlink Packets transmitted. Trigger: When RTP Downlink Packets are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-downlink-byts-tx | Indicates the total number of RTP Downlink Bytes transmitted. Trigger: When RTP Downlink Bytes are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-receiver-report-rx | Indicates the total number of RTCP Receiver Report received (From HNB). When RTCP Receiver Report are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-receiver-report-tx | Indicates the total number of RTCP Receiver Report transmitted (To HNB). When RTCP Receiver Report are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-sender-report-rx | Indicates the total number of RTCP Sender Report received (From HNB). When RTCP Sender Report are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-sender-report-tx | Indicates the total number of RTCP Sender Report transmitted (To HNB). When RTCP Sender Report are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-sdes-report-rx | Indicates the total number of RTCP SDES Report received. When RTCP SDES Report are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-sdes-report-tx | Indicates the total number of RTCP SDES Report transmitted. When RTCP SDES Report are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-bye-report-rx | Indicates the total number of RTCP BYE Report received. When RTCP BYE Report are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-app-report-rx | Indicates the total number of RTCP APP Report received. When RTCP APP Report are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-pkts-rx | Indicates the total number of RTCP Uplink Packets received. When RTCP Uplink Packets are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-byts-rx | Indicates the total number of RTCP Uplink Bytes received. When RTCP Uplink Bytes are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-pkts-dropped | Indicates the total number of RTCP Uplink Packets dropped. When RTCP Uplink Packets are dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-pkts-drop-rab_not-in_conn_state | Indicates the total number of RTCP Uplink Packets dropped with cause RAB not in CONNETED state. When RTCP Uplink Packets are dropped by HNB-GW with cause RAB not in CONNETED state. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-pkts-dropped-misc | Indicates the total number of RTCP Uplink Packets dropped with cause Miscellaneous. When RTCP Uplink Packets are dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-byts-dropped | Indicates the total number of RTCP Uplink Bytes dropped. When RTCP Uplink Bytes are dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-byts-drop-rab_not-in_conn_state | Indicates the total number of RTCP Uplink Bytes dropped with cause RAB not in CONNETED state. When RTCP Uplink Bytes are dropped by HNB-GW with cause RAB not in CONNETED state. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-uplink-byts-dropped-misc | Indicates the total number of RTCP Uplink Bytes dropped with cause Miscellaneous. When RTCP Uplink Bytes are dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-downlink-pkts-tx | Indicates the total number of RTCP Downlink Packets transmitted. When RTCP Downlink Packets are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtcp-downlink-byts-tx | Indicates the total number of RTCP Downlink Bytes transmitted. When RTCP Downlink Bytes are transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-uplink-pkts-rx | Indicates the total number of RTP-MUX Uplink Packets received. Trigger: When RTP-MUX Uplink Packets are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-uplink-byts-rx | Indicates the total number of RTP-MUX Uplink Bytes received. Trigger: When RTP-MUX Uplink Bytes are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-uplink-pkts-dropped | Indicates the total number of RTP-MUX Uplink Packets dropped. Trigger: When RTP-MUX Uplink Packets are dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-uplink-pkts-dropped-misc | Indicates the total number of RTP-MUX Uplink Packets dropped with cause Miscellaneous. Trigger: When RTP-MUX Uplink Packets are dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-uplink-byts-dropped | Indicates the total number of RTP-MUX Uplink Bytes dropped. Trigger: When RTP-MUX Uplink Bytes are dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-uplink-byts-dropped-misc | Indicates the total number of RTP-MUX Uplink Bytes dropped with cause Miscellaneous. Trigger: When RTP-MUX Uplink Bytes are dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-rtp-stream-rcvd | Indicates the total number of RTP-MUX RTP Stream received. Trigger: When RTP-MUX RTP Stream are received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-rtp-stream-dropped | Indicates the total number of RTP-MUX RTP Stream Dropped. Trigger: When RTP-MUX RTP Stream are Dropped by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
rtp-mux-rtp-stream-dropped-misc | Indicates the total number of RTP-MUX RTP Stream Dropped with cause Miscellaneous. Trigger: When RTP-MUX RTP Stream are Dropped by HNB-GW with cause Miscellaneous. Availability: Across all HNB-GW Services | Unsigned Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.