# MIP HA Assignment Table Configuration Mode Commands

The Mobile IP HA Assignment Table Configuration Mode is used to assign specific Home Agent (HA) IP addresses to ranges of Mobile Node (MN) IP addresses.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
hoa-range

This command assigns ranges of Mobile Node (MN) IP addresses to specific Home agent IP addresses.
Platform:

ASR 5000
Product:

HA
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] hoa-range ip_addressip_address2 ha ip_address3

no

Removes the specified Home Agent assignment from the assignment table.
ip_address ip_address2

Specifies a range of MN IP addresses. ip_address and ip_address2 must be specified in IPv4 dotted-decimal or IPv6 colon-separated notation.
ha ip_address3

Specifies the IP address of the Home Agent to assign to MNs that are within the specified range. ip_address3 must be specified in IPv4 dotted-decimal or IPv6 colon-separated notation.
Usage:

Use this command to assign ranges of MN IP addresses to specific HAs.

IMPORTANT:

A maximum of eight MIP HA assignment tables can be configured per context with a maximum of eight MIP HA assignment tables across all contexts.

IMPORTANT:

A maximum of 256 non-overlapping hoa-ranges can be configured per MIP HA Assignment table with a maximum of 256 non-overlapping hoa-ranges across all MIP HA Assignment tables.
Example:
The following command assigns any MN IP address that falls in the range of 192.168.100.0 through 192.168.101.0 to the HA with the IP address of 192.168.200.10:

    hoa-range 192.168.100.0
    192.168.101.0 ha 192.168.200.10