# MAP Service Configuration Mode Commands

The MAP Service Configuration Mode is used to configure properties for Mobile Application Part (MAP) service.

Mobile Application Part (MAP) is a protocol which provides an application layer for the various nodes in the core mobile network and GPRS and UMTS core network to communicate with each other in order to provide services to mobile phone users. The MAP service provides the application-layer protocol support used to access the Home Location Register (HLR).

    [<context_name>]hostname(config-map-service-<svc_name>)#

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
access-protocol

Configures access protocol parameters for the MAP service as defined for a specific SCCP network instance.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    access-protocol sccp-network sccp_id ssn   subsys_num no access-protocol
    sccp-network sccp_id ssn   subsys_num

sccp-network sccp_id

Specifies the ID number of the SCCP network to use for the SGSN connection.

sccp_id : Must be an integer from 1 to 16.
ssn subsys_num

Identifies the subsystem number for the destination.

subsys_num: Enter an integer from 1 through 255.
no

Removes the access protocol SCCP network instance ID from the configuration.
Usage:

Use this command to associate access protocol parameters to a specific instance of the MAP service for an SCCP network.
Example:
The following command associates the access protocols with the SCCP network ID #10:

    access-protocol sccp-network 10

application-context-name

Configure the operation timer(s) for one or more MAP application contexts.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    application-context-name application operation-timer value

    default application-context-name application operation-timer

default

Resets the operation timers for all applications to system defaults.
application
Select one of the following applications to enable the application:

- authentication-failure-report : Sets the reporting operation timer for authentication failure. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- cancel-location : Sets the cancel location operation timer. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- check-imei : Sets the check-IMEI operation timer. The setting range for this timer is 15 to 30 seconds for releases 8.0 and 8.1 and 1 to 30 seconds for releases 9.0 and higher. The default setting is 15 seconds.
- delete-subscriber-data : Sets the delete subscriber data operation timer. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- mo-fwd-sm : Sets the operation timer for fowarding mobile-originated SMS. The setting range for this timer is 1 to 10 minutes and the default setting is 1 minute (60 seconds).
- ms-purge : Sets the operation timer for MS-purge function. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- mt-fwd-sm : Sets the operation timer for fowarding mobile-terminated SMS. The setting range for this timer is 1 to 10 minutes and the default setting is 1 minute (60 seconds).
- ready-for-sm : Sets the operation timer for the ready for SMS operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- send-authentication-info : Sets the operation timer for the sending authentication information operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- stand-alone-insert-subscriber-data : Sets the operation timer for the standalone insert subscriber data operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- ugl-insert-subscriber-data : Sets the operation timer for the insert subscriber data portion of the update GPRS location operation. TThe setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.
- update-gprs-location : Sets the operation timer for the update GPRS location operation. The setting range for this timer is 15 to 30 seconds and the default setting is 15 seconds.

operation-timervalue

Configures the operation timer for the selected application. Timer values are indicated above.
Usage:

Repeat this command entering a different application each time to enable multiple applications.
Example:

    application-context-name  stand-alone-insert-subscriber-data
    operation-timer operation-timer 20

auth-vectors

Configures the number of authorization vectors to be requested from the home location register (HLR) during call setup to provide subscriber authentication.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    auth-vectors number-to-request numberdefault auth-vectors
    number-to-request

default

Resets the number of vectors requested from the HLR to the system default.
number-to-request number

number: Must be an integer from 1 to 5 to define the number of authorization vectors be requested from the HLR.

Default is 5.
Usage:

Set the number of requests to be received from the HLR.
Example:

    auth-vectors number-to-request 4

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
equipment-identity-register

Defines the information relevant to the equipment-identity-register (EIR) used by the SGSN.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    equipment-identity-register { isdn  E.164_num | point
    code pt_code } [ source-ssn ssn| check-imei-every-n-eventstimes]no equipment-identity-register { isdn E.164_num |  point codept_code }

no

Deletes the EIR configuration.
isdn number

Enter the E.164 number of the EIR.

number: must be a string of 1 to 15 digits.
point code pt_code
Enter SS7 point code address of the EIR in dotted-decimal format according to variant settings:

- ITU Range 0.0.1 to 7.255.7
- ANSI Range 0.0.1 to 255.255.255
- TTC Range 0.0.1 to 15.31.255
- or a string of 1 to 11 characters

source-ssn ssn

Identifies the subsystem number (SSN) to be used.

ssn must be an integer from 1 to 255.
check-imei-every-n-events times

Configures the frequency with which a ‘check IMEI’ message is sent to the EIR. When set, the SGSN skips sending the ‘check IMEI’ message for the first N-1 where IMDI/IMEISV is received.
times :

- For releases 8.0 and 8.1, the value must be an integer from 1 to 15.
- For releases 9.0 and higher, the value must be an integer from 1 to 255.

IMPORTANT:

This feature requires the enabling of verify-equipment-identity for IMEI or IMEISV as specified with the the gmm retrieve-equipment-identity imei command of the call-control-profile configuration mode.
Usage:

Configure the identity of the EIR that the SGSN uses and the interaction parameters.

Increasing the check-imei-every-n-events frequency enables the EIR to avoid overload as the number of data-only devices attaching to the network increases.
Example:
Configure EIR with point code 1.255.1 to perform IMEI check after every 61st received Attach Request message:

    equipment-identity-register
    point code 1.255.1 check-imei-every-n-events 62

exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
gmlc
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    gmlc { isdn E.164_number | point-code point-code } [ gsn-address ipv4
    address ] [ source-ssn SSN_value ]no
    gmlc { isdn | point-code }

no

Deletes the GMLC configuration. When the no form of the command is used the SGSN aborts all active Location Requests towards that GMLC and stops the Location Service functions.
isdn number

Enter the E.164 number of the GMLC.

number: must be a string of 1 to 15 digits.

IMPORTANT:

isdn can not be used if point-code is used.
point-code pt_code
Enter SS7 point code address of the GMLC in dotted-decimal format according to variant settings:

- ITU Range 0.0.1 to 7.255.7
- ANSI Range 0.0.1 to 255.255.255
- TTC Range 0.0.1 to 15.31.255
- or a string of 1 to 11 characters

IMPORTANT:

point-code can not be used if isdn is used.
gsn-address ipv4 address

Identifies the IP address of the GMLC of the local PLMN. The address will be published to the HLR in the MAP Update_GPRS_Location Request.

ipv4 address must be a standard dotted-decimal notation.

IMPORTANT:

Even though gsn-address is optional per the CLI grammar, this keyword is a mandatory parameter when configuring the GMLC for the location service feature in the SGSN.
source-ssn ssn

Identifies the subsystem number (SSN) to be used.

ssn must be an integer from 1 to 255.
Usage:

This command identifies the GMLC associated with the MAP Service configuration in support of the Location Services functionality enabled on the SGSN.

Only one GMLC can be defined per MAP Service configuration.

Related Commands:

- associate map-service in the Location Service configuration mode associates this MAP service when configuration Location Services functionality.

Example:
Use a command similar to the following to define a gateway mobility location center (GMLC) with an ISDN ID of 491720499, a GSN address of 192.168.64.1, and an SSN of 131:

    gmlc
    isdn 491720499 gsn-address 192.168.64.1 ssn 131

hlr

This command enters the configuration mode for the home location register (HLR). The HLR is a database containing the subscriber profile information for all mobile stations (MS) / user equipment (UE) connecting to a specific GPRS or UMTS core network.

IMPORTANT:

The commands and options for this mode are documented in the HLR Configuration Mode chapter.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    hlr

policy

This command configures the Transaction Capabilities Application Part (TCAP) -specific MAP policy for either ANSI or ITU SS7 variants.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    [ default ] policy
    tcap { use-received-destination-address | use-received-source-address }

use-received-destination-address

Selecting this keyword overwrites stored CG and CD addresses with a new address received in first TC CNT msg
use-received-source-address

Selecting this keyword instructs the MAP service to use the received source address for the dialog.
Usage:

Use this command to determine how TCAP will handle MAP messages.
Example:

    policy tcap use-received-destination-address

short-message-service

This command enables and disables the short message service (SMS service) and provides access to the SMS Service configuration mode.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    short-message-serviceno short-message-service

no

Disables the SMS service.
Usage:

Enter the command to access the SMS service configuration mode to fine tune the SMS functionality.
Example:

    short-message-service