# GT-Format2 Configuration Mode Commands

The GT-Format2 configuration mode is a sub-mode for either the Global Title Translation Association configuration mode or the Global Title Translation Address-Map configuration mode. This sub-mode configures a set of rules used in the global title translation (GTT) process.
Upon accessing this mode, your prompt should look similar to the following:

    [local]<hostname>(config-gtt-format<#>)#

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the configuration mode and returns to the Exec mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Change the mode back to the Exec mode.
exit

Exits the configuration mode and returns to the Global configuration mode.
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Return to the Global configuration mode.
translation-type

Configures the translation type to be applied during the translation process.
Platform:

ASR 5000
Product:

SGSN
Privilege:

Security Administrator, Administrator
Syntax

    translation-type number

number

Must be an integer between 0 and 255.

Default is 0
Usage:

Use this command to configure the GTT translation type to be applied during global title translation process.

Example

Example

    translation-type 232