# CSCF Schema Statistics

The CSCF schema provides operational statistics that can be used for monitoring and troubleshooting the following products: SCM
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the CSCF Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | VPN Name This is a key variable. Type: Information | String
vpnid | VPN ID This is a key variable. Type: Information | Int32
svcname | Service Name This is a key variable. Type: Information | String
svcid | Service ID This is a key variable. Type: Information | Int32
curregusers | Current Registered Users Type: Gauge | Int32
failedauth | Total number of Failed Authentications. Type: Counter | Int64
regexp | Total number of Registration Expires. Type: Counter | Int64
total-roaming-ue-regs | Total number of Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-succ-regs | Total number of 200 OK Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-fail-regs | Total number of Failed Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-regs-403 | Total number of 403 responses to Registration from Roaming UE. Type: Counter | Int64
total-roaming-ue-re-regs | Total number of Re-Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-succ-re- regs | Total number of 200 OK Re-Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-fail-re-regs | Total number of Failed Re-Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-re-regs-403 | Total number of 403 responses to Re-Registration from Roaming UE. Type: Counter | Int64
total-roaming-ue-de-regs | Total number of De-Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-succ-de-regs | Total number of 200 OK De-Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-fail-de-regs | Total number of Failed De-Registrations from Roaming UE. Type: Counter | Int64
total-roaming-ue-de-regs- 403 | Total number of 403 responses to De-Registration from Roaming UE. Type: Counter | Int64
de-regs-fromue | Total number of De-registrations from UE. Type: Counter | Int64
de-regs-fromnw | Total number of De-registrations from Network. Type: Counter | Int64
sec-regs | Total number of Secure Registrations. Type: Counter | Int64
fail-sec-regs | Total number of Failed Secure Registrations Type: Counter | Int64
emerg-regs | Total number of Emergency Registrations. Type: Counter | Int64
mo-call-succ-rate | Mobile Originating calls success rate. Type: Gauge | Float
mt-call-succ-rate | Mobile Terminating calls success rate. Type: Gauge | Float
mo-voice-call-succ-rate | Mobile Originating VOICE calls success rate. Type: Gauge | Float
mt-voice-call-succ-rate | Mobile Terminating VOICE calls success rate. Type: Gauge | Float
mo-video-call-succ-rate | Mobile Originating VIDEO calls success rate. Type: Gauge | Float
mt-video-call-succ-rate | Mobile Terminating VIDEO calls success rate. Type: Gauge | Float
callattrx | Total number of Call Attempts received. Type: Counter | Int64
callatttx | Total number of Call Attempts transmitted. Type: Counter | Int64
callsuccrx | Total number of Call Success received. Type: Counter | Int64
callsucctx | Total number of Call Success transmitted. Type: Counter | Int64
callfailrx | Total number of Call Failures received. Type: Counter | Int64
callfailtx | Total number of Call Failures transmitted. Type: Counter | Int64
curcscfsess | Total number of current CSCF Sessions. Type: Gauge | Int32
totalcscfsess | Total number of CSCF Sessions. Type: Counter | Int64
call-resp-3xxrx | Total number of Call 3xx Responses received. Type: Counter | Int64
call-resp-3xxtx | Total number of Call 3xx Responses transmitted. Type: Counter | Int64
call-resp-402rx | Total number of Call 402 Responses received. Type: Counter | Int64
call-resp-402tx | Total number of Call 402 Responses transmitted. Type: Counter | Int64
call-resp-403rx | Total number of Call 403 Responses received. Type: Counter | Int64
call-resp-403tx | Total number of Call 403 Responses transmitted. Type: Counter | Int64
call-resp-404rx | Total number of Call 404 Responses received. Type: Counter | Int64
call-resp-404tx | Total number of Call 404 Responses transmitted. Type: Counter | Int64
call-resp-407rx | Total number of Call 407 Responses received. Type: Counter | Int64
call-resp-407tx | Total number of Call 407 Responses transmitted. Type: Counter | Int64
call-resp-408rx | Total number of Call 408 Responses received. Type: Counter | Int64
call-resp-408tx | Total number of Call 408 Responses transmitted. Type: Counter | Int64
call-resp-420rx | Total number of Call 420 Responses received. Type: Counter | Int64
call-resp-420tx | Total number of Call 420 Responses transmitted. Type: Counter | Int64
call-resp-421rx | Total number of Call 421 Responses received. Type: Counter | Int64
call-resp-421tx | Total number of Call 421 Responses transmitted. Type: Counter | Int64
call-resp-480rx | Total number of Call 480 Responses received. Type: Counter | Int64
call-resp-480tx | Total number of Call 480 Responses transmitted. Type: Counter | Int64
call-resp-486rx | Total number of Call 486 Responses received. Type: Counter | Int64
call-resp-486tx | Total number of Call 486 Responses transmitted. Type: Counter | Int64
call-resp-487rx | Total number of Call 487 Responses received. Type: Counter | Int64
call-resp-487tx | Total number of Call 487 Responses transmitted. Type: Counter | Int64
call-resp-488rx | Total number of Call 488 Responses received. Type: Counter | Int64
call-resp-488tx | Total number of Call 488 Responses transmitted. Type: Counter | Int64
call-resp-4xxrx | Total number of Call 4xx Responses received. Type: Counter | Int64
call-resp-4xxtx | Total number of Call 4xx Responses transmitted. Type: Counter | Int64
call-resp-500rx | Total number of Call 500 Responses received. Type: Counter | Int64
call-resp-500tx | Total number of Call 500 Responses transmitted. Type: Counter | Int64
call-resp-503rx | Total number of Call 503 Responses received. Type: Counter | Int64
call-resp-503tx | Total number of Call 503 Responses transmitted. Type: Counter | Int64
call-resp-5xxrx | Total number of Call 5xx Responses received. Type: Counter | Int64
call-resp-5xxtx | Total number of Call 5xx Responses transmitted. Type: Counter | Int64
call-resp-6xxrx | Total number of Call 6xx Responses received. Type: Counter | Int64
call-resp-6xxtx | Total number of Call 6xx Responses transmitted. Type: Counter | Int64
call-rel-attrx | Total number of Call Release Attempts received. Type: Counter | Int64
call-rel-atttx | Total number of Call Release Attempts transmitted. Type: Counter | Int64
call-rel-succrx | Total number of Call Release Success received. Type: Counter | Int64
call-rel-succtx | Total number of Call Release Success transmitted. Type: Counter | Int64
call-rel-failrx | Total number of Call Release Failures received. Type: Counter | Int64
call-rel-failtx | Total number of Call Release Failures transmitted. Type: Counter | Int64
reg-attrx | Total number of Registration Attempts received. Type: Counter | Int64
reg-atttx | Total number of Registration Attempts transmitted. Type: Counter | Int64
reg-succrx | Total number of Registration Successes received. Type: Counter | Int64
reg-succtx | Total number of Registration Successes transmitted. Type: Counter | Int64
reg-failrx | Total number of Registration Failures received. Type: Counter | Int64
reg-failtx | Total number of Registration Failures transmitted. Type: Counter | Int64
reg-resp-401rx | Total number of Registration 401 Responses received. Type: Counter | Int64
reg-resp-401tx | Total number of Registration 401 Responses transmitted. Type: Counter | Int64
reg-resp-403rx | Total number of Registration 403 Responses received. Type: Counter | Int64
reg-resp-403tx | Total number of Registration 403 Responses transmitted. Type: Counter | Int64
reg-resp-404rx | Total number of Registration 404 Responses received. Type: Counter | Int64
reg-resp-404tx | Total number of Registration 404 Responses transmitted. Type: Counter | Int64
reg-resp-420rx | Total number of Registration 420 Responses received. Type: Counter | Int64
reg-resp-420tx | Total number of Registration 420 Responses transmitted. Type: Counter | Int64
reg-resp-439rx | Total number of Registration 439 Responses received. Type: Counter | Int64
reg-resp-439tx | Total number of Registration 439 Responses transmitted. Type: Counter | Int64
reg-resp-4xxrx | Total number of Registration 4xx Responses received. Type: Counter | Int64
reg-resp-4xxtx | Total number of Registration 4xx Responses transmitted. Type: Counter | Int64
reg-resp-500rx | Total number of Registration 500 Responses received. Type: Counter | Int64
reg-resp-500tx | Total number of Registration 500 Responses transmitted. Type: Counter | Int64
reg-resp-5xxrx | Total number of Registration 5xx Responses received. Type: Counter | Int64
reg-resp-5xxtx | Total number of Registration 5xx Responses transmitted. Type: Counter | Int64
reg-resp-6xxrx | Total number of Registration 6xx Responses received. Type: Counter | Int64
reg-resp-6xxtx | Total number of Registration 6xx Responses transmitted. Type: Counter | Int64
rereg-attrx | Total number of Refresh Registration Attempts received. Type: Counter | Int64
rereg-atttx | Total number of Refresh Registration Attempts transmitted. Type: Counter | Int64
rereg-succrx | Total Refresh Registration Successes received. Type: Counter | Int64
rereg-succtx | Total number of Refresh Registration Successes transmitted. Type: Counter | Int64
rereg-failrx | Total number of Refresh Registration Failures received. Type: Counter | Int64
rereg-failtx | Total number of Refresh Registration Failures transmitted. Type: Counter | Int64
rereg-resp-401rx | Total number of Refresh Registration 401 Responses received. Type: Counter | Int64
rereg-resp-401tx | Total number of Refresh Registration 401 Responses transmitted. Type: Counter | Int64
rereg-resp-403rx | Total number of Refresh Registration 403 Responses received. Type: Counter | Int64
rereg-resp-403tx | Total number of Refresh Registration 403 Responses transmitted. Type: Counter | Int64
rereg-resp-404rx | Total number of Refresh Registration 404 Responses received. Type: Counter | Int64
rereg-resp-404tx | Total number of Refresh Registration 404 Responses transmitted. Type: Counter | Int64
rereg-resp-420rx | Total number of Refresh Registration 420 Responses received. Type: Counter | Int64
rereg-resp-420tx | Total number of Refresh Registration 420 Responses transmitted. Type: Counter | Int64
rereg-resp-439rx | Total number of Refresh Registration 439 Responses received. Type: Counter | Int64
rereg-resp-439tx | Total number of Refresh Registration 439 Responses transmitted. Type: Counter | Int64
rereg-resp-4xxrx | Total number of Refresh Registration 4xx Responses received. Type: Counter | Int64
rereg-resp-4xxtx | Total number of Refresh Registration 4xx Responses transmitted. Type: Counter | Int64
rereg-resp-500rx | Total number of Refresh Registration 500 Responses received. Type: Counter | Int64
rereg-resp-500tx | Total number of Refresh Registration 500 Responses transmitted. Type: Counter | Int64
rereg-resp-5xxrx | Total number of Refresh Registration 5xx Responses received. Type: Counter | Int64
rereg-resp-5xxtx | Total number of Refresh Registration 5xx Responses transmitted. Type: Counter | Int64
rereg-resp-6xxrx | Total number of Refresh Registration 6xx Responses received. Type: Counter | Int64
rereg-resp-6xxtx | Total number of Refresh Registration 6xx Responses transmitted. Type: Counter | Int64
dereg-attrx | Total number of Deregistration Attempts received. Type: Counter | Int64
dereg-atttx | Total number of Deregistration Attempts transmitted. Type: Counter | Int64
dereg-succrx | Total number of Deregistration Successes received. Type: Counter | Int64
dereg-succtx | Total number of Deregistration Successes transmitted. Type: Counter | Int64
dereg-failrx | Total number of Deregistration Failures received. Type: Counter | Int64
dereg-failtx | Total number of Deregistration Failures transmitted. Type: Counter | Int64
dereg-resp-401rx | Total number of Deregister 401 Responses received. Type: Counter | Int64
dereg-resp-401tx | Total number of Deregister 401 Responses transmitted. Type: Counter | Int64
dereg-resp-403rx | Total number of Deregister 403 Responses received. Type: Counter | Int64
dereg-resp-403tx | Total number of Deregister 403 Responses transmitted. Type: Counter | Int64
dereg-resp-404rx | Total number of Deregister 404 Responses received. Type: Counter | Int64
dereg-resp-404tx | Total number of Deregister 404 Responses transmitted. Type: Counter | Int64
dereg-resp-420rx | Total number of Deregister 420 Responses received. Type: Counter | Int64
dereg-resp-420tx | Total number of Deregister 420 Responses transmitted. Type: Counter | Int64
dereg-resp-4xxrx | Total number of Deregister 4xx Responses received. Type: Counter | Int64
dereg-resp-4xxtx | Total number of Deregister 4xx Responses transmitted. Type: Counter | Int64
dereg-resp-500rx | Total number of Deregister 500 Responses received. Type: Counter | Int64
dereg-resp-500tx | Total number of Deregister 500 Responses transmitted. Type: Counter | Int64
dereg-resp-5xxrx | Total number of Deregister 5xx Responses received. Type: Counter | Int64
dereg-resp-5xxtx | Total number of Deregister 5xx Responses transmitted. Type: Counter | Int64
dereg-resp-6xxrx | Total number of Deregister 6xx Responses received. Type: Counter | Int64
dereg-resp-6xxtx | Total number of Deregister 6xx Responses transmitted. Type: Counter | Int64
subscribe-attempt-rx | Total number of Subscribe attempts received. Type: Counter | Int64
subscribe-attempt-tx | Total number of Subscribe attempts transmitted. Type: Counter | Int64
subscribe-success-rx | Total number of Subscribe successes received. Type: Counter | Int64
subscribe-success-tx | Total number of Subscribe successes transmitted. Type: Counter | Int64
subscribe-failure-rx | Total number of Subscribe failures received. Type: Counter | Int64
subscribe-failure-tx | Total number of Subscribe failures transmitted. Type: Counter | Int64
notify-attempt-rx | Total number of Notify attempts received. Type: Counter | Int64
notify-attempt-tx | Total number of Notify attempts transmitted. Type: Counter | Int64
notify-success-rx | Total number of Notify successes received. Type: Counter | Int64
notify-success-tx | Total number of Notify successes transmitted. Type: Counter | Int64
notify-failure-rx | Total number of Notify failures received. Type: Counter | Int64
notify-failure-tx | Total number of Notify failures transmitted. Type: Counter | Int64
publish-attempt-rx | Total number of Publish attempts received. Type: Counter | Int64
publish-attempt-tx | Total number of Publish Attempts attempts transmitted. Type: Counter | Int64
publish-success-rx | Total number of Publish successes received. Type: Counter | Int64
publish-success-tx | Total number of Publish successes transmitted. Type: Counter | Int64
publish-failure-rx | Total number of Publish failures received. Type: Counter | Int64
publish-failure-tx | Total number of Publish failures transmitted. Type: Counter | Int64
msgsum-subs-attrx | Total number of “msg-summary” Subscription attempts received. Type: Counter | Int64
msgsum-subs-atttx | Total number of “msg-summary” Subscription attempts transmitted. Type: Counter | Int64
msgsum-subs-succrx | Total number of “msg-summary” Subscription successes received. Type: Counter | Int64
msgsum-subs-succtx | Total number of “msg-summary” Subscription successes transmitted. Type: Counter | Int64
msgsum-subs-failrx | Total number of “msg-summary” Subscription failures received. Type: Counter | Int64
msgsum-subs-failtx | Total number of “msg-summary” Subscription failures transmitted. Type: Counter | Int64
msgsum-subs-resp-200rx | Total number of “msg-summary” Subscription 200 Responses received. Type: Counter | Int64
msgsum-subs-resp-200tx | Total number of “msg-summary” Subscription 200 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-202rx | Total number of “msg-summary” Subscription 202 Responses received. Type: Counter | Int64
msgsum-subs-resp-202tx | Total number of “msg-summary” Subscription 202 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-400rx | Total number of “msg-summary” Subscription 400 Responses received. Type: Counter | Int64
msgsum-subs-resp-400tx | Total number of “msg-summary” Subscription 400 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-403rx | Total number of “msg-summary” Subscription 403 Responses received. Type: Counter | Int64
msgsum-subs-resp-403tx | Total number of “msg-summary” Subscription 403 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-481rx | Total number of “msg-summary” Subscription 481 Responses received. Type: Counter | Int64
msgsum-subs-resp-481tx | Total number of “msg-summary” Subscription 481 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-489rx | Total number of “msg-summary” Subscription 489 Responses received. Type: Counter | Int64
msgsum-subs-resp-489tx | Total number of “msg-summary” Subscription 489 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-500rx | Total number of “msg-summary” Subscription 500 Responses received. Type: Counter | Int64
msgsum-subs-resp-500tx | Total number of “msg-summary” Subscription 500 Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-3xxrx | Total number of “msg-summary” Subscription 3XX Responses received. Type: Counter | Int64
msgsum-subs-resp-3xxtx | Total number of “msg-summary” Subscription 3XX Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-4xxrx | Total number of “msg-summary” Subscription 4XX Responses received. Type: Counter | Int64
msgsum-subs-resp-4xxtx | Total number of “msg-summary” Subscription 4XX Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-5xxrx | Total number of “msg-summary” Subscription 5XX Responses received. Type: Counter | Int64
msgsum-subs-resp-5xxtx | Total number of “msg-summary” Subscription 5XX Responses transmitted. Type: Counter | Int64
msgsum-subs-resp-6xxrx | Total number of “msg-summary” Subscription 6XX Responses received. Type: Counter | Int64
msgsum-subs-resp-6xxtx | Total number of “msg-summary” Subscription 6XX Responses transmitted. Type: Counter | Int64
msgsum-resubs-attrx | Total number of “msg-summary” Refresh Subscription Attempts received. Type: Counter | Int64
msgsum-resubs-atttx | Total number of “msg-summary” Refresh Subscription Attempts transmitted. Type: Counter | Int64
msgsum-resubs-succrx | Total number of “msg-summary” Refresh Subscription Successes received. Type: Counter | Int64
msgsum-resubs-succtx | Total number of “msg-summary” Refresh Subscription Successes transmitted. Type: Counter | Int64
msgsum-resubs-failrx | Total number of “msg-summary” Refresh Subscription Failures received. Type: Counter | Int64
msgsum-resubs-failtx | Total number of “msg-summary” Refresh Subscription Failures transmitted. Type: Counter | Int64
msgsum-resubs-resp-200rx | Total number of “msg-summary” Refresh Subscription 200 Responses received. Type: Counter | Int64
msgsum-resubs-resp-200tx | Total number of “msg-summary” Refresh Subscription 200 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-202rx | Total number of “msg-summary” Refresh Subscription 202 Responses received. Type: Counter | Int64
msgsum-resubs-resp-202tx | Total number of “msg-summary” Refresh Subscription 202 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-400rx | Total number of “msg-summary” Refresh Subscription 400 Responses received. Type: Counter | Int64
msgsum-resubs-resp-400tx | Total number of “msg-summary” Refresh Subscription 400 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-403rx | Total number of “msg-summary” Refresh Subscription 403 Responses received. Type: Counter | Int64
msgsum-resubs-resp-403tx | Total number of “msg-summary” Refresh Subscription 403 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-481rx | Total number of “msg-summary” Refresh Subscription 481 Responses received. Type: Counter | Int64
msgsum-resubs-resp-481tx | Total number of “msg-summary” Refresh Subscription 481 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-489rx | Total number of “msg-summary” Refresh Subscription 489 Responses received. Type: Counter | Int64
msgsum-resubs-resp-489tx | Total number of “msg-summary” Refresh Subscription 489 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-500rx | Total number of “msg-summary” Refresh Subscription 500 Responses received. Type: Counter | Int64
msgsum-resubs-resp-500tx | Total number of “msg-summary” Refresh Subscription 500 Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-3xxrx | Total number of “msg-summary” Refresh Subscription 3XX Responses received. Type: Counter | Int64
msgsum-resubs-resp-3xxtx | Total number of “msg-summary” Refresh Subscription 3XX Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-4xxrx | Total number of “msg-summary” Refresh Subscription 4XX Responses received. Type: Counter | Int64
msgsum-resubs-resp-4xxtx | Total number of “msg-summary” Refresh Subscription 4XX Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-5xxrx | Total number of “msg-summary” Refresh Subscription 5XX Responses received. Type: Counter | Int64
msgsum-resubs-resp-5xxtx | Total number of “msg-summary” Refresh Subscription 5XX Responses transmitted. Type: Counter | Int64
msgsum-resubs-resp-6xxrx | Total number of “msg-summary” Refresh Subscription 6XX Responses received. Type: Counter | Int64
msgsum-resubs-resp-6xxtx | Total number of “msg-summary” Refresh Subscription 6XX Responses transmitted. Type: Counter | Int64
msgsum-unsubs-attrx | Total number of “msg-summary” Un-Subscription Attempts received. Type: Counter | Int64
msgsum-unsubs-atttx | Total number of “msg-summary” Un-Subscription Attempts transmitted. Type: Counter | Int64
msgsum-unsubs-succrx | Total number of “msg-summary” Un-Subscription Successes received. Type: Counter | Int64
msgsum-unsubs-succtx | Total number of “msg-summary” Un-Subscription Successes transmitted. Type: Counter | Int64
msgsum-unsubs-failrx | Total number of “msg-summary” Un-Subscription Failures received. Type: Counter | Int64
msgsum-unsubs-failtx | Total number of “msg-summary” Un-Subscription Failures transmitted. Type: Counter | Int64
msgsum-unsubs-resp-200rx | Total number of “msg-summary” Un-Subscription 200 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-200tx | Total number of “msg-summary” Un-Subscription 200 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-202rx | Total number of “msg-summary” Un-Subscription 202 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-202tx | Total number of “msg-summary” Un-Subscription 202 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-400rx | Total number of “msg-summary” Un-Subscription 400 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-400tx | Total number of “msg-summary” Un-Subscription 400 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-403rx | Total number of “msg-summary” Un-Subscription 403 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-403tx | Total number of “msg-summary” Un-Subscription 403 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-481rx | Total number of “msg-summary” Un-Subscription 481 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-481tx | Total number of “msg-summary” Un-Subscription 481 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-489rx | Total number of “msg-summary” Un-Subscription 489 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-489tx | Total number of “msg-summary” Un-Subscription 489 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-500rx | Total number of “msg-summary” Un-Subscription 500 Responses received. Type: Counter | Int64
msgsum-unsubs-resp-500tx | Total number of “msg-summary” Un-Subscription 500 Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-3xxrx | Total number of “msg-summary” Un-Subscription 3XX Responses received. Type: Counter | Int64
msgsum-unsubs-resp-3xxtx | Total number of “msg-summary” Un-Subscription 3XX Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-4xxrx | Total number of “msg-summary” Un-Subscription 4XX Responses received. Type: Counter | Int64
msgsum-unsubs-resp-4xxtx | Total number of “msg-summary” Un-Subscription 4XX Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-5xxrx | Total number of “msg-summary” Un-Subscription 5XX Responses received. Type: Counter | Int64
msgsum-unsubs-resp-5xxtx | Total number of “msg-summary” Un-Subscription 5XX Responses transmitted. Type: Counter | Int64
msgsum-unsubs-resp-6xxrx | Total number of “msg-summary” Un-Subscription 6XX Responses received. Type: Counter | Int64
msgsum-unsubs-resp-6xxtx | Total number of “msg-summary” Un-Subscription 6XX Responses transmitted. Type: Counter | Int64
msgsum-notify-attrx | Total number of “msg-summary” Notify Attempts received. Type: Counter | Int64
msgsum-notify-atttx | Total number of “msg-summary” Notify Attempts transmitted. Type: Counter | Int64
msgsum-notify-succrx | Total number of “msg-summary” Notify Successes received. Type: Counter | Int64
msgsum-notify-succtx | Total number of “msg-summary” Notify Successes transmitted. Type: Counter | Int64
msgsum-notify-failrx | Total number of “msg-summary” Notify Failures received. Type: Counter | Int64
msgsum-notify-failtx | Total number of “msg-summary” Notify Failures transmitted. Type: Counter | Int64
msgsum-notify-resp-3xxrx | Total number of “msg-summary” Notify 3XX Responses received. Type: Counter | Int64
msgsum-notify-resp-3xxtx | Total number of “msg-summary” Notify 3XX Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-400rx | Total number of “msg-summary” Notify 400 Responses received. Type: Counter | Int64
msgsum-notify-resp-400tx | Total number of “msg-summary” Notify 400 Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-481rx | Total number of “msg-summary” Notify 481 Responses received. Type: Counter | Int64
msgsum-notify-resp-481tx | Total number of “msg-summary” Notify 481 Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-489rx | Total number of “msg-summary” Notify 489 Responses received. Type: Counter | Int64
msgsum-notify-resp-489tx | Total number of “msg-summary” Notify 489 Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-4xxrx | Total number of “msg-summary” Notify 4XX Responses received. Type: Counter | Int64
msgsum-notify-resp-4xxtx | Total number of “msg-summary” Notify 4XX Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-500rx | Total number of “msg-summary” Notify 500 Responses received. Type: Counter | Int64
msgsum-notify-resp-500tx | Total number of “msg-summary” Notify 500 Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-5xxrx | Total number of “msg-summary” Notify 5XX Responses received. Type: Counter | Int64
msgsum-notify-resp-5xxtx | Total number of “msg-summary” Notify 5XX Responses transmitted. Type: Counter | Int64
msgsum-notify-resp-6xxrx | Total number of “msg-summary” Notify 6XX Responses received. Type: Counter | Int64
msgsum-notify-resp-6xxtx | Total number of “msg-summary” Notify 6XX Responses transmitted. Type: Counter | Int64
msgsum-pub-attrx | Total number of “msg-summary” Publish Attempts received. Type: Counter | Int64
msgsum-pub-atttx | Total number of “msg-summary” Publish Attempts transmitted. Type: Counter | Int64
msgsum-pub-succrx | Total number of “msg-summary” Publish Successes received. Type: Counter | Int64
msgsum-pub-succtx | Total number of “msg-summary” Publish Successes transmitted. Type: Counter | Int64
msgsum-pub-failrx | Total number of “msg-summary” Publish Failures received. Type: Counter | Int64
msgsum-pub-failtx | Total number of “msg-summary” Publish Failures transmitted. Type: Counter | Int64
msgsum-pub-resp-3xxrx | Total number of “msg-summary” Publish 3XX Responses received. Type: Counter | Int64
msgsum-pub-resp-3xxtx | Total number of “msg-summary” Publish 3XX Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-400rx | Total number of “msg-summary” Publish 400 Responses received. Type: Counter | Int64
msgsum-pub-resp-400tx | Total number of “msg-summary” Publish 400 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-404rx | Total number of “msg-summary” Publish 404 Responses received. Type: Counter | Int64
msgsum-pub-resp-404tx | Total number of “msg-summary” Publish 404 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-412rx | Total number of “msg-summary” Publish 412 Responses received. Type: Counter | Int64
msgsum-pub-resp-412tx | Total number of “msg-summary” Publish 412 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-423rx | Total number of “msg-summary” Publish 423 Responses received. Type: Counter | Int64
msgsum-pub-resp-423tx | Total number of “msg-summary” Publish 423 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-489rx | Total number of “msg-summary” Publish 489 Responses received. Type: Counter | Int64
msgsum-pub-resp-489tx | Total number of “msg-summary” Publish 489 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-4xxrx | Total number of “msg-summary” Publish 4XX Responses received. Type: Counter | Int64
msgsum-pub-resp-4xxtx | Total number of “msg-summary” Publish 4XX Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-500rx | Total number of “msg-summary” Publish 500 Responses received. Type: Counter | Int64
msgsum-pub-resp-500tx | Total number of “msg-summary” Publish 500 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-503rx | Total number of “msg-summary” Publish 503 Responses received. Type: Counter | Int64
msgsum-pub-resp-503tx | Total number of “msg-summary” Publish 503 Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-5xxrx | Total number of “msg-summary” Publish 5XX Responses received. Type: Counter | Int64
msgsum-pub-resp-5xxtx | Total number of “msg-summary” Publish 5XX Responses transmitted. Type: Counter | Int64
msgsum-pub-resp-6xxrx | Total number of “msg-summary” Publish 6XX Responses received. Type: Counter | Int64
msgsum-pub-resp-6xxtx | Total number of “msg-summary” Publish 6XX Responses transmitted. Type: Counter | Int64
msgsum-unpub-attrx | Total number of “msg-summary” Un-Publish Attempts received. Type: Counter | Int64
msgsum-unpub-atttx | Total number of “msg-summary” Un-Publish Attempts transmitted. Type: Counter | Int64
msgsum-unpub-succrx | Total number of “msg-summary” Un-Publish Successes received. Type: Counter | Int64
msgsum-unpub-succtx | Total number of “msg-summary” Un-Publish Successes transmitted. Type: Counter | Int64
msgsum-unpub-failrx | Total number of “msg-summary” Un-Publish Failures received. Type: Counter | Int64
msgsum-unpub-failtx | Total number of “msg-summary” Un-Publish Failures transmitted. Type: Counter | Int64
msgsum-unpub-resp-3xxrx | Total number of “msg-summary” Un-Publish 3XX Responses received. Type: Counter | Int64
msgsum-unpub-resp-3xxtx | Total number of “msg-summary” Un-Publish 3XX Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-400rx | Total number of “msg-summary” Un-Publish 400 Responses received. Type: Counter | Int64
msgsum-unpub-resp-400tx | Total number of “msg-summary” Un-Publish 400 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-404rx | Total number of “msg-summary” Un-Publish 404 Responses received. Type: Counter | Int64
msgsum-unpub-resp-404tx | Total number of “msg-summary” Un-Publish 404 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-412rx | Total number of “msg-summary” Un-Publish 412 Responses received. Type: Counter | Int64
msgsum-unpub-resp-412tx | Total number of “msg-summary” Un-Publish 412 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-423rx | Total number of “msg-summary” Un-Publish 423 Responses received. Type: Counter | Int64
msgsum-unpub-resp-423tx | Total number of “msg-summary” Un-Publish 423 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-489rx | Total number of “msg-summary” Un-Publish 489 Responses received. Type: Counter | Int64
msgsum-unpub-resp-489tx | Total number of “msg-summary” Un-Publish 489 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-4xxrx | Total number of “msg-summary” Un-Publish 4XX Responses received. Type: Counter | Int64
msgsum-unpub-resp-4xxtx | Total number of “msg-summary” Un-Publish 4XX Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-500rx | Total number of “msg-summary” Un-Publish 500 Responses received. Type: Counter | Int64
msgsum-unpub-resp-500tx | Total number of “msg-summary” Un-Publish 500 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-503rx | Total number of “msg-summary” Un-Publish 503 Responses received. Type: Counter | Int64
msgsum-unpub-resp-503tx | Total number of “msg-summary” Un-Publish 503 Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-5xxrx | Total number of “msg-summary” Un-Publish 5XX Responses received. Type: Counter | Int64
msgsum-unpub-resp-5xxtx | Total number of “msg-summary” Un-Publish 5XX Responses transmitted. Type: Counter | Int64
msgsum-unpub-resp-6xxrx | Total number of “msg-summary” Un-Publish 6XX Responses received. Type: Counter | Int64
msgsum-unpub-resp-6xxtx | Total number of “msg-summary” Un-Publish 6XX Responses transmitted. Type: Counter | Int64
pres-subs-attrx | Total number of “presence” Subscription Attempts received. Type: Counter | Int64
pres-subs-atttx | Total number of “presence” Subscription Attempts transmitted. Type: Counter | Int64
pres-subs-succrx | Total number of “presence” Subscription Successes received. Type: Counter | Int64
pres-subs-succtx | Total number of “presence” Subscription Successes transmitted. Type: Counter | Int64
pres-subs-failrx | Total number of “presence” Subscription Failures received. Type: Counter | Int64
pres-subs-failtx | Total number of “presence” Subscription Failures transmitted. Type: Counter | Int64
pres-subs-resp-200rx | Total number of “presence” Subscription 200 Responses received. Type: Counter | Int64
pres-subs-resp-200tx | Total number of “presence” Subscription 200 Responses transmitted. Type: Counter | Int64
pres-subs-resp-202rx | Total number of “presence” Subscription 202 Responses received. Type: Counter | Int64
pres-subs-resp-202tx | Total number of “presence” Subscription 202 Responses transmitted. Type: Counter | Int64
pres-subs-resp-400rx | Total number of “presence” Subscription 400 Responses received. Type: Counter | Int64
pres-subs-resp-400tx | Total number of “presence” Subscription 400 Responses transmitted. Type: Counter | Int64
pres-subs-resp-403rx | Total number of “presence” Subscription 403 Responses received. Type: Counter | Int64
pres-subs-resp-403tx | Total number of “presence” Subscription 403 Responses transmitted. Type: Counter | Int64
pres-subs-resp-481rx | Total number of “presence” Subscription 481 Responses received. Type: Counter | Int64
pres-subs-resp-481tx | Total number of “presence” Subscription 481 Responses transmitted. Type: Counter | Int64
pres-subs-resp-489rx | Total number of “presence” Subscription 489 Responses received. Type: Counter | Int64
pres-subs-resp-489tx | Total number of “presence” Subscription 489 Responses transmitted. Type: Counter | Int64
pres-subs-resp-500rx | Total number of “presence” Subscription 500 Responses received. Type: Counter | Int64
pres-subs-resp-500tx | Total number of “presence” Subscription 500 Responses transmitted. Type: Counter | Int64
pres-subs-resp-3xxrx | Total number of “presence” Subscription 3XX Responses received. Type: Counter | Int64
pres-subs-resp-3xxtx | Total number of “presence” Subscription 3XX Responses transmitted. Type: Counter | Int64
pres-subs-resp-4xxrx | Total number of “presence” Subscription 4XX Responses received. Type: Counter | Int64
pres-subs-resp-4xxtx | Total number of “presence” Subscription 4XX Responses transmitted. Type: Counter | Int64
pres-subs-resp-5xxrx | Total number of “presence” Subscription 5XX Responses received. Type: Counter | Int64
pres-subs-resp-5xxtx | Total number of “presence” Subscription 5XX Responses transmitted. Type: Counter | Int64
pres-subs-resp-6xxrx | Total number of “presence” Subscription 6XX Responses received. Type: Counter | Int64
pres-subs-resp-6xxtx | Total number of “presence” Subscription 6XX Responses transmitted. Type: Counter | Int64
pres-resubs-attrx | Total number of “presence” Refresh Subscription Attempts received. Type: Counter | Int64
pres-resubs-atttx | Total number of “presence” Refresh Subscription Attempts transmitted. Type: Counter | Int64
pres-resubs-succrx | Total number of “presence” Refresh Subscription Successes received. Type: Counter | Int64
pres-resubs-succtx | Total number of “presence” Refresh Subscription Successes transmitted. Type: Counter | Int64
pres-resubs-failrx | Total number of “presence” Refresh Subscription Failures received. Type: Counter | Int64
pres-resubs-failtx | Total number of “presence” Refresh Subscription Failures transmitted. Type: Counter | Int64
pres-resubs-resp-200rx | Total number of “presence” Refresh Subscription 200 Responses received. Type: Counter | Int64
pres-resubs-resp-200tx | Total number of “presence” Refresh Subscription 200 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-202rx | Total number of “presence” Refresh Subscription 202 Responses received. Type: Counter | Int64
pres-resubs-resp-202tx | Total number of “presence” Refresh Subscription 202 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-400rx | Total number of “presence” Refresh Subscription 400 Responses received. Type: Counter | Int64
pres-resubs-resp-400tx | Total number of “presence” Refresh Subscription 400 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-403rx | Total number of “presence” Refresh Subscription 403 Responses received. Type: Counter | Int64
pres-resubs-resp-403tx | Total number of “presence” Refresh Subscription 403 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-481rx | Total number of “presence” Refresh Subscription 481 Responses received. Type: Counter | Int64
pres-resubs-resp-481tx | Total number of “presence” Refresh Subscription 481 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-489rx | Total number of “presence” Refresh Subscription 489 Responses received. Type: Counter | Int64
pres-resubs-resp-489tx | Total number of “presence” Refresh Subscription 489 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-500rx | Total number of “presence” Refresh Subscription 500 Responses received. Type: Counter | Int64
pres-resubs-resp-500tx | Total number of “presence” Refresh Subscription 500 Responses transmitted. Type: Counter | Int64
pres-resubs-resp-3xxrx | Total number of “presence” Refresh Subscription 3XX Responses received. Type: Counter | Int64
pres-resubs-resp-3xxtx | Total number of “presence” Refresh Subscription 3XX Responses transmitted. Type: Counter | Int64
pres-resubs-resp-4xxrx | Total number of “presence” Refresh Subscription 4XX Responses received. Type: Counter | Int64
pres-resubs-resp-4xxtx | Total number of “presence” Refresh Subscription 4XX Responses transmitted. Type: Counter | Int64
pres-resubs-resp-5xxrx | Total number of “presence” Refresh Subscription 5XX Responses received. Type: Counter | Int64
pres-resubs-resp-5xxtx | Total number of “presence” Refresh Subscription 5XX Responses transmitted. Type: Counter | Int64
pres-resubs-resp-6xxrx | Total number of “presence” Refresh Subscription 6XX Responses received. Type: Counter | Int64
pres-resubs-resp-6xxtx | Total number of “presence” Refresh Subscription 6XX Responses transmitted. Type: Counter | Int64
pres-unsubs-attrx | Total number of “presence” Un-Subscription Attempts received. Type: Counter | Int64
pres-unsubs-atttx | Total number of “presence” Un-Subscription Attempts transmitted. Type: Counter | Int64
pres-unsubs-succrx | Total number of “presence” Un-Subscription Successes received. Type: Counter | Int64
pres-unsubs-succtx | Total number of “presence” Un-Subscription Successes transmitted. Type: Counter | Int64
pres-unsubs-failrx | Total number of “presence” Un-Subscription Failures received. Type: Counter | Int64
pres-unsubs-failtx | Total number of “presence” Un-Subscription Failures transmitted. Type: Counter | Int64
pres-unsubs-resp-200rx | Total number of “presence” Un-Subscription 200 Responses received. Type: Counter | Int64
pres-unsubs-resp-200tx | Total number of “presence” Un-Subscription 200 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-202rx | Total number of “presence” Un-Subscription 202 Responses received. Type: Counter | Int64
pres-unsubs-resp-202tx | Total number of “presence” Un-Subscription 202 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-400rx | Total number of “presence” Un-Subscription 400 Responses received. Type: Counter | Int64
pres-unsubs-resp-400tx | Total number of “presence” Un-Subscription 400 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-403rx | Total number of “presence” Un-Subscription 403 Responses received. Type: Counter | Int64
pres-unsubs-resp-403tx | Total number of “presence” Un-Subscription 403 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-481rx | Total number of “presence” Un-Subscription 481 Responses received. Type: Counter | Int64
pres-unsubs-resp-481tx | Total number of “presence” Un-Subscription 481 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-489rx | Total number of “presence” Un-Subscription 489 Responses received. Type: Counter | Int64
pres-unsubs-resp-489tx | Total number of “presence” Un-Subscription 489 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-500rx | Total number of “presence” Un-Subscription 500 Responses received. Type: Counter | Int64
pres-unsubs-resp-500tx | Total number of “presence” Un-Subscription 500 Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-3xxrx | Total number of “presence” Un-Subscription 3XX Responses received. Type: Counter | Int64
pres-unsubs-resp-3xxtx | Total number of “presence” Un-Subscription 3XX Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-4xxrx | Total number of “presence” Un-Subscription 4XX Responses received. Type: Counter | Int64
pres-unsubs-resp-4xxtx | Total number of “presence” Un-Subscription 4XX Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-5xxrx | Total number of “presence” Un-Subscription 5XX Responses received. Type: Counter | Int64
pres-unsubs-resp-5xxtx | Total number of “presence” Un-Subscription 5XX Responses transmitted. Type: Counter | Int64
pres-unsubs-resp-6xxrx | Total number of “presence” Un-Subscription 6XX Responses received. Type: Counter | Int64
pres-unsubs-resp-6xxtx | Total number of “presence” Un-Subscription 6XX Responses transmitted. Type: Counter | Int64
pres-notify-attrx | Total number of “presence” Notify Attempts received. Type: Counter | Int64
pres-notify-atttx | Total number of “presence” Notify Attempts transmitted. Type: Counter | Int64
pres-notify-succrx | Total number of “presence” Notify Successes received. Type: Counter | Int64
pres-notify-succtx | Total number of “presence” Notify Successes transmitted. Type: Counter | Int64
pres-notify-failrx | Total number of “presence” Notify Failures received. Type: Counter | Int64
pres-notify-failtx | Total number of “presence” Notify Failures transmitted. Type: Counter | Int64
pres-notify-resp-3xxrx | Total number of “presence” Notify 3XX Responses received. Type: Counter | Int64
pres-notify-resp-3xxtx | Total number of “presence” Notify 3XX Responses transmitted. Type: Counter | Int64
pres-notify-resp-400rx | Total number of “presence” Notify 400 Responses received. Type: Counter | Int64
pres-notify-resp-400tx | Total number of “presence” Notify 400 Responses transmitted. Type: Counter | Int64
pres-notify-resp-481rx | Total number of “presence” Notify 481 Responses received. Type: Counter | Int64
pres-notify-resp-481tx | Total number of “presence” Notify 481 Responses transmitted. Type: Counter | Int64
pres-notify-resp-489rx | Total number of “presence” Notify 489 Responses received. Type: Counter | Int64
pres-notify-resp-489tx | Total number of “presence” Notify 489 Responses transmitted. Type: Counter | Int64
pres-notify-resp-4xxrx | Total number of “presence” Notify 4XX Responses received. Type: Counter | Int64
pres-notify-resp-4xxtx | Total number of “presence” Notify 4XX Responses transmitted. Type: Counter | Int64
pres-notify-resp-500rx | Total number of “presence” Notify 500 Responses received. Type: Counter | Int64
pres-notify-resp-500tx | Total number of “presence” Notify 500 Responses transmitted. Type: Counter | Int64
pres-notify-resp-5xxrx | Total number of “presence” Notify 5XX Responses received. Type: Counter | Int64
pres-notify-resp-5xxtx | Total number of “presence” Notify 5XX Responses transmitted. Type: Counter | Int64
pres-notify-resp-6xxrx | Total number of “presence” Notify 6XX Responses received. Type: Counter | Int64
pres-notify-resp-6xxtx | Total number of “presence” Notify 6XX Responses transmitted. Type: Counter | Int64
pres-pub-attrx | Total number of “presence” Publish Attempts received. Type: Counter | Int64
pres-pub-atttx | Total number of “presence” Publish Attempts transmitted. Type: Counter | Int64
pres-pub-succrx | Total number of “presence” Publish Successes received. Type: Counter | Int64
pres-pub-succtx | Total number of “presence” Publish Successes transmitted. Type: Counter | Int64
pres-pub-failrx | Total number of “presence” Publish Failures received. Type: Counter | Int64
pres-pub-failtx | Total number of “presence” Publish Failures transmitted. Type: Counter | Int64
pres-pub-resp-3xxrx | Total number of “presence” Publish 3XX Responses received. Type: Counter | Int64
pres-pub-resp-3xxtx | Total number of “presence” Publish 3XX Responses transmitted. Type: Counter | Int64
pres-pub-resp-400rx | Total number of “presence” Publish 400 Responses received. Type: Counter | Int64
pres-pub-resp-400tx | Total number of “presence” Publish 400 Responses transmitted. Type: Counter | Int64
pres-pub-resp-404rx | Total number of “presence” Publish 404 Responses received. Type: Counter | Int64
pres-pub-resp-404tx | Total number of “presence” Publish 404 Responses transmitted. Type: Counter | Int64
pres-pub-resp-412rx | Total number of “presence” Publish 412 Responses received. Type: Counter | Int64
pres-pub-resp-412tx | Total number of “presence” Publish 412 Responses transmitted. Type: Counter | Int64
pres-pub-resp-423rx | Total number of “presence” Publish 423 Responses received. Type: Counter | Int64
pres-pub-resp-423tx | Total number of “presence” Publish 423 Responses transmitted. Type: Counter | Int64
pres-pub-resp-489rx | Total number of “presence” Publish 489 Responses received. Type: Counter | Int64
pres-pub-resp-489tx | Total number of “presence” Publish 489 Responses transmitted. Type: Counter | Int64
pres-pub-resp-4xxrx | Total number of “presence” Publish 4XX Responses received. Type: Counter | Int64
pres-pub-resp-4xxtx | Total number of “presence” Publish 4XX Responses transmitted. Type: Counter | Int64
pres-pub-resp-500rx | Total number of “presence” Publish 500 Responses received. Type: Counter | Int64
pres-pub-resp-500tx | Total number of “presence” Publish 500 Responses transmitted. Type: Counter | Int64
pres-pub-resp-503rx | Total number of “presence” Publish 503 Responses received. Type: Counter | Int64
pres-pub-resp-503tx | Total number of “presence” Publish 503 Responses transmitted. Type: Counter | Int64
pres-pub-resp-5xxrx | Total number of “presence” Publish 5XX Responses received. Type: Counter | Int64
pres-pub-resp-5xxtx | Total number of “presence” Publish 5XX Responses transmitted. Type: Counter | Int64
pres-pub-resp-6xxrx | Total number of “presence” Publish 6XX Responses received. Type: Counter | Int64
pres-pub-resp-6xxtx | Total number of “presence” Publish 6XX Responses transmitted. Type: Counter | Int64
pres-unpub-attrx | Total number of “presence” Un-Publish Attempts received. Type: Counter | Int64
pres-unpub-atttx | Total number of “presence” Un-Publish Attempts transmitted. Type: Counter | Int64
pres-unpub-succrx | Total number of “presence” Un-Publish Successes received. Type: Counter | Int64
pres-unpub-succtx | Total number of “presence” Un-Publish Successes transmitted. Type: Counter | Int64
pres-unpub-failrx | Total number of “presence” Un-Publish Failures received. Type: Counter | Int64
pres-unpub-failtx | Total number of “presence” Un-Publish Failures transmitted. Type: Counter | Int64
pres-unpub-resp-3xxrx | Total number of “presence” Un-Publish 3XX Responses received. Type: Counter | Int64
pres-unpub-resp-3xxtx | Total number of “presence” Un-Publish 3XX Responses transmitted. Type: Counter | Int64
pres-unpub-resp-400rx | Total number of “presence” Un-Publish 400 Responses received. Type: Counter | Int64
pres-unpub-resp-400tx | Total number of “presence” Un-Publish 400 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-404rx | Total number of “presence” Un-Publish 404 Responses received. Type: Counter | Int64
pres-unpub-resp-404tx | Total number of “presence” Un-Publish 404 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-412rx | Total number of “presence” Un-Publish 412 Responses received. Type: Counter | Int64
pres-unpub-resp-412tx | Total number of “presence” Un-Publish 412 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-423rx | Total number of “presence” Un-Publish 423 Responses received. Type: Counter | Int64
pres-unpub-resp-423tx | Total number of “presence” Un-Publish 423 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-489rx | Total number of “presence” Un-Publish 489 Responses received. Type: Counter | Int64
pres-unpub-resp-489tx | Total number of “presence” Un-Publish 489 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-4xxrx | Total number of “presence” Un-Publish 4XX Responses received. Type: Counter | Int64
pres-unpub-resp-4xxtx | Total number of “presence” Un-Publish 4XX Responses transmitted. Type: Counter | Int64
pres-unpub-resp-500rx | Total number of “presence” Un-Publish 500 Responses received. Type: Counter | Int64
pres-unpub-resp-500tx | Total number of “presence” Un-Publish 500 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-503rx | Total number of “presence” Un-Publish 503 Responses received. Type: Counter | Int64
pres-unpub-resp-503tx | Total number of “presence” Un-Publish 503 Responses transmitted. Type: Counter | Int64
pres-unpub-resp-5xxrx | Total number of “presence” Un-Publish 5XX Responses received. Type: Counter | Int64
pres-unpub-resp-5xxtx | Total number of “presence” Un-Publish 5XX Responses transmitted. Type: Counter | Int64
pres-unpub-resp-6xxrx | Total number of “presence” Un-Publish 6XX Responses received. Type: Counter | Int64
pres-unpub-resp-6xxtx | Total number of “presence” Un-Publish 6XX Responses transmitted. Type: Counter | Int64
reg-subs-attrx | Total number of “reg” Subscription Attempts received. Type: Counter | Int64
reg-subs-atttx | Total number of “reg” Subscription Attempts transmitted. Type: Counter | Int64
reg-subs-succrx | Total number of “reg” Subscription Successes received. Type: Counter | Int64
reg-subs-succtx | Total number of “reg” Subscription Successes transmitted. Type: Counter | Int64
reg-subs-failrx | Total number of “reg” Subscription Failures received. Type: Counter | Int64
reg-subs-failtx | Total number of “reg” Subscription Failures transmitted. Type: Counter | Int64
reg-subs-resp-200rx | Total number of “reg” Subscription 200 Responses received. Type: Counter | Int64
reg-subs-resp-200tx | Total number of “reg” Subscription 200 Responses transmitted. Type: Counter | Int64
reg-subs-resp-202rx | Total number of “reg” Subscription 202 Responses received. Type: Counter | Int64
reg-subs-resp-202tx | Total number of “reg” Subscription 202 Responses transmitted. Type: Counter | Int64
reg-subs-resp-400rx | Total number of “reg” Subscription 400 Responses received. Type: Counter | Int64
reg-subs-resp-400tx | Total number of “reg” Subscription 400 Responses transmitted. Type: Counter | Int64
reg-subs-resp-403rx | Total number of “reg” Subscription 403 Responses received. Type: Counter | Int64
reg-subs-resp-403tx | Total number of “reg” Subscription 403 Responses transmitted. Type: Counter | Int64
reg-subs-resp-481rx | Total number of “reg” Subscription 481 Responses received. Type: Counter | Int64
reg-subs-resp-481tx | Total number of “reg” Subscription 481 Responses transmitted. Type: Counter | Int64
reg-subs-resp-489rx | Total number of “reg” Subscription 489 Responses received. Type: Counter | Int64
reg-subs-resp-489tx | Total number of “reg” Subscription 489 Responses transmitted. Type: Counter | Int64
reg-subs-resp-500rx | Total number of “reg” Subscription 500 Responses received. Type: Counter | Int64
reg-subs-resp-500tx | Total number of “reg” Subscription 500 Responses transmitted. Type: Counter | Int64
reg-subs-resp-3xxrx | Total number of “reg” Subscription 3XX Responses received. Type: Counter | Int64
reg-subs-resp-3xxtx | Total number of “reg” Subscription 3XX Responses transmitted. Type: Counter | Int64
reg-subs-resp-4xxrx | Total number of “reg” Subscription 4XX Responses received. Type: Counter | Int64
reg-subs-resp-4xxtx | Total number of “reg” Subscription 4XX Responses transmitted. Type: Counter | Int64
reg-subs-resp-5xxrx | Total number of “reg” Subscription 5XX Responses received. Type: Counter | Int64
reg-subs-resp-5xxtx | Total number of “reg” Subscription 5XX Responses transmitted. Type: Counter | Int64
reg-subs-resp-6xxrx | Total number of “reg” Subscription 6XX Responses received. Type: Counter | Int64
reg-subs-resp-6xxtx | Total number of “reg” Subscription 6XX Responses transmitted. Type: Counter | Int64
reg-resubs-attrx | Total number of “reg” Refresh Subscription Attempts received. Type: Counter | Int64
reg-resubs-atttx | Total number of “reg” Refresh Subscription Attempts transmitted. Type: Counter | Int64
reg-resubs-succrx | Total number of “reg” Refresh Subscription Successes received. Type: Counter | Int64
reg-resubs-succtx | Total number of “reg” Refresh Subscription Successes transmitted. Type: Counter | Int64
reg-resubs-failrx | Total number of “reg” Refresh Subscription Failures received. Type: Counter | Int64
reg-resubs-failtx | Total number of “reg” Refresh Subscription Failures transmitted. Type: Counter | Int64
reg-resubs-resp-200rx | Total number of “reg” Refresh Subscription 200 Responses received. Type: Counter | Int64
reg-resubs-resp-200tx | Total number of “reg” Refresh Subscription 200 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-202rx | Total number of “reg” Refresh Subscription 202 Responses received. Type: Counter | Int64
reg-resubs-resp-202tx | Total number of “reg” Refresh Subscription 202 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-400rx | Total number of “reg” Refresh Subscription 400 Responses received. Type: Counter | Int64
reg-resubs-resp-400tx | Total number of “reg” Refresh Subscription 400 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-403rx | Total number of “reg” Refresh Subscription 403 Responses received. Type: Counter | Int64
reg-resubs-resp-403tx | Total number of “reg” Refresh Subscription 403 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-481rx | Total number of “reg” Refresh Subscription 481 Responses received. Type: Counter | Int64
reg-resubs-resp-481tx | Total number of “reg” Refresh Subscription 481 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-489rx | Total number of “reg” Refresh Subscription 489 Responses received. Type: Counter | Int64
reg-resubs-resp-489tx | Total number of “reg” Refresh Subscription 489 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-500rx | Total number of “reg” Refresh Subscription 500 Responses received. Type: Counter | Int64
reg-resubs-resp-500tx | Total number of “reg” Refresh Subscription 500 Responses transmitted. Type: Counter | Int64
reg-resubs-resp-3xxrx | Total number of “reg” Refresh Subscription 3XX Responses received. Type: Counter | Int64
reg-resubs-resp-3xxtx | Total number of “reg” Refresh Subscription 3XX Responses transmitted. Type: Counter | Int64
reg-resubs-resp-4xxrx | Total number of “reg” Refresh Subscription 4XX Responses received. Type: Counter | Int64
reg-resubs-resp-4xxtx | Total number of “reg” Refresh Subscription 4XX Responses transmitted. Type: Counter | Int64
reg-resubs-resp-5xxrx | Total number of “reg” Refresh Subscription 5XX Responses received. Type: Counter | Int64
reg-resubs-resp-5xxtx | Total number of “reg” Refresh Subscription 5XX Responses transmitted. Type: Counter | Int64
reg-resubs-resp-6xxrx | Total number of “reg” Refresh Subscription 6XX Responses received. Type: Counter | Int64
reg-resubs-resp-6xxtx | Total number of “reg” Refresh Subscription 6XX Responses transmitted. Type: Counter | Int64
reg-unsubs-attrx | Total number of “reg” Un-Subscription Attempts received. Type: Counter | Int64
reg-unsubs-atttx | Total number of “reg” Un-Subscription Attempts transmitted. Type: Counter | Int64
reg-unsubs-succrx | Total number of “reg” Un-Subscription Successes received. Type: Counter | Int64
reg-unsubs-succtx | Total number of “reg” Un-Subscription Successes transmitted. Type: Counter | Int64
reg-unsubs-failrx | Total number of “reg” Un-Subscription Failures received. Type: Counter | Int64
reg-unsubs-failtx | Total number of “reg” Un-Subscription Failures transmitted. Type: Counter | Int64
reg-unsubs-resp-200rx | Total number of “reg” Un-Subscription 200 Responses received. Type: Counter | Int64
reg-unsubs-resp-200tx | Total number of “reg” Un-Subscription 200 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-202rx | Total number of “reg” Un-Subscription 202 Responses received. Type: Counter | Int64
reg-unsubs-resp-202tx | Total number of “reg” Un-Subscription 202 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-400rx | Total number of “reg” Un-Subscription 400 Responses received. Type: Counter | Int64
reg-unsubs-resp-400tx | Total number of “reg” Un-Subscription 400 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-403rx | Total number of “reg” Un-Subscription 403 Responses received. Type: Counter | Int64
reg-unsubs-resp-403tx | Total number of “reg” Un-Subscription 403 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-481rx | Total number of “reg” Un-Subscription 481 Responses received. Type: Counter | Int64
reg-unsubs-resp-481tx | Total number of “reg” Un-Subscription 481 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-489rx | Total number of “reg” Un-Subscription 489 Responses received. Type: Counter | Int64
reg-unsubs-resp-489tx | Total number of “reg” Un-Subscription 489 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-500rx | Total number of “reg” Un-Subscription 500 Responses received. Type: Counter | Int64
reg-unsubs-resp-500tx | Total number of “reg” Un-Subscription 500 Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-3xxrx | Total number of “reg” Un-Subscription 3XX Responses received. Type: Counter | Int64
reg-unsubs-resp-3xxtx | Total number of “reg” Un-Subscription 3XX Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-4xxrx | Total number of “reg” Un-Subscription 4XX Responses received. Type: Counter | Int64
reg-unsubs-resp-4xxtx | Total number of “reg” Un-Subscription 4XX Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-5xxrx | Total number of “reg” Un-Subscription 5XX Responses received. Type: Counter | Int64
reg-unsubs-resp-5xxtx | Total number of “reg” Un-Subscription 5XX Responses transmitted. Type: Counter | Int64
reg-unsubs-resp-6xxrx | Total number of “reg” Un-Subscription 6XX Responses received. Type: Counter | Int64
reg-unsubs-resp-6xxtx | Total number of “reg” Un-Subscription 6XX Responses transmitted. Type: Counter | Int64
reg-notify-attrx | Total number of “reg” Notify Attempts received. Type: Counter | Int64
reg-notify-atttx | Total number of “reg” Notify Attempts transmitted. Type: Counter | Int64
reg-notify-succrx | Total number of “reg” Notify Successes received. Type: Counter | Int64
reg-notify-succtx | Total number of “reg” Notify Successes transmitted. Type: Counter | Int64
reg-notify-failrx | Total number of “reg” Notify Failures received. Type: Counter | Int64
reg-notify-failtx | Total number of “reg” Notify Failures transmitted. Type: Counter | Int64
reg-notify-resp-3xxrx | Total number of “reg” Notify 3XX Responses received. Type: Counter | Int64
reg-notify-resp-3xxtx | Total number of “reg” Notify 3XX Responses transmitted. Type: Counter | Int64
reg-notify-resp-400rx | Total number of “reg” Notify 400 Responses received. Type: Counter | Int64
reg-notify-resp-400tx | Total number of “reg” Notify 400 Responses transmitted. Type: Counter | Int64
reg-notify-resp-481rx | Total number of “reg” Notify 481 Responses received. Type: Counter | Int64
reg-notify-resp-481tx | Total number of “reg” Notify 481 Responses transmitted. Type: Counter | Int64
reg-notify-resp-489rx | Total number of “reg” Notify 489 Responses received. Type: Counter | Int64
reg-notify-resp-489tx | Total number of “reg” Notify 489 Responses transmitted. Type: Counter | Int64
reg-notify-resp-4xxrx | Total number of “reg” Notify 4XX Responses received. Type: Counter | Int64
reg-notify-resp-4xxtx | Total number of “reg” Notify 4XX Responses transmitted. Type: Counter | Int64
reg-notify-resp-500rx | Total number of “reg” Notify 500 Responses received. Type: Counter | Int64
reg-notify-resp-500tx | Total number of “reg” Notify 500 Responses transmitted. Type: Counter | Int64
reg-notify-resp-5xxrx | Total number of “reg” Notify 5XX Responses received. Type: Counter | Int64
reg-notify-resp-5xxtx | Total number of “reg” Notify 5XX Responses transmitted. Type: Counter | Int64
reg-notify-resp-6xxrx | Total number of “reg” Notify 6XX Responses received. Type: Counter | Int64
reg-notify-resp-6xxtx | Total number of “reg” Notify 6XX Responses transmitted. Type: Counter | Int64
reg-pub-attrx | Total number of “reg” Publish Attempts received. Type: Counter | Int64
reg-pub-atttx | Total number of “reg” Publish Attempts transmitted. Type: Counter | Int64
reg-pub-succrx | Total number of “reg” Publish Successes received. Type: Counter | Int64
reg-pub-succtx | Total number of “reg” Publish Successes transmitted. Type: Counter | Int64
reg-pub-failrx | Total number of “reg” Publish Failures received. Type: Counter | Int64
reg-pub-failtx | Total number of “reg” Publish Failures transmitted. Type: Counter | Int64
reg-pub-resp-3xxrx | Total number of “reg” Publish 3XX Responses received. Type: Counter | Int64
reg-pub-resp-3xxtx | Total number of “reg” Publish 3XX Responses transmitted. Type: Counter | Int64
reg-pub-resp-400rx | Total number of “reg” Publish 400 Responses received. Type: Counter | Int64
reg-pub-resp-400tx | Total number of “reg” Publish 400 Responses transmitted. Type: Counter | Int64
reg-pub-resp-404rx | Total number of “reg” Publish 404 Responses received. Type: Counter | Int64
reg-pub-resp-404tx | Total number of “reg” Publish 404 Responses transmitted. Type: Counter | Int64
reg-pub-resp-412rx | Total number of “reg” Publish 412 Responses received. Type: Counter | Int64
reg-pub-resp-412tx | Total number of “reg” Publish 412 Responses transmitted. Type: Counter | Int64
reg-pub-resp-423rx | Total number of “reg” Publish 423 Responses received. Type: Counter | Int64
reg-pub-resp-423tx | Total number of “reg” Publish 423 Responses transmitted. Type: Counter | Int64
reg-pub-resp-489rx | Total number of “reg” Publish 489 Responses received. Type: Counter | Int64
reg-pub-resp-489tx | Total number of “reg” Publish 489 Responses transmitted. Type: Counter | Int64
reg-pub-resp-4xxrx | Total number of “reg” Publish 4XX Responses received. Type: Counter | Int64
reg-pub-resp-4xxtx | Total number of “reg” Publish 4XX Responses transmitted. Type: Counter | Int64
reg-pub-resp-500rx | Total number of “reg” Publish 500 Responses received. Type: Counter | Int64
reg-pub-resp-500tx | Total number of “reg” Publish 500 Responses transmitted. Type: Counter | Int64
reg-pub-resp-503rx | Total number of “reg” Publish 503 Responses received. Type: Counter | Int64
reg-pub-resp-503tx | Total number of “reg” Publish 503 Responses transmitted. Type: Counter | Int64
reg-pub-resp-5xxrx | Total number of “reg” Publish 5XX Responses received. Type: Counter | Int64
reg-pub-resp-5xxtx | Total number of “reg” Publish 5XX Responses transmitted. Type: Counter | Int64
reg-pub-resp-6xxrx | Total number of “reg” Publish 6XX Responses received. Type: Counter | Int64
reg-pub-resp-6xxtx | Total number of “reg” Publish 6XX Responses transmitted. Type: Counter | Int64
reg-unpub-attrx | Total number of “reg” Un-Publish Attempts received. Type: Counter | Int64
reg-unpub-atttx | Total number of “reg” Un-Publish Attempts transmitted. Type: Counter | Int64
reg-unpub-succrx | Total number of “reg” Un-Publish Successes received. Type: Counter | Int64
reg-unpub-succtx | Total number of “reg” Un-Publish Successes transmitted. Type: Counter | Int64
reg-unpub-failrx | Total number of “reg” Un-Publish Failures received. Type: Counter | Int64
reg-unpub-failtx | Total number of “reg” Un-Publish Failures transmitted. Type: Counter | Int64
reg-unpub-resp-3xxrx | Total number of “reg” Un-Publish 3XX Responses received. Type: Counter | Int64
reg-unpub-resp-3xxtx | Total number of “reg” Un-Publish 3XX Responses transmitted. Type: Counter | Int64
reg-unpub-resp-400rx | Total number of “reg” Un-Publish 400 Responses received. Type: Counter | Int64
reg-unpub-resp-400tx | Total number of “reg” Un-Publish 400 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-404rx | Total number of “reg” Un-Publish 404 Responses received. Type: Counter | Int64
reg-unpub-resp-404tx | Total number of “reg” Un-Publish 404 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-412rx | Total number of “reg” Un-Publish 412 Responses received. Type: Counter | Int64
reg-unpub-resp-412tx | Total number of “reg” Un-Publish 412 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-423rx | Total number of “reg” Un-Publish 423 Responses received. Type: Counter | Int64
reg-unpub-resp-423tx | Total number of “reg” Un-Publish 423 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-489rx | Total number of “reg” Un-Publish 489 Responses received. Type: Counter | Int64
reg-unpub-resp-489tx | Total number of “reg” Un-Publish 489 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-4xxrx | Total number of “reg” Un-Publish 4XX Responses received. Type: Counter | Int64
reg-unpub-resp-4xxtx | Total number of “reg” Un-Publish 4XX Responses transmitted. Type: Counter | Int64
reg-unpub-resp-500rx | Total number of “reg” Un-Publish 500 Responses received. Type: Counter | Int64
reg-unpub-resp-500tx | Total number of “reg” Un-Publish 500 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-503rx | Total number of “reg” Un-Publish 503 Responses received. Type: Counter | Int64
reg-unpub-resp-503tx | Total number of “reg” Un-Publish 503 Responses transmitted. Type: Counter | Int64
reg-unpub-resp-5xxrx | Total number of “reg” Un-Publish 5XX Responses received. Type: Counter | Int64
reg-unpub-resp-5xxtx | Total number of “reg” Un-Publish 5XX Responses transmitted. Type: Counter | Int64
reg-unpub-resp-6xxrx | Total number of “reg” Un-Publish 6XX Responses received. Type: Counter | Int64
reg-unpub-resp-6xxtx | Total number of “reg” Un-Publish 6XX Responses transmitted. Type: Counter | Int64
winfo-subs-attrx | Total number of “winfo” Subscription Attempts received. Type: Counter | Int64
winfo-subs-atttx | Total number of “winfo” Subscription Attempts transmitted. Type: Counter | Int64
winfo-subs-succrx | Total number of “winfo” Subscription Successes received. Type: Counter | Int64
winfo-subs-succtx | Total number of “winfo” Subscription Successes transmitted. Type: Counter | Int64
winfo-subs-failrx | Total number of “winfo” Subscription Failures received. Type: Counter | Int64
winfo-subs-failtx | Total number of “winfo” Subscription Failures transmitted. Type: Counter | Int64
winfo-subs-resp-200rx | Total number of “winfo” Subscription 200 Responses received. Type: Counter | Int64
winfo-subs-resp-200tx | Total number of “winfo” Subscription 200 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-202rx | Total number of “winfo” Subscription 202 Responses received. Type: Counter | Int64
winfo-subs-resp-202tx | Total number of “winfo” Subscription 202 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-400rx | Total number of “winfo” Subscription 400 Responses received. Type: Counter | Int64
winfo-subs-resp-400tx | Total number of “winfo” Subscription 400 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-403rx | Total number of “winfo” Subscription 403 Responses received. Type: Counter | Int64
winfo-subs-resp-403tx | Total number of “winfo” Subscription 403 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-481rx | Total number of “winfo” Subscription 481 Responses received. Type: Counter | Int64
winfo-subs-resp-481tx | Total number of “winfo” Subscription 481 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-489rx | Total number of “winfo” Subscription 489 Responses received. Type: Counter | Int64
winfo-subs-resp-489tx | Total number of “winfo” Subscription 489 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-500rx | Total number of “winfo” Subscription 500 Responses received. Type: Counter | Int64
winfo-subs-resp-500tx | Total number of “winfo” Subscription 500 Responses transmitted. Type: Counter | Int64
winfo-subs-resp-3xxrx | Total number of “winfo” Subscription 3XX Responses received. Type: Counter | Int64
winfo-subs-resp-3xxtx | Total number of “winfo” Subscription 3XX Responses transmitted. Type: Counter | Int64
winfo-subs-resp-4xxrx | Total number of “winfo” Subscription 4XX Responses received. Type: Counter | Int64
winfo-subs-resp-4xxtx | Total number of “winfo” Subscription 4XX Responses transmitted. Type: Counter | Int64
winfo-subs-resp-5xxrx | Total number of “winfo” Subscription 5XX Responses received. Type: Counter | Int64
winfo-subs-resp-5xxtx | Total number of “winfo” Subscription 5XX Responses transmitted. Type: Counter | Int64
winfo-subs-resp-6xxrx | Total number of “winfo” Subscription 6XX Responses received. Type: Counter | Int64
winfo-subs-resp-6xxtx | Total number of “winfo” Subscription 6XX Responses transmitted. Type: Counter | Int64
winfo-resubs-attrx | Total number of “winfo” Refresh Subscription Attempts received. Type: Counter | Int64
winfo-resubs-atttx | Total number of “winfo” Refresh Subscription Attempts transmitted. Type: Counter | Int64
winfo-resubs-succrx | Total number of “winfo” Refresh Subscription Successes received. Type: Counter | Int64
winfo-resubs-succtx | Total number of “winfo” Refresh Subscription Successes transmitted. Type: Counter | Int64
winfo-resubs-failrx | Total number of “winfo” Refresh Subscription Failures received. Type: Counter | Int64
winfo-resubs-failtx | Total number of “winfo” Refresh Subscription Failures transmitted. Type: Counter | Int64
winfo-resubs-resp-200rx | Total number of “winfo” Refresh Subscription 200 Responses received. Type: Counter | Int64
winfo-resubs-resp-200tx | Total number of “winfo” Refresh Subscription 200 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-202rx | Total number of “winfo” Refresh Subscription 202 Responses received. Type: Counter | Int64
winfo-resubs-resp-202tx | Total number of “winfo” Refresh Subscription 202 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-400rx | Total number of “winfo” Refresh Subscription 400 Responses received. Type: Counter | Int64
winfo-resubs-resp-400tx | Total number of “winfo” Refresh Subscription 400 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-403rx | Total number of “winfo” Refresh Subscription 403 Responses received. Type: Counter | Int64
winfo-resubs-resp-403tx | Total number of “winfo” Refresh Subscription 403 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-481rx | Total number of “winfo” Refresh Subscription 481 Responses received. Type: Counter | Int64
winfo-resubs-resp-481tx | Total number of “winfo” Refresh Subscription 481 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-489rx | Total number of “winfo” Refresh Subscription 489 Responses received. Type: Counter | Int64
winfo-resubs-resp-489tx | Total number of “winfo” Refresh Subscription 489 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-500rx | Total number of “winfo” Refresh Subscription 500 Responses received. Type: Counter | Int64
winfo-resubs-resp-500tx | Total number of “winfo” Refresh Subscription 500 Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-3xxrx | Total number of “winfo” Refresh Subscription 3XX Responses received. Type: Counter | Int64
winfo-resubs-resp-3xxtx | Total number of “winfo” Refresh Subscription 3XX Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-4xxrx | Total number of “winfo” Refresh Subscription 4XX Responses received. Type: Counter | Int64
winfo-resubs-resp-4xxtx | Total number of “winfo” Refresh Subscription 4XX Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-5xxrx | Total number of “winfo” Refresh Subscription 5XX Responses received. Type: Counter | Int64
winfo-resubs-resp-5xxtx | Total number of “winfo” Refresh Subscription 5XX Responses transmitted. Type: Counter | Int64
winfo-resubs-resp-6xxrx | Total number of “winfo” Refresh Subscription 6XX Responses received. Type: Counter | Int64
winfo-resubs-resp-6xxtx | Total number of “winfo” Refresh Subscription 6XX Responses transmitted. Type: Counter | Int64
winfo-unsubs-attrx | Total number of “winfo” Un-Subscription Attempts received. Type: Counter | Int64
winfo-unsubs-atttx | Total number of “winfo” Un-Subscription Attempts transmitted. Type: Counter | Int64
winfo-unsubs-succrx | Total number of “winfo” Un-Subscription Successes received. Type: Counter | Int64
winfo-unsubs-succtx | Total number of “winfo” Un-Subscription Successes transmitted. Type: Counter | Int64
winfo-unsubs-failrx | Total number of “winfo” Un-Subscription Failures received. Type: Counter | Int64
winfo-unsubs-failtx | Total number of “winfo” Un-Subscription Failures transmitted. Type: Counter | Int64
winfo-unsubs-resp-200rx | Total number of “winfo” Un-Subscription 200 Responses received. Type: Counter | Int64
winfo-unsubs-resp-200tx | Total number of “winfo” Un-Subscription 200 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-202rx | Total number of “winfo” Un-Subscription 202 Responses received. Type: Counter | Int64
winfo-unsubs-resp-202tx | Total number of “winfo” Un-Subscription 202 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-400rx | Total number of “winfo” Un-Subscription 400 Responses received. Type: Counter | Int64
winfo-unsubs-resp-400tx | Total number of “winfo” Un-Subscription 400 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-403rx | Total number of “winfo” Un-Subscription 403 Responses received. Type: Counter | Int64
winfo-unsubs-resp-403tx | Total number of “winfo” Un-Subscription 403 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-481rx | Total number of “winfo” Un-Subscription 481 Responses received. Type: Counter | Int64
winfo-unsubs-resp-481tx | Total number of “winfo” Un-Subscription 481 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-489rx | Total number of “winfo” Un-Subscription 489 Responses received. Type: Counter | Int64
winfo-unsubs-resp-489tx | Total number of “winfo” Un-Subscription 489 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-500rx | Total number of “winfo” Un-Subscription 500 Responses received. Type: Counter | Int64
winfo-unsubs-resp-500tx | Total number of “winfo” Un-Subscription 500 Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-3xxrx | Total number of “winfo” Un-Subscription 3XX Responses received. Type: Counter | Int64
winfo-unsubs-resp-3xxtx | Total number of “winfo” Un-Subscription 3XX Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-4xxrx | Total number of “winfo” Un-Subscription 4XX Responses received. Type: Counter | Int64
winfo-unsubs-resp-4xxtx | Total number of “winfo” Un-Subscription 4XX Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-5xxrx | Total number of “winfo” Un-Subscription 5XX Responses received. Type: Counter | Int64
winfo-unsubs-resp-5xxtx | Total number of “winfo” Un-Subscription 5XX Responses transmitted. Type: Counter | Int64
winfo-unsubs-resp-6xxrx | Total number of “winfo” Un-Subscription 6XX Responses received. Type: Counter | Int64
winfo-unsubs-resp-6xxtx | Total number of “winfo” Un-Subscription 6XX Responses transmitted. Type: Counter | Int64
winfo-notify-attrx | Total number of “winfo” Notify Attempts received. Type: Counter | Int64
winfo-notify-atttx | Total number of “winfo” Notify Attempts transmitted. Type: Counter | Int64
winfo-notify-succrx | Total number of “winfo” Notify Successes received. Type: Counter | Int64
winfo-notify-succtx | Total number of “winfo” Notify Successes transmitted. Type: Counter | Int64
winfo-notify-failrx | Total number of “winfo” Notify Failures received. Type: Counter | Int64
winfo-notify-failtx | Total number of “winfo” Notify Failures transmitted. Type: Counter | Int64
winfo-notify-resp-3xxrx | Total number of “winfo” Notify 3XX Responses received. Type: Counter | Int64
winfo-notify-resp-3xxtx | Total number of “winfo” Notify 3XX Responses transmitted. Type: Counter | Int64
winfo-notify-resp-400rx | Total number of “winfo” Notify 400 Responses received. Type: Counter | Int64
winfo-notify-resp-400tx | Total number of “winfo” Notify 400 Responses transmitted. Type: Counter | Int64
winfo-notify-resp-481rx | Total number of “winfo” Notify 481 Responses received. Type: Counter | Int64
winfo-notify-resp-481tx | Total number of “winfo” Notify 481 Responses transmitted. Type: Counter | Int64
winfo-notify-resp-489rx | Total number of “winfo” Notify 489 Responses received. Type: Counter | Int64
winfo-notify-resp-489tx | Total number of “winfo” Notify 489 Responses transmitted. Type: Counter | Int64
winfo-notify-resp-4xxrx | Total number of “winfo” Notify 4XX Responses received. Type: Counter | Int64
winfo-notify-resp-4xxtx | Total number of “winfo” Notify 4XX Responses transmitted. Type: Counter | Int64
winfo-notify-resp-500rx | Total number of “winfo” Notify 500 Responses received. Type: Counter | Int64
winfo-notify-resp-500tx | Total number of “winfo” Notify 500 Responses transmitted. Type: Counter | Int64
winfo-notify-resp-5xxrx | Total number of “winfo” Notify 5XX Responses received. Type: Counter | Int64
winfo-notify-resp-5xxtx | Total number of “winfo” Notify 5XX Responses transmitted. Type: Counter | Int64
winfo-notify-resp-6xxrx | Total number of “winfo” Notify 6XX Responses received. Type: Counter | Int64
winfo-notify-resp-6xxtx | Total number of “winfo” Notify 6XX Responses transmitted. Type: Counter | Int64
winfo-pub-attrx | Total number of “winfo” Publish Attempts received. Type: Counter | Int64
winfo-pub-atttx | Total number of “winfo” Publish Attempts transmitted. Type: Counter | Int64
winfo-pub-succrx | Total number of “winfo” Publish Successes received. Type: Counter | Int64
winfo-pub-succtx | Total number of “winfo” Publish Successes transmitted. Type: Counter | Int64
winfo-pub-failrx | Total number of “winfo” Publish Failures received. Type: Counter | Int64
winfo-pub-failtx | Total number of “winfo” Publish Failures transmitted. Type: Counter | Int64
winfo-pub-resp-3xxrx | Total number of “winfo” Publish 3XX Responses received. Type: Counter | Int64
winfo-pub-resp-3xxtx | Total number of “winfo” Publish 3XX Responses transmitted. Type: Counter | Int64
winfo-pub-resp-400rx | Total number of “winfo” Publish 400 Responses received. Type: Counter | Int64
winfo-pub-resp-400tx | Total number of “winfo” Publish 400 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-404rx | Total number of “winfo” Publish 404 Responses received. Type: Counter | Int64
winfo-pub-resp-404tx | Total number of “winfo” Publish 404 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-412rx | Total number of “winfo” Publish 412 Responses received. Type: Counter | Int64
winfo-pub-resp-412tx | Total number of “winfo” Publish 412 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-423rx | Total number of “winfo” Publish 423 Responses received. Type: Counter | Int64
winfo-pub-resp-423tx | Total number of “winfo” Publish 423 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-489rx | Total number of “winfo” Publish 489 Responses received. Type: Counter | Int64
winfo-pub-resp-489tx | Total number of “winfo” Publish 489 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-4xxrx | Total number of “winfo” Publish 4XX Responses received. Type: Counter | Int64
winfo-pub-resp-4xxtx | Total number of “winfo” Publish 4XX Responses transmitted. Type: Counter | Int64
winfo-pub-resp-500rx | Total number of “winfo” Publish 500 Responses received. Type: Counter | Int64
winfo-pub-resp-500tx | Total number of “winfo” Publish 500 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-503rx | Total number of “winfo” Publish 503 Responses received. Type: Counter | Int64
winfo-pub-resp-503tx | Total number of “winfo” Publish 503 Responses transmitted. Type: Counter | Int64
winfo-pub-resp-5xxrx | Total number of “winfo” Publish 5XX Responses received. Type: Counter | Int64
winfo-pub-resp-5xxtx | Total number of “winfo” Publish 5XX Responses transmitted. Type: Counter | Int64
winfo-pub-resp-6xxrx | Total number of “winfo” Publish 6XX Responses received. Type: Counter | Int64
winfo-pub-resp-6xxtx | Total number of “winfo” Publish 6XX Responses transmitted. Type: Counter | Int64
winfo-unpub-attrx | Total number of “winfo” Un-Publish Attempts received. Type: Counter | Int64
winfo-unpub-atttx | Total number of “winfo” Un-Publish Attempts transmitted. Type: Counter | Int64
winfo-unpub-succrx | Total number of “winfo” Un-Publish Successes received. Type: Counter | Int64
winfo-unpub-succtx | Total number of “winfo” Un-Publish Successes transmitted. Type: Counter | Int64
winfo-unpub-failrx | Total number of “winfo” Un-Publish Failures received. Type: Counter | Int64
winfo-unpub-failtx | Total number of “winfo” Un-Publish Failures transmitted. Type: Counter | Int64
winfo-unpub-resp-3xxrx | Total number of “winfo” Un-Publish 3XX Responses received. Type: Counter | Int64
winfo-unpub-resp-3xxtx | Total number of “winfo” Un-Publish 3XX Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-400rx | Total number of “winfo” Un-Publish 400 Responses received. Type: Counter | Int64
winfo-unpub-resp-400tx | Total number of “winfo” Un-Publish 400 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-404rx | Total number of “winfo” Un-Publish 404 Responses received. Type: Counter | Int64
winfo-unpub-resp-404tx | Total number of “winfo” Un-Publish 404 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-412rx | Total number of “winfo” Un-Publish 412 Responses received. Type: Counter | Int64
winfo-unpub-resp-412tx | Total number of “winfo” Un-Publish 412 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-423rx | Total number of “winfo” Un-Publish 423 Responses received. Type: Counter | Int64
winfo-unpub-resp-423tx | Total number of “winfo” Un-Publish 423 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-489rx | Total number of “winfo” Un-Publish 489 Responses received. Type: Counter | Int64
winfo-unpub-resp-489tx | Total number of “winfo” Un-Publish 489 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-4xxrx | Total number of “winfo” Un-Publish 4XX Responses received. Type: Counter | Int64
winfo-unpub-resp-4xxtx | Total number of “winfo” Un-Publish 4XX Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-500rx | Total number of “winfo” Un-Publish 500 Responses received. Type: Counter | Int64
winfo-unpub-resp-500tx | Total number of “winfo” Un-Publish 500 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-503rx | Total number of “winfo” Un-Publish 503 Responses received. Type: Counter | Int64
winfo-unpub-resp-503tx | Total number of “winfo” Un-Publish 503 Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-5xxrx | Total number of “winfo” Un-Publish 5XX Responses received. Type: Counter | Int64
winfo-unpub-resp-5xxtx | Total number of “winfo” Un-Publish 5XX Responses transmitted. Type: Counter | Int64
winfo-unpub-resp-6xxrx | Total number of “winfo” Un-Publish 6XX Responses received. Type: Counter | Int64
winfo-unpub-resp-6xxtx | Total number of “winfo” Un-Publish 6XX Responses transmitted. Type: Counter | Int64
message-attrx | Total number of Message attempts received. Type: Counter | Int32
message-atttx | Total number of Message attempts transmitted. Type: Counter | Int32
message-succrx | Total number of Message success received. Type: Counter | Int32
message-succtx | Total number of Message success transmitted. Type: Counter | Int32
message-failrx | Total number of Message failures received. Type: Counter | Int32
message-failtx | Total number of Message failures transmitted. Type: Counter | Int32
message-3xx-rx | Total number of Message 3xx Responses received. Type: Counter | Int32
message-3xx-tx | Total number of Message 3xx Responses transmitted. Type: Counter | Int32
message-400-rx | Total number of Message 400 Responses received. Type: Counter | Int32
message-400-tx | Total number of Message 400 Responses transmitted. Type: Counter | Int32
message-403-rx | Total number of Message 403 Responses received. Type: Counter | Int32
message-403-tx | Total number of Message 403 Responses transmitted. Type: Counter | Int32
message-404-rx | Total number of Message 404 Responses received. Type: Counter | Int32
message-404-tx | Total number of Message 404 Responses transmitted. Type: Counter | Int32
message-413-rx | Total number of Message 413 Responses received. Type: Counter | Int32
message-413-tx | Total number of Message 413 Responses transmitted. Type: Counter | Int32
message-415-rx | Total number of Message 415 Responses received. Type: Counter | Int32
message-415-tx | Total number of Message 415 Responses transmitted. Type: Counter | Int32
message-416-rx | Total number of Message 416 Responses received. Type: Counter | Int32
message-416-tx | Total number of Message 416 Responses transmitted. Type: Counter | Int32
message-420-rx | Total number of Message 420 Responses received. Type: Counter | Int32
message-420-tx | Total number of Message 420 Responses transmitted. Type: Counter | Int32
message-421-rx | Total number of Message 421 Response received. Type: Counter | Int32
message-421-tx | Total number of Message 421 Responses transmitted. Type: Counter | Int32
message-480-rx | Total number of Message 480 Responses received. Type: Counter | Int32
message-480-tx | Total number of Message 480 Responses transmitted. Type: Counter | Int32
message-488-rx | Total number of Message 488 Responses received. Type: Counter | Int32
message-488-tx | Total number of Message 488 Responses transmitted. Type: Counter | Int32
message-4xx-rx | Total number of Message 4xx Responses received. Type: Counter | Int32
message-4xx-tx | Total number of Message 4xx Responses transmitted. Type: Counter | Int32
message-500-rx | Total number of Message 500 Responses received. Type: Counter | Int32
message-500-tx | Total number of Message 500 Responses transmitted. Type: Counter | Int32
message-513-rx | Total number of Message 513 Responses received. Type: Counter | Int32
message-513-tx | Total number of Message 513 Responses transmitted. Type: Counter | Int32
message-5xx-rx | Total number of Message 5xx Responses received. Type: Counter | Int32
message-5xx-tx | Total number of Message 5xx Responses transmitted. Type: Counter | Int32
message-6xx-rx | Total number of Message 6xx Responses received. Type: Counter | Int32
message-6xx-tx | Total number of Total Message 6xx Responses transmitted. Type: Counter | Int32
callrejpdf | Total number of Call Rejects from PDF. Type: Counter | Int64
callrejloc | Total number of Call Rejects from Proxy (local). Type: Counter | Int64
sesstimeexp | Total number of Session Timer Expires. Type: Counter | Int64
hssacc | Total number of HSS Accesses. Type: Counter | Int64
emergcalls | Total number of Emergency Calls. Type: Counter | Int64
emerg-priv-calls | Total number of User-requested Privacy Calls. Applicable only for E-CSCF. Type: Counter | Int64
tollfreecalls | Total number of Toll Free Calls. Type: Counter | Int64
premservcalls | Total number of Premium Service Calls. Type: Counter | Int64
internationalcalls | Total number of International Calls. Type: Counter | Int64
longDistancecalls | Total number of Long Distance Calls. Type: Counter | Int64
opassistcalls | Total number of Operator Assisted Calls. Type: Counter | Int64
dirassistcalls | Total number of Directory Assisted Calls. Type: Counter | Int64
largerthansipmaxsize | Total number of Too Large SIP Messages. Type: Counter | Int64
rtp-sent | Total number of RTP packets sent. Type: Counter | Int64
rtcp-sent | Total number of RTCP packets sent. Type: Counter | Int64
rtp-recv | Total number of RTP packets received. Type: Counter | Int64
msrp-sent | Total number of MSRP TCP packets sent. Type: Counter | Int64
msrp-recv | Total number of MSRP TCP packets received. Type: Counter | Int64
callrel-from-ue | Total number of Call Releases initiated by UE. Type: Counter | Int64
callrel-from-nw | Total number of Call Releases initiated by Network. Type: Counter | Int64
callrel-from-radioloss | Total number of Call Releases initiated by Radio Loss. Type: Counter | Int64
callrel-from-local | Total number of Call Releases initiated by CSCF (Local). Type: Counter | Int64
sigcomp-req-comp | Total number of Requests Compressed. Type: Counter | Int64
sigcomp-req-decomp | Total number of Requests Decompressed. Type: Counter | Int64
sigcomp-resp-comp | Total number of Responses Compressed. Type: Counter | Int64
sigcomp-resp-decomp | Total number of Responses Decompressed. Type: Counter | Int64
sigcomp-nack-rx | Total number of NACK Packets received. Type: Counter | Int64
sigcomp-nack-tx | Total number of NACK Packets transmitted. Type: Counter | Int64
sigcomp-comp-fail | Total number of Compression Failures. Type: Counter | Int64
sigcomp-decomp-fail | Total number of Decompression Failures. Type: Counter | Int64
sigcomp-bestout-compratio | Best Outgoing Message Compression Ratio Type: Gauge | Float
sigcomp-worstout-compratio | Worst Outgoing Message Compression Ratio Type: Gauge | Float
sigcomp-bestin-compratio | Best Incoming Message Compression Ratio Type: Gauge | Float
sigcomp-worstin-compratio | Worst Incoming Message Compression Ratio Type: Gauge | Float
sigcomp-averagein- compratio | Average Incoming Message Compression Ratio Type: Gauge | Float
sigcomp-averageout- compratio | Average Outgoing Message Compression Ratio Type: Gauge | Float
min-invite-proc-time | Minimum Invite Process Time Type: Gauge | Int32
max-invite-proc-time | Maximum Invite Process Timer Type: Gauge | Int32
min-first-resp-time | Minimum First Response Time Type: Gauge | Int32
max-first-resp-time | Maximum First Response Time Type: Gauge | Int32
min-post-dial-delay | Minimum Post-Dial Delay Type: Gauge | Int32
max-post-dial-delay | Maximum Post-Dial Delay Type: Gauge | Int32
min-session-setup-delay | Minimum Session Setup Delay Type: Gauge | Int32
max-session-setup-delay | Maximum Session Setup Delay Type: Gauge | Int32
min-post-answer-delay | Minimum Post Answer Delay Type: Gauge | Int32
max-post-answer-delay | Maximum Post Answer Delay Type: Gauge | Int32
min-session-rel-delay | Minimum Session Release Delay Type: Gauge | Int32
max-session-rel-delay | Maximum Session Release Delay Type: Gauge | Int32
active-tcp-conn | Total number of Active TCP connections. Type: Gauge | Int64
closed-tcp-conn | Total number of Closed TCP connections. Type: Counter | Int64
succ-tcp-conn-out | Total number of Successful Outgoing connections. Type: Counter | Int64
fail-tcp-conn-out | Total number of Failed Outgoing connections. Type: Counter | Int64
succ-tcp-conn-in | Total number of Successful Incoming connections. Type: Counter | Int64
fail-tcp-conn-in | Total number of Failed Incoming connections. Type: Counter | Int64
migrated-tcp-conn | Total number of TCP connections migrated from Cscfmgr to Sessmgr for load balancing. Type: Counter | Int64
packet-tcp-rx | Total number of TCP/IP packets received by CSCF service. Type: Counter | Int64
packet-tcp-tx | Total number of TCP/IP packets transmitted by CSCF service. Type: Counter | Int64
bytes-tcp-rx | Total number of TCP/IP bytes received by CSCF service. Type: Counter | Int64
bytes-tcp-tx | Total number of TCP/IP bytes transmitted by CSCF service. Type: Counter | Int64
message-tcp-request-rx | Total number of TCP requests received over TCP. Type: Counter | Int64
message-tcp-request-tx | Total number of TCP requests transmitted over TCP. Type: Counter | Int64
message-tcp-response-rx | Total number of TCP responses received over TCP. Type: Counter | Int64
message-tcp-response-tx | Total number of TCP responses transmitted over TCP. Type: Counter | Int64
message-tcp-mtu-switch | Total number of times CSCF switched from UDP to TCP because of message size larger than MTU. Type: Counter | Int64
sip-tcp-subs | Total number of subscribers using TCP for SIP. Type: Gauge | Int64
msrp-active-tcp-conn | Total number of active MSRP TCP connections. Type: Counter | Int64
msrp-closed-tcp-conn | Total number of closed MSRP TCP connections. Type: Counter | Int64
msrp-succ-tcp-conn-out | Total number of outgoing MSRP TCP connections established successfully. Type: Counter | Int64
msrp-fail-tcp-conn-out | Total number of failed outgoing MSRP TCP connections. Type: Counter | Int64
msrp-succ-tcp-conn-in | Total number of incoming MSRP TCP connections established successfully. Type: Counter | Int64
msrp-fail-tcp-conn-in | Total number of failed incoming MSRP TCP connections. Type: Counter | Int64
msrp-packet-rx | Total number of MSRP packets received. Type: Counter | Int64
msrp-packet-tx | Total number of MSRP packets transmitted. Type: Counter | Int64
msrp-bytes-rx | Total number of MSRP bytes received. Type: Counter | Int64
msrp-bytes-tx | Total number of MSRP bytes transmitted. Type: Counter | Int64
msrp-tcp-subs | Total number of subscribers with TCP connection for MSRP. Type: Gauge | Int64
reg-rejdueto-secagree | Total number of Registration Rejects due to Security Agreement Type: Counter | Int64
reg-rejdueto-algomismatch | Total number of Registration Rejects due to Algorithm Mismatch Type: Counter | Int64
msg-drops-duetoerror | Total number of Message drops due to error. Type: Counter | Int64
sec-rereg | Total number of Secure re-registrations Type: Counter | Int64
sec-dereg | Total number of Secure de-registrations Type: Counter | Int64
msgs-withincorr-sec-verify | Total number of Messages with Incorrect security Verify Type: Counter | Int64
sec-assoc-rejects | Total number of Security Associations rejected. Type: Counter | Int64
sub-with-sec-conn | Total number of Subscribers with secure connections. Type: Gauge | Int32
sub-with-unsec-conn | Total number of Subscribers with unsecure connections. Type: Gauge | Int32
ipsec-pktrx | Total number of IP-Sec Packets received. Type: Counter | Int64
ipsec-pkttx | Total number of IP-Sec Packets transmitted. Type: Counter | Int64
ipsec-octrx | Total number of IP-Sec Octets received. Type: Counter | Int64
ipsec-octtx | Total number of IP-Sec Octets transmitted. Type: Counter | Int64
active-ipsec-tcp-conn | Total number of Active IPSec TCP connections Type: Gauge | Int64
closed-ipsec-tcp-conn | Total number of Closed IPSec TCP connections Type: Counter | Int64
succ-ipsec-tcp-conn-out | Total number of Successful IPSec Outgoing connections Type: Counter | Int64
fail-ipsec-tcp-conn-out | Total number of Failed IPSec Outgoing connections Type: Counter | Int64
succ-ipsec-tcp-conn-in | Total number of Successful IPSec Incoming connections Type: Counter | Int64
fail-ipsec-tcp-conn-in | Total number of Failed IPSec Incoming connections Type: Counter | Int64
regreqrx | Total number of Register requests received. Type: Counter | Int64
regreqtx | Total number of Register requests transmitted. Type: Counter | Int64
invreqrx | Total number of Invite requests received. Type: Counter | Int64
invreqtx | Total number of Invite requests transmitted. Type: Counter | Int64
ackreqrx | Total number of ACK requests received. Type: Counter | Int64
ackreqtx | Total number of ACK requests transmitted. Type: Counter | Int64
byereqrx | Total number of Bye requests received. Type: Counter | Int64
byereqtx | Total number of Bye requests transmitted. Type: Counter | Int64
cancreqrx | Total number of Cancel requests received. Type: Counter | Int64
cancreqtx | Total number of Cancel requests transmitted. Type: Counter | Int64
optreqrx | Total number of Options requests received. Type: Counter | Int64
optreqtx | Total number of Options requests transmitted. Type: Counter | Int64
prackreqrx | Total number of PRACK requests received. Type: Counter | Int64
prackreqtx | Total number of PRACK requests transmitted. Type: Counter | Int64
subreqrx | Total number of Subscribe requests received. Type: Counter | Int64
subreqtx | Total number of Subscribe requests transmitted. Type: Counter | Int64
notreqrx | Total number of Notify requests received. Type: Counter | Int64
notreqtx | Total number of Notify requests transmitted. Type: Counter | Int64
refreqrx | Total number of Refer requests received. Type: Counter | Int64
refreqtx | Total number of Refer requests transmitted. Type: Counter | Int64
inforeqrx | Total number of Info requests received. Type: Counter | Int64
inforeqtx | Total number of Info requests transmitted. Type: Counter | Int64
updreqrx | Total number of Update requests received. Type: Counter | Int64
updreqtx | Total number of Update requests transmitted. Type: Counter | Int64
msgreqrx | Total number of Message requests received. Type: Counter | Int64
msgreqtx | Total number of Message requests transmitted. Type: Counter | Int64
pubreqrx | Total number of Publish requests received. Type: Counter | Int64
pubreqtx | Total number of Publish requests transmitted. Type: Counter | Int64
tryrsprx | Total number of Trying responses received. Type: Counter | Int64
tryrsptx | Total number of Trying responses transmitted. Type: Counter | Int64
rngrsprx | Total number of Ringing responses received. Type: Counter | Int64
rngrsptx | Total number of Ringing responses transmitted. Type: Counter | Int64
fwdrsprx | Total number of Forwarded responses received. Type: Counter | Int64
fwdrsptx | Total number of Forwarded responses transmitted. Type: Counter | Int64
quersprx | Total number of Queued responses received. Type: Counter | Int64
quersptx | Total number of Queued responses transmitted. Type: Counter | Int64
prgrsprx | Total number of Progress responses received. Type: Counter | Int64
prgrsptx | Total number of Progress responses transmitted. Type: Counter | Int64
200-regrsprx | Total number of 200OK Register responses received. Type: Counter | Int64
200-regrsptx | Total number of 200OK Register responses transmitted. Type: Counter | Int64
200-invrsprx | Total number of 200OK Invite responses received. Type: Counter | Int64
200-invrsptx | Total number of 200OK Invite responses transmitted. Type: Counter | Int64
200-byersprx | Total number of 200OK Bye responses received. Type: Counter | Int64
200-byersptx | Total number of 200OK Bye responses transmitted. Type: Counter | Int64
200-cnlrsprx | Total number of 200OK Cancel responses received. Type: Counter | Int64
200-cnlrsptx | Total number of 200OK Cancel responses transmitted. Type: Counter | Int64
200-optrsprx | Total number of 200OK Options responses received. Type: Counter | Int64
200-optrsptx | Total number of 200OK Options responses transmitted. Type: Counter | Int64
200-prackrsprx | Total number of 200OK PRACK responses received. Type: Counter | Int64
200-prackrsptx | Total number of 200OK PRACK responses transmitted. Type: Counter | Int64
200-subrsprx | Total number of 200OK Subscribe responses received. Type: Counter | Int64
200-subrsptx | Total number of 200OK Subscribe responses transmitted. Type: Counter | Int64
200-notrsprx | Total number of 200OK Notify responses received. Type: Counter | Int64
200-notrsptx | Total number of 200OK Notify responses transmitted. Type: Counter | Int64
200-infrsprx | Total number of 200OK Info responses received. Type: Counter | Int64
200-infrsptx | Total number of 200OK Info responses transmitted. Type: Counter | Int64
200-updrsprx | Total number of 200OK Update responses received. Type: Counter | Int64
200-updrsptx | Total number of 200OK Update responses transmitted. Type: Counter | Int64
200-pubrsprx | Total number of 200OK Publish responses received. Type: Counter | Int64
200-pubrsptx | Total number of 200OK Publish responses transmitted. Type: Counter | Int64
200-refrsprx | Total number of 200OK Refer responses received. Type: Counter | Int64
200-refrsptx | Total number of 200OK Refer responses transmitted. Type: Counter | Int64
200-msgrsprx | Total number of 200OK Message responses received. Type: Counter | Int64
200-msgrsptx | Total number of 200OK Message responses transmitted. Type: Counter | Int64
202-refrsprx | Total number of 202Accepted Refer responses received. Type: Counter | Int64
202-refrsptx | Total number of 202Accepted Refer responses transmitted. Type: Counter | Int64
202-subrsprx | Total number of 202Accepted Subscribe responses received. Type: Counter | Int64
202-subrsptx | Total number of 202Accepted Subscribe responses transmitted. Type: Counter | Int64
mchrsprx | Total number of Multiple Choices responses received. Type: Counter | Int64
mchrsptx | Total number of Multiple Choices responses transmitted. Type: Counter | Int64
mpersprx | Total number of Moved Permanently responses received. Type: Counter | Int64
mpersptx | Total number of Moved Permanently responses transmitted. Type: Counter | Int64
mtersprx | Total number of Moved Temporarily responses received. Type: Counter | Int64
mtersptx | Total number of Moved Temporarily responses transmitted. Type: Counter | Int64
upxrsprx | Total number of Use Proxy responses received. Type: Counter | Int64
upxrsptx | Total number of Use Proxy responses transmitted. Type: Counter | Int64
altrsprx | Total number of Alternative Service responses received. Type: Counter | Int64
altrsptx | Total number of Alternative Service responses transmitted. Type: Counter | Int64
brqerrrx | Total number of BadRequest errors received. Type: Counter | Int64
brqerrtx | Total number of BadRequest errors transmitted. Type: Counter | Int64
uauerrrx | Total number of UnAuthorized errors received. Type: Counter | Int64
uauerrtx | Total number of UnAuthorized errors transmitted. Type: Counter | Int64
prerrrx | Total number of Payment Required Errors received. Type: Counter | Int64
prerrtx | Total number of Payment Required Errors transmitted. Type: Counter | Int64
forerrrx | Total number of Forbidden errors received. Type: Counter | Int64
forerrtx | Total number of Forbidden errors transmitted. Type: Counter | Int64
nfderrrx | Total number of NotFound errors received. Type: Counter | Int64
nfderrtx | Total number of NotFound errors transmitted. Type: Counter | Int64
mnaerrrx | Total number of MethodNotAllowed errors received. Type: Counter | Int64
mnaerrtx | Total number of MethodNotAllowed errors transmitted. Type: Counter | Int64
nac406errrx | Total number of NotAcceptable(406) errors received. Type: Counter | Int64
nac406errtx | Total number of NotAcceptable(406) errors transmitted. Type: Counter | Int64
parerrrx | Total number of ProxyAuthRequired errors received. Type: Counter | Int64
parerrtx | Total number of ProxyAuthRequired errors transmitted. Type: Counter | Int64
rtoerrrx | Total number of RequestTimeout errors received. Type: Counter | Int64
rtoerrtx | Total number of RequestTimeout errors transmitted. Type: Counter | Int64
conferrrx | Total number of Conflict Errors received. Type: Counter | Int64
conferrtx | Total number of Conflict Errors transmitted. Type: Counter | Int64
lrerrrx | Total number of Length Required Errors received. Type: Counter | Int64
lrerrtx | Total number of Length Required Errors transmitted. Type: Counter | Int64
gonerrrx | Total number of Gone errors received. Type: Counter | Int64
gonerrtx | Total number of Gone errors transmitted. Type: Counter | Int64
crferrrx | Total number of ConditionalRequestFail errors received. Type: Counter | Int64
crferrtx | Total number of ConditionalRequestFail errors transmitted. Type: Counter | Int64
relerrrx | Total number of RequestEntityTooLarge errors received. Type: Counter | Int64
relerrtx | Total number of RequestEntityTooLarge errors transmitted. Type: Counter | Int64
rulerrrx | Total number of RequestURITooLong errors received. Type: Counter | Int64
rulerrtx | Total number of RequestURITooLong errors transmitted. Type: Counter | Int64
umterrrx | Total number of UnsupportedMediaType errors received. Type: Counter | Int64
umterrtx | Total number of UnsupportedMediaType errors transmitted. Type: Counter | Int64
uuserrrx | Total number of Unsupported URI Scheme errors received. Type: Counter | Int64
uuserrtx | Total number of Unsupported URI Scheme errors transmitted. Type: Counter | Int64
bexerrrx | Total number of BadExtension errors received. Type: Counter | Int64
bexerrtx | Total number of BadExtension errors transmitted. Type: Counter | Int64
exrerrrx | Total number of Extension Required errors received. Type: Counter | Int64
exrerrtx | Total number of Extension Required errors transmitted. Type: Counter | Int64
sitserrrx | Total number of Session Interval Too Small errors received Type: Counter | Int64
sitserrtx | Total number of Session Interval Too Small errors transmitted Type: Counter | Int64
fhloerrrx | Total number of First Hop Lacks Outbound Support (439) errors received. Type: Counter | Int64
fhloerrtx | Total number of First Hop Lacks Outbound Support (439) errors transmitted. Type: Counter | Int64
itberrrx | Total number of Interval Too Brief errors received. Type: Counter | Int64
itberrtx | Total number of Interval Too Brief errors transmitted. Type: Counter | Int64
blierrrx | Total number of Bad Location Information errors received. Type: Counter | Int64
blierrtx | Total number of Bad Location Information errors transmitted. Type: Counter | Int64
tnaerrrx | Total number of TempNotAvailable errors received. Type: Counter | Int64
tnaerrtx | Total number of TempNotAvailable errors transmitted. Type: Counter | Int64
tdnerrrx | Total number of Transaction Does Not Exist errors received. Type: Counter | Int64
tdnerrtx | Total number of Transaction Does Not Exist errors transmitted. Type: Counter | Int64
ldterrrx | Total number of LoopDetected errors received. Type: Counter | Int64
ldterrtx | Total number of LoopDetected errors transmitted. Type: Counter | Int64
tmherrrx | Total number of TooManyHops errors received. Type: Counter | Int64
tmherrtx | Total number of TooManyHops errors transmitted. Type: Counter | Int64
adierrrx | Total number of AddrIncomplete errors received. Type: Counter | Int64
adierrtx | Total number of AddrIncomplete errors transmitted. Type: Counter | Int64
amberrrx | Total number of Ambiguous errors received. Type: Counter | Int64
amberrtx | Total number of Ambiguous errors transmitted. Type: Counter | Int64
bhrerrrx | Total number of BusyHere errors received. Type: Counter | Int64
bhrerrtx | Total number of BusyHere errors transmitted. Type: Counter | Int64
rqcerrrx | Total number of RequestCancel errors received. Type: Counter | Int64
rqcerrtx | Total number of RequestCancel errors transmitted. Type: Counter | Int64
namerrrx | Total number of NotAcceptableMedia errors received. Type: Counter | Int64
namerrtx | Total number of NotAcceptableMedia errors transmitted. Type: Counter | Int64
beerrrx | Total number of Bad Event errors received. Type: Counter | Int64
beerrtx | Total number of Bad Event errors transmitted. Type: Counter | Int64
trperrrx | Total number of Request Pending errors received. Type: Counter | Int64
trperrtx | Total number of Request Pending errors transmitted. Type: Counter | Int64
udperrrx | Total number of Undecipherable errors received. Type: Counter | Int64
udperrtx | Total number of Undecipherable errors transmitted. Type: Counter | Int64
sarerrrx | Total number of sec-agree Required Errors received. Type: Counter | Int64
sarerrtx | Total number of Sec-agree Required Errors transmitted. Type: Counter | Int64
ineerrrx | Total number of InternalError errors received. Type: Counter | Int64
ineerrtx | Total number of InternalError errors transmitted. Type: Counter | Int64
nimerrrx | Total number of NotImplemented errors received. Type: Counter | Int64
nimerrtx | Total number of NotImplemented errors transmitted. Type: Counter | Int64
bgterrrx | Total number of BadGateway errors received. Type: Counter | Int64
bgterrtx | Total number of BadGateway errors transmitted. Type: Counter | Int64
suaerrrx | Total number of ServiceUnavailable errors received. Type: Counter | Int64
suaerrtx | Total number of ServiceUnavailable errors transmitted. Type: Counter | Int64
gtterrrx | Total number of GatewayTimeout errors received. Type: Counter | Int64
gtterrtx | Total number of GatewayTimeout errors transmitted. Type: Counter | Int64
bsverrrx | Total number of BadSipVersion errors received. Type: Counter | Int64
bsverrtx | Total number of BadSipVersion errors transmitted. Type: Counter | Int64
mtlerrrx | Total number of Message Too Large errors received. Type: Counter | Int64
mtlerrtx | Total number of Message Too Large errors transmitted. Type: Counter | Int64
pcferrrx | Total number of Precondition Failure errors received. Type: Counter | Int64
pcferrtx | Total number of Precondition Failure errors transmitted. Type: Counter | Int64
bewerrrx | Total BusyEverywhere errors received. Total number of Type: Counter | Int64
bewerrtx | Total number of BusyEverywhere errors transmitted. Type: Counter | Int64
decerrrx | Total number of Decline errors received. Type: Counter | Int64
decerrtx | Total number of Decline errors transmitted. Type: Counter | Int64
neaerrrx | Total number of NotExistAnywhere errors received. Type: Counter | Int64
neaerrtx | Total number of NotExistAnywhere errors transmitted. Type: Counter | Int64
nac606errrx | Total number of NotAcceptable(606) errors received. Type: Counter | Int64
nac606errtx | Total number of NotAcceptable(606) errors transmitted. Type: Counter | Int64
callsetuptime | Sum of setup times – For calculating average call setup time. Type: Counter | Int64
callscounted | Total number of calls, for which setup time is added in setup times. Type: Counter | Int64
tot-sip-invalid-msgs-rx | Total number of SIP Invalid Messages received. Type: Counter | Int64
tot-sip-msgs-rx | Total number of SIP Messages received. Type: Counter | Int64
tot-sip-msgs-tx | Total number of SIP Messages transmitted. Type: Counter | Int64
tot-sip-msgs-proc | Total number of SIP Messages Processed. Type: Counter | Int64
regreqretx | Total number of REGISTER Requests Re-transmitted. Type: Counter | Int64
invreqretx | Total number of INVITE Requests Re-transmitted. Type: Counter | Int64
byereqretx | Total number of BYE Requests Re-transmitted. Type: Counter | Int64
cancreqretx | Total number of CANCEL Requests Re-transmitted. Type: Counter | Int64
ackreqretx | Total number of ACK Requests Re-transmitted. Type: Counter | Int64
notifyreqretx | Total number of NOTIFY Requests Re-transmitted. Type: Counter | Int64
publishreqretx | Total number of PUBLISH Requests Re-transmitted. Type: Counter | Int64
referreqretx | Total number of REFER Requests Re-transmitted. Type: Counter | Int64
subscribereqretx | Total number of SUBSCRIBE Requests Re-transmitted. Type: Counter | Int64
req-retx | Total number of SIP Requests Re-transmitted. Type: Counter | Int64
resp-retx | Total number of SIP Responses Re-transmitted. Type: Counter | Int64
reqresp-retx | Total number of SIP messages Re-transmitted. Type: Counter | Int64
calldur-lt-01sec | Total calls with duration less than 01 sec. Type: Counter | Int32
calldur-01to10sec | Total calls with duration between 01 and 10 seconds. Type: Counter | Int32
calldur-10to30sec | Total calls with duration between 10 and 30 seconds. Type: Counter | Int32
calldur-30to60sec | Total calls with duration between 30 and 60 seconds. Type: Counter | Int32
calldur-60to90sec | Total calls with duration between 60 and 90 seconds. Type: Counter | Int32
calldur-90to120sec | Total calls with duration between 90 and 120 seconds. Type: Counter | Int32
calldur-120to150sec | Total calls with duration between 120 and 150 seconds. Type: Counter | Int32
calldur-150to180sec | Total calls with duration between 150 and 180 seconds. Type: Counter | Int32
calldur-03to04min | Total calls with duration between 03 and 04 minutes. Type: Counter | Int32
calldur-04to05min | Total calls with duration between 04 and 05 minutes. Type: Counter | Int32
calldur-05to06min | Total calls with duration between 05 and 06 minutes. Type: Counter | Int32
calldur-06to07min | Total calls with duration between 06 and 07 minutes. Type: Counter | Int32
calldur-07to08min | Total calls with duration between 07 and 08 minutes. Type: Counter | Int32
calldur-08to09min | Total calls with duration between 08 and 09 minutes. Type: Counter | Int32
calldur-09to11min | Total calls with duration between 09 and 11 minutes. Type: Counter | Int32
calldur-11to13min | Total calls with duration between 11 and 13 minutes. Type: Counter | Int32
calldur-13to15min | Total calls with duration between 13 and 15 minutes. Type: Counter | Int32
calldur-15to17min | Total calls with duration between 15 and 17 minutes. Type: Counter | Int32
calldur-17to19min | Total calls with duration between 17 and 19 minutes. Type: Counter | Int32
calldur-19to21min | Total calls with duration between 19 and 21 minutes. Type: Counter | Int32
calldur-21to23min | Total calls with duration between 21 and 23 minutes. Type: Counter | Int32
calldur-23to25min | Total calls with duration between 23 and 25 minutes. Type: Counter | Int32
calldur-25to27min | Total calls with duration between 25 and 27 minutes. Type: Counter | Int32
calldur-27to29min | Total calls with duration between 27 and 29 minutes. Type: Counter | Int32
calldur-29to60min | Total calls with duration between 29 and 60 minutes. Type: Counter | Int32
calldur-gt-60min | Total calls with duration more than 60 minutes. Type: Counter | Int32
subsetup<200ms | Total number of subscriptions setup in less than 200 milliseconds. Type: Counter | Int32
subsetup200-400ms | Total number of subscriptions setup in 200 to 400 milliseconds. Type: Counter | Int32
subsetup400-600ms | Total number of subscriptions setup in 400 to 600 milliseconds. Type: Counter | Int32
subsetup600-800ms | Total number of subscriptions setup in 600 to 800 milliseconds. Type: Counter | Int32
subsetup800-1000ms | Total number of subscriptions setup in 800 to 1000 milliseconds. Type: Counter | Int32
subsetup1000-1200ms | Total number of subscriptions setup in 1000 to 1200 milliseconds. Type: Counter | Int32
subsetup1200-1400ms | Total number of subscriptions setup in 1200 to 1400 milliseconds. Type: Counter | Int32
subsetup1400-1600ms | Total number of subscriptions setup in 1400 to 1600 milliseconds. Type: Counter | Int32
subsetup1600-1800ms | Total number of subscriptions setup in 1600 to 1800 milliseconds. Type: Counter | Int32
subsetup1800-2000ms | Total number of subscriptions setup in 1800 to 2000 milliseconds. Type: Counter | Int32
subsetup2000-2200ms | Total number of subscriptions setup in 2000 to 2200 milliseconds. Type: Counter | Int32
subsetup2200-2400ms | Total number of subscriptions setup in 2200 to 2400 milliseconds. Type: Counter | Int32
subsetup2400-2600ms | Total number of subscriptions setup in 2400 to 2600 milliseconds. Type: Counter | Int32
subsetup2600-2800ms | Total number of subscriptions setup in 2600 to 2800 milliseconds. Type: Counter | Int32
subsetup2800-3000ms | Total number of subscriptions setup in 2800 to 3000 milliseconds. Type: Counter | Int32
subsetup3-5sec | Total number of subscriptions setup in 3 to 5 seconds. Type: Counter | Int32
subsetup5-7sec | Total number of subscriptions setup in 5 to 7 seconds. Type: Counter | Int32
subsetup7-9sec | Total number of subscriptions setup in 7 to 9 seconds. Type: Counter | Int32
subsetup9-11sec | Total number of subscriptions setup in 9 to 11 seconds. Type: Counter | Int32
subsetup11-13sec | Total number of subscriptions setup in 11 to 13 seconds. Type: Counter | Int32
subsetup13-15sec | Total number of subscriptions setup in 13 to 15 seconds. Type: Counter | Int32
subsetup15-17sec | Total number of subscriptions setup in 15 to 17 seconds. Type: Counter | Int32
subsetup17-19sec | Total number of subscriptions setup in 17 to 19 seconds. Type: Counter | Int32
subsetup19-21sec | Total number of subscriptions setup in 19 to 21 seconds. Type: Counter | Int32
subsetup>21sec | Total number of subscriptions setup in more than 21 seconds. Type: Counter | Int32
subdur<1hr | Total number of subscription duration less than 1 hour. Type: Counter | Int32
subdur1-2hr | Total number of subscription duration 1 to 2 hours. Type: Counter | Int32
subdur2-3hr | Total number of subscription duration 2 to 3 hours. Type: Counter | Int32
subdur3-4hr | Total number of subscription duration 3 to 4 hours. Type: Counter | Int32
subdur4-5hr | Total number of subscription duration 4 to 5 hours. Type: Counter | Int32
subdur5-6hr | Total number of subscription duration 5 to 6 hours. Type: Counter | Int32
subdur6-7hr | Total number of subscription duration 6 to 7 hours. Type: Counter | Int32
subdur7-8hr | Total number of subscription duration 7 to 8 hours. Type: Counter | Int32
subdur8-9hr | Total number of subscription duration 8 to 9 hours. Type: Counter | Int32
subdur9-10hr | Total number of subscription duration 9 to 10 hours. Type: Counter | Int32
subdur>10hr | Total number of subscription duration more than 10 hours. Type: Counter | Int32
curr-reg-subs | Total number of currently registered users. Type: Gauge | Int64
active-reg-subs | Total number of active registered users. Type: Gauge | Int64
curr-sigcomp-subs | Total number of currently registered SIGCOMP users. Type: Gauge | Int64
active-sigcomp-subs | Total number of active registered SIGCOMP users. Type: Gauge | Int64
curr-ipsec-subs | Total number of currently registered IPSEC users. Type: Gauge | Int64
active-ipsec-subs | Total number of active registered IPSEC users. Type: Gauge | Int64
active-voip-subs | Active registered VOIP users. Type: Gauge | Int64
curr-presence-subs | Total number of currently registered PRESENCE users. Type: Gauge | Int64
active-presence-subs | Total number of active registered PRESENCE users. Type: Gauge | Int64
active-im-subs | Total number of active registered IM users. Type: Gauge | Int64
dpeca-curr-sessions | The total number of DPECA sessions currently active. Type: Gauge | Int32
dpeca-tot-sess-init | Total number of DPECA sessions initiated by sending AAR Initial Request message. Type: Counter | Int32
dpeca-tot-sess-terminated | Total number of terminated DPECA sessions. Type: Counter | Int32
dpeca-tot-sess-failovers | Total number of peer-switches attempted. Type: Counter | Int32
dpeca-tot-sess-failover-err | Total number of peer-switches failed. Type: Counter | Int32
dpeca-tot-msg-received | Total number of messages received. Type: Counter | Int32
dpeca-tot-msg-sent | Total number of messages sent. Type: Counter | Int32
dpeca-tot-aar-sent | Total number of AAR request messages sent from DPECA module. Type: Counter | Int32
dpeca-tot-aaa-received | Total number of AAA answer messages received. Type: Counter | Int32
dpeca-tot-uncorr-aaa | Total number of Uncorrelated AAA messages. Type: Counter | Int32
dpeca-tot-uncorr-sta | Total number of Uncorrelated STA messages. Type: Counter | Int32
dpeca-tot-aari-sent | Total number of AAR Initial requests sent. Type: Counter | Int32
dpeca-tot-aaai-received | Total number of AAA answer messages received in response to the AAR-Initial requests. Type: Counter | Int32
dpeca-tot-aaai-accepted | Total number of AAA messages accepted as successful without any errors. Type: Counter | Int32
dpeca-tot-aaai-rejected | Total number of AAA messages rejected as erroneous. Type: Counter | Int32
dpeca-tot-aaai-timeout | Total number of AAA answers to Initial request timed out. Type: Counter | Int32
dpeca-tot-aaru-sent | Total number of AAR Update messages sent Type: Counter | Int32
dpeca-tot-aaau-received | Total number of AAA answer messages received in response to the AAR-Update requests. Type: Counter | Int32
dpeca-tot-aaau-timeout | Total number of AAA answers to Update request timed out. Type: Counter | Int32
dpeca-tot-str-sent | Total number of STR messages sent. Type: Counter | Int32
dpeca-tot-sta-received | Total number of STA messages received. Type: Counter | Int32
dpeca-tot-sta-timeout | Total number of STA answers timed out. Type: Counter | Int32
dpeca-tot-asr-received | Total number of ASR messages received. Type: Counter | Int32
dpeca-tot-asa-sent | Total number of ASA messages sent. Type: Counter | Int32
dpeca-tot-rar-received | Total number of RAR messages received. Type: Counter | Int32
dpeca-tot-raa-sent | Total number of RAA messages sent. Type: Counter | Int32
dpeca-tot-protocol-err | Total number of diameter protocol errors that were received from PCRF. Type: Counter | Int32
dpeca-tot-aaa-parse-err | Total number of AAA parse-errors. Type: Counter | Int32
dpeca-tot-unk-sess-req | Total number of unknown session requests. Type: Counter | Int32
dpeca-tot-unk-cmd-codes | Total number of unknown command codes (unsupported command codes). Type: Counter | Int32
dpeca-tc-logout | Total number of sessions terminated as the user logged out. Type: Counter | Int32
dpeca-tc-service-not-prov | Total number of sessions terminated as the requested service is not provided. Type: Counter | Int32
dpeca-tc-bad-ans | Total number of sessions terminated with a bad answer. Type: Counter | Int32
dpeca-tc-administrative | Total number of sessions terminated administratively. Type: Counter | Int32
dpeca-tc-link-broken | Total number of sessions terminated due to link broken. Type: Counter | Int32
dpeca-tc-auth-expired | Total number of sessions terminated due to auth-expiry. Type: Counter | Int32
dpeca-tc-user-moved | Total number of sessions terminated as the user-moved. Type: Counter | Int32
dpeca-tc-session-timeout | Total number of sessions terminated due to session timeout. Type: Counter | Int32
dpeca-auth-rejected | Total number of authorization rejected errors. Type: Counter | Int32
dpeca-other-errors | Total number of other miscellaneous DPECA errors. Type: Counter | Int32
dpeca-exp-res-invalid- service-info | Total number of answer messages received with Experimental-Result-Code as 5061 - INVALID_SERVICE_INFORMATION. Type: Counter | Int32
dpeca-exp-res-filter- restrictions | Total number of answer messages received with Experimental-Result-Code as 5062 - FILTER_RESTRICTIONS. Type: Counter | Int32
dpeca-exp-res-req-service- not-authorized | Total number of answer messages received with Experimental-Result-Code as 5063 - REQUESTED_SERVICE_NOT_AUTHORIZED. Type: Counter | Int32
dpeca-exp-res-duplicated-af-session | Total number of answer messages received with Experimental-Result-Code as 5064 - DUPLICATED_AF_SESSION. Type: Counter | Int32
dpeca-exp-res-ipcan-session-not-avail | Total number of answer messages received with Experimental-Result-Code as 5065 - IP_CAN_SESSION_NOT_AVAILABLE Type: Counter | Int32
perf-att-init-reg | Total number of initial registrations received at CSCF. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-att-init-reg-3gpp-geran | Total number of initial registrations received at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-init-reg-3gpp-utran- fdd | Total number of initial registrations received at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-init-reg-3gpp2-1x | Total number of initial registrations received at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-init-reg-ieee-80211a | Total number of initial registrations received at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-init-reg-ieee-80211b | Total number of initial registrations received at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-init-reg-other-at | Total number of initial registrations received at CSCF for any other access technology. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-init-reg | Total number of success responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-succ-init-reg-3gpp- geran | Total number of success responses sent for initial registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-init-reg-3gpp-utran-fdd | Total number of success responses sent for initial registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-init-reg-3gpp2-1x | Total number of success responses sent for initial registration with access technology 3GPP2-1X. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-init-reg-ieee- 80211a | Total number of success responses sent for initial registration with access technology IEEE-802.11a. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-init-reg-ieee- 80211b | Total number of success responses sent for initial registration with access technology IEEE-802.11b. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-init-reg-other | Total number of success responses sent for initial registration for any other access technologies. Applicable only for P-CSCF. Type: Counter | Int64
perf-fail-init-reg | Total number of failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-init-reg-401 | Total number of (401 Unauthorized) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-init-reg-403 | Total number of (403 Forbidden) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-init-reg-404 | Total number of (404 Not Found) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-init-reg-420 | Total number of (420 Bad Extension) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-init-reg-500 | Total number of (500 Internal Error) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-init-reg-other | Total number of other failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-mean-init-reg-setup | Average time (in milliseconds) between the instance REGISTER is received by P-CSCF and 200 response is sent for the REGISTER. The average is reset every 10 minutes. Applicable only for P-CSCF. Type: Gauge | Int32
perf-att-rereg | Total number of refresh registrations received at CSCF. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-att-rereg-3gpp-geran | Total number of refresh registrations received at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-rereg-3gpp-utran-fdd | Total number of refresh registrations received at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-rereg-3gpp2-1x | Total number of refresh registrations received at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-rereg-ieee-80211a | Total number of refresh registrations received at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-rereg-ieee-80211b | Total number of refresh registrations received at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-rereg-other-at | Total number of refresh registrations received at CSCF for any other access technology. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-rereg | Total number of success responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-succ-rereg-3gpp-geran | Total number of success responses sent for refresh registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-rereg-3gpp-utran- fdd | Total number of success responses sent for refresh registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-rereg-3gpp2-1x | Total number of success responses sent for refresh registration with access technology 3GPP2-1X. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-rereg-ieee-80211a | Total number of success responses sent for refresh registration with access technology IEEE-802.11a. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-rereg-ieee-80211b | Total number of success responses sent for refresh registration with access technology IEEE-802.11b. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-rereg-other | Total number of success responses sent for refresh registration for any other access technology. Applicable only for P-CSCF. Type: Counter | Int64
perf-fail-rereg | Total number of failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF Type: Counter | Int64
perf-fail-rereg-401 | Total number of (401 Unauthorized) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-rereg-403 | Total number of (403 Forbidden) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-rereg-404 | Total number of (404 Not Found) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-rereg-420 | Total number of (420 Bad Extension) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-rereg-500 | Total number of (500 Internal Error) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-rereg-other | Total number of other failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-att-dereg-ue | Total number of de-registrations received from UE at CSCF. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-att-dereg-ue-3gpp- geran | Total number of de-registrations received from UE at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-dereg-ue-3gpp-utran-fdd | Total number of de-registrations received from UE at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-dereg-ue-3gpp2-1x | Total number of de-registrations received from UE at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-dereg-ue-ieee- 80211a | Total number of de-registrations received from UE at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-dereg-ue-ieee- 80211b | Total number of de-registrations received from UE at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. Type: Counter | Int64
perf-att-dereg-ue-other-at | Total number of de-registrations received from UE at CSCF for any other access technology. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-dereg-ue | Total number of success responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-succ-dereg-ue-3gpp- geran | Total number of success responses sent for de-registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-dereg-ue-3gpp- utran-fdd | Total number of success responses sent for de-registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-dereg-ue- 3gpp2-1x | Total number of success responses sent for de-registration with access technology 3GPP2-1X. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-dereg-ue-ieee- 80211a | Total number of success responses sent for de-registration with access technology IEEE-802.11a. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-dereg-ue-ieee- 80211b | Total number of success responses sent for de-registration with access technology IEEE-802.11b. Applicable only for P-CSCF. Type: Counter | Int64
perf-succ-dereg-ue-other | Total number of success responses sent for de-registration for any other access technology. Applicable only for P-CSCF. Type: Counter | Int64
perf-fail-dereg-ue | Total number of failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF Type: Counter | Int64
perf-fail-dereg-ue-401 | Total number of (401 Unauthorized) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-dereg-ue-403 | Total number of (403 Forbidden) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-dereg-ue-404 | Total number of (404 Not Found) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-dereg-ue-420 | Total number of (420 Bad Extension) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-dereg-ue-500 | Total number of (500 Internal Error) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-fail-dereg-ue-other | Total number of other failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. Type: Counter | Int64
perf-att-dereg-hss | Total number of de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-dereg-hss | Total number of success responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss | Total number of failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss-401 | Total number of (401 Unauthorized) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss-403 | Total number of (403 Forbidden) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss-404 | Total number of (404 Not Found) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss-420 | Total number of (420 Bad Extension) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss-500 | Total number of (500 Internal Error) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-hss-other | Total number of other failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-dereg-serv | Total number of de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-dereg-serv | Total number of success responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv | Total number of failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv-401 | Total number of (401 Unauthorized) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv-403 | Total number of (403 Forbidden) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv-404 | Total number of (404 Not Found) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv-420 | Total number of (420 Bad Extension) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv-500 | Total number of (500 Internal Error) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-dereg-serv-other | Total number of other failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-3rdparty-reg | Total number of 3rd Party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-3rdparty-reg | Total number of success responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg | Total number of failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg-401 | Total number of (401 Unauthorized) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg-403 | Total number of (403 Forbidden) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg-404 | Total number of (404 Not Found) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg-420 | Total number of (420 Bad Extension) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg-500 | Total number of (500 Internal Error) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-3rdparty-reg-other | Total number of other failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-uar | Total number of user registration status query procedures attempted at I-CSCF. Applicable only for I-CSCF. Type: Counter | Int64
perf-succ-uaa | Total number of success response for user registration status queries attempted at I-CSCF. Applicable only for I-CSCF. Type: Counter | Int64
perf-fail-uaa | Total number of failure response for user registration status queries attempted at I-CSCF. Applicable only for I-CSCF. Type: Counter | Int64
perf-att-sar | Total number of S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-saa | Total number of success responses for S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-saa | Total number of failure responses for S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-session | Total number of attempted session establishments at CSCF. Type: Counter | Int64
perf-succ-session-180 | Total number of 180 responses for successful session establishments at CSCF. Type: Counter | Int64
perf-succ-session-200 | Total number of 200 responses (without 180 response) for successful session establishments at CSCF. Type: Counter | Int64
perf-ans-session | Total number of 200 responses for session establishments at CSCF. Type: Counter | Int64
perf-fail-session | Total number of failure responses for session establishments at CSCF. Type: Counter | Int64
perf-att-lir | Total number of user location query procedures attempted at I-CSCF. Applicable only for I-CSCF. Type: Counter | Int64
perf-succ-lia | Total number of success responses for user location queries attempted at I-CSCF. Applicable only for I-CSCF. Type: Counter | Int64
perf-fail-lia | Total number of failure responses for user location queries attempted at I-CSCF. Applicable only for I-CSCF. Type: Counter | Int64
perf-att-session-frm-oth- domain | Total number of session establishments from users of other domains. Applicable only for I-CSCF & S-CSCF. Type: Counter | Int64
perf-frbdn-session-frm-oth- domain | Total number of forbidden sessions for session establishments from users of other domains. Applicable only for I-CSCF & S-CSCF. Type: Counter | Int64
perf-att-session-to-oth-domain | Total number of session establishments to users of other domains. Applicable only for I-CSCF & S-CSCF. Type: Counter | Int64
perf-frbdn-session-to-oth-domain | Total number of forbidden sessions for session establishments to users of other domains. Applicable only for I-CSCF & S-CSCF. Type: Counter | Int64
perf-att-init-reg-visited | Total number of initial registrations of visiting users from other IMS network domains. Applicable only for P-CSCF. Type: Counter | Int64
perf-frbdn-init-reg-visited | Total number of forbidden messages sent for the visiting users. Applicable only for P-CSCF. Type: Counter | Int64
perf-rmg-users-out | Total number of roaming users to other network domains. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-mar | Total number of Multimedia-Authentication-Requests attempted. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-maa | Total number of successful Multimedia-Authentication-Answers received. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-maa | Total number of failure Multimedia-Authentication-Answers received. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-ppr | Total number of HSS-initiated user profile updates attempted. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-ppa | Total number of success responses for HSS-initiated user profile update. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-ppa | Total number of failure responses for HSS-initiated user profile update. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-subscribe | Total number of subscription procedures attempted at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-subscribe | Total number of success responses for subscriptions. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-subscribe | Total number of failure responses for subscriptions. Applicable only for S-CSCF. Type: Counter | Int64
perf-att-notify | Total number of notify procedures attempted at S-CSCF. Applicable only for S-CSCF. Type: Counter | Int64
perf-succ-notify | Total number of success responses for notify. Applicable only for S-CSCF. Type: Counter | Int64
perf-fail-notify | Total number of failure responses for notify. Applicable only for S-CSCF. Type: Counter | Int64
de2a-session-init | Total number of DE2A sessions initiated by sending UDR message. Type: Counter | Int32
de2a-session-active | Total number of DE2A sessions currently active. Type: Counter | Int32
de2a-udr-sent | Total number UDR messages sent. Type: Counter | Int32
de2a-uda-received | Total number of UDA messages received Type: Counter | Int32
de2a-uda-err-3xxx | Total number of messages with protocol errors. Type: Counter | Int32
de2a-uda-parse-err | Total number of bad UDA messages received. Type: Counter | Int32
de2a-udr-err | Total number of UDR send errors. Type: Counter | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.