# show gtpu-service

This chapter includes the show gtpu-service command output tables.
show gtpu-service all
Table 1. show gtpu-service all Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the service configured in the named context.
Context | The name of the context where the service is configured.
State | The status of the service, i.e., “Initiated”.
Echo Interval | The duration between the sending of GTP-U echo messages.
Include UDP Port Ext.Hdr | Indicates if an extension header, in the GTP-U packet header, allowing for error indication messages will be added.
Max-retransmissions | The number of user data packet request message retransmissions that can be sent before an error condition is established.
Retransmission Timeout | The number of seconds between the re-sending of GTP-U echo messages
IPSEC Tunnel Idle Timeout | The number of seconds an IPSec tunnel is idle before tunnel deletion is triggered.
Allow Error-Indication | Indicates if the error indication will be allowed or suppressed upon the receipt of a user data packet for a non-existent session.
Address List | Identifies the IP address used to transmit/receive GTP-U packets.
Path Failure Detection on gtp echo msgs | Identifies if the path failure detection is enabled upon reaching the maximum number of echo retransmissions.