# CSCF URN List Configuration Mode Commands

The CSCF URN List Configuration Mode is used to map URNs to URIs for emergency and local call services.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
cscf-urn-service-mapping

Adds an entry to the service URN mapping table that maps uniform resource names (URNs) to URIs in order to direct specific service-oriented identifiers to the proper location in a network. The table is used after CSCF translation if the result is a local service.
Platform:

ASR 5000
Product:

SCM
Privilege:

Administrator
Syntax

    [ no ] cscf-urn-service-mapping
    urn urn uri uri

no

Removes an entry from the service URN mapping table.
urn urn

Specifies the URN to be routed via a URL to the appropriate destination. urn must be from 1 to 79 alpha and/or numeric characters.
uri uri

Specifies the URI used to route the URN to the appropriate location. uri must be from 1 to 79 alpha and/or numeric characters.
Usage:

Use this command to add an entry to the service URN mapping table that routes a translated URN to a URI for local services.

IMPORTANT:

Service URN mapping tables are limited to 30 URN to URI mapping entries.
Example:
The following command map URN business to URI corp@123.45.678.9:5020 and adds it to the service URN mapping table:

    cscf-urn-service-mapping
    urn business uri corp@123.45.678.9:5020

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.