# ASN RAN Peer Map Configuration Mode Commands

Use the RAN Peer Map Configuration Mode to create and manage global mapping tables of Radio Access Network base station peers.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
ran-peer

Configure the MAC and IP addresses of the base station peers you are adding to this map.
Platform:

ASR 5000
Product:

ASN-GW
Privilege:

Administrator
Syntax

    [ no ] ran-peer
    id mac_address address ip_address [mode{non-legacy | legacy}]

no

Removes the base station peer entry from this map.
id mac_address address ip_address

id mac_address: Configures the MAC address of the base station peer in this map.

mac_address must be in one of the following formats:

nn:nn:nn:nn:nn:nn or nn-nn-nn-nn-nn-nn

address ip_address: Specifies the IP address of the base station peer in IPv4 dotted-decimal or IPv6 colon-separated notation.

mode {non-legacy | legacy}: Default mode is non-legacy.
Usage:

Use this command to add base station peers to this peer map.
Example:
The following command adds a base station peer to this map:

    ran-peer id 00:05:47:00:37:44
    address 12.345.76.789