# show mipha

This chapter includes the show mipha command output tables.
show mipha statistics ha-service
Table 1. show mipha statistics ha-service Command Output Descriptions

Field | Description
--- | ---
HA Service | The name of the HA service for which the statistics are displayed.
MIP AAA Authentication
Attempts | The number of authentication attempts by the HA including those that are authenticated locally.
Success | The number of authentication attempts completed successfully by the HA including those that are authenticated locally.
Total Failures | The total number of failed AAA authentication attempts that were facilitated.
Actual Auth Failures | The total number of AAA authentication attempts that were rejected by the AAA server.
Misc Auth Failures | The total number of miscellaneous authorization failures.
Registration Request Received
Total Received Reg | The total number of registration requests received.
Total Accepted Reg | The total number of registration requests accepted.
Total Denied Reg | The total number of registration requests that were denied.
Total Discarded Reg | The total number of registration requests that were discarded.
Congestion Discarded Reg | The total number of requests discarded when congestion control is enabled and the system is in a congested state.
Initial Reg Requests
Received | The total number of initial registration requests received.
Accepted | The total number of initial registration requests accepted.
Denied | The total number of initial registration requests denied.
Renew Reg Requests
Received | The total number of renewal registration requests received.
Accepted | The total number of renewal registration requests accepted.
Denied | The total number of renewal registration requests denied.
DeReg Requests
Received | The total number of requests for de-registration received.
Accepted | The total number of requests for de-registration accepted.
Denied | The total number of requests for de-registration denied.
Registration Reply Sent
Total | The total number of registration replies sent.
Accepted Reg | The total number of successful registration replies sent.
Accepted DeReg | The total number of successful de-registration replies sent.
Denied | The total number of denied registration replies sent.
Bad Request | The total number of denied registration replies that were sent with a reply code of 86H (Registration Denied - poorly formed request).
Mismatched ID | The total number of denied registration replies that were sent with a reply code of 85H (Registration Denied - registration identification mismatch).
MN Auth Failure | The total number of denied registration replies that were sent with a reply code of 83H (Registration Denied - mobile node failed authentication).
FA Auth Failure | The total number of denied registration replies that were sent with a reply code of 84H (Registration Denied - home agent failed authentication).
Admin Prohibited | The total number of denied registration replies that were sent with a reply code of 81H (Registration Denied - administratively prohibited).
No Resources | The total number of denied registration replies that were sent with a reply code of 82H (Registration Denied - insufficient resources).
Simul Bindings Exceeded | The total number of denied registration replies that were sent with a reply code of 87H (Registration Denied - too many simultaneous mobility bindings).
Unknown HA | The total number of denied registration replies that were sent with a reply code of 88H (Registration Denied - unknown home agent address).
Rev Tunnel Unavailable | The total number of denied registration replies that were sent with a reply code of 89H (Registration Denied - reverse tunneling unavailable).
Rev Tunnel Mandatory | The total number of denied registration replies that were sent with a reply code of 8AH (Registration Denied - reverse tunneling mandatory).
Encap Unavailable | The total number of denied registration replies that were sent with a reply code of 8BH (Registration Denied - reverse tunneling encapsulation style unavailable).
Send Error | The total number of errors that occurred while sending replies.
Handoff Requests
Received | The total number of handoff request received by HA for an existing session.
Accepted | The total number of handoff request accepted by HA.
Denied | The total number of handoff request denied by HA.
Unspecified Reason | The total number of denied registration replies that were sent with a reply code of 80H (Registration Denied - reason unspecified).
Unknown CVSE Rcvd | The total number of messages discarded because of an FA reply code of 100 (Critical Vendor Specific Extension Received).
UDP Encap Unavailable | Indicates registration denial caused by unavailable (minimal or GRE) UDP tunnel encapsulation modes.
RRQ Denied Overload/Congestion Control
Admin Prohibited(reject) | The number of RRQs rejected when congestion control is enabled and the system is in a congested state.
Unknown HA (redirect) | The number of RRQs redirected to an alternate HA when congestion control is enabled and the system is in a congested state.
Registration Revocation |
Sent | Total registration revocation messages sent to the FA.
Retries Sent | Total registration revocation messages re-sent to the FA.
Ack Rcvd | Total registration revocation request acknowledgements received from the FA.
Not Acknowledged | Total registration revocation request messages that timed-out before an acknowledgement was received from the FA.
Rcvd | Total registration revocation request messages received from the FA.
Ack Sent | Total registration revocation request acknowledgements sent to the FA.
P-AAA Messages:
BC Query Requests:
Received | The total number of Binding Cache requests received from the proxy-AAA server.
Accepted | The total number of Binding Cache requests received from the proxy-AAA server that were accepted.
Denied | The total number of Binding Cache requests from the proxy-AAA server that were denied.
BC Query Responses:
Sent | The total number of Binding Cache responses that were sent to the proxy-AAA server.
BC Found | The total number of Binding Cache responses that were sent to the proxy-AAA server that indicated that the requested binding context was found.
BC Not Found | The total number of Binding Cache responses that were sent to the proxy-AAA server that indicated that the requested binding context was not found.
IP Pool Overflow | The total number of Binding Cache responses that were sent to the proxy-AAA server that indicated that there is an IP Pool overflow condition for the requested binding context.
Miscellaneous | The total number of Binding Cache responses that were sent to the proxy-AAA server that indicated other miscellaneous errors for the requested binding context.
HA-IPSEC Tunnels
Requests Received | The total number of HA-IPSEC tunnel session requests received.
Initiated | The total number of HA-IPSEC session requests received and initiated.
Denied | The total number of HA-IPSEC session requests received and denied.
Discarded | The total number of HA-IPSEC sessions initiated and discarded.
Connected | The total number of HA-IPSEC sessions initiated and connected.
Failed | The total number of HA-IPSEC sessions initiated, connected and failed.
Tunnel Data Received
Total Packets | Total number of encapsulated packets received by this system.
IPIP | Total number of IP-in-IP encapsulated packets received by this system.
GRE | Total number of GRE tunneled packets received by this system.
IP-UDP | Total number of IP-in-UDP packets received by the system.
MIP-IPSEC | Total Number of MIP IP Sec packets received by the system.
Total Bytes | Total number of encapsulated bytes received by this system.
IPIP | Total number of IP-in-IP encapsulated bytes received by this system.
GRE | Total number of GRE encapsulated bytes received by this system
IP-UDP | Total number of IP-in-UDP bytes received by the system.
MIP-IPSEC | Total Number of MIP IP Sec bytes received by the system.
Errors
Protocol Type Error | Total number of encapsulated packets received with protocol type errors.
GRE Key Absent | Total number of GRE tunneled key absent errors received.
GRE Checksum Error | Total number of checksum errors that occurred in GRE tunnels received by this system.
Invalid Packet Length | Total number of encapsulated packets received with invalid packet lengths.
No Session Found | Total number of errors that occurred due to no session being present in received tunnels.
Tunnel Data Sent
Total Packets | The total number of encapsulated packets sent by this system.
IPIP | The total number of IP-in-IP encapsulated packets sent by this system.
GRE | The total number of GRE encapsulated packets sent by this system.
IP-UDP | Total number of IP-in-UDP packets sent by the system.
MIP-IPSEC | Total Number of MIP IP Sec packets sent by the system.
Total Bytes | The total number of encapsulated bytes sent by this system.
IPIP | The total number of IP-in-IP encapsulated bytes sent by this system.
GRE | The total number of GRE encapsulated bytes sent by this system
IP-UDP | Total number of IP-in-UDP bytes sent by the system.
MIP-IPSEC | Total Number of MIP IP Sec bytes sent by the system.
Total Disconnects | The total number of sessions that were disconnected.
Lifetime expiry | The total number of sessions that were disconnected due to the expiration of their lifetime setting.
Deregistrations | The total number of sessions that were disconnected due to de-registrations.
Admin Drops | The total number of sessions that were disconnected due to an administrative clearing of calls (i.e. executing the clear subscribers command).
FA Revocations | The total number of disconnects that were due to revocations received from the FA.
IPSEC Tunnel Down | The total number of sessions that were disconnected due to IPSEC tunnels down.
Other Reasons | The total number of disconnects that were due to reasons other than those already listed.
HA Monitoring |
Monitor RRQ Received | The total number of HA monitor request messages received by this HA due to inactivity.
Monitor RRP Sent | The total number of HA monitor response messages sent by this HA.

show mipha full username
Table 2. show mipha full username Command Output Descriptions

Field | Description
--- | ---
Username | Subscriber’s username
Callid | Subscriber’s call identification number
MSID | Subscriber’s mobile station identification number (MSID)
Home Address | IP address assigned to the subscriber’s mobile node for the session
HA Address | IP address of the HA facilitating the subscriber’s MIP session
Send NAI Extension in Revocation Message | Indicates whether or not an NAI extension is sent in a revocation message for this user. Options are: No Yes
Binding # | The mobility binding record (MBR) number associated with a particular subscriber session. Since it is possible for a single subscriber to have multiple bindings, information for each of the subscriber’s binding records will be displayed according to the MBR number.
Care of Address | The IP address of the device terminating the tunnel to the mobile node. The address may belong to either a Foreign Agent that is facilitating the subscriber’s Mobile IP session or another device that the mobile node is associated (co-located) with.
FA Address | The IP address of the Foreign Agent that is facilitating the subscriber’s Mobile IP session.
Lifetime | The maximum amount of time that the subscriber’s session can remain registered.
Remaining Life | The amount of time that is currently available to the subscriber to remain registered.
Reverse Tunneling | Displays whether or not reverse tunneling is enabled for the subscriber’s session.
Encapsulation Type | The encapsulation method used for the subscriber’s session.
GRE Key | The key that uniquely identifies the subscriber session when the Generic Routing Encapsulation (GRE) protocol Encapsulation Type
IPSec Required | Indicates whether or not IPSec is required for the subscriber Mobile IP session.
IPSec Ctrl Tunnel Estab. | If IPSec is required for the session, this field indicates whether or not the control tunnel has been established.
IPSec Data Tunnel Estab. | If IPSec is required for the session, this field indicates whether or not the data tunnel has been established.
Revocation Negotiated | Indicates whether or not MIP Registration Revocation was negotiated between the FA and the HA for this subscriber session. Options are: No Yes
Rev I bit Negotiated | Indicates whether or not the Revocation I bit was negotiated. Possible values are : No Yes
Colocated COA | Indicates whether or not the subscribers that registered a MIP colocated COA directly with the HA. Options are: No Yes
NAT Detected | Indicates whether or not network address translation (NAT) is detected.Options are: No Yes
MN-HA-Key-Present | The security parameter index (SPI) key used to verify a trusted host environment and that communications are to be established between known hosts. Checks for presence of mobile node (MN) - home agent (HA) key. Options are: True False
MN-HA-SPI | Mobile node (MN) - home agent (HA) security parameter index (SPI).
FA-HA-Key-Present | The security parameter index (SPI) key used to verify a trusted host environment and that communications are to be established between known hosts. Checks for presence of the FA - HA key. Options are: True False
FA-HA-SPI | FA - HA security parameter index (SPI)
HA-RK-Key-Present | The HA root key (RK) received by the HA from the AAA in the Radius Access-Accept. Checks for presence of HA-RK key. Options are: True False Note: True indicates a WiMAX session.
HA-RK-SPI | HA - RK security parameter index (SPI) Note: This field applies to WiMAX sessions only.
HA-RK-Lifetime | The total lifetime applied to an HA-RK. Note: This field applies to WiMAX sessions only.
HA-RK-Remaining-Lifetime | Thew total remaining lifetime for the HA-RK. Note: This field applies to WiMAX sessions only.

show mipha peers ha-service
Table 3. show mipha peers ha-service Command Output Descriptions

Field | Description
--- | ---
Context | The name of the context where the HA service is located.
HA Service | The name of the HA service.
Peer Address | The IP address of the peer.
Current Sessions | The number of sessions currently running on the peer.
Total Sessions | The total number of current and past sessions for the peer.
IP Security | Specifies if IP security is enabled or disabled on the peer.
FA-HA Authentication | Specifies if FA-HA authentication is enabled or disabled on the peer.
Total Peers | The total number of peers in the output of this show command.
Total Current Sessions | The total number of sessions across all peers in the output of this show command.