# Local Policy Ruledef Configuration Mode Commands

The Local Policy Ruledef Configuration Mode is used to configure the rule definitions to be used for local QoS policies.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
condition

This command is used to configure the conditions which trigger the ruledef event.
Platform:

ASR 5000
Product:

P-GW
Privilege:

Security Administrator, Administrator
Syntax

    condition priority priority { variable { eq | ge | gt | le | lt | match | ne | nomatch } regex | string_value | int_value | set }no condition priority priority

priority priority

Specifies a priority for the specified condition.

priority must be unique and an integer from 1 to 2048.
variable
The following variables are supported:

- apnThe APN associated with the current session expressed as an alphanumeric string of 1 through 63 characters.
- arpThe APN associated with the current session expressed as an integer from 1 through 15.
- bandwidthTotal bandwidth associated with the QCI and ARP value associated with the request, expresed as an integer from 0 through 1000000000.
- dateDate value to match. <Clock in format YYYY:MM:DD>
- day-of-monthThe day of the month to match the rule to, expressed as an integer from 1 through 31.
- day-of-weekSunday...Saturday, expressed as an integer from 1 to 7.
- imeisvIMEISV of the user equipment expressed as an alphanumeric string of 1 through 63 characters.
- imsiIMSI associated with the subscriber expressed as an alphanumeric string of 1 through 63 characters.
- meidMEID associated with the subscriber expressed as an alphanumeric string of 1 through 63 characters.
- month-of-yearJan, Feb….Dec, expressed as an integer from 1 through 12.
- msisdnMSISDN associated with the session expressed as an alphanumeric string of 1 through 63 characters.
- naiNAI associated with the session expressed as an alphanumeric string of 1 through 63 characters.
- pdn-countNumber of PDNs associated with the same APN, expressed as an integer from 0 through 1000000000.
- qciQCI associated with the current event expressed as an nteger from 1 through 254.
- radio-access-technologyRadio access technology associated with the subscriber: cdma-1xrtt: CDMA 1X RTT radio access technology cdma-evdo: CDMA-EVDO radio access technology cdma-evdo-reva: CDMA EVDO REVA radio access technology cdma-other: Other CDMA radio access technologies ehrpd: EHRPD radio access technology eutran: EUTRAN radio access technology gan: GAN radio access technology gprs-geran: GPRS GERAN radio access technology gprs-other: Other GPRS radio access technology hspa: HSPA radio access technology unknown: Unknown radio access technology wcdma-utran: WCDMA UTRAN radio access technology wimax: WiMax radio access technology wireless-lan: Wireless LAN radio access technology
- serving-node-addressIP address associated with the current node serving the subscriber entered using IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation.
- serving-plmnPLMN associated with the current node serving the subscribe expressed as an alphanumeric string of 1 through 63 characters.
- time-of-dayTime associated with the change. <Clock in format HH:mm:ss or HH:mm >

eq | ge | gt | le | lt | match | ne | nomatch

eq: Operation equal to

ge: Operation greater than or equal to

gt: Operation greater than

le: Operation less than or equal to

lt: Operation less than

match: Operation match

ne: Operation not equal to

nomatch: Operation nomatch
no condition priority priority

Deletes the specified condition.
Usage:

Use this command to configure the conditions which trigger the ruledef event. A ruledef represents a set of matching conditions.

This command can be entered multiple times to configure multiple conditions for a ruledef. The conditions are examined in priority order until a match is found and the corresponding condition is applied.
Example:
The following command creates a condition with priority set to 5 and configured match apn myapn*:

    condition priority
    5 apn match myapn*

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.