> show ps-network
> This chapter includes the show ps-network command output tables.
> show ps-network all status
> show ps-network all status Command Output Descriptions

> Field | Description
> PS Network name | Indicates the name of the Packet Switched (PS) network instance for which status is displayed.
> Associated SCCP-Network | Indicates the name of the Signalling Connection Control Part (SCCP) network service instance which in associated with referecned PS network instance.
> Associated GTPU Service | Indicates the name of the GTP-U service instance which in associated with referecned PS network instance.
> GTPU Context Name | Indicates the name of the context in which GTP-U service instance is configured.
> SGSN Point Code | Indicates the address of SGSN in SS7 point code notation which is serving the referenced PS network instance.
> Status | Indicates the status of SGSN which is serving the referenced PS network instance.
> Network Status | Indicates the status of network in which the referenced PS network instance is placed.
> NRI | Indicates the Network Resource Identication (NRI) bit configuration status for the referenced PS network.
> IDNNS | Indicates the Intra-Domain NAS Node Selector (IDNNS) configuration status for the referenced PS network to transport the NRI value.
> CORE NODE MAP | Indicates the core node mapping configuration status for the referenced PS network.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883