> show bssap
> This chapter includes the show bssap command output tables.
> show bssap+ statistics
> show bssap+ statistics Command Output Descriptions

> Field | Description
> Bssap+ Statistics | Base station system application part plus related statistics.
> Number of Subscribers in Gs-Associated State | Total number of subscriber in Gs associated state or using Gs interface for connectivity between SGSN and VLR.
> Number of Associated Vlrs | Total number of VLRs associated with this BSSAP+ application.
> Alert Req Rcvd | Total number of alert request messages received by BSSAP+ application from VLR.
> Alert Ack Sent | Total number of acknowledge messages sent by BSSAP+ application in response to alert requests messages.
> Alert Rej Sent | Total number of messages sent by BSSAP+ application to reject the alert requests.
> Location Upd Req Sent | Total number of location update request messages sent by BSSAP+ application.
> Location Upd Acc Rcvd | Total number of location update accept messages sent by BSSAP+ application from VLR.
> Location Upd Rej Rcvd | Total number of messages sent by BSSAP+ application to reject the location update requests from VLR.
> GPRS Detach Ind Sent | Total number of GPRS detach indication messages sent by BSSAP+ application.
> GPRS Detach Ack Rcvd | Total number of acknowledge messages received by BSSAP+ application in response to GPRS detach indication messages sent to VLR.
> IMSI Detach Ind Sent | Total number of IMSI detach indication messages sent by BSSAP+ application to VLR.
> IMSI Detach Ack Rcvd | Total number of acknowledge messages received by BSSAP+ application in response to IMSI detach indication messages sent to VLR.
> Mobile Status Rcvd | Total number of mobile status messages received by BSSAP+ application from VLR.
> Mobile Status Sent | Total number of mobile status messages sent by BSSAP+ application to VLR.
> Paging Req Rcvd | Total number of paging request messages received by BSSAP+ application from VLR.
> Paging Rej Sent | Total number of messages sent by BSSAP+ application to reject the received paging request messages from VLR.
> MS Unreachable Sent | Total number of messages sent by BSSAP+ application to indicate that mobile is unreachable to VLR.
> TMSI Reloc Comp Sent | Total number of messages sent by BSSAP+ application with TMSI relocation components to VLR.
> MS Info Req Rcvd | Total number of MS information request messages received by BSSAP+ application from VLR.
> MS Info Rsp Sent | Total number of response messages sent by BSSAP+ application in response to MS information request messages from VLR.
> MM Info Req Rcvd | Total number of mobility management (MM) information request messages received by BSSAP+ application from VLR.
> MS Activity Ind Sent | Total number of MS activity indication messages sent by BSSAP+ application to VLR.
> Reset Ind Rcvd | Total number of reset indicator messages received by BSSAP+ application from VLR.
> Reset Ack Sent | Total number of acknowledge messages sent by BSSAP+ application in response to reset indicator message received from VLR.
> Reset Ind Sent | Total number of reset indicator messages sent by BSSAP+ application to VLR.
> Reset Ack Rcvd | Total number of acknowledge messages received by BSSAP+ application in response to reset indicator message sent to VLR.
> Downlink Tnnl Req Rcvd | Total number of downlink tunnel request messages received by BSSAP+ application from VLR.
> Uplink Tnnl Req Sent | Total number of uplink tunnel request messages sent by BSSAP+ application to VLR.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883