> ASN Paging Group Configuration Mode Commands
> Use the Paging Group Configuration Mode to create and manage Paging Agents for the paging and location register controller within the ASN PC-LR service.
> Important: This functionality is still in development stage.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> paging
> Use to configure the paging parameters within the paging group for PC-LR functionality.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> paging { cycle cycle_value | interval interval_value | node id mac_address address ip_address | offset algorithm uniform start start_value increment inc_value count count_value }
> no paging { cycle | node id mac_address | offset }
> no
> Disables the configured paging parameters within this paging group.
> cycle cycle_value
> Specifies the cycle in which the paging message is transmitted within the paging group.
> Enter an integer for cycle_value from 0 through 65535.
> interval interval_value
> Specifies the maximum duration in frames of Paging Listening Interval; used in calculation of Paging Listening Interval.
> interval_value must be an integer from 1 through 5.
> node id mac_address address ip_address
> id mac_address: Configures the MAC address of the node in the paging group.
> mac_address must be in one of the following formats:
> nn:nn:nn:nn:nn:nn or nn-nn-nn-nn-nn-nn
> address ip_address: Specifies the IP address of the node. Express ip_address in IPv4 or IPv6 dotted decimal notation.
> Important: Configure up to 128 paging nodes per paging group.
> offset algorithm uniform start start_value increment inc_value count count_value
> start start_value: Specifies the starting value of the available offset.
> For start_value, enter an integer from 0 through 65535.
> increment inc_value: Specifies the distance between two offsets.
> For inc_value, enter an integer from 0 through 65535.
> count count_value: Specifies the number of offsets available.
> For count_value, enter an integer from 0 through 65535.
> Offsets are uniformly load balanced across the available range. For this configuration:
> paging offset algorithm uniform start 10 increment 10 count 4
> the following occurs:
> if MS1, MS2,...MS100, perform IM-Entry, then offset assigned: MS1=10, MS2=20, MS3=30, MS4=40, MS5=10, MS6=20, etc.
> Usage
> Use this command to define the paging behavior of a paging group. There must be only one instance of paging parameters per paging group.
> Example
> The following example configures the paging cycle for a paging group to 10.
> paging cycle 10
> The following example configures a paging node in the group:
> paging node id 00:05:47:00:37:44 address 12.345.76.789

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883