> PCC-Event-Notification-Interface-Endpoint Configuration Mode Commands
> The PCC-Event-Notification-Interface-Endpoint configuration mode is used to enable the event notification interface mechanism on IPCF and to configure the Event Notification collection server endpoint related parameters.
> Important: This configuration mode is supported from StarOS Release 12.1 onward.
> address
> This command binds an IP address to the local IPCF node which is to be used for event notification processing with remote event collection server endpoint during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> address ip_address
> ip_address
> Specifies the IP address bind with local IPCF node to be used by the event collection server endpoint for event message processing during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> Usage
> Use this command to bind an IP address to interact with the remote event notification collection server endpoint to which the event messages are sent for IP-CAN session events.
> Example
> Following command binds the 1.2.3.4 for event notification message with remote event notification endpoint.
> address 1.2.3.4
> peer name
> This command binds/associates a remote Event Notification collection server as peer having specified IP address and optionally port for event notification during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> peer name peer_name address ip_address [port port_num]
> name peer_name
> Sets the in PCC-Event-Notification-Interface-Endpoint instance to use a particular peer node configured by a peer name peer_name for event notification interface.
> The peer_name is name of the peer node to be sued for event collection and must be an alphanumerical string from 1 through 31 characters. peer_name allows punctuation marks.
> ip-address ip_address
> Sets the PCC-Event-Notification-Interface-Endpoint instance to bind the particular peer node name with IP address ip_address in IPv4 or IPv6 notation for event notification message processing.
> The ip_address is an IP address in IPv4/IPv6 notation.
> port port_num
> This optional keyword sets a particular port number to be used with in the PCC-Event-Notification-Interface-Endpoint instance to configure a particular peer node having a pre assigned IP address ip_address in IPv4 or IPv6 notation for event notification message processing.
> The port_num must be an integer between 1 and 65535.
> Usage
> Use this command to bind/associate a remote Event Notification collection server as peer having specified IP address and optionally port for event notification during IP-CAN session in the PCC-Event-Notification-Interface-Endpoint instance.
> Multiple peers can be configured using this command and peer selection methods, primary-secondary or round-robin can be applied using peer select-algorithm command for event notification during IP-CAN session in this configuration mode.
> Example
> Following command configures and associates an Event Notification peer node named event_peer_1 having an IP address 1.2.3.4 with port number as 2345 in an PCC-Event-Notification-Interface-Endpoint instance.
> peer name event_peer_1 ip-address 1.2.3.4 port 2345
> peer select-algorithm
> This command applies the peer selection algorithm to select the configured remote Event Notification collection server during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> peer select-algorithm {primary-secondary | round-robin}
> primary-secondary
> Sets the PCC-Event-Notification-Interface-Endpoint peer selection algorithm to select the configured remote peer servers in primary and secondary method during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> This mode is applicable only when multiple peers are configured and primary and secondary peer is defined using peer select-peer command in this configuration mode.
> round-robin
> Sets the PCC-Event-Notification-Interface-Endpoint peer selection algorithm to select the configured remote peer servers in round-robin method mode during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> This mode is applicable only when multiple peers are configured in this configuration mode.
> Usage
> Use this command apply the peer selection algorithm to select the configured remote Event Notification collection server during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> Example
> Following command configures the peer selection algorithm to select the configured remote peer in round-robin method in PCC-Event-Notification-Interface-Endpoint instance.
> peer select-algorithm round-robin
> Following command configures the peer selection algorithm to select the configured primary and secondary remote peers in primary-secondary method in PCC-Event-Notification-Interface-Endpoint instance.
> peer select-algorithm primary-secondary
> peer select-peer
> This command sets the configured remote Event Notification collection server as primary and secondary servers for event notification collection during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> peer select-peer pri_peer_name secondary sec_peer_name
> pri_peer_name
> Sets the configured remote PCC-Event-Notification-Interface-Endpoint peer as primary peer for event notification collection during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> pri_peer_name must be a pre-configured peer name configured with peer name command in this configuration mode.
> secondary sec_peer_name
> Sets the configured remote PCC-Event-Notification-Interface-Endpoint peer as secondary peer for event notification collection during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> sec_peer_name must be a pre-configured peer name configured with peer name command in this configuration mode.
> Usage
> Use this command to set the configured remote Event Notification collection server as primary and secondary node for event notification collection during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> This configuration is used when peer selection algorithm is set to primary-secondary using peer select-algorithm command in this configuration mode.
> Example
> Following command configures the specified peer event1 as primary and event2 as secondary node for event notification collection during IP-CAN session in PCC-Event-Notification-Interface-Endpoint instance.
> peer select-peer event1 secondary event2

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883