> Configuring MegaRAID for MUR Applications
> CISCO UCS servers support a MegaRAID controller. This allows for configuring the UCS hard disks into hardware RAID arrays. The MegaRAID controller provides the BIOS utility for configuring the RAID. This chapter describes how to configure MegaRAID; this is for Mobility Unified Reporting System (MUR) applications only.
> Option Recommendations
> The following options are recommended for MUR applications:

> • | Separate disk arrays for the Operating System, MUR, and the PostGRES (data directory).

> • | RAID level. This is a combination of five (5) and zero (0) depending on the fault tolerance.

> • | Stripe size should be 256KB.

> The following RAID Controller parameters are recommended:

> • | Read Policy - Select Adaptive Read-Ahead.

> • | Write Policy - Select Write Back.

> • | I/O Policy - Select Direct I/O.

> Sample Configuration
> In the following example, the UCS server has 12 disks each of 280GB. The disks are configured into the following three groups:

> • | Single (1) disk in RAID-0 for the OS (The System Administrator should select the number of disks and RAID level).

> • | RAID-0 array with four (4) disks for the MUR application.

> • | RAID-0 array with four (4) disks for the MUR application.

> Using the MegaRAID BIOS to Configure the RAID Array
> Use the following steps to configure the RAID array using the MegaRAID BIOS.
> Creating Virtual Drives
> Use the following steps to create virtual drives.

> 1. | While the system is booting, press <Ctrl><H> to start the WebBIOS utility.

> 2. | Press Start to enter the utility. If the drives are already configured, the screen will show the current RAID configuration with virtual drives for all the RAID disk groups. In this case, the drives show as being unconfigured, as depicted below:

> 3. | From the left pane, select Configuration Wizard.

> Important: In the even that there are already any unwanted virtual drives configured, select the Clear Configuration radio button in the Wizard to delete the default virtual drives.

> 4. | Select the New Configuration radio button to start creating virtual drives. If you did not delete any drives in the previous step and want to configure them now, select the Add Configuration radio button.

> 5. | Press Next and then select Manual Configuration.

> 6. | Press Next. The Drive Group Definitions screen opens as depicted below:

> 7. | Click on the first disk in the list (Slot 1)as shown in the image above. This disk is the single disk selected to be the virtual drive for the operating system and it will be added to Drive Group0. Select Drive Group0 and press the Accept DG button, as depicted below:

> 8. | To configure the next drive group in this example, use the <Ctrl> key to select the next four disks (Slots 2 through 5) and press the Add to Array button. This creates Drive Group1 as depicted below:

> 9. | Use the same method described in Step 8 to select the remaining four disks and create Drive Group2.

> You are now ready to configure the spans.
> Configuring Spans
> Continue the configuration using the following steps to configure spans. Spans are used to take Drive Groups and use them to create a nested RAID array.

> 1. | Press Next. The Span Definition screen opens as depicted below. Because this example only considers RAID-0 and RAID-5 arrays, the span will be created with only one group.

> 2. | Select Drive Group0 and press the Add to Span button when it activates.

> 3. | Press Next to open the Virtual Drive Definition screen as depicted below. This is where RAID parameters are configured for the Disk Groups created earlier.

> 4. | Complete this screen using the example parameters established in the Storage Recommendations section in this document.

> 5. | Press the Accept button to open a confirmation page where you confirm a Battery Backup Unit (BBU) is installed when using the Write Back with BBU policy option in the Virtual Drive Definition screen in Step 4. Press Yes to confirm.

> 6. | Press the Back button to return to the Span Definition screen. Repeat steps 2 through 5 to add Disk Group1 and Disk Group2 to separate spans and configure the RAID parameters. The following screen detail depicts the virtual drives window after all Groups are added correctly:

> 7. | Press the Accept button to confirm the configuration.

> 8. | Save the configuration and the utility will initialize the drives and display a final screen displaying the new virtual drives, as depicted below:

> 9. | If necessary, check the properties for the drives by pressing the Back button to go back to the Main menu, as depicted below:

> Continue to the next section to set the boot drive.
> Setting the Boot Drive
> You earlier created a separate drive for the operating system and added it to DriveGroup0. Use the following steps to set this drive as the boot drive.

> 1. | From the Main menu, select the Virtual Drives option in the left pane.

> 2. | Select the drive created for the operating system,

> 3. | Select the Set Boot Drive radio button.

> 4. | Press the Go button to change the settings.

> 5. | Press the Exit button to save the changes and exit the utility.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883