> FA Service Thresholds
> An FA Service threshold generates alerts or alarms for registration reply errors for individual FA services.
> Alerts or alarms are triggered for the FA threshold based on the following rules:

> • | Enter condition: Actual number of errors > High Thresholds

> • | Clear condition: Actual number of errors < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm is not generated until the end of the polling interval.
> Configuring FA Service Thresholds
> Use the following example to configure the threshold, set the polling interval for the threshold and enable monitoring of the threshold.
> configure
> context <context_name>
> fa-service <name>
> threshold reg-reply-error <high_thresh> [ clear <low_thresh> ]
> exit
> exit
> threshold poll fa-reg-reply-error interval <time>
> threshold monitoring fa-service
> end
> Saving Your Configuration
> When you configure thresholds they are not permanent unless you save the changes. When you have completed configuring thresholds, save your configuration as described in the Saving Your Configuration chapter.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883