> BMSC Profile Configuration Mode Commands
> The BMSC Profile Configuration Mode is used to configure Broadcast Multicast Service Center profiles for Multimedia Broadcast Multicast Service (MBMS) applications. The mode is accessed by entering the bmsc-profile command from the Context Configuration Mode.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Returns the CLI prompt to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> Example
> end
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the previous or parent mode.
> Example
> exit
> gmb diameter dictionary
> This command specifies the Diameter dictionary for the Gmb interface in BM-SC profile of MBMS user service.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gmb diameter dictionary { custom1 | custom10 | custom2 | custom3 | custom4 | custom5 | custom6 | custom7 | custom8 | custom9 | standard }
> default gmb diameter dictionary
> custom1 ... custom10
> Custom-defined Diameter dictionary. Specific to customer requirement.
> standard
> Default: Enabled
> Specifies the standard Gmb Diameter dictionary conforming to 3GPP TS 29.061 (Rel. 7).
> default
> Sets the Diameter dictionary to standard.
> Usage
> Use this command to select the Gmb Diameter dictionary in BM-SC profile of MBMS user service.
> Example
> The following command sets the Gmb Diameter dictionary to TS 29.061 (Rel. 7) specific:
> gmb diameter dictionary standard
> gmb diameter endpoint
> This command specifies the Diameter endpoint name for Gmb interface in BM-SC profile of MBMS user service.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gmb diameter endpoint endpoint_name
> no gmb diameter endpoint
> no
> Removes the previously configured Diameter endpoint name for Gmb interface in BM-SC profile of MBMS user service.
> endpoint_name
> Specifies the Diameter endpoint name for Gmb interface. This must be present in all Diameter messages and is the endpoint that originates the Diameter message.
> endpoint_name must be an alpha and/or numeric string of length between 1 to 63 characters.
> Usage
> Use this command to create a Gmb Diameter endpoint for BM-SC profile.
> Example
> The following command creates a Diameter endpoint named test1 in BM-SC profile of MBMS user service:
> gmb diameter endpoint test1
> gmb diameter peer-select
> This command specifies the peer ids of BM-SC Diameter primary and secondary host in BM-SC profile for MBMS user service.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gmb diameter peer-select peer peer_name [ realm realm_name ] [ secondary-peer sec_peer_name [ realm sec_realm_name ] ]
> gmb diameter peer-select
> no
> Removes the previously configured BM-SC Diameter peer ids configured in BM-SC profile of MBMS user service.
> peer peer_name
> Specifies the primary diameter host id for BM-SC in this BM-SC profile for MBMS user service. This is a unique name that is specified for the primary peer.
> peer_name must be an alpha and/or numeric string of from 1 through 127 characters and it allows punctuation marks.
> realm realm_name
> Specifies the realm or domain for Gmb diameter peer. The realm may typically be a company or service name.
> realm_name must be an alpha and/or numeric string of from 1 to 127 characters and allows punctuation marks.
> secondary-peer sec_peer_name
> Specifies a back-up host that is used for fail-over processing. When the route-table does not find an AVAILABLE route the secondary host performs a fail-over processing.
> sec_peer_name must be an alpha and/or numeric string of from 1 through 127 characters and it allows punctuation marks.
> realm sec_realm_name
> Specifies the realm or domain for Gmb diameter secondary host. The realm may typically be a company or service name.
> sec_realm_name must be an alpha and/or numeric string of from 1 to 127 characters and allows punctuation marks.
> Usage
> Use this command to select a BM-SC Diameter peer and realm in this BM-SC profile for MBMS user service.
> Example
> The following command selects a Gmb Diameter peer named test1 and a realm of companyx:
> gmb diameter peer-select peer test1 realm companyx
> gmb user-data
> This command configures the parameters in this BM-SC profile for user data of MBMS user service.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gmb user-data { mode-preference { multicast | unicast } | unicast-self-address self_ip_address }
> default gmb user-data mode-preference
> no gmb user-data unicast-self-address
> no
> Removes the configured self address of GGSN for unicast in BM-SC profile for user data of MBMS user service.
> defualt
> Sets the user data mode to unicast in BM-SC profile for user data of MBMS user service.
> mode-preference { multicast | unicast }
> Default: unicast
> Specifies the preferred mode of GGSN for receiving MBMS suer service data.
> multicast: specifies the preferred mode as multicast for MBMS user service.
> Important: Note that this multicast keyword is not supported in this release.
> unicast: specifies the preferred mode as unicast for MBMS user service.
> unicast-self-address self_ip_address
> Specifies the GGSN’s IP address for BM-SC to use as outer destination address for the IP-in-IP tunnel to send multicast data if configured preferred data mode is unicast.
> self_ip_address must be the IPv4 address in dotted decimal notation.
> This command must be configured if GGSN's user-data mode-preference is Unicast.
> Usage
> Use this command to configure user data mode and other parameters in BM-SC profile for user data of MBMS user service.
> GGSN can receive multicast data from BM-SC in one of two modes - Multicast or Unicast. In Unicast mode, BM-SC tunnels the multicast data to the GGSN in an IP-in-IP tunnel instead of direct multicast. This command with mode-preference keyword configures the GGSN's preferred mode for receiving multicast data.
> Important: Both GGSN and BM-SC must support the Unicast mode of multicast data transfer. If any of GGSN or BM-SC doesn't support Multicast mode, BM-SC will transfer multicast data using Unicast mode only.
> Use unicast-self-address keyword to configure GGSN's IP address which the BM-SC should use as the outer destination address for the IP-in-IP tunnel to send multicast data if the selected user data mode to receive multicast data is Unicast (i.e. either of GGSN or BM-SC doesn't support Multicast mode of data transfer).
> Example
> The following command sets the MBMS data transfer mode to unicast:
> default gmb user-data mode-preference

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883