> ASN RAN Peer Map Configuration Mode Commands
> Use the RAN Peer Map Configuration Mode to create and manage global mapping tables of base station peers.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> ran-peer
> Use this command to configure the MAC and IP addresses of the base station peers you are adding to this map.
> Product
> ASN GW
> Privilege
> Administrator
> Syntax
> [ no ] ran-peer id mac_address address ip_address [mode{non-legacy | legacy}]
> no
> Removes the base station peer entry from this map.
> id mac_address address ip_address
> id mac_address: Configures the MAC address of the base station peer in this map.
> mac_address must be in one of the following formats:
> nn:nn:nn:nn:nn:nn or nn-nn-nn-nn-nn-nn
> address ip_address: Specifies the IP address of the base station peer. Express ip_address in IPv4 or IPv6 dotted decimal notation.
> mode {non-legacy | legacy}: Default mode is non-legacy.
> Usage
> Use this command to add base station peers to this peer map.
> Example
> The following command adds a base station peer to this map:
> ran-peer id 00:05:47:00:37:44 address 12.345.76.789

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883