> Total Session Thresholds
> Threshold monitoring can be enabled for the total session counts described in the following table.

> Value | Description | To configure, go to section:
> PDSN Services | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all PDSN services counted during the polling interval. | Total PDSN Session Thresholds
> GGSN Services | Enables the generation of alerts or alarms based on the total number of PDP contexts (active and dormant) facilitated by all GGSN services counted during the polling interval. | Total GGSN Session Thresholds
> GPRS Services | Enables the generation of alerts or alarms based on the total number of GPRS sessions or the total number of PDP sessions facilitated by the GPRS services counted during the polling interval. | Total GPRS Session Thresholds Total GPRS PDP Contexts Thresholds
> HA Services | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all HA services counted during the polling interval. | Total HA Session Thresholds
> HNB-GW Services | Enables the generation of alerts or alarms based on the total number of HNB, UE, Iu sessions (active and dormant) facilitated by all HNB-GW services counted during the polling interval. | Total HNB-GW Session Thresholds
> HSGW Service | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all HSGW services counted during the polling interval. | Total HSGW Session Thresholds
> LMA Service | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all LMA services counted during the polling interval. | Total LMA Session Thresholds
> LNS Services | Enables the generation of alerts or alarms based on the total number of sessions facilitated by all LNS services counted during the polling interval. | Total LNS Session Thresholds
> MME Service | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all MME services counted during the polling interval. | Total MME Session Thresholds
> P-GW Service | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all P-GW services counted during the polling interval. | Total P-GW Session Thresholds
> SGSN Services | Enables the generation of alerts or alarms based on the total number of SGSN sessions or the total number of PDP sessions facilitated by the SGSN services counted during the polling interval. | Total SGSN Session Thresholds Total SGSN PDP Contexts Thresholds
> S-GW Service | Enables the generation of alerts or alarms based on the total number of sessions (active and dormant) facilitated by all S-GW services counted during the polling interval. | Total S-GW Session Thresholds

> ‌
> Saving Your Configuration
> When you configure thresholds they are not permanent unless you save the changes. When you have completed configuring thresholds, save your configuration as described in the Verifying and Saving Your Configuration chapter.
> Total PDSN Session Thresholds
> Total PDSN session thresholds generate alerts or alarms based on the total number of sessions facilitated by any PDSN service configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all PDSN sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total PDSN Session Thresholds
> Use the following example to configure the total PDSN session thresholds:
> configure
> threshold total-pdsn-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-pdsn-sessions interval <time>
> threshold monitoring pdsn-service
> end
> Total GGSN Session Thresholds
> Total GGSN session thresholds generate alerts or alarms based on the total number of PDP contexts facilitated by all GGSN services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all GGSN PDP contexts based on the following rules:

> • | Enter condition: Actual total number of PDP contexts > or = High Threshold

> • | Clear condition: Actual total number of PDP contexts < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total GGSN Session Thresholds
> Use the following example to configure the per-GGSN service thresholds:
> configure
> threshold total-ggsn-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-ggsn-sessions interval <time>
> threshold monitoring ggsn-service
> end
> Total GPRS Session Thresholds
> Total GPRS session thresholds generate alerts or alarms based on the total number of attached subscribers facilitated by all GPRS services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all subscribers attached to the GPRS based on the following rules:

> • | Enter condition: Actual total number of attached subscribers > or = High Threshold

> • | Clear condition: Actual total number of attached subscribers < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total GPRS Session Thresholds
> Use the following example to configure the per-SGSN service thresholds:
> configure
> threshold total-gprs-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-gprs-sessions interval <time>
> threshold monitoring gprs-service
> end
> Total GPRS PDP Contexts Thresholds
> Total GPRS PDP contexts thresholds generate alerts or alarms based on the total number of PDP contexts facilitated by all GPRS services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all GPRS PDP contexts based on the following rules:

> • | Enter condition: Actual total number of PDP contexts > or = High Threshold

> • | Clear condition: Actual total number of PDP contexts < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total GPRS PDP Context Thresholds
> Use the following example to configure the per-GPRS service thresholds:
> configure
> threshold total-gprs-pdp-sessions <high_thresh> [ clear <low_thresh>]
> threshold poll total-gprs-pdp-sessions interval <time>
> threshold monitoring gprs-service
> end
> Total HA Session Thresholds
> Total HA session thresholds generate alerts or alarms based on the total number of sessions facilitated by all HA services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all HA sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total HA Session Thresholds
> Use the following example to configure the total HA session thresholds:
> configure
> threshold total-ha-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-ha-sessions interval <time>
> threshold monitoring ha-service
> end
> Total HNB-GW Session Thresholds
> Total HNB-GW service session thresholds generate alerts or alarms based on the total number of IuH, IuCS, and IuPS sessions facilitated by all HNB-GW services configured on the system during the specified polling interval. Thresholds for IuH session is provided for HNB and UE seperately.
> Alerts or alarms are triggered for the total of all IuH, IuCS, or IuPS sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total HNB Session Thresholds
> Use the following example to configure the thresholds for total HNB sessions over IuH interface between HNB and HNB-GW service on HNB-GW node:
> configure
> threshold total-hnbgw-hnb-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-hnbgw-hnb-sessions interval <time>
> threshold monitoring hnbgw-service
> end
> Configuring Total UE Session Thresholds
> Use the following example to configure the thresholds for total UE sessions over IuH interface between HNB and HNB-GW service on HNB-GW node:
> configure
> threshold total-hnbgw-ue-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-hnbgw-ue-sessions interval <time>
> threshold monitoring hnbgw-service
> end
> Configuring Total Iu Session Thresholds
> Use the following example to configure the thresholds for total IuPS and/or IuCS sessions over Iu interface between HNB-GW and CN node:
> configure
> threshold total-hnbgw-iu-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-hnbgw-iu-sessions interval <time>
> threshold monitoring hnbgw-service
> end
> Total HSGW Session Thresholds
> Total HSGW session thresholds generate alerts or alarms based on the total number of sessions facilitated by all HSGW services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all HSGW sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total HSGW Session Thresholds
> Use the following example to configure the total HSGW session thresholds:
> configure
> threshold total-hsgw-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-hsgw-sessions interval <time>
> threshold monitoring hsgw-service
> end
> Total LMA Session Thresholds
> Total LMA session thresholds generate alerts or alarms based on the total number of sessions facilitated by all HSGW services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all LMA sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total LMA Session Thresholds
> Use the following example to configure the total LMA session thresholds:
> configure
> threshold total-lma-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-lma-sessions interval <time>
> threshold monitoring lma-service
> end
> Total LNS Session Thresholds
> Total LNS session thresholds generate alerts or alarms based on the total number of sessions facilitated by all LNS services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all LNS sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total LNS Session Thresholds
> Use the following example to configure the total LNS session thresholds:
> configure
> threshold total-lns-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-lns-sessions interval <time>
> threshold monitoring lns-service
> end
> Total MME Session Thresholds
> Total MME session thresholds generate alerts or alarms based on the total number of sessions facilitated by all MME services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all MME sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total MME Session Thresholds
> Use the following example to configure the total P-GW session thresholds:
> configure
> threshold total-mme-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-mme-sessions interval <time>
> threshold monitoring mme-service
> end
> Total P-GW Session Thresholds
> Total P-GW session thresholds generate alerts or alarms based on the total number of sessions facilitated by all P-GW services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all P-GW sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total P-GW Session Thresholds
> Use the following example to configure the total P-GW session thresholds:
> configure
> threshold total-pgw-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-pgw-sessions interval <time>
> threshold monitoring pgw-service
> end
> Total SGSN Session Thresholds
> Total SGSN session thresholds generate alerts or alarms based on the total number of attached subscribers facilitated by all SGSN services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all subscribers attached to the SGSN based on the following rules:

> • | Enter condition: Actual total number of attached subscribers > or = High Threshold

> • | Clear condition: Actual total number of attached subscribers < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total SGSN Session Thresholds
> Use the following example to configure the per-SGSN service thresholds:
> configure
> threshold total-sgsn-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-sgsn-sessions interval <time>
> threshold monitoring sgsn-service
> end
> Total SGSN PDP Contexts Thresholds
> Total SGSN PDP contexts thresholds generate alerts or alarms based on the total number of PDP contexts facilitated by all SGSN services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all SGSN PDP contexts based on the following rules:

> • | Enter condition: Actual total number of PDP contexts > or = High Threshold

> • | Clear condition: Actual total number of PDP contexts < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total SGSN PDP Context Thresholds
> Use the following example to configure the per-SGSN service thresholds:
> configure
> threshold total-sgsn-pdp-sessions <high_thresh> [ clear <low_thresh>]
> threshold poll total-sgsn-pdp-sessions interval <time>
> threshold monitoring sgsn-service
> end
> Total S-GW Session Thresholds
> Total S-GW session thresholds generate alerts or alarms based on the total number of sessions facilitated by all S-GW services configured on the system during the specified polling interval.
> Alerts or alarms are triggered for the total of all S-GW sessions based on the following rules:

> • | Enter condition: Actual total number of sessions > or = High Threshold

> • | Clear condition: Actual total number of sessions < Low Threshold

> If a trigger condition occurs within the polling interval, the alert or alarm will not be generated until the end of the polling interval.
> Configuring Total S-GW Session Thresholds
> Use the following example to configure the total S-GW session thresholds:
> configure
> threshold total-sgw-sessions <high_thresh> [ clear <low_thresh> ]
> threshold poll total-sgw-sessions interval <time>
> threshold monitoring sgw-service
> end

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883