> System Element Configuration Procedures
> This chapter presents interface and port configuration procedures. Before beginning these procedures, refer to your product-specific administration guide for configuration information for your product.
> This chapter includes the following:

> • | Creating Contexts

> • | Creating and Configuring Ethernet Interfaces and Ports

> • | Creating and Configuring ATM Interfaces and Ports

> • | Creating and Configuring Frame Relay Interfaces and Ports

> Important: Make sure at least one Packet Services Card (PSC) is active before you configure system elements. Refer to Configuring System Settings in this guide for information and instructions on activating PSCs.
> Creating Contexts
> Even though multiple contexts can be configured to perform specific functions, they are all created using the same procedure.
> Important: Commands used in the configuration examples in this section represent the most common or likely commands and/or keyword options. In many cases, other commands and/or keyword options are available. Refer to the Command Line Interface Reference for complete information regarding all commands.
> To create a context, apply the following example configuration:
> configure
> context <name>
> end
> Repeat to configure additional contexts.
> Important: We recommend that if your system is using Fast Ether Line Cards (FELCs, Ethernet 10/100), at least one context be configured per physical port in order to ensure adequate bandwidth for subscriber sessions.
> Viewing and Verifying Contexts

> Step 1 | Verify that your contexts were successfully created by entering the following command:

> show context all
> The output is a two-column table similar to the example below. This example shows that two contexts were created: one named source and one named destination.
> Context Name ContextID State
> ------------ --------- -----
> local 1 Active
> source 2 Active
> destination 3 Active
> The left column lists the contexts that are currently configured. The center column lists the corresponding context ID for each of the configured contexts. The third column lists the current state of the context.

> Step 2 | Save your configuration as described in the Verifying and Saving Your Configuration chapter.

> Step 3 | Now that the context has been created, interfaces and specific functionality can be configured within the context. Proceed to other sections in this chapter for instructions on configuring specific services and options.

> Creating and Configuring Ethernet Interfaces and Ports
> Regardless of the type of application interface, the procedure to create and configure it consists of the following:

> Step 1 | Create an interface and assign an IP address and subnet mask to it by applying the example configuration in the Creating an Interface

> Step 2 | Assign a physical port for use by the interface and bind the port to the interface by applying the example configuration in the Configuring a Port and Binding it to an Interface section.

> Step 3 | Optionally configure a static route for the interface by applying the example configuration in the Configuring a Static Route for an Interface section.

> Step 4 | Repeat the above steps for each interface to be configured.

> Important: This section provides the minimum instructions for configuring interfaces and ports to allow the system to communicate on the network. Commands that configure additional interface or port properties are provided in the Ethernet Port Configuration Mode and Ethernet Interface Configuration Mode chapters of the Command Line Interface Reference.
> Caution: To ensure that system line card and port-level redundancy mechanisms function properly, the Spanning Tree protocol must be disabled on devices connected directly to any system port. Failure to turn off the Spanning Tree protocol may result in failures in the redundancy mechanisms or service outage.
> Creating an Interface
> Use the following example to create a new interface in a context:
> configure
> context <name>
> interface <name>
> ip address <address subnetmask> [ secondary ]
> end
> Notes:

> • | Option: Add the loopback keyword option to the interface <name> command, to set the interface type as “loopback” which is always UP and not bound to any physical port.

> • | Option: Add the secondary keyword to the ip address command, to assign multiple IP addresses to the interface. IP addresses can be entered using IPv4 dotted-decimal or IPv6 colon-separated notation.

> • | Option: In the interface config mode, add the port-switch-on-L3-fail address command, to configure the interface for switchover to the port on the redundant line card if connectivity to a specified IP address is lost. This IP address can be entered using IPv4 dotted-decimal or IPv6 colon-separated notation.

> Configuring a Port and Binding It to an Interface
> Use the following example configuration to configure and assign a port to an interface:
> configure
> port ethernet <slot#/port#>
> description <description>
> no shutdown
> bind interface <interface_name> <context_name>
> end
> Notes:

> • | For port ethernet slot#, use the actual chassis slot in which the line card is installed. This could be any number from 17 to 23, or 26 to 39, or 42 to 48.

> • | Option: In the Ethernet Port configuration mode, add the preferred slot slot# command if LC port redundancy was enabled at the card level and you want to specify a port preference.

> • | Option: In the Ethernet Port configuration mode, configure the port speed, if needed, by entering the medium command. Refer to the Command Line Interface Reference for a complete explanation of this command.

> • | Binding associates the port and all of its settings to the named interface.

> Configuring a Static Route for an Interface
> Use the following example to configure a static route for an interface:
> configure
> context <name>
> ip route <ip_address> <netmask> next-hop <gw_address> <interface_name>
> end
> Notes:

> • | ip_address and netmask are the IP address and subnet mask of the target network. This IP address can be entered using IPv4 dotted-decimal or IPv6 colon-separated notation.

> • | gw_address is the IP address of the default gateway or next-hop route. This IP address can be entered using IPv4 dotted-decimal or IPv6 colon-separated notation.

> • | To configure a route to the gateway router, use 0.0.0.0 for the network and mask variables.

> • | Repeat as needed. Multiple static routes can be configured to the same destination to provide an alternative means of communication in case the preferred route fails.

> Viewing and Verifying Port Configuration

> Step 1 | Verify that your interface configuration settings are correct by entering the following commands:

> context <context_name>
> show ip interface
> context_name represents the name of the context in which the interface was created. The output from these commands should be similar to the following example.
> In this example an interface named mgmt1 was configured in the local context.
> Intf Name: mgmt1
> Intf Type: Broadcast
> IP State: UP (Bound to 17/1 untagged, ifIndex 285278209)
> IP Address: 192.168.100.3 Subnet Mask: 255.255.255.0
> Bcast Address: 192.168.100.255 MTU: 1500
> Resoln Type: ARP ARP timeout: 3600 secs
> L3 monitor LC-port switchover: Disabled
> Number of Secondary Addresses: 0
> Total interface count: 1

> Step 2 | Verify that your port configuration settings are correct by entering the following command:

> show configuration port <slot#/port#>
> slot# is the chassis slot number of the line card on which the physical port resides. slot# can be any integer value from 17 to 39, and 42 to 48.
> This command produces an output similar to that displayed in the following example that shows the configuration for port 1 on the line card installed in chassis slot 17.
> In this example, the port is bound to an interface called rp1 configured in a context called source.
> config
> port ethernet 17/1
> description LC17/1_RP1
> no shutdown
> bind interface rp1 source
> #exit end

> Step 3 | Verify that your static route(s) was configured properly by entering the following command:

> show ip static-route
> This command produces an output similar to that displayed in the following example that shows a static route to a gateway with an IP address of 192.168.250.1
> Destination Nexthop Protocol Prec Cost Interface
> 0.0.0.0/0 192.168.250.1 Static 0 0 SPIO1
> 0.0.0.0/0 192.168.250.1 Static 0 0 rp1 source

> Step 4 | Save the configuration as described in the Verifying and Saving Your Configuration chapter.

> Creating and Configuring ATM Interfaces and Ports
> This section describes the minimum configuration required to use IP over ATM (IPoA) through an Optical ATM line card (OLC/OLC2). The procedures describe how to:

> Step 1 | Set the framing method for a specific OLC-type line card and make the card “active” by using the procedure defined in Enabling the OLC (ATM) Line Card .

> Step 2 | Create an IP over ATM interface (PVC interface) by following the example configuration in the Creating an IP Interface for Use with an ATM Port section.

> Step 3 | Enable the ATM port, create the IPoA (PVC) interface for the ATM port, and enable the PVC by applying the example configuration in the Configuring an ATM Port to Use an IP Interface section.

> Steps 2 and 3 together configure the data plane.

> Step 4 | Configure an ATM port to use with an SS7 link ID by applying the example configuration in the Configuring an ATM Port for an SS7 Link section.

> Step 4 configures the control plane through an SS7/IPoA (PVC) interface.
> Important: Do not attempt to bind the link at this time. Complete the rest of the procedure (steps 5, 6, and 7) and return to bind the link to the port. The SS7 link can only be bound to the ATM port after the configuration for the SS7 routing domain has been completed as described in the 3G SGSN Configuration section of the SGSN Administration Guide.

> Step 5 | Configure the appropriate timing source (BITS from the SPIO or line-timing from an attached remote) to ensure transmit synchronization by applying the example configuration in the Configuring Transmit Timing Source section of the Configuring System Settings chapter.

> Step 6 | Verify the port and interface configuration with the procedure Verifying Port and Interface Configuration .

> Step 7 | Save the configuration as described in the Verifying and Saving Your Configuration chapter.

> Enabling the OLC (ATM) Line Card
> Use the following example to select an OLC and set the framing type:
> configure
> card <slot#>
> framing <SDH|SONET>
> no shutdown
> end
> Notes:

> • | The default framing type is SONET (Synchronous Optical Network) for an Optical (ATM) line card.

> • | Setting the framing method is required to make the card operational.

> • | Entering no shutdown makes the card active.

> Creating an IP Interface for Use with an ATM Port
> Use the following example to create an IP interface to use with ATM:
> configure
> context <ctxt_name>
> interface <intf_name> point-to-point
> ip address <ip_addr> <net_mask>
> ip address <ip_addr> <net_mask> secondary
> end
> Notes:

> • | The context must be the one in which you have or will configure the SGSN service.

> • | You must enter the point-to-point keyword to create the PVC (Permanent Virtual Connection) interface for the IP over ATM.

> Configuring an ATM Port to Use an IP Interface
> Use the following example to configure an ATM port to use with an IP interface:
> configure
> port atm <slot#>/<port#>
> no shutdown
> pvc vpi <vpi_num> vci <vci_num>
> no shutdown
> bind interface <ifc_name> <ctx_name>
> end
> Notes:

> • | The context must be the one you used when creating the IP interface (PVC) for the ATM port.

> Configuring an ATM Port for an SS7 Link
> Use the following example to configure an ATM port to use with an SS7 (Signalling System No. 7) link:
> configure
> port atm <slot#>/<port#>
> no shutdown
> pvc vpi <vpi_num> vci <vci_num>
> no shutdown
> end
> Notes:

> • | The PVC for the SS7 link has been created but can not be bound unless the SS7 routing domain configuration has already been completed (see the SGSN Administration Guide).

> • | Complete optional ATM port configuration (see the ATM Port Configuration Mode in the Command Line Interface Reference) and the other steps in this procedure to set timing and save the configuration.

> Binding an SS7 Link to an ATM Port
> Use the following example to bind an already configured SS7 link to a PVC interface for an ATM port:
> configure
> port atm <slot#>/<port#>
> pvc vpi <vpi_num> vci <vci_num>
> bind link ss7-routing-domain <ss7rd_id> linkset-id <id> link-id <id>
> end
> Notes:

> • | Save the configuration as described in the Saving Your Configuration chapter.

> Verifying Port and Interface Configuration

> Step 1 | Verify that your interface configuration settings are correct by entering the following commands:

> context <context_name>
> show ip interface
> context_name represents the name of the context in which the interface was created. The output from these commands should look similar to that displayed in the following example.
> In this example an interface named mgmt1 was configured in the local context.
> Intf Name: ipoa
> Intf Type: Point to point
> IP State: UP (Bound to 31/1 untagged, ifIndex 285278209)
> IP Address: 192.168.100.3 Subnet Mask: 255.255.255.0
> Bcast Address: 192.168.100.255 MTU: 1500
> Resoln Type: ARP ARP timeout: 3600 secs
> Number of Secondary Addresses: 0
> Total interface count: 1

> Step 2 | Verify that your port configuration settings are correct by entering the following command:

> show configuration port <slot#>/<port#>
> This command produces an output similar to that displayed in the following example:
> config
> port atm 31/1
> no shutdown
> pvc vpi 121 vci 4444
> no shutdown
> bind interface ipoa sgsn3g
> #exit
> end
> Creating and Configuring Frame Relay Interfaces and Ports
> This section shows the minimum configuration required to configure a frame relay interface on a channelized line card. To create and configure the frame relay interfaces and ports:

> Step 1 | Select a channelized line card (CLC/CLC2) and set the framing method by applying the example configuration in the Setting the Characteristics of the Channelized Line Card section.

> Step 2 | Configure the path, framing, mapping, Frame Relay characteristics, and the data link connection identifiers (DLCIs) as illustrated in the example configuration in the Configuring the Channel Characteristics section.

> Step 3 | Configure the appropriate timing source (BITS from the SPIO or line-timing from attached remote) to ensure transmit synchronization by applying the example configuration in the Configuring Transmit Timing Source section in the Configuring System Settings chapter.

> Important: Before you can move to Step 4 to bind a DLCI to a port, you must complete the link configuration by configuring Peer-NSEIs and/or SS7 routing domains as described in the SGSN Service Configuration Procedures chapter of the SGSN Administration Guide. Return to this procedure when your link configuration is complete.

> Step 4 | Bind the link to the port by applying the example configuration in the section for Binding a DLCI .

> Step 5 | Verify the card, port and link configuration and status with the commands illustrated in

> Step 6 | Save the configuration as described in the Verifying and Saving Your Configuration chapter.

> Setting the Characteristics of the Channelized Line Card
> Use the following example to set the operational characteristics, the framing type, the header type, the service type, and the boot time E1 framing type, for the Frame Relay Channelized Line Card (CLC):
> configure
> card <slot>
> framing <framing_type> [ ds1 | e1 ]
> header-type { 2-byte | 4-byte }
> initial-e1-framing { crc4 | standard }
> service-type frame-relay
> no shutdown
> end
> Notes:

> • | Make a note of the information you configure - you will need it again later for the path command used to configure channel characteristics.

> • | The default framing_type is SONET for the channelized line card.

> • | With releases 8.1 and higher, we recommend that you include the signal type, either ds1 (24 timeslots, 1.536 Mbps) or e1 (32 timeslots, 2.048 Mbps ), when defining the framing.

> • | With releases 8.1 and higher, you need to set the service-type for the CLC card to frame-relay. All other options are not fully supported at this time.

> Configuring the Channel Characteristics
> Use the following example to configure the path, framing, mapping, timeslots, and the Frame Relay interface and LMI characteristics for a specific CLC/CLC2 port:
> configure
> port channelized <slot#>/<port#>
> path <path_id> { ds1 | e1 } <number_of_connections> <frame_mapping> <multiplex#> <multiplex#> framing <framing_mode> mapping-mode <mapping_mode> [ timeslots <timeslot#> [ <timeslot#> ] ]
> Important: You should record the path definition values you enter as the information will be needed again with other configuration commands.
> frame-relay path <path_id> { ds1 | e1 } <number_of_connections> [ timeslot <timeslot#> [ intf-type <intf_type> [ lmi-type <lmi_type> ] ] ]
> dlci path <path_id> { ds1 | e1 } <number_of_connections> { dlci <dlci_id> | timeslot <timeslot#> }
> no shutdown
> end
> Binding a DLCI
> Use the following procedure to bind the data link conneciton identifier (DLCI) to the channelized (Frame Relay) port.
> Important: This procedure should not be attempted until after the configuration is completed for Peer-NSEIs and/or SS7 routing domains as described in the SGSN Administration Guide.
> configure
> port channelized <port#>
> bind link { peer-nsei <nse_id> ns-vc-id <nsvc_id> | ss7-routing-domain <ss7rd_id> linkset-id <id> link-id <id>}
> end
> Verifying the Frame Relay Interface Configuration and Status
> Several commands generate display outputs that provide information about the Frame Relay card, port, DLCI and link configurations. The most commonly used commands are illustrated below. All of these commands are issued from the Exec mode.
> Display Port and DLCI Configuration Details
> [local]<hostname>#show port info 27/1
> Port: 27/1
> Port Type : STM1/OC3 Channelized
> Description : (None Set)
> Controlled By Card : 11 (Packet Services Card)
> Redundancy Mode : Port Mode
> Framing Mode : SDH
> Redundant With : Not Redundant
> Preferred Port : Non-Revertive
> Physical ifIndex : 453050368
> Administrative State : Disabled
> Link State : Unknown
> Line Timing : Yes
> SFP Module : Not Present
> Path 1 e1 1 : tu12-au3 1/1 crc4 bit-async
> Timeslots : 12-14
> Frame Relay Intf Typ : DCE
> Frame Relay LMI Type : Q933A
> Frame Relay LMI n391 : 6
> Frame Relay LMI n392 : 2
> Frame Relay LMI n393 : 2
> Frame Relay LMI t391 : 10
> Frame Relay LMI t392 : 15
> Frame Relay DLCI 243
> Logical ifIndex : 453050369
> Admin State : Disabled
> Operational State : Down, Standby
> Shaping : WFQ: Weight 1
> Number of DLCI : 1
> Reserved Bandwidth : 0 of 192000 bits/sec
> Path 1 e1 2 : Unused
> Number of DLCI : 1
> Display Port and DLCI Configuration and Status
> The following display is only a partial output of the show command to illustrate the channelized port and DLCIs.
> show port table
> Port Type Admin Oper Link State Redundant With
> ---- ---------------------- -------- ---- ---- -------- --------------
> 27/1 STM1/OC3 Channelized Enabled - Up - None
> FR DLCI 1 1 1 52 Enabled Up - Active -
> FR DLCI 1 2 1 53 Enabled Down - Active -

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883