> Context Schema Statistics
> The Context schema provides operational statistics that can be used for monitoring and troubleshooting the following products: All
> Bulk Statistic Variables in the Context Schema

> Variables | Description | Data Type
> vpnname | Name of the VPN context. This is a key variable. Type: Information | String
> vpnid | Identifier for VPN context. This is a key variable. Type: Information | Int32
> sfw-total-rxpackets | Description: Total number of packets received by the Stateful Firewall in-line service. Triggers: Increments when a packet is received by the Stateful Firewall in-line service. Availability: Per Active Charging Service. | Int64
> sfw-total-rxbytes | Description: Total number of bytes received by the Stateful Firewall in-line service. Triggers: Increments when a packet having layload is received by the Stateful Firewall in-line service. Availability: Per Active Charging Service. | Int64
> sfw-total-txpackets | Description:: Total number of packets transmitted by the Stateful Firewall in-line service. Triggers: Increments when a packet is sent by the Stateful Firewall in-line service. Availability: Per Active Charging Service. | Int64
> sfw-total-txbytes | Description:: Total number of bytes transmitted by the Stateful Firewall in-line service. Triggers: ncrements when a packet having layload is forwarded by the Stateful Firewall in-line service. Availability: Per Active Charging Service. | Int64
> sfw-total-injectedpkts | Description:: Total number of packets injected by the Stateful Firewall in-line service. Triggers: Increments when a Firewall module creates and sends packets like RST. Availability: Per Active Charging Service. | Int64
> sfw-total-injectedbytes | Description:: Total number of bytes injected by the Stateful Firewall in-line service. Triggers: Increments when a Firewall module creates and sends packets like RST with data. Availability: Per Active Charging Service. | Int64
> sfw-dnlnk-droppkts | Description:: Total number of packets dropped by the Stateful Firewall in-line service in downlink direction. Triggers: Increments when Firewall drops a downlink packet due to any reason. Availability: Per Active Charging Service. | Int64
> sfw-dnlnk-dropbytes | Description:: Total number of bytes dropped by the Stateful Firewall in-line service in downlink direction. Triggers: Increments when Firewall drops a downlink packet with data due to any reason. Availability: Per Active Charging Service. | Int64
> sfw-uplnk-droppkts | Description:: Total number of packets dropped by the Stateful Firewall in-line service in uplink direction. Triggers: Increments when Firewall drops an uplink packet due to any reason. Availability: Per Active Charging Service. | Int64
> sfw-uplnk-dropbytes | Description:: Total number of bytes dropped by the Stateful Firewall in-line service in uplink direction. Triggers: Increments when Firewall drops an uplink packet with data due to any reason. Availability: Per Active Charging Service. | Int64
> sfw-total-malpackets | Description:: Total number of invalid packets received by the Stateful Firewall in-line service. Triggers: Increments when any packet is malformed and dropped by Firewall. Availability: Per Active Charging Service. | Int64
> sfw-ip-discardpackets | Description:: Total number of IP packets discarded by the Stateful Firewall in-line service. Triggers: Increments when any IP packet is discarded. Availability: Per Active Charging Service. | Int64
> sfw-ip-malpackets | Description:: Total number of invalid IP packets received by the Stateful Firewall in-line service. Triggers: Increments when any IP packet is malformed and discarded. Availability: Per Active Charging Service. | Int64
> sfw-icmp-discardpackets | Description:: Total number of invalid ICMP packets discarded by the Stateful Firewall in-line service. Triggers: Increments when any ICMP packet is discarded. Availability: Per Active Charging Service. | Int64
> sfw-icmp-malpackets | Description:: Total number of invalid ICMP packets received by the Stateful Firewall in-line service. Triggers: Increments when any ICMP packet is malformed and discarded. Availability: Per Active Charging Service. | Int64
> sfw-tcp-discardpackets | Description:: Total number of invalid TCP packets discarded by the Stateful Firewall in-line service. Triggers: Increments when any TCP packet is discarded. Availability: Per Active Charging Service. | Int64
> sfw-tcp-malpackets | Description:: Total number of invalid TCP packets received by the Stateful Firewall in-line service. Triggers: Increments when any TCP packet is malformed and discarded. Availability: Per Active Charging Service. | Int64
> sfw-udp-discardpackets | Description:: Total number of invalid UDP packets discarded by the Stateful Firewall in-line service. Triggers: Increments when any UDP packet is discarded. Availability: Per Active Charging Service. | Int64
> sfw-udp-malpackets | Description:: Total number of invalid UDP packets received by the Stateful Firewall in-line service. Triggers: Increments when any UDP packet is malformed and discarded. Availability: Per Active Charging Service. | Int64
> sfw-ipv6-discardpackets | Description:: Total number of IPv6 packets discarded by the Stateful Firewall in-line service. Triggers: Increments when any IPv6 packet is discarded. Availability: Per Active Charging Service. | Int64
> sfw-ipv6-malpackets | Description:: Total number of malformed IPv6 packets identified by the Stateful Firewall in-line service. Triggers: Increments when any IPv6 packet is malformed and discarded. Availability: Per Active Charging Service. | Int64
> sfw-icmpv6-discardpackets | Description:: Total number of ICMPv6 packets discarded by the Stateful Firewall in-line service. Triggers: Increments when any ICMPv6 packet is discarded. Availability: Per Active Charging Service. | Int64
> sfw-icmpv6-malpackets | Description:: Total number of malformed ICMPv6 packets indentified by the Stateful Firewall in-line service. Triggers: Increments when any ICMPv6 packet is malformed and discarded. Availability: Per Active Charging Service. | Int64
> sfw-total-dosattacks | Description:: Total number of DoS attacks detected by the Stateful Firewall in-line service. Triggers: Increments when a DOS attack is detected. Availability: Per Active Charging Service. | Int64
> sfw-total-flows | Description:: Total number of flows processed by the Stateful Firewall in-line service. Triggers: Increments when a new flow is processed by Firewall. Availability: Per Active Charging Service. | Int32
> dns-local-a-atmpts | Total number of local A query attempts. | Int32
> dns-local-srv-atmpts | Total number of local SRV query attempts. | Int32
> dns-local-aaaa-atmpts | Total number of local AAAA query attempts. | Int32
> dns-local-naptr-atmpts | Total number of local NAPTR query attempts. | Int32
> dns-local-a-succs | Total number of local A query successes. | Int32
> dns-local-srv-succs | Total number of local SRV query successes. | Int32
> dns-local-aaaa-succs | Total number of local AAAA query successes. | Int32
> dns-local-naptr-succs | Total number of local NAPTR query successes. | Int32
> dns-local-a-fails | Total number of local A query failures. | Int32
> dns-local-srv-fails | Total number of local SRV query failures. | Int32
> ns-local-aaaa-fails | Total number of local AAAA query failures. | Int32
> dns-local-naptr-fails | Total number of local NAPTR query failures. | Int32
> dns-primary-ns-a-atmpts | Total number of A query attempts to Primary Name server. | Int32
> dns-primary-ns-srv-atmpts | Total number of local SRV query attempts to Primary Name server. | Int32
> dns-primary-ns-aaaa-atmpts | Total number of local AAAA query attempts to Primary Name server. | Int32
> dns-primary-ns-naptr-atmpts | Total number of local NAPTR query attempts to Primary Name server. | Int32
> dns-primary-ns-a-succs | Total number of A query successes from Primary Name server. | Int32
> dns-primary-ns-srv-succs | Total number of local SRV query successes from Primary Name server. | Int32
> dns-primary-ns-aaaa-succs | Total number of local AAAA query successes from Primary Name server. | Int32
> dns-primary-ns-naptr-succs | Total number of local NAPTR query successes from Primary Name server. | Int32
> dns-primary-ns-a-fails | Total number of local A query failures from Primary Name server. | Int32
> dns-primary-ns-srv-fails | Total number of local SRV query failures from Primary Name server. | Int32
> dns-primary-ns-aaaa-fails | Total number of local AAAA query failures from Primary Name server. | Int32
> dns-primary-ns-naptr-fails | Total number of local NAPTR query failures from Primary Name server. | Int32
> dns-secondary-ns-a-atmpts | Total number of A query attempts to Secondary Name server. | Int32
> dns-secondary-ns-srv-atmpts | Total number of local SRV query attempts to Secondary Name server. | Int32
> dns-secondary-ns-aaaa-atmpts | Total number of local AAAA query attempts to Secondary Name server. | Int32
> dns-secondary-ns-naptr-atmpts | Total number of local NAPTR query attempts to Secondary Name server. | Int32
> dns-secondary-ns-a-succs | Total number of A query successes from Secondary Name server. | Int32
> dns-secondary-ns-srv-succs | Total number of local SRV query successes from Secondary Name server. | Int32
> dns-secondary-ns-aaaa-succs | Total number of local AAAA query successes from Secondary Name server. | Int32
> dns-secondary-ns-naptr-succs | Total number of local NAPTR query successes from Secondary Name server. | Int32
> dns-secondary-ns-a-fails | Total number of local A query failures from Secondary Name server. | Int32
> dns-secondary-ns-srv-fails | Total number of local SRV query failures from Secondary Name server. | Int32
> dns-secondary-ns-aaaa-fails | Total number of local AAAA query failures from Secondary Name server. | Int32
> dns-secondary-ns-naptr-fails | Total number of local NAPTR query failures from Secondary Name server. | Int32
> bgp-maxroute | Maximum number of BGP routes. It is the sum of all the VRFs in a context. Type: Information | Int32
> bgp-totroute | Total number of BGP routes. It is the sum of all the VRFs in a context. Type: Information | Int32
> Important: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883