> show gs-service
> This chapter includes the show gs-service command output tables.
> show gs-service all
> show gs-service all Command Output Descriptions

> Field | Description
> Service name | The Gs service that is running in this session.
> State | Status of the Gs service.
> Context | The name of the context in which Gs service is running.
> SGSN Number | The E.164 number for the SGSN to associate with the Gs service.
> SSN | Indicates the subsystem number configured or not. If configured it indicates SSN.
> Self SCCP Network Id | Indicates the SCCP network identifier configured or not. If configured it indicates SSCP network identifier.
> T6-1 Timeout | Indicates the retransmission timer (T6-1) value to guard the location update. Default: 10 seconds Range: 10 to 90 seconds
> T8 Timeout | Indicates the retransmission timer (T8) value to guard the explicit IMSI detach from the GPRS service procedure. Default: 4 seconds Range: 1 to 30 seconds
> T9 Timeout | Indicates the retransmission timer (T9) value to guard the explicit IMSI detach from the non-GPRS service procedure. Default: 4 seconds Range: 1 to 30 seconds
> T10 Timeout | Indicates the retransmission timer (T10) value to guard the implicit IMSI detach from the non-GPRS service procedure. Default: 4 seconds Range: 1 to 30 seconds
> T12-1 Timeout | Indicates the retransmission timer value (T12-1) in minutes to control the resetting of SGSN-Reset variable procedure. Default: 54 minutes (plus 8 seconds for transmission delay) Range: 0 to 380 minutes
> T12-2 Timeout | Indicates the retransmission timer (T10) value to guard the SGSN reset procedure. Default: 4 seconds Range: 1 to 30 seconds
> Max N8 Retries | Indicates the maximum retransmission allowed for procedure for explicit IMSI detach message from GPRS service (N8). Default: 2 retries Range: 0 to 10 retries
> Max N9 Retries | Indicates the maximum retransmission allowed for procedure for explicit IMSI detach message from non-GPRS service (N9). Default: 2 retries Range: 0 to 10 retries
> Max N10 Retries | Indicates the maximum retransmission allowed for procedure for implicit IMSI detach message from non-GPRS service (N10). Default: 2 retries Range: 0 to 10 retries
> Max N12 Retries | Indicates the maximum retransmission allowed for N12 procedure for sending BSSAP+ Reset Indication message (N12). Default: 2 retries Range: 0 to 10 retries
> GS Service Configurations
> LAC Id | Indicates the subscriber location area code identifier configured in Gs service. Range: 1 through 65535
> Pool Type | Type of pool area (non-pool area or pool area) configured in Gs service. Possible values are:
> • | Non Pool Area
> • | Pool Area
> Pool Area/ Non Pool Area name | Name of the configured Non-pool area or pool area in Gs service.
> Pool Area Configurations
> Pool Area Name | Name of the configured pool area in Gs service.
> Default Vlr | Name of the default VLR attached to this pool area.
> LAC in Pool Area | Indicates the subscriber location area code identifier configured in this pool area. Range: 1 through 65535
> VLR Hash Type | Indicates the type of hash configured for this pool area. Possible values are:
> • | Value
> • | Range
> Value / Range | Indicates the value of hash or range of hash.
> Vlr Name | Name of the VLR attached to this pool area.
> Non-Pool Area Configurations
> Non-Pool Area Name | Name of the configured non-pool area in Gs service.
> Vlr Name | Name of the VLR attached to this non-pool area.
> LAC in Pool Area | Indicates the subscriber location area code identifier configured in this non-pool area. Range: 1 through 65535
> VLR Configurations
> VLR Name | Name of the VLR attached to this Gs service.
> ISDN Numbe | Indicates the E.164 ISDN number of configured VLR.
> SSN | Indicates the subsystem number configured or not. If configured it indicates SSN.
> Point Code | Indicates the configured point code address for VLR in SS7 address format.a
> SGSN Reset | Indicates whether SGSN reset function is allowed or not. Possible values are:
> • | TRUE
> • | FALSE

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883